**Spillage Emergency Plan**

**Avonmouth**

|  |  |
| --- | --- |
| **Critical Equipment / Information** | **Location** |
| Spill Kits & Granules | Weighbridge, Haz cage (HRRC), Transfer Station  |
| Spillage Disposal Containers  | Haz Cage (HRRC)  |
| Quarantine Area | Haz Cage (HRRC) |
| Interceptor 1&2 controls | 1: Grass area behind fuel tank2: Grass area by Clinical Waste Co. |
| PPE | Gloves in the spill kit, other in site offices |
| First Aiders and Fire Wardens | Listed on notice board  |
| Site Address:  | Kings Weston LaneAvonmouthBristol BS11 0YS |

|  |  |  |
| --- | --- | --- |
| **Name** | **Position** | **Contacts Number** |
| Lee Andow / Kevin Perryman-Doyle | Site Supervisors | 07710 396972 / 07736 638779 |
| Craig Powell | Operation Manager  | 07795 446343 |
| Lucy Edgar  | SHEQ Director | 07970 955489 |
| Emergency Services | Fire / Ambulance / Police | 999 |
| Environmental Agency (surface & ground water) | Incident hotline (24h) | 0800 807060 |
| Cleaning Tanker  | Aquarius Waste  | 01179869815 (24h Emergency Call Out) |
| Wessex Water | Emergency Contact Number | 0345 6004600 |

**Spillage Emergency Plan**

|  |  |
| --- | --- |
| **Discovering Spill*** Notify personnel in the immediate area (call or verbally)
* Attend to contaminated personnel
* If flammable/volatile,
* Control any ignition sources & ventilate
* Evacuate area (if necessary – activate Fire Alarm)
* Cordon off area

**Protective Equipment** * Look at signs & labels for any hazard symbols
* Put on suitable PPE to avoid skin & eyes contact
* If respiratory protection, contact Emergency Services or

Specialise clean-up company or refer to Asbestos SWP* Spill Kit contains protective gloves. Other PPE in site office

**Containment (if safe)*** Stop the spill at source (e-stop, return to upright, plug leak)
* Capture spill (into secondary container)
* Divert/contain any spill on floor (socks/booms in spill kit)
* Protect any drains (drain cover/ plug in spill kit)
* Isolate interceptor pumps (turn power off)

**Absorption*** Spread absorbent granules or pads/socks in a circle around

the spill* Note: White pads are usually for oils only
* Infill until the spill is covered and allow time to absorb
 | **Contaminated Personnel*** Contaminated clothing must be removed immediately
* Apply first aid (if necessary)
* Use emergency showers (if necessary)
* If further medical attention required, take the Safety Data Sheet,

or any details about the substance from labels, transfer note, etc.**Clean up – Small spills*** Once spill is fully absorbed, pick up granules and move to 205l clip top drum (blue). Ensure area is swept clean
* Once full, move to storage area and arrange disposal

**Clean up – Large spills*** Mobile plant, sweepers, tankers and specialise contractors may be

required to clean large spills * Move to designated sealed container, in quarantine area, pending disposal

**Clean up – Batteries** * Use plastic scoop to transfer into hazardous waste bag and knot the top of the bag and place into another hazardous waste.

Bag and tie this up. Arrange disposal**Report and disposal*** All spillages must be reported to management
* Manager to notify Regulators (see page 1) if spillage enters surface water, groundwater or sewer
 |