**Spillage Emergency Plan**

**Avonmouth**

|  |  |
| --- | --- |
| **Critical Equipment / Information** | **Location** |
| Spill Kits & Granules | Weighbridge, Haz cage (HRRC), Transfer Station |
| Spillage Disposal Containers | Haz Cage (HRRC) |
| Quarantine Area | Haz Cage (HRRC) |
| Interceptor 1&2 controls | 1: Grass area behind fuel tank  2: Grass area by Clinical Waste Co. |
| PPE | Gloves in the spill kit, other in site offices |
| First Aiders and Fire Wardens | Listed on notice board |
| Site Address: | Kings Weston Lane  Avonmouth  Bristol  BS11 0YS |

|  |  |  |
| --- | --- | --- |
| **Name** | **Position** | **Contacts Number** |
| Lee Andow / Kevin Perryman-Doyle | Site Supervisors | 07710 396972 / 07736 638779 |
| Craig Powell | Operation Manager | 07795 446343 |
| Lucy Edgar | SHEQ Director | 07970 955489 |
| Emergency Services | Fire / Ambulance / Police | 999 |
| Environmental Agency (surface & ground water) | Incident hotline (24h) | 0800 807060 |
| Cleaning Tanker | Aquarius Waste | 01179869815 (24h Emergency Call Out) |
| Wessex Water | Emergency Contact Number | 0345 6004600 |

**Spillage Emergency Plan**

|  |  |
| --- | --- |
| **Discovering Spill**   * Notify personnel in the immediate area (call or verbally) * Attend to contaminated personnel * If flammable/volatile, * Control any ignition sources & ventilate * Evacuate area (if necessary – activate Fire Alarm) * Cordon off area   **Protective Equipment**   * Look at signs & labels for any hazard symbols * Put on suitable PPE to avoid skin & eyes contact * If respiratory protection, contact Emergency Services or   Specialise clean-up company or refer to Asbestos SWP   * Spill Kit contains protective gloves. Other PPE in site office   **Containment (if safe)**   * Stop the spill at source (e-stop, return to upright, plug leak) * Capture spill (into secondary container) * Divert/contain any spill on floor (socks/booms in spill kit) * Protect any drains (drain cover/ plug in spill kit) * Isolate interceptor pumps (turn power off)   **Absorption**   * Spread absorbent granules or pads/socks in a circle around   the spill   * Note: White pads are usually for oils only * Infill until the spill is covered and allow time to absorb | **Contaminated Personnel**   * Contaminated clothing must be removed immediately * Apply first aid (if necessary) * Use emergency showers (if necessary) * If further medical attention required, take the Safety Data Sheet,   or any details about the substance from labels, transfer note, etc.  **Clean up – Small spills**   * Once spill is fully absorbed, pick up granules and move to 205l clip top drum (blue). Ensure area is swept clean * Once full, move to storage area and arrange disposal   **Clean up – Large spills**   * Mobile plant, sweepers, tankers and specialise contractors may be   required to clean large spills   * Move to designated sealed container, in quarantine area, pending disposal   **Clean up – Batteries**   * Use plastic scoop to transfer into hazardous waste bag and knot the top of the bag and place into another hazardous waste.   Bag and tie this up. Arrange disposal  **Report and disposal**   * All spillages must be reported to management * Manager to notify Regulators (see page 1) if spillage enters surface water, groundwater or sewer |