**JOHN HADDOCK WASTE MANAGEMENT**

**OUR REFERENCE EPR/KB3103TN/A001**

**DATE 03/06/2021**

**NON- TECHNICAL SUMMARY**

The site will be a small site accepting only their own waste from their MINI and MIDI skips with a maximum of twelve skips per day.

The skips will be tipped in an enclosed three-sided shed with bays and sorted by hand and recyclables recovered and placed into the bays to await baling.

The residual waste will be loaded on to a roll on roll off bin for despatch to landfill.

The site will not be accepting food waste or putrescible waste therefore should not create any odour therefore no need for odour management plan (OMP).

The site will not be accepting dusty loads therefore no need for Emissions (Dust) Management Plan (DMP).

As most of the work will be done by hand and the upright baler is almost silent there should be no need for a Noise Management Plan (NMP).

As the site is not accepting food waste then there should be no need for a Pest Management Plan (PMP) But if signs of pests appear then the company will engage a pest management company.

To summarise this is a low impact operation that will be micromanaged by the director.

Input will be low approximately 5000 tons absolute maximum 10000 tons

Hazard management will be high.

John Haddock assocMCIWM