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Farm name: Cherry Rock Farm, Old Oak Farm, Newberries Farm	Operator: G & S Phelps	Permit number: EPR/NP3239UE
Review Date: 18th May 2026

	Schedule 1 activity or directly associated activity (DAA) description
	Relevant technical guidance note

	Feed storage and preparation
	· Selection and use of feed are in accordance with Sector Guidance Note (SGN) EPR6.09 ‘How to comply with your environmental permit for intensive farming’
· Feed is stored in purpose-built, covered, feed silos and tanks located next to broiler sheds. Feed is delivered to the farm by lorry from feed suppliers. Feed is blown, augured or pumped directly from the lorry into the relevant storage silos. Feed is piped from the silos to the sheds, minimising dust emissions. t
· Areas around buildings are kept free from build-up of manure and spilt feed
· [bookmark: _Hlk44918202]Selection and use of feed are in accordance with SGN EPR6.09 ‘How to comply with your environmental permit for intensive farming’
· Rations are matched to the animals’ needs. A nutritionist is employed to regularly review and reformulate diets, to optimise production and minimise excretion of nutrients. 

	Dirty Water & Manure storage
	· All manure is kept within broiler houses until houses are destocked.
· Manure is removed from buildings and exported directly to a third party.
· Dirty water pits are present at all sites. Diverter valves are used when water entering the pits is required to be stored. This occurs at wash down after destocking.
· All dirty water is exported off sites to a third party.
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	Dirty water and manure management
	· All dirty water and manure is exported from the site. Records are kept of the arrangements in place when dirty water and manure is exported from the site. We have written confirmation that the recipient will spread dirty water and manures to land in accordance with the Defra Code of Good Agricultural Practice and that the spreading will be in accordance with a manure management plan for receiving land.
· There are contingency arrangements in place, should the land become unavailable

	Fuel, oils and chemical storage
	· Fuel oil, oils, pesticides and veterinary medicines are all stored in bunded areas capable of retaining any spillage
· Fuel oil for the standby generators is stored in bunded tanks that meets the requirements of SSAFO. The bund has a capacity of 110% of the oil tank. The bund base and walls are impermeable to oil and water and designed to catch leaks from tank fittings (including the tanker connection point, site gauge and shut-off valve). The tank is not within 
10 m of a watercourse. There are no yard drains, ditches or land drains within 10 m. The tank tap through which fuel oil can be discharged is within the bund. The tap is locked shut when not in use
· The hose and tap are locked inside the bund when not in use


	Housing
	· Housing design and management is in accordance with SGN EPR6.09 ‘How to comply with your environmental permit for intensive farming’
· Litter housing system is in use at the farm. 
· Maintenance and upgrades take place regularly. The housing and drainage have been assessed as BAT.



	
	· The animal housing is of insulated construction. The housing is well insulated, where appropriate, and the sheds have a damp-proof course, which helps to reduce heat loss and condensation
· All buildings and structures on site are maintained in good repair, in accordance with the management system. There is a programme of inspection and planned preventative maintenance for the housing and drainage. Floors and walls are kept clean. Any cracks and damaged areas of yards and walls are repaired
· Litter is removed when houses are destocked.
· Drinkers have been designed to prevent leakage.
· Service checks are carried out on the ventilation system monthly.

	Drainage
	· There are no direct releases to ground water.
· Diverter valves are in place for when the yards are dirty in order to stop dirty water entering reed beds, swales and ditches.
· Copies of Drainage Plans are kept with the all compliance documentation.
· The clean water drainage systems are not contaminated. 
· Yard areas are kept visibly clean, drainage channels are kept clear and spilt feed and dust are cleaned up
· Drainage from the animal housing and water from cleaning out is treated as dirty and directed to the dirty water tanks for storage and removal. 
· Disinfectant footbaths are designed not to overflow. Used disinfectant is added to the dirty water storage.

	Livestock numbers and movements
	· A system is in place to record the number of animals on the farm at any one time. Animal movements on and off the farm are also recorded; these records will be available for inspection.

	Carcase incinerator
	· Fallen stock is disposed of in accordance with the current Animal By-Products Regulations. 
· All dead stock is disposed of via deadstock collection, as per the site plan to avoid contamination in lockable bins. 


	Pollution prevention measures
	· All operations are assessed annually for opportunities to reduce pollution risk and implementation schedules developed as appropriate
· All staff are trained in pollution risk identification, minimisation and emergency procedures for general site activity and activity relating to their work duties
· There is an accident management plan in place, with a procedure to review incidents

	Veterinary medicines and pest
	· Pesticides and veterinary medicines are kept in a store capable of retaining spillage, resistant to fire, and are kept



	control
	dry, frost-free and secure. Vermin control chemicals are brought on site by a registered contractor for use as needed. Chemicals to control flies and other insect pests will be stored within bunded and locked store.

	Hazardous waste
	· Veterinary waste is removed by the vet for safe disposal. Other hazardous waste, such as fluorescent light bulbs, waste oil, aerosols, etc. are removed by a licensed contractor with an adequate audit trail, meeting the requirements of the Environmental Permitting Regulations



Buildings inventory

For location of buildings, refer to the Site Plans

	Building name and ref on plan
	No of places
	Type of ventilation
	Floor type
	Manure management
	Feed
	Other

	Cherry Rock Farm – Houses 1-4
	150,000
	Side extraction
	Solid
	Litter. Removed when houses are destocked.
	Dry feed
	Insulated building

	Old Oak Farm – Houses 1-6
	240,000
	High Velocity Roof Fans >5.5m
	Solid
	Litter. Removed when houses are destocked.
	Dry Feed
	Insulated building

	Newberries Farm – Houses 1-4 
	115,000
	High Velocity Roof Fans >5.5m
	Solid
	Litter. Removed when houses are destocked
	Dry Feed
	Insulated building





Emissions

Table of emission points

	Emission point reference
	Emission point description and location
	Source

	Air

	Cherry Rock Farm
	Side extraction ventilation
	Houses 1-4


	Cherry Rock Farm
	Biomass boiler (NGR – SO 78151 26424)
	2 boilers with a thermal input of 0.221 MWth each

	Old Oak Farm
	High Velocity Roof Fans
	Houses 1-6

	Old Oak Farm
	Biomass Boiler (NGR – SO 77459 26539)
	1 boiler with a thermal input of 1.094 MWth 

	Newberries Farm
	High Velocity Roof Fans
	Houses 1-4

	Newberries Farm
	Biomass Boiler (NGR – SO 78880 26017)
	2 boilers with a thermal input of 0.221 MWth each

	Land

	Cherry Rock Farm

	Soakaway to ditch via reed bed at South of the site
	Discharge of clean roof and yard water via French drains from reed bed to ditch via soakaway.

	Old Oak Farm

	Soakway to ditch via swale at Southwest of the site
	Discharge of clean roof and yard water via French drains from swale to ditch via soakaway.

	Newberries Farm
	Soakaway to ditch via diverter valve in tank at North of site
	Discharge of clean roof and yard water via French drains from diverter valve in underground tank to ditch

	Water

	Cherry Rock Farm
	Discharge to ditch via reed bed
	Roof water from buildings and clean yard water via French drains

	Old Oak Farm
	Discharge to ditch via swale
	Roof Water from buildings and clean yard water via French drains

	Newberries Farm
	Discharge to ditch via diverter valve in underground tank
	Roof water from buildings and clean yard water via French drains



Flies
The farm manager undertakes regular inspections of the site. Appropriate actions are in place to prevent and control flies, should a nuisance arise. See Pest Management Plan (page 13).


Site operations and pollution prevention measures
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	Fueling
	Spillage on yard, overflowing
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	As above. Automatic closing
	As above
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	bund when not in use
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	Feed
	Nutrients: Phosphorus and nitrogen

Dust
	Delivery to storage areas: dry bulk
	Spillage, split or failed pipework, dust, failure of bins
	None
	Yes
	Purpose-made dedicated stores
	Pipework and bins inspected monthly to assess condition

	
	
	Delivery to
	Spillage, split bags
	None
	Yes
	Purpose-made dedicated stores storesstores
	Regular inspection

	
	
	storage
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	areas: dry
	
	
	
	
	equipment

	
	
	bagged
	
	
	
	
	

	
	
	Distribution: all
	Broken augers
	None
	Yes
	Auger runs only when necessary. Mostly within buildings
	Regular inspection of facilities and equipment
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	Nutrients,
	Storage
	Structural failure
	None
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Diverter valves in place to prevent storage of clean water.
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	Transfer from storage to tanker
	Pipework failure
Leaking tanker
	None
	Yes
	All equipment is regularly serviced.
All equipment used for removal serviced and maintained by third party removing dirty water.
	Regular  inspection of facilities and equipment

	
	
	Road transport to field
	Tanker failure, road accident
	None
	Yes
	Fully trained operators
All tanker work completed by external contractors with their own equipment

	Regular inspection of facilities and equipment

	
	
	Field
	Surface run-off, drain
	None
	Yes
	Spreading in accordance with
	Regular soil nutrient

	
	
	spreading
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	Management Plan

	Pesticides
	List
	Delivery and
	Spillage, leaks, overflowing,
	None
	Yes
	Transfer directly from delivery
	Deliveries monitored

	and biocides
	substances
	transfer from
	contamination of clean
	
	
	vehicle to dedicated store
	Regular inspection

	
	used
	vehicle to
	drains
	
	
	Damaged or suspect packaging
	of facilities and

	
	
	on-site
	
	
	
	rejected at time of delivery
	equipment

	
	
	storage
	
	
	
	Dedicated contained store to
	Full application

	
	
	Storage of
	
	
	
	current specification
	records

	
	
	pesticides
	
	
	
	Records kept
	Regular inspection

	
	
	Mixing of
	
	
	
	Dedicated mixing area,
	of storage area

	
	
	pesticides
	
	
	
	impermeable base, drains to
	Records kept

	
	
	Application
	
	
	
	Dirty water store.
	

	
	
	foot dip and
	
	
	
	Trained staff with appropriate
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	qualifications
	

	
	
	use
	
	
	
	Relevant Codes of Practice
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	followed
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Pest Management Plan

On-site and Pest Management Plan (PMP) assessment (options not mandatory): Template checklist for poultry farms

	Source
	Method
	On site check
	PMP
check
	Comment

	PMP
	Manage site activities in accordance with the PMP
	
	
	

	Fly monitoring
	Follow routine monitoring for flies using:
resting counts; adhesive paper fly catches, fly larval counts, other
	
	
	Regular checks of building by Farm Partner

	
	Fly species identified
	
	
	

	
	Trigger levels followed for the relevant monitoring method/s to initiate insecticidal control
	
	
	

	Manure management
	Daily check of water lines and drinkers for defects and/or spillages
	
	
	All checks completed daily by farm staff

	
	Buildings are watertight, with no water ingress from outside
	
	
	All checked daily by farm staff

	
	Manure holding areas well ventilated
	
	
	N/A

	
	Liquid feed stores are appropriately sealed and external sources and surrounding areas are kept as clean as practically possible. Try to organise vents so that flies cannot pass through these
	
	
	N/A

	
	Slurry removed frequently in accordance to NVZ regulations and FRfW
	
	
	N/A

	Infrastructure
	Buildings are in good condition and kept well maintained
	
	
	Maintenance Schedule kept

	Carcases
	Fallen stock is removed frequently
	
	
	Regular checks by Farm Partner

	
	Fallen stock bins are covered and locked
	
	
	Regular checks by Farm Partner

	Housekeeping
	Spillages are cleaned up as soon as possible
	
	
	Regular checks by Farm Partner

	
	Rubbish bins are emptied regularly
	
	
	Regular checks by Farm Partner



	Insecticide control options
	Insecticide labels are complied with and records kept of all treatments
	
	
	When required

	
	Fly baits used
	
	
	When required







[image: ]
image1.wmf

image3.png
AHDB





image2.png




