____________________________________________________________________________
____________________________________________________________________________
______________________________ ADMS 6.0 (6.0) ______________________________
_________________ Atmospheric Dispersion Modelling System __________________
____________________________________________________________________________
___ Copyright (C) 2023 Cambridge Environmental Research Consultants Ltd. ___
____________________________________________________________________________
_______________ This run was made at 20:41 on the 29/04/2025 _______________
____________________________________________________________________________
_______________________________ Report File ________________________________
____________________________________________________________________________


1. SETUP INFORMATION:

 Site name         :  Wood End 1000 @ 1
 Project name      :
 Coordinate system :  Unspecified regular Cartesian

 Input file pathname            : Z:\PROJECTS\WORKING\Wood_End_Ashperton\ADMS\fs\WEA_fs_2124.APL
 Command-line options           : /E1 /ADMS

 Model information:
  - Pathname C:\Program Files (x86)\CERC\ADMS 6\ADMSModel.exe
  - Version 6.0.0.1
  - Build number 8802
  - Release date March 2023


2. MODEL OPTIONS:

 Complex terrain
  - Modelling hills
  - Pathname of hills data Z:\PROJECTS\WORKING\Wood_End_Ashperton\ADMS\WEA_20km.ter
  - Modelling variable roughness
  - Pathname of roughness data Z:\PROJECTS\WORKING\Wood_End_Ashperton\ADMS\WEA_20km.ruf
  - Calculation grid resolution               = 64x64
  - Generating flow field output


3. SOURCE OPTIONS:

 Your run includes the following sources:

 1 volume source
  - 'H4_SIDE'

 VOLUME SOURCE GEOMETRY:

                    Source name, Height(m),               1st vertex, No. of vertices, Total area(m2), Depth(m),
                        H4_SIDE,      1.50,     (363828.9, 241280.6),               4,        1393.00,     3.00,

 EMISSION DATA:

                    Source name,     Units,        NH3,
                        H4_SIDE,    g/m3/s, 0.7580E-05,


4. METEOROLOGY:

 Site data:
  - Latitude (degrees)                        =     52.07
  - Dispersion site:
     > Surface roughness calculated from values in roughness file
        ~ Using model default Minimum Monin-Obukhov length (m)
        ~ Surface albedo                      =       .230 (Model default)
        ~ Priestley-Taylor parameter          =      1.000 (Model default)
        ~ Precipitation at dispersion site same as at met site
  - Meteorological measurement site:
     > Surface roughness (m)                  =       .186
        ~ Minimum Monin-Obukhov length same as at dispersion site
        ~ Surface albedo same as at dispersion site
        ~ Priestley-Taylor parameter same as at dispersion site

 Meteorological data:
  - From file Z:\PROJECTS\WORKING\Wood_End_Ashperton\ADMS\GFS_52.068_-2.529_01012021_01012025_NBLD.met
  - Sequential met data
  - Height of recorded wind (m)               =     10.0
  - Met lines with wind speed at 10m less than .75m/s are not modelled


5. BACKGROUND DATA:



6. GRID OPTIONS:

 Cartesian co-ordinate system
 Specified points output
  - 'anemo' at (363800.0, 241300.0, 10.0)


7. OUTPUT OPTIONS:

 Single source modelled
  - 'H4_SIDE'

 POLLUTANT OUTPUT DATA:

                      Pollutant,                                  Statistic, Condition, Percentiles, Exceedences, Validity,
                            NH3,    Short-term 1-hourly non-rolling (ug/m3),      None,         ---,         ---,     75.0,


____________________________ End of Report File ____________________________
