**N**

**Diverter valve**

**Location**

Of a 17 pig week cycle, yard is dirty for last 7weeks and clean for 10weeks. Yard is cleaned at the end of cycle and diverter switched to attenuation pond for clean weeks. After 10weeks, diverter valve is switched to Slurry store where yard has potential to be contaminated.

FYM Pad to slurry store

ONLY

Ditch D1

**Lined & covered Slurry Lagoon**

Ditch D2

Clean Roof Water to ditch

Clean Roof Water to harvesting tank

Clean Roof Water to ditch

Yard water dirty weeks 10-17 of pig cycle to Slurry Store

Yard water dirty weeks 10-17 of pig cycle to Slurry Store

FYM Pad to slurry store ONLY

Dirty Wash water to sumps

Straw

Shed

Clean Roof Water to ditch

Clean Roof Water to harvesting tank