**ARSWL 7 – Waste Types, Tonnages and Treatment Techniques - Apex Site, Cardrew Way, Cardrew Industrial Estate, Redruth, Cornwall TR15 1SS**

The only waste types to be accepted are those shown in the table below –

|  |  |  |
| --- | --- | --- |
| **Waste code** | **Description of waste** | **State** |
| 20 03 04 | Septic tank sludge | Sludge, Liquid |
| 16 10 02 | Aqueous liquid wastes other than those mentioned in 16 10 01  ***Portaloo toilets only, non hazardous waste stream*** | Sludge, Liquid |
| 20 03 03 | Street-cleaning residues and gully wastes | Solid. Sludge, Liquid |
| 19 08 05 | Sludge’s from treatment of urban waste water  ***Sludges and liquids from sewage / waste water treatment works*** | Sludge, Liquid |

**Treatment Capacity**

The maximum quantity of waste to be received within 1 week in 350 tonnes.

The maximum quantity of waste to be received within 1 year is 25,000 tonnes

Note: Max 50 tonnes per day disposal to the foul sewer.

**Storage of Waste**

The maximum volume of waste to be stored at any one time is 40 tonnes that will be within the screening and dewatering process.

40 Tonnes of gully waste

**Treatment Techniques**

The only treatment techniques will be screening and de-watering.