|  |  |
| --- | --- |
| Location | Lincoln Street Site Yard |
| Persons Covered | Li-Batt Recycling Staff, Slicker Recycling Drivers & Contractor Drivers |
| Activity Reference | Unloading Waste from Road Tanker to Storage Tank |
| COSHH Reference *(If applicable)* | 0001, 0002, 0003, 0004, 0005, 0006 |

# 

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Hazard | | People at Risk (NR) | Probability Event Will Occur (PE) | Frequency of Exposure (FE) | Likely Severity (LS) | **Hazard rating number**  ***(PE) x (FE) x (NR) x (LS)*** | **Overall**  **Risk** |
| **1** | Musculoskeletal injury whilst manual handling. | 1 | 2 | 4 | 3 | 24 | Medium |
| **2** | Falling from elevated position whilst attempting ascent or decent. | 1 | 1 | 4 | 4 | 16 | Medium |
| **3** | Fall from an elevated position. | 1 | 1 | 4 | 4 | 16 | Medium |
| **4** | Ingestion of waste fluid. | 1 | 1 | 4 | 3 | 12 | Low |
| **5** | Inhalation of waste fluid. | 1 | 1 | 4 | 3 | 12 | Low |
| **6** | Waste fluid contacting the skin. | 1 | 1 | 4 | 3 | 12 | Low |
| **7** | Waste fluid contacting the eye. | 1 | 1 | 4 | 3 | 12 | Low |
| **8** | Impact with a moving vehicle. | 2 | 1 | 4 | 4 | 32 | Medium |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Probability (PE)** | **Frequency (FE)** | **Likely Severity (LS)** | **People at Risk (NR)** | **Score** |  | **Overall Risk** | |
| Unlikely | Monthly | None | 1-2 | 1 |  | 1-12 | Low |
| Possible | Weekly | Minor Injury | 2-5 | 2 |  | 13 - 48 | Medium |
| Likely | Daily | Moderate Injury | 5-10 | 3 |  | >49 | High |
| Very Likely | >3x Daily | Severe Injury | >10 | 4 |  |  |  |

|  |  |
| --- | --- |
| **Existing Control Measures** | **Acceptable? (Y/N & Comments if required)** |
| The Working at Height Procedure (LSPP02) is always followed. | Y |
| The Unloading Waste from Road Tanker to Storage Tank procedure is always followed. | Y |
| Training in access and egress routes provided. | Y |
| On site access and egress routes are routinely inspected. | Y |
| Guard rails are always used when operating on top of a road tanker. | Y |
| Vehicles are placed in a state of permanent stop via parking brake or wheel chocks before work commences. | Y |

|  |  |
| --- | --- |
| Two-person maximum limit on top of road tankers when working. | Y |
| Access and egress equipment e.g. ladder or step, is inspected before use. | Y |
| Any obstacles that could/would impede the operator are removed from the area before work commences. | Y |
| Manual Handling Procedure is always followed. | Y |
| The traffic management procedure is always followed. | Y |
| Full coveralls worn always by production staff. | Y |
| Gloves and toe cap boots provided. | Y |
| Face mask and eye protection provided. | Y |
| Effective high visibility waistcoat provided. | Y |

|  |  |  |  |
| --- | --- | --- | --- |
| Further actions | **Responsibility** | **Completed** | **Review** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |