**Staxton Hens Standby Generator.**

Staxton Hens poultry operations has a standby generator.

The generator has a thermal input of 243kw.

Generator will not be tested more than 50hrs per annum.

Generator will not be operated more than 500hrs per annum averaged over 3 years, as backup for mains interruption, including testing.