Non-Technical Summary

Butterwick Whins has a permit for 65,000 bird places for the production of free range eggs, housed in two poultry houses.
Proposed Changes

Operator is proposing a further two poultry houses for the production of free range eggs. Both houses will operate an aviary system with twice weekly litter belt removal. Free range bird places to increase to 128,000 places. Ventilation will be by gable fans in both new houses. No heating requirement. All clean drainage (excepting periods of washdown) will be French drains piped to covered underground soakaways. No discharges off-site. All dirty water will be contained by underground dirty water tanks, prior to being exported off-site. Additional ground to be included in the site boundary.
Birds will be housed at point of lay (17 weeks old) and depopulated at the end of the birds egg laying cycle (76 weeks old), this will be done on an all-out all in basis. There will be approximately one cycle per annum (14 months). Birds are allowed to range by means of pop holes at the base of sides of the houses. The houses use an aviary system with twice weekly litter belt removal.
Before bird arrival the house floor will be covered to a minimum depth of 2 cm of bulk shavings. Temperature and humidity will be closely monitored on a daily basis to achieve bird comfort and a relative humidity of 55-60%, this should achieve litter with a high dry matter content which is important to minimising emissions. Ventilation is by gable extraction fans on poultry houses. The birds themselves generate sufficient heat to negate the need for any additional heating.
Water is via a nipple drinking system fitted with cups to reduce leakage and spills leading to drier litter.

Birds are fed a minimum of three diets during their cycle, with gradually reducing levels of protein and phosphorous as bird age increases.

Feed is delivered from a UKAS accredited feed mill and blown into bulk feed bins situated adjacent to the houses, from the feed bins the feed is augered into the houses and distributed to the birds via a pan or chain feeding system.

Fallen stock will be recorded daily and securely stored in vermin proof containers awaiting regular collection by a licenced renderer.

Manure belts are operated twice weekly removing litter from the houses.

At depletion any remaining litter will be removed from the site and used on operator controlled land. The site will then be pressure washed, disinfected and dried out prior to the cycle beginning again. All wash waters will be contained in sealed underground tanks.

The above measures are designed to reduce emissions, trees and hedges will trap dust particles reducing odour. Ammonia emissions will be reduced by reduced protein feed, maintaining good litter conditions. Containment of wash waters will prevent pollutants being released to the environment.

Records of tonnages of litter and wash water removal are recorded, wash water will be exported off site.
