**Lower Easton Farm Poultry Units Standby Generators.**

Lower Easton Farm poultry operations has two standby generators, each serving 4 poultry houses.

Generators have a thermal input of 990kw each.

Generators will not be test run more than 50hrs per annum.

Generators will not be operated more than 500hrs per annum averaged over 3 years, as backup for mains interruption, including testing.