BF Appendix 11 Proposed arrangement west end of new poultry building

Identical arrangements on other house

Duty fans (2)

Concrete plinth

Draining to swale

Support high capacity fans.(4) (summer only)

Rear plantation predominantly conifers

All exhaust fans to west end. Possible louvres to direct air downwards

Embankment made from site preparation material

To swale