**Anslow Farm Standby Generator.**

Anslow Farm poultry operations has a standby generator.

The generator has a thermal input of 848kw.

Generator will not be test run more than 50hrs per annum.

Generator will not be operated more than 500hrs per annum averaged over 3 years, as backup for mains interruption.