**Biomass Boiler**

Biomass boiler Nominal heat output 350Kwh

Number of boilers 1 Total heat output 350 Kwh

Thermal input 400kw

Back up gas heaters

Exhaust stack heights 1m above roof

Adjacent building – none within 25m

Farm Centre Grid Reference 421553,325081

Exhaust stack Grid Reference

421599,325017

Biomass fuel – Approved biomass, eg. virgin woodchip/Miscanthus