Table 1a – Types of activities

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Schedule 1 listed activities | | | | | | |
| Installation name | Schedule 1 references (See note 1) | Description of the Activity (See note 2) | Activity capacity (See note 3) | Annex I (D codes) and Annex II (R codes) and descriptions | Hazardous waste treatment capacity (if this applies) (See note 3) | Non-hazardous waste treatment capacity (if this applies) (See note 3) |
| Add extra rows if you need them. | Put your main activity first |  |  | For installations that take waste only | For installations that take waste only | For installations that take waste only |
| Factory | Section 6.8 Part A(1)(d)(ii) | Treating and processing materials intended for the production of food products from vegetable raw materials at a plant with a finished production capacity of more than 300 tonnes per day | Existing - 175 tonnes per hour  Increase to – 215 tonnes per hour due to the introduction of a third canning line (6th line overall) |  |  |  |
| Directly associated activities (See note 4) | | | | | | |
| Name of DAA | | Description of the DAA (please identify the schedule 1 activity it serves) | | | | |
| AR3 - Production of steam | | Section 6.8 Part A(1)(d)(ii) – Replace existing Natural gas fired 5.54 MW boiler 1 with a 9.17 MW boiler | | | | |