Higher Hall Farm Standby Generator.

Higher Hall Farm poultry operations has a standby generator.
Generator has a thermal input of 0.550MWth.
Generator will not be test run more than 50hrs per annum.
Generator will not be operated more than 500hrs per annum averaged over 3 years, as backup for mains interruption, including testing.
