Odour Assessment Higher Hall Farm
	Hazard
	Receptor
	Pathway
	Risk Management
	Probability of Exposure
	Consequence
	What is the overall risk

	


Odour from the manufacture and selection of feed
	


Sensitive receptors within 400m of installation
	
    



       Air
	Measures as described in EPR 6.09 Sector Guidance Note. Odour Management at Intensive Livestock Installations. No on site milling and mixing. Feed specifications prepared by the feed compounder’s nutrition specialist.
	




     Unlikely
	




Odour annoyance
	




Not significant if managed carefully.

	


Odour from feed delivery or storage
	


Sensitive receptors within 400m of installation
	
    



       Air
	Measures as described in EPR 6.09 Sector Guidance Note. Feed delivery will be sealed to minimise atmospheric dust. Any feed spillage of feed around bin is immediately swept up. Condition of feed bins is checked frequently so that any leaks or damage can be identified.
	




     Unlikely
	




Odour annoyance
	




Not significant.

	Odours arising from problems with housing ventilation system, inadequate air movement within house leading to high humidity and wet litter. Inadequate system design, causing poor dispersal of odours
	


Sensitive receptors within 400m of installation
	
    



       Air
	Measures as described in EPR 6.09 Sector Guidance Note. The ventilation system will regularly adjusted according to age and requirements of the flock
The ventilation will be designed to efficiently remove moisture from the house.
	




     Unlikely
	




Odour annoyance
	




Not significant.

	


Litter management: odours arising from wet litter (see above) The use of insufficient or poor quality litter. Spillage of water from drinking systems. Disease outbreaks, leading to wet litter.
	





Sensitive receptors within 400m of installation
	


    



       Air
	Measures as described in EPR 6.09 Sector Guidance Note. Controls on feed and ventilation (see above) help to maintain litter quality. Additional controls include insulated walls and ceilings to prevent condensation. Concrete floors to prevent water ingress. Stocking density at optimum level to prevent overcrowding. Use health plan, with specialist veterinary input used as necessary
	




     Unlikely
	




Odour annoyance
	




Not significant.

	Carcase disposal: inadequate storage of carcasses on site.
	Sensitive receptors within 400m of installation
	

       Air
	Measures as described in EPR 6.09 Sector Guidance Note. Carcasses are placed in sealed containers awaiting regular collection by a licensed renderer.
	


     Unlikely
	

Odour annoyance
	

Not significant.

	





House clean out
(de littering)
	




Sensitive receptors within 400m of installation
	






       Air
	Litter is carefully placed into trailers close to the house entrances. Trailers are sheeted before transporting off site. De littering will be avoided at weekends during summer months. No litter is stored on site. Litter will be exported off site for use in an AD plant.
	






     Likely
	






Odour annoyance
	






Not significant if carefully managed.

	House clean out
(Disinfection and fumigation)

	Sensitive receptors within 400m of installation
	

       Air
	Carried out by specialist contractors using DEFRA approved chemicals observing correct dilution rates.
	

     Unlikely
	
Odour annoyance
	
Not significant if carefully managed.



