**Strawberry Hill Farm Standby Generator.**

Strawberry Hill Farm poultry operations has a standby generator for use in the event of mains power failure.

The generator has a thermal input of 727kw.

Generator will not be tested more than 50hrs per annum.

Emergency use will not exceed 500hrs per annum averaged over 3 years.