**Hergest Camp Additional Odour Reduction**

**Installation of Heat Exchangers**

As a further measure to reduce odour emissions at the request of the Environment Agency, operator is proposing to install heat exchangers.

These can be installed within the site boundary and with no major infrastructure changes required to the poultry houses.

These will be the Big Dutchman Heat Exchangers, specifications, operations and maintenance requirements are in the attachments accompanying this document.

These heat exchangers will be cleaned and maintained by replacing filters at the crop turnaround with new cartridge filters. Therefore, there will be no need for extra underground dirty water storage tanks.

Emissions test report documents attached.