**Biomass Boiler at Westfields Farm Poultry Unit**

Boilers – Nominal heat output 199Kw each

Number of boilers 3 Total heat output 597Kw

Thermal input 215kwh each, total combined 645Kw

Exhaust stack height 1m above building heights.

Adjacent building heights 5m

Farm Centre Grid Reference 513786,446053

Exhaust stack Grid References

513858,446074 – 513796,446095 – 513744,446087

All three boilers meet the eligibility criteria for RHI.

Biomass fuel – Approved biomass, eg. virgin woodchip/Miscanthus/straw

Boiler ash securely stored and spread with litter under exemption.