EPR/VP3138FM/V003 Duly Making

Duly Making Questions

1. Non-Tech Summary (NTS)
Please update NTS adding following key points :

· Please add  attenuation type for roof water  and lightly contaminated yard water attenuation 
· Please confirm ONLY poultry house heating is via LPG heaters not a combination of biomass boilers and LPG heaters.
· Please confirm no new poultry houses just reusage of existing five houses.
· Please remove partial surrender requirements as this is not possible via a variation application

NB! We  require that either you remove partial area surrender from this application or withdraw variation application and resubmit as two applications to be determined together i.e. variation and partial surrender.

Updated the description of the drainage for roof water and lightly contaminated yard water in the non-technical summary for the introductory note on p3 and updated the key points on p2.

Removed the reference to a partial surrender of land not used for rearing poultry and returned the boundary in the updated the Drainage Schematic. Surrender of the land is not material to apply for change of use from ducks to broilers and will not be subject to a separate application. 

2. Odour Management Plan
· Please confirm if receptors within 100 m are operator /operator staff owned or not
· If operator /staff owned these can be removed from receptor tables
· If non staff receptors within 100 m please add to OMP statement that any substantiated odour complaints will trigger a review and improvement action plan with timescales in writing to Environment Agency for approval

None of the sensitive receptors have any control over the installation.

Confirmed some of the dwelling houses are owned and let by a farming partnership where Mr Christopher Sargent (the operator) is one of the partners, but the partnership has no control of the permitted day-to-day activity of rearing poultry or management of pollution prevention measures on the installation.

Added both actions and contingency actions in the Review and Complaints sections respectively on pp15-16. Used the words prescribed by the EA in another recent application. Submitted: -

Application Variation V003 Odour Management Plan 10082026.

3. Site Drainage Plan
· Please Update plan to cover following points
· Plan to include:
· Gable end fan outlets from poultry house 5 with area included for discharge and  area to either a) contain dust to prevent discharge into drains or b) include lightly contaminated drainage arrows and attenuation type for this drainage before leaving boundary
· Please confirm pond used for receipt of poultry house 1–3-yard area is unlined acting as a soakaway.
· For poultry houses 4/5-yard areas it appears lightly contaminated yard water does not go to pond within boundary. Please address attenuation for these yard areas confirming type of attenuation ,adding to plan and ensuring within installation boundary. Specifically, please address how drains cannot flow off site without attenuation.
· For each discharge of light contaminated yard water from boundary please ensure attenuation in place.

Updated the Drainage Schematic and labelling for all the points. 

Applying to enclose the solid wall underground pipe and the ditch on the north side of the farmyard. The ditch is already providing the attenuation of the lightly contaminated surface water runoff the concrete apron for all the poultry houses 1-5. 

Applying to enclose the pond inside the boundary on account it is also already providing a soakaway for  roof water runoff from houses 1-3 and conveys any excess into the inlet and offsite. 

Plus, updated the site condition report on p1, under surface waters, hydrology & catchment on p4, under historical land uses on p6 and under changes to the activity boundary on p9. Submitted:- 

Application Variation V003 Drainage Schematic 09082026
Application Variation V003 Site Condition Report 10082026.

4. Tech standards document
· Please ensure technical standards document and drainage are consistent
· Please add an emissions table to document with all air , water and land emissions ; in line with site drainage plan review above , with clear attenuation for yard water as review above and as below adding macerator location if location fixed when in use
· If there are multiple discharges from boundary of clean water after attenuation, please list each one and source of water i.e. roof /yard water and correct poultry houses.

Updated Table 2 Emissions (releases) at Friars Farm on pp6-7 in the technical standards. Submitted: -

Application Variation V003 Summary, Technical Standards and Control Measures 10082026.

5. Installation Boundary Plan
· Please resupply a plan with closer scale to allow locating features to be show 
· Please review boundary area
· Please ensure poultry houses are numbered
· Please revise plan to not surrender land area within this application.
Created a plan at a scale of 1:2500 showing locating features outside of the existing and proposed extension of the boundary. Submitted: -

Application Variation V003 Location Plan 10082026

6. Macerator 
Please provide a simple overview of macerator with capacity for eggs to be fed to it in kgs/hour , how often to be used per annum and cycle time for each usage
Please confirm if to be located when used in a specific location and if so, add location to emissions plan.

Added additional information in Table 4 Measures to control emissions at Friars Farm on pp10-11 in the technical standards. Location already marked on the Drainage Schematic.

7. Modelling

Please provide modelling input files for ammonia modelling.

Submitted via Google WeTransfer.
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