**Sheds 1-4 Weston Poultry Unit**

17 chimney fans per house at a proposed height of 6m can be taller if required.

Fan 3680M, cap at 30 Pa = 20.555 m3/h

m/s= 20.555 / (3600 x 0,5m2) = 11,41 m/s