**Middleton Stoney Litter Burning**

Existing boiler will use untreated litter produced on site as fuel with any surplus sold.

The litter store will have a maximum capacity of 300 tonnes, with an average annual storage of 150t for emission purposes, the store is operated under negative pressure with air drawn through the store for the combustion process. Store will remain sealed during the flock growing cycle reducing the potential for fugitive emission release and biosecurity.