**Biomass Boiler**

Make and Boiler Model – Jutsen Nominal heat output 1500Kw

Number of boilers 1 Total heat output 1500 Kw

Thermal Input 1725kw

Back up kerosene boiler

Exhaust stack heights 2.2m above roof heights

Adjacent building eaves heights 5.5 m

Farm Centre Grid Reference 340295,433169

Exhaust stack Grid Reference

340167,433243

Biomass fuel – Virgin Woodchip/ARB/Grade A.

MCPD compliant