**The Junctions Standby Generator.**

The Junctions poultry operations has a standby generator, each serving 5 poultry houses.

Generator has a thermal input of 757kw.

Generator will not be test run more than 50hrs per annum.

Generator will not be operated more than 500hrs per annum averaged over 3 years, as backup for mains interruption, including testing.