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Packaging For Recycling/Reuse

EWCs Accepted – 15-01-10*, 150102, 150104
Container Sizes – IBCs, 25L, 60L, 120L, 205L, <25L, <1L only with prior consent and additional info supplier
Conditions - <1% contamination by volume, contaminants must be readily removable in aqueous conditions. No POPs, No Water/Air Reactive, Non-Highly Toxic, Non-malodorous, no residues of prescribed substances, No-pressurised containers, no metallic or fine organic powders that may present an explosion / reactivity hazard. Materials may be assessed upon receipt to confirm suitability by waste acceptance testing through onsite laboratory or information on chemical composition

Materials – Plastic, Steel, Glass 
HP Codes Accepted – HP2 (with pre-treatment), HP3 (with pre-treatment) HP4, HP5, HP6 (cat 3,4 only), HP7, HP8, HP10, HP11, HP12, HP13, HP14, HP15

Hazard Statements Unsuitable for Treatment – Not accepted for Treatment
HP1 (or reactivity) – H200, H201, H202, H203, H204, H205
HP3 – H220, H221, H222, H223, H230, H231, H232, H240, H241, H242, H250, H251, H260, H261
HP6 – H300, H310, H330
Gases – H229, H280
Supplemental Hazards – EUH001, EUH006, EUH014, EUH018, EUH029

Suitable for Pre-treatment (see pre-treatment process)

HP2 – H270, H271, H272
HP3 - H225, H226, H228, H242

Pre-acceptance checks

Material must be clearly labelled with nature of previous contents and full list supplied for technical assessment. Containers must be nominally empty. Material must be presented palletised or in suitable containers to enable offloading a forklift truck
Containers must have lids and be sealed if they contain any liquid residues
Containers must be transported in accordance with ADR as appropriate

Acceptance Checks

Materials received are checked for compliance against pre-acceptance information supplied by customer against pre-acceptance information for suitability for washing process by site chemists. Any containers containing excess residues (>1%) and quarantined and customer is informed. Any containers received falling outside of scope of pre-acceptance information are quarantined pending approval of suitability to process or routing to third party disposal site (such as Highly Toxic materials or pressurised containers). Materials with excess residues will be assessed in-line with site waste acceptance procedures and residues sampled to enable compliant disposal. Where containers are received without previous contents being identified these are quarantined pending supplementary information supplied by the customer.
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