{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Read me","Power generation backup","Waste SML"," DfR and Inert landfill","Sewage Sludge AD","Tool","Comments","ValidationLists"],"not_rendered":{"charts":0,"images":10,"macros":1,"external_links":0,"defined_names":13,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Read me","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Power generation backup","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Waste SML","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":" DfR and Inert landfill","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sewage Sludge AD","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Tool","index":5,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,1,0,2]]}
[null,"QUALITATIVE NOISE SCREENING ASSESSMENT TOOL (QNST)"]
[]
[null,"STEP 1"]
[null,"STEP 2","Select from the drop-down lists"]
[]
[null,"Activity Containment","mainly indoors, some external delivery and goods handling",null,{"$f":"VLOOKUP(C6,Activity_containment,2,FALSE)","v":2},{"$f":"E6","v":2}]
[null,"Activity Type","wood recycling/ processing",null,{"$f":"VLOOKUP(C7,Activity_type,2,FALSE)","v":18},{"$f":"E7","v":18}]
[null,"Operation at night","NO",null,{"$f":"VLOOKUP(C8,Night_operation,2,FALSE)","v":0},{"$f":"E8","v":0}]
[null,"Operation Size","medium",null,{"$f":"VLOOKUP(C9,Operation_size,2,FALSE)","v":3}]
[null,"Input distance from site to the nearest residential receptor (m)",335,null,{"$f":"1*(60-20*LOG(distance_r))","v":9.4991038592630943},{"$f":"0.5*E10","v":4.7495519296315472}]
[null,"Residential receptor Location","rural",null,{"$f":"VLOOKUP(C11,Rec_location,2,FALSE)","v":10}]
[null,"Residential receptor proximity to other major noise source (m) e.g. busy road, other industrial activities, etc.","> 200",null,{"$f":"VLOOKUP(C12,Rec_disto_mainsource,2,FALSE)","v":10}]
[null,null,null,null,{"$f":"SUM(E6:E12)","v":52.499103859263094},{"$f":"SUM(F6,F7,F8,F9,F10)","v":24.749551929631547}]
[null,"STEP 3"]
[]
[null,"EVALUATION","NIA and NMP are not required"]
[]
[null,"Note that you need to reset the tool everytime you change a parameter or do a new screening."]
[null,"Before use copy to workspace. After use save to EDRM in Excel 97 - 03 format with QNST in subject/ title field."]

{"sheet":"Comments","index":6,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["Date","Comments"]

{"sheet":"ValidationLists","index":7,"n_rows":57,"n_cols":3,"rows_kept":57,"cut":false,"hidden":true,"merged":[]}
[null,"ACTIVITY CRITERIA","SCORE"]
[null,"activity containment"]
[null,"wholly indoors, no significant external delivery traffic",1]
[null,"mainly indoors, some external delivery and goods handling",2]
[null,"mainly indoors, external delivery, goods handling and storage",6]
[null,"mainly outdoors with external delivery, goods handling and storage ",8]
[null,"mainly outdoors with external delivery, goods handling, storage & processing",12]
[]
[null,"activity type (score from NIRS noise data) "]
[null,"anaerobic digestion",11]
[null,"chemical manufacturing",1]
[null,"composting",8]
[null,"DfR with no waste processing",-20]
[null,"DfR with waste processing",13]
[null,"ELV",20]
[null,"energy from waste",9]
[null,"food processing",7]
[null,"glass recycling",20]
[null,"ferrous and non-ferrous metal manufacture, handling & stocking",16]
[null,"landfill",5]
[null,"inert landfill with no waste processing",-20]
[null,"landfill with waste processing",16]
[null,"power generation",4]
[null,"power generation backup/ peaking ",11]
[null,"scrap metal",20]
[null,"sewage sludge AD",-10]
[null,"soil and aggregates",13]
[null,"waste transfer & storage with no processing",5]
[null,"waste recycling/ transfer/ treatment",15]
[null,"waste recycling/ transfer/ treatment of predominantly hard materials",20]
[null,"wood recycling/ processing",18]
[null,"other",4]
[null,"Operation size"]
[null,"small",0]
[null,"medium",3]
[null,"large",6]
[]
[null,"RECEPTOR CRITERIA","SCORE"]
[null,"Nearest Receptor distance (m)"]
[null,"Score for distance from boundary site to nearest receptor",{"$f":"60-20*LOG(distance_r)","v":9.4991038592630943}]
[null,"(linked to input distance_r at the 'User' sheet)"]
[null,"Receptor location"]
[null,"rural",10]
[null,"suburban",8]
[null,"urban",5]
[null,"inner city",3]
[]
[null,"Receptor proximity to other major noise source, e.g. busy road, other industrial activities (m)"]
[null,"< 50 m",2]
[null,"50 - 100",4]
[null,"100 - 200",7]
[null,"> 200",10]
[]
[null,"OPERATION AT NIGHT","SCORE"]
[null,"YES",10]
[null,"YES but ENCLOSED",3]
[null,"NO",0]