# Yew Tree Dairy PartCo Limited

# 416.065368.00001

# FORM PART B6 Addendum

Discharge points W1 and W2 discharge to the same United Utilities foul sewer (refer Figure 1 and Figure 2 below).

The discharge points include:

* Discharge point W1 – Runoff from the yard, internal spills, effluent from evaporative process (where not passed through the reverse osmosis plant).
* Discharge point W2 – foul drainage, over pumping from the attenuation tank (when required).

A computer screen shot of a map

Description automatically generated

Figure 1 – Effluent Discharge Points

A screenshot of a computer

Description automatically generated

Figure 2 – Drainage Plan