Noise Management Plan

Catfoss Airfield Ltd
Bewholme Farm Poultry Unit
The operations at Bewholme Farm Poultry Unit has the potential for noise production, prevailing wind is from the south west indicating the receptors located to the north east of the site would potentially be the highest at risk, the following plan has been prepared as part of the EPR permit application to prevent or minimise noise at Bewholme Farm  Poultry Unit. Bewholme Farm Poultry Unit has not been the subject of noise complaints, siting and location of noisy operations are sited as far as practical to be screened by woodland and buildings. Noise management plan to be reviewed annually or following a substantiated noise complaint.
Complaints Procedure

In the event of a substantiated noise complaint, the cause would be investigated and actions taken listed in the noise/contingency plans to cease the release. Area officer would be notified immediately, a review of the NMP conducted at the earliest opportunity with any changes communicated to Area officer for approval. A complaints report would be filled out and retained on site.

Example Noise Complaint form attached.

Bewholme Farm Poultry Unit operations have sensitive receptors within 400m of the site boundary. The site has no history of substantiated noise complaints.
The Table below gives location and direction of all sensitive receptors.
	Receptor Name
	Description
	Distance
	Orientation
	National Grid Reference

	Commercial building on Catfoss Industrial Estate, 
	Commercial 
	315m
	Southwest 
	513253,449041

	Commercial Building Catfoss Industrial Estate,
	Commercial
	304m
	Southwest 
	513268,449096

	Commercial Building Catfoss Industrial Estate off moor cottage rd 
	Commercial
	329m
	Southwest
	513264,449174

	Commercial Building Catfoss Industrial Estate, off Moor cottage rd.
	Commercial
	355m
	Northwest 
	513282,449260

	Commercial Building Catfoss Industrial Estate,off moor cottage rd
	Commercial
	361m
	Southwest
	513216,449134

	Commercial Building Catfoss Industrial Estate off moor cottage rd. 
	Commercial
	400m
	Southwest 
	513210,449106

	Commercial Building Catfoss Industrial Estate off moor cottage rd. 
	Commercial
	360m
	Southwest
	513210,449103

	Commercial Building Catfoss Industrial Estate off moor cottage rd. 
	Commercial
	399m
	Northwest
	513188,449348

	Farm building off new road 
	Commercial
	352m
	Northwest
	513235,449407

	Farm building off new road 
	Commercial
	348m
	Northwest
	513241,449531

	Farm building off new road 
	Commercial 
	384m
	Northwest
	513208,449501

	Commercial Building Catfoss Industrial Estate off moor cottage rd.
	Commercial
	333m
	Northwest
	513260,449355

	Commercial Building Catfoss Industrial Estate off moor cottage rd
	Commercial
	375m
	Northwest
	513239,449305

	Commercial building off Catfoss Lane
	Commercial
	397m
	Southwest 
	513199,448905

	Commercial building off Catfoss Lane
	Commercial
	348m
	South
	513398,448732

	Commercial building off Catfoss Lane
	Commercial
	317m
	South 
	513578,448687

	Commercial building off Catfoss Lane
	Commercial
	79m
	South 
	513623,448994

	Commercial building off Catfoss Lane 
	Commercial 
	97m
	South 
	513615,448968

	Property off Moor cottage Road
	Residential 
	340m
	North
	513567,449795

	Commercial building off Warley Cross
	Commercial 
	386m
	North
	513566,449835

	Commercial building off Warley Cross
	Commercial
	392m
	North 
	513525,449848

	Commercial building off Warley Cross
	Commercial
	400m
	North
	513553,449855

	Commercial building off Warley Cross
	Commercial
	375m
	North
	513531,449821

	Commercial building off Warley Cross
	Commercial 
	360m
	North
	513541,449808

	Farm property off Catfoss lane
	Residential
	19m
	West
	513563,449069

	Farm property off Warley Cross
	Residential 
	287m
	Northwest 
	513300,449455


A walk around assessment will be conducted to establish possible sources of noise emissions, and consideration given to different operations occurring during the whole of the production cycle.

Noise Management Plan

The main possible noise sources/operations are listed below:

1. Ventilation Fans

2. Feed Deliveries

3. Feeding Systems

4. Fuel Deliveries

5. Alarms Systems

6. Bird Catching

7. Clean out Operations

8. Maintenance + Repairs

9. Set up and Placement

10. Standby Generator testing 

                  A table listing these sources with measures to control/reduce noise emissions is listed below.

                  In the event of a complaint a report would be filled in (example attached)

The measures given in Noise plan reference the Noise Assessment document completed as part of the H1 Assessment

Other reference documents are the Emergency plan, Technical Standards and Routine Maintenance Schedule.

Noise Management Plan

	Potential Noise Problem
	Minimisation Techniques
	In Place Y/N
	Completion

Date

	Ventilation Fans
	Noise assessed during twice daily inspections (07.00-10.00 hrs and 16.00-18.00 hrs)
Large capacity roof mounted fans, reducing number of fans required

Fans operated on an intermittent programme

Regular end of cycle maintenance by qualified electrician. See routine maintenance schedule
Any noisy fans isolated and electrician notified
See Inspection and maintenance schedule/Technical standards

See site plan
	YES

YES

YES

Yes
Yes

	

	Feed Deliveries
	Delivery lorries fitted with silencers

Large capacity lorries to reduce no. of deliveries

Road/track maintenance

Time restricted if required
	YES

YES

YES
If required
	Continuous

If required

	Feeding Systems
	Daily inspections of bin stocks to prevent augers running empty (07.00-10.00 hrs and 16.00-18.00 hrs)
Feed bins located to reduce vehicle movements

Internal feeders checked twice daily to ensure correct operation (07.00-10.00 hrs and 16.00-18.00 hrs)
Regular end of cycle maintenance by qualified electrician. See Inspection and maintenance schedule/Technical standards
	YES

YES

YES

YES
	

	Fuel Deliveries
	Time restricted if required
Large capacity vehicles used
	If required Yes
	If required

	Vehicle movements
	Speed restriction on site 10mph

No idling engines or reversing warnings

Vehicles regularly maintained

Movements routed away from receptors as far as practical
	Yes

YES

YES

YES
	

	Alarm Systems
	Use of pagers or mobile phones

No audible alarms on site


	YES

YES
	

	Bird Catching
	Catch teams fully trained and advised of need to keep noise to a minimum ie no shouting or playing of loud music.
Crates to be handled carefully prior to house entry

Lorries scheduled to minimise duration of catch

Doors operated for entry and exit of forklift

Lorries parked as close as possible to doors to reduce forklift travel

Screen curtains fitted to lorries

See Inspection and maintenance schedule/Technical standards/Key responsibilities


	YES

YES

YES

YES

YES

YES


	

	Clean out operations
	Litter removal during normal working hours (07.00-18.00 hrs)
Trailers parked as close as possible to doors to reduce loader travel.
Large trailers used to reduce traffic.
All vehicles fitted with silencers.

Washing done during normal working hours 07.00hrs - 18.00hrs. 
Pressure washer machines to be operated at sides of buildings, screening from nearest receptors.

See Inspection and maintenance schedule/Technical standards/Key responsibilities.

	YES

YES

YES

YES

YES

YES
	

	Maintenance/Repair
	During normal working hours (07.00-1800 hrs excepting emergencies/breakdown
Routine end of cycle servicing. See Inspection and maintenance schedule/Technical standards/Key responsibilities


	YES

YES
	

	Set up/Placement
	Normal working hours 07.00hrs - 18.00hrs. See Inspection and maintenance schedule/Technical standards/Key responsibilities


	YES
	

	Standby Generator
	Test run weekly, typically 10.00am on Mondays. Housed in acoustic jacket. See Inspection and maintenance schedule/Technical standards/Key responsibilities

See site plan


	YES
	

	Noisy operations
	Sited as far as practical to be screened by other buildings and woodland.
	YES
	


Signed                                            Date                                               Review Date

Key Responsibilities
	Task
	Staff position responsible

	Noise assessments
	Manager

	Ventilation fans
	Site Supervisor/Maintenance team

	Roadway maintenance
	Manager

	Vehicle maintenance
	Manager/Mill Transport Manager

	Daily feed bin inspections
	Site Supervisor/Stockman

	Internal feeder checks
	Site Supervisor/Stockman

	Overseeing deliveries
	Site Supervisor/Stockman

	Overseeing bird catching
	Site Supervisor/Stockman

	Overseeing cleanout operations
	Site Supervisor/Stockman/Manager

	Alarm system/standby generator testing 
	Site Supervisor/Stockman


Monitoring Procedure

No monitoring currently undertaken. If substantiated complaints are founded then monitoring to take place on site to identify source of issue immediate action to be taken to minimise / rectify Source.
 Noise Complaint Form
	Installation to which complaint relates 
	Date received
	Reference number



	Name and Address of

Caller 


	

	Telephone Number
	

	Location of caller to Installation
	

	Time and Date of complaint
	

	Date/Time and Duration of 

Noise
	

	Callers description of Noise


	

	Other comments from caller


	

	Weather conditions 


	

	Wind direction/Speed


	

	Any previous complaints relating to this noise
	

	Any other comments


	

	Other information


	

	Potential source of noise


	

	Operations being carried out at time of complaint


	

	Follow up. Date/Time caller

Contacted
	

	Action Taken:


	

	Amendments required to plan


	

	Completed By:
	
	Signed:


	


Noise management plan to be reviewed annually or any changes to operations or following a substantiated noise complaint.
Version 1 July 2026
