{"text_format":"1","workbook":"xlsx","n_sheets":17,"sheets":["Summary","GraphData","FlatData","AssetDataExtract","FlatMaint","FlatRepair","RepairData","MaintData","Calculator","Instructions","Model","ValidationLists","AssetList","MaterialsData","MaterialValidationList","PlantList","DistanceLists"],"not_rendered":{"charts":8,"images":2,"macros":1,"external_links":1,"defined_names":112,"comments":1,"pivot_tables":8},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Summary","index":0,"n_rows":13,"n_cols":13,"rows_kept":13,"cut":false,"hidden":false,"merged":[[12,12,12,14],[5,1,5,3],[8,6,8,8],[9,6,9,8],[11,6,11,8],[12,6,12,8],[8,1,8,3],[8,12,8,14],[9,12,9,14],[11,12,11,14],[11,1,11,3],[12,1,12,3],[9,1,9,3]]}
[]
[]
[]
[]
[]
[null,"Summary"]
[]
[]
[null,"SOP",null,null,null,null,"Project manager",null,null,null,null,null,"Produced by"]
[null,{"$f":"IF(Calculator!$G$10=\"\",\"-\",Calculator!$G$10)","v":"IMSE50017"},null,null,null,null,{"$f":"IF(Calculator!$I$10=\"\",\"-\",Calculator!$I$10)","v":"Heather Taylor"},null,null,null,null,null,{"$f":"IF(Calculator!$E$10=\"\",\"-\",Calculator!$E$10)","v":"VHJ"}]
[]
[null,"Project name",null,null,null,null,"Date produced",null,null,null,null,null,"Reviewed by"]
[null,{"$f":"IF(Calculator!$H$10=\"\",\"-\",Calculator!$H$10)","v":"Oxford FAS"},null,null,null,null,{"$f":"IF(Calculator!$C$10=\"\",\"-\",Calculator!$C$10)","v":42583},null,null,null,null,null,{"$f":"IF(Calculator!$F$10=\"\",\"-\",Calculator!$F$10)","v":"-"}]

{"sheet":"GraphData","index":1,"n_rows":105,"n_cols":23,"rows_kept":105,"cut":false,"hidden":true,"merged":[]}
["Culmative Whole Life Carbon",null,null,"Whole Life Carbon by Asset",null,null,"Whole Life Carbon per New Build Stage",null,null,"Whole Life Operational Carbon per Asset",null,null,"Whole Life Use Carbon Operational stage",null,null,"Carbon by Stage",null,null,"Material Carbon",null,null,"Whole Life New Build per Asset"]
["Row Labels","Whole Life carbon",null,"Row Labels","Whole Life Carbon",null,"Values",null,null,"Row Labels","Whole Life Operational Carbon",null,"Values",null,null,"Values",null,null,"Row Labels","CO2e (t) ",null,"Row Labels","Sum of WLCDF"]
[0,1833.0440159490679,null,"(blank)",null,null,"Materials",1809.4145040000001,null,"(blank)",null,null,"Use ",3.5292202163767392,null,"Capital Carbon",1833.0440159490679,null,"Steel",1744.0524,null,"(blank)"]
[1,2040.4188273403722,null,"Bridge - Pedestrian",10431.990501132987,null,"Materials Transport ",1.7827364568500002,null,"Bridge - Pedestrian",8106.0783515732637,null,"Maintenance ",6732.681317044955,null,"Operational Carbon",8106.0783515732637,null,"Stone",3.081,null,"Bridge - Pedestrian",10431.990501132987]
[2,2323.4669423003479,null,"Grand Total",10431.990501132987,null,"People Transport ",10.040254635476996,null,"Grand Total",8106.0783515732637,null,"Repair",1369.8678143119284,null,"Replacement Carbon",722.43695498945863,null,"(blank)",0,null,"Grand Total",10431.990501132987]
[3,2517.0535477205954,null,null,null,null,"Plant Transport ",0.26511050064000069,null,null,null,null,"Energy",0,null,"Refurbishment Carbon",231.23957849294123,null,"Concrete",37.225103999999995]
[4,2781.2819917542724,null,null,null,null,"Site Establishment ",11.288744736000005,null,null,null,null,null,null,null,"Demolition Carbon",3.6201670655063309,null,"Timber",25.055999999999997]
[5,2961.997159361682,null,null,null,null,"Plant Use ",0,null,null,null,null,null,null,null,"Residual Carbon",-464.42856693723741,null,"Grand Total",1809.4145040000001]
[6,3208.6572392082849,null,null,null,null,"Waste ",0.25266562010085347]
[7,3377.3567818883098]
[8,3607.6166057783448]
[9,3765.0994340170669]
[10,3980.0494434828984]
[11,4127.0613487677092]
[12,4327.7194826479226]
[13,4464.9566693125462]
[14,4652.2731844052796]
[15,4780.3855666448871]
[16,4955.2475378392983]
[17,5074.841817509403]
[18,5238.0773387065474]
[19,5349.7198784812017]
[20,5614.5821691580795]
[21,5718.8016746538015]
[22,5861.0520008853791]
[23,5958.3420244525305]
[24,6091.1342261203199]
[25,6181.9555041591557]
[26,6305.9184453412499]
[27,6390.7010802114546]
[28,6506.4218122538305]
[29,6585.5673091104245]
[30,7014.2641612970174]
[31,7100.1145741412765]
[32,7217.8615538368203]
[33,7298.7838017812628]
[34,7409.7716231551376]
[35,7486.048603025477]
[36,7590.6652694161594]
[37,7662.5636386030192]
[38,7761.1748803700875]
[39,7828.9459890390099]
[40,7949.3789462866544]
[41,8013.2597160754394]
[42,8100.874527164362]
[43,8161.0882794395857]
[44,8243.673641951531]
[45,8300.43087851975]
[46,8378.2755033778376]
[47,8431.7746423807785]
[48,8505.1506673200638]
[49,8555.578736886413]
[50,8675.7957383668272]
[51,8723.3290304455804]
[52,8788.5226782316731]
[53,8833.3273648927661]
[54,8894.7786305974441]
[55,8937.0113449542096]
[56,8994.9350566185312]
[57,9034.7434404028336]
[58,9089.342094059466]
[59,9126.8653137637757]
[60,9485.0269825138803]
[61,9520.3962159046896]
[62,9568.9064125122422]
[63,9602.2453072156168]
[64,9647.9708200891691]
[65,9679.3959258516097]
[66,9722.4966072292646]
[67,9752.1177833650363]
[68,9792.7443093124912]
[69,9820.6651087618011]
[70,9858.9595059221883]
[71,9885.2775372628512]
[72,9921.373679368975]
[73,9946.1809480471384]
[74,9980.2050239318814]
[75,10003.5882539047]
[76,10050.010611935262]
[77,10082.070257644791]
[78,10126.255726323494]
[79,10156.770558646662]
[80,10230.225761141623]
[81,10259.270217844221]
[82,10299.300071684473]
[83,10326.945003703602]
[84,10365.045994866245]
[85,10391.358839143822]
[86,10427.623911041637]
[87,10452.668855029813]
[88,10487.186472541118]
[89,10511.024610780905]
[90,10641.405189118139]
[91,10664.094672273201]
[92,10695.365930114518]
[93,10716.962106823679]
[94,10746.726540224101]
[95,10767.282092118603]
[96,10795.612308323645]
[97,10815.177378538519]
[98,10842.142486169731]
[99,10860.76480166277]
[100,10431.990501133001]
["(blank)",10431.990501133001]
["Grand Total"]

{"sheet":"FlatData","index":2,"n_rows":506,"n_cols":60,"rows_kept":506,"cut":false,"hidden":true,"merged":[]}
["Asset ID","Asset description","Asset class","Sub-Asset ref.","Sub-Asset description","Sub-Asset category","Standard life","Expected new build life","Refurbishment type","Expected refurbished Life","First intervention","Last Refurb","Last Replace","Remaining Life","Last intervention","Weighted Split","Materials","Materials Transport","People Transport","Plant Transport","Site Establishment","Plant use","Waste","New Build Co2e","Use","Energy","Refurbishment","Den - Material Waste","Dem - Plant use","Dem - People","Year","Profile","Discount Factor","MaterialsDF","Materials TransportDF","People TransportDF","Plant TransportDF","Site EstablishmentDF","Plant UseDF","WasteDF","CapitalDF","UseDF","MaintenanceDF","RepairDF","EnergyDF","OP Co2eDF","RefurbDF","Dem - MaterialsDF","Dem - Plant","Dem - PeopleDf","ReplacementDF","WLCDF","Residual","Replace Materials TransportDF","Replace People TransportDF","Replace Plant TransportDF","Replace MaterialsDF","Replace Site EstablishmentDF","Replace Plant UseDF","Replace WasteDF"]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,0,1,{"$f":"VLOOKUP(AE2,ValidationLists!$M$1:$N$102,2,FALSE)","v":1},{"$f":"IF(AE2=0,Q2*AG2,0)","v":883.50840000000005},{"$f":"IF(AE2=0,R2*AG2,0)","v":1.0741763547000001},{"$f":"IF(AE2=0,S2*AG2,0)","v":4.9024970723805303},{"$f":"IF(AE2=0,T2*AG2,0)","v":0.12944925207897301},{"$f":"IF(AE2=0,U2*AG2,0)","v":5.5121149839704104},{"$f":"IF(AE2=0,V2*AG2,0)","v":0},{"$f":"IF(AE2=0,W2*AG2,0)","v":0.120639908490131},{"$f":"IF(AE2=0,AH2+AI2+AJ2+AK2+AL2+AM2+AN2,0)","v":895.24727757162009},{"$f":"IF(OR(AF2=3,AF2=2,AF2=0),Y2*AG2,0)","v":0},{"$f":"IF(OR(AF2=3,AF2=2,AF2=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D2,FlatMaint!$Y$2:$Y$10000,AE2)*AG2,0)","v":0},{"$f":"IF(OR(AF2=3,AF2=2,AF2=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D2,FlatRepair!$Y$2:$Y$10000,AE2)*AG2,0)","v":0},{"$f":"IF(OR(AF2=3,AF2=2,AF2=0),Z2*AG2,0)","v":0},{"$f":"AP2+AQ2+AR2+AS2","v":0},{"$f":"IF(AF2=2,AA2*AG2,0)","v":0},{"$f":"IF(AF2=3,AB2*AG2,0)","v":0},{"$f":"IF(AF2=3,AC2*AG2,0)","v":0},{"$f":"IF(AF2=3,AD2*AG2,0)","v":0},{"$f":"IF($AF$2=3,BB2+BC2+BD2+BE2+BF2+BG2+BH2,BB2+BC2+BD2+BE2+BF2+BG2+BH2)","v":0},{"$f":"AO2+AT2+AU2+AV2+AW2+AX2+AY2+BA2","v":895.24727757162009},{"$f":"IFERROR(IF(AE2=100,IF(O2=3,(N2/H2)*(X2*AG2)*-1,(N2/M2)*(X2*AG2)*-1),0),0)","v":0},{"$f":"IF($AF2=3,IF($AF$2=2,(R2/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I2,Refurb_Poss_Tbl[%]))*AG2,IF($AF$2=3,(R2*AG2)-AV2,R2*AG2)),0)","v":0},{"$f":"IF(AF2=3,IF($AF$2=2,(S2/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I2,Refurb_Poss_Tbl[%]))*AG2,IF($AF$2=3,(S2*AG2)-AX2,S2*AG2)),0)","v":0},{"$f":"IF($AF2=3,IF($AF$2=2,(T2/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I2,Refurb_Poss_Tbl[%]))*AG2,T2*$AG2),0)","v":0},{"$f":"IF($AF2=3,IF($AF$2=2,(Q2/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I2,Refurb_Poss_Tbl[%]))*AG2,Q2*$AG2),0)","v":0},{"$f":"IF($AF2=3,IF($AF$2=2,(U2/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I2,Refurb_Poss_Tbl[%]))*AG2,U2*$AG2),0)","v":0},{"$f":"IF($AF2=3,IF($AF$2=2,(V2/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I2,Refurb_Poss_Tbl[%]))*AG2,IF($AF$2=3,(V2*AG2)-AW2,V2*AG2)),0)","v":0},{"$f":"IF($AF2=3,IF($AF$2=2,(W2/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I2,Refurb_Poss_Tbl[%]))*AG2,W2*$AG2),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,1,0,{"$f":"VLOOKUP(AE3,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.96618357487922713},{"$f":"IF(AE3=0,Q3*AG3,0)","v":0},{"$f":"IF(AE3=0,R3*AG3,0)","v":0},{"$f":"IF(AE3=0,S3*AG3,0)","v":0},{"$f":"IF(AE3=0,T3*AG3,0)","v":0},{"$f":"IF(AE3=0,U3*AG3,0)","v":0},{"$f":"IF(AE3=0,V3*AG3,0)","v":0},{"$f":"IF(AE3=0,W3*AG3,0)","v":0},{"$f":"IF(AE3=0,AH3+AI3+AJ3+AK3+AL3+AM3+AN3,0)","v":0},{"$f":"IF(OR(AF3=3,AF3=2,AF3=0),Y3*AG3,0)","v":5.3050774138103766E-2},{"$f":"IF(OR(AF3=3,AF3=2,AF3=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D3,FlatMaint!$Y$2:$Y$10000,AE3)*AG3,0)","v":85.377900635748816},{"$f":"IF(OR(AF3=3,AF3=2,AF3=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D3,FlatRepair!$Y$2:$Y$10000,AE3)*AG3,0)","v":0},{"$f":"IF(OR(AF3=3,AF3=2,AF3=0),Z3*AG3,0)","v":0},{"$f":"AP3+AQ3+AR3+AS3","v":85.430951409886916},{"$f":"IF(AF3=2,AA3*AG3,0)","v":0},{"$f":"IF(AF3=3,AB3*AG3,0)","v":0},{"$f":"IF(AF3=3,AC3*AG3,0)","v":0},{"$f":"IF(AF3=3,AD3*AG3,0)","v":0},{"$f":"IF($AF$2=3,BB3+BC3+BD3+BE3+BF3+BG3+BH3,BB3+BC3+BD3+BE3+BF3+BG3+BH3)","v":0},{"$f":"AO3+AT3+AU3+AV3+AW3+AX3+AY3+BA3","v":85.430951409886916},{"$f":"IFERROR(IF(AE3=100,IF(O3=3,(N3/H3)*(X3*AG3)*-1,(N3/M3)*(X3*AG3)*-1),0),0)","v":0},{"$f":"IF($AF3=3,IF($AF$2=2,(R3/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I3,Refurb_Poss_Tbl[%]))*AG3,IF($AF$2=3,(R3*AG3)-AV3,R3*AG3)),0)","v":0},{"$f":"IF(AF3=3,IF($AF$2=2,(S3/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I3,Refurb_Poss_Tbl[%]))*AG3,IF($AF$2=3,(S3*AG3)-AX3,S3*AG3)),0)","v":0},{"$f":"IF($AF3=3,IF($AF$2=2,(T3/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I3,Refurb_Poss_Tbl[%]))*AG3,T3*$AG3),0)","v":0},{"$f":"IF($AF3=3,IF($AF$2=2,(Q3/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I3,Refurb_Poss_Tbl[%]))*AG3,Q3*$AG3),0)","v":0},{"$f":"IF($AF3=3,IF($AF$2=2,(U3/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I3,Refurb_Poss_Tbl[%]))*AG3,U3*$AG3),0)","v":0},{"$f":"IF($AF3=3,IF($AF$2=2,(V3/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I3,Refurb_Poss_Tbl[%]))*AG3,IF($AF$2=3,(V3*AG3)-AW3,V3*AG3)),0)","v":0},{"$f":"IF($AF3=3,IF($AF$2=2,(W3/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I3,Refurb_Poss_Tbl[%]))*AG3,W3*$AG3),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,2,0,{"$f":"VLOOKUP(AE4,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.93351070036640305},0,0,0,0,0,0,0,0,5.1256786606863544E-2,{"$f":"IF(OR(AF4=3,AF4=2,AF4=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D4,FlatMaint!$Y$2:$Y$10000,AE4)*AG4,0)","v":82.490725251931224},{"$f":"IF(OR(AF4=3,AF4=2,AF4=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D4,FlatRepair!$Y$2:$Y$10000,AE4)*AG4,0)","v":0},0,82.54198203853808,0,0,0,0,0,82.54198203853808,0,{"$f":"IF($AF4=3,IF($AF$2=2,(R4/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I4,Refurb_Poss_Tbl[%]))*AG4,IF($AF$2=3,(R4*AG4)-AV4,R4*AG4)),0)","v":0},{"$f":"IF(AF4=3,IF($AF$2=2,(S4/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I4,Refurb_Poss_Tbl[%]))*AG4,IF($AF$2=3,(S4*AG4)-AX4,S4*AG4)),0)","v":0},{"$f":"IF($AF4=3,IF($AF$2=2,(T4/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I4,Refurb_Poss_Tbl[%]))*AG4,T4*$AG4),0)","v":0},{"$f":"IF($AF4=3,IF($AF$2=2,(Q4/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I4,Refurb_Poss_Tbl[%]))*AG4,Q4*$AG4),0)","v":0},{"$f":"IF($AF4=3,IF($AF$2=2,(U4/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I4,Refurb_Poss_Tbl[%]))*AG4,U4*$AG4),0)","v":0},{"$f":"IF($AF4=3,IF($AF$2=2,(V4/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I4,Refurb_Poss_Tbl[%]))*AG4,IF($AF$2=3,(V4*AG4)-AW4,V4*AG4)),0)","v":0},{"$f":"IF($AF4=3,IF($AF$2=2,(W4/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I4,Refurb_Poss_Tbl[%]))*AG4,W4*$AG4),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,3,0,{"$f":"VLOOKUP(AE5,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.90194270566802237},0,0,0,0,0,0,0,0,4.9523465320641114E-2,{"$f":"IF(OR(AF5=3,AF5=2,AF5=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D5,FlatMaint!$Y$2:$Y$10000,AE5)*AG5,0)","v":79.701183818291042},{"$f":"IF(OR(AF5=3,AF5=2,AF5=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D5,FlatRepair!$Y$2:$Y$10000,AE5)*AG5,0)","v":0},0,79.750707283611689,0,0,0,0,0,79.750707283611689,0,{"$f":"IF($AF5=3,IF($AF$2=2,(R5/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I5,Refurb_Poss_Tbl[%]))*AG5,IF($AF$2=3,(R5*AG5)-AV5,R5*AG5)),0)","v":0},{"$f":"IF(AF5=3,IF($AF$2=2,(S5/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I5,Refurb_Poss_Tbl[%]))*AG5,IF($AF$2=3,(S5*AG5)-AX5,S5*AG5)),0)","v":0},{"$f":"IF($AF5=3,IF($AF$2=2,(T5/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I5,Refurb_Poss_Tbl[%]))*AG5,T5*$AG5),0)","v":0},{"$f":"IF($AF5=3,IF($AF$2=2,(Q5/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I5,Refurb_Poss_Tbl[%]))*AG5,Q5*$AG5),0)","v":0},{"$f":"IF($AF5=3,IF($AF$2=2,(U5/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I5,Refurb_Poss_Tbl[%]))*AG5,U5*$AG5),0)","v":0},{"$f":"IF($AF5=3,IF($AF$2=2,(V5/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I5,Refurb_Poss_Tbl[%]))*AG5,IF($AF$2=3,(V5*AG5)-AW5,V5*AG5)),0)","v":0},{"$f":"IF($AF5=3,IF($AF$2=2,(W5/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I5,Refurb_Poss_Tbl[%]))*AG5,W5*$AG5),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,4,0,{"$f":"VLOOKUP(AE6,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.87144222769857238},0,0,0,0,0,0,0,0,4.7848758763904459E-2,{"$f":"IF(OR(AF6=3,AF6=2,AF6=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D6,FlatMaint!$Y$2:$Y$10000,AE6)*AG6,0)","v":77.005974703662844},{"$f":"IF(OR(AF6=3,AF6=2,AF6=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D6,FlatRepair!$Y$2:$Y$10000,AE6)*AG6,0)","v":0},0,77.053823462426749,0,0,0,0,0,77.053823462426749,0,{"$f":"IF($AF6=3,IF($AF$2=2,(R6/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I6,Refurb_Poss_Tbl[%]))*AG6,IF($AF$2=3,(R6*AG6)-AV6,R6*AG6)),0)","v":0},{"$f":"IF(AF6=3,IF($AF$2=2,(S6/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I6,Refurb_Poss_Tbl[%]))*AG6,IF($AF$2=3,(S6*AG6)-AX6,S6*AG6)),0)","v":0},{"$f":"IF($AF6=3,IF($AF$2=2,(T6/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I6,Refurb_Poss_Tbl[%]))*AG6,T6*$AG6),0)","v":0},{"$f":"IF($AF6=3,IF($AF$2=2,(Q6/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I6,Refurb_Poss_Tbl[%]))*AG6,Q6*$AG6),0)","v":0},{"$f":"IF($AF6=3,IF($AF$2=2,(U6/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I6,Refurb_Poss_Tbl[%]))*AG6,U6*$AG6),0)","v":0},{"$f":"IF($AF6=3,IF($AF$2=2,(V6/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I6,Refurb_Poss_Tbl[%]))*AG6,IF($AF$2=3,(V6*AG6)-AW6,V6*AG6)),0)","v":0},{"$f":"IF($AF6=3,IF($AF$2=2,(W6/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I6,Refurb_Poss_Tbl[%]))*AG6,W6*$AG6),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,5,0,{"$f":"VLOOKUP(AE7,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.84197316685852419},0,0,0,0,0,0,0,0,4.6230684796042962E-2,{"$f":"IF(OR(AF7=3,AF7=2,AF7=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D7,FlatMaint!$Y$2:$Y$10000,AE7)*AG7,0)","v":74.401907926244306},{"$f":"IF(OR(AF7=3,AF7=2,AF7=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D7,FlatRepair!$Y$2:$Y$10000,AE7)*AG7,0)","v":0},0,74.448138611040349,0,0,0,0,0,74.448138611040349,0,{"$f":"IF($AF7=3,IF($AF$2=2,(R7/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I7,Refurb_Poss_Tbl[%]))*AG7,IF($AF$2=3,(R7*AG7)-AV7,R7*AG7)),0)","v":0},{"$f":"IF(AF7=3,IF($AF$2=2,(S7/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I7,Refurb_Poss_Tbl[%]))*AG7,IF($AF$2=3,(S7*AG7)-AX7,S7*AG7)),0)","v":0},{"$f":"IF($AF7=3,IF($AF$2=2,(T7/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I7,Refurb_Poss_Tbl[%]))*AG7,T7*$AG7),0)","v":0},{"$f":"IF($AF7=3,IF($AF$2=2,(Q7/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I7,Refurb_Poss_Tbl[%]))*AG7,Q7*$AG7),0)","v":0},{"$f":"IF($AF7=3,IF($AF$2=2,(U7/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I7,Refurb_Poss_Tbl[%]))*AG7,U7*$AG7),0)","v":0},{"$f":"IF($AF7=3,IF($AF$2=2,(V7/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I7,Refurb_Poss_Tbl[%]))*AG7,IF($AF$2=3,(V7*AG7)-AW7,V7*AG7)),0)","v":0},{"$f":"IF($AF7=3,IF($AF$2=2,(W7/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I7,Refurb_Poss_Tbl[%]))*AG7,W7*$AG7),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,6,0,{"$f":"VLOOKUP(AE8,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.81350064430775282},0,0,0,0,0,0,0,0,4.4667328305355518E-2,{"$f":"IF(OR(AF8=3,AF8=2,AF8=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D8,FlatMaint!$Y$2:$Y$10000,AE8)*AG8,0)","v":71.885901378013827},{"$f":"IF(OR(AF8=3,AF8=2,AF8=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D8,FlatRepair!$Y$2:$Y$10000,AE8)*AG8,0)","v":0},0,71.930568706319178,0,0,0,0,0,71.930568706319178,0,{"$f":"IF($AF8=3,IF($AF$2=2,(R8/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I8,Refurb_Poss_Tbl[%]))*AG8,IF($AF$2=3,(R8*AG8)-AV8,R8*AG8)),0)","v":0},{"$f":"IF(AF8=3,IF($AF$2=2,(S8/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I8,Refurb_Poss_Tbl[%]))*AG8,IF($AF$2=3,(S8*AG8)-AX8,S8*AG8)),0)","v":0},{"$f":"IF($AF8=3,IF($AF$2=2,(T8/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I8,Refurb_Poss_Tbl[%]))*AG8,T8*$AG8),0)","v":0},{"$f":"IF($AF8=3,IF($AF$2=2,(Q8/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I8,Refurb_Poss_Tbl[%]))*AG8,Q8*$AG8),0)","v":0},{"$f":"IF($AF8=3,IF($AF$2=2,(U8/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I8,Refurb_Poss_Tbl[%]))*AG8,U8*$AG8),0)","v":0},{"$f":"IF($AF8=3,IF($AF$2=2,(V8/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I8,Refurb_Poss_Tbl[%]))*AG8,IF($AF$2=3,(V8*AG8)-AW8,V8*AG8)),0)","v":0},{"$f":"IF($AF8=3,IF($AF$2=2,(W8/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I8,Refurb_Poss_Tbl[%]))*AG8,W8*$AG8),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,7,0,{"$f":"VLOOKUP(AE9,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.78599096068381913},0,0,0,0,0,0,0,0,4.3156838942372482E-2,{"$f":"IF(OR(AF9=3,AF9=2,AF9=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D9,FlatMaint!$Y$2:$Y$10000,AE9)*AG9,0)","v":69.454977176824954},{"$f":"IF(OR(AF9=3,AF9=2,AF9=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D9,FlatRepair!$Y$2:$Y$10000,AE9)*AG9,0)","v":0},0,69.49813401576732,0,0,0,0,0,69.49813401576732,0,{"$f":"IF($AF9=3,IF($AF$2=2,(R9/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I9,Refurb_Poss_Tbl[%]))*AG9,IF($AF$2=3,(R9*AG9)-AV9,R9*AG9)),0)","v":0},{"$f":"IF(AF9=3,IF($AF$2=2,(S9/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I9,Refurb_Poss_Tbl[%]))*AG9,IF($AF$2=3,(S9*AG9)-AX9,S9*AG9)),0)","v":0},{"$f":"IF($AF9=3,IF($AF$2=2,(T9/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I9,Refurb_Poss_Tbl[%]))*AG9,T9*$AG9),0)","v":0},{"$f":"IF($AF9=3,IF($AF$2=2,(Q9/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I9,Refurb_Poss_Tbl[%]))*AG9,Q9*$AG9),0)","v":0},{"$f":"IF($AF9=3,IF($AF$2=2,(U9/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I9,Refurb_Poss_Tbl[%]))*AG9,U9*$AG9),0)","v":0},{"$f":"IF($AF9=3,IF($AF$2=2,(V9/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I9,Refurb_Poss_Tbl[%]))*AG9,IF($AF$2=3,(V9*AG9)-AW9,V9*AG9)),0)","v":0},{"$f":"IF($AF9=3,IF($AF$2=2,(W9/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I9,Refurb_Poss_Tbl[%]))*AG9,W9*$AG9),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,8,0,{"$f":"VLOOKUP(AE10,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.75941155621625056},0,0,0,0,0,0,0,0,4.1697428929828494E-2,{"$f":"IF(OR(AF10=3,AF10=2,AF10=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D10,FlatMaint!$Y$2:$Y$10000,AE10)*AG10,0)","v":67.106258141859868},{"$f":"IF(OR(AF10=3,AF10=2,AF10=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D10,FlatRepair!$Y$2:$Y$10000,AE10)*AG10,0)","v":0},0,67.147955570789691,0,0,0,0,0,67.147955570789691,0,{"$f":"IF($AF10=3,IF($AF$2=2,(R10/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I10,Refurb_Poss_Tbl[%]))*AG10,IF($AF$2=3,(R10*AG10)-AV10,R10*AG10)),0)","v":0},{"$f":"IF(AF10=3,IF($AF$2=2,(S10/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I10,Refurb_Poss_Tbl[%]))*AG10,IF($AF$2=3,(S10*AG10)-AX10,S10*AG10)),0)","v":0},{"$f":"IF($AF10=3,IF($AF$2=2,(T10/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I10,Refurb_Poss_Tbl[%]))*AG10,T10*$AG10),0)","v":0},{"$f":"IF($AF10=3,IF($AF$2=2,(Q10/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I10,Refurb_Poss_Tbl[%]))*AG10,Q10*$AG10),0)","v":0},{"$f":"IF($AF10=3,IF($AF$2=2,(U10/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I10,Refurb_Poss_Tbl[%]))*AG10,U10*$AG10),0)","v":0},{"$f":"IF($AF10=3,IF($AF$2=2,(V10/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I10,Refurb_Poss_Tbl[%]))*AG10,IF($AF$2=3,(V10*AG10)-AW10,V10*AG10)),0)","v":0},{"$f":"IF($AF10=3,IF($AF$2=2,(W10/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I10,Refurb_Poss_Tbl[%]))*AG10,W10*$AG10),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,9,0,{"$f":"VLOOKUP(AE11,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.73373097218961414},0,0,0,0,0,0,0,0,4.0287370946694205E-2,{"$f":"IF(OR(AF11=3,AF11=2,AF11=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D11,FlatMaint!$Y$2:$Y$10000,AE11)*AG11,0)","v":64.836964388270417},{"$f":"IF(OR(AF11=3,AF11=2,AF11=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D11,FlatRepair!$Y$2:$Y$10000,AE11)*AG11,0)","v":0},0,64.877251759217117,0,0,0,0,0,64.877251759217117,0,{"$f":"IF($AF11=3,IF($AF$2=2,(R11/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I11,Refurb_Poss_Tbl[%]))*AG11,IF($AF$2=3,(R11*AG11)-AV11,R11*AG11)),0)","v":0},{"$f":"IF(AF11=3,IF($AF$2=2,(S11/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I11,Refurb_Poss_Tbl[%]))*AG11,IF($AF$2=3,(S11*AG11)-AX11,S11*AG11)),0)","v":0},{"$f":"IF($AF11=3,IF($AF$2=2,(T11/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I11,Refurb_Poss_Tbl[%]))*AG11,T11*$AG11),0)","v":0},{"$f":"IF($AF11=3,IF($AF$2=2,(Q11/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I11,Refurb_Poss_Tbl[%]))*AG11,Q11*$AG11),0)","v":0},{"$f":"IF($AF11=3,IF($AF$2=2,(U11/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I11,Refurb_Poss_Tbl[%]))*AG11,U11*$AG11),0)","v":0},{"$f":"IF($AF11=3,IF($AF$2=2,(V11/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I11,Refurb_Poss_Tbl[%]))*AG11,IF($AF$2=3,(V11*AG11)-AW11,V11*AG11)),0)","v":0},{"$f":"IF($AF11=3,IF($AF$2=2,(W11/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I11,Refurb_Poss_Tbl[%]))*AG11,W11*$AG11),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,10,0,{"$f":"VLOOKUP(AE12,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.70891881370977217},0,0,0,0,0,0,0,0,3.8924996083762521E-2,{"$f":"IF(OR(AF12=3,AF12=2,AF12=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D12,FlatMaint!$Y$2:$Y$10000,AE12)*AG12,0)","v":62.644410036976247},{"$f":"IF(OR(AF12=3,AF12=2,AF12=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D12,FlatRepair!$Y$2:$Y$10000,AE12)*AG12,0)","v":0},0,62.683335033060011,0,0,0,0,0,62.683335033060011,0,{"$f":"IF($AF12=3,IF($AF$2=2,(R12/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I12,Refurb_Poss_Tbl[%]))*AG12,IF($AF$2=3,(R12*AG12)-AV12,R12*AG12)),0)","v":0},{"$f":"IF(AF12=3,IF($AF$2=2,(S12/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I12,Refurb_Poss_Tbl[%]))*AG12,IF($AF$2=3,(S12*AG12)-AX12,S12*AG12)),0)","v":0},{"$f":"IF($AF12=3,IF($AF$2=2,(T12/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I12,Refurb_Poss_Tbl[%]))*AG12,T12*$AG12),0)","v":0},{"$f":"IF($AF12=3,IF($AF$2=2,(Q12/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I12,Refurb_Poss_Tbl[%]))*AG12,Q12*$AG12),0)","v":0},{"$f":"IF($AF12=3,IF($AF$2=2,(U12/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I12,Refurb_Poss_Tbl[%]))*AG12,U12*$AG12),0)","v":0},{"$f":"IF($AF12=3,IF($AF$2=2,(V12/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I12,Refurb_Poss_Tbl[%]))*AG12,IF($AF$2=3,(V12*AG12)-AW12,V12*AG12)),0)","v":0},{"$f":"IF($AF12=3,IF($AF$2=2,(W12/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I12,Refurb_Poss_Tbl[%]))*AG12,W12*$AG12),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,11,0,{"$f":"VLOOKUP(AE13,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.68494571372924851},0,0,0,0,0,0,0,0,3.7608691868369584E-2,{"$f":"IF(OR(AF13=3,AF13=2,AF13=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D13,FlatMaint!$Y$2:$Y$10000,AE13)*AG13,0)","v":60.526000035725851},{"$f":"IF(OR(AF13=3,AF13=2,AF13=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D13,FlatRepair!$Y$2:$Y$10000,AE13)*AG13,0)","v":0},0,60.563608727594222,0,0,0,0,0,60.563608727594222,0,{"$f":"IF($AF13=3,IF($AF$2=2,(R13/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I13,Refurb_Poss_Tbl[%]))*AG13,IF($AF$2=3,(R13*AG13)-AV13,R13*AG13)),0)","v":0},{"$f":"IF(AF13=3,IF($AF$2=2,(S13/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I13,Refurb_Poss_Tbl[%]))*AG13,IF($AF$2=3,(S13*AG13)-AX13,S13*AG13)),0)","v":0},{"$f":"IF($AF13=3,IF($AF$2=2,(T13/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I13,Refurb_Poss_Tbl[%]))*AG13,T13*$AG13),0)","v":0},{"$f":"IF($AF13=3,IF($AF$2=2,(Q13/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I13,Refurb_Poss_Tbl[%]))*AG13,Q13*$AG13),0)","v":0},{"$f":"IF($AF13=3,IF($AF$2=2,(U13/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I13,Refurb_Poss_Tbl[%]))*AG13,U13*$AG13),0)","v":0},{"$f":"IF($AF13=3,IF($AF$2=2,(V13/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I13,Refurb_Poss_Tbl[%]))*AG13,IF($AF$2=3,(V13*AG13)-AW13,V13*AG13)),0)","v":0},{"$f":"IF($AF13=3,IF($AF$2=2,(W13/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I13,Refurb_Poss_Tbl[%]))*AG13,W13*$AG13),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,12,0,{"$f":"VLOOKUP(AE14,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.66178329828912896},0,0,0,0,0,0,0,0,3.6336900355912638E-2,{"$f":"IF(OR(AF14=3,AF14=2,AF14=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D14,FlatMaint!$Y$2:$Y$10000,AE14)*AG14,0)","v":58.479227087657819},{"$f":"IF(OR(AF14=3,AF14=2,AF14=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D14,FlatRepair!$Y$2:$Y$10000,AE14)*AG14,0)","v":0},0,58.515563988013731,0,0,0,0,0,58.515563988013731,0,{"$f":"IF($AF14=3,IF($AF$2=2,(R14/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I14,Refurb_Poss_Tbl[%]))*AG14,IF($AF$2=3,(R14*AG14)-AV14,R14*AG14)),0)","v":0},{"$f":"IF(AF14=3,IF($AF$2=2,(S14/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I14,Refurb_Poss_Tbl[%]))*AG14,IF($AF$2=3,(S14*AG14)-AX14,S14*AG14)),0)","v":0},{"$f":"IF($AF14=3,IF($AF$2=2,(T14/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I14,Refurb_Poss_Tbl[%]))*AG14,T14*$AG14),0)","v":0},{"$f":"IF($AF14=3,IF($AF$2=2,(Q14/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I14,Refurb_Poss_Tbl[%]))*AG14,Q14*$AG14),0)","v":0},{"$f":"IF($AF14=3,IF($AF$2=2,(U14/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I14,Refurb_Poss_Tbl[%]))*AG14,U14*$AG14),0)","v":0},{"$f":"IF($AF14=3,IF($AF$2=2,(V14/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I14,Refurb_Poss_Tbl[%]))*AG14,IF($AF$2=3,(V14*AG14)-AW14,V14*AG14)),0)","v":0},{"$f":"IF($AF14=3,IF($AF$2=2,(W14/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I14,Refurb_Poss_Tbl[%]))*AG14,W14*$AG14),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,13,0,{"$f":"VLOOKUP(AE15,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.63940415293635666},0,0,0,0,0,0,0,0,3.510811628590594E-2,{"$f":"IF(OR(AF15=3,AF15=2,AF15=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D15,FlatMaint!$Y$2:$Y$10000,AE15)*AG15,0)","v":56.501668683727381},{"$f":"IF(OR(AF15=3,AF15=2,AF15=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D15,FlatRepair!$Y$2:$Y$10000,AE15)*AG15,0)","v":0},0,56.536776800013286,0,0,0,0,0,56.536776800013286,0,{"$f":"IF($AF15=3,IF($AF$2=2,(R15/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I15,Refurb_Poss_Tbl[%]))*AG15,IF($AF$2=3,(R15*AG15)-AV15,R15*AG15)),0)","v":0},{"$f":"IF(AF15=3,IF($AF$2=2,(S15/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I15,Refurb_Poss_Tbl[%]))*AG15,IF($AF$2=3,(S15*AG15)-AX15,S15*AG15)),0)","v":0},{"$f":"IF($AF15=3,IF($AF$2=2,(T15/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I15,Refurb_Poss_Tbl[%]))*AG15,T15*$AG15),0)","v":0},{"$f":"IF($AF15=3,IF($AF$2=2,(Q15/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I15,Refurb_Poss_Tbl[%]))*AG15,Q15*$AG15),0)","v":0},{"$f":"IF($AF15=3,IF($AF$2=2,(U15/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I15,Refurb_Poss_Tbl[%]))*AG15,U15*$AG15),0)","v":0},{"$f":"IF($AF15=3,IF($AF$2=2,(V15/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I15,Refurb_Poss_Tbl[%]))*AG15,IF($AF$2=3,(V15*AG15)-AW15,V15*AG15)),0)","v":0},{"$f":"IF($AF15=3,IF($AF$2=2,(W15/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I15,Refurb_Poss_Tbl[%]))*AG15,W15*$AG15),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,14,0,{"$f":"VLOOKUP(AE16,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.61778179027667302},0,0,0,0,0,0,0,0,3.3920885300392209E-2,{"$f":"IF(OR(AF16=3,AF16=2,AF16=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D16,FlatMaint!$Y$2:$Y$10000,AE16)*AG16,0)","v":54.590984235485386},{"$f":"IF(OR(AF16=3,AF16=2,AF16=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D16,FlatRepair!$Y$2:$Y$10000,AE16)*AG16,0)","v":0},0,54.624905120785776,0,0,0,0,0,54.624905120785776,0,{"$f":"IF($AF16=3,IF($AF$2=2,(R16/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I16,Refurb_Poss_Tbl[%]))*AG16,IF($AF$2=3,(R16*AG16)-AV16,R16*AG16)),0)","v":0},{"$f":"IF(AF16=3,IF($AF$2=2,(S16/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I16,Refurb_Poss_Tbl[%]))*AG16,IF($AF$2=3,(S16*AG16)-AX16,S16*AG16)),0)","v":0},{"$f":"IF($AF16=3,IF($AF$2=2,(T16/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I16,Refurb_Poss_Tbl[%]))*AG16,T16*$AG16),0)","v":0},{"$f":"IF($AF16=3,IF($AF$2=2,(Q16/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I16,Refurb_Poss_Tbl[%]))*AG16,Q16*$AG16),0)","v":0},{"$f":"IF($AF16=3,IF($AF$2=2,(U16/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I16,Refurb_Poss_Tbl[%]))*AG16,U16*$AG16),0)","v":0},{"$f":"IF($AF16=3,IF($AF$2=2,(V16/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I16,Refurb_Poss_Tbl[%]))*AG16,IF($AF$2=3,(V16*AG16)-AW16,V16*AG16)),0)","v":0},{"$f":"IF($AF16=3,IF($AF$2=2,(W16/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I16,Refurb_Poss_Tbl[%]))*AG16,W16*$AG16),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,15,0,{"$f":"VLOOKUP(AE17,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.59689061862480497},0,0,0,0,0,0,0,0,3.2773802222601178E-2,{"$f":"IF(OR(AF17=3,AF17=2,AF17=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D17,FlatMaint!$Y$2:$Y$10000,AE17)*AG17,0)","v":52.744912304816808},{"$f":"IF(OR(AF17=3,AF17=2,AF17=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D17,FlatRepair!$Y$2:$Y$10000,AE17)*AG17,0)","v":0},0,52.777686107039408,0,0,0,0,0,52.777686107039408,0,{"$f":"IF($AF17=3,IF($AF$2=2,(R17/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I17,Refurb_Poss_Tbl[%]))*AG17,IF($AF$2=3,(R17*AG17)-AV17,R17*AG17)),0)","v":0},{"$f":"IF(AF17=3,IF($AF$2=2,(S17/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I17,Refurb_Poss_Tbl[%]))*AG17,IF($AF$2=3,(S17*AG17)-AX17,S17*AG17)),0)","v":0},{"$f":"IF($AF17=3,IF($AF$2=2,(T17/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I17,Refurb_Poss_Tbl[%]))*AG17,T17*$AG17),0)","v":0},{"$f":"IF($AF17=3,IF($AF$2=2,(Q17/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I17,Refurb_Poss_Tbl[%]))*AG17,Q17*$AG17),0)","v":0},{"$f":"IF($AF17=3,IF($AF$2=2,(U17/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I17,Refurb_Poss_Tbl[%]))*AG17,U17*$AG17),0)","v":0},{"$f":"IF($AF17=3,IF($AF$2=2,(V17/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I17,Refurb_Poss_Tbl[%]))*AG17,IF($AF$2=3,(V17*AG17)-AW17,V17*AG17)),0)","v":0},{"$f":"IF($AF17=3,IF($AF$2=2,(W17/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I17,Refurb_Poss_Tbl[%]))*AG17,W17*$AG17),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,16,0,{"$f":"VLOOKUP(AE18,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.57670591171478747},0,0,0,0,0,0,0,0,3.1665509393817563E-2,{"$f":"IF(OR(AF18=3,AF18=2,AF18=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D18,FlatMaint!$Y$2:$Y$10000,AE18)*AG18,0)","v":50.961267927359238},{"$f":"IF(OR(AF18=3,AF18=2,AF18=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D18,FlatRepair!$Y$2:$Y$10000,AE18)*AG18,0)","v":0},0,50.992933436753056,0,0,0,0,0,50.992933436753056,0,{"$f":"IF($AF18=3,IF($AF$2=2,(R18/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I18,Refurb_Poss_Tbl[%]))*AG18,IF($AF$2=3,(R18*AG18)-AV18,R18*AG18)),0)","v":0},{"$f":"IF(AF18=3,IF($AF$2=2,(S18/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I18,Refurb_Poss_Tbl[%]))*AG18,IF($AF$2=3,(S18*AG18)-AX18,S18*AG18)),0)","v":0},{"$f":"IF($AF18=3,IF($AF$2=2,(T18/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I18,Refurb_Poss_Tbl[%]))*AG18,T18*$AG18),0)","v":0},{"$f":"IF($AF18=3,IF($AF$2=2,(Q18/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I18,Refurb_Poss_Tbl[%]))*AG18,Q18*$AG18),0)","v":0},{"$f":"IF($AF18=3,IF($AF$2=2,(U18/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I18,Refurb_Poss_Tbl[%]))*AG18,U18*$AG18),0)","v":0},{"$f":"IF($AF18=3,IF($AF$2=2,(V18/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I18,Refurb_Poss_Tbl[%]))*AG18,IF($AF$2=3,(V18*AG18)-AW18,V18*AG18)),0)","v":0},{"$f":"IF($AF18=3,IF($AF$2=2,(W18/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I18,Refurb_Poss_Tbl[%]))*AG18,W18*$AG18),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,17,0,{"$f":"VLOOKUP(AE19,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.55720377943457733},0,0,0,0,0,0,0,0,3.0594695066490405E-2,{"$f":"IF(OR(AF19=3,AF19=2,AF19=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D19,FlatMaint!$Y$2:$Y$10000,AE19)*AG19,0)","v":49.237940026434053},{"$f":"IF(OR(AF19=3,AF19=2,AF19=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D19,FlatRepair!$Y$2:$Y$10000,AE19)*AG19,0)","v":0},0,49.268534721500544,0,0,0,0,0,49.268534721500544,0,{"$f":"IF($AF19=3,IF($AF$2=2,(R19/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I19,Refurb_Poss_Tbl[%]))*AG19,IF($AF$2=3,(R19*AG19)-AV19,R19*AG19)),0)","v":0},{"$f":"IF(AF19=3,IF($AF$2=2,(S19/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I19,Refurb_Poss_Tbl[%]))*AG19,IF($AF$2=3,(S19*AG19)-AX19,S19*AG19)),0)","v":0},{"$f":"IF($AF19=3,IF($AF$2=2,(T19/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I19,Refurb_Poss_Tbl[%]))*AG19,T19*$AG19),0)","v":0},{"$f":"IF($AF19=3,IF($AF$2=2,(Q19/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I19,Refurb_Poss_Tbl[%]))*AG19,Q19*$AG19),0)","v":0},{"$f":"IF($AF19=3,IF($AF$2=2,(U19/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I19,Refurb_Poss_Tbl[%]))*AG19,U19*$AG19),0)","v":0},{"$f":"IF($AF19=3,IF($AF$2=2,(V19/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I19,Refurb_Poss_Tbl[%]))*AG19,IF($AF$2=3,(V19*AG19)-AW19,V19*AG19)),0)","v":0},{"$f":"IF($AF19=3,IF($AF$2=2,(W19/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I19,Refurb_Poss_Tbl[%]))*AG19,W19*$AG19),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,18,0,{"$f":"VLOOKUP(AE20,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.53836113955031628},0,0,0,0,0,0,0,0,2.9560091851681552E-2,{"$f":"IF(OR(AF20=3,AF20=2,AF20=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D20,FlatMaint!$Y$2:$Y$10000,AE20)*AG20,0)","v":47.572888914429036},{"$f":"IF(OR(AF20=3,AF20=2,AF20=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D20,FlatRepair!$Y$2:$Y$10000,AE20)*AG20,0)","v":0},0,47.602449006280715,0,0,0,0,0,47.602449006280715,0,{"$f":"IF($AF20=3,IF($AF$2=2,(R20/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I20,Refurb_Poss_Tbl[%]))*AG20,IF($AF$2=3,(R20*AG20)-AV20,R20*AG20)),0)","v":0},{"$f":"IF(AF20=3,IF($AF$2=2,(S20/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I20,Refurb_Poss_Tbl[%]))*AG20,IF($AF$2=3,(S20*AG20)-AX20,S20*AG20)),0)","v":0},{"$f":"IF($AF20=3,IF($AF$2=2,(T20/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I20,Refurb_Poss_Tbl[%]))*AG20,T20*$AG20),0)","v":0},{"$f":"IF($AF20=3,IF($AF$2=2,(Q20/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I20,Refurb_Poss_Tbl[%]))*AG20,Q20*$AG20),0)","v":0},{"$f":"IF($AF20=3,IF($AF$2=2,(U20/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I20,Refurb_Poss_Tbl[%]))*AG20,U20*$AG20),0)","v":0},{"$f":"IF($AF20=3,IF($AF$2=2,(V20/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I20,Refurb_Poss_Tbl[%]))*AG20,IF($AF$2=3,(V20*AG20)-AW20,V20*AG20)),0)","v":0},{"$f":"IF($AF20=3,IF($AF$2=2,(W20/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I20,Refurb_Poss_Tbl[%]))*AG20,W20*$AG20),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,19,0,{"$f":"VLOOKUP(AE21,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.52015569038677911},0,0,0,0,0,0,0,0,2.8560475219015998E-2,{"$f":"IF(OR(AF21=3,AF21=2,AF21=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D21,FlatMaint!$Y$2:$Y$10000,AE21)*AG21,0)","v":45.964143878675408},{"$f":"IF(OR(AF21=3,AF21=2,AF21=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D21,FlatRepair!$Y$2:$Y$10000,AE21)*AG21,0)","v":0},0,45.992704353894425,0,0,0,0,0,45.992704353894425,0,{"$f":"IF($AF21=3,IF($AF$2=2,(R21/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I21,Refurb_Poss_Tbl[%]))*AG21,IF($AF$2=3,(R21*AG21)-AV21,R21*AG21)),0)","v":0},{"$f":"IF(AF21=3,IF($AF$2=2,(S21/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I21,Refurb_Poss_Tbl[%]))*AG21,IF($AF$2=3,(S21*AG21)-AX21,S21*AG21)),0)","v":0},{"$f":"IF($AF21=3,IF($AF$2=2,(T21/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I21,Refurb_Poss_Tbl[%]))*AG21,T21*$AG21),0)","v":0},{"$f":"IF($AF21=3,IF($AF$2=2,(Q21/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I21,Refurb_Poss_Tbl[%]))*AG21,Q21*$AG21),0)","v":0},{"$f":"IF($AF21=3,IF($AF$2=2,(U21/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I21,Refurb_Poss_Tbl[%]))*AG21,U21*$AG21),0)","v":0},{"$f":"IF($AF21=3,IF($AF$2=2,(V21/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I21,Refurb_Poss_Tbl[%]))*AG21,IF($AF$2=3,(V21*AG21)-AW21,V21*AG21)),0)","v":0},{"$f":"IF($AF21=3,IF($AF$2=2,(W21/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I21,Refurb_Poss_Tbl[%]))*AG21,W21*$AG21),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,20,2,{"$f":"VLOOKUP(AE22,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.50256588443167061},0,0,0,0,0,0,0,0,2.7594662047358449E-2,{"$f":"IF(OR(AF22=3,AF22=2,AF22=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D22,FlatMaint!$Y$2:$Y$10000,AE22)*AG22,0)","v":44.409800848961744},{"$f":"IF(OR(AF22=3,AF22=2,AF22=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D22,FlatRepair!$Y$2:$Y$10000,AE22)*AG22,0)","v":0},0,44.4373955110091,112.48018495945662,0,0,0,0,156.91758047046574,0,{"$f":"IF($AF22=3,IF($AF$2=2,(R22/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I22,Refurb_Poss_Tbl[%]))*AG22,IF($AF$2=3,(R22*AG22)-AV22,R22*AG22)),0)","v":0},{"$f":"IF(AF22=3,IF($AF$2=2,(S22/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I22,Refurb_Poss_Tbl[%]))*AG22,IF($AF$2=3,(S22*AG22)-AX22,S22*AG22)),0)","v":0},{"$f":"IF($AF22=3,IF($AF$2=2,(T22/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I22,Refurb_Poss_Tbl[%]))*AG22,T22*$AG22),0)","v":0},{"$f":"IF($AF22=3,IF($AF$2=2,(Q22/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I22,Refurb_Poss_Tbl[%]))*AG22,Q22*$AG22),0)","v":0},{"$f":"IF($AF22=3,IF($AF$2=2,(U22/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I22,Refurb_Poss_Tbl[%]))*AG22,U22*$AG22),0)","v":0},{"$f":"IF($AF22=3,IF($AF$2=2,(V22/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I22,Refurb_Poss_Tbl[%]))*AG22,IF($AF$2=3,(V22*AG22)-AW22,V22*AG22)),0)","v":0},{"$f":"IF($AF22=3,IF($AF$2=2,(W22/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I22,Refurb_Poss_Tbl[%]))*AG22,W22*$AG22),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,21,0,{"$f":"VLOOKUP(AE23,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.48557090283253213},0,0,0,0,0,0,0,0,2.6661509224500925E-2,{"$f":"IF(OR(AF23=3,AF23=2,AF23=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D23,FlatMaint!$Y$2:$Y$10000,AE23)*AG23,0)","v":42.908020143924404},{"$f":"IF(OR(AF23=3,AF23=2,AF23=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D23,FlatRepair!$Y$2:$Y$10000,AE23)*AG23,0)","v":0},0,42.934681653148907,0,0,0,0,0,42.934681653148907,0,{"$f":"IF($AF23=3,IF($AF$2=2,(R23/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I23,Refurb_Poss_Tbl[%]))*AG23,IF($AF$2=3,(R23*AG23)-AV23,R23*AG23)),0)","v":0},{"$f":"IF(AF23=3,IF($AF$2=2,(S23/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I23,Refurb_Poss_Tbl[%]))*AG23,IF($AF$2=3,(S23*AG23)-AX23,S23*AG23)),0)","v":0},{"$f":"IF($AF23=3,IF($AF$2=2,(T23/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I23,Refurb_Poss_Tbl[%]))*AG23,T23*$AG23),0)","v":0},{"$f":"IF($AF23=3,IF($AF$2=2,(Q23/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I23,Refurb_Poss_Tbl[%]))*AG23,Q23*$AG23),0)","v":0},{"$f":"IF($AF23=3,IF($AF$2=2,(U23/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I23,Refurb_Poss_Tbl[%]))*AG23,U23*$AG23),0)","v":0},{"$f":"IF($AF23=3,IF($AF$2=2,(V23/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I23,Refurb_Poss_Tbl[%]))*AG23,IF($AF$2=3,(V23*AG23)-AW23,V23*AG23)),0)","v":0},{"$f":"IF($AF23=3,IF($AF$2=2,(W23/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I23,Refurb_Poss_Tbl[%]))*AG23,W23*$AG23),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,22,0,{"$f":"VLOOKUP(AE24,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.46915063075606966},0,0,0,0,0,0,0,0,2.5759912294203789E-2,{"$f":"IF(OR(AF24=3,AF24=2,AF24=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D24,FlatMaint!$Y$2:$Y$10000,AE24)*AG24,0)","v":41.457024293646761},{"$f":"IF(OR(AF24=3,AF24=2,AF24=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D24,FlatRepair!$Y$2:$Y$10000,AE24)*AG24,0)","v":0},0,41.482784205940966,0,0,0,0,0,41.482784205940966,0,{"$f":"IF($AF24=3,IF($AF$2=2,(R24/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I24,Refurb_Poss_Tbl[%]))*AG24,IF($AF$2=3,(R24*AG24)-AV24,R24*AG24)),0)","v":0},{"$f":"IF(AF24=3,IF($AF$2=2,(S24/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I24,Refurb_Poss_Tbl[%]))*AG24,IF($AF$2=3,(S24*AG24)-AX24,S24*AG24)),0)","v":0},{"$f":"IF($AF24=3,IF($AF$2=2,(T24/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I24,Refurb_Poss_Tbl[%]))*AG24,T24*$AG24),0)","v":0},{"$f":"IF($AF24=3,IF($AF$2=2,(Q24/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I24,Refurb_Poss_Tbl[%]))*AG24,Q24*$AG24),0)","v":0},{"$f":"IF($AF24=3,IF($AF$2=2,(U24/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I24,Refurb_Poss_Tbl[%]))*AG24,U24*$AG24),0)","v":0},{"$f":"IF($AF24=3,IF($AF$2=2,(V24/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I24,Refurb_Poss_Tbl[%]))*AG24,IF($AF$2=3,(V24*AG24)-AW24,V24*AG24)),0)","v":0},{"$f":"IF($AF24=3,IF($AF$2=2,(W24/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I24,Refurb_Poss_Tbl[%]))*AG24,W24*$AG24),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,23,0,{"$f":"VLOOKUP(AE25,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.45328563358074364},0,0,0,0,0,0,0,0,2.4888804148989169E-2,{"$f":"IF(OR(AF25=3,AF25=2,AF25=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D25,FlatMaint!$Y$2:$Y$10000,AE25)*AG25,0)","v":40.055095935890591},{"$f":"IF(OR(AF25=3,AF25=2,AF25=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D25,FlatRepair!$Y$2:$Y$10000,AE25)*AG25,0)","v":0},0,40.079984740039578,0,0,0,0,0,40.079984740039578,0,{"$f":"IF($AF25=3,IF($AF$2=2,(R25/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I25,Refurb_Poss_Tbl[%]))*AG25,IF($AF$2=3,(R25*AG25)-AV25,R25*AG25)),0)","v":0},{"$f":"IF(AF25=3,IF($AF$2=2,(S25/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I25,Refurb_Poss_Tbl[%]))*AG25,IF($AF$2=3,(S25*AG25)-AX25,S25*AG25)),0)","v":0},{"$f":"IF($AF25=3,IF($AF$2=2,(T25/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I25,Refurb_Poss_Tbl[%]))*AG25,T25*$AG25),0)","v":0},{"$f":"IF($AF25=3,IF($AF$2=2,(Q25/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I25,Refurb_Poss_Tbl[%]))*AG25,Q25*$AG25),0)","v":0},{"$f":"IF($AF25=3,IF($AF$2=2,(U25/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I25,Refurb_Poss_Tbl[%]))*AG25,U25*$AG25),0)","v":0},{"$f":"IF($AF25=3,IF($AF$2=2,(V25/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I25,Refurb_Poss_Tbl[%]))*AG25,IF($AF$2=3,(V25*AG25)-AW25,V25*AG25)),0)","v":0},{"$f":"IF($AF25=3,IF($AF$2=2,(W25/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I25,Refurb_Poss_Tbl[%]))*AG25,W25*$AG25),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,24,0,{"$f":"VLOOKUP(AE26,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.43795713389443841},0,0,0,0,0,0,0,0,2.4047153767139302E-2,{"$f":"IF(OR(AF26=3,AF26=2,AF26=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D26,FlatMaint!$Y$2:$Y$10000,AE26)*AG26,0)","v":38.700575783469183},{"$f":"IF(OR(AF26=3,AF26=2,AF26=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D26,FlatRepair!$Y$2:$Y$10000,AE26)*AG26,0)","v":0},0,38.724622937236326,0,0,0,0,0,38.724622937236326,0,{"$f":"IF($AF26=3,IF($AF$2=2,(R26/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I26,Refurb_Poss_Tbl[%]))*AG26,IF($AF$2=3,(R26*AG26)-AV26,R26*AG26)),0)","v":0},{"$f":"IF(AF26=3,IF($AF$2=2,(S26/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I26,Refurb_Poss_Tbl[%]))*AG26,IF($AF$2=3,(S26*AG26)-AX26,S26*AG26)),0)","v":0},{"$f":"IF($AF26=3,IF($AF$2=2,(T26/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I26,Refurb_Poss_Tbl[%]))*AG26,T26*$AG26),0)","v":0},{"$f":"IF($AF26=3,IF($AF$2=2,(Q26/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I26,Refurb_Poss_Tbl[%]))*AG26,Q26*$AG26),0)","v":0},{"$f":"IF($AF26=3,IF($AF$2=2,(U26/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I26,Refurb_Poss_Tbl[%]))*AG26,U26*$AG26),0)","v":0},{"$f":"IF($AF26=3,IF($AF$2=2,(V26/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I26,Refurb_Poss_Tbl[%]))*AG26,IF($AF$2=3,(V26*AG26)-AW26,V26*AG26)),0)","v":0},{"$f":"IF($AF26=3,IF($AF$2=2,(W26/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I26,Refurb_Poss_Tbl[%]))*AG26,W26*$AG26),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,25,0,{"$f":"VLOOKUP(AE27,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.42314698926998884},0,0,0,0,0,0,0,0,2.3233964992405123E-2,{"$f":"IF(OR(AF27=3,AF27=2,AF27=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D27,FlatMaint!$Y$2:$Y$10000,AE27)*AG27,0)","v":37.391860660356699},{"$f":"IF(OR(AF27=3,AF27=2,AF27=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D27,FlatRepair!$Y$2:$Y$10000,AE27)*AG27,0)","v":0},0,37.415094625349106,0,0,0,0,0,37.415094625349106,0,{"$f":"IF($AF27=3,IF($AF$2=2,(R27/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I27,Refurb_Poss_Tbl[%]))*AG27,IF($AF$2=3,(R27*AG27)-AV27,R27*AG27)),0)","v":0},{"$f":"IF(AF27=3,IF($AF$2=2,(S27/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I27,Refurb_Poss_Tbl[%]))*AG27,IF($AF$2=3,(S27*AG27)-AX27,S27*AG27)),0)","v":0},{"$f":"IF($AF27=3,IF($AF$2=2,(T27/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I27,Refurb_Poss_Tbl[%]))*AG27,T27*$AG27),0)","v":0},{"$f":"IF($AF27=3,IF($AF$2=2,(Q27/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I27,Refurb_Poss_Tbl[%]))*AG27,Q27*$AG27),0)","v":0},{"$f":"IF($AF27=3,IF($AF$2=2,(U27/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I27,Refurb_Poss_Tbl[%]))*AG27,U27*$AG27),0)","v":0},{"$f":"IF($AF27=3,IF($AF$2=2,(V27/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I27,Refurb_Poss_Tbl[%]))*AG27,IF($AF$2=3,(V27*AG27)-AW27,V27*AG27)),0)","v":0},{"$f":"IF($AF27=3,IF($AF$2=2,(W27/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I27,Refurb_Poss_Tbl[%]))*AG27,W27*$AG27),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,26,0,{"$f":"VLOOKUP(AE28,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.40883767079225974},0,0,0,0,0,0,0,0,2.2448275354980795E-2,{"$f":"IF(OR(AF28=3,AF28=2,AF28=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D28,FlatMaint!$Y$2:$Y$10000,AE28)*AG28,0)","v":36.127401604209375},{"$f":"IF(OR(AF28=3,AF28=2,AF28=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D28,FlatRepair!$Y$2:$Y$10000,AE28)*AG28,0)","v":0},0,36.149849879564357,0,0,0,0,0,36.149849879564357,0,{"$f":"IF($AF28=3,IF($AF$2=2,(R28/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I28,Refurb_Poss_Tbl[%]))*AG28,IF($AF$2=3,(R28*AG28)-AV28,R28*AG28)),0)","v":0},{"$f":"IF(AF28=3,IF($AF$2=2,(S28/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I28,Refurb_Poss_Tbl[%]))*AG28,IF($AF$2=3,(S28*AG28)-AX28,S28*AG28)),0)","v":0},{"$f":"IF($AF28=3,IF($AF$2=2,(T28/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I28,Refurb_Poss_Tbl[%]))*AG28,T28*$AG28),0)","v":0},{"$f":"IF($AF28=3,IF($AF$2=2,(Q28/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I28,Refurb_Poss_Tbl[%]))*AG28,Q28*$AG28),0)","v":0},{"$f":"IF($AF28=3,IF($AF$2=2,(U28/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I28,Refurb_Poss_Tbl[%]))*AG28,U28*$AG28),0)","v":0},{"$f":"IF($AF28=3,IF($AF$2=2,(V28/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I28,Refurb_Poss_Tbl[%]))*AG28,IF($AF$2=3,(V28*AG28)-AW28,V28*AG28)),0)","v":0},{"$f":"IF($AF28=3,IF($AF$2=2,(W28/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I28,Refurb_Poss_Tbl[%]))*AG28,W28*$AG28),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,27,0,{"$f":"VLOOKUP(AE29,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39501224231136206},0,0,0,0,0,0,0,0,2.1689154932348593E-2,{"$f":"IF(OR(AF29=3,AF29=2,AF29=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D29,FlatMaint!$Y$2:$Y$10000,AE29)*AG29,0)","v":34.905702033052535},{"$f":"IF(OR(AF29=3,AF29=2,AF29=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D29,FlatRepair!$Y$2:$Y$10000,AE29)*AG29,0)","v":0},0,34.927391187984881,0,0,0,0,0,34.927391187984881,0,{"$f":"IF($AF29=3,IF($AF$2=2,(R29/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I29,Refurb_Poss_Tbl[%]))*AG29,IF($AF$2=3,(R29*AG29)-AV29,R29*AG29)),0)","v":0},{"$f":"IF(AF29=3,IF($AF$2=2,(S29/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I29,Refurb_Poss_Tbl[%]))*AG29,IF($AF$2=3,(S29*AG29)-AX29,S29*AG29)),0)","v":0},{"$f":"IF($AF29=3,IF($AF$2=2,(T29/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I29,Refurb_Poss_Tbl[%]))*AG29,T29*$AG29),0)","v":0},{"$f":"IF($AF29=3,IF($AF$2=2,(Q29/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I29,Refurb_Poss_Tbl[%]))*AG29,Q29*$AG29),0)","v":0},{"$f":"IF($AF29=3,IF($AF$2=2,(U29/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I29,Refurb_Poss_Tbl[%]))*AG29,U29*$AG29),0)","v":0},{"$f":"IF($AF29=3,IF($AF$2=2,(V29/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I29,Refurb_Poss_Tbl[%]))*AG29,IF($AF$2=3,(V29*AG29)-AW29,V29*AG29)),0)","v":0},{"$f":"IF($AF29=3,IF($AF$2=2,(W29/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I29,Refurb_Poss_Tbl[%]))*AG29,W29*$AG29),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,28,0,{"$f":"VLOOKUP(AE30,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38165434039745127},0,0,0,0,0,0,0,0,2.0955705248645984E-2,{"$f":"IF(OR(AF30=3,AF30=2,AF30=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D30,FlatMaint!$Y$2:$Y$10000,AE30)*AG30,0)","v":33.725315973963802},{"$f":"IF(OR(AF30=3,AF30=2,AF30=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D30,FlatRepair!$Y$2:$Y$10000,AE30)*AG30,0)","v":0},0,33.746271679212448,0,0,0,0,0,33.746271679212448,0,{"$f":"IF($AF30=3,IF($AF$2=2,(R30/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I30,Refurb_Poss_Tbl[%]))*AG30,IF($AF$2=3,(R30*AG30)-AV30,R30*AG30)),0)","v":0},{"$f":"IF(AF30=3,IF($AF$2=2,(S30/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I30,Refurb_Poss_Tbl[%]))*AG30,IF($AF$2=3,(S30*AG30)-AX30,S30*AG30)),0)","v":0},{"$f":"IF($AF30=3,IF($AF$2=2,(T30/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I30,Refurb_Poss_Tbl[%]))*AG30,T30*$AG30),0)","v":0},{"$f":"IF($AF30=3,IF($AF$2=2,(Q30/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I30,Refurb_Poss_Tbl[%]))*AG30,Q30*$AG30),0)","v":0},{"$f":"IF($AF30=3,IF($AF$2=2,(U30/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I30,Refurb_Poss_Tbl[%]))*AG30,U30*$AG30),0)","v":0},{"$f":"IF($AF30=3,IF($AF$2=2,(V30/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I30,Refurb_Poss_Tbl[%]))*AG30,IF($AF$2=3,(V30*AG30)-AW30,V30*AG30)),0)","v":0},{"$f":"IF($AF30=3,IF($AF$2=2,(W30/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I30,Refurb_Poss_Tbl[%]))*AG30,W30*$AG30),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,29,0,{"$f":"VLOOKUP(AE31,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36874815497338298},0,0,0,0,0,0,0,0,2.0247058211252167E-2,{"$f":"IF(OR(AF31=3,AF31=2,AF31=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D31,FlatMaint!$Y$2:$Y$10000,AE31)*AG31,0)","v":32.584846351655855},{"$f":"IF(OR(AF31=3,AF31=2,AF31=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D31,FlatRepair!$Y$2:$Y$10000,AE31)*AG31,0)","v":0},0,32.605093409867109,0,0,0,0,0,32.605093409867109,0,{"$f":"IF($AF31=3,IF($AF$2=2,(R31/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I31,Refurb_Poss_Tbl[%]))*AG31,IF($AF$2=3,(R31*AG31)-AV31,R31*AG31)),0)","v":0},{"$f":"IF(AF31=3,IF($AF$2=2,(S31/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I31,Refurb_Poss_Tbl[%]))*AG31,IF($AF$2=3,(S31*AG31)-AX31,S31*AG31)),0)","v":0},{"$f":"IF($AF31=3,IF($AF$2=2,(T31/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I31,Refurb_Poss_Tbl[%]))*AG31,T31*$AG31),0)","v":0},{"$f":"IF($AF31=3,IF($AF$2=2,(Q31/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I31,Refurb_Poss_Tbl[%]))*AG31,Q31*$AG31),0)","v":0},{"$f":"IF($AF31=3,IF($AF$2=2,(U31/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I31,Refurb_Poss_Tbl[%]))*AG31,U31*$AG31),0)","v":0},{"$f":"IF($AF31=3,IF($AF$2=2,(V31/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I31,Refurb_Poss_Tbl[%]))*AG31,IF($AF$2=3,(V31*AG31)-AW31,V31*AG31)),0)","v":0},{"$f":"IF($AF31=3,IF($AF$2=2,(W31/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I31,Refurb_Poss_Tbl[%]))*AG31,W31*$AG31),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,30,3,{"$f":"VLOOKUP(AE32,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35627841060230236},0,0,0,0,0,0,0,0,1.9562375083335422E-2,{"$f":"IF(OR(AF32=3,AF32=2,AF32=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D32,FlatMaint!$Y$2:$Y$10000,AE32)*AG32,0)","v":31.482943334933189},{"$f":"IF(OR(AF32=3,AF32=2,AF32=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D32,FlatRepair!$Y$2:$Y$10000,AE32)*AG32,0)","v":0},0,31.502505710016525,0,0.81664650218935075,2.3059986892176604E-2,0.87332693246508597,318.95727714925499,352.17281628081815,0,{"$f":"IF($AF32=3,IF($AF$2=2,(R32/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I32,Refurb_Poss_Tbl[%]))*AG32,IF($AF$2=3,(R32*AG32)-AV32,R32*AG32)),0)","v":0.382705844359091},{"$f":"IF(AF32=3,IF($AF$2=2,(S32/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I32,Refurb_Poss_Tbl[%]))*AG32,IF($AF$2=3,(S32*AG32)-AX32,S32*AG32)),0)","v":1.7466538649301759},{"$f":"IF($AF32=3,IF($AF$2=2,(T32/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I32,Refurb_Poss_Tbl[%]))*AG32,T32*$AG32),0)","v":4.6119973784353292E-2},{"$f":"IF($AF32=3,IF($AF$2=2,(Q32/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I32,Refurb_Poss_Tbl[%]))*AG32,Q32*$AG32),0)","v":314.77496850578319},{"$f":"IF($AF32=3,IF($AF$2=2,(U32/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I32,Refurb_Poss_Tbl[%]))*AG32,U32*$AG32),0)","v":1.9638475655461132},{"$f":"IF($AF32=3,IF($AF$2=2,(V32/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I32,Refurb_Poss_Tbl[%]))*AG32,IF($AF$2=3,(V32*AG32)-AW32,V32*AG32)),0)","v":0},{"$f":"IF($AF32=3,IF($AF$2=2,(W32/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I32,Refurb_Poss_Tbl[%]))*AG32,W32*$AG32),0)","v":4.2981394852071073E-2}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,31,0,{"$f":"VLOOKUP(AE33,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39998714516107459},0,0,0,0,0,0,0,0,2.1962314665448072E-2,{"$f":"IF(OR(AF33=3,AF33=2,AF33=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D33,FlatMaint!$Y$2:$Y$10000,AE33)*AG33,0)","v":35.345314930868923},{"$f":"IF(OR(AF33=3,AF33=2,AF33=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D33,FlatRepair!$Y$2:$Y$10000,AE33)*AG33,0)","v":0},0,35.367277245534375,0,0,0,0,0,35.367277245534375,0,{"$f":"IF($AF33=3,IF($AF$2=2,(R33/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I33,Refurb_Poss_Tbl[%]))*AG33,IF($AF$2=3,(R33*AG33)-AV33,R33*AG33)),0)","v":0},{"$f":"IF(AF33=3,IF($AF$2=2,(S33/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I33,Refurb_Poss_Tbl[%]))*AG33,IF($AF$2=3,(S33*AG33)-AX33,S33*AG33)),0)","v":0},{"$f":"IF($AF33=3,IF($AF$2=2,(T33/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I33,Refurb_Poss_Tbl[%]))*AG33,T33*$AG33),0)","v":0},{"$f":"IF($AF33=3,IF($AF$2=2,(Q33/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I33,Refurb_Poss_Tbl[%]))*AG33,Q33*$AG33),0)","v":0},{"$f":"IF($AF33=3,IF($AF$2=2,(U33/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I33,Refurb_Poss_Tbl[%]))*AG33,U33*$AG33),0)","v":0},{"$f":"IF($AF33=3,IF($AF$2=2,(V33/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I33,Refurb_Poss_Tbl[%]))*AG33,IF($AF$2=3,(V33*AG33)-AW33,V33*AG33)),0)","v":0},{"$f":"IF($AF33=3,IF($AF$2=2,(W33/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I33,Refurb_Poss_Tbl[%]))*AG33,W33*$AG33),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,32,0,{"$f":"VLOOKUP(AE34,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38833703413696569},0,0,0,0,0,0,0,0,2.1322635597522403E-2,{"$f":"IF(OR(AF34=3,AF34=2,AF34=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D34,FlatMaint!$Y$2:$Y$10000,AE34)*AG34,0)","v":34.315839738707702},{"$f":"IF(OR(AF34=3,AF34=2,AF34=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D34,FlatRepair!$Y$2:$Y$10000,AE34)*AG34,0)","v":0},0,34.337162374305223,0,0,0,0,0,34.337162374305223,0,{"$f":"IF($AF34=3,IF($AF$2=2,(R34/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I34,Refurb_Poss_Tbl[%]))*AG34,IF($AF$2=3,(R34*AG34)-AV34,R34*AG34)),0)","v":0},{"$f":"IF(AF34=3,IF($AF$2=2,(S34/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I34,Refurb_Poss_Tbl[%]))*AG34,IF($AF$2=3,(S34*AG34)-AX34,S34*AG34)),0)","v":0},{"$f":"IF($AF34=3,IF($AF$2=2,(T34/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I34,Refurb_Poss_Tbl[%]))*AG34,T34*$AG34),0)","v":0},{"$f":"IF($AF34=3,IF($AF$2=2,(Q34/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I34,Refurb_Poss_Tbl[%]))*AG34,Q34*$AG34),0)","v":0},{"$f":"IF($AF34=3,IF($AF$2=2,(U34/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I34,Refurb_Poss_Tbl[%]))*AG34,U34*$AG34),0)","v":0},{"$f":"IF($AF34=3,IF($AF$2=2,(V34/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I34,Refurb_Poss_Tbl[%]))*AG34,IF($AF$2=3,(V34*AG34)-AW34,V34*AG34)),0)","v":0},{"$f":"IF($AF34=3,IF($AF$2=2,(W34/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I34,Refurb_Poss_Tbl[%]))*AG34,W34*$AG34),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,33,0,{"$f":"VLOOKUP(AE35,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.37702624673491814},0,0,0,0,0,0,0,0,2.0701587958759614E-2,{"$f":"IF(OR(AF35=3,AF35=2,AF35=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D35,FlatMaint!$Y$2:$Y$10000,AE35)*AG35,0)","v":33.31634926088126},{"$f":"IF(OR(AF35=3,AF35=2,AF35=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D35,FlatRepair!$Y$2:$Y$10000,AE35)*AG35,0)","v":0},0,33.337050848840022,0,0,0,0,0,33.337050848840022,0,{"$f":"IF($AF35=3,IF($AF$2=2,(R35/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I35,Refurb_Poss_Tbl[%]))*AG35,IF($AF$2=3,(R35*AG35)-AV35,R35*AG35)),0)","v":0},{"$f":"IF(AF35=3,IF($AF$2=2,(S35/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I35,Refurb_Poss_Tbl[%]))*AG35,IF($AF$2=3,(S35*AG35)-AX35,S35*AG35)),0)","v":0},{"$f":"IF($AF35=3,IF($AF$2=2,(T35/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I35,Refurb_Poss_Tbl[%]))*AG35,T35*$AG35),0)","v":0},{"$f":"IF($AF35=3,IF($AF$2=2,(Q35/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I35,Refurb_Poss_Tbl[%]))*AG35,Q35*$AG35),0)","v":0},{"$f":"IF($AF35=3,IF($AF$2=2,(U35/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I35,Refurb_Poss_Tbl[%]))*AG35,U35*$AG35),0)","v":0},{"$f":"IF($AF35=3,IF($AF$2=2,(V35/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I35,Refurb_Poss_Tbl[%]))*AG35,IF($AF$2=3,(V35*AG35)-AW35,V35*AG35)),0)","v":0},{"$f":"IF($AF35=3,IF($AF$2=2,(W35/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I35,Refurb_Poss_Tbl[%]))*AG35,W35*$AG35),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,34,0,{"$f":"VLOOKUP(AE36,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36604489974263904},0,0,0,0,0,0,0,0,2.0098629086174387E-2,{"$f":"IF(OR(AF36=3,AF36=2,AF36=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D36,FlatMaint!$Y$2:$Y$10000,AE36)*AG36,0)","v":32.345970156195406},{"$f":"IF(OR(AF36=3,AF36=2,AF36=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D36,FlatRepair!$Y$2:$Y$10000,AE36)*AG36,0)","v":0},0,32.366068785281584,0,0,0,0,0,32.366068785281584,0,{"$f":"IF($AF36=3,IF($AF$2=2,(R36/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I36,Refurb_Poss_Tbl[%]))*AG36,IF($AF$2=3,(R36*AG36)-AV36,R36*AG36)),0)","v":0},{"$f":"IF(AF36=3,IF($AF$2=2,(S36/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I36,Refurb_Poss_Tbl[%]))*AG36,IF($AF$2=3,(S36*AG36)-AX36,S36*AG36)),0)","v":0},{"$f":"IF($AF36=3,IF($AF$2=2,(T36/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I36,Refurb_Poss_Tbl[%]))*AG36,T36*$AG36),0)","v":0},{"$f":"IF($AF36=3,IF($AF$2=2,(Q36/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I36,Refurb_Poss_Tbl[%]))*AG36,Q36*$AG36),0)","v":0},{"$f":"IF($AF36=3,IF($AF$2=2,(U36/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I36,Refurb_Poss_Tbl[%]))*AG36,U36*$AG36),0)","v":0},{"$f":"IF($AF36=3,IF($AF$2=2,(V36/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I36,Refurb_Poss_Tbl[%]))*AG36,IF($AF$2=3,(V36*AG36)-AW36,V36*AG36)),0)","v":0},{"$f":"IF($AF36=3,IF($AF$2=2,(W36/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I36,Refurb_Poss_Tbl[%]))*AG36,W36*$AG36),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,35,0,{"$f":"VLOOKUP(AE37,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35538339780838735},0,0,0,0,0,0,0,0,1.9513232122499401E-2,{"$f":"IF(OR(AF37=3,AF37=2,AF37=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D37,FlatMaint!$Y$2:$Y$10000,AE37)*AG37,0)","v":31.403854520578058},{"$f":"IF(OR(AF37=3,AF37=2,AF37=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D37,FlatRepair!$Y$2:$Y$10000,AE37)*AG37,0)","v":0},0,31.423367752700557,0,0,0,0,0,31.423367752700557,0,{"$f":"IF($AF37=3,IF($AF$2=2,(R37/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I37,Refurb_Poss_Tbl[%]))*AG37,IF($AF$2=3,(R37*AG37)-AV37,R37*AG37)),0)","v":0},{"$f":"IF(AF37=3,IF($AF$2=2,(S37/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I37,Refurb_Poss_Tbl[%]))*AG37,IF($AF$2=3,(S37*AG37)-AX37,S37*AG37)),0)","v":0},{"$f":"IF($AF37=3,IF($AF$2=2,(T37/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I37,Refurb_Poss_Tbl[%]))*AG37,T37*$AG37),0)","v":0},{"$f":"IF($AF37=3,IF($AF$2=2,(Q37/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I37,Refurb_Poss_Tbl[%]))*AG37,Q37*$AG37),0)","v":0},{"$f":"IF($AF37=3,IF($AF$2=2,(U37/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I37,Refurb_Poss_Tbl[%]))*AG37,U37*$AG37),0)","v":0},{"$f":"IF($AF37=3,IF($AF$2=2,(V37/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I37,Refurb_Poss_Tbl[%]))*AG37,IF($AF$2=3,(V37*AG37)-AW37,V37*AG37)),0)","v":0},{"$f":"IF($AF37=3,IF($AF$2=2,(W37/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I37,Refurb_Poss_Tbl[%]))*AG37,W37*$AG37),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,36,0,{"$f":"VLOOKUP(AE38,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.34503242505668674},0,0,0,0,0,0,0,0,1.8944885555824659E-2,{"$f":"IF(OR(AF38=3,AF38=2,AF38=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D38,FlatMaint!$Y$2:$Y$10000,AE38)*AG38,0)","v":30.489179146192289},{"$f":"IF(OR(AF38=3,AF38=2,AF38=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D38,FlatRepair!$Y$2:$Y$10000,AE38)*AG38,0)","v":0},0,30.508124031748114,0,0,0,0,0,30.508124031748114,0,{"$f":"IF($AF38=3,IF($AF$2=2,(R38/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I38,Refurb_Poss_Tbl[%]))*AG38,IF($AF$2=3,(R38*AG38)-AV38,R38*AG38)),0)","v":0},{"$f":"IF(AF38=3,IF($AF$2=2,(S38/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I38,Refurb_Poss_Tbl[%]))*AG38,IF($AF$2=3,(S38*AG38)-AX38,S38*AG38)),0)","v":0},{"$f":"IF($AF38=3,IF($AF$2=2,(T38/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I38,Refurb_Poss_Tbl[%]))*AG38,T38*$AG38),0)","v":0},{"$f":"IF($AF38=3,IF($AF$2=2,(Q38/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I38,Refurb_Poss_Tbl[%]))*AG38,Q38*$AG38),0)","v":0},{"$f":"IF($AF38=3,IF($AF$2=2,(U38/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I38,Refurb_Poss_Tbl[%]))*AG38,U38*$AG38),0)","v":0},{"$f":"IF($AF38=3,IF($AF$2=2,(V38/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I38,Refurb_Poss_Tbl[%]))*AG38,IF($AF$2=3,(V38*AG38)-AW38,V38*AG38)),0)","v":0},{"$f":"IF($AF38=3,IF($AF$2=2,(W38/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I38,Refurb_Poss_Tbl[%]))*AG38,W38*$AG38),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,37,0,{"$f":"VLOOKUP(AE39,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.33498293694823961},0,0,0,0,0,0,0,0,1.8393092772645305E-2,{"$f":"IF(OR(AF39=3,AF39=2,AF39=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D39,FlatMaint!$Y$2:$Y$10000,AE39)*AG39,0)","v":29.601144802128442},{"$f":"IF(OR(AF39=3,AF39=2,AF39=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D39,FlatRepair!$Y$2:$Y$10000,AE39)*AG39,0)","v":0},0,29.619537894901086,0,0,0,0,0,29.619537894901086,0,{"$f":"IF($AF39=3,IF($AF$2=2,(R39/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I39,Refurb_Poss_Tbl[%]))*AG39,IF($AF$2=3,(R39*AG39)-AV39,R39*AG39)),0)","v":0},{"$f":"IF(AF39=3,IF($AF$2=2,(S39/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I39,Refurb_Poss_Tbl[%]))*AG39,IF($AF$2=3,(S39*AG39)-AX39,S39*AG39)),0)","v":0},{"$f":"IF($AF39=3,IF($AF$2=2,(T39/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I39,Refurb_Poss_Tbl[%]))*AG39,T39*$AG39),0)","v":0},{"$f":"IF($AF39=3,IF($AF$2=2,(Q39/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I39,Refurb_Poss_Tbl[%]))*AG39,Q39*$AG39),0)","v":0},{"$f":"IF($AF39=3,IF($AF$2=2,(U39/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I39,Refurb_Poss_Tbl[%]))*AG39,U39*$AG39),0)","v":0},{"$f":"IF($AF39=3,IF($AF$2=2,(V39/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I39,Refurb_Poss_Tbl[%]))*AG39,IF($AF$2=3,(V39*AG39)-AW39,V39*AG39)),0)","v":0},{"$f":"IF($AF39=3,IF($AF$2=2,(W39/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I39,Refurb_Poss_Tbl[%]))*AG39,W39*$AG39),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,38,0,{"$f":"VLOOKUP(AE40,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.3252261523769317},0,0,0,0,0,0,0,0,1.7857371623927483E-2,{"$f":"IF(OR(AF40=3,AF40=2,AF40=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D40,FlatMaint!$Y$2:$Y$10000,AE40)*AG40,0)","v":28.738975536047036},{"$f":"IF(OR(AF40=3,AF40=2,AF40=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D40,FlatRepair!$Y$2:$Y$10000,AE40)*AG40,0)","v":0},0,28.756832907670965,0,0,0,0,0,28.756832907670965,0,{"$f":"IF($AF40=3,IF($AF$2=2,(R40/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I40,Refurb_Poss_Tbl[%]))*AG40,IF($AF$2=3,(R40*AG40)-AV40,R40*AG40)),0)","v":0},{"$f":"IF(AF40=3,IF($AF$2=2,(S40/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I40,Refurb_Poss_Tbl[%]))*AG40,IF($AF$2=3,(S40*AG40)-AX40,S40*AG40)),0)","v":0},{"$f":"IF($AF40=3,IF($AF$2=2,(T40/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I40,Refurb_Poss_Tbl[%]))*AG40,T40*$AG40),0)","v":0},{"$f":"IF($AF40=3,IF($AF$2=2,(Q40/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I40,Refurb_Poss_Tbl[%]))*AG40,Q40*$AG40),0)","v":0},{"$f":"IF($AF40=3,IF($AF$2=2,(U40/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I40,Refurb_Poss_Tbl[%]))*AG40,U40*$AG40),0)","v":0},{"$f":"IF($AF40=3,IF($AF$2=2,(V40/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I40,Refurb_Poss_Tbl[%]))*AG40,IF($AF$2=3,(V40*AG40)-AW40,V40*AG40)),0)","v":0},{"$f":"IF($AF40=3,IF($AF$2=2,(W40/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I40,Refurb_Poss_Tbl[%]))*AG40,W40*$AG40),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,39,0,{"$f":"VLOOKUP(AE41,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.31575354599702099},0,0,0,0,0,0,0,0,1.7337254003813085E-2,{"$f":"IF(OR(AF41=3,AF41=2,AF41=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D41,FlatMaint!$Y$2:$Y$10000,AE41)*AG41,0)","v":27.901917996162162},{"$f":"IF(OR(AF41=3,AF41=2,AF41=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D41,FlatRepair!$Y$2:$Y$10000,AE41)*AG41,0)","v":0},0,27.919255250165975,0,0,0,0,0,27.919255250165975,0,{"$f":"IF($AF41=3,IF($AF$2=2,(R41/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I41,Refurb_Poss_Tbl[%]))*AG41,IF($AF$2=3,(R41*AG41)-AV41,R41*AG41)),0)","v":0},{"$f":"IF(AF41=3,IF($AF$2=2,(S41/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I41,Refurb_Poss_Tbl[%]))*AG41,IF($AF$2=3,(S41*AG41)-AX41,S41*AG41)),0)","v":0},{"$f":"IF($AF41=3,IF($AF$2=2,(T41/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I41,Refurb_Poss_Tbl[%]))*AG41,T41*$AG41),0)","v":0},{"$f":"IF($AF41=3,IF($AF$2=2,(Q41/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I41,Refurb_Poss_Tbl[%]))*AG41,Q41*$AG41),0)","v":0},{"$f":"IF($AF41=3,IF($AF$2=2,(U41/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I41,Refurb_Poss_Tbl[%]))*AG41,U41*$AG41),0)","v":0},{"$f":"IF($AF41=3,IF($AF$2=2,(V41/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I41,Refurb_Poss_Tbl[%]))*AG41,IF($AF$2=3,(V41*AG41)-AW41,V41*AG41)),0)","v":0},{"$f":"IF($AF41=3,IF($AF$2=2,(W41/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I41,Refurb_Poss_Tbl[%]))*AG41,W41*$AG41),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,40,0,{"$f":"VLOOKUP(AE42,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.30655684077380685},0,0,0,0,0,0,0,0,1.6832285440595233E-2,{"$f":"IF(OR(AF42=3,AF42=2,AF42=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D42,FlatMaint!$Y$2:$Y$10000,AE42)*AG42,0)","v":27.089240772972978},{"$f":"IF(OR(AF42=3,AF42=2,AF42=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D42,FlatRepair!$Y$2:$Y$10000,AE42)*AG42,0)","v":0},0,27.106073058413575,0,0,0,0,0,27.106073058413575,0,{"$f":"IF($AF42=3,IF($AF$2=2,(R42/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I42,Refurb_Poss_Tbl[%]))*AG42,IF($AF$2=3,(R42*AG42)-AV42,R42*AG42)),0)","v":0},{"$f":"IF(AF42=3,IF($AF$2=2,(S42/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I42,Refurb_Poss_Tbl[%]))*AG42,IF($AF$2=3,(S42*AG42)-AX42,S42*AG42)),0)","v":0},{"$f":"IF($AF42=3,IF($AF$2=2,(T42/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I42,Refurb_Poss_Tbl[%]))*AG42,T42*$AG42),0)","v":0},{"$f":"IF($AF42=3,IF($AF$2=2,(Q42/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I42,Refurb_Poss_Tbl[%]))*AG42,Q42*$AG42),0)","v":0},{"$f":"IF($AF42=3,IF($AF$2=2,(U42/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I42,Refurb_Poss_Tbl[%]))*AG42,U42*$AG42),0)","v":0},{"$f":"IF($AF42=3,IF($AF$2=2,(V42/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I42,Refurb_Poss_Tbl[%]))*AG42,IF($AF$2=3,(V42*AG42)-AW42,V42*AG42)),0)","v":0},{"$f":"IF($AF42=3,IF($AF$2=2,(W42/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I42,Refurb_Poss_Tbl[%]))*AG42,W42*$AG42),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,41,0,{"$f":"VLOOKUP(AE43,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.29762800075126877},0,0,0,0,0,0,0,0,1.6342024699607022E-2,{"$f":"IF(OR(AF43=3,AF43=2,AF43=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D43,FlatMaint!$Y$2:$Y$10000,AE43)*AG43,0)","v":26.300233760167938},{"$f":"IF(OR(AF43=3,AF43=2,AF43=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D43,FlatRepair!$Y$2:$Y$10000,AE43)*AG43,0)","v":0},0,26.316575784867545,0,0,0,0,0,26.316575784867545,0,{"$f":"IF($AF43=3,IF($AF$2=2,(R43/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I43,Refurb_Poss_Tbl[%]))*AG43,IF($AF$2=3,(R43*AG43)-AV43,R43*AG43)),0)","v":0},{"$f":"IF(AF43=3,IF($AF$2=2,(S43/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I43,Refurb_Poss_Tbl[%]))*AG43,IF($AF$2=3,(S43*AG43)-AX43,S43*AG43)),0)","v":0},{"$f":"IF($AF43=3,IF($AF$2=2,(T43/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I43,Refurb_Poss_Tbl[%]))*AG43,T43*$AG43),0)","v":0},{"$f":"IF($AF43=3,IF($AF$2=2,(Q43/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I43,Refurb_Poss_Tbl[%]))*AG43,Q43*$AG43),0)","v":0},{"$f":"IF($AF43=3,IF($AF$2=2,(U43/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I43,Refurb_Poss_Tbl[%]))*AG43,U43*$AG43),0)","v":0},{"$f":"IF($AF43=3,IF($AF$2=2,(V43/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I43,Refurb_Poss_Tbl[%]))*AG43,IF($AF$2=3,(V43*AG43)-AW43,V43*AG43)),0)","v":0},{"$f":"IF($AF43=3,IF($AF$2=2,(W43/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I43,Refurb_Poss_Tbl[%]))*AG43,W43*$AG43),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,42,0,{"$f":"VLOOKUP(AE44,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28895922403035801},0,0,0,0,0,0,0,0,1.5866043397676718E-2,{"$f":"IF(OR(AF44=3,AF44=2,AF44=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D44,FlatMaint!$Y$2:$Y$10000,AE44)*AG44,0)","v":25.534207534143629},{"$f":"IF(OR(AF44=3,AF44=2,AF44=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D44,FlatRepair!$Y$2:$Y$10000,AE44)*AG44,0)","v":0},0,25.550073577541305,0,0,0,0,0,25.550073577541305,0,{"$f":"IF($AF44=3,IF($AF$2=2,(R44/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I44,Refurb_Poss_Tbl[%]))*AG44,IF($AF$2=3,(R44*AG44)-AV44,R44*AG44)),0)","v":0},{"$f":"IF(AF44=3,IF($AF$2=2,(S44/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I44,Refurb_Poss_Tbl[%]))*AG44,IF($AF$2=3,(S44*AG44)-AX44,S44*AG44)),0)","v":0},{"$f":"IF($AF44=3,IF($AF$2=2,(T44/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I44,Refurb_Poss_Tbl[%]))*AG44,T44*$AG44),0)","v":0},{"$f":"IF($AF44=3,IF($AF$2=2,(Q44/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I44,Refurb_Poss_Tbl[%]))*AG44,Q44*$AG44),0)","v":0},{"$f":"IF($AF44=3,IF($AF$2=2,(U44/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I44,Refurb_Poss_Tbl[%]))*AG44,U44*$AG44),0)","v":0},{"$f":"IF($AF44=3,IF($AF$2=2,(V44/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I44,Refurb_Poss_Tbl[%]))*AG44,IF($AF$2=3,(V44*AG44)-AW44,V44*AG44)),0)","v":0},{"$f":"IF($AF44=3,IF($AF$2=2,(W44/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I44,Refurb_Poss_Tbl[%]))*AG44,W44*$AG44),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,43,0,{"$f":"VLOOKUP(AE45,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28054293595180391},0,0,0,0,0,0,0,0,1.5403925628812348E-2,{"$f":"IF(OR(AF45=3,AF45=2,AF45=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D45,FlatMaint!$Y$2:$Y$10000,AE45)*AG45,0)","v":24.790492751595757},{"$f":"IF(OR(AF45=3,AF45=2,AF45=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D45,FlatRepair!$Y$2:$Y$10000,AE45)*AG45,0)","v":0},0,24.80589667722457,0,0,0,0,0,24.80589667722457,0,{"$f":"IF($AF45=3,IF($AF$2=2,(R45/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I45,Refurb_Poss_Tbl[%]))*AG45,IF($AF$2=3,(R45*AG45)-AV45,R45*AG45)),0)","v":0},{"$f":"IF(AF45=3,IF($AF$2=2,(S45/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I45,Refurb_Poss_Tbl[%]))*AG45,IF($AF$2=3,(S45*AG45)-AX45,S45*AG45)),0)","v":0},{"$f":"IF($AF45=3,IF($AF$2=2,(T45/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I45,Refurb_Poss_Tbl[%]))*AG45,T45*$AG45),0)","v":0},{"$f":"IF($AF45=3,IF($AF$2=2,(Q45/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I45,Refurb_Poss_Tbl[%]))*AG45,Q45*$AG45),0)","v":0},{"$f":"IF($AF45=3,IF($AF$2=2,(U45/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I45,Refurb_Poss_Tbl[%]))*AG45,U45*$AG45),0)","v":0},{"$f":"IF($AF45=3,IF($AF$2=2,(V45/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I45,Refurb_Poss_Tbl[%]))*AG45,IF($AF$2=3,(V45*AG45)-AW45,V45*AG45)),0)","v":0},{"$f":"IF($AF45=3,IF($AF$2=2,(W45/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I45,Refurb_Poss_Tbl[%]))*AG45,W45*$AG45),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,44,0,{"$f":"VLOOKUP(AE46,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.27237178247747956},0,0,0,0,0,0,0,0,1.4955267600788689E-2,{"$f":"IF(OR(AF46=3,AF46=2,AF46=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D46,FlatMaint!$Y$2:$Y$10000,AE46)*AG46,0)","v":24.068439564656078},{"$f":"IF(OR(AF46=3,AF46=2,AF46=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D46,FlatRepair!$Y$2:$Y$10000,AE46)*AG46,0)","v":0},0,24.083394832256868,0,0,0,0,0,24.083394832256868,0,{"$f":"IF($AF46=3,IF($AF$2=2,(R46/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I46,Refurb_Poss_Tbl[%]))*AG46,IF($AF$2=3,(R46*AG46)-AV46,R46*AG46)),0)","v":0},{"$f":"IF(AF46=3,IF($AF$2=2,(S46/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I46,Refurb_Poss_Tbl[%]))*AG46,IF($AF$2=3,(S46*AG46)-AX46,S46*AG46)),0)","v":0},{"$f":"IF($AF46=3,IF($AF$2=2,(T46/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I46,Refurb_Poss_Tbl[%]))*AG46,T46*$AG46),0)","v":0},{"$f":"IF($AF46=3,IF($AF$2=2,(Q46/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I46,Refurb_Poss_Tbl[%]))*AG46,Q46*$AG46),0)","v":0},{"$f":"IF($AF46=3,IF($AF$2=2,(U46/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I46,Refurb_Poss_Tbl[%]))*AG46,U46*$AG46),0)","v":0},{"$f":"IF($AF46=3,IF($AF$2=2,(V46/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I46,Refurb_Poss_Tbl[%]))*AG46,IF($AF$2=3,(V46*AG46)-AW46,V46*AG46)),0)","v":0},{"$f":"IF($AF46=3,IF($AF$2=2,(W46/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I46,Refurb_Poss_Tbl[%]))*AG46,W46*$AG46),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,45,0,{"$f":"VLOOKUP(AE47,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.26443862376454325},0,0,0,0,0,0,0,0,1.4519677282319114E-2,{"$f":"IF(OR(AF47=3,AF47=2,AF47=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D47,FlatMaint!$Y$2:$Y$10000,AE47)*AG47,0)","v":23.367417053064152},{"$f":"IF(OR(AF47=3,AF47=2,AF47=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D47,FlatRepair!$Y$2:$Y$10000,AE47)*AG47,0)","v":0},0,23.381936730346471,0,0,0,0,0,23.381936730346471,0,{"$f":"IF($AF47=3,IF($AF$2=2,(R47/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I47,Refurb_Poss_Tbl[%]))*AG47,IF($AF$2=3,(R47*AG47)-AV47,R47*AG47)),0)","v":0},{"$f":"IF(AF47=3,IF($AF$2=2,(S47/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I47,Refurb_Poss_Tbl[%]))*AG47,IF($AF$2=3,(S47*AG47)-AX47,S47*AG47)),0)","v":0},{"$f":"IF($AF47=3,IF($AF$2=2,(T47/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I47,Refurb_Poss_Tbl[%]))*AG47,T47*$AG47),0)","v":0},{"$f":"IF($AF47=3,IF($AF$2=2,(Q47/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I47,Refurb_Poss_Tbl[%]))*AG47,Q47*$AG47),0)","v":0},{"$f":"IF($AF47=3,IF($AF$2=2,(U47/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I47,Refurb_Poss_Tbl[%]))*AG47,U47*$AG47),0)","v":0},{"$f":"IF($AF47=3,IF($AF$2=2,(V47/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I47,Refurb_Poss_Tbl[%]))*AG47,IF($AF$2=3,(V47*AG47)-AW47,V47*AG47)),0)","v":0},{"$f":"IF($AF47=3,IF($AF$2=2,(W47/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I47,Refurb_Poss_Tbl[%]))*AG47,W47*$AG47),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,46,0,{"$f":"VLOOKUP(AE48,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.25673652792674101},0,0,0,0,0,0,0,0,1.4096774060503995E-2,{"$f":"IF(OR(AF48=3,AF48=2,AF48=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D48,FlatMaint!$Y$2:$Y$10000,AE48)*AG48,0)","v":22.686812672877817},{"$f":"IF(OR(AF48=3,AF48=2,AF48=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D48,FlatRepair!$Y$2:$Y$10000,AE48)*AG48,0)","v":0},0,22.700909446938322,0,0,0,0,0,22.700909446938322,0,{"$f":"IF($AF48=3,IF($AF$2=2,(R48/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I48,Refurb_Poss_Tbl[%]))*AG48,IF($AF$2=3,(R48*AG48)-AV48,R48*AG48)),0)","v":0},{"$f":"IF(AF48=3,IF($AF$2=2,(S48/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I48,Refurb_Poss_Tbl[%]))*AG48,IF($AF$2=3,(S48*AG48)-AX48,S48*AG48)),0)","v":0},{"$f":"IF($AF48=3,IF($AF$2=2,(T48/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I48,Refurb_Poss_Tbl[%]))*AG48,T48*$AG48),0)","v":0},{"$f":"IF($AF48=3,IF($AF$2=2,(Q48/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I48,Refurb_Poss_Tbl[%]))*AG48,Q48*$AG48),0)","v":0},{"$f":"IF($AF48=3,IF($AF$2=2,(U48/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I48,Refurb_Poss_Tbl[%]))*AG48,U48*$AG48),0)","v":0},{"$f":"IF($AF48=3,IF($AF$2=2,(V48/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I48,Refurb_Poss_Tbl[%]))*AG48,IF($AF$2=3,(V48*AG48)-AW48,V48*AG48)),0)","v":0},{"$f":"IF($AF48=3,IF($AF$2=2,(W48/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I48,Refurb_Poss_Tbl[%]))*AG48,W48*$AG48),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,47,0,{"$f":"VLOOKUP(AE49,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24925876497741845},0,0,0,0,0,0,0,0,1.3686188408256306E-2,{"$f":"IF(OR(AF49=3,AF49=2,AF49=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D49,FlatMaint!$Y$2:$Y$10000,AE49)*AG49,0)","v":22.026031721240599},{"$f":"IF(OR(AF49=3,AF49=2,AF49=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D49,FlatRepair!$Y$2:$Y$10000,AE49)*AG49,0)","v":0},0,22.039717909648857,0,0,0,0,0,22.039717909648857,0,{"$f":"IF($AF49=3,IF($AF$2=2,(R49/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I49,Refurb_Poss_Tbl[%]))*AG49,IF($AF$2=3,(R49*AG49)-AV49,R49*AG49)),0)","v":0},{"$f":"IF(AF49=3,IF($AF$2=2,(S49/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I49,Refurb_Poss_Tbl[%]))*AG49,IF($AF$2=3,(S49*AG49)-AX49,S49*AG49)),0)","v":0},{"$f":"IF($AF49=3,IF($AF$2=2,(T49/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I49,Refurb_Poss_Tbl[%]))*AG49,T49*$AG49),0)","v":0},{"$f":"IF($AF49=3,IF($AF$2=2,(Q49/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I49,Refurb_Poss_Tbl[%]))*AG49,Q49*$AG49),0)","v":0},{"$f":"IF($AF49=3,IF($AF$2=2,(U49/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I49,Refurb_Poss_Tbl[%]))*AG49,U49*$AG49),0)","v":0},{"$f":"IF($AF49=3,IF($AF$2=2,(V49/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I49,Refurb_Poss_Tbl[%]))*AG49,IF($AF$2=3,(V49*AG49)-AW49,V49*AG49)),0)","v":0},{"$f":"IF($AF49=3,IF($AF$2=2,(W49/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I49,Refurb_Poss_Tbl[%]))*AG49,W49*$AG49),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,48,0,{"$f":"VLOOKUP(AE50,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24199880094894996},0,0,0,0,0,0,0,0,1.3287561561413889E-2,{"$f":"IF(OR(AF50=3,AF50=2,AF50=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D50,FlatMaint!$Y$2:$Y$10000,AE50)*AG50,0)","v":21.384496816738444},{"$f":"IF(OR(AF50=3,AF50=2,AF50=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D50,FlatRepair!$Y$2:$Y$10000,AE50)*AG50,0)","v":0},0,21.397784378299857,0,0,0,0,0,21.397784378299857,0,{"$f":"IF($AF50=3,IF($AF$2=2,(R50/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I50,Refurb_Poss_Tbl[%]))*AG50,IF($AF$2=3,(R50*AG50)-AV50,R50*AG50)),0)","v":0},{"$f":"IF(AF50=3,IF($AF$2=2,(S50/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I50,Refurb_Poss_Tbl[%]))*AG50,IF($AF$2=3,(S50*AG50)-AX50,S50*AG50)),0)","v":0},{"$f":"IF($AF50=3,IF($AF$2=2,(T50/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I50,Refurb_Poss_Tbl[%]))*AG50,T50*$AG50),0)","v":0},{"$f":"IF($AF50=3,IF($AF$2=2,(Q50/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I50,Refurb_Poss_Tbl[%]))*AG50,Q50*$AG50),0)","v":0},{"$f":"IF($AF50=3,IF($AF$2=2,(U50/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I50,Refurb_Poss_Tbl[%]))*AG50,U50*$AG50),0)","v":0},{"$f":"IF($AF50=3,IF($AF$2=2,(V50/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I50,Refurb_Poss_Tbl[%]))*AG50,IF($AF$2=3,(V50*AG50)-AW50,V50*AG50)),0)","v":0},{"$f":"IF($AF50=3,IF($AF$2=2,(W50/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I50,Refurb_Poss_Tbl[%]))*AG50,W50*$AG50),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,49,0,{"$f":"VLOOKUP(AE51,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.2349502921834466},0,0,0,0,0,0,0,0,1.2900545205256206E-2,{"$f":"IF(OR(AF51=3,AF51=2,AF51=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D51,FlatMaint!$Y$2:$Y$10000,AE51)*AG51,0)","v":20.7616473948917},{"$f":"IF(OR(AF51=3,AF51=2,AF51=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D51,FlatRepair!$Y$2:$Y$10000,AE51)*AG51,0)","v":0},0,20.774547940096955,0,0,0,0,0,20.774547940096955,0,{"$f":"IF($AF51=3,IF($AF$2=2,(R51/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I51,Refurb_Poss_Tbl[%]))*AG51,IF($AF$2=3,(R51*AG51)-AV51,R51*AG51)),0)","v":0},{"$f":"IF(AF51=3,IF($AF$2=2,(S51/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I51,Refurb_Poss_Tbl[%]))*AG51,IF($AF$2=3,(S51*AG51)-AX51,S51*AG51)),0)","v":0},{"$f":"IF($AF51=3,IF($AF$2=2,(T51/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I51,Refurb_Poss_Tbl[%]))*AG51,T51*$AG51),0)","v":0},{"$f":"IF($AF51=3,IF($AF$2=2,(Q51/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I51,Refurb_Poss_Tbl[%]))*AG51,Q51*$AG51),0)","v":0},{"$f":"IF($AF51=3,IF($AF$2=2,(U51/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I51,Refurb_Poss_Tbl[%]))*AG51,U51*$AG51),0)","v":0},{"$f":"IF($AF51=3,IF($AF$2=2,(V51/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I51,Refurb_Poss_Tbl[%]))*AG51,IF($AF$2=3,(V51*AG51)-AW51,V51*AG51)),0)","v":0},{"$f":"IF($AF51=3,IF($AF$2=2,(W51/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I51,Refurb_Poss_Tbl[%]))*AG51,W51*$AG51),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,50,2,{"$f":"VLOOKUP(AE52,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22810707978975397},0,0,0,0,0,0,0,0,1.2524801170151655E-2,{"$f":"IF(OR(AF52=3,AF52=2,AF52=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D52,FlatMaint!$Y$2:$Y$10000,AE52)*AG52,0)","v":20.156939218341453},{"$f":"IF(OR(AF52=3,AF52=2,AF52=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D52,FlatRepair!$Y$2:$Y$10000,AE52)*AG52,0)","v":0},0,20.169464019511604,51.053060544147385,0,0,0,0,71.222524563658993,0,{"$f":"IF($AF52=3,IF($AF$2=2,(R52/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I52,Refurb_Poss_Tbl[%]))*AG52,IF($AF$2=3,(R52*AG52)-AV52,R52*AG52)),0)","v":0},{"$f":"IF(AF52=3,IF($AF$2=2,(S52/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I52,Refurb_Poss_Tbl[%]))*AG52,IF($AF$2=3,(S52*AG52)-AX52,S52*AG52)),0)","v":0},{"$f":"IF($AF52=3,IF($AF$2=2,(T52/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I52,Refurb_Poss_Tbl[%]))*AG52,T52*$AG52),0)","v":0},{"$f":"IF($AF52=3,IF($AF$2=2,(Q52/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I52,Refurb_Poss_Tbl[%]))*AG52,Q52*$AG52),0)","v":0},{"$f":"IF($AF52=3,IF($AF$2=2,(U52/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I52,Refurb_Poss_Tbl[%]))*AG52,U52*$AG52),0)","v":0},{"$f":"IF($AF52=3,IF($AF$2=2,(V52/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I52,Refurb_Poss_Tbl[%]))*AG52,IF($AF$2=3,(V52*AG52)-AW52,V52*AG52)),0)","v":0},{"$f":"IF($AF52=3,IF($AF$2=2,(W52/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I52,Refurb_Poss_Tbl[%]))*AG52,W52*$AG52),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,51,0,{"$f":"VLOOKUP(AE53,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22146318426189707},0,0,0,0,0,0,0,0,1.2160001136069569E-2,{"$f":"IF(OR(AF53=3,AF53=2,AF53=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D53,FlatMaint!$Y$2:$Y$10000,AE53)*AG53,0)","v":19.569843901302384},{"$f":"IF(OR(AF53=3,AF53=2,AF53=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D53,FlatRepair!$Y$2:$Y$10000,AE53)*AG53,0)","v":0},0,19.582003902438455,0,0,0,0,0,19.582003902438455,0,{"$f":"IF($AF53=3,IF($AF$2=2,(R53/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I53,Refurb_Poss_Tbl[%]))*AG53,IF($AF$2=3,(R53*AG53)-AV53,R53*AG53)),0)","v":0},{"$f":"IF(AF53=3,IF($AF$2=2,(S53/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I53,Refurb_Poss_Tbl[%]))*AG53,IF($AF$2=3,(S53*AG53)-AX53,S53*AG53)),0)","v":0},{"$f":"IF($AF53=3,IF($AF$2=2,(T53/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I53,Refurb_Poss_Tbl[%]))*AG53,T53*$AG53),0)","v":0},{"$f":"IF($AF53=3,IF($AF$2=2,(Q53/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I53,Refurb_Poss_Tbl[%]))*AG53,Q53*$AG53),0)","v":0},{"$f":"IF($AF53=3,IF($AF$2=2,(U53/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I53,Refurb_Poss_Tbl[%]))*AG53,U53*$AG53),0)","v":0},{"$f":"IF($AF53=3,IF($AF$2=2,(V53/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I53,Refurb_Poss_Tbl[%]))*AG53,IF($AF$2=3,(V53*AG53)-AW53,V53*AG53)),0)","v":0},{"$f":"IF($AF53=3,IF($AF$2=2,(W53/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I53,Refurb_Poss_Tbl[%]))*AG53,W53*$AG53),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,52,0,{"$f":"VLOOKUP(AE54,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.215012800254269},0,0,0,0,0,0,0,0,1.1805826345698611E-2,{"$f":"IF(OR(AF54=3,AF54=2,AF54=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D54,FlatMaint!$Y$2:$Y$10000,AE54)*AG54,0)","v":18.999848447866391},{"$f":"IF(OR(AF54=3,AF54=2,AF54=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D54,FlatRepair!$Y$2:$Y$10000,AE54)*AG54,0)","v":0},0,19.011654274212091,0,0,0,0,0,19.011654274212091,0,{"$f":"IF($AF54=3,IF($AF$2=2,(R54/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I54,Refurb_Poss_Tbl[%]))*AG54,IF($AF$2=3,(R54*AG54)-AV54,R54*AG54)),0)","v":0},{"$f":"IF(AF54=3,IF($AF$2=2,(S54/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I54,Refurb_Poss_Tbl[%]))*AG54,IF($AF$2=3,(S54*AG54)-AX54,S54*AG54)),0)","v":0},{"$f":"IF($AF54=3,IF($AF$2=2,(T54/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I54,Refurb_Poss_Tbl[%]))*AG54,T54*$AG54),0)","v":0},{"$f":"IF($AF54=3,IF($AF$2=2,(Q54/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I54,Refurb_Poss_Tbl[%]))*AG54,Q54*$AG54),0)","v":0},{"$f":"IF($AF54=3,IF($AF$2=2,(U54/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I54,Refurb_Poss_Tbl[%]))*AG54,U54*$AG54),0)","v":0},{"$f":"IF($AF54=3,IF($AF$2=2,(V54/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I54,Refurb_Poss_Tbl[%]))*AG54,IF($AF$2=3,(V54*AG54)-AW54,V54*AG54)),0)","v":0},{"$f":"IF($AF54=3,IF($AF$2=2,(W54/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I54,Refurb_Poss_Tbl[%]))*AG54,W54*$AG54),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,53,0,{"$f":"VLOOKUP(AE55,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20875029150899907},0,0,0,0,0,0,0,0,1.1461967325920983E-2,{"$f":"IF(OR(AF55=3,AF55=2,AF55=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D55,FlatMaint!$Y$2:$Y$10000,AE55)*AG55,0)","v":18.446454803753781},{"$f":"IF(OR(AF55=3,AF55=2,AF55=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D55,FlatRepair!$Y$2:$Y$10000,AE55)*AG55,0)","v":0},0,18.457916771079702,0,0,0,0,0,18.457916771079702,0,{"$f":"IF($AF55=3,IF($AF$2=2,(R55/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I55,Refurb_Poss_Tbl[%]))*AG55,IF($AF$2=3,(R55*AG55)-AV55,R55*AG55)),0)","v":0},{"$f":"IF(AF55=3,IF($AF$2=2,(S55/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I55,Refurb_Poss_Tbl[%]))*AG55,IF($AF$2=3,(S55*AG55)-AX55,S55*AG55)),0)","v":0},{"$f":"IF($AF55=3,IF($AF$2=2,(T55/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I55,Refurb_Poss_Tbl[%]))*AG55,T55*$AG55),0)","v":0},{"$f":"IF($AF55=3,IF($AF$2=2,(Q55/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I55,Refurb_Poss_Tbl[%]))*AG55,Q55*$AG55),0)","v":0},{"$f":"IF($AF55=3,IF($AF$2=2,(U55/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I55,Refurb_Poss_Tbl[%]))*AG55,U55*$AG55),0)","v":0},{"$f":"IF($AF55=3,IF($AF$2=2,(V55/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I55,Refurb_Poss_Tbl[%]))*AG55,IF($AF$2=3,(V55*AG55)-AW55,V55*AG55)),0)","v":0},{"$f":"IF($AF55=3,IF($AF$2=2,(W55/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I55,Refurb_Poss_Tbl[%]))*AG55,W55*$AG55),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,54,0,{"$f":"VLOOKUP(AE56,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20267018593106703},0,0,0,0,0,0,0,0,1.1128123617399011E-2,{"$f":"IF(OR(AF56=3,AF56=2,AF56=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D56,FlatMaint!$Y$2:$Y$10000,AE56)*AG56,0)","v":17.909179421120175},{"$f":"IF(OR(AF56=3,AF56=2,AF56=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D56,FlatRepair!$Y$2:$Y$10000,AE56)*AG56,0)","v":0},0,17.920307544737575,0,0,0,0,0,17.920307544737575,0,{"$f":"IF($AF56=3,IF($AF$2=2,(R56/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I56,Refurb_Poss_Tbl[%]))*AG56,IF($AF$2=3,(R56*AG56)-AV56,R56*AG56)),0)","v":0},{"$f":"IF(AF56=3,IF($AF$2=2,(S56/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I56,Refurb_Poss_Tbl[%]))*AG56,IF($AF$2=3,(S56*AG56)-AX56,S56*AG56)),0)","v":0},{"$f":"IF($AF56=3,IF($AF$2=2,(T56/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I56,Refurb_Poss_Tbl[%]))*AG56,T56*$AG56),0)","v":0},{"$f":"IF($AF56=3,IF($AF$2=2,(Q56/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I56,Refurb_Poss_Tbl[%]))*AG56,Q56*$AG56),0)","v":0},{"$f":"IF($AF56=3,IF($AF$2=2,(U56/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I56,Refurb_Poss_Tbl[%]))*AG56,U56*$AG56),0)","v":0},{"$f":"IF($AF56=3,IF($AF$2=2,(V56/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I56,Refurb_Poss_Tbl[%]))*AG56,IF($AF$2=3,(V56*AG56)-AW56,V56*AG56)),0)","v":0},{"$f":"IF($AF56=3,IF($AF$2=2,(W56/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I56,Refurb_Poss_Tbl[%]))*AG56,W56*$AG56),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,55,0,{"$f":"VLOOKUP(AE57,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19676717080686118},0,0,0,0,0,0,0,0,1.0804003512037873E-2,{"$f":"IF(OR(AF57=3,AF57=2,AF57=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D57,FlatMaint!$Y$2:$Y$10000,AE57)*AG57,0)","v":17.387552836039003},{"$f":"IF(OR(AF57=3,AF57=2,AF57=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D57,FlatRepair!$Y$2:$Y$10000,AE57)*AG57,0)","v":0},0,17.398356839551042,0,0,0,0,0,17.398356839551042,0,{"$f":"IF($AF57=3,IF($AF$2=2,(R57/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I57,Refurb_Poss_Tbl[%]))*AG57,IF($AF$2=3,(R57*AG57)-AV57,R57*AG57)),0)","v":0},{"$f":"IF(AF57=3,IF($AF$2=2,(S57/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I57,Refurb_Poss_Tbl[%]))*AG57,IF($AF$2=3,(S57*AG57)-AX57,S57*AG57)),0)","v":0},{"$f":"IF($AF57=3,IF($AF$2=2,(T57/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I57,Refurb_Poss_Tbl[%]))*AG57,T57*$AG57),0)","v":0},{"$f":"IF($AF57=3,IF($AF$2=2,(Q57/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I57,Refurb_Poss_Tbl[%]))*AG57,Q57*$AG57),0)","v":0},{"$f":"IF($AF57=3,IF($AF$2=2,(U57/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I57,Refurb_Poss_Tbl[%]))*AG57,U57*$AG57),0)","v":0},{"$f":"IF($AF57=3,IF($AF$2=2,(V57/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I57,Refurb_Poss_Tbl[%]))*AG57,IF($AF$2=3,(V57*AG57)-AW57,V57*AG57)),0)","v":0},{"$f":"IF($AF57=3,IF($AF$2=2,(W57/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I57,Refurb_Poss_Tbl[%]))*AG57,W57*$AG57),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,56,0,{"$f":"VLOOKUP(AE58,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19103608816200118},0,0,0,0,0,0,0,0,1.0489323798095026E-2,{"$f":"IF(OR(AF58=3,AF58=2,AF58=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D58,FlatMaint!$Y$2:$Y$10000,AE58)*AG58,0)","v":16.881119258290298},{"$f":"IF(OR(AF58=3,AF58=2,AF58=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D58,FlatRepair!$Y$2:$Y$10000,AE58)*AG58,0)","v":0},0,16.891608582088391,0,0,0,0,0,16.891608582088391,0,{"$f":"IF($AF58=3,IF($AF$2=2,(R58/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I58,Refurb_Poss_Tbl[%]))*AG58,IF($AF$2=3,(R58*AG58)-AV58,R58*AG58)),0)","v":0},{"$f":"IF(AF58=3,IF($AF$2=2,(S58/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I58,Refurb_Poss_Tbl[%]))*AG58,IF($AF$2=3,(S58*AG58)-AX58,S58*AG58)),0)","v":0},{"$f":"IF($AF58=3,IF($AF$2=2,(T58/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I58,Refurb_Poss_Tbl[%]))*AG58,T58*$AG58),0)","v":0},{"$f":"IF($AF58=3,IF($AF$2=2,(Q58/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I58,Refurb_Poss_Tbl[%]))*AG58,Q58*$AG58),0)","v":0},{"$f":"IF($AF58=3,IF($AF$2=2,(U58/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I58,Refurb_Poss_Tbl[%]))*AG58,U58*$AG58),0)","v":0},{"$f":"IF($AF58=3,IF($AF$2=2,(V58/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I58,Refurb_Poss_Tbl[%]))*AG58,IF($AF$2=3,(V58*AG58)-AW58,V58*AG58)),0)","v":0},{"$f":"IF($AF58=3,IF($AF$2=2,(W58/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I58,Refurb_Poss_Tbl[%]))*AG58,W58*$AG58),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,57,0,{"$f":"VLOOKUP(AE59,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18547193025437006},0,0,0,0,0,0,0,0,1.0183809512713617E-2,{"$f":"IF(OR(AF59=3,AF59=2,AF59=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D59,FlatMaint!$Y$2:$Y$10000,AE59)*AG59,0)","v":16.389436173097373},{"$f":"IF(OR(AF59=3,AF59=2,AF59=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D59,FlatRepair!$Y$2:$Y$10000,AE59)*AG59,0)","v":0},0,16.399619982610087,0,0,0,0,0,16.399619982610087,0,{"$f":"IF($AF59=3,IF($AF$2=2,(R59/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I59,Refurb_Poss_Tbl[%]))*AG59,IF($AF$2=3,(R59*AG59)-AV59,R59*AG59)),0)","v":0},{"$f":"IF(AF59=3,IF($AF$2=2,(S59/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I59,Refurb_Poss_Tbl[%]))*AG59,IF($AF$2=3,(S59*AG59)-AX59,S59*AG59)),0)","v":0},{"$f":"IF($AF59=3,IF($AF$2=2,(T59/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I59,Refurb_Poss_Tbl[%]))*AG59,T59*$AG59),0)","v":0},{"$f":"IF($AF59=3,IF($AF$2=2,(Q59/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I59,Refurb_Poss_Tbl[%]))*AG59,Q59*$AG59),0)","v":0},{"$f":"IF($AF59=3,IF($AF$2=2,(U59/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I59,Refurb_Poss_Tbl[%]))*AG59,U59*$AG59),0)","v":0},{"$f":"IF($AF59=3,IF($AF$2=2,(V59/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I59,Refurb_Poss_Tbl[%]))*AG59,IF($AF$2=3,(V59*AG59)-AW59,V59*AG59)),0)","v":0},{"$f":"IF($AF59=3,IF($AF$2=2,(W59/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I59,Refurb_Poss_Tbl[%]))*AG59,W59*$AG59),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,58,0,{"$f":"VLOOKUP(AE60,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18006983519841754},0,0,0,0,0,0,0,0,9.8871937016637053E-3,{"$f":"IF(OR(AF60=3,AF60=2,AF60=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D60,FlatMaint!$Y$2:$Y$10000,AE60)*AG60,0)","v":15.912073954463471},{"$f":"IF(OR(AF60=3,AF60=2,AF60=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D60,FlatRepair!$Y$2:$Y$10000,AE60)*AG60,0)","v":0},0,15.921961148165135,0,0,0,0,0,15.921961148165135,0,{"$f":"IF($AF60=3,IF($AF$2=2,(R60/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I60,Refurb_Poss_Tbl[%]))*AG60,IF($AF$2=3,(R60*AG60)-AV60,R60*AG60)),0)","v":0},{"$f":"IF(AF60=3,IF($AF$2=2,(S60/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I60,Refurb_Poss_Tbl[%]))*AG60,IF($AF$2=3,(S60*AG60)-AX60,S60*AG60)),0)","v":0},{"$f":"IF($AF60=3,IF($AF$2=2,(T60/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I60,Refurb_Poss_Tbl[%]))*AG60,T60*$AG60),0)","v":0},{"$f":"IF($AF60=3,IF($AF$2=2,(Q60/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I60,Refurb_Poss_Tbl[%]))*AG60,Q60*$AG60),0)","v":0},{"$f":"IF($AF60=3,IF($AF$2=2,(U60/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I60,Refurb_Poss_Tbl[%]))*AG60,U60*$AG60),0)","v":0},{"$f":"IF($AF60=3,IF($AF$2=2,(V60/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I60,Refurb_Poss_Tbl[%]))*AG60,IF($AF$2=3,(V60*AG60)-AW60,V60*AG60)),0)","v":0},{"$f":"IF($AF60=3,IF($AF$2=2,(W60/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I60,Refurb_Poss_Tbl[%]))*AG60,W60*$AG60),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,59,0,{"$f":"VLOOKUP(AE61,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.17482508271691022},0,0,0,0,0,0,0,0,9.5992171860812669E-3,{"$f":"IF(OR(AF61=3,AF61=2,AF61=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D61,FlatMaint!$Y$2:$Y$10000,AE61)*AG61,0)","v":15.448615489770358},{"$f":"IF(OR(AF61=3,AF61=2,AF61=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D61,FlatRepair!$Y$2:$Y$10000,AE61)*AG61,0)","v":0},0,15.45821470695644,0,0,0,0,0,15.45821470695644,0,{"$f":"IF($AF61=3,IF($AF$2=2,(R61/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I61,Refurb_Poss_Tbl[%]))*AG61,IF($AF$2=3,(R61*AG61)-AV61,R61*AG61)),0)","v":0},{"$f":"IF(AF61=3,IF($AF$2=2,(S61/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I61,Refurb_Poss_Tbl[%]))*AG61,IF($AF$2=3,(S61*AG61)-AX61,S61*AG61)),0)","v":0},{"$f":"IF($AF61=3,IF($AF$2=2,(T61/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I61,Refurb_Poss_Tbl[%]))*AG61,T61*$AG61),0)","v":0},{"$f":"IF($AF61=3,IF($AF$2=2,(Q61/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I61,Refurb_Poss_Tbl[%]))*AG61,Q61*$AG61),0)","v":0},{"$f":"IF($AF61=3,IF($AF$2=2,(U61/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I61,Refurb_Poss_Tbl[%]))*AG61,U61*$AG61),0)","v":0},{"$f":"IF($AF61=3,IF($AF$2=2,(V61/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I61,Refurb_Poss_Tbl[%]))*AG61,IF($AF$2=3,(V61*AG61)-AW61,V61*AG61)),0)","v":0},{"$f":"IF($AF61=3,IF($AF$2=2,(W61/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I61,Refurb_Poss_Tbl[%]))*AG61,W61*$AG61),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,60,3,{"$f":"VLOOKUP(AE62,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1697330900164177},0,0,0,0,0,0,0,0,9.3196283360012303E-3,{"$f":"IF(OR(AF62=3,AF62=2,AF62=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D62,FlatMaint!$Y$2:$Y$10000,AE62)*AG62,0)","v":14.998655815311029},{"$f":"IF(OR(AF62=3,AF62=2,AF62=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D62,FlatRepair!$Y$2:$Y$10000,AE62)*AG62,0)","v":0},0,15.00797544364703,0,0.38905510449922837,1.0985910777839118E-2,0.4160579884457935,151.95308675101666,167.77716119838655,0,{"$f":"IF($AF62=3,IF($AF$2=2,(R62/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I62,Refurb_Poss_Tbl[%]))*AG62,IF($AF$2=3,(R62*AG62)-AV62,R62*AG62)),0)","v":0.18232327190580255},{"$f":"IF(AF62=3,IF($AF$2=2,(S62/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I62,Refurb_Poss_Tbl[%]))*AG62,IF($AF$2=3,(S62*AG62)-AX62,S62*AG62)),0)","v":0.83211597689158878},{"$f":"IF($AF62=3,IF($AF$2=2,(T62/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I62,Refurb_Poss_Tbl[%]))*AG62,T62*$AG62),0)","v":2.1971821555678273E-2},{"$f":"IF($AF62=3,IF($AF$2=2,(Q62/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I62,Refurb_Poss_Tbl[%]))*AG62,Q62*$AG62),0)","v":149.96061078746118},{"$f":"IF($AF62=3,IF($AF$2=2,(U62/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I62,Refurb_Poss_Tbl[%]))*AG62,U62*$AG62),0)","v":0.93558830875509447},{"$f":"IF($AF62=3,IF($AF$2=2,(V62/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I62,Refurb_Poss_Tbl[%]))*AG62,IF($AF$2=3,(V62*AG62)-AW62,V62*AG62)),0)","v":0},{"$f":"IF($AF62=3,IF($AF$2=2,(W62/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I62,Refurb_Poss_Tbl[%]))*AG62,W62*$AG62),0)","v":2.0476584447327799E-2}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,61,0,{"$f":"VLOOKUP(AE63,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.16478940778292983},0,0,0,0,0,0,0,0,9.0481828504866326E-3,{"$f":"IF(OR(AF63=3,AF63=2,AF63=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D63,FlatMaint!$Y$2:$Y$10000,AE63)*AG63,0)","v":14.561801762437895},{"$f":"IF(OR(AF63=3,AF63=2,AF63=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D63,FlatRepair!$Y$2:$Y$10000,AE63)*AG63,0)","v":0},0,14.570849945288382,0,0,0,0,0,14.570849945288382,0,{"$f":"IF($AF63=3,IF($AF$2=2,(R63/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I63,Refurb_Poss_Tbl[%]))*AG63,IF($AF$2=3,(R63*AG63)-AV63,R63*AG63)),0)","v":0},{"$f":"IF(AF63=3,IF($AF$2=2,(S63/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I63,Refurb_Poss_Tbl[%]))*AG63,IF($AF$2=3,(S63*AG63)-AX63,S63*AG63)),0)","v":0},{"$f":"IF($AF63=3,IF($AF$2=2,(T63/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I63,Refurb_Poss_Tbl[%]))*AG63,T63*$AG63),0)","v":0},{"$f":"IF($AF63=3,IF($AF$2=2,(Q63/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I63,Refurb_Poss_Tbl[%]))*AG63,Q63*$AG63),0)","v":0},{"$f":"IF($AF63=3,IF($AF$2=2,(U63/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I63,Refurb_Poss_Tbl[%]))*AG63,U63*$AG63),0)","v":0},{"$f":"IF($AF63=3,IF($AF$2=2,(V63/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I63,Refurb_Poss_Tbl[%]))*AG63,IF($AF$2=3,(V63*AG63)-AW63,V63*AG63)),0)","v":0},{"$f":"IF($AF63=3,IF($AF$2=2,(W63/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I63,Refurb_Poss_Tbl[%]))*AG63,W63*$AG63),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,62,0,{"$f":"VLOOKUP(AE64,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15998971629410663},0,0,0,0,0,0,0,0,8.7846435441617798E-3,{"$f":"IF(OR(AF64=3,AF64=2,AF64=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D64,FlatMaint!$Y$2:$Y$10000,AE64)*AG64,0)","v":14.137671614017373},{"$f":"IF(OR(AF64=3,AF64=2,AF64=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D64,FlatRepair!$Y$2:$Y$10000,AE64)*AG64,0)","v":0},0,14.146456257561535,0,0,0,0,0,14.146456257561535,0,{"$f":"IF($AF64=3,IF($AF$2=2,(R64/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I64,Refurb_Poss_Tbl[%]))*AG64,IF($AF$2=3,(R64*AG64)-AV64,R64*AG64)),0)","v":0},{"$f":"IF(AF64=3,IF($AF$2=2,(S64/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I64,Refurb_Poss_Tbl[%]))*AG64,IF($AF$2=3,(S64*AG64)-AX64,S64*AG64)),0)","v":0},{"$f":"IF($AF64=3,IF($AF$2=2,(T64/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I64,Refurb_Poss_Tbl[%]))*AG64,T64*$AG64),0)","v":0},{"$f":"IF($AF64=3,IF($AF$2=2,(Q64/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I64,Refurb_Poss_Tbl[%]))*AG64,Q64*$AG64),0)","v":0},{"$f":"IF($AF64=3,IF($AF$2=2,(U64/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I64,Refurb_Poss_Tbl[%]))*AG64,U64*$AG64),0)","v":0},{"$f":"IF($AF64=3,IF($AF$2=2,(V64/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I64,Refurb_Poss_Tbl[%]))*AG64,IF($AF$2=3,(V64*AG64)-AW64,V64*AG64)),0)","v":0},{"$f":"IF($AF64=3,IF($AF$2=2,(W64/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I64,Refurb_Poss_Tbl[%]))*AG64,W64*$AG64),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,63,0,{"$f":"VLOOKUP(AE65,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15532982164476369},0,0,0,0,0,0,0,0,8.5287801399628899E-3,{"$f":"IF(OR(AF65=3,AF65=2,AF65=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D65,FlatMaint!$Y$2:$Y$10000,AE65)*AG65,0)","v":13.725894770890651},{"$f":"IF(OR(AF65=3,AF65=2,AF65=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D65,FlatRepair!$Y$2:$Y$10000,AE65)*AG65,0)","v":0},0,13.734423551030615,0,0,0,0,0,13.734423551030615,0,{"$f":"IF($AF65=3,IF($AF$2=2,(R65/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I65,Refurb_Poss_Tbl[%]))*AG65,IF($AF$2=3,(R65*AG65)-AV65,R65*AG65)),0)","v":0},{"$f":"IF(AF65=3,IF($AF$2=2,(S65/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I65,Refurb_Poss_Tbl[%]))*AG65,IF($AF$2=3,(S65*AG65)-AX65,S65*AG65)),0)","v":0},{"$f":"IF($AF65=3,IF($AF$2=2,(T65/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I65,Refurb_Poss_Tbl[%]))*AG65,T65*$AG65),0)","v":0},{"$f":"IF($AF65=3,IF($AF$2=2,(Q65/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I65,Refurb_Poss_Tbl[%]))*AG65,Q65*$AG65),0)","v":0},{"$f":"IF($AF65=3,IF($AF$2=2,(U65/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I65,Refurb_Poss_Tbl[%]))*AG65,U65*$AG65),0)","v":0},{"$f":"IF($AF65=3,IF($AF$2=2,(V65/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I65,Refurb_Poss_Tbl[%]))*AG65,IF($AF$2=3,(V65*AG65)-AW65,V65*AG65)),0)","v":0},{"$f":"IF($AF65=3,IF($AF$2=2,(W65/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I65,Refurb_Poss_Tbl[%]))*AG65,W65*$AG65),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,64,0,{"$f":"VLOOKUP(AE66,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15080565208229488},0,0,0,0,0,0,0,0,8.2803690679251387E-3,{"$f":"IF(OR(AF66=3,AF66=2,AF66=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D66,FlatMaint!$Y$2:$Y$10000,AE66)*AG66,0)","v":13.326111428049179},{"$f":"IF(OR(AF66=3,AF66=2,AF66=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D66,FlatRepair!$Y$2:$Y$10000,AE66)*AG66,0)","v":0},0,13.334391797117105,0,0,0,0,0,13.334391797117105,0,{"$f":"IF($AF66=3,IF($AF$2=2,(R66/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I66,Refurb_Poss_Tbl[%]))*AG66,IF($AF$2=3,(R66*AG66)-AV66,R66*AG66)),0)","v":0},{"$f":"IF(AF66=3,IF($AF$2=2,(S66/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I66,Refurb_Poss_Tbl[%]))*AG66,IF($AF$2=3,(S66*AG66)-AX66,S66*AG66)),0)","v":0},{"$f":"IF($AF66=3,IF($AF$2=2,(T66/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I66,Refurb_Poss_Tbl[%]))*AG66,T66*$AG66),0)","v":0},{"$f":"IF($AF66=3,IF($AF$2=2,(Q66/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I66,Refurb_Poss_Tbl[%]))*AG66,Q66*$AG66),0)","v":0},{"$f":"IF($AF66=3,IF($AF$2=2,(U66/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I66,Refurb_Poss_Tbl[%]))*AG66,U66*$AG66),0)","v":0},{"$f":"IF($AF66=3,IF($AF$2=2,(V66/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I66,Refurb_Poss_Tbl[%]))*AG66,IF($AF$2=3,(V66*AG66)-AW66,V66*AG66)),0)","v":0},{"$f":"IF($AF66=3,IF($AF$2=2,(W66/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I66,Refurb_Poss_Tbl[%]))*AG66,W66*$AG66),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,65,0,{"$f":"VLOOKUP(AE67,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14641325444882999},{"$f":"IF(AE67=0,Q67*AG67,0)","v":0},{"$f":"IF(AE67=0,R67*AG67,0)","v":0},{"$f":"IF(AE67=0,S67*AG67,0)","v":0},{"$f":"IF(AE67=0,T67*AG67,0)","v":0},{"$f":"IF(AE67=0,U67*AG67,0)","v":0},{"$f":"IF(AE67=0,V67*AG67,0)","v":0},{"$f":"IF(AE67=0,W67*AG67,0)","v":0},{"$f":"IF(AE67=0,AH67+AI67+AJ67+AK67+AL67+AM67+AN67,0)","v":0},{"$f":"IF(OR(AF67=3,AF67=2,AF67=0),Y67*AG67,0)","v":8.0391932698302328E-3},{"$f":"IF(OR(AF67=3,AF67=2,AF67=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D67,FlatMaint!$Y$2:$Y$10000,AE67)*AG67,0)","v":12.937972260241922},{"$f":"IF(OR(AF67=3,AF67=2,AF67=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D67,FlatRepair!$Y$2:$Y$10000,AE67)*AG67,0)","v":0},{"$f":"IF(OR(AF67=3,AF67=2,AF67=0),Z67*AG67,0)","v":0},{"$f":"AP67+AQ67+AR67+AS67","v":12.946011453511753},{"$f":"IF(AF67=2,AA67*AG67,0)","v":0},{"$f":"IF(AF67=3,AB67*AG67,0)","v":0},{"$f":"IF(AF67=3,AC67*AG67,0)","v":0},{"$f":"IF(AF67=3,AD67*AG67,0)","v":0},{"$f":"IF($AF$2=3,BB67+BC67+BD67+BE67+BF67+BG67+BH67,BB67+BC67+BD67+BE67+BF67+BG67+BH67)","v":0},{"$f":"AO67+AT67+AU67+AV67+AW67+AX67+AY67+BA67","v":12.946011453511753},{"$f":"IFERROR(IF(AE67=100,IF(O67=3,(N67/H67)*(X67*AG67)*-1,(N67/M67)*(X67*AG67)*-1),0),0)","v":0},{"$f":"IF($AF67=3,IF($AF$2=2,(R67/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I67,Refurb_Poss_Tbl[%]))*AG67,IF($AF$2=3,(R67*AG67)-AV67,R67*AG67)),0)","v":0},{"$f":"IF(AF67=3,IF($AF$2=2,(S67/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I67,Refurb_Poss_Tbl[%]))*AG67,IF($AF$2=3,(S67*AG67)-AX67,S67*AG67)),0)","v":0},{"$f":"IF($AF67=3,IF($AF$2=2,(T67/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I67,Refurb_Poss_Tbl[%]))*AG67,T67*$AG67),0)","v":0},{"$f":"IF($AF67=3,IF($AF$2=2,(Q67/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I67,Refurb_Poss_Tbl[%]))*AG67,Q67*$AG67),0)","v":0},{"$f":"IF($AF67=3,IF($AF$2=2,(U67/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I67,Refurb_Poss_Tbl[%]))*AG67,U67*$AG67),0)","v":0},{"$f":"IF($AF67=3,IF($AF$2=2,(V67/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I67,Refurb_Poss_Tbl[%]))*AG67,IF($AF$2=3,(V67*AG67)-AW67,V67*AG67)),0)","v":0},{"$f":"IF($AF67=3,IF($AF$2=2,(W67/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I67,Refurb_Poss_Tbl[%]))*AG67,W67*$AG67),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,66,0,{"$f":"VLOOKUP(AE68,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14214879072701941},0,0,0,0,0,0,0,0,7.805042009543915E-3,{"$f":"IF(OR(AF68=3,AF68=2,AF68=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D68,FlatMaint!$Y$2:$Y$10000,AE68)*AG68,0)","v":12.56113811673973},{"$f":"IF(OR(AF68=3,AF68=2,AF68=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D68,FlatRepair!$Y$2:$Y$10000,AE68)*AG68,0)","v":0},0,12.568943158749274,0,0,0,0,0,12.568943158749274,0,{"$f":"IF($AF68=3,IF($AF$2=2,(R68/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I68,Refurb_Poss_Tbl[%]))*AG68,IF($AF$2=3,(R68*AG68)-AV68,R68*AG68)),0)","v":0},{"$f":"IF(AF68=3,IF($AF$2=2,(S68/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I68,Refurb_Poss_Tbl[%]))*AG68,IF($AF$2=3,(S68*AG68)-AX68,S68*AG68)),0)","v":0},{"$f":"IF($AF68=3,IF($AF$2=2,(T68/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I68,Refurb_Poss_Tbl[%]))*AG68,T68*$AG68),0)","v":0},{"$f":"IF($AF68=3,IF($AF$2=2,(Q68/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I68,Refurb_Poss_Tbl[%]))*AG68,Q68*$AG68),0)","v":0},{"$f":"IF($AF68=3,IF($AF$2=2,(U68/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I68,Refurb_Poss_Tbl[%]))*AG68,U68*$AG68),0)","v":0},{"$f":"IF($AF68=3,IF($AF$2=2,(V68/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I68,Refurb_Poss_Tbl[%]))*AG68,IF($AF$2=3,(V68*AG68)-AW68,V68*AG68)),0)","v":0},{"$f":"IF($AF68=3,IF($AF$2=2,(W68/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I68,Refurb_Poss_Tbl[%]))*AG68,W68*$AG68),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,67,0,{"$f":"VLOOKUP(AE69,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1380085346864266},0,0,0,0,0,0,0,0,7.5777106888775866E-3,{"$f":"IF(OR(AF69=3,AF69=2,AF69=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D69,FlatMaint!$Y$2:$Y$10000,AE69)*AG69,0)","v":12.195279724990028},{"$f":"IF(OR(AF69=3,AF69=2,AF69=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D69,FlatRepair!$Y$2:$Y$10000,AE69)*AG69,0)","v":0},0,12.202857435678906,0,0,0,0,0,12.202857435678906,0,{"$f":"IF($AF69=3,IF($AF$2=2,(R69/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I69,Refurb_Poss_Tbl[%]))*AG69,IF($AF$2=3,(R69*AG69)-AV69,R69*AG69)),0)","v":0},{"$f":"IF(AF69=3,IF($AF$2=2,(S69/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I69,Refurb_Poss_Tbl[%]))*AG69,IF($AF$2=3,(S69*AG69)-AX69,S69*AG69)),0)","v":0},{"$f":"IF($AF69=3,IF($AF$2=2,(T69/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I69,Refurb_Poss_Tbl[%]))*AG69,T69*$AG69),0)","v":0},{"$f":"IF($AF69=3,IF($AF$2=2,(Q69/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I69,Refurb_Poss_Tbl[%]))*AG69,Q69*$AG69),0)","v":0},{"$f":"IF($AF69=3,IF($AF$2=2,(U69/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I69,Refurb_Poss_Tbl[%]))*AG69,U69*$AG69),0)","v":0},{"$f":"IF($AF69=3,IF($AF$2=2,(V69/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I69,Refurb_Poss_Tbl[%]))*AG69,IF($AF$2=3,(V69*AG69)-AW69,V69*AG69)),0)","v":0},{"$f":"IF($AF69=3,IF($AF$2=2,(W69/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I69,Refurb_Poss_Tbl[%]))*AG69,W69*$AG69),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,68,0,{"$f":"VLOOKUP(AE70,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13398886862759865},0,0,0,0,0,0,0,0,7.3570006688131913E-3,{"$f":"IF(OR(AF70=3,AF70=2,AF70=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D70,FlatMaint!$Y$2:$Y$10000,AE70)*AG70,0)","v":11.84007740290294},{"$f":"IF(OR(AF70=3,AF70=2,AF70=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D70,FlatRepair!$Y$2:$Y$10000,AE70)*AG70,0)","v":0},0,11.847434403571754,0,0,0,0,0,11.847434403571754,0,{"$f":"IF($AF70=3,IF($AF$2=2,(R70/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I70,Refurb_Poss_Tbl[%]))*AG70,IF($AF$2=3,(R70*AG70)-AV70,R70*AG70)),0)","v":0},{"$f":"IF(AF70=3,IF($AF$2=2,(S70/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I70,Refurb_Poss_Tbl[%]))*AG70,IF($AF$2=3,(S70*AG70)-AX70,S70*AG70)),0)","v":0},{"$f":"IF($AF70=3,IF($AF$2=2,(T70/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I70,Refurb_Poss_Tbl[%]))*AG70,T70*$AG70),0)","v":0},{"$f":"IF($AF70=3,IF($AF$2=2,(Q70/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I70,Refurb_Poss_Tbl[%]))*AG70,Q70*$AG70),0)","v":0},{"$f":"IF($AF70=3,IF($AF$2=2,(U70/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I70,Refurb_Poss_Tbl[%]))*AG70,U70*$AG70),0)","v":0},{"$f":"IF($AF70=3,IF($AF$2=2,(V70/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I70,Refurb_Poss_Tbl[%]))*AG70,IF($AF$2=3,(V70*AG70)-AW70,V70*AG70)),0)","v":0},{"$f":"IF($AF70=3,IF($AF$2=2,(W70/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I70,Refurb_Poss_Tbl[%]))*AG70,W70*$AG70),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,69,0,{"$f":"VLOOKUP(AE71,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13008628022096957},0,0,0,0,0,0,0,0,7.1427190959351379E-3,{"$f":"IF(OR(AF71=3,AF71=2,AF71=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D71,FlatMaint!$Y$2:$Y$10000,AE71)*AG71,0)","v":11.495220779517419},{"$f":"IF(OR(AF71=3,AF71=2,AF71=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D71,FlatRepair!$Y$2:$Y$10000,AE71)*AG71,0)","v":0},0,11.502363498613354,0,0,0,0,0,11.502363498613354,0,{"$f":"IF($AF71=3,IF($AF$2=2,(R71/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I71,Refurb_Poss_Tbl[%]))*AG71,IF($AF$2=3,(R71*AG71)-AV71,R71*AG71)),0)","v":0},{"$f":"IF(AF71=3,IF($AF$2=2,(S71/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I71,Refurb_Poss_Tbl[%]))*AG71,IF($AF$2=3,(S71*AG71)-AX71,S71*AG71)),0)","v":0},{"$f":"IF($AF71=3,IF($AF$2=2,(T71/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I71,Refurb_Poss_Tbl[%]))*AG71,T71*$AG71),0)","v":0},{"$f":"IF($AF71=3,IF($AF$2=2,(Q71/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I71,Refurb_Poss_Tbl[%]))*AG71,Q71*$AG71),0)","v":0},{"$f":"IF($AF71=3,IF($AF$2=2,(U71/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I71,Refurb_Poss_Tbl[%]))*AG71,U71*$AG71),0)","v":0},{"$f":"IF($AF71=3,IF($AF$2=2,(V71/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I71,Refurb_Poss_Tbl[%]))*AG71,IF($AF$2=3,(V71*AG71)-AW71,V71*AG71)),0)","v":0},{"$f":"IF($AF71=3,IF($AF$2=2,(W71/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I71,Refurb_Poss_Tbl[%]))*AG71,W71*$AG71),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,70,0,{"$f":"VLOOKUP(AE72,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12629735943783454},0,0,0,0,0,0,0,0,6.9346787339176095E-3,{"$f":"IF(OR(AF72=3,AF72=2,AF72=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D72,FlatMaint!$Y$2:$Y$10000,AE72)*AG72,0)","v":11.160408523803321},{"$f":"IF(OR(AF72=3,AF72=2,AF72=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D72,FlatRepair!$Y$2:$Y$10000,AE72)*AG72,0)","v":0},0,11.167343202537239,0,0,0,0,0,11.167343202537239,0,{"$f":"IF($AF72=3,IF($AF$2=2,(R72/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I72,Refurb_Poss_Tbl[%]))*AG72,IF($AF$2=3,(R72*AG72)-AV72,R72*AG72)),0)","v":0},{"$f":"IF(AF72=3,IF($AF$2=2,(S72/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I72,Refurb_Poss_Tbl[%]))*AG72,IF($AF$2=3,(S72*AG72)-AX72,S72*AG72)),0)","v":0},{"$f":"IF($AF72=3,IF($AF$2=2,(T72/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I72,Refurb_Poss_Tbl[%]))*AG72,T72*$AG72),0)","v":0},{"$f":"IF($AF72=3,IF($AF$2=2,(Q72/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I72,Refurb_Poss_Tbl[%]))*AG72,Q72*$AG72),0)","v":0},{"$f":"IF($AF72=3,IF($AF$2=2,(U72/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I72,Refurb_Poss_Tbl[%]))*AG72,U72*$AG72),0)","v":0},{"$f":"IF($AF72=3,IF($AF$2=2,(V72/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I72,Refurb_Poss_Tbl[%]))*AG72,IF($AF$2=3,(V72*AG72)-AW72,V72*AG72)),0)","v":0},{"$f":"IF($AF72=3,IF($AF$2=2,(W72/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I72,Refurb_Poss_Tbl[%]))*AG72,W72*$AG72),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,71,0,{"$f":"VLOOKUP(AE73,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12261879557071313},0,0,0,0,0,0,0,0,6.7326977999200089E-3,{"$f":"IF(OR(AF73=3,AF73=2,AF73=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D73,FlatMaint!$Y$2:$Y$10000,AE73)*AG73,0)","v":10.835348081362445},{"$f":"IF(OR(AF73=3,AF73=2,AF73=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D73,FlatRepair!$Y$2:$Y$10000,AE73)*AG73,0)","v":0},0,10.842080779162366,0,0,0,0,0,10.842080779162366,0,{"$f":"IF($AF73=3,IF($AF$2=2,(R73/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I73,Refurb_Poss_Tbl[%]))*AG73,IF($AF$2=3,(R73*AG73)-AV73,R73*AG73)),0)","v":0},{"$f":"IF(AF73=3,IF($AF$2=2,(S73/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I73,Refurb_Poss_Tbl[%]))*AG73,IF($AF$2=3,(S73*AG73)-AX73,S73*AG73)),0)","v":0},{"$f":"IF($AF73=3,IF($AF$2=2,(T73/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I73,Refurb_Poss_Tbl[%]))*AG73,T73*$AG73),0)","v":0},{"$f":"IF($AF73=3,IF($AF$2=2,(Q73/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I73,Refurb_Poss_Tbl[%]))*AG73,Q73*$AG73),0)","v":0},{"$f":"IF($AF73=3,IF($AF$2=2,(U73/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I73,Refurb_Poss_Tbl[%]))*AG73,U73*$AG73),0)","v":0},{"$f":"IF($AF73=3,IF($AF$2=2,(V73/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I73,Refurb_Poss_Tbl[%]))*AG73,IF($AF$2=3,(V73*AG73)-AW73,V73*AG73)),0)","v":0},{"$f":"IF($AF73=3,IF($AF$2=2,(W73/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I73,Refurb_Poss_Tbl[%]))*AG73,W73*$AG73),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,72,0,{"$f":"VLOOKUP(AE74,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1190473743404982},0,0,0,0,0,0,0,0,6.5365998057475812E-3,{"$f":"IF(OR(AF74=3,AF74=2,AF74=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D74,FlatMaint!$Y$2:$Y$10000,AE74)*AG74,0)","v":10.519755418798491},{"$f":"IF(OR(AF74=3,AF74=2,AF74=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D74,FlatRepair!$Y$2:$Y$10000,AE74)*AG74,0)","v":0},0,10.526292018604238,0,0,0,0,0,10.526292018604238,0,{"$f":"IF($AF74=3,IF($AF$2=2,(R74/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I74,Refurb_Poss_Tbl[%]))*AG74,IF($AF$2=3,(R74*AG74)-AV74,R74*AG74)),0)","v":0},{"$f":"IF(AF74=3,IF($AF$2=2,(S74/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I74,Refurb_Poss_Tbl[%]))*AG74,IF($AF$2=3,(S74*AG74)-AX74,S74*AG74)),0)","v":0},{"$f":"IF($AF74=3,IF($AF$2=2,(T74/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I74,Refurb_Poss_Tbl[%]))*AG74,T74*$AG74),0)","v":0},{"$f":"IF($AF74=3,IF($AF$2=2,(Q74/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I74,Refurb_Poss_Tbl[%]))*AG74,Q74*$AG74),0)","v":0},{"$f":"IF($AF74=3,IF($AF$2=2,(U74/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I74,Refurb_Poss_Tbl[%]))*AG74,U74*$AG74),0)","v":0},{"$f":"IF($AF74=3,IF($AF$2=2,(V74/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I74,Refurb_Poss_Tbl[%]))*AG74,IF($AF$2=3,(V74*AG74)-AW74,V74*AG74)),0)","v":0},{"$f":"IF($AF74=3,IF($AF$2=2,(W74/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I74,Refurb_Poss_Tbl[%]))*AG74,W74*$AG74),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,73,0,{"$f":"VLOOKUP(AE75,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11557997508786232},0,0,0,0,0,0,0,0,6.3462134036384281E-3,{"$f":"IF(OR(AF75=3,AF75=2,AF75=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D75,FlatMaint!$Y$2:$Y$10000,AE75)*AG75,0)","v":10.213354775532515},{"$f":"IF(OR(AF75=3,AF75=2,AF75=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D75,FlatRepair!$Y$2:$Y$10000,AE75)*AG75,0)","v":0},0,10.219700988936154,0,0,0,0,0,10.219700988936154,0,{"$f":"IF($AF75=3,IF($AF$2=2,(R75/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I75,Refurb_Poss_Tbl[%]))*AG75,IF($AF$2=3,(R75*AG75)-AV75,R75*AG75)),0)","v":0},{"$f":"IF(AF75=3,IF($AF$2=2,(S75/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I75,Refurb_Poss_Tbl[%]))*AG75,IF($AF$2=3,(S75*AG75)-AX75,S75*AG75)),0)","v":0},{"$f":"IF($AF75=3,IF($AF$2=2,(T75/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I75,Refurb_Poss_Tbl[%]))*AG75,T75*$AG75),0)","v":0},{"$f":"IF($AF75=3,IF($AF$2=2,(Q75/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I75,Refurb_Poss_Tbl[%]))*AG75,Q75*$AG75),0)","v":0},{"$f":"IF($AF75=3,IF($AF$2=2,(U75/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I75,Refurb_Poss_Tbl[%]))*AG75,U75*$AG75),0)","v":0},{"$f":"IF($AF75=3,IF($AF$2=2,(V75/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I75,Refurb_Poss_Tbl[%]))*AG75,IF($AF$2=3,(V75*AG75)-AW75,V75*AG75)),0)","v":0},{"$f":"IF($AF75=3,IF($AF$2=2,(W75/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I75,Refurb_Poss_Tbl[%]))*AG75,W75*$AG75),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,74,0,{"$f":"VLOOKUP(AE76,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11221356804646829},0,0,0,0,0,0,0,0,6.1613722365421644E-3,{"$f":"IF(OR(AF76=3,AF76=2,AF76=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D76,FlatMaint!$Y$2:$Y$10000,AE76)*AG76,0)","v":9.9158784228471042},{"$f":"IF(OR(AF76=3,AF76=2,AF76=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D76,FlatRepair!$Y$2:$Y$10000,AE76)*AG76,0)","v":0},0,9.9220397950836468,0,0,0,0,0,9.9220397950836468,0,{"$f":"IF($AF76=3,IF($AF$2=2,(R76/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I76,Refurb_Poss_Tbl[%]))*AG76,IF($AF$2=3,(R76*AG76)-AV76,R76*AG76)),0)","v":0},{"$f":"IF(AF76=3,IF($AF$2=2,(S76/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I76,Refurb_Poss_Tbl[%]))*AG76,IF($AF$2=3,(S76*AG76)-AX76,S76*AG76)),0)","v":0},{"$f":"IF($AF76=3,IF($AF$2=2,(T76/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I76,Refurb_Poss_Tbl[%]))*AG76,T76*$AG76),0)","v":0},{"$f":"IF($AF76=3,IF($AF$2=2,(Q76/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I76,Refurb_Poss_Tbl[%]))*AG76,Q76*$AG76),0)","v":0},{"$f":"IF($AF76=3,IF($AF$2=2,(U76/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I76,Refurb_Poss_Tbl[%]))*AG76,U76*$AG76),0)","v":0},{"$f":"IF($AF76=3,IF($AF$2=2,(V76/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I76,Refurb_Poss_Tbl[%]))*AG76,IF($AF$2=3,(V76*AG76)-AW76,V76*AG76)),0)","v":0},{"$f":"IF($AF76=3,IF($AF$2=2,(W76/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I76,Refurb_Poss_Tbl[%]))*AG76,W76*$AG76),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,75,0,{"$f":"VLOOKUP(AE77,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10894521169560026},0,0,0,0,0,0,0,0,5.9819147927593821E-3,{"$f":"IF(OR(AF77=3,AF77=2,AF77=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D77,FlatMaint!$Y$2:$Y$10000,AE77)*AG77,0)","v":9.627066429948643},{"$f":"IF(OR(AF77=3,AF77=2,AF77=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D77,FlatRepair!$Y$2:$Y$10000,AE77)*AG77,0)","v":0},0,9.6330483447414021,0,0,0,0,0,9.6330483447414021,0,{"$f":"IF($AF77=3,IF($AF$2=2,(R77/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I77,Refurb_Poss_Tbl[%]))*AG77,IF($AF$2=3,(R77*AG77)-AV77,R77*AG77)),0)","v":0},{"$f":"IF(AF77=3,IF($AF$2=2,(S77/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I77,Refurb_Poss_Tbl[%]))*AG77,IF($AF$2=3,(S77*AG77)-AX77,S77*AG77)),0)","v":0},{"$f":"IF($AF77=3,IF($AF$2=2,(T77/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I77,Refurb_Poss_Tbl[%]))*AG77,T77*$AG77),0)","v":0},{"$f":"IF($AF77=3,IF($AF$2=2,(Q77/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I77,Refurb_Poss_Tbl[%]))*AG77,Q77*$AG77),0)","v":0},{"$f":"IF($AF77=3,IF($AF$2=2,(U77/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I77,Refurb_Poss_Tbl[%]))*AG77,U77*$AG77),0)","v":0},{"$f":"IF($AF77=3,IF($AF$2=2,(V77/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I77,Refurb_Poss_Tbl[%]))*AG77,IF($AF$2=3,(V77*AG77)-AW77,V77*AG77)),0)","v":0},{"$f":"IF($AF77=3,IF($AF$2=2,(W77/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I77,Refurb_Poss_Tbl[%]))*AG77,W77*$AG77),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,76,0,{"$f":"VLOOKUP(AE78,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15310389176729922},0,0,0,0,0,0,0,0,8.4065597811750839E-3,{"$f":"IF(OR(AF78=3,AF78=2,AF78=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D78,FlatMaint!$Y$2:$Y$10000,AE78)*AG78,0)","v":13.529197968293834},{"$f":"IF(OR(AF78=3,AF78=2,AF78=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D78,FlatRepair!$Y$2:$Y$10000,AE78)*AG78,0)","v":0},0,13.537604528075009,0,0,0,0,0,13.537604528075009,0,{"$f":"IF($AF78=3,IF($AF$2=2,(R78/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I78,Refurb_Poss_Tbl[%]))*AG78,IF($AF$2=3,(R78*AG78)-AV78,R78*AG78)),0)","v":0},{"$f":"IF(AF78=3,IF($AF$2=2,(S78/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I78,Refurb_Poss_Tbl[%]))*AG78,IF($AF$2=3,(S78*AG78)-AX78,S78*AG78)),0)","v":0},{"$f":"IF($AF78=3,IF($AF$2=2,(T78/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I78,Refurb_Poss_Tbl[%]))*AG78,T78*$AG78),0)","v":0},{"$f":"IF($AF78=3,IF($AF$2=2,(Q78/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I78,Refurb_Poss_Tbl[%]))*AG78,Q78*$AG78),0)","v":0},{"$f":"IF($AF78=3,IF($AF$2=2,(U78/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I78,Refurb_Poss_Tbl[%]))*AG78,U78*$AG78),0)","v":0},{"$f":"IF($AF78=3,IF($AF$2=2,(V78/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I78,Refurb_Poss_Tbl[%]))*AG78,IF($AF$2=3,(V78*AG78)-AW78,V78*AG78)),0)","v":0},{"$f":"IF($AF78=3,IF($AF$2=2,(W78/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I78,Refurb_Poss_Tbl[%]))*AG78,W78*$AG78),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,77,0,{"$f":"VLOOKUP(AE79,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14936965050468218},0,0,0,0,0,0,0,0,8.2015217377317904E-3,{"$f":"IF(OR(AF79=3,AF79=2,AF79=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D79,FlatMaint!$Y$2:$Y$10000,AE79)*AG79,0)","v":13.199217530042766},{"$f":"IF(OR(AF79=3,AF79=2,AF79=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D79,FlatRepair!$Y$2:$Y$10000,AE79)*AG79,0)","v":0},0,13.207419051780498,0,0,0,0,0,13.207419051780498,0,{"$f":"IF($AF79=3,IF($AF$2=2,(R79/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I79,Refurb_Poss_Tbl[%]))*AG79,IF($AF$2=3,(R79*AG79)-AV79,R79*AG79)),0)","v":0},{"$f":"IF(AF79=3,IF($AF$2=2,(S79/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I79,Refurb_Poss_Tbl[%]))*AG79,IF($AF$2=3,(S79*AG79)-AX79,S79*AG79)),0)","v":0},{"$f":"IF($AF79=3,IF($AF$2=2,(T79/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I79,Refurb_Poss_Tbl[%]))*AG79,T79*$AG79),0)","v":0},{"$f":"IF($AF79=3,IF($AF$2=2,(Q79/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I79,Refurb_Poss_Tbl[%]))*AG79,Q79*$AG79),0)","v":0},{"$f":"IF($AF79=3,IF($AF$2=2,(U79/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I79,Refurb_Poss_Tbl[%]))*AG79,U79*$AG79),0)","v":0},{"$f":"IF($AF79=3,IF($AF$2=2,(V79/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I79,Refurb_Poss_Tbl[%]))*AG79,IF($AF$2=3,(V79*AG79)-AW79,V79*AG79)),0)","v":0},{"$f":"IF($AF79=3,IF($AF$2=2,(W79/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I79,Refurb_Poss_Tbl[%]))*AG79,W79*$AG79),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,78,0,{"$f":"VLOOKUP(AE80,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14572648829725093},0,0,0,0,0,0,0,0,8.0014846221773579E-3,{"$f":"IF(OR(AF80=3,AF80=2,AF80=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D80,FlatMaint!$Y$2:$Y$10000,AE80)*AG80,0)","v":12.877285395163677},{"$f":"IF(OR(AF80=3,AF80=2,AF80=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D80,FlatRepair!$Y$2:$Y$10000,AE80)*AG80,0)","v":0},0,12.885286879785854,0,0,0,0,0,12.885286879785854,0,{"$f":"IF($AF80=3,IF($AF$2=2,(R80/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I80,Refurb_Poss_Tbl[%]))*AG80,IF($AF$2=3,(R80*AG80)-AV80,R80*AG80)),0)","v":0},{"$f":"IF(AF80=3,IF($AF$2=2,(S80/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I80,Refurb_Poss_Tbl[%]))*AG80,IF($AF$2=3,(S80*AG80)-AX80,S80*AG80)),0)","v":0},{"$f":"IF($AF80=3,IF($AF$2=2,(T80/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I80,Refurb_Poss_Tbl[%]))*AG80,T80*$AG80),0)","v":0},{"$f":"IF($AF80=3,IF($AF$2=2,(Q80/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I80,Refurb_Poss_Tbl[%]))*AG80,Q80*$AG80),0)","v":0},{"$f":"IF($AF80=3,IF($AF$2=2,(U80/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I80,Refurb_Poss_Tbl[%]))*AG80,U80*$AG80),0)","v":0},{"$f":"IF($AF80=3,IF($AF$2=2,(V80/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I80,Refurb_Poss_Tbl[%]))*AG80,IF($AF$2=3,(V80*AG80)-AW80,V80*AG80)),0)","v":0},{"$f":"IF($AF80=3,IF($AF$2=2,(W80/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I80,Refurb_Poss_Tbl[%]))*AG80,W80*$AG80),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,79,0,{"$f":"VLOOKUP(AE81,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14217218370463502},0,0,0,0,0,0,0,0,7.8063264606608347E-3,{"$f":"IF(OR(AF81=3,AF81=2,AF81=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D81,FlatMaint!$Y$2:$Y$10000,AE81)*AG81,0)","v":12.563205263574316},{"$f":"IF(OR(AF81=3,AF81=2,AF81=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D81,FlatRepair!$Y$2:$Y$10000,AE81)*AG81,0)","v":0},0,12.571011590034978,0,0,0,0,0,12.571011590034978,0,{"$f":"IF($AF81=3,IF($AF$2=2,(R81/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I81,Refurb_Poss_Tbl[%]))*AG81,IF($AF$2=3,(R81*AG81)-AV81,R81*AG81)),0)","v":0},{"$f":"IF(AF81=3,IF($AF$2=2,(S81/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I81,Refurb_Poss_Tbl[%]))*AG81,IF($AF$2=3,(S81*AG81)-AX81,S81*AG81)),0)","v":0},{"$f":"IF($AF81=3,IF($AF$2=2,(T81/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I81,Refurb_Poss_Tbl[%]))*AG81,T81*$AG81),0)","v":0},{"$f":"IF($AF81=3,IF($AF$2=2,(Q81/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I81,Refurb_Poss_Tbl[%]))*AG81,Q81*$AG81),0)","v":0},{"$f":"IF($AF81=3,IF($AF$2=2,(U81/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I81,Refurb_Poss_Tbl[%]))*AG81,U81*$AG81),0)","v":0},{"$f":"IF($AF81=3,IF($AF$2=2,(V81/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I81,Refurb_Poss_Tbl[%]))*AG81,IF($AF$2=3,(V81*AG81)-AW81,V81*AG81)),0)","v":0},{"$f":"IF($AF81=3,IF($AF$2=2,(W81/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I81,Refurb_Poss_Tbl[%]))*AG81,W81*$AG81),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,80,2,{"$f":"VLOOKUP(AE82,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13870456946793663},0,0,0,0,0,0,0,0,7.6159282543032548E-3,{"$f":"IF(OR(AF82=3,AF82=2,AF82=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D82,FlatMaint!$Y$2:$Y$10000,AE82)*AG82,0)","v":12.256785622999335},{"$f":"IF(OR(AF82=3,AF82=2,AF82=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D82,FlatRepair!$Y$2:$Y$10000,AE82)*AG82,0)","v":0},0,12.264401551253638,31.04372205072848,0,0,0,0,43.308123601982118,0,{"$f":"IF($AF82=3,IF($AF$2=2,(R82/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I82,Refurb_Poss_Tbl[%]))*AG82,IF($AF$2=3,(R82*AG82)-AV82,R82*AG82)),0)","v":0},{"$f":"IF(AF82=3,IF($AF$2=2,(S82/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I82,Refurb_Poss_Tbl[%]))*AG82,IF($AF$2=3,(S82*AG82)-AX82,S82*AG82)),0)","v":0},{"$f":"IF($AF82=3,IF($AF$2=2,(T82/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I82,Refurb_Poss_Tbl[%]))*AG82,T82*$AG82),0)","v":0},{"$f":"IF($AF82=3,IF($AF$2=2,(Q82/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I82,Refurb_Poss_Tbl[%]))*AG82,Q82*$AG82),0)","v":0},{"$f":"IF($AF82=3,IF($AF$2=2,(U82/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I82,Refurb_Poss_Tbl[%]))*AG82,U82*$AG82),0)","v":0},{"$f":"IF($AF82=3,IF($AF$2=2,(V82/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I82,Refurb_Poss_Tbl[%]))*AG82,IF($AF$2=3,(V82*AG82)-AW82,V82*AG82)),0)","v":0},{"$f":"IF($AF82=3,IF($AF$2=2,(W82/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I82,Refurb_Poss_Tbl[%]))*AG82,W82*$AG82),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,81,0,{"$f":"VLOOKUP(AE83,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13532153118823087},0,0,0,0,0,0,0,0,7.4301739066373225E-3,{"$f":"IF(OR(AF83=3,AF83=2,AF83=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D83,FlatMaint!$Y$2:$Y$10000,AE83)*AG83,0)","v":11.957839632194473},{"$f":"IF(OR(AF83=3,AF83=2,AF83=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D83,FlatRepair!$Y$2:$Y$10000,AE83)*AG83,0)","v":0},0,11.96526980610111,0,0,0,0,0,11.96526980610111,0,{"$f":"IF($AF83=3,IF($AF$2=2,(R83/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I83,Refurb_Poss_Tbl[%]))*AG83,IF($AF$2=3,(R83*AG83)-AV83,R83*AG83)),0)","v":0},{"$f":"IF(AF83=3,IF($AF$2=2,(S83/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I83,Refurb_Poss_Tbl[%]))*AG83,IF($AF$2=3,(S83*AG83)-AX83,S83*AG83)),0)","v":0},{"$f":"IF($AF83=3,IF($AF$2=2,(T83/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I83,Refurb_Poss_Tbl[%]))*AG83,T83*$AG83),0)","v":0},{"$f":"IF($AF83=3,IF($AF$2=2,(Q83/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I83,Refurb_Poss_Tbl[%]))*AG83,Q83*$AG83),0)","v":0},{"$f":"IF($AF83=3,IF($AF$2=2,(U83/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I83,Refurb_Poss_Tbl[%]))*AG83,U83*$AG83),0)","v":0},{"$f":"IF($AF83=3,IF($AF$2=2,(V83/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I83,Refurb_Poss_Tbl[%]))*AG83,IF($AF$2=3,(V83*AG83)-AW83,V83*AG83)),0)","v":0},{"$f":"IF($AF83=3,IF($AF$2=2,(W83/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I83,Refurb_Poss_Tbl[%]))*AG83,W83*$AG83),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,82,0,{"$f":"VLOOKUP(AE84,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13202100603729841},0,0,0,0,0,0,0,0,7.2489501528169003E-3,{"$f":"IF(OR(AF84=3,AF84=2,AF84=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D84,FlatMaint!$Y$2:$Y$10000,AE84)*AG84,0)","v":11.666185007018999},{"$f":"IF(OR(AF84=3,AF84=2,AF84=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D84,FlatRepair!$Y$2:$Y$10000,AE84)*AG84,0)","v":0},0,11.673433957171817,0,0,0,0,0,11.673433957171817,0,{"$f":"IF($AF84=3,IF($AF$2=2,(R84/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I84,Refurb_Poss_Tbl[%]))*AG84,IF($AF$2=3,(R84*AG84)-AV84,R84*AG84)),0)","v":0},{"$f":"IF(AF84=3,IF($AF$2=2,(S84/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I84,Refurb_Poss_Tbl[%]))*AG84,IF($AF$2=3,(S84*AG84)-AX84,S84*AG84)),0)","v":0},{"$f":"IF($AF84=3,IF($AF$2=2,(T84/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I84,Refurb_Poss_Tbl[%]))*AG84,T84*$AG84),0)","v":0},{"$f":"IF($AF84=3,IF($AF$2=2,(Q84/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I84,Refurb_Poss_Tbl[%]))*AG84,Q84*$AG84),0)","v":0},{"$f":"IF($AF84=3,IF($AF$2=2,(U84/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I84,Refurb_Poss_Tbl[%]))*AG84,U84*$AG84),0)","v":0},{"$f":"IF($AF84=3,IF($AF$2=2,(V84/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I84,Refurb_Poss_Tbl[%]))*AG84,IF($AF$2=3,(V84*AG84)-AW84,V84*AG84)),0)","v":0},{"$f":"IF($AF84=3,IF($AF$2=2,(W84/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I84,Refurb_Poss_Tbl[%]))*AG84,W84*$AG84),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,83,0,{"$f":"VLOOKUP(AE85,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12880098149980332},0,0,0,0,0,0,0,0,7.0721464905530726E-3,{"$f":"IF(OR(AF85=3,AF85=2,AF85=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D85,FlatMaint!$Y$2:$Y$10000,AE85)*AG85,0)","v":11.381643909286828},{"$f":"IF(OR(AF85=3,AF85=2,AF85=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D85,FlatRepair!$Y$2:$Y$10000,AE85)*AG85,0)","v":0},0,11.388716055777381,0,0,0,0,0,11.388716055777381,0,{"$f":"IF($AF85=3,IF($AF$2=2,(R85/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I85,Refurb_Poss_Tbl[%]))*AG85,IF($AF$2=3,(R85*AG85)-AV85,R85*AG85)),0)","v":0},{"$f":"IF(AF85=3,IF($AF$2=2,(S85/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I85,Refurb_Poss_Tbl[%]))*AG85,IF($AF$2=3,(S85*AG85)-AX85,S85*AG85)),0)","v":0},{"$f":"IF($AF85=3,IF($AF$2=2,(T85/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I85,Refurb_Poss_Tbl[%]))*AG85,T85*$AG85),0)","v":0},{"$f":"IF($AF85=3,IF($AF$2=2,(Q85/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I85,Refurb_Poss_Tbl[%]))*AG85,Q85*$AG85),0)","v":0},{"$f":"IF($AF85=3,IF($AF$2=2,(U85/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I85,Refurb_Poss_Tbl[%]))*AG85,U85*$AG85),0)","v":0},{"$f":"IF($AF85=3,IF($AF$2=2,(V85/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I85,Refurb_Poss_Tbl[%]))*AG85,IF($AF$2=3,(V85*AG85)-AW85,V85*AG85)),0)","v":0},{"$f":"IF($AF85=3,IF($AF$2=2,(W85/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I85,Refurb_Poss_Tbl[%]))*AG85,W85*$AG85),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,84,0,{"$f":"VLOOKUP(AE86,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1256594941461496},0,0,0,0,0,0,0,0,6.8996551127347063E-3,{"$f":"IF(OR(AF86=3,AF86=2,AF86=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D86,FlatMaint!$Y$2:$Y$10000,AE86)*AG86,0)","v":11.104042838328613},{"$f":"IF(OR(AF86=3,AF86=2,AF86=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D86,FlatRepair!$Y$2:$Y$10000,AE86)*AG86,0)","v":0},0,11.110942493441348,0,0,0,0,0,11.110942493441348,0,{"$f":"IF($AF86=3,IF($AF$2=2,(R86/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I86,Refurb_Poss_Tbl[%]))*AG86,IF($AF$2=3,(R86*AG86)-AV86,R86*AG86)),0)","v":0},{"$f":"IF(AF86=3,IF($AF$2=2,(S86/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I86,Refurb_Poss_Tbl[%]))*AG86,IF($AF$2=3,(S86*AG86)-AX86,S86*AG86)),0)","v":0},{"$f":"IF($AF86=3,IF($AF$2=2,(T86/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I86,Refurb_Poss_Tbl[%]))*AG86,T86*$AG86),0)","v":0},{"$f":"IF($AF86=3,IF($AF$2=2,(Q86/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I86,Refurb_Poss_Tbl[%]))*AG86,Q86*$AG86),0)","v":0},{"$f":"IF($AF86=3,IF($AF$2=2,(U86/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I86,Refurb_Poss_Tbl[%]))*AG86,U86*$AG86),0)","v":0},{"$f":"IF($AF86=3,IF($AF$2=2,(V86/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I86,Refurb_Poss_Tbl[%]))*AG86,IF($AF$2=3,(V86*AG86)-AW86,V86*AG86)),0)","v":0},{"$f":"IF($AF86=3,IF($AF$2=2,(W86/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I86,Refurb_Poss_Tbl[%]))*AG86,W86*$AG86),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,85,0,{"$f":"VLOOKUP(AE87,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1225946284352679},0,0,0,0,0,0,0,0,6.7313708416923959E-3,{"$f":"IF(OR(AF87=3,AF87=2,AF87=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D87,FlatMaint!$Y$2:$Y$10000,AE87)*AG87,0)","v":10.833212525198647},{"$f":"IF(OR(AF87=3,AF87=2,AF87=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D87,FlatRepair!$Y$2:$Y$10000,AE87)*AG87,0)","v":0},0,10.839943896040339,0,0,0,0,0,10.839943896040339,0,{"$f":"IF($AF87=3,IF($AF$2=2,(R87/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I87,Refurb_Poss_Tbl[%]))*AG87,IF($AF$2=3,(R87*AG87)-AV87,R87*AG87)),0)","v":0},{"$f":"IF(AF87=3,IF($AF$2=2,(S87/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I87,Refurb_Poss_Tbl[%]))*AG87,IF($AF$2=3,(S87*AG87)-AX87,S87*AG87)),0)","v":0},{"$f":"IF($AF87=3,IF($AF$2=2,(T87/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I87,Refurb_Poss_Tbl[%]))*AG87,T87*$AG87),0)","v":0},{"$f":"IF($AF87=3,IF($AF$2=2,(Q87/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I87,Refurb_Poss_Tbl[%]))*AG87,Q87*$AG87),0)","v":0},{"$f":"IF($AF87=3,IF($AF$2=2,(U87/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I87,Refurb_Poss_Tbl[%]))*AG87,U87*$AG87),0)","v":0},{"$f":"IF($AF87=3,IF($AF$2=2,(V87/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I87,Refurb_Poss_Tbl[%]))*AG87,IF($AF$2=3,(V87*AG87)-AW87,V87*AG87)),0)","v":0},{"$f":"IF($AF87=3,IF($AF$2=2,(W87/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I87,Refurb_Poss_Tbl[%]))*AG87,W87*$AG87),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,86,0,{"$f":"VLOOKUP(AE88,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11960451554660284},0,0,0,0,0,0,0,0,6.5671910650657531E-3,{"$f":"IF(OR(AF88=3,AF88=2,AF88=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D88,FlatMaint!$Y$2:$Y$10000,AE88)*AG88,0)","v":10.568987829462095},{"$f":"IF(OR(AF88=3,AF88=2,AF88=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D88,FlatRepair!$Y$2:$Y$10000,AE88)*AG88,0)","v":0},0,10.575555020527162,0,0,0,0,0,10.575555020527162,0,{"$f":"IF($AF88=3,IF($AF$2=2,(R88/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I88,Refurb_Poss_Tbl[%]))*AG88,IF($AF$2=3,(R88*AG88)-AV88,R88*AG88)),0)","v":0},{"$f":"IF(AF88=3,IF($AF$2=2,(S88/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I88,Refurb_Poss_Tbl[%]))*AG88,IF($AF$2=3,(S88*AG88)-AX88,S88*AG88)),0)","v":0},{"$f":"IF($AF88=3,IF($AF$2=2,(T88/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I88,Refurb_Poss_Tbl[%]))*AG88,T88*$AG88),0)","v":0},{"$f":"IF($AF88=3,IF($AF$2=2,(Q88/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I88,Refurb_Poss_Tbl[%]))*AG88,Q88*$AG88),0)","v":0},{"$f":"IF($AF88=3,IF($AF$2=2,(U88/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I88,Refurb_Poss_Tbl[%]))*AG88,U88*$AG88),0)","v":0},{"$f":"IF($AF88=3,IF($AF$2=2,(V88/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I88,Refurb_Poss_Tbl[%]))*AG88,IF($AF$2=3,(V88*AG88)-AW88,V88*AG88)),0)","v":0},{"$f":"IF($AF88=3,IF($AF$2=2,(W88/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I88,Refurb_Poss_Tbl[%]))*AG88,W88*$AG88),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,87,0,{"$f":"VLOOKUP(AE89,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11668733224058814},0,0,0,0,0,0,0,0,6.4070156732348813E-3,{"$f":"IF(OR(AF89=3,AF89=2,AF89=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D89,FlatMaint!$Y$2:$Y$10000,AE89)*AG89,0)","v":10.311207638499607},{"$f":"IF(OR(AF89=3,AF89=2,AF89=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D89,FlatRepair!$Y$2:$Y$10000,AE89)*AG89,0)","v":0},0,10.317614654172841,0,0,0,0,0,10.317614654172841,0,{"$f":"IF($AF89=3,IF($AF$2=2,(R89/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I89,Refurb_Poss_Tbl[%]))*AG89,IF($AF$2=3,(R89*AG89)-AV89,R89*AG89)),0)","v":0},{"$f":"IF(AF89=3,IF($AF$2=2,(S89/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I89,Refurb_Poss_Tbl[%]))*AG89,IF($AF$2=3,(S89*AG89)-AX89,S89*AG89)),0)","v":0},{"$f":"IF($AF89=3,IF($AF$2=2,(T89/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I89,Refurb_Poss_Tbl[%]))*AG89,T89*$AG89),0)","v":0},{"$f":"IF($AF89=3,IF($AF$2=2,(Q89/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I89,Refurb_Poss_Tbl[%]))*AG89,Q89*$AG89),0)","v":0},{"$f":"IF($AF89=3,IF($AF$2=2,(U89/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I89,Refurb_Poss_Tbl[%]))*AG89,U89*$AG89),0)","v":0},{"$f":"IF($AF89=3,IF($AF$2=2,(V89/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I89,Refurb_Poss_Tbl[%]))*AG89,IF($AF$2=3,(V89*AG89)-AW89,V89*AG89)),0)","v":0},{"$f":"IF($AF89=3,IF($AF$2=2,(W89/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I89,Refurb_Poss_Tbl[%]))*AG89,W89*$AG89),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,88,0,{"$f":"VLOOKUP(AE90,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11384129974691526},0,0,0,0,0,0,0,0,6.2507469982779331E-3,{"$f":"IF(OR(AF90=3,AF90=2,AF90=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D90,FlatMaint!$Y$2:$Y$10000,AE90)*AG90,0)","v":10.059714769267908},{"$f":"IF(OR(AF90=3,AF90=2,AF90=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D90,FlatRepair!$Y$2:$Y$10000,AE90)*AG90,0)","v":0},0,10.065965516266186,0,0,0,0,0,10.065965516266186,0,{"$f":"IF($AF90=3,IF($AF$2=2,(R90/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I90,Refurb_Poss_Tbl[%]))*AG90,IF($AF$2=3,(R90*AG90)-AV90,R90*AG90)),0)","v":0},{"$f":"IF(AF90=3,IF($AF$2=2,(S90/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I90,Refurb_Poss_Tbl[%]))*AG90,IF($AF$2=3,(S90*AG90)-AX90,S90*AG90)),0)","v":0},{"$f":"IF($AF90=3,IF($AF$2=2,(T90/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I90,Refurb_Poss_Tbl[%]))*AG90,T90*$AG90),0)","v":0},{"$f":"IF($AF90=3,IF($AF$2=2,(Q90/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I90,Refurb_Poss_Tbl[%]))*AG90,Q90*$AG90),0)","v":0},{"$f":"IF($AF90=3,IF($AF$2=2,(U90/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I90,Refurb_Poss_Tbl[%]))*AG90,U90*$AG90),0)","v":0},{"$f":"IF($AF90=3,IF($AF$2=2,(V90/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I90,Refurb_Poss_Tbl[%]))*AG90,IF($AF$2=3,(V90*AG90)-AW90,V90*AG90)),0)","v":0},{"$f":"IF($AF90=3,IF($AF$2=2,(W90/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I90,Refurb_Poss_Tbl[%]))*AG90,W90*$AG90),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,89,0,{"$f":"VLOOKUP(AE91,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11106468267991736},0,0,0,0,0,0,0,0,6.098289754417497E-3,{"$f":"IF(OR(AF91=3,AF91=2,AF91=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D91,FlatMaint!$Y$2:$Y$10000,AE91)*AG91,0)","v":9.814355872456499},{"$f":"IF(OR(AF91=3,AF91=2,AF91=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D91,FlatRepair!$Y$2:$Y$10000,AE91)*AG91,0)","v":0},0,9.8204541622109165,0,0,0,0,0,9.8204541622109165,0,{"$f":"IF($AF91=3,IF($AF$2=2,(R91/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I91,Refurb_Poss_Tbl[%]))*AG91,IF($AF$2=3,(R91*AG91)-AV91,R91*AG91)),0)","v":0},{"$f":"IF(AF91=3,IF($AF$2=2,(S91/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I91,Refurb_Poss_Tbl[%]))*AG91,IF($AF$2=3,(S91*AG91)-AX91,S91*AG91)),0)","v":0},{"$f":"IF($AF91=3,IF($AF$2=2,(T91/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I91,Refurb_Poss_Tbl[%]))*AG91,T91*$AG91),0)","v":0},{"$f":"IF($AF91=3,IF($AF$2=2,(Q91/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I91,Refurb_Poss_Tbl[%]))*AG91,Q91*$AG91),0)","v":0},{"$f":"IF($AF91=3,IF($AF$2=2,(U91/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I91,Refurb_Poss_Tbl[%]))*AG91,U91*$AG91),0)","v":0},{"$f":"IF($AF91=3,IF($AF$2=2,(V91/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I91,Refurb_Poss_Tbl[%]))*AG91,IF($AF$2=3,(V91*AG91)-AW91,V91*AG91)),0)","v":0},{"$f":"IF($AF91=3,IF($AF$2=2,(W91/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I91,Refurb_Poss_Tbl[%]))*AG91,W91*$AG91),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,90,3,{"$f":"VLOOKUP(AE92,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10835578798040717},0,0,0,0,0,0,0,0,5.9495509799195089E-3,{"$f":"IF(OR(AF92=3,AF92=2,AF92=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D92,FlatMaint!$Y$2:$Y$10000,AE92)*AG92,0)","v":9.5749813389819494},{"$f":"IF(OR(AF92=3,AF92=2,AF92=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D92,FlatRepair!$Y$2:$Y$10000,AE92)*AG92,0)","v":0},0,9.5809308899618681,0,0.24836861458031489,7.0132878562457288E-3,0.26560696667471523,97.005224198587172,107.10714395766031,0,{"$f":"IF($AF92=3,IF($AF$2=2,(R92/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I92,Refurb_Poss_Tbl[%]))*AG92,IF($AF$2=3,(R92*AG92)-AV92,R92*AG92)),0)","v":0.11639322534343985},{"$f":"IF(AF92=3,IF($AF$2=2,(S92/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I92,Refurb_Poss_Tbl[%]))*AG92,IF($AF$2=3,(S92*AG92)-AX92,S92*AG92)),0)","v":0.53121393334943157},{"$f":"IF($AF92=3,IF($AF$2=2,(T92/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I92,Refurb_Poss_Tbl[%]))*AG92,T92*$AG92),0)","v":1.4026575712491482E-2},{"$f":"IF($AF92=3,IF($AF$2=2,(Q92/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I92,Refurb_Poss_Tbl[%]))*AG92,Q92*$AG92),0)","v":95.733248869308767},{"$f":"IF($AF92=3,IF($AF$2=2,(U92/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I92,Refurb_Poss_Tbl[%]))*AG92,U92*$AG92),0)","v":0.59726956252672325},{"$f":"IF($AF92=3,IF($AF$2=2,(V92/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I92,Refurb_Poss_Tbl[%]))*AG92,IF($AF$2=3,(V92*AG92)-AW92,V92*AG92)),0)","v":0},{"$f":"IF($AF92=3,IF($AF$2=2,(W92/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I92,Refurb_Poss_Tbl[%]))*AG92,W92*$AG92),0)","v":1.3072032346332356E-2}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,91,0,{"$f":"VLOOKUP(AE93,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10571296388332406},0,0,0,0,0,0,0,0,5.8044399804092761E-3,{"$f":"IF(OR(AF93=3,AF93=2,AF93=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D93,FlatMaint!$Y$2:$Y$10000,AE93)*AG93,0)","v":9.3414452087628774},{"$f":"IF(OR(AF93=3,AF93=2,AF93=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D93,FlatRepair!$Y$2:$Y$10000,AE93)*AG93,0)","v":0},0,9.3472496487432863,0,0,0,0,0,9.3472496487432863,0,{"$f":"IF($AF93=3,IF($AF$2=2,(R93/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I93,Refurb_Poss_Tbl[%]))*AG93,IF($AF$2=3,(R93*AG93)-AV93,R93*AG93)),0)","v":0},{"$f":"IF(AF93=3,IF($AF$2=2,(S93/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I93,Refurb_Poss_Tbl[%]))*AG93,IF($AF$2=3,(S93*AG93)-AX93,S93*AG93)),0)","v":0},{"$f":"IF($AF93=3,IF($AF$2=2,(T93/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I93,Refurb_Poss_Tbl[%]))*AG93,T93*$AG93),0)","v":0},{"$f":"IF($AF93=3,IF($AF$2=2,(Q93/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I93,Refurb_Poss_Tbl[%]))*AG93,Q93*$AG93),0)","v":0},{"$f":"IF($AF93=3,IF($AF$2=2,(U93/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I93,Refurb_Poss_Tbl[%]))*AG93,U93*$AG93),0)","v":0},{"$f":"IF($AF93=3,IF($AF$2=2,(V93/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I93,Refurb_Poss_Tbl[%]))*AG93,IF($AF$2=3,(V93*AG93)-AW93,V93*AG93)),0)","v":0},{"$f":"IF($AF93=3,IF($AF$2=2,(W93/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I93,Refurb_Poss_Tbl[%]))*AG93,W93*$AG93),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,92,0,{"$f":"VLOOKUP(AE94,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10313459891056008},0,0,0,0,0,0,0,0,5.6628682735700275E-3,{"$f":"IF(OR(AF94=3,AF94=2,AF94=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D94,FlatMaint!$Y$2:$Y$10000,AE94)*AG94,0)","v":9.1136050817198822},{"$f":"IF(OR(AF94=3,AF94=2,AF94=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D94,FlatRepair!$Y$2:$Y$10000,AE94)*AG94,0)","v":0},0,9.1192679499934517,0,0,0,0,0,9.1192679499934517,0,{"$f":"IF($AF94=3,IF($AF$2=2,(R94/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I94,Refurb_Poss_Tbl[%]))*AG94,IF($AF$2=3,(R94*AG94)-AV94,R94*AG94)),0)","v":0},{"$f":"IF(AF94=3,IF($AF$2=2,(S94/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I94,Refurb_Poss_Tbl[%]))*AG94,IF($AF$2=3,(S94*AG94)-AX94,S94*AG94)),0)","v":0},{"$f":"IF($AF94=3,IF($AF$2=2,(T94/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I94,Refurb_Poss_Tbl[%]))*AG94,T94*$AG94),0)","v":0},{"$f":"IF($AF94=3,IF($AF$2=2,(Q94/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I94,Refurb_Poss_Tbl[%]))*AG94,Q94*$AG94),0)","v":0},{"$f":"IF($AF94=3,IF($AF$2=2,(U94/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I94,Refurb_Poss_Tbl[%]))*AG94,U94*$AG94),0)","v":0},{"$f":"IF($AF94=3,IF($AF$2=2,(V94/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I94,Refurb_Poss_Tbl[%]))*AG94,IF($AF$2=3,(V94*AG94)-AW94,V94*AG94)),0)","v":0},{"$f":"IF($AF94=3,IF($AF$2=2,(W94/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I94,Refurb_Poss_Tbl[%]))*AG94,W94*$AG94),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,93,0,{"$f":"VLOOKUP(AE95,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10061912088835129},0,0,0,0,0,0,0,0,5.5247495351902695E-3,{"$f":"IF(OR(AF95=3,AF95=2,AF95=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D95,FlatMaint!$Y$2:$Y$10000,AE95)*AG95,0)","v":8.8913220309462258},{"$f":"IF(OR(AF95=3,AF95=2,AF95=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D95,FlatRepair!$Y$2:$Y$10000,AE95)*AG95,0)","v":0},0,8.8968467804814164,0,0,0,0,0,8.8968467804814164,0,{"$f":"IF($AF95=3,IF($AF$2=2,(R95/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I95,Refurb_Poss_Tbl[%]))*AG95,IF($AF$2=3,(R95*AG95)-AV95,R95*AG95)),0)","v":0},{"$f":"IF(AF95=3,IF($AF$2=2,(S95/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I95,Refurb_Poss_Tbl[%]))*AG95,IF($AF$2=3,(S95*AG95)-AX95,S95*AG95)),0)","v":0},{"$f":"IF($AF95=3,IF($AF$2=2,(T95/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I95,Refurb_Poss_Tbl[%]))*AG95,T95*$AG95),0)","v":0},{"$f":"IF($AF95=3,IF($AF$2=2,(Q95/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I95,Refurb_Poss_Tbl[%]))*AG95,Q95*$AG95),0)","v":0},{"$f":"IF($AF95=3,IF($AF$2=2,(U95/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I95,Refurb_Poss_Tbl[%]))*AG95,U95*$AG95),0)","v":0},{"$f":"IF($AF95=3,IF($AF$2=2,(V95/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I95,Refurb_Poss_Tbl[%]))*AG95,IF($AF$2=3,(V95*AG95)-AW95,V95*AG95)),0)","v":0},{"$f":"IF($AF95=3,IF($AF$2=2,(W95/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I95,Refurb_Poss_Tbl[%]))*AG95,W95*$AG95),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,94,0,{"$f":"VLOOKUP(AE96,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.8164995988635415E-2},0,0,0,0,0,0,0,0,5.389999546527093E-3,{"$f":"IF(OR(AF96=3,AF96=2,AF96=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D96,FlatMaint!$Y$2:$Y$10000,AE96)*AG96,0)","v":8.6744605179963177},{"$f":"IF(OR(AF96=3,AF96=2,AF96=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D96,FlatRepair!$Y$2:$Y$10000,AE96)*AG96,0)","v":0},0,8.6798505175428442,0,0,0,0,0,8.6798505175428442,0,{"$f":"IF($AF96=3,IF($AF$2=2,(R96/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I96,Refurb_Poss_Tbl[%]))*AG96,IF($AF$2=3,(R96*AG96)-AV96,R96*AG96)),0)","v":0},{"$f":"IF(AF96=3,IF($AF$2=2,(S96/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I96,Refurb_Poss_Tbl[%]))*AG96,IF($AF$2=3,(S96*AG96)-AX96,S96*AG96)),0)","v":0},{"$f":"IF($AF96=3,IF($AF$2=2,(T96/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I96,Refurb_Poss_Tbl[%]))*AG96,T96*$AG96),0)","v":0},{"$f":"IF($AF96=3,IF($AF$2=2,(Q96/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I96,Refurb_Poss_Tbl[%]))*AG96,Q96*$AG96),0)","v":0},{"$f":"IF($AF96=3,IF($AF$2=2,(U96/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I96,Refurb_Poss_Tbl[%]))*AG96,U96*$AG96),0)","v":0},{"$f":"IF($AF96=3,IF($AF$2=2,(V96/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I96,Refurb_Poss_Tbl[%]))*AG96,IF($AF$2=3,(V96*AG96)-AW96,V96*AG96)),0)","v":0},{"$f":"IF($AF96=3,IF($AF$2=2,(W96/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I96,Refurb_Poss_Tbl[%]))*AG96,W96*$AG96),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,95,0,{"$f":"VLOOKUP(AE97,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.577072779379063E-2},0,0,0,0,0,0,0,0,5.2585361429532606E-3,{"$f":"IF(OR(AF97=3,AF97=2,AF97=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D97,FlatMaint!$Y$2:$Y$10000,AE97)*AG97,0)","v":8.4628883102403094},{"$f":"IF(OR(AF97=3,AF97=2,AF97=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D97,FlatRepair!$Y$2:$Y$10000,AE97)*AG97,0)","v":0},0,8.468146846383263,0,0,0,0,0,8.468146846383263,0,{"$f":"IF($AF97=3,IF($AF$2=2,(R97/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I97,Refurb_Poss_Tbl[%]))*AG97,IF($AF$2=3,(R97*AG97)-AV97,R97*AG97)),0)","v":0},{"$f":"IF(AF97=3,IF($AF$2=2,(S97/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I97,Refurb_Poss_Tbl[%]))*AG97,IF($AF$2=3,(S97*AG97)-AX97,S97*AG97)),0)","v":0},{"$f":"IF($AF97=3,IF($AF$2=2,(T97/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I97,Refurb_Poss_Tbl[%]))*AG97,T97*$AG97),0)","v":0},{"$f":"IF($AF97=3,IF($AF$2=2,(Q97/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I97,Refurb_Poss_Tbl[%]))*AG97,Q97*$AG97),0)","v":0},{"$f":"IF($AF97=3,IF($AF$2=2,(U97/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I97,Refurb_Poss_Tbl[%]))*AG97,U97*$AG97),0)","v":0},{"$f":"IF($AF97=3,IF($AF$2=2,(V97/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I97,Refurb_Poss_Tbl[%]))*AG97,IF($AF$2=3,(V97*AG97)-AW97,V97*AG97)),0)","v":0},{"$f":"IF($AF97=3,IF($AF$2=2,(W97/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I97,Refurb_Poss_Tbl[%]))*AG97,W97*$AG97),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,96,0,{"$f":"VLOOKUP(AE98,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.3434856384185999E-2},0,0,0,0,0,0,0,0,5.130279163856841E-3,{"$f":"IF(OR(AF98=3,AF98=2,AF98=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D98,FlatMaint!$Y$2:$Y$10000,AE98)*AG98,0)","v":8.2564764002344493},{"$f":"IF(OR(AF98=3,AF98=2,AF98=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D98,FlatRepair!$Y$2:$Y$10000,AE98)*AG98,0)","v":0},0,8.261606679398307,0,0,0,0,0,8.261606679398307,0,{"$f":"IF($AF98=3,IF($AF$2=2,(R98/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I98,Refurb_Poss_Tbl[%]))*AG98,IF($AF$2=3,(R98*AG98)-AV98,R98*AG98)),0)","v":0},{"$f":"IF(AF98=3,IF($AF$2=2,(S98/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I98,Refurb_Poss_Tbl[%]))*AG98,IF($AF$2=3,(S98*AG98)-AX98,S98*AG98)),0)","v":0},{"$f":"IF($AF98=3,IF($AF$2=2,(T98/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I98,Refurb_Poss_Tbl[%]))*AG98,T98*$AG98),0)","v":0},{"$f":"IF($AF98=3,IF($AF$2=2,(Q98/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I98,Refurb_Poss_Tbl[%]))*AG98,Q98*$AG98),0)","v":0},{"$f":"IF($AF98=3,IF($AF$2=2,(U98/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I98,Refurb_Poss_Tbl[%]))*AG98,U98*$AG98),0)","v":0},{"$f":"IF($AF98=3,IF($AF$2=2,(V98/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I98,Refurb_Poss_Tbl[%]))*AG98,IF($AF$2=3,(V98*AG98)-AW98,V98*AG98)),0)","v":0},{"$f":"IF($AF98=3,IF($AF$2=2,(W98/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I98,Refurb_Poss_Tbl[%]))*AG98,W98*$AG98),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,97,0,{"$f":"VLOOKUP(AE99,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.1155957447986352E-2},0,0,0,0,0,0,0,0,5.0051504037627722E-3,{"$f":"IF(OR(AF99=3,AF99=2,AF99=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D99,FlatMaint!$Y$2:$Y$10000,AE99)*AG99,0)","v":8.0550989270580011},{"$f":"IF(OR(AF99=3,AF99=2,AF99=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D99,FlatRepair!$Y$2:$Y$10000,AE99)*AG99,0)","v":0},0,8.060104077461764,0,0,0,0,0,8.060104077461764,0,{"$f":"IF($AF99=3,IF($AF$2=2,(R99/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I99,Refurb_Poss_Tbl[%]))*AG99,IF($AF$2=3,(R99*AG99)-AV99,R99*AG99)),0)","v":0},{"$f":"IF(AF99=3,IF($AF$2=2,(S99/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I99,Refurb_Poss_Tbl[%]))*AG99,IF($AF$2=3,(S99*AG99)-AX99,S99*AG99)),0)","v":0},{"$f":"IF($AF99=3,IF($AF$2=2,(T99/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I99,Refurb_Poss_Tbl[%]))*AG99,T99*$AG99),0)","v":0},{"$f":"IF($AF99=3,IF($AF$2=2,(Q99/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I99,Refurb_Poss_Tbl[%]))*AG99,Q99*$AG99),0)","v":0},{"$f":"IF($AF99=3,IF($AF$2=2,(U99/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I99,Refurb_Poss_Tbl[%]))*AG99,U99*$AG99),0)","v":0},{"$f":"IF($AF99=3,IF($AF$2=2,(V99/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I99,Refurb_Poss_Tbl[%]))*AG99,IF($AF$2=3,(V99*AG99)-AW99,V99*AG99)),0)","v":0},{"$f":"IF($AF99=3,IF($AF$2=2,(W99/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I99,Refurb_Poss_Tbl[%]))*AG99,W99*$AG99),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,98,0,{"$f":"VLOOKUP(AE100,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.8932641412669614E-2},0,0,0,0,0,0,0,0,4.8830735646466072E-3,{"$f":"IF(OR(AF100=3,AF100=2,AF100=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D100,FlatMaint!$Y$2:$Y$10000,AE100)*AG100,0)","v":7.858633099568781},{"$f":"IF(OR(AF100=3,AF100=2,AF100=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D100,FlatRepair!$Y$2:$Y$10000,AE100)*AG100,0)","v":0},0,7.8635161731334273,0,0,0,0,0,7.8635161731334273,0,{"$f":"IF($AF100=3,IF($AF$2=2,(R100/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I100,Refurb_Poss_Tbl[%]))*AG100,IF($AF$2=3,(R100*AG100)-AV100,R100*AG100)),0)","v":0},{"$f":"IF(AF100=3,IF($AF$2=2,(S100/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I100,Refurb_Poss_Tbl[%]))*AG100,IF($AF$2=3,(S100*AG100)-AX100,S100*AG100)),0)","v":0},{"$f":"IF($AF100=3,IF($AF$2=2,(T100/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I100,Refurb_Poss_Tbl[%]))*AG100,T100*$AG100),0)","v":0},{"$f":"IF($AF100=3,IF($AF$2=2,(Q100/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I100,Refurb_Poss_Tbl[%]))*AG100,Q100*$AG100),0)","v":0},{"$f":"IF($AF100=3,IF($AF$2=2,(U100/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I100,Refurb_Poss_Tbl[%]))*AG100,U100*$AG100),0)","v":0},{"$f":"IF($AF100=3,IF($AF$2=2,(V100/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I100,Refurb_Poss_Tbl[%]))*AG100,IF($AF$2=3,(V100*AG100)-AW100,V100*AG100)),0)","v":0},{"$f":"IF($AF100=3,IF($AF$2=2,(W100/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I100,Refurb_Poss_Tbl[%]))*AG100,W100*$AG100),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,99,0,{"$f":"VLOOKUP(AE101,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.6763552597726459E-2},0,0,0,0,0,0,0,0,4.763974209411324E-3,{"$f":"IF(OR(AF101=3,AF101=2,AF101=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D101,FlatMaint!$Y$2:$Y$10000,AE101)*AG101,0)","v":7.6669591215305184},{"$f":"IF(OR(AF101=3,AF101=2,AF101=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D101,FlatRepair!$Y$2:$Y$10000,AE101)*AG101,0)","v":0},0,7.6717230957399298,0,0,0,0,0,7.6717230957399298,0,{"$f":"IF($AF101=3,IF($AF$2=2,(R101/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I101,Refurb_Poss_Tbl[%]))*AG101,IF($AF$2=3,(R101*AG101)-AV101,R101*AG101)),0)","v":0},{"$f":"IF(AF101=3,IF($AF$2=2,(S101/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I101,Refurb_Poss_Tbl[%]))*AG101,IF($AF$2=3,(S101*AG101)-AX101,S101*AG101)),0)","v":0},{"$f":"IF($AF101=3,IF($AF$2=2,(T101/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I101,Refurb_Poss_Tbl[%]))*AG101,T101*$AG101),0)","v":0},{"$f":"IF($AF101=3,IF($AF$2=2,(Q101/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I101,Refurb_Poss_Tbl[%]))*AG101,Q101*$AG101),0)","v":0},{"$f":"IF($AF101=3,IF($AF$2=2,(U101/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I101,Refurb_Poss_Tbl[%]))*AG101,U101*$AG101),0)","v":0},{"$f":"IF($AF101=3,IF($AF$2=2,(V101/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I101,Refurb_Poss_Tbl[%]))*AG101,IF($AF$2=3,(V101*AG101)-AW101,V101*AG101)),0)","v":0},{"$f":"IF($AF101=3,IF($AF$2=2,(W101/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I101,Refurb_Poss_Tbl[%]))*AG101,W101*$AG101),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50840000000005,883.50840000000005,1.0741763547000001,4.9024970723805303,0.12944925207897301,5.5121149839704104,0,0.120639908490131,895.24727757161997,5.4907551232937397E-2,0,223.81181939290499,2.29215826131249,6.4724626039486394E-2,2.4512485361902598,100,0,{"$f":"VLOOKUP(AE102,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.4647368388025807E-2},0,0,0,0,0,0,0,0,4.6477797164988528E-3,{"$f":"IF(OR(AF102=3,AF102=2,AF102=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D102,FlatMaint!$Y$2:$Y$10000,AE102)*AG102,0)","v":7.4799601185663587},{"$f":"IF(OR(AF102=3,AF102=2,AF102=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D102,FlatRepair!$Y$2:$Y$10000,AE102)*AG102,0)","v":0},0,7.4846078982828574,0,0,0,0,0,-371.41702261662778,-378.90163051491061,{"$f":"IF($AF102=3,IF($AF$2=2,(R102/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I102,Refurb_Poss_Tbl[%]))*AG102,IF($AF$2=3,(R102*AG102)-AV102,R102*AG102)),0)","v":0},{"$f":"IF(AF102=3,IF($AF$2=2,(S102/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I102,Refurb_Poss_Tbl[%]))*AG102,IF($AF$2=3,(S102*AG102)-AX102,S102*AG102)),0)","v":0},{"$f":"IF($AF102=3,IF($AF$2=2,(T102/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I102,Refurb_Poss_Tbl[%]))*AG102,T102*$AG102),0)","v":0},{"$f":"IF($AF102=3,IF($AF$2=2,(Q102/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I102,Refurb_Poss_Tbl[%]))*AG102,Q102*$AG102),0)","v":0},{"$f":"IF($AF102=3,IF($AF$2=2,(U102/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I102,Refurb_Poss_Tbl[%]))*AG102,U102*$AG102),0)","v":0},{"$f":"IF($AF102=3,IF($AF$2=2,(V102/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I102,Refurb_Poss_Tbl[%]))*AG102,IF($AF$2=3,(V102*AG102)-AW102,V102*AG102)),0)","v":0},{"$f":"IF($AF102=3,IF($AF$2=2,(W102/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I102,Refurb_Poss_Tbl[%]))*AG102,W102*$AG102),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,0,1,{"$f":"VLOOKUP(AE103,ValidationLists!$M$1:$N$102,2,FALSE)","v":1},27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608837,0,{"$f":"IF(OR(AF103=3,AF103=2,AF103=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D103,FlatMaint!$Y$2:$Y$10000,AE103)*AG103,0)","v":0},{"$f":"IF(OR(AF103=3,AF103=2,AF103=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D103,FlatRepair!$Y$2:$Y$10000,AE103)*AG103,0)","v":0},0,0,0,0,0,0,0,27.856251354608837,0,{"$f":"IF($AF103=3,IF($AF$2=2,(R103/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I103,Refurb_Poss_Tbl[%]))*AG103,IF($AF$2=3,(R103*AG103)-AV103,R103*AG103)),0)","v":0},{"$f":"IF(AF103=3,IF($AF$2=2,(S103/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I103,Refurb_Poss_Tbl[%]))*AG103,IF($AF$2=3,(S103*AG103)-AX103,S103*AG103)),0)","v":0},{"$f":"IF($AF103=3,IF($AF$2=2,(T103/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I103,Refurb_Poss_Tbl[%]))*AG103,T103*$AG103),0)","v":0},{"$f":"IF($AF103=3,IF($AF$2=2,(Q103/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I103,Refurb_Poss_Tbl[%]))*AG103,Q103*$AG103),0)","v":0},{"$f":"IF($AF103=3,IF($AF$2=2,(U103/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I103,Refurb_Poss_Tbl[%]))*AG103,U103*$AG103),0)","v":0},{"$f":"IF($AF103=3,IF($AF$2=2,(V103/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I103,Refurb_Poss_Tbl[%]))*AG103,IF($AF$2=3,(V103*AG103)-AW103,V103*AG103)),0)","v":0},{"$f":"IF($AF103=3,IF($AF$2=2,(W103/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I103,Refurb_Poss_Tbl[%]))*AG103,W103*$AG103),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,1,0,{"$f":"VLOOKUP(AE104,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.96618357487922713},0,0,0,0,0,0,0,0,1.6349873371740871E-3,{"$f":"IF(OR(AF104=3,AF104=2,AF104=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D104,FlatMaint!$Y$2:$Y$10000,AE104)*AG104,0)","v":26.323083244444444},{"$f":"IF(OR(AF104=3,AF104=2,AF104=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D104,FlatRepair!$Y$2:$Y$10000,AE104)*AG104,0)","v":0},0,26.324718231781617,0,0,0,0,0,26.324718231781617,0,{"$f":"IF($AF104=3,IF($AF$2=2,(R104/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I104,Refurb_Poss_Tbl[%]))*AG104,IF($AF$2=3,(R104*AG104)-AV104,R104*AG104)),0)","v":0},{"$f":"IF(AF104=3,IF($AF$2=2,(S104/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I104,Refurb_Poss_Tbl[%]))*AG104,IF($AF$2=3,(S104*AG104)-AX104,S104*AG104)),0)","v":0},{"$f":"IF($AF104=3,IF($AF$2=2,(T104/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I104,Refurb_Poss_Tbl[%]))*AG104,T104*$AG104),0)","v":0},{"$f":"IF($AF104=3,IF($AF$2=2,(Q104/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I104,Refurb_Poss_Tbl[%]))*AG104,Q104*$AG104),0)","v":0},{"$f":"IF($AF104=3,IF($AF$2=2,(U104/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I104,Refurb_Poss_Tbl[%]))*AG104,U104*$AG104),0)","v":0},{"$f":"IF($AF104=3,IF($AF$2=2,(V104/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I104,Refurb_Poss_Tbl[%]))*AG104,IF($AF$2=3,(V104*AG104)-AW104,V104*AG104)),0)","v":0},{"$f":"IF($AF104=3,IF($AF$2=2,(W104/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I104,Refurb_Poss_Tbl[%]))*AG104,W104*$AG104),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,2,0,{"$f":"VLOOKUP(AE105,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.93351070036640305},0,0,0,0,0,0,0,0,1.5796979103131277E-3,{"$f":"IF(OR(AF105=3,AF105=2,AF105=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D105,FlatMaint!$Y$2:$Y$10000,AE105)*AG105,0)","v":25.432930670960815},{"$f":"IF(OR(AF105=3,AF105=2,AF105=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D105,FlatRepair!$Y$2:$Y$10000,AE105)*AG105,0)","v":0},0,25.434510368871127,0,0,0,0,0,25.434510368871127,0,{"$f":"IF($AF105=3,IF($AF$2=2,(R105/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I105,Refurb_Poss_Tbl[%]))*AG105,IF($AF$2=3,(R105*AG105)-AV105,R105*AG105)),0)","v":0},{"$f":"IF(AF105=3,IF($AF$2=2,(S105/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I105,Refurb_Poss_Tbl[%]))*AG105,IF($AF$2=3,(S105*AG105)-AX105,S105*AG105)),0)","v":0},{"$f":"IF($AF105=3,IF($AF$2=2,(T105/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I105,Refurb_Poss_Tbl[%]))*AG105,T105*$AG105),0)","v":0},{"$f":"IF($AF105=3,IF($AF$2=2,(Q105/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I105,Refurb_Poss_Tbl[%]))*AG105,Q105*$AG105),0)","v":0},{"$f":"IF($AF105=3,IF($AF$2=2,(U105/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I105,Refurb_Poss_Tbl[%]))*AG105,U105*$AG105),0)","v":0},{"$f":"IF($AF105=3,IF($AF$2=2,(V105/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I105,Refurb_Poss_Tbl[%]))*AG105,IF($AF$2=3,(V105*AG105)-AW105,V105*AG105)),0)","v":0},{"$f":"IF($AF105=3,IF($AF$2=2,(W105/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I105,Refurb_Poss_Tbl[%]))*AG105,W105*$AG105),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,3,0,{"$f":"VLOOKUP(AE106,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.90194270566802237},0,0,0,0,0,0,0,0,1.5262781742155826E-3,{"$f":"IF(OR(AF106=3,AF106=2,AF106=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D106,FlatMaint!$Y$2:$Y$10000,AE106)*AG106,0)","v":24.57287987532446},{"$f":"IF(OR(AF106=3,AF106=2,AF106=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D106,FlatRepair!$Y$2:$Y$10000,AE106)*AG106,0)","v":0},0,24.574406153498675,0,0,0,0,0,24.574406153498675,0,{"$f":"IF($AF106=3,IF($AF$2=2,(R106/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I106,Refurb_Poss_Tbl[%]))*AG106,IF($AF$2=3,(R106*AG106)-AV106,R106*AG106)),0)","v":0},{"$f":"IF(AF106=3,IF($AF$2=2,(S106/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I106,Refurb_Poss_Tbl[%]))*AG106,IF($AF$2=3,(S106*AG106)-AX106,S106*AG106)),0)","v":0},{"$f":"IF($AF106=3,IF($AF$2=2,(T106/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I106,Refurb_Poss_Tbl[%]))*AG106,T106*$AG106),0)","v":0},{"$f":"IF($AF106=3,IF($AF$2=2,(Q106/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I106,Refurb_Poss_Tbl[%]))*AG106,Q106*$AG106),0)","v":0},{"$f":"IF($AF106=3,IF($AF$2=2,(U106/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I106,Refurb_Poss_Tbl[%]))*AG106,U106*$AG106),0)","v":0},{"$f":"IF($AF106=3,IF($AF$2=2,(V106/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I106,Refurb_Poss_Tbl[%]))*AG106,IF($AF$2=3,(V106*AG106)-AW106,V106*AG106)),0)","v":0},{"$f":"IF($AF106=3,IF($AF$2=2,(W106/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I106,Refurb_Poss_Tbl[%]))*AG106,W106*$AG106),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,4,0,{"$f":"VLOOKUP(AE107,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.87144222769857238},0,0,0,0,0,0,0,0,1.4746649026237512E-3,{"$f":"IF(OR(AF107=3,AF107=2,AF107=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D107,FlatMaint!$Y$2:$Y$10000,AE107)*AG107,0)","v":23.741912923018806},{"$f":"IF(OR(AF107=3,AF107=2,AF107=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D107,FlatRepair!$Y$2:$Y$10000,AE107)*AG107,0)","v":0},0,23.743387587921429,0,0,0,0,0,23.743387587921429,0,{"$f":"IF($AF107=3,IF($AF$2=2,(R107/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I107,Refurb_Poss_Tbl[%]))*AG107,IF($AF$2=3,(R107*AG107)-AV107,R107*AG107)),0)","v":0},{"$f":"IF(AF107=3,IF($AF$2=2,(S107/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I107,Refurb_Poss_Tbl[%]))*AG107,IF($AF$2=3,(S107*AG107)-AX107,S107*AG107)),0)","v":0},{"$f":"IF($AF107=3,IF($AF$2=2,(T107/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I107,Refurb_Poss_Tbl[%]))*AG107,T107*$AG107),0)","v":0},{"$f":"IF($AF107=3,IF($AF$2=2,(Q107/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I107,Refurb_Poss_Tbl[%]))*AG107,Q107*$AG107),0)","v":0},{"$f":"IF($AF107=3,IF($AF$2=2,(U107/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I107,Refurb_Poss_Tbl[%]))*AG107,U107*$AG107),0)","v":0},{"$f":"IF($AF107=3,IF($AF$2=2,(V107/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I107,Refurb_Poss_Tbl[%]))*AG107,IF($AF$2=3,(V107*AG107)-AW107,V107*AG107)),0)","v":0},{"$f":"IF($AF107=3,IF($AF$2=2,(W107/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I107,Refurb_Poss_Tbl[%]))*AG107,W107*$AG107),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,5,0,{"$f":"VLOOKUP(AE108,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.84197316685852419},0,0,0,0,0,0,0,0,1.4247970073659436E-3,{"$f":"IF(OR(AF108=3,AF108=2,AF108=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D108,FlatMaint!$Y$2:$Y$10000,AE108)*AG108,0)","v":22.939046302433631},{"$f":"IF(OR(AF108=3,AF108=2,AF108=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D108,FlatRepair!$Y$2:$Y$10000,AE108)*AG108,0)","v":0},0,22.940471099440998,0,0,0,0,0,22.940471099440998,0,{"$f":"IF($AF108=3,IF($AF$2=2,(R108/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I108,Refurb_Poss_Tbl[%]))*AG108,IF($AF$2=3,(R108*AG108)-AV108,R108*AG108)),0)","v":0},{"$f":"IF(AF108=3,IF($AF$2=2,(S108/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I108,Refurb_Poss_Tbl[%]))*AG108,IF($AF$2=3,(S108*AG108)-AX108,S108*AG108)),0)","v":0},{"$f":"IF($AF108=3,IF($AF$2=2,(T108/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I108,Refurb_Poss_Tbl[%]))*AG108,T108*$AG108),0)","v":0},{"$f":"IF($AF108=3,IF($AF$2=2,(Q108/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I108,Refurb_Poss_Tbl[%]))*AG108,Q108*$AG108),0)","v":0},{"$f":"IF($AF108=3,IF($AF$2=2,(U108/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I108,Refurb_Poss_Tbl[%]))*AG108,U108*$AG108),0)","v":0},{"$f":"IF($AF108=3,IF($AF$2=2,(V108/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I108,Refurb_Poss_Tbl[%]))*AG108,IF($AF$2=3,(V108*AG108)-AW108,V108*AG108)),0)","v":0},{"$f":"IF($AF108=3,IF($AF$2=2,(W108/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I108,Refurb_Poss_Tbl[%]))*AG108,W108*$AG108),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,6,0,{"$f":"VLOOKUP(AE109,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.81350064430775282},0,0,0,0,0,0,0,0,1.3766154660540516E-3,{"$f":"IF(OR(AF109=3,AF109=2,AF109=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D109,FlatMaint!$Y$2:$Y$10000,AE109)*AG109,0)","v":22.163329760805439},{"$f":"IF(OR(AF109=3,AF109=2,AF109=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D109,FlatRepair!$Y$2:$Y$10000,AE109)*AG109,0)","v":0},0,22.164706376271493,0,0,0,0,0,22.164706376271493,0,{"$f":"IF($AF109=3,IF($AF$2=2,(R109/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I109,Refurb_Poss_Tbl[%]))*AG109,IF($AF$2=3,(R109*AG109)-AV109,R109*AG109)),0)","v":0},{"$f":"IF(AF109=3,IF($AF$2=2,(S109/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I109,Refurb_Poss_Tbl[%]))*AG109,IF($AF$2=3,(S109*AG109)-AX109,S109*AG109)),0)","v":0},{"$f":"IF($AF109=3,IF($AF$2=2,(T109/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I109,Refurb_Poss_Tbl[%]))*AG109,T109*$AG109),0)","v":0},{"$f":"IF($AF109=3,IF($AF$2=2,(Q109/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I109,Refurb_Poss_Tbl[%]))*AG109,Q109*$AG109),0)","v":0},{"$f":"IF($AF109=3,IF($AF$2=2,(U109/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I109,Refurb_Poss_Tbl[%]))*AG109,U109*$AG109),0)","v":0},{"$f":"IF($AF109=3,IF($AF$2=2,(V109/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I109,Refurb_Poss_Tbl[%]))*AG109,IF($AF$2=3,(V109*AG109)-AW109,V109*AG109)),0)","v":0},{"$f":"IF($AF109=3,IF($AF$2=2,(W109/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I109,Refurb_Poss_Tbl[%]))*AG109,W109*$AG109),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,7,0,{"$f":"VLOOKUP(AE110,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.78599096068381913},0,0,0,0,0,0,0,0,1.3300632522261367E-3,{"$f":"IF(OR(AF110=3,AF110=2,AF110=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D110,FlatMaint!$Y$2:$Y$10000,AE110)*AG110,0)","v":21.413845179522163},{"$f":"IF(OR(AF110=3,AF110=2,AF110=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D110,FlatRepair!$Y$2:$Y$10000,AE110)*AG110,0)","v":0},0,21.415175242774389,0,0,0,0,0,21.415175242774389,0,{"$f":"IF($AF110=3,IF($AF$2=2,(R110/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I110,Refurb_Poss_Tbl[%]))*AG110,IF($AF$2=3,(R110*AG110)-AV110,R110*AG110)),0)","v":0},{"$f":"IF(AF110=3,IF($AF$2=2,(S110/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I110,Refurb_Poss_Tbl[%]))*AG110,IF($AF$2=3,(S110*AG110)-AX110,S110*AG110)),0)","v":0},{"$f":"IF($AF110=3,IF($AF$2=2,(T110/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I110,Refurb_Poss_Tbl[%]))*AG110,T110*$AG110),0)","v":0},{"$f":"IF($AF110=3,IF($AF$2=2,(Q110/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I110,Refurb_Poss_Tbl[%]))*AG110,Q110*$AG110),0)","v":0},{"$f":"IF($AF110=3,IF($AF$2=2,(U110/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I110,Refurb_Poss_Tbl[%]))*AG110,U110*$AG110),0)","v":0},{"$f":"IF($AF110=3,IF($AF$2=2,(V110/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I110,Refurb_Poss_Tbl[%]))*AG110,IF($AF$2=3,(V110*AG110)-AW110,V110*AG110)),0)","v":0},{"$f":"IF($AF110=3,IF($AF$2=2,(W110/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I110,Refurb_Poss_Tbl[%]))*AG110,W110*$AG110),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,8,0,{"$f":"VLOOKUP(AE111,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.75941155621625056},0,0,0,0,0,0,0,0,1.2850852678513403E-3,{"$f":"IF(OR(AF111=3,AF111=2,AF111=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D111,FlatMaint!$Y$2:$Y$10000,AE111)*AG111,0)","v":20.689705487461033},{"$f":"IF(OR(AF111=3,AF111=2,AF111=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D111,FlatRepair!$Y$2:$Y$10000,AE111)*AG111,0)","v":0},0,20.690990572728886,0,0,0,0,0,20.690990572728886,0,{"$f":"IF($AF111=3,IF($AF$2=2,(R111/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I111,Refurb_Poss_Tbl[%]))*AG111,IF($AF$2=3,(R111*AG111)-AV111,R111*AG111)),0)","v":0},{"$f":"IF(AF111=3,IF($AF$2=2,(S111/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I111,Refurb_Poss_Tbl[%]))*AG111,IF($AF$2=3,(S111*AG111)-AX111,S111*AG111)),0)","v":0},{"$f":"IF($AF111=3,IF($AF$2=2,(T111/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I111,Refurb_Poss_Tbl[%]))*AG111,T111*$AG111),0)","v":0},{"$f":"IF($AF111=3,IF($AF$2=2,(Q111/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I111,Refurb_Poss_Tbl[%]))*AG111,Q111*$AG111),0)","v":0},{"$f":"IF($AF111=3,IF($AF$2=2,(U111/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I111,Refurb_Poss_Tbl[%]))*AG111,U111*$AG111),0)","v":0},{"$f":"IF($AF111=3,IF($AF$2=2,(V111/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I111,Refurb_Poss_Tbl[%]))*AG111,IF($AF$2=3,(V111*AG111)-AW111,V111*AG111)),0)","v":0},{"$f":"IF($AF111=3,IF($AF$2=2,(W111/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I111,Refurb_Poss_Tbl[%]))*AG111,W111*$AG111),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,9,0,{"$f":"VLOOKUP(AE112,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.73373097218961414},0,0,0,0,0,0,0,0,1.241628278117237E-3,{"$f":"IF(OR(AF112=3,AF112=2,AF112=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D112,FlatMaint!$Y$2:$Y$10000,AE112)*AG112,0)","v":19.990053611073463},{"$f":"IF(OR(AF112=3,AF112=2,AF112=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D112,FlatRepair!$Y$2:$Y$10000,AE112)*AG112,0)","v":0},0,19.991295239351579,0,0,0,0,0,19.991295239351579,0,{"$f":"IF($AF112=3,IF($AF$2=2,(R112/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I112,Refurb_Poss_Tbl[%]))*AG112,IF($AF$2=3,(R112*AG112)-AV112,R112*AG112)),0)","v":0},{"$f":"IF(AF112=3,IF($AF$2=2,(S112/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I112,Refurb_Poss_Tbl[%]))*AG112,IF($AF$2=3,(S112*AG112)-AX112,S112*AG112)),0)","v":0},{"$f":"IF($AF112=3,IF($AF$2=2,(T112/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I112,Refurb_Poss_Tbl[%]))*AG112,T112*$AG112),0)","v":0},{"$f":"IF($AF112=3,IF($AF$2=2,(Q112/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I112,Refurb_Poss_Tbl[%]))*AG112,Q112*$AG112),0)","v":0},{"$f":"IF($AF112=3,IF($AF$2=2,(U112/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I112,Refurb_Poss_Tbl[%]))*AG112,U112*$AG112),0)","v":0},{"$f":"IF($AF112=3,IF($AF$2=2,(V112/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I112,Refurb_Poss_Tbl[%]))*AG112,IF($AF$2=3,(V112*AG112)-AW112,V112*AG112)),0)","v":0},{"$f":"IF($AF112=3,IF($AF$2=2,(W112/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I112,Refurb_Poss_Tbl[%]))*AG112,W112*$AG112),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,10,0,{"$f":"VLOOKUP(AE113,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.70891881370977217},0,0,0,0,0,0,0,0,1.1996408484224513E-3,{"$f":"IF(OR(AF113=3,AF113=2,AF113=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D113,FlatMaint!$Y$2:$Y$10000,AE113)*AG113,0)","v":19.314061459974361},{"$f":"IF(OR(AF113=3,AF113=2,AF113=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D113,FlatRepair!$Y$2:$Y$10000,AE113)*AG113,0)","v":0},0,19.315261100822784,0,0,0,0,0,19.315261100822784,0,{"$f":"IF($AF113=3,IF($AF$2=2,(R113/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I113,Refurb_Poss_Tbl[%]))*AG113,IF($AF$2=3,(R113*AG113)-AV113,R113*AG113)),0)","v":0},{"$f":"IF(AF113=3,IF($AF$2=2,(S113/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I113,Refurb_Poss_Tbl[%]))*AG113,IF($AF$2=3,(S113*AG113)-AX113,S113*AG113)),0)","v":0},{"$f":"IF($AF113=3,IF($AF$2=2,(T113/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I113,Refurb_Poss_Tbl[%]))*AG113,T113*$AG113),0)","v":0},{"$f":"IF($AF113=3,IF($AF$2=2,(Q113/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I113,Refurb_Poss_Tbl[%]))*AG113,Q113*$AG113),0)","v":0},{"$f":"IF($AF113=3,IF($AF$2=2,(U113/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I113,Refurb_Poss_Tbl[%]))*AG113,U113*$AG113),0)","v":0},{"$f":"IF($AF113=3,IF($AF$2=2,(V113/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I113,Refurb_Poss_Tbl[%]))*AG113,IF($AF$2=3,(V113*AG113)-AW113,V113*AG113)),0)","v":0},{"$f":"IF($AF113=3,IF($AF$2=2,(W113/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I113,Refurb_Poss_Tbl[%]))*AG113,W113*$AG113),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,11,0,{"$f":"VLOOKUP(AE114,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.68494571372924851},0,0,0,0,0,0,0,0,1.1590732834999532E-3,{"$f":"IF(OR(AF114=3,AF114=2,AF114=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D114,FlatMaint!$Y$2:$Y$10000,AE114)*AG114,0)","v":18.660928946835135},{"$f":"IF(OR(AF114=3,AF114=2,AF114=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D114,FlatRepair!$Y$2:$Y$10000,AE114)*AG114,0)","v":0},0,18.662088020118635,0,0,0,0,0,18.662088020118635,0,{"$f":"IF($AF114=3,IF($AF$2=2,(R114/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I114,Refurb_Poss_Tbl[%]))*AG114,IF($AF$2=3,(R114*AG114)-AV114,R114*AG114)),0)","v":0},{"$f":"IF(AF114=3,IF($AF$2=2,(S114/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I114,Refurb_Poss_Tbl[%]))*AG114,IF($AF$2=3,(S114*AG114)-AX114,S114*AG114)),0)","v":0},{"$f":"IF($AF114=3,IF($AF$2=2,(T114/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I114,Refurb_Poss_Tbl[%]))*AG114,T114*$AG114),0)","v":0},{"$f":"IF($AF114=3,IF($AF$2=2,(Q114/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I114,Refurb_Poss_Tbl[%]))*AG114,Q114*$AG114),0)","v":0},{"$f":"IF($AF114=3,IF($AF$2=2,(U114/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I114,Refurb_Poss_Tbl[%]))*AG114,U114*$AG114),0)","v":0},{"$f":"IF($AF114=3,IF($AF$2=2,(V114/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I114,Refurb_Poss_Tbl[%]))*AG114,IF($AF$2=3,(V114*AG114)-AW114,V114*AG114)),0)","v":0},{"$f":"IF($AF114=3,IF($AF$2=2,(W114/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I114,Refurb_Poss_Tbl[%]))*AG114,W114*$AG114),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,12,0,{"$f":"VLOOKUP(AE115,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.66178329828912896},0,0,0,0,0,0,0,0,1.1198775685989884E-3,{"$f":"IF(OR(AF115=3,AF115=2,AF115=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D115,FlatMaint!$Y$2:$Y$10000,AE115)*AG115,0)","v":18.029883040420419},{"$f":"IF(OR(AF115=3,AF115=2,AF115=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D115,FlatRepair!$Y$2:$Y$10000,AE115)*AG115,0)","v":0},0,18.031002917989017,0,0,0,0,0,18.031002917989017,0,{"$f":"IF($AF115=3,IF($AF$2=2,(R115/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I115,Refurb_Poss_Tbl[%]))*AG115,IF($AF$2=3,(R115*AG115)-AV115,R115*AG115)),0)","v":0},{"$f":"IF(AF115=3,IF($AF$2=2,(S115/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I115,Refurb_Poss_Tbl[%]))*AG115,IF($AF$2=3,(S115*AG115)-AX115,S115*AG115)),0)","v":0},{"$f":"IF($AF115=3,IF($AF$2=2,(T115/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I115,Refurb_Poss_Tbl[%]))*AG115,T115*$AG115),0)","v":0},{"$f":"IF($AF115=3,IF($AF$2=2,(Q115/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I115,Refurb_Poss_Tbl[%]))*AG115,Q115*$AG115),0)","v":0},{"$f":"IF($AF115=3,IF($AF$2=2,(U115/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I115,Refurb_Poss_Tbl[%]))*AG115,U115*$AG115),0)","v":0},{"$f":"IF($AF115=3,IF($AF$2=2,(V115/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I115,Refurb_Poss_Tbl[%]))*AG115,IF($AF$2=3,(V115*AG115)-AW115,V115*AG115)),0)","v":0},{"$f":"IF($AF115=3,IF($AF$2=2,(W115/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I115,Refurb_Poss_Tbl[%]))*AG115,W115*$AG115),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,13,0,{"$f":"VLOOKUP(AE116,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.63940415293635666},0,0,0,0,0,0,0,0,1.0820073126560279E-3,{"$f":"IF(OR(AF116=3,AF116=2,AF116=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D116,FlatMaint!$Y$2:$Y$10000,AE116)*AG116,0)","v":17.420176850647753},{"$f":"IF(OR(AF116=3,AF116=2,AF116=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D116,FlatRepair!$Y$2:$Y$10000,AE116)*AG116,0)","v":0},0,17.42125885796041,0,0,0,0,0,17.42125885796041,0,{"$f":"IF($AF116=3,IF($AF$2=2,(R116/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I116,Refurb_Poss_Tbl[%]))*AG116,IF($AF$2=3,(R116*AG116)-AV116,R116*AG116)),0)","v":0},{"$f":"IF(AF116=3,IF($AF$2=2,(S116/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I116,Refurb_Poss_Tbl[%]))*AG116,IF($AF$2=3,(S116*AG116)-AX116,S116*AG116)),0)","v":0},{"$f":"IF($AF116=3,IF($AF$2=2,(T116/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I116,Refurb_Poss_Tbl[%]))*AG116,T116*$AG116),0)","v":0},{"$f":"IF($AF116=3,IF($AF$2=2,(Q116/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I116,Refurb_Poss_Tbl[%]))*AG116,Q116*$AG116),0)","v":0},{"$f":"IF($AF116=3,IF($AF$2=2,(U116/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I116,Refurb_Poss_Tbl[%]))*AG116,U116*$AG116),0)","v":0},{"$f":"IF($AF116=3,IF($AF$2=2,(V116/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I116,Refurb_Poss_Tbl[%]))*AG116,IF($AF$2=3,(V116*AG116)-AW116,V116*AG116)),0)","v":0},{"$f":"IF($AF116=3,IF($AF$2=2,(W116/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I116,Refurb_Poss_Tbl[%]))*AG116,W116*$AG116),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,14,0,{"$f":"VLOOKUP(AE117,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.61778179027667302},0,0,0,0,0,0,0,0,1.0454176933874662E-3,{"$f":"IF(OR(AF117=3,AF117=2,AF117=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D117,FlatMaint!$Y$2:$Y$10000,AE117)*AG117,0)","v":16.831088744587198},{"$f":"IF(OR(AF117=3,AF117=2,AF117=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D117,FlatRepair!$Y$2:$Y$10000,AE117)*AG117,0)","v":0},0,16.832134162280585,0,0,0,0,0,16.832134162280585,0,{"$f":"IF($AF117=3,IF($AF$2=2,(R117/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I117,Refurb_Poss_Tbl[%]))*AG117,IF($AF$2=3,(R117*AG117)-AV117,R117*AG117)),0)","v":0},{"$f":"IF(AF117=3,IF($AF$2=2,(S117/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I117,Refurb_Poss_Tbl[%]))*AG117,IF($AF$2=3,(S117*AG117)-AX117,S117*AG117)),0)","v":0},{"$f":"IF($AF117=3,IF($AF$2=2,(T117/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I117,Refurb_Poss_Tbl[%]))*AG117,T117*$AG117),0)","v":0},{"$f":"IF($AF117=3,IF($AF$2=2,(Q117/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I117,Refurb_Poss_Tbl[%]))*AG117,Q117*$AG117),0)","v":0},{"$f":"IF($AF117=3,IF($AF$2=2,(U117/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I117,Refurb_Poss_Tbl[%]))*AG117,U117*$AG117),0)","v":0},{"$f":"IF($AF117=3,IF($AF$2=2,(V117/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I117,Refurb_Poss_Tbl[%]))*AG117,IF($AF$2=3,(V117*AG117)-AW117,V117*AG117)),0)","v":0},{"$f":"IF($AF117=3,IF($AF$2=2,(W117/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I117,Refurb_Poss_Tbl[%]))*AG117,W117*$AG117),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,15,0,{"$f":"VLOOKUP(AE118,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.59689061862480497},0,0,0,0,0,0,0,0,1.010065404239098E-3,{"$f":"IF(OR(AF118=3,AF118=2,AF118=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D118,FlatMaint!$Y$2:$Y$10000,AE118)*AG118,0)","v":16.261921492354784},{"$f":"IF(OR(AF118=3,AF118=2,AF118=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D118,FlatRepair!$Y$2:$Y$10000,AE118)*AG118,0)","v":0},0,16.262931557759021,0,0,0,0,0,16.262931557759021,0,{"$f":"IF($AF118=3,IF($AF$2=2,(R118/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I118,Refurb_Poss_Tbl[%]))*AG118,IF($AF$2=3,(R118*AG118)-AV118,R118*AG118)),0)","v":0},{"$f":"IF(AF118=3,IF($AF$2=2,(S118/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I118,Refurb_Poss_Tbl[%]))*AG118,IF($AF$2=3,(S118*AG118)-AX118,S118*AG118)),0)","v":0},{"$f":"IF($AF118=3,IF($AF$2=2,(T118/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I118,Refurb_Poss_Tbl[%]))*AG118,T118*$AG118),0)","v":0},{"$f":"IF($AF118=3,IF($AF$2=2,(Q118/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I118,Refurb_Poss_Tbl[%]))*AG118,Q118*$AG118),0)","v":0},{"$f":"IF($AF118=3,IF($AF$2=2,(U118/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I118,Refurb_Poss_Tbl[%]))*AG118,U118*$AG118),0)","v":0},{"$f":"IF($AF118=3,IF($AF$2=2,(V118/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I118,Refurb_Poss_Tbl[%]))*AG118,IF($AF$2=3,(V118*AG118)-AW118,V118*AG118)),0)","v":0},{"$f":"IF($AF118=3,IF($AF$2=2,(W118/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I118,Refurb_Poss_Tbl[%]))*AG118,W118*$AG118),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,16,0,{"$f":"VLOOKUP(AE119,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.57670591171478747},0,0,0,0,0,0,0,0,9.7590860312956349E-4,{"$f":"IF(OR(AF119=3,AF119=2,AF119=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D119,FlatMaint!$Y$2:$Y$10000,AE119)*AG119,0)","v":15.712001441888681},{"$f":"IF(OR(AF119=3,AF119=2,AF119=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D119,FlatRepair!$Y$2:$Y$10000,AE119)*AG119,0)","v":0},0,15.71297735049181,0,0,0,0,0,15.71297735049181,0,{"$f":"IF($AF119=3,IF($AF$2=2,(R119/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I119,Refurb_Poss_Tbl[%]))*AG119,IF($AF$2=3,(R119*AG119)-AV119,R119*AG119)),0)","v":0},{"$f":"IF(AF119=3,IF($AF$2=2,(S119/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I119,Refurb_Poss_Tbl[%]))*AG119,IF($AF$2=3,(S119*AG119)-AX119,S119*AG119)),0)","v":0},{"$f":"IF($AF119=3,IF($AF$2=2,(T119/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I119,Refurb_Poss_Tbl[%]))*AG119,T119*$AG119),0)","v":0},{"$f":"IF($AF119=3,IF($AF$2=2,(Q119/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I119,Refurb_Poss_Tbl[%]))*AG119,Q119*$AG119),0)","v":0},{"$f":"IF($AF119=3,IF($AF$2=2,(U119/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I119,Refurb_Poss_Tbl[%]))*AG119,U119*$AG119),0)","v":0},{"$f":"IF($AF119=3,IF($AF$2=2,(V119/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I119,Refurb_Poss_Tbl[%]))*AG119,IF($AF$2=3,(V119*AG119)-AW119,V119*AG119)),0)","v":0},{"$f":"IF($AF119=3,IF($AF$2=2,(W119/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I119,Refurb_Poss_Tbl[%]))*AG119,W119*$AG119),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,17,0,{"$f":"VLOOKUP(AE120,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.55720377943457733},0,0,0,0,0,0,0,0,9.4290686292711461E-4,{"$f":"IF(OR(AF120=3,AF120=2,AF120=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D120,FlatMaint!$Y$2:$Y$10000,AE120)*AG120,0)","v":15.180677721631579},{"$f":"IF(OR(AF120=3,AF120=2,AF120=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D120,FlatRepair!$Y$2:$Y$10000,AE120)*AG120,0)","v":0},0,15.181620628494505,0,0,0,0,0,15.181620628494505,0,{"$f":"IF($AF120=3,IF($AF$2=2,(R120/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I120,Refurb_Poss_Tbl[%]))*AG120,IF($AF$2=3,(R120*AG120)-AV120,R120*AG120)),0)","v":0},{"$f":"IF(AF120=3,IF($AF$2=2,(S120/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I120,Refurb_Poss_Tbl[%]))*AG120,IF($AF$2=3,(S120*AG120)-AX120,S120*AG120)),0)","v":0},{"$f":"IF($AF120=3,IF($AF$2=2,(T120/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I120,Refurb_Poss_Tbl[%]))*AG120,T120*$AG120),0)","v":0},{"$f":"IF($AF120=3,IF($AF$2=2,(Q120/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I120,Refurb_Poss_Tbl[%]))*AG120,Q120*$AG120),0)","v":0},{"$f":"IF($AF120=3,IF($AF$2=2,(U120/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I120,Refurb_Poss_Tbl[%]))*AG120,U120*$AG120),0)","v":0},{"$f":"IF($AF120=3,IF($AF$2=2,(V120/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I120,Refurb_Poss_Tbl[%]))*AG120,IF($AF$2=3,(V120*AG120)-AW120,V120*AG120)),0)","v":0},{"$f":"IF($AF120=3,IF($AF$2=2,(W120/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I120,Refurb_Poss_Tbl[%]))*AG120,W120*$AG120),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,18,0,{"$f":"VLOOKUP(AE121,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.53836113955031628},0,0,0,0,0,0,0,0,9.1102112360107689E-4,{"$f":"IF(OR(AF121=3,AF121=2,AF121=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D121,FlatMaint!$Y$2:$Y$10000,AE121)*AG121,0)","v":14.667321470175439},{"$f":"IF(OR(AF121=3,AF121=2,AF121=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D121,FlatRepair!$Y$2:$Y$10000,AE121)*AG121,0)","v":0},0,14.66823249129904,0,0,0,0,0,14.66823249129904,0,{"$f":"IF($AF121=3,IF($AF$2=2,(R121/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I121,Refurb_Poss_Tbl[%]))*AG121,IF($AF$2=3,(R121*AG121)-AV121,R121*AG121)),0)","v":0},{"$f":"IF(AF121=3,IF($AF$2=2,(S121/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I121,Refurb_Poss_Tbl[%]))*AG121,IF($AF$2=3,(S121*AG121)-AX121,S121*AG121)),0)","v":0},{"$f":"IF($AF121=3,IF($AF$2=2,(T121/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I121,Refurb_Poss_Tbl[%]))*AG121,T121*$AG121),0)","v":0},{"$f":"IF($AF121=3,IF($AF$2=2,(Q121/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I121,Refurb_Poss_Tbl[%]))*AG121,Q121*$AG121),0)","v":0},{"$f":"IF($AF121=3,IF($AF$2=2,(U121/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I121,Refurb_Poss_Tbl[%]))*AG121,U121*$AG121),0)","v":0},{"$f":"IF($AF121=3,IF($AF$2=2,(V121/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I121,Refurb_Poss_Tbl[%]))*AG121,IF($AF$2=3,(V121*AG121)-AW121,V121*AG121)),0)","v":0},{"$f":"IF($AF121=3,IF($AF$2=2,(W121/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I121,Refurb_Poss_Tbl[%]))*AG121,W121*$AG121),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,19,0,{"$f":"VLOOKUP(AE122,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.52015569038677911},0,0,0,0,0,0,0,0,8.8021364599137879E-4,{"$f":"IF(OR(AF122=3,AF122=2,AF122=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D122,FlatMaint!$Y$2:$Y$10000,AE122)*AG122,0)","v":14.171325091956948},{"$f":"IF(OR(AF122=3,AF122=2,AF122=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D122,FlatRepair!$Y$2:$Y$10000,AE122)*AG122,0)","v":0},0,14.17220530560294,0,0,0,0,0,14.17220530560294,0,{"$f":"IF($AF122=3,IF($AF$2=2,(R122/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I122,Refurb_Poss_Tbl[%]))*AG122,IF($AF$2=3,(R122*AG122)-AV122,R122*AG122)),0)","v":0},{"$f":"IF(AF122=3,IF($AF$2=2,(S122/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I122,Refurb_Poss_Tbl[%]))*AG122,IF($AF$2=3,(S122*AG122)-AX122,S122*AG122)),0)","v":0},{"$f":"IF($AF122=3,IF($AF$2=2,(T122/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I122,Refurb_Poss_Tbl[%]))*AG122,T122*$AG122),0)","v":0},{"$f":"IF($AF122=3,IF($AF$2=2,(Q122/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I122,Refurb_Poss_Tbl[%]))*AG122,Q122*$AG122),0)","v":0},{"$f":"IF($AF122=3,IF($AF$2=2,(U122/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I122,Refurb_Poss_Tbl[%]))*AG122,U122*$AG122),0)","v":0},{"$f":"IF($AF122=3,IF($AF$2=2,(V122/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I122,Refurb_Poss_Tbl[%]))*AG122,IF($AF$2=3,(V122*AG122)-AW122,V122*AG122)),0)","v":0},{"$f":"IF($AF122=3,IF($AF$2=2,(W122/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I122,Refurb_Poss_Tbl[%]))*AG122,W122*$AG122),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,20,0,{"$f":"VLOOKUP(AE123,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.50256588443167061},0,0,0,0,0,0,0,0,8.5044796714142874E-4,{"$f":"IF(OR(AF123=3,AF123=2,AF123=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D123,FlatMaint!$Y$2:$Y$10000,AE123)*AG123,0)","v":13.692101538122655},{"$f":"IF(OR(AF123=3,AF123=2,AF123=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D123,FlatRepair!$Y$2:$Y$10000,AE123)*AG123,0)","v":0},0,13.692951986089797,0,0,0,0,0,13.692951986089797,0,{"$f":"IF($AF123=3,IF($AF$2=2,(R123/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I123,Refurb_Poss_Tbl[%]))*AG123,IF($AF$2=3,(R123*AG123)-AV123,R123*AG123)),0)","v":0},{"$f":"IF(AF123=3,IF($AF$2=2,(S123/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I123,Refurb_Poss_Tbl[%]))*AG123,IF($AF$2=3,(S123*AG123)-AX123,S123*AG123)),0)","v":0},{"$f":"IF($AF123=3,IF($AF$2=2,(T123/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I123,Refurb_Poss_Tbl[%]))*AG123,T123*$AG123),0)","v":0},{"$f":"IF($AF123=3,IF($AF$2=2,(Q123/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I123,Refurb_Poss_Tbl[%]))*AG123,Q123*$AG123),0)","v":0},{"$f":"IF($AF123=3,IF($AF$2=2,(U123/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I123,Refurb_Poss_Tbl[%]))*AG123,U123*$AG123),0)","v":0},{"$f":"IF($AF123=3,IF($AF$2=2,(V123/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I123,Refurb_Poss_Tbl[%]))*AG123,IF($AF$2=3,(V123*AG123)-AW123,V123*AG123)),0)","v":0},{"$f":"IF($AF123=3,IF($AF$2=2,(W123/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I123,Refurb_Poss_Tbl[%]))*AG123,W123*$AG123),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,21,0,{"$f":"VLOOKUP(AE124,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.48557090283253213},0,0,0,0,0,0,0,0,8.2168885714147726E-4,{"$f":"IF(OR(AF124=3,AF124=2,AF124=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D124,FlatMaint!$Y$2:$Y$10000,AE124)*AG124,0)","v":13.229083611712714},{"$f":"IF(OR(AF124=3,AF124=2,AF124=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D124,FlatRepair!$Y$2:$Y$10000,AE124)*AG124,0)","v":0},0,13.229905300569856,0,0,0,0,0,13.229905300569856,0,{"$f":"IF($AF124=3,IF($AF$2=2,(R124/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I124,Refurb_Poss_Tbl[%]))*AG124,IF($AF$2=3,(R124*AG124)-AV124,R124*AG124)),0)","v":0},{"$f":"IF(AF124=3,IF($AF$2=2,(S124/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I124,Refurb_Poss_Tbl[%]))*AG124,IF($AF$2=3,(S124*AG124)-AX124,S124*AG124)),0)","v":0},{"$f":"IF($AF124=3,IF($AF$2=2,(T124/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I124,Refurb_Poss_Tbl[%]))*AG124,T124*$AG124),0)","v":0},{"$f":"IF($AF124=3,IF($AF$2=2,(Q124/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I124,Refurb_Poss_Tbl[%]))*AG124,Q124*$AG124),0)","v":0},{"$f":"IF($AF124=3,IF($AF$2=2,(U124/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I124,Refurb_Poss_Tbl[%]))*AG124,U124*$AG124),0)","v":0},{"$f":"IF($AF124=3,IF($AF$2=2,(V124/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I124,Refurb_Poss_Tbl[%]))*AG124,IF($AF$2=3,(V124*AG124)-AW124,V124*AG124)),0)","v":0},{"$f":"IF($AF124=3,IF($AF$2=2,(W124/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I124,Refurb_Poss_Tbl[%]))*AG124,W124*$AG124),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,22,0,{"$f":"VLOOKUP(AE125,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.46915063075606966},0,0,0,0,0,0,0,0,7.9390227743137895E-4,{"$f":"IF(OR(AF125=3,AF125=2,AF125=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D125,FlatMaint!$Y$2:$Y$10000,AE125)*AG125,0)","v":12.781723296340784},{"$f":"IF(OR(AF125=3,AF125=2,AF125=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D125,FlatRepair!$Y$2:$Y$10000,AE125)*AG125,0)","v":0},0,12.782517198618216,0,0,0,0,0,12.782517198618216,0,{"$f":"IF($AF125=3,IF($AF$2=2,(R125/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I125,Refurb_Poss_Tbl[%]))*AG125,IF($AF$2=3,(R125*AG125)-AV125,R125*AG125)),0)","v":0},{"$f":"IF(AF125=3,IF($AF$2=2,(S125/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I125,Refurb_Poss_Tbl[%]))*AG125,IF($AF$2=3,(S125*AG125)-AX125,S125*AG125)),0)","v":0},{"$f":"IF($AF125=3,IF($AF$2=2,(T125/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I125,Refurb_Poss_Tbl[%]))*AG125,T125*$AG125),0)","v":0},{"$f":"IF($AF125=3,IF($AF$2=2,(Q125/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I125,Refurb_Poss_Tbl[%]))*AG125,Q125*$AG125),0)","v":0},{"$f":"IF($AF125=3,IF($AF$2=2,(U125/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I125,Refurb_Poss_Tbl[%]))*AG125,U125*$AG125),0)","v":0},{"$f":"IF($AF125=3,IF($AF$2=2,(V125/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I125,Refurb_Poss_Tbl[%]))*AG125,IF($AF$2=3,(V125*AG125)-AW125,V125*AG125)),0)","v":0},{"$f":"IF($AF125=3,IF($AF$2=2,(W125/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I125,Refurb_Poss_Tbl[%]))*AG125,W125*$AG125),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,23,0,{"$f":"VLOOKUP(AE126,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.45328563358074364},0,0,0,0,0,0,0,0,7.6705534051340967E-4,{"$f":"IF(OR(AF126=3,AF126=2,AF126=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D126,FlatMaint!$Y$2:$Y$10000,AE126)*AG126,0)","v":12.349491107575638},{"$f":"IF(OR(AF126=3,AF126=2,AF126=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D126,FlatRepair!$Y$2:$Y$10000,AE126)*AG126,0)","v":0},0,12.350258162916152,0,0,0,0,0,12.350258162916152,0,{"$f":"IF($AF126=3,IF($AF$2=2,(R126/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I126,Refurb_Poss_Tbl[%]))*AG126,IF($AF$2=3,(R126*AG126)-AV126,R126*AG126)),0)","v":0},{"$f":"IF(AF126=3,IF($AF$2=2,(S126/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I126,Refurb_Poss_Tbl[%]))*AG126,IF($AF$2=3,(S126*AG126)-AX126,S126*AG126)),0)","v":0},{"$f":"IF($AF126=3,IF($AF$2=2,(T126/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I126,Refurb_Poss_Tbl[%]))*AG126,T126*$AG126),0)","v":0},{"$f":"IF($AF126=3,IF($AF$2=2,(Q126/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I126,Refurb_Poss_Tbl[%]))*AG126,Q126*$AG126),0)","v":0},{"$f":"IF($AF126=3,IF($AF$2=2,(U126/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I126,Refurb_Poss_Tbl[%]))*AG126,U126*$AG126),0)","v":0},{"$f":"IF($AF126=3,IF($AF$2=2,(V126/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I126,Refurb_Poss_Tbl[%]))*AG126,IF($AF$2=3,(V126*AG126)-AW126,V126*AG126)),0)","v":0},{"$f":"IF($AF126=3,IF($AF$2=2,(W126/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I126,Refurb_Poss_Tbl[%]))*AG126,W126*$AG126),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,24,0,{"$f":"VLOOKUP(AE127,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.43795713389443841},0,0,0,0,0,0,0,0,7.4111627102744918E-4,{"$f":"IF(OR(AF127=3,AF127=2,AF127=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D127,FlatMaint!$Y$2:$Y$10000,AE127)*AG127,0)","v":11.931875466256658},{"$f":"IF(OR(AF127=3,AF127=2,AF127=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D127,FlatRepair!$Y$2:$Y$10000,AE127)*AG127,0)","v":0},0,11.932616582527686,0,0,0,0,0,11.932616582527686,0,{"$f":"IF($AF127=3,IF($AF$2=2,(R127/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I127,Refurb_Poss_Tbl[%]))*AG127,IF($AF$2=3,(R127*AG127)-AV127,R127*AG127)),0)","v":0},{"$f":"IF(AF127=3,IF($AF$2=2,(S127/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I127,Refurb_Poss_Tbl[%]))*AG127,IF($AF$2=3,(S127*AG127)-AX127,S127*AG127)),0)","v":0},{"$f":"IF($AF127=3,IF($AF$2=2,(T127/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I127,Refurb_Poss_Tbl[%]))*AG127,T127*$AG127),0)","v":0},{"$f":"IF($AF127=3,IF($AF$2=2,(Q127/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I127,Refurb_Poss_Tbl[%]))*AG127,Q127*$AG127),0)","v":0},{"$f":"IF($AF127=3,IF($AF$2=2,(U127/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I127,Refurb_Poss_Tbl[%]))*AG127,U127*$AG127),0)","v":0},{"$f":"IF($AF127=3,IF($AF$2=2,(V127/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I127,Refurb_Poss_Tbl[%]))*AG127,IF($AF$2=3,(V127*AG127)-AW127,V127*AG127)),0)","v":0},{"$f":"IF($AF127=3,IF($AF$2=2,(W127/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I127,Refurb_Poss_Tbl[%]))*AG127,W127*$AG127),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,25,0,{"$f":"VLOOKUP(AE128,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.42314698926998884},0,0,0,0,0,0,0,0,7.1605436814246295E-4,{"$f":"IF(OR(AF128=3,AF128=2,AF128=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D128,FlatMaint!$Y$2:$Y$10000,AE128)*AG128,0)","v":11.528382093001603},{"$f":"IF(OR(AF128=3,AF128=2,AF128=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D128,FlatRepair!$Y$2:$Y$10000,AE128)*AG128,0)","v":0},0,11.529098147369746,0,0,0,0,0,11.529098147369746,0,{"$f":"IF($AF128=3,IF($AF$2=2,(R128/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I128,Refurb_Poss_Tbl[%]))*AG128,IF($AF$2=3,(R128*AG128)-AV128,R128*AG128)),0)","v":0},{"$f":"IF(AF128=3,IF($AF$2=2,(S128/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I128,Refurb_Poss_Tbl[%]))*AG128,IF($AF$2=3,(S128*AG128)-AX128,S128*AG128)),0)","v":0},{"$f":"IF($AF128=3,IF($AF$2=2,(T128/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I128,Refurb_Poss_Tbl[%]))*AG128,T128*$AG128),0)","v":0},{"$f":"IF($AF128=3,IF($AF$2=2,(Q128/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I128,Refurb_Poss_Tbl[%]))*AG128,Q128*$AG128),0)","v":0},{"$f":"IF($AF128=3,IF($AF$2=2,(U128/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I128,Refurb_Poss_Tbl[%]))*AG128,U128*$AG128),0)","v":0},{"$f":"IF($AF128=3,IF($AF$2=2,(V128/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I128,Refurb_Poss_Tbl[%]))*AG128,IF($AF$2=3,(V128*AG128)-AW128,V128*AG128)),0)","v":0},{"$f":"IF($AF128=3,IF($AF$2=2,(W128/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I128,Refurb_Poss_Tbl[%]))*AG128,W128*$AG128),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,26,0,{"$f":"VLOOKUP(AE129,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.40883767079225974},0,0,0,0,0,0,0,0,6.9183996921977104E-4,{"$f":"IF(OR(AF129=3,AF129=2,AF129=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D129,FlatMaint!$Y$2:$Y$10000,AE129)*AG129,0)","v":11.138533423189955},{"$f":"IF(OR(AF129=3,AF129=2,AF129=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D129,FlatRepair!$Y$2:$Y$10000,AE129)*AG129,0)","v":0},0,11.139225263159174,0,0,0,0,0,11.139225263159174,0,{"$f":"IF($AF129=3,IF($AF$2=2,(R129/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I129,Refurb_Poss_Tbl[%]))*AG129,IF($AF$2=3,(R129*AG129)-AV129,R129*AG129)),0)","v":0},{"$f":"IF(AF129=3,IF($AF$2=2,(S129/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I129,Refurb_Poss_Tbl[%]))*AG129,IF($AF$2=3,(S129*AG129)-AX129,S129*AG129)),0)","v":0},{"$f":"IF($AF129=3,IF($AF$2=2,(T129/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I129,Refurb_Poss_Tbl[%]))*AG129,T129*$AG129),0)","v":0},{"$f":"IF($AF129=3,IF($AF$2=2,(Q129/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I129,Refurb_Poss_Tbl[%]))*AG129,Q129*$AG129),0)","v":0},{"$f":"IF($AF129=3,IF($AF$2=2,(U129/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I129,Refurb_Poss_Tbl[%]))*AG129,U129*$AG129),0)","v":0},{"$f":"IF($AF129=3,IF($AF$2=2,(V129/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I129,Refurb_Poss_Tbl[%]))*AG129,IF($AF$2=3,(V129*AG129)-AW129,V129*AG129)),0)","v":0},{"$f":"IF($AF129=3,IF($AF$2=2,(W129/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I129,Refurb_Poss_Tbl[%]))*AG129,W129*$AG129),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,27,0,{"$f":"VLOOKUP(AE130,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39501224231136206},0,0,0,0,0,0,0,0,6.6844441470509277E-4,{"$f":"IF(OR(AF130=3,AF130=2,AF130=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D130,FlatMaint!$Y$2:$Y$10000,AE130)*AG130,0)","v":10.761868041729425},{"$f":"IF(OR(AF130=3,AF130=2,AF130=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D130,FlatRepair!$Y$2:$Y$10000,AE130)*AG130,0)","v":0},0,10.76253648614413,0,0,0,0,0,10.76253648614413,0,{"$f":"IF($AF130=3,IF($AF$2=2,(R130/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I130,Refurb_Poss_Tbl[%]))*AG130,IF($AF$2=3,(R130*AG130)-AV130,R130*AG130)),0)","v":0},{"$f":"IF(AF130=3,IF($AF$2=2,(S130/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I130,Refurb_Poss_Tbl[%]))*AG130,IF($AF$2=3,(S130*AG130)-AX130,S130*AG130)),0)","v":0},{"$f":"IF($AF130=3,IF($AF$2=2,(T130/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I130,Refurb_Poss_Tbl[%]))*AG130,T130*$AG130),0)","v":0},{"$f":"IF($AF130=3,IF($AF$2=2,(Q130/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I130,Refurb_Poss_Tbl[%]))*AG130,Q130*$AG130),0)","v":0},{"$f":"IF($AF130=3,IF($AF$2=2,(U130/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I130,Refurb_Poss_Tbl[%]))*AG130,U130*$AG130),0)","v":0},{"$f":"IF($AF130=3,IF($AF$2=2,(V130/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I130,Refurb_Poss_Tbl[%]))*AG130,IF($AF$2=3,(V130*AG130)-AW130,V130*AG130)),0)","v":0},{"$f":"IF($AF130=3,IF($AF$2=2,(W130/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I130,Refurb_Poss_Tbl[%]))*AG130,W130*$AG130),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,28,0,{"$f":"VLOOKUP(AE131,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38165434039745127},{"$f":"IF(AE131=0,Q131*AG131,0)","v":0},{"$f":"IF(AE131=0,R131*AG131,0)","v":0},{"$f":"IF(AE131=0,S131*AG131,0)","v":0},{"$f":"IF(AE131=0,T131*AG131,0)","v":0},{"$f":"IF(AE131=0,U131*AG131,0)","v":0},{"$f":"IF(AE131=0,V131*AG131,0)","v":0},{"$f":"IF(AE131=0,W131*AG131,0)","v":0},{"$f":"IF(AE131=0,AH131+AI131+AJ131+AK131+AL131+AM131+AN131,0)","v":0},{"$f":"IF(OR(AF131=3,AF131=2,AF131=0),Y131*AG131,0)","v":6.4584001420781912E-4},{"$f":"IF(OR(AF131=3,AF131=2,AF131=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D131,FlatMaint!$Y$2:$Y$10000,AE131)*AG131,0)","v":10.397940136936642},{"$f":"IF(OR(AF131=3,AF131=2,AF131=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D131,FlatRepair!$Y$2:$Y$10000,AE131)*AG131,0)","v":0},{"$f":"IF(OR(AF131=3,AF131=2,AF131=0),Z131*AG131,0)","v":0},{"$f":"AP131+AQ131+AR131+AS131","v":10.39858597695085},{"$f":"IF(AF131=2,AA131*AG131,0)","v":0},{"$f":"IF(AF131=3,AB131*AG131,0)","v":0},{"$f":"IF(AF131=3,AC131*AG131,0)","v":0},{"$f":"IF(AF131=3,AD131*AG131,0)","v":0},{"$f":"IF($AF$2=3,BB131+BC131+BD131+BE131+BF131+BG131+BH131,BB131+BC131+BD131+BE131+BF131+BG131+BH131)","v":0},{"$f":"AO131+AT131+AU131+AV131+AW131+AX131+AY131+BA131","v":10.39858597695085},{"$f":"IFERROR(IF(AE131=100,IF(O131=3,(N131/H131)*(X131*AG131)*-1,(N131/M131)*(X131*AG131)*-1),0),0)","v":0},{"$f":"IF($AF131=3,IF($AF$2=2,(R131/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I131,Refurb_Poss_Tbl[%]))*AG131,IF($AF$2=3,(R131*AG131)-AV131,R131*AG131)),0)","v":0},{"$f":"IF(AF131=3,IF($AF$2=2,(S131/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I131,Refurb_Poss_Tbl[%]))*AG131,IF($AF$2=3,(S131*AG131)-AX131,S131*AG131)),0)","v":0},{"$f":"IF($AF131=3,IF($AF$2=2,(T131/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I131,Refurb_Poss_Tbl[%]))*AG131,T131*$AG131),0)","v":0},{"$f":"IF($AF131=3,IF($AF$2=2,(Q131/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I131,Refurb_Poss_Tbl[%]))*AG131,Q131*$AG131),0)","v":0},{"$f":"IF($AF131=3,IF($AF$2=2,(U131/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I131,Refurb_Poss_Tbl[%]))*AG131,U131*$AG131),0)","v":0},{"$f":"IF($AF131=3,IF($AF$2=2,(V131/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I131,Refurb_Poss_Tbl[%]))*AG131,IF($AF$2=3,(V131*AG131)-AW131,V131*AG131)),0)","v":0},{"$f":"IF($AF131=3,IF($AF$2=2,(W131/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I131,Refurb_Poss_Tbl[%]))*AG131,W131*$AG131),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,29,0,{"$f":"VLOOKUP(AE132,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36874815497338298},0,0,0,0,0,0,0,0,6.2400001372736158E-4,{"$f":"IF(OR(AF132=3,AF132=2,AF132=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D132,FlatMaint!$Y$2:$Y$10000,AE132)*AG132,0)","v":10.046318972885647},{"$f":"IF(OR(AF132=3,AF132=2,AF132=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D132,FlatRepair!$Y$2:$Y$10000,AE132)*AG132,0)","v":0},0,10.046942972899375,0,0,0,0,0,10.046942972899375,0,{"$f":"IF($AF132=3,IF($AF$2=2,(R132/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I132,Refurb_Poss_Tbl[%]))*AG132,IF($AF$2=3,(R132*AG132)-AV132,R132*AG132)),0)","v":0},{"$f":"IF(AF132=3,IF($AF$2=2,(S132/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I132,Refurb_Poss_Tbl[%]))*AG132,IF($AF$2=3,(S132*AG132)-AX132,S132*AG132)),0)","v":0},{"$f":"IF($AF132=3,IF($AF$2=2,(T132/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I132,Refurb_Poss_Tbl[%]))*AG132,T132*$AG132),0)","v":0},{"$f":"IF($AF132=3,IF($AF$2=2,(Q132/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I132,Refurb_Poss_Tbl[%]))*AG132,Q132*$AG132),0)","v":0},{"$f":"IF($AF132=3,IF($AF$2=2,(U132/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I132,Refurb_Poss_Tbl[%]))*AG132,U132*$AG132),0)","v":0},{"$f":"IF($AF132=3,IF($AF$2=2,(V132/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I132,Refurb_Poss_Tbl[%]))*AG132,IF($AF$2=3,(V132*AG132)-AW132,V132*AG132)),0)","v":0},{"$f":"IF($AF132=3,IF($AF$2=2,(W132/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I132,Refurb_Poss_Tbl[%]))*AG132,W132*$AG132),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,30,0,{"$f":"VLOOKUP(AE133,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35627841060230236},0,0,0,0,0,0,0,0,6.0289856398778891E-4,{"$f":"IF(OR(AF133=3,AF133=2,AF133=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D133,FlatMaint!$Y$2:$Y$10000,AE133)*AG133,0)","v":9.7065883795996584},{"$f":"IF(OR(AF133=3,AF133=2,AF133=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D133,FlatRepair!$Y$2:$Y$10000,AE133)*AG133,0)","v":0},0,9.7071912781636467,0,0,0,0,0,9.7071912781636467,0,{"$f":"IF($AF133=3,IF($AF$2=2,(R133/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I133,Refurb_Poss_Tbl[%]))*AG133,IF($AF$2=3,(R133*AG133)-AV133,R133*AG133)),0)","v":0},{"$f":"IF(AF133=3,IF($AF$2=2,(S133/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I133,Refurb_Poss_Tbl[%]))*AG133,IF($AF$2=3,(S133*AG133)-AX133,S133*AG133)),0)","v":0},{"$f":"IF($AF133=3,IF($AF$2=2,(T133/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I133,Refurb_Poss_Tbl[%]))*AG133,T133*$AG133),0)","v":0},{"$f":"IF($AF133=3,IF($AF$2=2,(Q133/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I133,Refurb_Poss_Tbl[%]))*AG133,Q133*$AG133),0)","v":0},{"$f":"IF($AF133=3,IF($AF$2=2,(U133/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I133,Refurb_Poss_Tbl[%]))*AG133,U133*$AG133),0)","v":0},{"$f":"IF($AF133=3,IF($AF$2=2,(V133/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I133,Refurb_Poss_Tbl[%]))*AG133,IF($AF$2=3,(V133*AG133)-AW133,V133*AG133)),0)","v":0},{"$f":"IF($AF133=3,IF($AF$2=2,(W133/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I133,Refurb_Poss_Tbl[%]))*AG133,W133*$AG133),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,31,0,{"$f":"VLOOKUP(AE134,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39998714516107459},0,0,0,0,0,0,0,0,6.7686300447874733E-4,{"$f":"IF(OR(AF134=3,AF134=2,AF134=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D134,FlatMaint!$Y$2:$Y$10000,AE134)*AG134,0)","v":10.897406240940041},{"$f":"IF(OR(AF134=3,AF134=2,AF134=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D134,FlatRepair!$Y$2:$Y$10000,AE134)*AG134,0)","v":0},0,10.89808310394452,0,0,0,0,0,10.89808310394452,0,{"$f":"IF($AF134=3,IF($AF$2=2,(R134/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I134,Refurb_Poss_Tbl[%]))*AG134,IF($AF$2=3,(R134*AG134)-AV134,R134*AG134)),0)","v":0},{"$f":"IF(AF134=3,IF($AF$2=2,(S134/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I134,Refurb_Poss_Tbl[%]))*AG134,IF($AF$2=3,(S134*AG134)-AX134,S134*AG134)),0)","v":0},{"$f":"IF($AF134=3,IF($AF$2=2,(T134/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I134,Refurb_Poss_Tbl[%]))*AG134,T134*$AG134),0)","v":0},{"$f":"IF($AF134=3,IF($AF$2=2,(Q134/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I134,Refurb_Poss_Tbl[%]))*AG134,Q134*$AG134),0)","v":0},{"$f":"IF($AF134=3,IF($AF$2=2,(U134/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I134,Refurb_Poss_Tbl[%]))*AG134,U134*$AG134),0)","v":0},{"$f":"IF($AF134=3,IF($AF$2=2,(V134/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I134,Refurb_Poss_Tbl[%]))*AG134,IF($AF$2=3,(V134*AG134)-AW134,V134*AG134)),0)","v":0},{"$f":"IF($AF134=3,IF($AF$2=2,(W134/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I134,Refurb_Poss_Tbl[%]))*AG134,W134*$AG134),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,32,0,{"$f":"VLOOKUP(AE135,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38833703413696569},0,0,0,0,0,0,0,0,6.5714854803761884E-4,{"$f":"IF(OR(AF135=3,AF135=2,AF135=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D135,FlatMaint!$Y$2:$Y$10000,AE135)*AG135,0)","v":10.58000605916509},{"$f":"IF(OR(AF135=3,AF135=2,AF135=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D135,FlatRepair!$Y$2:$Y$10000,AE135)*AG135,0)","v":0},0,10.580663207713128,0,0,0,0,0,10.580663207713128,0,{"$f":"IF($AF135=3,IF($AF$2=2,(R135/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I135,Refurb_Poss_Tbl[%]))*AG135,IF($AF$2=3,(R135*AG135)-AV135,R135*AG135)),0)","v":0},{"$f":"IF(AF135=3,IF($AF$2=2,(S135/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I135,Refurb_Poss_Tbl[%]))*AG135,IF($AF$2=3,(S135*AG135)-AX135,S135*AG135)),0)","v":0},{"$f":"IF($AF135=3,IF($AF$2=2,(T135/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I135,Refurb_Poss_Tbl[%]))*AG135,T135*$AG135),0)","v":0},{"$f":"IF($AF135=3,IF($AF$2=2,(Q135/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I135,Refurb_Poss_Tbl[%]))*AG135,Q135*$AG135),0)","v":0},{"$f":"IF($AF135=3,IF($AF$2=2,(U135/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I135,Refurb_Poss_Tbl[%]))*AG135,U135*$AG135),0)","v":0},{"$f":"IF($AF135=3,IF($AF$2=2,(V135/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I135,Refurb_Poss_Tbl[%]))*AG135,IF($AF$2=3,(V135*AG135)-AW135,V135*AG135)),0)","v":0},{"$f":"IF($AF135=3,IF($AF$2=2,(W135/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I135,Refurb_Poss_Tbl[%]))*AG135,W135*$AG135),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,33,0,{"$f":"VLOOKUP(AE136,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.37702624673491814},0,0,0,0,0,0,0,0,6.3800829906564933E-4,{"$f":"IF(OR(AF136=3,AF136=2,AF136=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D136,FlatMaint!$Y$2:$Y$10000,AE136)*AG136,0)","v":10.271850542878729},{"$f":"IF(OR(AF136=3,AF136=2,AF136=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D136,FlatRepair!$Y$2:$Y$10000,AE136)*AG136,0)","v":0},0,10.272488551177794,0,0,0,0,0,10.272488551177794,0,{"$f":"IF($AF136=3,IF($AF$2=2,(R136/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I136,Refurb_Poss_Tbl[%]))*AG136,IF($AF$2=3,(R136*AG136)-AV136,R136*AG136)),0)","v":0},{"$f":"IF(AF136=3,IF($AF$2=2,(S136/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I136,Refurb_Poss_Tbl[%]))*AG136,IF($AF$2=3,(S136*AG136)-AX136,S136*AG136)),0)","v":0},{"$f":"IF($AF136=3,IF($AF$2=2,(T136/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I136,Refurb_Poss_Tbl[%]))*AG136,T136*$AG136),0)","v":0},{"$f":"IF($AF136=3,IF($AF$2=2,(Q136/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I136,Refurb_Poss_Tbl[%]))*AG136,Q136*$AG136),0)","v":0},{"$f":"IF($AF136=3,IF($AF$2=2,(U136/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I136,Refurb_Poss_Tbl[%]))*AG136,U136*$AG136),0)","v":0},{"$f":"IF($AF136=3,IF($AF$2=2,(V136/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I136,Refurb_Poss_Tbl[%]))*AG136,IF($AF$2=3,(V136*AG136)-AW136,V136*AG136)),0)","v":0},{"$f":"IF($AF136=3,IF($AF$2=2,(W136/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I136,Refurb_Poss_Tbl[%]))*AG136,W136*$AG136),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,34,0,{"$f":"VLOOKUP(AE137,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36604489974263904},0,0,0,0,0,0,0,0,6.1942553307344612E-4,{"$f":"IF(OR(AF137=3,AF137=2,AF137=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D137,FlatMaint!$Y$2:$Y$10000,AE137)*AG137,0)","v":9.9726704299793507},{"$f":"IF(OR(AF137=3,AF137=2,AF137=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D137,FlatRepair!$Y$2:$Y$10000,AE137)*AG137,0)","v":0},0,9.9732898555124248,0,0,0,0,0,9.9732898555124248,0,{"$f":"IF($AF137=3,IF($AF$2=2,(R137/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I137,Refurb_Poss_Tbl[%]))*AG137,IF($AF$2=3,(R137*AG137)-AV137,R137*AG137)),0)","v":0},{"$f":"IF(AF137=3,IF($AF$2=2,(S137/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I137,Refurb_Poss_Tbl[%]))*AG137,IF($AF$2=3,(S137*AG137)-AX137,S137*AG137)),0)","v":0},{"$f":"IF($AF137=3,IF($AF$2=2,(T137/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I137,Refurb_Poss_Tbl[%]))*AG137,T137*$AG137),0)","v":0},{"$f":"IF($AF137=3,IF($AF$2=2,(Q137/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I137,Refurb_Poss_Tbl[%]))*AG137,Q137*$AG137),0)","v":0},{"$f":"IF($AF137=3,IF($AF$2=2,(U137/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I137,Refurb_Poss_Tbl[%]))*AG137,U137*$AG137),0)","v":0},{"$f":"IF($AF137=3,IF($AF$2=2,(V137/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I137,Refurb_Poss_Tbl[%]))*AG137,IF($AF$2=3,(V137*AG137)-AW137,V137*AG137)),0)","v":0},{"$f":"IF($AF137=3,IF($AF$2=2,(W137/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I137,Refurb_Poss_Tbl[%]))*AG137,W137*$AG137),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,35,0,{"$f":"VLOOKUP(AE138,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35538339780838735},0,0,0,0,0,0,0,0,6.0138401269266598E-4,{"$f":"IF(OR(AF138=3,AF138=2,AF138=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D138,FlatMaint!$Y$2:$Y$10000,AE138)*AG138,0)","v":9.6822043009508238},{"$f":"IF(OR(AF138=3,AF138=2,AF138=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D138,FlatRepair!$Y$2:$Y$10000,AE138)*AG138,0)","v":0},0,9.6828056849635171,0,0,0,0,0,9.6828056849635171,0,{"$f":"IF($AF138=3,IF($AF$2=2,(R138/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I138,Refurb_Poss_Tbl[%]))*AG138,IF($AF$2=3,(R138*AG138)-AV138,R138*AG138)),0)","v":0},{"$f":"IF(AF138=3,IF($AF$2=2,(S138/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I138,Refurb_Poss_Tbl[%]))*AG138,IF($AF$2=3,(S138*AG138)-AX138,S138*AG138)),0)","v":0},{"$f":"IF($AF138=3,IF($AF$2=2,(T138/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I138,Refurb_Poss_Tbl[%]))*AG138,T138*$AG138),0)","v":0},{"$f":"IF($AF138=3,IF($AF$2=2,(Q138/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I138,Refurb_Poss_Tbl[%]))*AG138,Q138*$AG138),0)","v":0},{"$f":"IF($AF138=3,IF($AF$2=2,(U138/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I138,Refurb_Poss_Tbl[%]))*AG138,U138*$AG138),0)","v":0},{"$f":"IF($AF138=3,IF($AF$2=2,(V138/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I138,Refurb_Poss_Tbl[%]))*AG138,IF($AF$2=3,(V138*AG138)-AW138,V138*AG138)),0)","v":0},{"$f":"IF($AF138=3,IF($AF$2=2,(W138/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I138,Refurb_Poss_Tbl[%]))*AG138,W138*$AG138),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,36,0,{"$f":"VLOOKUP(AE139,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.34503242505668674},0,0,0,0,0,0,0,0,5.8386797348802528E-4,{"$f":"IF(OR(AF139=3,AF139=2,AF139=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D139,FlatMaint!$Y$2:$Y$10000,AE139)*AG139,0)","v":9.4001983504376927},{"$f":"IF(OR(AF139=3,AF139=2,AF139=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D139,FlatRepair!$Y$2:$Y$10000,AE139)*AG139,0)","v":0},0,9.4007822184111802,0,0,0,0,0,9.4007822184111802,0,{"$f":"IF($AF139=3,IF($AF$2=2,(R139/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I139,Refurb_Poss_Tbl[%]))*AG139,IF($AF$2=3,(R139*AG139)-AV139,R139*AG139)),0)","v":0},{"$f":"IF(AF139=3,IF($AF$2=2,(S139/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I139,Refurb_Poss_Tbl[%]))*AG139,IF($AF$2=3,(S139*AG139)-AX139,S139*AG139)),0)","v":0},{"$f":"IF($AF139=3,IF($AF$2=2,(T139/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I139,Refurb_Poss_Tbl[%]))*AG139,T139*$AG139),0)","v":0},{"$f":"IF($AF139=3,IF($AF$2=2,(Q139/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I139,Refurb_Poss_Tbl[%]))*AG139,Q139*$AG139),0)","v":0},{"$f":"IF($AF139=3,IF($AF$2=2,(U139/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I139,Refurb_Poss_Tbl[%]))*AG139,U139*$AG139),0)","v":0},{"$f":"IF($AF139=3,IF($AF$2=2,(V139/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I139,Refurb_Poss_Tbl[%]))*AG139,IF($AF$2=3,(V139*AG139)-AW139,V139*AG139)),0)","v":0},{"$f":"IF($AF139=3,IF($AF$2=2,(W139/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I139,Refurb_Poss_Tbl[%]))*AG139,W139*$AG139),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,37,0,{"$f":"VLOOKUP(AE140,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.33498293694823961},0,0,0,0,0,0,0,0,5.6686211018254886E-4,{"$f":"IF(OR(AF140=3,AF140=2,AF140=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D140,FlatMaint!$Y$2:$Y$10000,AE140)*AG140,0)","v":9.1264061654734885},{"$f":"IF(OR(AF140=3,AF140=2,AF140=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D140,FlatRepair!$Y$2:$Y$10000,AE140)*AG140,0)","v":0},0,9.1269730275836718,0,0,0,0,0,9.1269730275836718,0,{"$f":"IF($AF140=3,IF($AF$2=2,(R140/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I140,Refurb_Poss_Tbl[%]))*AG140,IF($AF$2=3,(R140*AG140)-AV140,R140*AG140)),0)","v":0},{"$f":"IF(AF140=3,IF($AF$2=2,(S140/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I140,Refurb_Poss_Tbl[%]))*AG140,IF($AF$2=3,(S140*AG140)-AX140,S140*AG140)),0)","v":0},{"$f":"IF($AF140=3,IF($AF$2=2,(T140/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I140,Refurb_Poss_Tbl[%]))*AG140,T140*$AG140),0)","v":0},{"$f":"IF($AF140=3,IF($AF$2=2,(Q140/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I140,Refurb_Poss_Tbl[%]))*AG140,Q140*$AG140),0)","v":0},{"$f":"IF($AF140=3,IF($AF$2=2,(U140/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I140,Refurb_Poss_Tbl[%]))*AG140,U140*$AG140),0)","v":0},{"$f":"IF($AF140=3,IF($AF$2=2,(V140/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I140,Refurb_Poss_Tbl[%]))*AG140,IF($AF$2=3,(V140*AG140)-AW140,V140*AG140)),0)","v":0},{"$f":"IF($AF140=3,IF($AF$2=2,(W140/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I140,Refurb_Poss_Tbl[%]))*AG140,W140*$AG140),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,38,0,{"$f":"VLOOKUP(AE141,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.3252261523769317},0,0,0,0,0,0,0,0,5.5035156328402807E-4,{"$f":"IF(OR(AF141=3,AF141=2,AF141=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D141,FlatMaint!$Y$2:$Y$10000,AE141)*AG141,0)","v":8.8605885101684372},{"$f":"IF(OR(AF141=3,AF141=2,AF141=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D141,FlatRepair!$Y$2:$Y$10000,AE141)*AG141,0)","v":0},0,8.8611388617317211,0,0,0,0,0,8.8611388617317211,0,{"$f":"IF($AF141=3,IF($AF$2=2,(R141/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I141,Refurb_Poss_Tbl[%]))*AG141,IF($AF$2=3,(R141*AG141)-AV141,R141*AG141)),0)","v":0},{"$f":"IF(AF141=3,IF($AF$2=2,(S141/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I141,Refurb_Poss_Tbl[%]))*AG141,IF($AF$2=3,(S141*AG141)-AX141,S141*AG141)),0)","v":0},{"$f":"IF($AF141=3,IF($AF$2=2,(T141/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I141,Refurb_Poss_Tbl[%]))*AG141,T141*$AG141),0)","v":0},{"$f":"IF($AF141=3,IF($AF$2=2,(Q141/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I141,Refurb_Poss_Tbl[%]))*AG141,Q141*$AG141),0)","v":0},{"$f":"IF($AF141=3,IF($AF$2=2,(U141/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I141,Refurb_Poss_Tbl[%]))*AG141,U141*$AG141),0)","v":0},{"$f":"IF($AF141=3,IF($AF$2=2,(V141/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I141,Refurb_Poss_Tbl[%]))*AG141,IF($AF$2=3,(V141*AG141)-AW141,V141*AG141)),0)","v":0},{"$f":"IF($AF141=3,IF($AF$2=2,(W141/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I141,Refurb_Poss_Tbl[%]))*AG141,W141*$AG141),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,39,0,{"$f":"VLOOKUP(AE142,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.31575354599702099},0,0,0,0,0,0,0,0,5.3432190610099798E-4,{"$f":"IF(OR(AF142=3,AF142=2,AF142=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D142,FlatMaint!$Y$2:$Y$10000,AE142)*AG142,0)","v":8.6025131166683835},{"$f":"IF(OR(AF142=3,AF142=2,AF142=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D142,FlatRepair!$Y$2:$Y$10000,AE142)*AG142,0)","v":0},0,8.6030474385744853,0,0,0,0,0,8.6030474385744853,0,{"$f":"IF($AF142=3,IF($AF$2=2,(R142/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I142,Refurb_Poss_Tbl[%]))*AG142,IF($AF$2=3,(R142*AG142)-AV142,R142*AG142)),0)","v":0},{"$f":"IF(AF142=3,IF($AF$2=2,(S142/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I142,Refurb_Poss_Tbl[%]))*AG142,IF($AF$2=3,(S142*AG142)-AX142,S142*AG142)),0)","v":0},{"$f":"IF($AF142=3,IF($AF$2=2,(T142/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I142,Refurb_Poss_Tbl[%]))*AG142,T142*$AG142),0)","v":0},{"$f":"IF($AF142=3,IF($AF$2=2,(Q142/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I142,Refurb_Poss_Tbl[%]))*AG142,Q142*$AG142),0)","v":0},{"$f":"IF($AF142=3,IF($AF$2=2,(U142/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I142,Refurb_Poss_Tbl[%]))*AG142,U142*$AG142),0)","v":0},{"$f":"IF($AF142=3,IF($AF$2=2,(V142/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I142,Refurb_Poss_Tbl[%]))*AG142,IF($AF$2=3,(V142*AG142)-AW142,V142*AG142)),0)","v":0},{"$f":"IF($AF142=3,IF($AF$2=2,(W142/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I142,Refurb_Poss_Tbl[%]))*AG142,W142*$AG142),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,40,0,{"$f":"VLOOKUP(AE143,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.30655684077380685},0,0,0,0,0,0,0,0,5.1875913213689142E-4,{"$f":"IF(OR(AF143=3,AF143=2,AF143=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D143,FlatMaint!$Y$2:$Y$10000,AE143)*AG143,0)","v":8.3519544822023164},{"$f":"IF(OR(AF143=3,AF143=2,AF143=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D143,FlatRepair!$Y$2:$Y$10000,AE143)*AG143,0)","v":0},0,8.3524732413344527,0,0,0,0,0,8.3524732413344527,0,{"$f":"IF($AF143=3,IF($AF$2=2,(R143/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I143,Refurb_Poss_Tbl[%]))*AG143,IF($AF$2=3,(R143*AG143)-AV143,R143*AG143)),0)","v":0},{"$f":"IF(AF143=3,IF($AF$2=2,(S143/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I143,Refurb_Poss_Tbl[%]))*AG143,IF($AF$2=3,(S143*AG143)-AX143,S143*AG143)),0)","v":0},{"$f":"IF($AF143=3,IF($AF$2=2,(T143/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I143,Refurb_Poss_Tbl[%]))*AG143,T143*$AG143),0)","v":0},{"$f":"IF($AF143=3,IF($AF$2=2,(Q143/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I143,Refurb_Poss_Tbl[%]))*AG143,Q143*$AG143),0)","v":0},{"$f":"IF($AF143=3,IF($AF$2=2,(U143/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I143,Refurb_Poss_Tbl[%]))*AG143,U143*$AG143),0)","v":0},{"$f":"IF($AF143=3,IF($AF$2=2,(V143/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I143,Refurb_Poss_Tbl[%]))*AG143,IF($AF$2=3,(V143*AG143)-AW143,V143*AG143)),0)","v":0},{"$f":"IF($AF143=3,IF($AF$2=2,(W143/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I143,Refurb_Poss_Tbl[%]))*AG143,W143*$AG143),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,41,0,{"$f":"VLOOKUP(AE144,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.29762800075126877},0,0,0,0,0,0,0,0,5.0364964285135082E-4,{"$f":"IF(OR(AF144=3,AF144=2,AF144=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D144,FlatMaint!$Y$2:$Y$10000,AE144)*AG144,0)","v":8.1086936720410829},{"$f":"IF(OR(AF144=3,AF144=2,AF144=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D144,FlatRepair!$Y$2:$Y$10000,AE144)*AG144,0)","v":0},0,8.1091973216839346,0,0,0,0,0,8.1091973216839346,0,{"$f":"IF($AF144=3,IF($AF$2=2,(R144/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I144,Refurb_Poss_Tbl[%]))*AG144,IF($AF$2=3,(R144*AG144)-AV144,R144*AG144)),0)","v":0},{"$f":"IF(AF144=3,IF($AF$2=2,(S144/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I144,Refurb_Poss_Tbl[%]))*AG144,IF($AF$2=3,(S144*AG144)-AX144,S144*AG144)),0)","v":0},{"$f":"IF($AF144=3,IF($AF$2=2,(T144/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I144,Refurb_Poss_Tbl[%]))*AG144,T144*$AG144),0)","v":0},{"$f":"IF($AF144=3,IF($AF$2=2,(Q144/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I144,Refurb_Poss_Tbl[%]))*AG144,Q144*$AG144),0)","v":0},{"$f":"IF($AF144=3,IF($AF$2=2,(U144/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I144,Refurb_Poss_Tbl[%]))*AG144,U144*$AG144),0)","v":0},{"$f":"IF($AF144=3,IF($AF$2=2,(V144/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I144,Refurb_Poss_Tbl[%]))*AG144,IF($AF$2=3,(V144*AG144)-AW144,V144*AG144)),0)","v":0},{"$f":"IF($AF144=3,IF($AF$2=2,(W144/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I144,Refurb_Poss_Tbl[%]))*AG144,W144*$AG144),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,42,0,{"$f":"VLOOKUP(AE145,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28895922403035801},0,0,0,0,0,0,0,0,4.8898023577801048E-4,{"$f":"IF(OR(AF145=3,AF145=2,AF145=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D145,FlatMaint!$Y$2:$Y$10000,AE145)*AG145,0)","v":7.8725181281952255},{"$f":"IF(OR(AF145=3,AF145=2,AF145=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D145,FlatRepair!$Y$2:$Y$10000,AE145)*AG145,0)","v":0},0,7.8730071084310032,0,0,0,0,0,7.8730071084310032,0,{"$f":"IF($AF145=3,IF($AF$2=2,(R145/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I145,Refurb_Poss_Tbl[%]))*AG145,IF($AF$2=3,(R145*AG145)-AV145,R145*AG145)),0)","v":0},{"$f":"IF(AF145=3,IF($AF$2=2,(S145/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I145,Refurb_Poss_Tbl[%]))*AG145,IF($AF$2=3,(S145*AG145)-AX145,S145*AG145)),0)","v":0},{"$f":"IF($AF145=3,IF($AF$2=2,(T145/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I145,Refurb_Poss_Tbl[%]))*AG145,T145*$AG145),0)","v":0},{"$f":"IF($AF145=3,IF($AF$2=2,(Q145/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I145,Refurb_Poss_Tbl[%]))*AG145,Q145*$AG145),0)","v":0},{"$f":"IF($AF145=3,IF($AF$2=2,(U145/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I145,Refurb_Poss_Tbl[%]))*AG145,U145*$AG145),0)","v":0},{"$f":"IF($AF145=3,IF($AF$2=2,(V145/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I145,Refurb_Poss_Tbl[%]))*AG145,IF($AF$2=3,(V145*AG145)-AW145,V145*AG145)),0)","v":0},{"$f":"IF($AF145=3,IF($AF$2=2,(W145/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I145,Refurb_Poss_Tbl[%]))*AG145,W145*$AG145),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,43,0,{"$f":"VLOOKUP(AE146,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28054293595180391},0,0,0,0,0,0,0,0,4.7473809298835974E-4,{"$f":"IF(OR(AF146=3,AF146=2,AF146=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D146,FlatMaint!$Y$2:$Y$10000,AE146)*AG146,0)","v":7.6432214836846857},{"$f":"IF(OR(AF146=3,AF146=2,AF146=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D146,FlatRepair!$Y$2:$Y$10000,AE146)*AG146,0)","v":0},0,7.6436962217776738,0,0,0,0,0,7.6436962217776738,0,{"$f":"IF($AF146=3,IF($AF$2=2,(R146/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I146,Refurb_Poss_Tbl[%]))*AG146,IF($AF$2=3,(R146*AG146)-AV146,R146*AG146)),0)","v":0},{"$f":"IF(AF146=3,IF($AF$2=2,(S146/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I146,Refurb_Poss_Tbl[%]))*AG146,IF($AF$2=3,(S146*AG146)-AX146,S146*AG146)),0)","v":0},{"$f":"IF($AF146=3,IF($AF$2=2,(T146/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I146,Refurb_Poss_Tbl[%]))*AG146,T146*$AG146),0)","v":0},{"$f":"IF($AF146=3,IF($AF$2=2,(Q146/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I146,Refurb_Poss_Tbl[%]))*AG146,Q146*$AG146),0)","v":0},{"$f":"IF($AF146=3,IF($AF$2=2,(U146/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I146,Refurb_Poss_Tbl[%]))*AG146,U146*$AG146),0)","v":0},{"$f":"IF($AF146=3,IF($AF$2=2,(V146/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I146,Refurb_Poss_Tbl[%]))*AG146,IF($AF$2=3,(V146*AG146)-AW146,V146*AG146)),0)","v":0},{"$f":"IF($AF146=3,IF($AF$2=2,(W146/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I146,Refurb_Poss_Tbl[%]))*AG146,W146*$AG146),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,44,0,{"$f":"VLOOKUP(AE147,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.27237178247747956},0,0,0,0,0,0,0,0,4.6091076989161143E-4,{"$f":"IF(OR(AF147=3,AF147=2,AF147=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D147,FlatMaint!$Y$2:$Y$10000,AE147)*AG147,0)","v":7.4206033822181423},{"$f":"IF(OR(AF147=3,AF147=2,AF147=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D147,FlatRepair!$Y$2:$Y$10000,AE147)*AG147,0)","v":0},0,7.4210642929880342,0,0,0,0,0,7.4210642929880342,0,{"$f":"IF($AF147=3,IF($AF$2=2,(R147/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I147,Refurb_Poss_Tbl[%]))*AG147,IF($AF$2=3,(R147*AG147)-AV147,R147*AG147)),0)","v":0},{"$f":"IF(AF147=3,IF($AF$2=2,(S147/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I147,Refurb_Poss_Tbl[%]))*AG147,IF($AF$2=3,(S147*AG147)-AX147,S147*AG147)),0)","v":0},{"$f":"IF($AF147=3,IF($AF$2=2,(T147/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I147,Refurb_Poss_Tbl[%]))*AG147,T147*$AG147),0)","v":0},{"$f":"IF($AF147=3,IF($AF$2=2,(Q147/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I147,Refurb_Poss_Tbl[%]))*AG147,Q147*$AG147),0)","v":0},{"$f":"IF($AF147=3,IF($AF$2=2,(U147/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I147,Refurb_Poss_Tbl[%]))*AG147,U147*$AG147),0)","v":0},{"$f":"IF($AF147=3,IF($AF$2=2,(V147/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I147,Refurb_Poss_Tbl[%]))*AG147,IF($AF$2=3,(V147*AG147)-AW147,V147*AG147)),0)","v":0},{"$f":"IF($AF147=3,IF($AF$2=2,(W147/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I147,Refurb_Poss_Tbl[%]))*AG147,W147*$AG147),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,45,0,{"$f":"VLOOKUP(AE148,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.26443862376454325},0,0,0,0,0,0,0,0,4.4748618436078779E-4,{"$f":"IF(OR(AF148=3,AF148=2,AF148=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D148,FlatMaint!$Y$2:$Y$10000,AE148)*AG148,0)","v":7.2044693031244096},{"$f":"IF(OR(AF148=3,AF148=2,AF148=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D148,FlatRepair!$Y$2:$Y$10000,AE148)*AG148,0)","v":0},0,7.2049167893087702,0,0,0,0,0,7.2049167893087702,0,{"$f":"IF($AF148=3,IF($AF$2=2,(R148/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I148,Refurb_Poss_Tbl[%]))*AG148,IF($AF$2=3,(R148*AG148)-AV148,R148*AG148)),0)","v":0},{"$f":"IF(AF148=3,IF($AF$2=2,(S148/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I148,Refurb_Poss_Tbl[%]))*AG148,IF($AF$2=3,(S148*AG148)-AX148,S148*AG148)),0)","v":0},{"$f":"IF($AF148=3,IF($AF$2=2,(T148/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I148,Refurb_Poss_Tbl[%]))*AG148,T148*$AG148),0)","v":0},{"$f":"IF($AF148=3,IF($AF$2=2,(Q148/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I148,Refurb_Poss_Tbl[%]))*AG148,Q148*$AG148),0)","v":0},{"$f":"IF($AF148=3,IF($AF$2=2,(U148/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I148,Refurb_Poss_Tbl[%]))*AG148,U148*$AG148),0)","v":0},{"$f":"IF($AF148=3,IF($AF$2=2,(V148/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I148,Refurb_Poss_Tbl[%]))*AG148,IF($AF$2=3,(V148*AG148)-AW148,V148*AG148)),0)","v":0},{"$f":"IF($AF148=3,IF($AF$2=2,(W148/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I148,Refurb_Poss_Tbl[%]))*AG148,W148*$AG148),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,46,0,{"$f":"VLOOKUP(AE149,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.25673652792674101},0,0,0,0,0,0,0,0,4.344526061755221E-4,{"$f":"IF(OR(AF149=3,AF149=2,AF149=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D149,FlatMaint!$Y$2:$Y$10000,AE149)*AG149,0)","v":6.9946303913829215},{"$f":"IF(OR(AF149=3,AF149=2,AF149=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D149,FlatRepair!$Y$2:$Y$10000,AE149)*AG149,0)","v":0},0,6.9950648439890974,0,0,0,0,0,6.9950648439890974,0,{"$f":"IF($AF149=3,IF($AF$2=2,(R149/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I149,Refurb_Poss_Tbl[%]))*AG149,IF($AF$2=3,(R149*AG149)-AV149,R149*AG149)),0)","v":0},{"$f":"IF(AF149=3,IF($AF$2=2,(S149/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I149,Refurb_Poss_Tbl[%]))*AG149,IF($AF$2=3,(S149*AG149)-AX149,S149*AG149)),0)","v":0},{"$f":"IF($AF149=3,IF($AF$2=2,(T149/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I149,Refurb_Poss_Tbl[%]))*AG149,T149*$AG149),0)","v":0},{"$f":"IF($AF149=3,IF($AF$2=2,(Q149/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I149,Refurb_Poss_Tbl[%]))*AG149,Q149*$AG149),0)","v":0},{"$f":"IF($AF149=3,IF($AF$2=2,(U149/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I149,Refurb_Poss_Tbl[%]))*AG149,U149*$AG149),0)","v":0},{"$f":"IF($AF149=3,IF($AF$2=2,(V149/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I149,Refurb_Poss_Tbl[%]))*AG149,IF($AF$2=3,(V149*AG149)-AW149,V149*AG149)),0)","v":0},{"$f":"IF($AF149=3,IF($AF$2=2,(W149/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I149,Refurb_Poss_Tbl[%]))*AG149,W149*$AG149),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,47,0,{"$f":"VLOOKUP(AE150,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24925876497741845},0,0,0,0,0,0,0,0,4.2179864677235153E-4,{"$f":"IF(OR(AF150=3,AF150=2,AF150=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D150,FlatMaint!$Y$2:$Y$10000,AE150)*AG150,0)","v":6.7909032926047779},{"$f":"IF(OR(AF150=3,AF150=2,AF150=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D150,FlatRepair!$Y$2:$Y$10000,AE150)*AG150,0)","v":0},0,6.7913250912515499,0,0,0,0,0,6.7913250912515499,0,{"$f":"IF($AF150=3,IF($AF$2=2,(R150/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I150,Refurb_Poss_Tbl[%]))*AG150,IF($AF$2=3,(R150*AG150)-AV150,R150*AG150)),0)","v":0},{"$f":"IF(AF150=3,IF($AF$2=2,(S150/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I150,Refurb_Poss_Tbl[%]))*AG150,IF($AF$2=3,(S150*AG150)-AX150,S150*AG150)),0)","v":0},{"$f":"IF($AF150=3,IF($AF$2=2,(T150/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I150,Refurb_Poss_Tbl[%]))*AG150,T150*$AG150),0)","v":0},{"$f":"IF($AF150=3,IF($AF$2=2,(Q150/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I150,Refurb_Poss_Tbl[%]))*AG150,Q150*$AG150),0)","v":0},{"$f":"IF($AF150=3,IF($AF$2=2,(U150/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I150,Refurb_Poss_Tbl[%]))*AG150,U150*$AG150),0)","v":0},{"$f":"IF($AF150=3,IF($AF$2=2,(V150/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I150,Refurb_Poss_Tbl[%]))*AG150,IF($AF$2=3,(V150*AG150)-AW150,V150*AG150)),0)","v":0},{"$f":"IF($AF150=3,IF($AF$2=2,(W150/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I150,Refurb_Poss_Tbl[%]))*AG150,W150*$AG150),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,48,0,{"$f":"VLOOKUP(AE151,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24199880094894996},0,0,0,0,0,0,0,0,4.0951324929354519E-4,{"$f":"IF(OR(AF151=3,AF151=2,AF151=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D151,FlatMaint!$Y$2:$Y$10000,AE151)*AG151,0)","v":6.5931099928201728},{"$f":"IF(OR(AF151=3,AF151=2,AF151=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D151,FlatRepair!$Y$2:$Y$10000,AE151)*AG151,0)","v":0},0,6.593519506069466,0,0,0,0,0,6.593519506069466,0,{"$f":"IF($AF151=3,IF($AF$2=2,(R151/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I151,Refurb_Poss_Tbl[%]))*AG151,IF($AF$2=3,(R151*AG151)-AV151,R151*AG151)),0)","v":0},{"$f":"IF(AF151=3,IF($AF$2=2,(S151/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I151,Refurb_Poss_Tbl[%]))*AG151,IF($AF$2=3,(S151*AG151)-AX151,S151*AG151)),0)","v":0},{"$f":"IF($AF151=3,IF($AF$2=2,(T151/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I151,Refurb_Poss_Tbl[%]))*AG151,T151*$AG151),0)","v":0},{"$f":"IF($AF151=3,IF($AF$2=2,(Q151/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I151,Refurb_Poss_Tbl[%]))*AG151,Q151*$AG151),0)","v":0},{"$f":"IF($AF151=3,IF($AF$2=2,(U151/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I151,Refurb_Poss_Tbl[%]))*AG151,U151*$AG151),0)","v":0},{"$f":"IF($AF151=3,IF($AF$2=2,(V151/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I151,Refurb_Poss_Tbl[%]))*AG151,IF($AF$2=3,(V151*AG151)-AW151,V151*AG151)),0)","v":0},{"$f":"IF($AF151=3,IF($AF$2=2,(W151/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I151,Refurb_Poss_Tbl[%]))*AG151,W151*$AG151),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,49,0,{"$f":"VLOOKUP(AE152,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.2349502921834466},0,0,0,0,0,0,0,0,3.975856789257721E-4,{"$f":"IF(OR(AF152=3,AF152=2,AF152=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D152,FlatMaint!$Y$2:$Y$10000,AE152)*AG152,0)","v":6.4010776629322077},{"$f":"IF(OR(AF152=3,AF152=2,AF152=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D152,FlatRepair!$Y$2:$Y$10000,AE152)*AG152,0)","v":0},0,6.401475248611133,0,0,0,0,0,6.401475248611133,0,{"$f":"IF($AF152=3,IF($AF$2=2,(R152/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I152,Refurb_Poss_Tbl[%]))*AG152,IF($AF$2=3,(R152*AG152)-AV152,R152*AG152)),0)","v":0},{"$f":"IF(AF152=3,IF($AF$2=2,(S152/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I152,Refurb_Poss_Tbl[%]))*AG152,IF($AF$2=3,(S152*AG152)-AX152,S152*AG152)),0)","v":0},{"$f":"IF($AF152=3,IF($AF$2=2,(T152/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I152,Refurb_Poss_Tbl[%]))*AG152,T152*$AG152),0)","v":0},{"$f":"IF($AF152=3,IF($AF$2=2,(Q152/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I152,Refurb_Poss_Tbl[%]))*AG152,Q152*$AG152),0)","v":0},{"$f":"IF($AF152=3,IF($AF$2=2,(U152/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I152,Refurb_Poss_Tbl[%]))*AG152,U152*$AG152),0)","v":0},{"$f":"IF($AF152=3,IF($AF$2=2,(V152/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I152,Refurb_Poss_Tbl[%]))*AG152,IF($AF$2=3,(V152*AG152)-AW152,V152*AG152)),0)","v":0},{"$f":"IF($AF152=3,IF($AF$2=2,(W152/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I152,Refurb_Poss_Tbl[%]))*AG152,W152*$AG152),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,50,0,{"$f":"VLOOKUP(AE153,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22810707978975397},0,0,0,0,0,0,0,0,3.8600551352016706E-4,{"$f":"IF(OR(AF153=3,AF153=2,AF153=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D153,FlatMaint!$Y$2:$Y$10000,AE153)*AG153,0)","v":6.2146385077011725},{"$f":"IF(OR(AF153=3,AF153=2,AF153=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D153,FlatRepair!$Y$2:$Y$10000,AE153)*AG153,0)","v":0},0,6.2150245132146926,0,0,0,0,0,6.2150245132146926,0,{"$f":"IF($AF153=3,IF($AF$2=2,(R153/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I153,Refurb_Poss_Tbl[%]))*AG153,IF($AF$2=3,(R153*AG153)-AV153,R153*AG153)),0)","v":0},{"$f":"IF(AF153=3,IF($AF$2=2,(S153/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I153,Refurb_Poss_Tbl[%]))*AG153,IF($AF$2=3,(S153*AG153)-AX153,S153*AG153)),0)","v":0},{"$f":"IF($AF153=3,IF($AF$2=2,(T153/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I153,Refurb_Poss_Tbl[%]))*AG153,T153*$AG153),0)","v":0},{"$f":"IF($AF153=3,IF($AF$2=2,(Q153/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I153,Refurb_Poss_Tbl[%]))*AG153,Q153*$AG153),0)","v":0},{"$f":"IF($AF153=3,IF($AF$2=2,(U153/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I153,Refurb_Poss_Tbl[%]))*AG153,U153*$AG153),0)","v":0},{"$f":"IF($AF153=3,IF($AF$2=2,(V153/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I153,Refurb_Poss_Tbl[%]))*AG153,IF($AF$2=3,(V153*AG153)-AW153,V153*AG153)),0)","v":0},{"$f":"IF($AF153=3,IF($AF$2=2,(W153/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I153,Refurb_Poss_Tbl[%]))*AG153,W153*$AG153),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,51,0,{"$f":"VLOOKUP(AE154,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22146318426189707},0,0,0,0,0,0,0,0,3.747626344855991E-4,{"$f":"IF(OR(AF154=3,AF154=2,AF154=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D154,FlatMaint!$Y$2:$Y$10000,AE154)*AG154,0)","v":6.0336296191273524},{"$f":"IF(OR(AF154=3,AF154=2,AF154=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D154,FlatRepair!$Y$2:$Y$10000,AE154)*AG154,0)","v":0},0,6.0340043817618376,0,0,0,0,0,6.0340043817618376,0,{"$f":"IF($AF154=3,IF($AF$2=2,(R154/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I154,Refurb_Poss_Tbl[%]))*AG154,IF($AF$2=3,(R154*AG154)-AV154,R154*AG154)),0)","v":0},{"$f":"IF(AF154=3,IF($AF$2=2,(S154/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I154,Refurb_Poss_Tbl[%]))*AG154,IF($AF$2=3,(S154*AG154)-AX154,S154*AG154)),0)","v":0},{"$f":"IF($AF154=3,IF($AF$2=2,(T154/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I154,Refurb_Poss_Tbl[%]))*AG154,T154*$AG154),0)","v":0},{"$f":"IF($AF154=3,IF($AF$2=2,(Q154/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I154,Refurb_Poss_Tbl[%]))*AG154,Q154*$AG154),0)","v":0},{"$f":"IF($AF154=3,IF($AF$2=2,(U154/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I154,Refurb_Poss_Tbl[%]))*AG154,U154*$AG154),0)","v":0},{"$f":"IF($AF154=3,IF($AF$2=2,(V154/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I154,Refurb_Poss_Tbl[%]))*AG154,IF($AF$2=3,(V154*AG154)-AW154,V154*AG154)),0)","v":0},{"$f":"IF($AF154=3,IF($AF$2=2,(W154/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I154,Refurb_Poss_Tbl[%]))*AG154,W154*$AG154),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,52,0,{"$f":"VLOOKUP(AE155,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.215012800254269},0,0,0,0,0,0,0,0,3.6384721794718362E-4,{"$f":"IF(OR(AF155=3,AF155=2,AF155=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D155,FlatMaint!$Y$2:$Y$10000,AE155)*AG155,0)","v":5.8578928341042253},{"$f":"IF(OR(AF155=3,AF155=2,AF155=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D155,FlatRepair!$Y$2:$Y$10000,AE155)*AG155,0)","v":0},0,5.8582566813221728,0,0,0,0,0,5.8582566813221728,0,{"$f":"IF($AF155=3,IF($AF$2=2,(R155/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I155,Refurb_Poss_Tbl[%]))*AG155,IF($AF$2=3,(R155*AG155)-AV155,R155*AG155)),0)","v":0},{"$f":"IF(AF155=3,IF($AF$2=2,(S155/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I155,Refurb_Poss_Tbl[%]))*AG155,IF($AF$2=3,(S155*AG155)-AX155,S155*AG155)),0)","v":0},{"$f":"IF($AF155=3,IF($AF$2=2,(T155/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I155,Refurb_Poss_Tbl[%]))*AG155,T155*$AG155),0)","v":0},{"$f":"IF($AF155=3,IF($AF$2=2,(Q155/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I155,Refurb_Poss_Tbl[%]))*AG155,Q155*$AG155),0)","v":0},{"$f":"IF($AF155=3,IF($AF$2=2,(U155/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I155,Refurb_Poss_Tbl[%]))*AG155,U155*$AG155),0)","v":0},{"$f":"IF($AF155=3,IF($AF$2=2,(V155/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I155,Refurb_Poss_Tbl[%]))*AG155,IF($AF$2=3,(V155*AG155)-AW155,V155*AG155)),0)","v":0},{"$f":"IF($AF155=3,IF($AF$2=2,(W155/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I155,Refurb_Poss_Tbl[%]))*AG155,W155*$AG155),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,53,0,{"$f":"VLOOKUP(AE156,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20875029150899907},0,0,0,0,0,0,0,0,3.5324972616231423E-4,{"$f":"IF(OR(AF156=3,AF156=2,AF156=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D156,FlatMaint!$Y$2:$Y$10000,AE156)*AG156,0)","v":5.687274596217696},{"$f":"IF(OR(AF156=3,AF156=2,AF156=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D156,FlatRepair!$Y$2:$Y$10000,AE156)*AG156,0)","v":0},0,5.6876278459438581,0,0,0,0,0,5.6876278459438581,0,{"$f":"IF($AF156=3,IF($AF$2=2,(R156/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I156,Refurb_Poss_Tbl[%]))*AG156,IF($AF$2=3,(R156*AG156)-AV156,R156*AG156)),0)","v":0},{"$f":"IF(AF156=3,IF($AF$2=2,(S156/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I156,Refurb_Poss_Tbl[%]))*AG156,IF($AF$2=3,(S156*AG156)-AX156,S156*AG156)),0)","v":0},{"$f":"IF($AF156=3,IF($AF$2=2,(T156/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I156,Refurb_Poss_Tbl[%]))*AG156,T156*$AG156),0)","v":0},{"$f":"IF($AF156=3,IF($AF$2=2,(Q156/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I156,Refurb_Poss_Tbl[%]))*AG156,Q156*$AG156),0)","v":0},{"$f":"IF($AF156=3,IF($AF$2=2,(U156/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I156,Refurb_Poss_Tbl[%]))*AG156,U156*$AG156),0)","v":0},{"$f":"IF($AF156=3,IF($AF$2=2,(V156/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I156,Refurb_Poss_Tbl[%]))*AG156,IF($AF$2=3,(V156*AG156)-AW156,V156*AG156)),0)","v":0},{"$f":"IF($AF156=3,IF($AF$2=2,(W156/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I156,Refurb_Poss_Tbl[%]))*AG156,W156*$AG156),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,54,0,{"$f":"VLOOKUP(AE157,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20267018593106703},0,0,0,0,0,0,0,0,3.4296089918671284E-4,{"$f":"IF(OR(AF157=3,AF157=2,AF157=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D157,FlatMaint!$Y$2:$Y$10000,AE157)*AG157,0)","v":5.521625821570578},{"$f":"IF(OR(AF157=3,AF157=2,AF157=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D157,FlatRepair!$Y$2:$Y$10000,AE157)*AG157,0)","v":0},0,5.5219687824697647,0,0,0,0,0,5.5219687824697647,0,{"$f":"IF($AF157=3,IF($AF$2=2,(R157/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I157,Refurb_Poss_Tbl[%]))*AG157,IF($AF$2=3,(R157*AG157)-AV157,R157*AG157)),0)","v":0},{"$f":"IF(AF157=3,IF($AF$2=2,(S157/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I157,Refurb_Poss_Tbl[%]))*AG157,IF($AF$2=3,(S157*AG157)-AX157,S157*AG157)),0)","v":0},{"$f":"IF($AF157=3,IF($AF$2=2,(T157/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I157,Refurb_Poss_Tbl[%]))*AG157,T157*$AG157),0)","v":0},{"$f":"IF($AF157=3,IF($AF$2=2,(Q157/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I157,Refurb_Poss_Tbl[%]))*AG157,Q157*$AG157),0)","v":0},{"$f":"IF($AF157=3,IF($AF$2=2,(U157/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I157,Refurb_Poss_Tbl[%]))*AG157,U157*$AG157),0)","v":0},{"$f":"IF($AF157=3,IF($AF$2=2,(V157/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I157,Refurb_Poss_Tbl[%]))*AG157,IF($AF$2=3,(V157*AG157)-AW157,V157*AG157)),0)","v":0},{"$f":"IF($AF157=3,IF($AF$2=2,(W157/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I157,Refurb_Poss_Tbl[%]))*AG157,W157*$AG157),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,55,0,{"$f":"VLOOKUP(AE158,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19676717080686118},0,0,0,0,0,0,0,0,3.3297174678321631E-4,{"$f":"IF(OR(AF158=3,AF158=2,AF158=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D158,FlatMaint!$Y$2:$Y$10000,AE158)*AG158,0)","v":5.3608017685151239},{"$f":"IF(OR(AF158=3,AF158=2,AF158=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D158,FlatRepair!$Y$2:$Y$10000,AE158)*AG158,0)","v":0},0,5.3611347402619067,0,0,0,0,0,5.3611347402619067,0,{"$f":"IF($AF158=3,IF($AF$2=2,(R158/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I158,Refurb_Poss_Tbl[%]))*AG158,IF($AF$2=3,(R158*AG158)-AV158,R158*AG158)),0)","v":0},{"$f":"IF(AF158=3,IF($AF$2=2,(S158/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I158,Refurb_Poss_Tbl[%]))*AG158,IF($AF$2=3,(S158*AG158)-AX158,S158*AG158)),0)","v":0},{"$f":"IF($AF158=3,IF($AF$2=2,(T158/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I158,Refurb_Poss_Tbl[%]))*AG158,T158*$AG158),0)","v":0},{"$f":"IF($AF158=3,IF($AF$2=2,(Q158/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I158,Refurb_Poss_Tbl[%]))*AG158,Q158*$AG158),0)","v":0},{"$f":"IF($AF158=3,IF($AF$2=2,(U158/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I158,Refurb_Poss_Tbl[%]))*AG158,U158*$AG158),0)","v":0},{"$f":"IF($AF158=3,IF($AF$2=2,(V158/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I158,Refurb_Poss_Tbl[%]))*AG158,IF($AF$2=3,(V158*AG158)-AW158,V158*AG158)),0)","v":0},{"$f":"IF($AF158=3,IF($AF$2=2,(W158/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I158,Refurb_Poss_Tbl[%]))*AG158,W158*$AG158),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,56,0,{"$f":"VLOOKUP(AE159,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19103608816200118},0,0,0,0,0,0,0,0,3.2327354056622948E-4,{"$f":"IF(OR(AF159=3,AF159=2,AF159=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D159,FlatMaint!$Y$2:$Y$10000,AE159)*AG159,0)","v":5.2046619111797323},{"$f":"IF(OR(AF159=3,AF159=2,AF159=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D159,FlatRepair!$Y$2:$Y$10000,AE159)*AG159,0)","v":0},0,5.2049851847202984,0,0,0,0,0,5.2049851847202984,0,{"$f":"IF($AF159=3,IF($AF$2=2,(R159/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I159,Refurb_Poss_Tbl[%]))*AG159,IF($AF$2=3,(R159*AG159)-AV159,R159*AG159)),0)","v":0},{"$f":"IF(AF159=3,IF($AF$2=2,(S159/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I159,Refurb_Poss_Tbl[%]))*AG159,IF($AF$2=3,(S159*AG159)-AX159,S159*AG159)),0)","v":0},{"$f":"IF($AF159=3,IF($AF$2=2,(T159/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I159,Refurb_Poss_Tbl[%]))*AG159,T159*$AG159),0)","v":0},{"$f":"IF($AF159=3,IF($AF$2=2,(Q159/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I159,Refurb_Poss_Tbl[%]))*AG159,Q159*$AG159),0)","v":0},{"$f":"IF($AF159=3,IF($AF$2=2,(U159/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I159,Refurb_Poss_Tbl[%]))*AG159,U159*$AG159),0)","v":0},{"$f":"IF($AF159=3,IF($AF$2=2,(V159/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I159,Refurb_Poss_Tbl[%]))*AG159,IF($AF$2=3,(V159*AG159)-AW159,V159*AG159)),0)","v":0},{"$f":"IF($AF159=3,IF($AF$2=2,(W159/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I159,Refurb_Poss_Tbl[%]))*AG159,W159*$AG159),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,57,0,{"$f":"VLOOKUP(AE160,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18547193025437006},0,0,0,0,0,0,0,0,3.1385780637498004E-4,{"$f":"IF(OR(AF160=3,AF160=2,AF160=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D160,FlatMaint!$Y$2:$Y$10000,AE160)*AG160,0)","v":5.0530698166793515},{"$f":"IF(OR(AF160=3,AF160=2,AF160=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D160,FlatRepair!$Y$2:$Y$10000,AE160)*AG160,0)","v":0},0,5.0533836744857261,0,0,0,0,0,5.0533836744857261,0,{"$f":"IF($AF160=3,IF($AF$2=2,(R160/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I160,Refurb_Poss_Tbl[%]))*AG160,IF($AF$2=3,(R160*AG160)-AV160,R160*AG160)),0)","v":0},{"$f":"IF(AF160=3,IF($AF$2=2,(S160/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I160,Refurb_Poss_Tbl[%]))*AG160,IF($AF$2=3,(S160*AG160)-AX160,S160*AG160)),0)","v":0},{"$f":"IF($AF160=3,IF($AF$2=2,(T160/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I160,Refurb_Poss_Tbl[%]))*AG160,T160*$AG160),0)","v":0},{"$f":"IF($AF160=3,IF($AF$2=2,(Q160/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I160,Refurb_Poss_Tbl[%]))*AG160,Q160*$AG160),0)","v":0},{"$f":"IF($AF160=3,IF($AF$2=2,(U160/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I160,Refurb_Poss_Tbl[%]))*AG160,U160*$AG160),0)","v":0},{"$f":"IF($AF160=3,IF($AF$2=2,(V160/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I160,Refurb_Poss_Tbl[%]))*AG160,IF($AF$2=3,(V160*AG160)-AW160,V160*AG160)),0)","v":0},{"$f":"IF($AF160=3,IF($AF$2=2,(W160/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I160,Refurb_Poss_Tbl[%]))*AG160,W160*$AG160),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,58,0,{"$f":"VLOOKUP(AE161,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18006983519841754},0,0,0,0,0,0,0,0,3.0471631686891269E-4,{"$f":"IF(OR(AF161=3,AF161=2,AF161=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D161,FlatMaint!$Y$2:$Y$10000,AE161)*AG161,0)","v":4.9058930259022837},{"$f":"IF(OR(AF161=3,AF161=2,AF161=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D161,FlatRepair!$Y$2:$Y$10000,AE161)*AG161,0)","v":0},0,4.9061977422191525,0,0,0,0,0,4.9061977422191525,0,{"$f":"IF($AF161=3,IF($AF$2=2,(R161/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I161,Refurb_Poss_Tbl[%]))*AG161,IF($AF$2=3,(R161*AG161)-AV161,R161*AG161)),0)","v":0},{"$f":"IF(AF161=3,IF($AF$2=2,(S161/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I161,Refurb_Poss_Tbl[%]))*AG161,IF($AF$2=3,(S161*AG161)-AX161,S161*AG161)),0)","v":0},{"$f":"IF($AF161=3,IF($AF$2=2,(T161/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I161,Refurb_Poss_Tbl[%]))*AG161,T161*$AG161),0)","v":0},{"$f":"IF($AF161=3,IF($AF$2=2,(Q161/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I161,Refurb_Poss_Tbl[%]))*AG161,Q161*$AG161),0)","v":0},{"$f":"IF($AF161=3,IF($AF$2=2,(U161/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I161,Refurb_Poss_Tbl[%]))*AG161,U161*$AG161),0)","v":0},{"$f":"IF($AF161=3,IF($AF$2=2,(V161/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I161,Refurb_Poss_Tbl[%]))*AG161,IF($AF$2=3,(V161*AG161)-AW161,V161*AG161)),0)","v":0},{"$f":"IF($AF161=3,IF($AF$2=2,(W161/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I161,Refurb_Poss_Tbl[%]))*AG161,W161*$AG161),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,59,0,{"$f":"VLOOKUP(AE162,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.17482508271691022},0,0,0,0,0,0,0,0,2.9584108433875015E-4,{"$f":"IF(OR(AF162=3,AF162=2,AF162=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D162,FlatMaint!$Y$2:$Y$10000,AE162)*AG162,0)","v":4.7630029377692065},{"$f":"IF(OR(AF162=3,AF162=2,AF162=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D162,FlatRepair!$Y$2:$Y$10000,AE162)*AG162,0)","v":0},0,4.763298778853545,0,0,0,0,0,4.763298778853545,0,{"$f":"IF($AF162=3,IF($AF$2=2,(R162/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I162,Refurb_Poss_Tbl[%]))*AG162,IF($AF$2=3,(R162*AG162)-AV162,R162*AG162)),0)","v":0},{"$f":"IF(AF162=3,IF($AF$2=2,(S162/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I162,Refurb_Poss_Tbl[%]))*AG162,IF($AF$2=3,(S162*AG162)-AX162,S162*AG162)),0)","v":0},{"$f":"IF($AF162=3,IF($AF$2=2,(T162/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I162,Refurb_Poss_Tbl[%]))*AG162,T162*$AG162),0)","v":0},{"$f":"IF($AF162=3,IF($AF$2=2,(Q162/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I162,Refurb_Poss_Tbl[%]))*AG162,Q162*$AG162),0)","v":0},{"$f":"IF($AF162=3,IF($AF$2=2,(U162/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I162,Refurb_Poss_Tbl[%]))*AG162,U162*$AG162),0)","v":0},{"$f":"IF($AF162=3,IF($AF$2=2,(V162/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I162,Refurb_Poss_Tbl[%]))*AG162,IF($AF$2=3,(V162*AG162)-AW162,V162*AG162)),0)","v":0},{"$f":"IF($AF162=3,IF($AF$2=2,(W162/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I162,Refurb_Poss_Tbl[%]))*AG162,W162*$AG162),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,60,2,{"$f":"VLOOKUP(AE163,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1697330900164177},0,0,0,0,0,0,0,0,2.8722435372694193E-4,{"$f":"IF(OR(AF163=3,AF163=2,AF163=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D163,FlatMaint!$Y$2:$Y$10000,AE163)*AG163,0)","v":4.6242746968633082},{"$f":"IF(OR(AF163=3,AF163=2,AF163=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D163,FlatRepair!$Y$2:$Y$10000,AE163)*AG163,0)","v":0},0,4.624561921217035,1.1820319046729451,0,0,0,0,5.8065938258899799,0,{"$f":"IF($AF163=3,IF($AF$2=2,(R163/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I163,Refurb_Poss_Tbl[%]))*AG163,IF($AF$2=3,(R163*AG163)-AV163,R163*AG163)),0)","v":0},{"$f":"IF(AF163=3,IF($AF$2=2,(S163/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I163,Refurb_Poss_Tbl[%]))*AG163,IF($AF$2=3,(S163*AG163)-AX163,S163*AG163)),0)","v":0},{"$f":"IF($AF163=3,IF($AF$2=2,(T163/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I163,Refurb_Poss_Tbl[%]))*AG163,T163*$AG163),0)","v":0},{"$f":"IF($AF163=3,IF($AF$2=2,(Q163/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I163,Refurb_Poss_Tbl[%]))*AG163,Q163*$AG163),0)","v":0},{"$f":"IF($AF163=3,IF($AF$2=2,(U163/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I163,Refurb_Poss_Tbl[%]))*AG163,U163*$AG163),0)","v":0},{"$f":"IF($AF163=3,IF($AF$2=2,(V163/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I163,Refurb_Poss_Tbl[%]))*AG163,IF($AF$2=3,(V163*AG163)-AW163,V163*AG163)),0)","v":0},{"$f":"IF($AF163=3,IF($AF$2=2,(W163/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I163,Refurb_Poss_Tbl[%]))*AG163,W163*$AG163),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,61,0,{"$f":"VLOOKUP(AE164,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.16478940778292983},0,0,0,0,0,0,0,0,2.7885859585139995E-4,{"$f":"IF(OR(AF164=3,AF164=2,AF164=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D164,FlatMaint!$Y$2:$Y$10000,AE164)*AG164,0)","v":4.4895870843333094},{"$f":"IF(OR(AF164=3,AF164=2,AF164=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D164,FlatRepair!$Y$2:$Y$10000,AE164)*AG164,0)","v":0},0,4.4898659429291605,0,0,0,0,0,4.4898659429291605,0,{"$f":"IF($AF164=3,IF($AF$2=2,(R164/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I164,Refurb_Poss_Tbl[%]))*AG164,IF($AF$2=3,(R164*AG164)-AV164,R164*AG164)),0)","v":0},{"$f":"IF(AF164=3,IF($AF$2=2,(S164/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I164,Refurb_Poss_Tbl[%]))*AG164,IF($AF$2=3,(S164*AG164)-AX164,S164*AG164)),0)","v":0},{"$f":"IF($AF164=3,IF($AF$2=2,(T164/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I164,Refurb_Poss_Tbl[%]))*AG164,T164*$AG164),0)","v":0},{"$f":"IF($AF164=3,IF($AF$2=2,(Q164/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I164,Refurb_Poss_Tbl[%]))*AG164,Q164*$AG164),0)","v":0},{"$f":"IF($AF164=3,IF($AF$2=2,(U164/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I164,Refurb_Poss_Tbl[%]))*AG164,U164*$AG164),0)","v":0},{"$f":"IF($AF164=3,IF($AF$2=2,(V164/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I164,Refurb_Poss_Tbl[%]))*AG164,IF($AF$2=3,(V164*AG164)-AW164,V164*AG164)),0)","v":0},{"$f":"IF($AF164=3,IF($AF$2=2,(W164/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I164,Refurb_Poss_Tbl[%]))*AG164,W164*$AG164),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,62,0,{"$f":"VLOOKUP(AE165,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15998971629410663},0,0,0,0,0,0,0,0,2.7073650082660192E-4,{"$f":"IF(OR(AF165=3,AF165=2,AF165=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D165,FlatMaint!$Y$2:$Y$10000,AE165)*AG165,0)","v":4.3588224119740868},{"$f":"IF(OR(AF165=3,AF165=2,AF165=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D165,FlatRepair!$Y$2:$Y$10000,AE165)*AG165,0)","v":0},0,4.3590931484749138,0,0,0,0,0,4.3590931484749138,0,{"$f":"IF($AF165=3,IF($AF$2=2,(R165/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I165,Refurb_Poss_Tbl[%]))*AG165,IF($AF$2=3,(R165*AG165)-AV165,R165*AG165)),0)","v":0},{"$f":"IF(AF165=3,IF($AF$2=2,(S165/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I165,Refurb_Poss_Tbl[%]))*AG165,IF($AF$2=3,(S165*AG165)-AX165,S165*AG165)),0)","v":0},{"$f":"IF($AF165=3,IF($AF$2=2,(T165/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I165,Refurb_Poss_Tbl[%]))*AG165,T165*$AG165),0)","v":0},{"$f":"IF($AF165=3,IF($AF$2=2,(Q165/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I165,Refurb_Poss_Tbl[%]))*AG165,Q165*$AG165),0)","v":0},{"$f":"IF($AF165=3,IF($AF$2=2,(U165/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I165,Refurb_Poss_Tbl[%]))*AG165,U165*$AG165),0)","v":0},{"$f":"IF($AF165=3,IF($AF$2=2,(V165/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I165,Refurb_Poss_Tbl[%]))*AG165,IF($AF$2=3,(V165*AG165)-AW165,V165*AG165)),0)","v":0},{"$f":"IF($AF165=3,IF($AF$2=2,(W165/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I165,Refurb_Poss_Tbl[%]))*AG165,W165*$AG165),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,63,0,{"$f":"VLOOKUP(AE166,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15532982164476369},0,0,0,0,0,0,0,0,2.6285097167631246E-4,{"$f":"IF(OR(AF166=3,AF166=2,AF166=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D166,FlatMaint!$Y$2:$Y$10000,AE166)*AG166,0)","v":4.2318664193923166},{"$f":"IF(OR(AF166=3,AF166=2,AF166=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D166,FlatRepair!$Y$2:$Y$10000,AE166)*AG166,0)","v":0},0,4.232129270363993,0,0,0,0,0,4.232129270363993,0,{"$f":"IF($AF166=3,IF($AF$2=2,(R166/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I166,Refurb_Poss_Tbl[%]))*AG166,IF($AF$2=3,(R166*AG166)-AV166,R166*AG166)),0)","v":0},{"$f":"IF(AF166=3,IF($AF$2=2,(S166/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I166,Refurb_Poss_Tbl[%]))*AG166,IF($AF$2=3,(S166*AG166)-AX166,S166*AG166)),0)","v":0},{"$f":"IF($AF166=3,IF($AF$2=2,(T166/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I166,Refurb_Poss_Tbl[%]))*AG166,T166*$AG166),0)","v":0},{"$f":"IF($AF166=3,IF($AF$2=2,(Q166/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I166,Refurb_Poss_Tbl[%]))*AG166,Q166*$AG166),0)","v":0},{"$f":"IF($AF166=3,IF($AF$2=2,(U166/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I166,Refurb_Poss_Tbl[%]))*AG166,U166*$AG166),0)","v":0},{"$f":"IF($AF166=3,IF($AF$2=2,(V166/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I166,Refurb_Poss_Tbl[%]))*AG166,IF($AF$2=3,(V166*AG166)-AW166,V166*AG166)),0)","v":0},{"$f":"IF($AF166=3,IF($AF$2=2,(W166/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I166,Refurb_Poss_Tbl[%]))*AG166,W166*$AG166),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,64,0,{"$f":"VLOOKUP(AE167,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15080565208229488},0,0,0,0,0,0,0,0,2.5519511813234229E-4,{"$f":"IF(OR(AF167=3,AF167=2,AF167=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D167,FlatMaint!$Y$2:$Y$10000,AE167)*AG167,0)","v":4.1086081741672986},{"$f":"IF(OR(AF167=3,AF167=2,AF167=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D167,FlatRepair!$Y$2:$Y$10000,AE167)*AG167,0)","v":0},0,4.1088633692854311,0,0,0,0,0,4.1088633692854311,0,{"$f":"IF($AF167=3,IF($AF$2=2,(R167/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I167,Refurb_Poss_Tbl[%]))*AG167,IF($AF$2=3,(R167*AG167)-AV167,R167*AG167)),0)","v":0},{"$f":"IF(AF167=3,IF($AF$2=2,(S167/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I167,Refurb_Poss_Tbl[%]))*AG167,IF($AF$2=3,(S167*AG167)-AX167,S167*AG167)),0)","v":0},{"$f":"IF($AF167=3,IF($AF$2=2,(T167/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I167,Refurb_Poss_Tbl[%]))*AG167,T167*$AG167),0)","v":0},{"$f":"IF($AF167=3,IF($AF$2=2,(Q167/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I167,Refurb_Poss_Tbl[%]))*AG167,Q167*$AG167),0)","v":0},{"$f":"IF($AF167=3,IF($AF$2=2,(U167/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I167,Refurb_Poss_Tbl[%]))*AG167,U167*$AG167),0)","v":0},{"$f":"IF($AF167=3,IF($AF$2=2,(V167/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I167,Refurb_Poss_Tbl[%]))*AG167,IF($AF$2=3,(V167*AG167)-AW167,V167*AG167)),0)","v":0},{"$f":"IF($AF167=3,IF($AF$2=2,(W167/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I167,Refurb_Poss_Tbl[%]))*AG167,W167*$AG167),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,65,0,{"$f":"VLOOKUP(AE168,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14641325444882999},0,0,0,0,0,0,0,0,2.4776225061392453E-4,{"$f":"IF(OR(AF168=3,AF168=2,AF168=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D168,FlatMaint!$Y$2:$Y$10000,AE168)*AG168,0)","v":3.9889399749197074},{"$f":"IF(OR(AF168=3,AF168=2,AF168=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D168,FlatRepair!$Y$2:$Y$10000,AE168)*AG168,0)","v":0},0,3.9891877371703215,0,0,0,0,0,3.9891877371703215,0,{"$f":"IF($AF168=3,IF($AF$2=2,(R168/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I168,Refurb_Poss_Tbl[%]))*AG168,IF($AF$2=3,(R168*AG168)-AV168,R168*AG168)),0)","v":0},{"$f":"IF(AF168=3,IF($AF$2=2,(S168/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I168,Refurb_Poss_Tbl[%]))*AG168,IF($AF$2=3,(S168*AG168)-AX168,S168*AG168)),0)","v":0},{"$f":"IF($AF168=3,IF($AF$2=2,(T168/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I168,Refurb_Poss_Tbl[%]))*AG168,T168*$AG168),0)","v":0},{"$f":"IF($AF168=3,IF($AF$2=2,(Q168/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I168,Refurb_Poss_Tbl[%]))*AG168,Q168*$AG168),0)","v":0},{"$f":"IF($AF168=3,IF($AF$2=2,(U168/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I168,Refurb_Poss_Tbl[%]))*AG168,U168*$AG168),0)","v":0},{"$f":"IF($AF168=3,IF($AF$2=2,(V168/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I168,Refurb_Poss_Tbl[%]))*AG168,IF($AF$2=3,(V168*AG168)-AW168,V168*AG168)),0)","v":0},{"$f":"IF($AF168=3,IF($AF$2=2,(W168/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I168,Refurb_Poss_Tbl[%]))*AG168,W168*$AG168),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,66,0,{"$f":"VLOOKUP(AE169,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14214879072701941},0,0,0,0,0,0,0,0,2.4054587438245104E-4,{"$f":"IF(OR(AF169=3,AF169=2,AF169=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D169,FlatMaint!$Y$2:$Y$10000,AE169)*AG169,0)","v":3.8727572572035993},{"$f":"IF(OR(AF169=3,AF169=2,AF169=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D169,FlatRepair!$Y$2:$Y$10000,AE169)*AG169,0)","v":0},0,3.8729978030779817,0,0,0,0,0,3.8729978030779817,0,{"$f":"IF($AF169=3,IF($AF$2=2,(R169/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I169,Refurb_Poss_Tbl[%]))*AG169,IF($AF$2=3,(R169*AG169)-AV169,R169*AG169)),0)","v":0},{"$f":"IF(AF169=3,IF($AF$2=2,(S169/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I169,Refurb_Poss_Tbl[%]))*AG169,IF($AF$2=3,(S169*AG169)-AX169,S169*AG169)),0)","v":0},{"$f":"IF($AF169=3,IF($AF$2=2,(T169/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I169,Refurb_Poss_Tbl[%]))*AG169,T169*$AG169),0)","v":0},{"$f":"IF($AF169=3,IF($AF$2=2,(Q169/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I169,Refurb_Poss_Tbl[%]))*AG169,Q169*$AG169),0)","v":0},{"$f":"IF($AF169=3,IF($AF$2=2,(U169/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I169,Refurb_Poss_Tbl[%]))*AG169,U169*$AG169),0)","v":0},{"$f":"IF($AF169=3,IF($AF$2=2,(V169/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I169,Refurb_Poss_Tbl[%]))*AG169,IF($AF$2=3,(V169*AG169)-AW169,V169*AG169)),0)","v":0},{"$f":"IF($AF169=3,IF($AF$2=2,(W169/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I169,Refurb_Poss_Tbl[%]))*AG169,W169*$AG169),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,67,0,{"$f":"VLOOKUP(AE170,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1380085346864266},0,0,0,0,0,0,0,0,2.3353968386645728E-4,{"$f":"IF(OR(AF170=3,AF170=2,AF170=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D170,FlatMaint!$Y$2:$Y$10000,AE170)*AG170,0)","v":3.7599585021394164},{"$f":"IF(OR(AF170=3,AF170=2,AF170=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D170,FlatRepair!$Y$2:$Y$10000,AE170)*AG170,0)","v":0},0,3.760192041823283,0,0,0,0,0,3.760192041823283,0,{"$f":"IF($AF170=3,IF($AF$2=2,(R170/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I170,Refurb_Poss_Tbl[%]))*AG170,IF($AF$2=3,(R170*AG170)-AV170,R170*AG170)),0)","v":0},{"$f":"IF(AF170=3,IF($AF$2=2,(S170/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I170,Refurb_Poss_Tbl[%]))*AG170,IF($AF$2=3,(S170*AG170)-AX170,S170*AG170)),0)","v":0},{"$f":"IF($AF170=3,IF($AF$2=2,(T170/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I170,Refurb_Poss_Tbl[%]))*AG170,T170*$AG170),0)","v":0},{"$f":"IF($AF170=3,IF($AF$2=2,(Q170/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I170,Refurb_Poss_Tbl[%]))*AG170,Q170*$AG170),0)","v":0},{"$f":"IF($AF170=3,IF($AF$2=2,(U170/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I170,Refurb_Poss_Tbl[%]))*AG170,U170*$AG170),0)","v":0},{"$f":"IF($AF170=3,IF($AF$2=2,(V170/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I170,Refurb_Poss_Tbl[%]))*AG170,IF($AF$2=3,(V170*AG170)-AW170,V170*AG170)),0)","v":0},{"$f":"IF($AF170=3,IF($AF$2=2,(W170/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I170,Refurb_Poss_Tbl[%]))*AG170,W170*$AG170),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,68,0,{"$f":"VLOOKUP(AE171,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13398886862759865},0,0,0,0,0,0,0,0,2.2673755715190029E-4,{"$f":"IF(OR(AF171=3,AF171=2,AF171=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D171,FlatMaint!$Y$2:$Y$10000,AE171)*AG171,0)","v":3.6504451477081719},{"$f":"IF(OR(AF171=3,AF171=2,AF171=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D171,FlatRepair!$Y$2:$Y$10000,AE171)*AG171,0)","v":0},0,3.6506718852653237,0,0,0,0,0,3.6506718852653237,0,{"$f":"IF($AF171=3,IF($AF$2=2,(R171/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I171,Refurb_Poss_Tbl[%]))*AG171,IF($AF$2=3,(R171*AG171)-AV171,R171*AG171)),0)","v":0},{"$f":"IF(AF171=3,IF($AF$2=2,(S171/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I171,Refurb_Poss_Tbl[%]))*AG171,IF($AF$2=3,(S171*AG171)-AX171,S171*AG171)),0)","v":0},{"$f":"IF($AF171=3,IF($AF$2=2,(T171/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I171,Refurb_Poss_Tbl[%]))*AG171,T171*$AG171),0)","v":0},{"$f":"IF($AF171=3,IF($AF$2=2,(Q171/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I171,Refurb_Poss_Tbl[%]))*AG171,Q171*$AG171),0)","v":0},{"$f":"IF($AF171=3,IF($AF$2=2,(U171/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I171,Refurb_Poss_Tbl[%]))*AG171,U171*$AG171),0)","v":0},{"$f":"IF($AF171=3,IF($AF$2=2,(V171/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I171,Refurb_Poss_Tbl[%]))*AG171,IF($AF$2=3,(V171*AG171)-AW171,V171*AG171)),0)","v":0},{"$f":"IF($AF171=3,IF($AF$2=2,(W171/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I171,Refurb_Poss_Tbl[%]))*AG171,W171*$AG171),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,69,0,{"$f":"VLOOKUP(AE172,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13008628022096957},0,0,0,0,0,0,0,0,2.2013355063291292E-4,{"$f":"IF(OR(AF172=3,AF172=2,AF172=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D172,FlatMaint!$Y$2:$Y$10000,AE172)*AG172,0)","v":3.5441215026292934},{"$f":"IF(OR(AF172=3,AF172=2,AF172=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D172,FlatRepair!$Y$2:$Y$10000,AE172)*AG172,0)","v":0},0,3.5443416361799263,0,0,0,0,0,3.5443416361799263,0,{"$f":"IF($AF172=3,IF($AF$2=2,(R172/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I172,Refurb_Poss_Tbl[%]))*AG172,IF($AF$2=3,(R172*AG172)-AV172,R172*AG172)),0)","v":0},{"$f":"IF(AF172=3,IF($AF$2=2,(S172/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I172,Refurb_Poss_Tbl[%]))*AG172,IF($AF$2=3,(S172*AG172)-AX172,S172*AG172)),0)","v":0},{"$f":"IF($AF172=3,IF($AF$2=2,(T172/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I172,Refurb_Poss_Tbl[%]))*AG172,T172*$AG172),0)","v":0},{"$f":"IF($AF172=3,IF($AF$2=2,(Q172/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I172,Refurb_Poss_Tbl[%]))*AG172,Q172*$AG172),0)","v":0},{"$f":"IF($AF172=3,IF($AF$2=2,(U172/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I172,Refurb_Poss_Tbl[%]))*AG172,U172*$AG172),0)","v":0},{"$f":"IF($AF172=3,IF($AF$2=2,(V172/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I172,Refurb_Poss_Tbl[%]))*AG172,IF($AF$2=3,(V172*AG172)-AW172,V172*AG172)),0)","v":0},{"$f":"IF($AF172=3,IF($AF$2=2,(W172/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I172,Refurb_Poss_Tbl[%]))*AG172,W172*$AG172),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,70,0,{"$f":"VLOOKUP(AE173,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12629735943783454},0,0,0,0,0,0,0,0,2.1372189381836207E-4,{"$f":"IF(OR(AF173=3,AF173=2,AF173=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D173,FlatMaint!$Y$2:$Y$10000,AE173)*AG173,0)","v":3.4408946627468868},{"$f":"IF(OR(AF173=3,AF173=2,AF173=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D173,FlatRepair!$Y$2:$Y$10000,AE173)*AG173,0)","v":0},0,3.4411083846407053,0,0,0,0,0,3.4411083846407053,0,{"$f":"IF($AF173=3,IF($AF$2=2,(R173/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I173,Refurb_Poss_Tbl[%]))*AG173,IF($AF$2=3,(R173*AG173)-AV173,R173*AG173)),0)","v":0},{"$f":"IF(AF173=3,IF($AF$2=2,(S173/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I173,Refurb_Poss_Tbl[%]))*AG173,IF($AF$2=3,(S173*AG173)-AX173,S173*AG173)),0)","v":0},{"$f":"IF($AF173=3,IF($AF$2=2,(T173/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I173,Refurb_Poss_Tbl[%]))*AG173,T173*$AG173),0)","v":0},{"$f":"IF($AF173=3,IF($AF$2=2,(Q173/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I173,Refurb_Poss_Tbl[%]))*AG173,Q173*$AG173),0)","v":0},{"$f":"IF($AF173=3,IF($AF$2=2,(U173/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I173,Refurb_Poss_Tbl[%]))*AG173,U173*$AG173),0)","v":0},{"$f":"IF($AF173=3,IF($AF$2=2,(V173/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I173,Refurb_Poss_Tbl[%]))*AG173,IF($AF$2=3,(V173*AG173)-AW173,V173*AG173)),0)","v":0},{"$f":"IF($AF173=3,IF($AF$2=2,(W173/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I173,Refurb_Poss_Tbl[%]))*AG173,W173*$AG173),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,71,0,{"$f":"VLOOKUP(AE174,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12261879557071313},0,0,0,0,0,0,0,0,2.074969842896719E-4,{"$f":"IF(OR(AF174=3,AF174=2,AF174=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D174,FlatMaint!$Y$2:$Y$10000,AE174)*AG174,0)","v":3.340674429851346},{"$f":"IF(OR(AF174=3,AF174=2,AF174=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D174,FlatRepair!$Y$2:$Y$10000,AE174)*AG174,0)","v":0},0,3.3408819268356358,0,0,0,0,0,3.3408819268356358,0,{"$f":"IF($AF174=3,IF($AF$2=2,(R174/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I174,Refurb_Poss_Tbl[%]))*AG174,IF($AF$2=3,(R174*AG174)-AV174,R174*AG174)),0)","v":0},{"$f":"IF(AF174=3,IF($AF$2=2,(S174/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I174,Refurb_Poss_Tbl[%]))*AG174,IF($AF$2=3,(S174*AG174)-AX174,S174*AG174)),0)","v":0},{"$f":"IF($AF174=3,IF($AF$2=2,(T174/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I174,Refurb_Poss_Tbl[%]))*AG174,T174*$AG174),0)","v":0},{"$f":"IF($AF174=3,IF($AF$2=2,(Q174/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I174,Refurb_Poss_Tbl[%]))*AG174,Q174*$AG174),0)","v":0},{"$f":"IF($AF174=3,IF($AF$2=2,(U174/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I174,Refurb_Poss_Tbl[%]))*AG174,U174*$AG174),0)","v":0},{"$f":"IF($AF174=3,IF($AF$2=2,(V174/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I174,Refurb_Poss_Tbl[%]))*AG174,IF($AF$2=3,(V174*AG174)-AW174,V174*AG174)),0)","v":0},{"$f":"IF($AF174=3,IF($AF$2=2,(W174/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I174,Refurb_Poss_Tbl[%]))*AG174,W174*$AG174),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,72,0,{"$f":"VLOOKUP(AE175,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1190473743404982},0,0,0,0,0,0,0,0,2.0145338280550671E-4,{"$f":"IF(OR(AF175=3,AF175=2,AF175=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D175,FlatMaint!$Y$2:$Y$10000,AE175)*AG175,0)","v":3.2433732328653848},{"$f":"IF(OR(AF175=3,AF175=2,AF175=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D175,FlatRepair!$Y$2:$Y$10000,AE175)*AG175,0)","v":0},0,3.2435746862481905,0,0,0,0,0,3.2435746862481905,0,{"$f":"IF($AF175=3,IF($AF$2=2,(R175/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I175,Refurb_Poss_Tbl[%]))*AG175,IF($AF$2=3,(R175*AG175)-AV175,R175*AG175)),0)","v":0},{"$f":"IF(AF175=3,IF($AF$2=2,(S175/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I175,Refurb_Poss_Tbl[%]))*AG175,IF($AF$2=3,(S175*AG175)-AX175,S175*AG175)),0)","v":0},{"$f":"IF($AF175=3,IF($AF$2=2,(T175/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I175,Refurb_Poss_Tbl[%]))*AG175,T175*$AG175),0)","v":0},{"$f":"IF($AF175=3,IF($AF$2=2,(Q175/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I175,Refurb_Poss_Tbl[%]))*AG175,Q175*$AG175),0)","v":0},{"$f":"IF($AF175=3,IF($AF$2=2,(U175/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I175,Refurb_Poss_Tbl[%]))*AG175,U175*$AG175),0)","v":0},{"$f":"IF($AF175=3,IF($AF$2=2,(V175/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I175,Refurb_Poss_Tbl[%]))*AG175,IF($AF$2=3,(V175*AG175)-AW175,V175*AG175)),0)","v":0},{"$f":"IF($AF175=3,IF($AF$2=2,(W175/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I175,Refurb_Poss_Tbl[%]))*AG175,W175*$AG175),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,73,0,{"$f":"VLOOKUP(AE176,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11557997508786232},0,0,0,0,0,0,0,0,1.955858085490356E-4,{"$f":"IF(OR(AF176=3,AF176=2,AF176=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D176,FlatMaint!$Y$2:$Y$10000,AE176)*AG176,0)","v":3.148906051325616},{"$f":"IF(OR(AF176=3,AF176=2,AF176=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D176,FlatRepair!$Y$2:$Y$10000,AE176)*AG176,0)","v":0},0,3.1491016371341649,0,0,0,0,0,3.1491016371341649,0,{"$f":"IF($AF176=3,IF($AF$2=2,(R176/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I176,Refurb_Poss_Tbl[%]))*AG176,IF($AF$2=3,(R176*AG176)-AV176,R176*AG176)),0)","v":0},{"$f":"IF(AF176=3,IF($AF$2=2,(S176/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I176,Refurb_Poss_Tbl[%]))*AG176,IF($AF$2=3,(S176*AG176)-AX176,S176*AG176)),0)","v":0},{"$f":"IF($AF176=3,IF($AF$2=2,(T176/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I176,Refurb_Poss_Tbl[%]))*AG176,T176*$AG176),0)","v":0},{"$f":"IF($AF176=3,IF($AF$2=2,(Q176/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I176,Refurb_Poss_Tbl[%]))*AG176,Q176*$AG176),0)","v":0},{"$f":"IF($AF176=3,IF($AF$2=2,(U176/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I176,Refurb_Poss_Tbl[%]))*AG176,U176*$AG176),0)","v":0},{"$f":"IF($AF176=3,IF($AF$2=2,(V176/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I176,Refurb_Poss_Tbl[%]))*AG176,IF($AF$2=3,(V176*AG176)-AW176,V176*AG176)),0)","v":0},{"$f":"IF($AF176=3,IF($AF$2=2,(W176/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I176,Refurb_Poss_Tbl[%]))*AG176,W176*$AG176),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,74,0,{"$f":"VLOOKUP(AE177,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11221356804646829},0,0,0,0,0,0,0,0,1.8988913451362685E-4,{"$f":"IF(OR(AF177=3,AF177=2,AF177=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D177,FlatMaint!$Y$2:$Y$10000,AE177)*AG177,0)","v":3.0571903410928316},{"$f":"IF(OR(AF177=3,AF177=2,AF177=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D177,FlatRepair!$Y$2:$Y$10000,AE177)*AG177,0)","v":0},0,3.0573802302273454,0,0,0,0,0,3.0573802302273454,0,{"$f":"IF($AF177=3,IF($AF$2=2,(R177/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I177,Refurb_Poss_Tbl[%]))*AG177,IF($AF$2=3,(R177*AG177)-AV177,R177*AG177)),0)","v":0},{"$f":"IF(AF177=3,IF($AF$2=2,(S177/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I177,Refurb_Poss_Tbl[%]))*AG177,IF($AF$2=3,(S177*AG177)-AX177,S177*AG177)),0)","v":0},{"$f":"IF($AF177=3,IF($AF$2=2,(T177/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I177,Refurb_Poss_Tbl[%]))*AG177,T177*$AG177),0)","v":0},{"$f":"IF($AF177=3,IF($AF$2=2,(Q177/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I177,Refurb_Poss_Tbl[%]))*AG177,Q177*$AG177),0)","v":0},{"$f":"IF($AF177=3,IF($AF$2=2,(U177/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I177,Refurb_Poss_Tbl[%]))*AG177,U177*$AG177),0)","v":0},{"$f":"IF($AF177=3,IF($AF$2=2,(V177/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I177,Refurb_Poss_Tbl[%]))*AG177,IF($AF$2=3,(V177*AG177)-AW177,V177*AG177)),0)","v":0},{"$f":"IF($AF177=3,IF($AF$2=2,(W177/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I177,Refurb_Poss_Tbl[%]))*AG177,W177*$AG177),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,75,0,{"$f":"VLOOKUP(AE178,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10894521169560026},0,0,0,0,0,0,0,0,1.8435838302293864E-4,{"$f":"IF(OR(AF178=3,AF178=2,AF178=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D178,FlatMaint!$Y$2:$Y$10000,AE178)*AG178,0)","v":2.9681459622260493},{"$f":"IF(OR(AF178=3,AF178=2,AF178=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D178,FlatRepair!$Y$2:$Y$10000,AE178)*AG178,0)","v":0},0,2.9683303206090721,0,0,0,0,0,2.9683303206090721,0,{"$f":"IF($AF178=3,IF($AF$2=2,(R178/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I178,Refurb_Poss_Tbl[%]))*AG178,IF($AF$2=3,(R178*AG178)-AV178,R178*AG178)),0)","v":0},{"$f":"IF(AF178=3,IF($AF$2=2,(S178/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I178,Refurb_Poss_Tbl[%]))*AG178,IF($AF$2=3,(S178*AG178)-AX178,S178*AG178)),0)","v":0},{"$f":"IF($AF178=3,IF($AF$2=2,(T178/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I178,Refurb_Poss_Tbl[%]))*AG178,T178*$AG178),0)","v":0},{"$f":"IF($AF178=3,IF($AF$2=2,(Q178/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I178,Refurb_Poss_Tbl[%]))*AG178,Q178*$AG178),0)","v":0},{"$f":"IF($AF178=3,IF($AF$2=2,(U178/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I178,Refurb_Poss_Tbl[%]))*AG178,U178*$AG178),0)","v":0},{"$f":"IF($AF178=3,IF($AF$2=2,(V178/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I178,Refurb_Poss_Tbl[%]))*AG178,IF($AF$2=3,(V178*AG178)-AW178,V178*AG178)),0)","v":0},{"$f":"IF($AF178=3,IF($AF$2=2,(W178/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I178,Refurb_Poss_Tbl[%]))*AG178,W178*$AG178),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,76,0,{"$f":"VLOOKUP(AE179,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15310389176729922},0,0,0,0,0,0,0,0,2.5908422666251236E-4,{"$f":"IF(OR(AF179=3,AF179=2,AF179=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D179,FlatMaint!$Y$2:$Y$10000,AE179)*AG179,0)","v":4.1712223151203949},{"$f":"IF(OR(AF179=3,AF179=2,AF179=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D179,FlatRepair!$Y$2:$Y$10000,AE179)*AG179,0)","v":0},0,4.1714813993470576,0,0,0,0,0,4.1714813993470576,0,{"$f":"IF($AF179=3,IF($AF$2=2,(R179/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I179,Refurb_Poss_Tbl[%]))*AG179,IF($AF$2=3,(R179*AG179)-AV179,R179*AG179)),0)","v":0},{"$f":"IF(AF179=3,IF($AF$2=2,(S179/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I179,Refurb_Poss_Tbl[%]))*AG179,IF($AF$2=3,(S179*AG179)-AX179,S179*AG179)),0)","v":0},{"$f":"IF($AF179=3,IF($AF$2=2,(T179/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I179,Refurb_Poss_Tbl[%]))*AG179,T179*$AG179),0)","v":0},{"$f":"IF($AF179=3,IF($AF$2=2,(Q179/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I179,Refurb_Poss_Tbl[%]))*AG179,Q179*$AG179),0)","v":0},{"$f":"IF($AF179=3,IF($AF$2=2,(U179/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I179,Refurb_Poss_Tbl[%]))*AG179,U179*$AG179),0)","v":0},{"$f":"IF($AF179=3,IF($AF$2=2,(V179/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I179,Refurb_Poss_Tbl[%]))*AG179,IF($AF$2=3,(V179*AG179)-AW179,V179*AG179)),0)","v":0},{"$f":"IF($AF179=3,IF($AF$2=2,(W179/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I179,Refurb_Poss_Tbl[%]))*AG179,W179*$AG179),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,77,0,{"$f":"VLOOKUP(AE180,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14936965050468218},0,0,0,0,0,0,0,0,2.5276509918293894E-4,{"$f":"IF(OR(AF180=3,AF180=2,AF180=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D180,FlatMaint!$Y$2:$Y$10000,AE180)*AG180,0)","v":4.0694851854833125},{"$f":"IF(OR(AF180=3,AF180=2,AF180=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D180,FlatRepair!$Y$2:$Y$10000,AE180)*AG180,0)","v":0},0,4.0697379505824953,0,0,0,0,0,4.0697379505824953,0,{"$f":"IF($AF180=3,IF($AF$2=2,(R180/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I180,Refurb_Poss_Tbl[%]))*AG180,IF($AF$2=3,(R180*AG180)-AV180,R180*AG180)),0)","v":0},{"$f":"IF(AF180=3,IF($AF$2=2,(S180/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I180,Refurb_Poss_Tbl[%]))*AG180,IF($AF$2=3,(S180*AG180)-AX180,S180*AG180)),0)","v":0},{"$f":"IF($AF180=3,IF($AF$2=2,(T180/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I180,Refurb_Poss_Tbl[%]))*AG180,T180*$AG180),0)","v":0},{"$f":"IF($AF180=3,IF($AF$2=2,(Q180/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I180,Refurb_Poss_Tbl[%]))*AG180,Q180*$AG180),0)","v":0},{"$f":"IF($AF180=3,IF($AF$2=2,(U180/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I180,Refurb_Poss_Tbl[%]))*AG180,U180*$AG180),0)","v":0},{"$f":"IF($AF180=3,IF($AF$2=2,(V180/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I180,Refurb_Poss_Tbl[%]))*AG180,IF($AF$2=3,(V180*AG180)-AW180,V180*AG180)),0)","v":0},{"$f":"IF($AF180=3,IF($AF$2=2,(W180/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I180,Refurb_Poss_Tbl[%]))*AG180,W180*$AG180),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,78,0,{"$f":"VLOOKUP(AE181,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14572648829725093},0,0,0,0,0,0,0,0,2.466000967638429E-4,{"$f":"IF(OR(AF181=3,AF181=2,AF181=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D181,FlatMaint!$Y$2:$Y$10000,AE181)*AG181,0)","v":3.9702294492520132},{"$f":"IF(OR(AF181=3,AF181=2,AF181=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D181,FlatRepair!$Y$2:$Y$10000,AE181)*AG181,0)","v":0},0,3.9704760493487772,0,0,0,0,0,3.9704760493487772,0,{"$f":"IF($AF181=3,IF($AF$2=2,(R181/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I181,Refurb_Poss_Tbl[%]))*AG181,IF($AF$2=3,(R181*AG181)-AV181,R181*AG181)),0)","v":0},{"$f":"IF(AF181=3,IF($AF$2=2,(S181/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I181,Refurb_Poss_Tbl[%]))*AG181,IF($AF$2=3,(S181*AG181)-AX181,S181*AG181)),0)","v":0},{"$f":"IF($AF181=3,IF($AF$2=2,(T181/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I181,Refurb_Poss_Tbl[%]))*AG181,T181*$AG181),0)","v":0},{"$f":"IF($AF181=3,IF($AF$2=2,(Q181/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I181,Refurb_Poss_Tbl[%]))*AG181,Q181*$AG181),0)","v":0},{"$f":"IF($AF181=3,IF($AF$2=2,(U181/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I181,Refurb_Poss_Tbl[%]))*AG181,U181*$AG181),0)","v":0},{"$f":"IF($AF181=3,IF($AF$2=2,(V181/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I181,Refurb_Poss_Tbl[%]))*AG181,IF($AF$2=3,(V181*AG181)-AW181,V181*AG181)),0)","v":0},{"$f":"IF($AF181=3,IF($AF$2=2,(W181/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I181,Refurb_Poss_Tbl[%]))*AG181,W181*$AG181),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,79,0,{"$f":"VLOOKUP(AE182,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14217218370463502},0,0,0,0,0,0,0,0,2.4058546025740765E-4,{"$f":"IF(OR(AF182=3,AF182=2,AF182=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D182,FlatMaint!$Y$2:$Y$10000,AE182)*AG182,0)","v":3.8733945846361095},{"$f":"IF(OR(AF182=3,AF182=2,AF182=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D182,FlatRepair!$Y$2:$Y$10000,AE182)*AG182,0)","v":0},0,3.8736351700963669,0,0,0,0,0,3.8736351700963669,0,{"$f":"IF($AF182=3,IF($AF$2=2,(R182/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I182,Refurb_Poss_Tbl[%]))*AG182,IF($AF$2=3,(R182*AG182)-AV182,R182*AG182)),0)","v":0},{"$f":"IF(AF182=3,IF($AF$2=2,(S182/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I182,Refurb_Poss_Tbl[%]))*AG182,IF($AF$2=3,(S182*AG182)-AX182,S182*AG182)),0)","v":0},{"$f":"IF($AF182=3,IF($AF$2=2,(T182/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I182,Refurb_Poss_Tbl[%]))*AG182,T182*$AG182),0)","v":0},{"$f":"IF($AF182=3,IF($AF$2=2,(Q182/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I182,Refurb_Poss_Tbl[%]))*AG182,Q182*$AG182),0)","v":0},{"$f":"IF($AF182=3,IF($AF$2=2,(U182/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I182,Refurb_Poss_Tbl[%]))*AG182,U182*$AG182),0)","v":0},{"$f":"IF($AF182=3,IF($AF$2=2,(V182/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I182,Refurb_Poss_Tbl[%]))*AG182,IF($AF$2=3,(V182*AG182)-AW182,V182*AG182)),0)","v":0},{"$f":"IF($AF182=3,IF($AF$2=2,(W182/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I182,Refurb_Poss_Tbl[%]))*AG182,W182*$AG182),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,80,0,{"$f":"VLOOKUP(AE183,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13870456946793663},0,0,0,0,0,0,0,0,2.3471752220234897E-4,{"$f":"IF(OR(AF183=3,AF183=2,AF183=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D183,FlatMaint!$Y$2:$Y$10000,AE183)*AG183,0)","v":3.7789215459864489},{"$f":"IF(OR(AF183=3,AF183=2,AF183=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D183,FlatRepair!$Y$2:$Y$10000,AE183)*AG183,0)","v":0},0,3.7791562635086513,0,0,0,0,0,3.7791562635086513,0,{"$f":"IF($AF183=3,IF($AF$2=2,(R183/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I183,Refurb_Poss_Tbl[%]))*AG183,IF($AF$2=3,(R183*AG183)-AV183,R183*AG183)),0)","v":0},{"$f":"IF(AF183=3,IF($AF$2=2,(S183/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I183,Refurb_Poss_Tbl[%]))*AG183,IF($AF$2=3,(S183*AG183)-AX183,S183*AG183)),0)","v":0},{"$f":"IF($AF183=3,IF($AF$2=2,(T183/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I183,Refurb_Poss_Tbl[%]))*AG183,T183*$AG183),0)","v":0},{"$f":"IF($AF183=3,IF($AF$2=2,(Q183/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I183,Refurb_Poss_Tbl[%]))*AG183,Q183*$AG183),0)","v":0},{"$f":"IF($AF183=3,IF($AF$2=2,(U183/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I183,Refurb_Poss_Tbl[%]))*AG183,U183*$AG183),0)","v":0},{"$f":"IF($AF183=3,IF($AF$2=2,(V183/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I183,Refurb_Poss_Tbl[%]))*AG183,IF($AF$2=3,(V183*AG183)-AW183,V183*AG183)),0)","v":0},{"$f":"IF($AF183=3,IF($AF$2=2,(W183/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I183,Refurb_Poss_Tbl[%]))*AG183,W183*$AG183),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,81,0,{"$f":"VLOOKUP(AE184,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13532153118823087},0,0,0,0,0,0,0,0,2.2899270458765755E-4,{"$f":"IF(OR(AF184=3,AF184=2,AF184=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D184,FlatMaint!$Y$2:$Y$10000,AE184)*AG184,0)","v":3.6867527277916579},{"$f":"IF(OR(AF184=3,AF184=2,AF184=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D184,FlatRepair!$Y$2:$Y$10000,AE184)*AG184,0)","v":0},0,3.6869817204962456,0,0,0,0,0,3.6869817204962456,0,{"$f":"IF($AF184=3,IF($AF$2=2,(R184/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I184,Refurb_Poss_Tbl[%]))*AG184,IF($AF$2=3,(R184*AG184)-AV184,R184*AG184)),0)","v":0},{"$f":"IF(AF184=3,IF($AF$2=2,(S184/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I184,Refurb_Poss_Tbl[%]))*AG184,IF($AF$2=3,(S184*AG184)-AX184,S184*AG184)),0)","v":0},{"$f":"IF($AF184=3,IF($AF$2=2,(T184/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I184,Refurb_Poss_Tbl[%]))*AG184,T184*$AG184),0)","v":0},{"$f":"IF($AF184=3,IF($AF$2=2,(Q184/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I184,Refurb_Poss_Tbl[%]))*AG184,Q184*$AG184),0)","v":0},{"$f":"IF($AF184=3,IF($AF$2=2,(U184/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I184,Refurb_Poss_Tbl[%]))*AG184,U184*$AG184),0)","v":0},{"$f":"IF($AF184=3,IF($AF$2=2,(V184/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I184,Refurb_Poss_Tbl[%]))*AG184,IF($AF$2=3,(V184*AG184)-AW184,V184*AG184)),0)","v":0},{"$f":"IF($AF184=3,IF($AF$2=2,(W184/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I184,Refurb_Poss_Tbl[%]))*AG184,W184*$AG184),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,82,0,{"$f":"VLOOKUP(AE185,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13202100603729841},0,0,0,0,0,0,0,0,2.2340751667088542E-4,{"$f":"IF(OR(AF185=3,AF185=2,AF185=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D185,FlatMaint!$Y$2:$Y$10000,AE185)*AG185,0)","v":3.5968319295528368},{"$f":"IF(OR(AF185=3,AF185=2,AF185=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D185,FlatRepair!$Y$2:$Y$10000,AE185)*AG185,0)","v":0},0,3.5970553370695075,0,0,0,0,0,3.5970553370695075,0,{"$f":"IF($AF185=3,IF($AF$2=2,(R185/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I185,Refurb_Poss_Tbl[%]))*AG185,IF($AF$2=3,(R185*AG185)-AV185,R185*AG185)),0)","v":0},{"$f":"IF(AF185=3,IF($AF$2=2,(S185/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I185,Refurb_Poss_Tbl[%]))*AG185,IF($AF$2=3,(S185*AG185)-AX185,S185*AG185)),0)","v":0},{"$f":"IF($AF185=3,IF($AF$2=2,(T185/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I185,Refurb_Poss_Tbl[%]))*AG185,T185*$AG185),0)","v":0},{"$f":"IF($AF185=3,IF($AF$2=2,(Q185/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I185,Refurb_Poss_Tbl[%]))*AG185,Q185*$AG185),0)","v":0},{"$f":"IF($AF185=3,IF($AF$2=2,(U185/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I185,Refurb_Poss_Tbl[%]))*AG185,U185*$AG185),0)","v":0},{"$f":"IF($AF185=3,IF($AF$2=2,(V185/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I185,Refurb_Poss_Tbl[%]))*AG185,IF($AF$2=3,(V185*AG185)-AW185,V185*AG185)),0)","v":0},{"$f":"IF($AF185=3,IF($AF$2=2,(W185/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I185,Refurb_Poss_Tbl[%]))*AG185,W185*$AG185),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,83,0,{"$f":"VLOOKUP(AE186,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12880098149980332},0,0,0,0,0,0,0,0,2.1795855284964429E-4,{"$f":"IF(OR(AF186=3,AF186=2,AF186=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D186,FlatMaint!$Y$2:$Y$10000,AE186)*AG186,0)","v":3.5091043215149624},{"$f":"IF(OR(AF186=3,AF186=2,AF186=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D186,FlatRepair!$Y$2:$Y$10000,AE186)*AG186,0)","v":0},0,3.5093222800678121,0,0,0,0,0,3.5093222800678121,0,{"$f":"IF($AF186=3,IF($AF$2=2,(R186/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I186,Refurb_Poss_Tbl[%]))*AG186,IF($AF$2=3,(R186*AG186)-AV186,R186*AG186)),0)","v":0},{"$f":"IF(AF186=3,IF($AF$2=2,(S186/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I186,Refurb_Poss_Tbl[%]))*AG186,IF($AF$2=3,(S186*AG186)-AX186,S186*AG186)),0)","v":0},{"$f":"IF($AF186=3,IF($AF$2=2,(T186/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I186,Refurb_Poss_Tbl[%]))*AG186,T186*$AG186),0)","v":0},{"$f":"IF($AF186=3,IF($AF$2=2,(Q186/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I186,Refurb_Poss_Tbl[%]))*AG186,Q186*$AG186),0)","v":0},{"$f":"IF($AF186=3,IF($AF$2=2,(U186/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I186,Refurb_Poss_Tbl[%]))*AG186,U186*$AG186),0)","v":0},{"$f":"IF($AF186=3,IF($AF$2=2,(V186/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I186,Refurb_Poss_Tbl[%]))*AG186,IF($AF$2=3,(V186*AG186)-AW186,V186*AG186)),0)","v":0},{"$f":"IF($AF186=3,IF($AF$2=2,(W186/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I186,Refurb_Poss_Tbl[%]))*AG186,W186*$AG186),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,84,0,{"$f":"VLOOKUP(AE187,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1256594941461496},0,0,0,0,0,0,0,0,2.1264249058501887E-4,{"$f":"IF(OR(AF187=3,AF187=2,AF187=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D187,FlatMaint!$Y$2:$Y$10000,AE187)*AG187,0)","v":3.4235164112341105},{"$f":"IF(OR(AF187=3,AF187=2,AF187=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D187,FlatRepair!$Y$2:$Y$10000,AE187)*AG187,0)","v":0},0,3.4237290537246956,0,0,0,0,0,3.4237290537246956,0,{"$f":"IF($AF187=3,IF($AF$2=2,(R187/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I187,Refurb_Poss_Tbl[%]))*AG187,IF($AF$2=3,(R187*AG187)-AV187,R187*AG187)),0)","v":0},{"$f":"IF(AF187=3,IF($AF$2=2,(S187/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I187,Refurb_Poss_Tbl[%]))*AG187,IF($AF$2=3,(S187*AG187)-AX187,S187*AG187)),0)","v":0},{"$f":"IF($AF187=3,IF($AF$2=2,(T187/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I187,Refurb_Poss_Tbl[%]))*AG187,T187*$AG187),0)","v":0},{"$f":"IF($AF187=3,IF($AF$2=2,(Q187/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I187,Refurb_Poss_Tbl[%]))*AG187,Q187*$AG187),0)","v":0},{"$f":"IF($AF187=3,IF($AF$2=2,(U187/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I187,Refurb_Poss_Tbl[%]))*AG187,U187*$AG187),0)","v":0},{"$f":"IF($AF187=3,IF($AF$2=2,(V187/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I187,Refurb_Poss_Tbl[%]))*AG187,IF($AF$2=3,(V187*AG187)-AW187,V187*AG187)),0)","v":0},{"$f":"IF($AF187=3,IF($AF$2=2,(W187/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I187,Refurb_Poss_Tbl[%]))*AG187,W187*$AG187),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,85,0,{"$f":"VLOOKUP(AE188,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1225946284352679},0,0,0,0,0,0,0,0,2.0745608837562815E-4,{"$f":"IF(OR(AF188=3,AF188=2,AF188=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D188,FlatMaint!$Y$2:$Y$10000,AE188)*AG188,0)","v":3.3400160109601078},{"$f":"IF(OR(AF188=3,AF188=2,AF188=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D188,FlatRepair!$Y$2:$Y$10000,AE188)*AG188,0)","v":0},0,3.3402234670484834,0,0,0,0,0,3.3402234670484834,0,{"$f":"IF($AF188=3,IF($AF$2=2,(R188/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I188,Refurb_Poss_Tbl[%]))*AG188,IF($AF$2=3,(R188*AG188)-AV188,R188*AG188)),0)","v":0},{"$f":"IF(AF188=3,IF($AF$2=2,(S188/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I188,Refurb_Poss_Tbl[%]))*AG188,IF($AF$2=3,(S188*AG188)-AX188,S188*AG188)),0)","v":0},{"$f":"IF($AF188=3,IF($AF$2=2,(T188/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I188,Refurb_Poss_Tbl[%]))*AG188,T188*$AG188),0)","v":0},{"$f":"IF($AF188=3,IF($AF$2=2,(Q188/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I188,Refurb_Poss_Tbl[%]))*AG188,Q188*$AG188),0)","v":0},{"$f":"IF($AF188=3,IF($AF$2=2,(U188/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I188,Refurb_Poss_Tbl[%]))*AG188,U188*$AG188),0)","v":0},{"$f":"IF($AF188=3,IF($AF$2=2,(V188/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I188,Refurb_Poss_Tbl[%]))*AG188,IF($AF$2=3,(V188*AG188)-AW188,V188*AG188)),0)","v":0},{"$f":"IF($AF188=3,IF($AF$2=2,(W188/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I188,Refurb_Poss_Tbl[%]))*AG188,W188*$AG188),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,86,0,{"$f":"VLOOKUP(AE189,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11960451554660284},0,0,0,0,0,0,0,0,2.0239618378110067E-4,{"$f":"IF(OR(AF189=3,AF189=2,AF189=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D189,FlatMaint!$Y$2:$Y$10000,AE189)*AG189,0)","v":3.2585522058147394},{"$f":"IF(OR(AF189=3,AF189=2,AF189=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D189,FlatRepair!$Y$2:$Y$10000,AE189)*AG189,0)","v":0},0,3.2587546019985205,0,0,0,0,0,3.2587546019985205,0,{"$f":"IF($AF189=3,IF($AF$2=2,(R189/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I189,Refurb_Poss_Tbl[%]))*AG189,IF($AF$2=3,(R189*AG189)-AV189,R189*AG189)),0)","v":0},{"$f":"IF(AF189=3,IF($AF$2=2,(S189/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I189,Refurb_Poss_Tbl[%]))*AG189,IF($AF$2=3,(S189*AG189)-AX189,S189*AG189)),0)","v":0},{"$f":"IF($AF189=3,IF($AF$2=2,(T189/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I189,Refurb_Poss_Tbl[%]))*AG189,T189*$AG189),0)","v":0},{"$f":"IF($AF189=3,IF($AF$2=2,(Q189/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I189,Refurb_Poss_Tbl[%]))*AG189,Q189*$AG189),0)","v":0},{"$f":"IF($AF189=3,IF($AF$2=2,(U189/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I189,Refurb_Poss_Tbl[%]))*AG189,U189*$AG189),0)","v":0},{"$f":"IF($AF189=3,IF($AF$2=2,(V189/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I189,Refurb_Poss_Tbl[%]))*AG189,IF($AF$2=3,(V189*AG189)-AW189,V189*AG189)),0)","v":0},{"$f":"IF($AF189=3,IF($AF$2=2,(W189/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I189,Refurb_Poss_Tbl[%]))*AG189,W189*$AG189),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,87,0,{"$f":"VLOOKUP(AE190,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11668733224058814},0,0,0,0,0,0,0,0,1.9745969149375674E-4,{"$f":"IF(OR(AF190=3,AF190=2,AF190=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D190,FlatMaint!$Y$2:$Y$10000,AE190)*AG190,0)","v":3.1790753227460873},{"$f":"IF(OR(AF190=3,AF190=2,AF190=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D190,FlatRepair!$Y$2:$Y$10000,AE190)*AG190,0)","v":0},0,3.179272782437581,0,0,0,0,0,3.179272782437581,0,{"$f":"IF($AF190=3,IF($AF$2=2,(R190/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I190,Refurb_Poss_Tbl[%]))*AG190,IF($AF$2=3,(R190*AG190)-AV190,R190*AG190)),0)","v":0},{"$f":"IF(AF190=3,IF($AF$2=2,(S190/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I190,Refurb_Poss_Tbl[%]))*AG190,IF($AF$2=3,(S190*AG190)-AX190,S190*AG190)),0)","v":0},{"$f":"IF($AF190=3,IF($AF$2=2,(T190/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I190,Refurb_Poss_Tbl[%]))*AG190,T190*$AG190),0)","v":0},{"$f":"IF($AF190=3,IF($AF$2=2,(Q190/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I190,Refurb_Poss_Tbl[%]))*AG190,Q190*$AG190),0)","v":0},{"$f":"IF($AF190=3,IF($AF$2=2,(U190/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I190,Refurb_Poss_Tbl[%]))*AG190,U190*$AG190),0)","v":0},{"$f":"IF($AF190=3,IF($AF$2=2,(V190/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I190,Refurb_Poss_Tbl[%]))*AG190,IF($AF$2=3,(V190*AG190)-AW190,V190*AG190)),0)","v":0},{"$f":"IF($AF190=3,IF($AF$2=2,(W190/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I190,Refurb_Poss_Tbl[%]))*AG190,W190*$AG190),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,88,0,{"$f":"VLOOKUP(AE191,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11384129974691526},0,0,0,0,0,0,0,0,1.9264360145732366E-4,{"$f":"IF(OR(AF191=3,AF191=2,AF191=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D191,FlatMaint!$Y$2:$Y$10000,AE191)*AG191,0)","v":3.101536900240085},{"$f":"IF(OR(AF191=3,AF191=2,AF191=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D191,FlatRepair!$Y$2:$Y$10000,AE191)*AG191,0)","v":0},0,3.1017295438415422,0,0,0,0,0,3.1017295438415422,0,{"$f":"IF($AF191=3,IF($AF$2=2,(R191/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I191,Refurb_Poss_Tbl[%]))*AG191,IF($AF$2=3,(R191*AG191)-AV191,R191*AG191)),0)","v":0},{"$f":"IF(AF191=3,IF($AF$2=2,(S191/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I191,Refurb_Poss_Tbl[%]))*AG191,IF($AF$2=3,(S191*AG191)-AX191,S191*AG191)),0)","v":0},{"$f":"IF($AF191=3,IF($AF$2=2,(T191/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I191,Refurb_Poss_Tbl[%]))*AG191,T191*$AG191),0)","v":0},{"$f":"IF($AF191=3,IF($AF$2=2,(Q191/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I191,Refurb_Poss_Tbl[%]))*AG191,Q191*$AG191),0)","v":0},{"$f":"IF($AF191=3,IF($AF$2=2,(U191/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I191,Refurb_Poss_Tbl[%]))*AG191,U191*$AG191),0)","v":0},{"$f":"IF($AF191=3,IF($AF$2=2,(V191/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I191,Refurb_Poss_Tbl[%]))*AG191,IF($AF$2=3,(V191*AG191)-AW191,V191*AG191)),0)","v":0},{"$f":"IF($AF191=3,IF($AF$2=2,(W191/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I191,Refurb_Poss_Tbl[%]))*AG191,W191*$AG191),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,89,0,{"$f":"VLOOKUP(AE192,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11106468267991736},0,0,0,0,0,0,0,0,1.8794497703153532E-4,{"$f":"IF(OR(AF192=3,AF192=2,AF192=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D192,FlatMaint!$Y$2:$Y$10000,AE192)*AG192,0)","v":3.0258896587708155},{"$f":"IF(OR(AF192=3,AF192=2,AF192=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D192,FlatRepair!$Y$2:$Y$10000,AE192)*AG192,0)","v":0},0,3.0260776037478472,0,0,0,0,0,3.0260776037478472,0,{"$f":"IF($AF192=3,IF($AF$2=2,(R192/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I192,Refurb_Poss_Tbl[%]))*AG192,IF($AF$2=3,(R192*AG192)-AV192,R192*AG192)),0)","v":0},{"$f":"IF(AF192=3,IF($AF$2=2,(S192/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I192,Refurb_Poss_Tbl[%]))*AG192,IF($AF$2=3,(S192*AG192)-AX192,S192*AG192)),0)","v":0},{"$f":"IF($AF192=3,IF($AF$2=2,(T192/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I192,Refurb_Poss_Tbl[%]))*AG192,T192*$AG192),0)","v":0},{"$f":"IF($AF192=3,IF($AF$2=2,(Q192/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I192,Refurb_Poss_Tbl[%]))*AG192,Q192*$AG192),0)","v":0},{"$f":"IF($AF192=3,IF($AF$2=2,(U192/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I192,Refurb_Poss_Tbl[%]))*AG192,U192*$AG192),0)","v":0},{"$f":"IF($AF192=3,IF($AF$2=2,(V192/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I192,Refurb_Poss_Tbl[%]))*AG192,IF($AF$2=3,(V192*AG192)-AW192,V192*AG192)),0)","v":0},{"$f":"IF($AF192=3,IF($AF$2=2,(W192/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I192,Refurb_Poss_Tbl[%]))*AG192,W192*$AG192),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,90,0,{"$f":"VLOOKUP(AE193,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10835578798040717},0,0,0,0,0,0,0,0,1.8336095320149786E-4,{"$f":"IF(OR(AF193=3,AF193=2,AF193=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D193,FlatMaint!$Y$2:$Y$10000,AE193)*AG193,0)","v":2.9520874719715273},{"$f":"IF(OR(AF193=3,AF193=2,AF193=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D193,FlatRepair!$Y$2:$Y$10000,AE193)*AG193,0)","v":0},0,2.9522708329247287,0,0,0,0,0,2.9522708329247287,0,{"$f":"IF($AF193=3,IF($AF$2=2,(R193/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I193,Refurb_Poss_Tbl[%]))*AG193,IF($AF$2=3,(R193*AG193)-AV193,R193*AG193)),0)","v":0},{"$f":"IF(AF193=3,IF($AF$2=2,(S193/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I193,Refurb_Poss_Tbl[%]))*AG193,IF($AF$2=3,(S193*AG193)-AX193,S193*AG193)),0)","v":0},{"$f":"IF($AF193=3,IF($AF$2=2,(T193/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I193,Refurb_Poss_Tbl[%]))*AG193,T193*$AG193),0)","v":0},{"$f":"IF($AF193=3,IF($AF$2=2,(Q193/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I193,Refurb_Poss_Tbl[%]))*AG193,Q193*$AG193),0)","v":0},{"$f":"IF($AF193=3,IF($AF$2=2,(U193/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I193,Refurb_Poss_Tbl[%]))*AG193,U193*$AG193),0)","v":0},{"$f":"IF($AF193=3,IF($AF$2=2,(V193/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I193,Refurb_Poss_Tbl[%]))*AG193,IF($AF$2=3,(V193*AG193)-AW193,V193*AG193)),0)","v":0},{"$f":"IF($AF193=3,IF($AF$2=2,(W193/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I193,Refurb_Poss_Tbl[%]))*AG193,W193*$AG193),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,91,0,{"$f":"VLOOKUP(AE194,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10571296388332406},0,0,0,0,0,0,0,0,1.7888873483072962E-4,{"$f":"IF(OR(AF194=3,AF194=2,AF194=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D194,FlatMaint!$Y$2:$Y$10000,AE194)*AG194,0)","v":2.880085338508807},{"$f":"IF(OR(AF194=3,AF194=2,AF194=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D194,FlatRepair!$Y$2:$Y$10000,AE194)*AG194,0)","v":0},0,2.8802642272436376,0,0,0,0,0,2.8802642272436376,0,{"$f":"IF($AF194=3,IF($AF$2=2,(R194/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I194,Refurb_Poss_Tbl[%]))*AG194,IF($AF$2=3,(R194*AG194)-AV194,R194*AG194)),0)","v":0},{"$f":"IF(AF194=3,IF($AF$2=2,(S194/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I194,Refurb_Poss_Tbl[%]))*AG194,IF($AF$2=3,(S194*AG194)-AX194,S194*AG194)),0)","v":0},{"$f":"IF($AF194=3,IF($AF$2=2,(T194/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I194,Refurb_Poss_Tbl[%]))*AG194,T194*$AG194),0)","v":0},{"$f":"IF($AF194=3,IF($AF$2=2,(Q194/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I194,Refurb_Poss_Tbl[%]))*AG194,Q194*$AG194),0)","v":0},{"$f":"IF($AF194=3,IF($AF$2=2,(U194/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I194,Refurb_Poss_Tbl[%]))*AG194,U194*$AG194),0)","v":0},{"$f":"IF($AF194=3,IF($AF$2=2,(V194/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I194,Refurb_Poss_Tbl[%]))*AG194,IF($AF$2=3,(V194*AG194)-AW194,V194*AG194)),0)","v":0},{"$f":"IF($AF194=3,IF($AF$2=2,(W194/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I194,Refurb_Poss_Tbl[%]))*AG194,W194*$AG194),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,92,0,{"$f":"VLOOKUP(AE195,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10313459891056008},{"$f":"IF(AE195=0,Q195*AG195,0)","v":0},{"$f":"IF(AE195=0,R195*AG195,0)","v":0},{"$f":"IF(AE195=0,S195*AG195,0)","v":0},{"$f":"IF(AE195=0,T195*AG195,0)","v":0},{"$f":"IF(AE195=0,U195*AG195,0)","v":0},{"$f":"IF(AE195=0,V195*AG195,0)","v":0},{"$f":"IF(AE195=0,W195*AG195,0)","v":0},{"$f":"IF(AE195=0,AH195+AI195+AJ195+AK195+AL195+AM195+AN195,0)","v":0},{"$f":"IF(OR(AF195=3,AF195=2,AF195=0),Y195*AG195,0)","v":1.745255949568094E-4},{"$f":"IF(OR(AF195=3,AF195=2,AF195=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D195,FlatMaint!$Y$2:$Y$10000,AE195)*AG195,0)","v":2.8098393546427389},{"$f":"IF(OR(AF195=3,AF195=2,AF195=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D195,FlatRepair!$Y$2:$Y$10000,AE195)*AG195,0)","v":0},{"$f":"IF(OR(AF195=3,AF195=2,AF195=0),Z195*AG195,0)","v":0},{"$f":"AP195+AQ195+AR195+AS195","v":2.8100138802376957},{"$f":"IF(AF195=2,AA195*AG195,0)","v":0},{"$f":"IF(AF195=3,AB195*AG195,0)","v":0},{"$f":"IF(AF195=3,AC195*AG195,0)","v":0},{"$f":"IF(AF195=3,AD195*AG195,0)","v":0},{"$f":"IF($AF$2=3,BB195+BC195+BD195+BE195+BF195+BG195+BH195,BB195+BC195+BD195+BE195+BF195+BG195+BH195)","v":0},{"$f":"AO195+AT195+AU195+AV195+AW195+AX195+AY195+BA195","v":2.8100138802376957},{"$f":"IFERROR(IF(AE195=100,IF(O195=3,(N195/H195)*(X195*AG195)*-1,(N195/M195)*(X195*AG195)*-1),0),0)","v":0},{"$f":"IF($AF195=3,IF($AF$2=2,(R195/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I195,Refurb_Poss_Tbl[%]))*AG195,IF($AF$2=3,(R195*AG195)-AV195,R195*AG195)),0)","v":0},{"$f":"IF(AF195=3,IF($AF$2=2,(S195/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I195,Refurb_Poss_Tbl[%]))*AG195,IF($AF$2=3,(S195*AG195)-AX195,S195*AG195)),0)","v":0},{"$f":"IF($AF195=3,IF($AF$2=2,(T195/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I195,Refurb_Poss_Tbl[%]))*AG195,T195*$AG195),0)","v":0},{"$f":"IF($AF195=3,IF($AF$2=2,(Q195/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I195,Refurb_Poss_Tbl[%]))*AG195,Q195*$AG195),0)","v":0},{"$f":"IF($AF195=3,IF($AF$2=2,(U195/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I195,Refurb_Poss_Tbl[%]))*AG195,U195*$AG195),0)","v":0},{"$f":"IF($AF195=3,IF($AF$2=2,(V195/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I195,Refurb_Poss_Tbl[%]))*AG195,IF($AF$2=3,(V195*AG195)-AW195,V195*AG195)),0)","v":0},{"$f":"IF($AF195=3,IF($AF$2=2,(W195/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I195,Refurb_Poss_Tbl[%]))*AG195,W195*$AG195),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,93,0,{"$f":"VLOOKUP(AE196,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10061912088835129},0,0,0,0,0,0,0,0,1.7026887312859452E-4,{"$f":"IF(OR(AF196=3,AF196=2,AF196=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D196,FlatMaint!$Y$2:$Y$10000,AE196)*AG196,0)","v":2.7413066874563303},{"$f":"IF(OR(AF196=3,AF196=2,AF196=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D196,FlatRepair!$Y$2:$Y$10000,AE196)*AG196,0)","v":0},0,2.7414769563294588,0,0,0,0,0,2.7414769563294588,0,{"$f":"IF($AF196=3,IF($AF$2=2,(R196/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I196,Refurb_Poss_Tbl[%]))*AG196,IF($AF$2=3,(R196*AG196)-AV196,R196*AG196)),0)","v":0},{"$f":"IF(AF196=3,IF($AF$2=2,(S196/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I196,Refurb_Poss_Tbl[%]))*AG196,IF($AF$2=3,(S196*AG196)-AX196,S196*AG196)),0)","v":0},{"$f":"IF($AF196=3,IF($AF$2=2,(T196/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I196,Refurb_Poss_Tbl[%]))*AG196,T196*$AG196),0)","v":0},{"$f":"IF($AF196=3,IF($AF$2=2,(Q196/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I196,Refurb_Poss_Tbl[%]))*AG196,Q196*$AG196),0)","v":0},{"$f":"IF($AF196=3,IF($AF$2=2,(U196/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I196,Refurb_Poss_Tbl[%]))*AG196,U196*$AG196),0)","v":0},{"$f":"IF($AF196=3,IF($AF$2=2,(V196/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I196,Refurb_Poss_Tbl[%]))*AG196,IF($AF$2=3,(V196*AG196)-AW196,V196*AG196)),0)","v":0},{"$f":"IF($AF196=3,IF($AF$2=2,(W196/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I196,Refurb_Poss_Tbl[%]))*AG196,W196*$AG196),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,94,0,{"$f":"VLOOKUP(AE197,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.8164995988635415E-2},0,0,0,0,0,0,0,0,1.6611597378399467E-4,{"$f":"IF(OR(AF197=3,AF197=2,AF197=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D197,FlatMaint!$Y$2:$Y$10000,AE197)*AG197,0)","v":2.6744455487378835},{"$f":"IF(OR(AF197=3,AF197=2,AF197=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D197,FlatRepair!$Y$2:$Y$10000,AE197)*AG197,0)","v":0},0,2.6746116647116676,0,0,0,0,0,2.6746116647116676,0,{"$f":"IF($AF197=3,IF($AF$2=2,(R197/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I197,Refurb_Poss_Tbl[%]))*AG197,IF($AF$2=3,(R197*AG197)-AV197,R197*AG197)),0)","v":0},{"$f":"IF(AF197=3,IF($AF$2=2,(S197/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I197,Refurb_Poss_Tbl[%]))*AG197,IF($AF$2=3,(S197*AG197)-AX197,S197*AG197)),0)","v":0},{"$f":"IF($AF197=3,IF($AF$2=2,(T197/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I197,Refurb_Poss_Tbl[%]))*AG197,T197*$AG197),0)","v":0},{"$f":"IF($AF197=3,IF($AF$2=2,(Q197/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I197,Refurb_Poss_Tbl[%]))*AG197,Q197*$AG197),0)","v":0},{"$f":"IF($AF197=3,IF($AF$2=2,(U197/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I197,Refurb_Poss_Tbl[%]))*AG197,U197*$AG197),0)","v":0},{"$f":"IF($AF197=3,IF($AF$2=2,(V197/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I197,Refurb_Poss_Tbl[%]))*AG197,IF($AF$2=3,(V197*AG197)-AW197,V197*AG197)),0)","v":0},{"$f":"IF($AF197=3,IF($AF$2=2,(W197/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I197,Refurb_Poss_Tbl[%]))*AG197,W197*$AG197),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,95,0,{"$f":"VLOOKUP(AE198,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.577072779379063E-2},0,0,0,0,0,0,0,0,1.6206436466731185E-4,{"$f":"IF(OR(AF198=3,AF198=2,AF198=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D198,FlatMaint!$Y$2:$Y$10000,AE198)*AG198,0)","v":2.609215169500374},{"$f":"IF(OR(AF198=3,AF198=2,AF198=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D198,FlatRepair!$Y$2:$Y$10000,AE198)*AG198,0)","v":0},0,2.6093772338650414,0,0,0,0,0,2.6093772338650414,0,{"$f":"IF($AF198=3,IF($AF$2=2,(R198/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I198,Refurb_Poss_Tbl[%]))*AG198,IF($AF$2=3,(R198*AG198)-AV198,R198*AG198)),0)","v":0},{"$f":"IF(AF198=3,IF($AF$2=2,(S198/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I198,Refurb_Poss_Tbl[%]))*AG198,IF($AF$2=3,(S198*AG198)-AX198,S198*AG198)),0)","v":0},{"$f":"IF($AF198=3,IF($AF$2=2,(T198/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I198,Refurb_Poss_Tbl[%]))*AG198,T198*$AG198),0)","v":0},{"$f":"IF($AF198=3,IF($AF$2=2,(Q198/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I198,Refurb_Poss_Tbl[%]))*AG198,Q198*$AG198),0)","v":0},{"$f":"IF($AF198=3,IF($AF$2=2,(U198/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I198,Refurb_Poss_Tbl[%]))*AG198,U198*$AG198),0)","v":0},{"$f":"IF($AF198=3,IF($AF$2=2,(V198/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I198,Refurb_Poss_Tbl[%]))*AG198,IF($AF$2=3,(V198*AG198)-AW198,V198*AG198)),0)","v":0},{"$f":"IF($AF198=3,IF($AF$2=2,(W198/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I198,Refurb_Poss_Tbl[%]))*AG198,W198*$AG198),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,96,0,{"$f":"VLOOKUP(AE199,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.3434856384185999E-2},0,0,0,0,0,0,0,0,1.5811157528518232E-4,{"$f":"IF(OR(AF199=3,AF199=2,AF199=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D199,FlatMaint!$Y$2:$Y$10000,AE199)*AG199,0)","v":2.5455757751223165},{"$f":"IF(OR(AF199=3,AF199=2,AF199=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D199,FlatRepair!$Y$2:$Y$10000,AE199)*AG199,0)","v":0},0,2.5457338866976018,0,0,0,0,0,2.5457338866976018,0,{"$f":"IF($AF199=3,IF($AF$2=2,(R199/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I199,Refurb_Poss_Tbl[%]))*AG199,IF($AF$2=3,(R199*AG199)-AV199,R199*AG199)),0)","v":0},{"$f":"IF(AF199=3,IF($AF$2=2,(S199/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I199,Refurb_Poss_Tbl[%]))*AG199,IF($AF$2=3,(S199*AG199)-AX199,S199*AG199)),0)","v":0},{"$f":"IF($AF199=3,IF($AF$2=2,(T199/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I199,Refurb_Poss_Tbl[%]))*AG199,T199*$AG199),0)","v":0},{"$f":"IF($AF199=3,IF($AF$2=2,(Q199/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I199,Refurb_Poss_Tbl[%]))*AG199,Q199*$AG199),0)","v":0},{"$f":"IF($AF199=3,IF($AF$2=2,(U199/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I199,Refurb_Poss_Tbl[%]))*AG199,U199*$AG199),0)","v":0},{"$f":"IF($AF199=3,IF($AF$2=2,(V199/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I199,Refurb_Poss_Tbl[%]))*AG199,IF($AF$2=3,(V199*AG199)-AW199,V199*AG199)),0)","v":0},{"$f":"IF($AF199=3,IF($AF$2=2,(W199/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I199,Refurb_Poss_Tbl[%]))*AG199,W199*$AG199),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,97,0,{"$f":"VLOOKUP(AE200,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.1155957447986352E-2},0,0,0,0,0,0,0,0,1.542551954001779E-4,{"$f":"IF(OR(AF200=3,AF200=2,AF200=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D200,FlatMaint!$Y$2:$Y$10000,AE200)*AG200,0)","v":2.4834885610949433},{"$f":"IF(OR(AF200=3,AF200=2,AF200=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D200,FlatRepair!$Y$2:$Y$10000,AE200)*AG200,0)","v":0},0,2.4836428162903434,0,0,0,0,0,2.4836428162903434,0,{"$f":"IF($AF200=3,IF($AF$2=2,(R200/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I200,Refurb_Poss_Tbl[%]))*AG200,IF($AF$2=3,(R200*AG200)-AV200,R200*AG200)),0)","v":0},{"$f":"IF(AF200=3,IF($AF$2=2,(S200/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I200,Refurb_Poss_Tbl[%]))*AG200,IF($AF$2=3,(S200*AG200)-AX200,S200*AG200)),0)","v":0},{"$f":"IF($AF200=3,IF($AF$2=2,(T200/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I200,Refurb_Poss_Tbl[%]))*AG200,T200*$AG200),0)","v":0},{"$f":"IF($AF200=3,IF($AF$2=2,(Q200/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I200,Refurb_Poss_Tbl[%]))*AG200,Q200*$AG200),0)","v":0},{"$f":"IF($AF200=3,IF($AF$2=2,(U200/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I200,Refurb_Poss_Tbl[%]))*AG200,U200*$AG200),0)","v":0},{"$f":"IF($AF200=3,IF($AF$2=2,(V200/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I200,Refurb_Poss_Tbl[%]))*AG200,IF($AF$2=3,(V200*AG200)-AW200,V200*AG200)),0)","v":0},{"$f":"IF($AF200=3,IF($AF$2=2,(W200/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I200,Refurb_Poss_Tbl[%]))*AG200,W200*$AG200),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,98,0,{"$f":"VLOOKUP(AE201,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.8932641412669614E-2},0,0,0,0,0,0,0,0,1.5049287356114918E-4,{"$f":"IF(OR(AF201=3,AF201=2,AF201=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D201,FlatMaint!$Y$2:$Y$10000,AE201)*AG201,0)","v":2.4229156693609202},{"$f":"IF(OR(AF201=3,AF201=2,AF201=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D201,FlatRepair!$Y$2:$Y$10000,AE201)*AG201,0)","v":0},0,2.4230661622344813,0,0,0,0,0,2.4230661622344813,0,{"$f":"IF($AF201=3,IF($AF$2=2,(R201/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I201,Refurb_Poss_Tbl[%]))*AG201,IF($AF$2=3,(R201*AG201)-AV201,R201*AG201)),0)","v":0},{"$f":"IF(AF201=3,IF($AF$2=2,(S201/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I201,Refurb_Poss_Tbl[%]))*AG201,IF($AF$2=3,(S201*AG201)-AX201,S201*AG201)),0)","v":0},{"$f":"IF($AF201=3,IF($AF$2=2,(T201/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I201,Refurb_Poss_Tbl[%]))*AG201,T201*$AG201),0)","v":0},{"$f":"IF($AF201=3,IF($AF$2=2,(Q201/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I201,Refurb_Poss_Tbl[%]))*AG201,Q201*$AG201),0)","v":0},{"$f":"IF($AF201=3,IF($AF$2=2,(U201/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I201,Refurb_Poss_Tbl[%]))*AG201,U201*$AG201),0)","v":0},{"$f":"IF($AF201=3,IF($AF$2=2,(V201/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I201,Refurb_Poss_Tbl[%]))*AG201,IF($AF$2=3,(V201*AG201)-AW201,V201*AG201)),0)","v":0},{"$f":"IF($AF201=3,IF($AF$2=2,(W201/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I201,Refurb_Poss_Tbl[%]))*AG201,W201*$AG201),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,99,0,{"$f":"VLOOKUP(AE202,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.6763552597726459E-2},0,0,0,0,0,0,0,0,1.4682231566941385E-4,{"$f":"IF(OR(AF202=3,AF202=2,AF202=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D202,FlatMaint!$Y$2:$Y$10000,AE202)*AG202,0)","v":2.3638201652301665},{"$f":"IF(OR(AF202=3,AF202=2,AF202=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D202,FlatRepair!$Y$2:$Y$10000,AE202)*AG202,0)","v":0},0,2.3639669875458358,0,0,0,0,0,2.3639669875458358,0,{"$f":"IF($AF202=3,IF($AF$2=2,(R202/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I202,Refurb_Poss_Tbl[%]))*AG202,IF($AF$2=3,(R202*AG202)-AV202,R202*AG202)),0)","v":0},{"$f":"IF(AF202=3,IF($AF$2=2,(S202/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I202,Refurb_Poss_Tbl[%]))*AG202,IF($AF$2=3,(S202*AG202)-AX202,S202*AG202)),0)","v":0},{"$f":"IF($AF202=3,IF($AF$2=2,(T202/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I202,Refurb_Poss_Tbl[%]))*AG202,T202*$AG202),0)","v":0},{"$f":"IF($AF202=3,IF($AF$2=2,(Q202/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I202,Refurb_Poss_Tbl[%]))*AG202,Q202*$AG202),0)","v":0},{"$f":"IF($AF202=3,IF($AF$2=2,(U202/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I202,Refurb_Poss_Tbl[%]))*AG202,U202*$AG202),0)","v":0},{"$f":"IF($AF202=3,IF($AF$2=2,(V202/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I202,Refurb_Poss_Tbl[%]))*AG202,IF($AF$2=3,(V202*AG202)-AW202,V202*AG202)),0)","v":0},{"$f":"IF($AF202=3,IF($AF$2=2,(W202/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I202,Refurb_Poss_Tbl[%]))*AG202,W202*$AG202),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229104,27.229104,0.22829150779999999,0.15109149233164601,3.9895343921807196E-3,0.169879485196166,0,7.3895334888847503E-2,27.856251354608801,1.69221189397518E-3,0,6.9640628386522101,0.41874023103680202,1.9947671960903598E-3,7.5545746165823005E-2,100,3,{"$f":"VLOOKUP(AE203,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.4647368388025807E-2},0,0,0,0,0,0,0,0,1.4324128357991593E-4,{"$f":"IF(OR(AF203=3,AF203=2,AF203=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D203,FlatMaint!$Y$2:$Y$10000,AE203)*AG203,0)","v":2.3061660148586984},{"$f":"IF(OR(AF203=3,AF203=2,AF203=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D203,FlatRepair!$Y$2:$Y$10000,AE203)*AG203,0)","v":0},0,2.3063092561422782,0,3.5445258595459217E-2,1.6885179369581E-4,6.3947486058467083E-3,2.3579583703230176,0.77634586825527485,-3.9299306172050237,{"$f":"IF($AF203=3,IF($AF$2=2,(R203/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I203,Refurb_Poss_Tbl[%]))*AG203,IF($AF$2=3,(R203*AG203)-AV203,R203*AG203)),0)","v":1.9324275360604465E-2},{"$f":"IF(AF203=3,IF($AF$2=2,(S203/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I203,Refurb_Poss_Tbl[%]))*AG203,IF($AF$2=3,(S203*AG203)-AX203,S203*AG203)),0)","v":1.2789497211693417E-2},{"$f":"IF($AF203=3,IF($AF$2=2,(T203/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I203,Refurb_Poss_Tbl[%]))*AG203,T203*$AG203),0)","v":3.3770358739162001E-4},{"$f":"IF($AF203=3,IF($AF$2=2,(Q203/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I203,Refurb_Poss_Tbl[%]))*AG203,Q203*$AG203),0)","v":2.3048719971638669},{"$f":"IF($AF203=3,IF($AF$2=2,(U203/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I203,Refurb_Poss_Tbl[%]))*AG203,U203*$AG203),0)","v":1.4379851364968039E-2},{"$f":"IF($AF203=3,IF($AF$2=2,(V203/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I203,Refurb_Poss_Tbl[%]))*AG203,IF($AF$2=3,(V203*AG203)-AW203,V203*AG203)),0)","v":0},{"$f":"IF($AF203=3,IF($AF$2=2,(W203/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I203,Refurb_Poss_Tbl[%]))*AG203,W203*$AG203),0)","v":6.2550456344928106E-3}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,0,1,{"$f":"VLOOKUP(AE204,ValidationLists!$M$1:$N$102,2,FALSE)","v":1},885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024108,0,{"$f":"IF(OR(AF204=3,AF204=2,AF204=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D204,FlatMaint!$Y$2:$Y$10000,AE204)*AG204,0)","v":0},{"$f":"IF(OR(AF204=3,AF204=2,AF204=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D204,FlatRepair!$Y$2:$Y$10000,AE204)*AG204,0)","v":0},0,0,0,0,0,0,0,896.48640996024108,0,{"$f":"IF($AF204=3,IF($AF$2=2,(R204/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I204,Refurb_Poss_Tbl[%]))*AG204,IF($AF$2=3,(R204*AG204)-AV204,R204*AG204)),0)","v":0},{"$f":"IF(AF204=3,IF($AF$2=2,(S204/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I204,Refurb_Poss_Tbl[%]))*AG204,IF($AF$2=3,(S204*AG204)-AX204,S204*AG204)),0)","v":0},{"$f":"IF($AF204=3,IF($AF$2=2,(T204/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I204,Refurb_Poss_Tbl[%]))*AG204,T204*$AG204),0)","v":0},{"$f":"IF($AF204=3,IF($AF$2=2,(Q204/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I204,Refurb_Poss_Tbl[%]))*AG204,Q204*$AG204),0)","v":0},{"$f":"IF($AF204=3,IF($AF$2=2,(U204/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I204,Refurb_Poss_Tbl[%]))*AG204,U204*$AG204),0)","v":0},{"$f":"IF($AF204=3,IF($AF$2=2,(V204/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I204,Refurb_Poss_Tbl[%]))*AG204,IF($AF$2=3,(V204*AG204)-AW204,V204*AG204)),0)","v":0},{"$f":"IF($AF204=3,IF($AF$2=2,(W204/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I204,Refurb_Poss_Tbl[%]))*AG204,W204*$AG204),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,1,0,{"$f":"VLOOKUP(AE205,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.96618357487922713},0,0,0,0,0,0,0,0,5.3176365472818073E-2,{"$f":"IF(OR(AF205=3,AF205=2,AF205=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D205,FlatMaint!$Y$2:$Y$10000,AE205)*AG205,0)","v":85.579987592270541},{"$f":"IF(OR(AF205=3,AF205=2,AF205=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D205,FlatRepair!$Y$2:$Y$10000,AE205)*AG205,0)","v":0},0,85.633163957743363,0,0,0,0,0,85.633163957743363,0,{"$f":"IF($AF205=3,IF($AF$2=2,(R205/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I205,Refurb_Poss_Tbl[%]))*AG205,IF($AF$2=3,(R205*AG205)-AV205,R205*AG205)),0)","v":0},{"$f":"IF(AF205=3,IF($AF$2=2,(S205/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I205,Refurb_Poss_Tbl[%]))*AG205,IF($AF$2=3,(S205*AG205)-AX205,S205*AG205)),0)","v":0},{"$f":"IF($AF205=3,IF($AF$2=2,(T205/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I205,Refurb_Poss_Tbl[%]))*AG205,T205*$AG205),0)","v":0},{"$f":"IF($AF205=3,IF($AF$2=2,(Q205/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I205,Refurb_Poss_Tbl[%]))*AG205,Q205*$AG205),0)","v":0},{"$f":"IF($AF205=3,IF($AF$2=2,(U205/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I205,Refurb_Poss_Tbl[%]))*AG205,U205*$AG205),0)","v":0},{"$f":"IF($AF205=3,IF($AF$2=2,(V205/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I205,Refurb_Poss_Tbl[%]))*AG205,IF($AF$2=3,(V205*AG205)-AW205,V205*AG205)),0)","v":0},{"$f":"IF($AF205=3,IF($AF$2=2,(W205/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I205,Refurb_Poss_Tbl[%]))*AG205,W205*$AG205),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,2,0,{"$f":"VLOOKUP(AE206,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.93351070036640305},0,0,0,0,0,0,0,0,5.1378130891611661E-2,{"$f":"IF(OR(AF206=3,AF206=2,AF206=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D206,FlatMaint!$Y$2:$Y$10000,AE206)*AG206,0)","v":82.685978350019852},{"$f":"IF(OR(AF206=3,AF206=2,AF206=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D206,FlatRepair!$Y$2:$Y$10000,AE206)*AG206,0)","v":82.685978350019852},0,165.42333483093131,0,0,0,0,0,165.42333483093131,0,{"$f":"IF($AF206=3,IF($AF$2=2,(R206/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I206,Refurb_Poss_Tbl[%]))*AG206,IF($AF$2=3,(R206*AG206)-AV206,R206*AG206)),0)","v":0},{"$f":"IF(AF206=3,IF($AF$2=2,(S206/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I206,Refurb_Poss_Tbl[%]))*AG206,IF($AF$2=3,(S206*AG206)-AX206,S206*AG206)),0)","v":0},{"$f":"IF($AF206=3,IF($AF$2=2,(T206/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I206,Refurb_Poss_Tbl[%]))*AG206,T206*$AG206),0)","v":0},{"$f":"IF($AF206=3,IF($AF$2=2,(Q206/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I206,Refurb_Poss_Tbl[%]))*AG206,Q206*$AG206),0)","v":0},{"$f":"IF($AF206=3,IF($AF$2=2,(U206/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I206,Refurb_Poss_Tbl[%]))*AG206,U206*$AG206),0)","v":0},{"$f":"IF($AF206=3,IF($AF$2=2,(V206/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I206,Refurb_Poss_Tbl[%]))*AG206,IF($AF$2=3,(V206*AG206)-AW206,V206*AG206)),0)","v":0},{"$f":"IF($AF206=3,IF($AF$2=2,(W206/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I206,Refurb_Poss_Tbl[%]))*AG206,W206*$AG206),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,3,0,{"$f":"VLOOKUP(AE207,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.90194270566802237},0,0,0,0,0,0,0,0,4.9640706175470214E-2,{"$f":"IF(OR(AF207=3,AF207=2,AF207=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D207,FlatMaint!$Y$2:$Y$10000,AE207)*AG207,0)","v":79.889834154608565},{"$f":"IF(OR(AF207=3,AF207=2,AF207=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D207,FlatRepair!$Y$2:$Y$10000,AE207)*AG207,0)","v":0},0,79.939474860784031,0,0,0,0,0,79.939474860784031,0,{"$f":"IF($AF207=3,IF($AF$2=2,(R207/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I207,Refurb_Poss_Tbl[%]))*AG207,IF($AF$2=3,(R207*AG207)-AV207,R207*AG207)),0)","v":0},{"$f":"IF(AF207=3,IF($AF$2=2,(S207/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I207,Refurb_Poss_Tbl[%]))*AG207,IF($AF$2=3,(S207*AG207)-AX207,S207*AG207)),0)","v":0},{"$f":"IF($AF207=3,IF($AF$2=2,(T207/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I207,Refurb_Poss_Tbl[%]))*AG207,T207*$AG207),0)","v":0},{"$f":"IF($AF207=3,IF($AF$2=2,(Q207/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I207,Refurb_Poss_Tbl[%]))*AG207,Q207*$AG207),0)","v":0},{"$f":"IF($AF207=3,IF($AF$2=2,(U207/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I207,Refurb_Poss_Tbl[%]))*AG207,U207*$AG207),0)","v":0},{"$f":"IF($AF207=3,IF($AF$2=2,(V207/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I207,Refurb_Poss_Tbl[%]))*AG207,IF($AF$2=3,(V207*AG207)-AW207,V207*AG207)),0)","v":0},{"$f":"IF($AF207=3,IF($AF$2=2,(W207/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I207,Refurb_Poss_Tbl[%]))*AG207,W207*$AG207),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,4,0,{"$f":"VLOOKUP(AE208,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.87144222769857238},0,0,0,0,0,0,0,0,4.7962034952145134E-2,{"$f":"IF(OR(AF208=3,AF208=2,AF208=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D208,FlatMaint!$Y$2:$Y$10000,AE208)*AG208,0)","v":77.188245560008284},{"$f":"IF(OR(AF208=3,AF208=2,AF208=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D208,FlatRepair!$Y$2:$Y$10000,AE208)*AG208,0)","v":77.188245560008284},0,154.42445315496872,0,0,0,0,0,154.42445315496872,0,{"$f":"IF($AF208=3,IF($AF$2=2,(R208/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I208,Refurb_Poss_Tbl[%]))*AG208,IF($AF$2=3,(R208*AG208)-AV208,R208*AG208)),0)","v":0},{"$f":"IF(AF208=3,IF($AF$2=2,(S208/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I208,Refurb_Poss_Tbl[%]))*AG208,IF($AF$2=3,(S208*AG208)-AX208,S208*AG208)),0)","v":0},{"$f":"IF($AF208=3,IF($AF$2=2,(T208/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I208,Refurb_Poss_Tbl[%]))*AG208,T208*$AG208),0)","v":0},{"$f":"IF($AF208=3,IF($AF$2=2,(Q208/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I208,Refurb_Poss_Tbl[%]))*AG208,Q208*$AG208),0)","v":0},{"$f":"IF($AF208=3,IF($AF$2=2,(U208/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I208,Refurb_Poss_Tbl[%]))*AG208,U208*$AG208),0)","v":0},{"$f":"IF($AF208=3,IF($AF$2=2,(V208/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I208,Refurb_Poss_Tbl[%]))*AG208,IF($AF$2=3,(V208*AG208)-AW208,V208*AG208)),0)","v":0},{"$f":"IF($AF208=3,IF($AF$2=2,(W208/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I208,Refurb_Poss_Tbl[%]))*AG208,W208*$AG208),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,5,0,{"$f":"VLOOKUP(AE209,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.84197316685852419},0,0,0,0,0,0,0,0,4.6340130388546036E-2,{"$f":"IF(OR(AF209=3,AF209=2,AF209=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D209,FlatMaint!$Y$2:$Y$10000,AE209)*AG209,0)","v":74.578015033824443},{"$f":"IF(OR(AF209=3,AF209=2,AF209=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D209,FlatRepair!$Y$2:$Y$10000,AE209)*AG209,0)","v":0},0,74.624355164212986,0,0,0,0,0,74.624355164212986,0,{"$f":"IF($AF209=3,IF($AF$2=2,(R209/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I209,Refurb_Poss_Tbl[%]))*AG209,IF($AF$2=3,(R209*AG209)-AV209,R209*AG209)),0)","v":0},{"$f":"IF(AF209=3,IF($AF$2=2,(S209/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I209,Refurb_Poss_Tbl[%]))*AG209,IF($AF$2=3,(S209*AG209)-AX209,S209*AG209)),0)","v":0},{"$f":"IF($AF209=3,IF($AF$2=2,(T209/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I209,Refurb_Poss_Tbl[%]))*AG209,T209*$AG209),0)","v":0},{"$f":"IF($AF209=3,IF($AF$2=2,(Q209/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I209,Refurb_Poss_Tbl[%]))*AG209,Q209*$AG209),0)","v":0},{"$f":"IF($AF209=3,IF($AF$2=2,(U209/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I209,Refurb_Poss_Tbl[%]))*AG209,U209*$AG209),0)","v":0},{"$f":"IF($AF209=3,IF($AF$2=2,(V209/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I209,Refurb_Poss_Tbl[%]))*AG209,IF($AF$2=3,(V209*AG209)-AW209,V209*AG209)),0)","v":0},{"$f":"IF($AF209=3,IF($AF$2=2,(W209/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I209,Refurb_Poss_Tbl[%]))*AG209,W209*$AG209),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,6,0,{"$f":"VLOOKUP(AE210,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.81350064430775282},0,0,0,0,0,0,0,0,4.4773072839174907E-2,{"$f":"IF(OR(AF210=3,AF210=2,AF210=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D210,FlatMaint!$Y$2:$Y$10000,AE210)*AG210,0)","v":72.056053172777226},{"$f":"IF(OR(AF210=3,AF210=2,AF210=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D210,FlatRepair!$Y$2:$Y$10000,AE210)*AG210,0)","v":72.056053172777226},0,144.15687941839363,0,0,0,0,0,144.15687941839363,0,{"$f":"IF($AF210=3,IF($AF$2=2,(R210/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I210,Refurb_Poss_Tbl[%]))*AG210,IF($AF$2=3,(R210*AG210)-AV210,R210*AG210)),0)","v":0},{"$f":"IF(AF210=3,IF($AF$2=2,(S210/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I210,Refurb_Poss_Tbl[%]))*AG210,IF($AF$2=3,(S210*AG210)-AX210,S210*AG210)),0)","v":0},{"$f":"IF($AF210=3,IF($AF$2=2,(T210/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I210,Refurb_Poss_Tbl[%]))*AG210,T210*$AG210),0)","v":0},{"$f":"IF($AF210=3,IF($AF$2=2,(Q210/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I210,Refurb_Poss_Tbl[%]))*AG210,Q210*$AG210),0)","v":0},{"$f":"IF($AF210=3,IF($AF$2=2,(U210/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I210,Refurb_Poss_Tbl[%]))*AG210,U210*$AG210),0)","v":0},{"$f":"IF($AF210=3,IF($AF$2=2,(V210/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I210,Refurb_Poss_Tbl[%]))*AG210,IF($AF$2=3,(V210*AG210)-AW210,V210*AG210)),0)","v":0},{"$f":"IF($AF210=3,IF($AF$2=2,(W210/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I210,Refurb_Poss_Tbl[%]))*AG210,W210*$AG210),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,7,0,{"$f":"VLOOKUP(AE211,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.78599096068381913},0,0,0,0,0,0,0,0,4.3259007574082034E-2,{"$f":"IF(OR(AF211=3,AF211=2,AF211=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D211,FlatMaint!$Y$2:$Y$10000,AE211)*AG211,0)","v":69.619375046161579},{"$f":"IF(OR(AF211=3,AF211=2,AF211=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D211,FlatRepair!$Y$2:$Y$10000,AE211)*AG211,0)","v":0},0,69.662634053735658,0,0,0,0,0,69.662634053735658,0,{"$f":"IF($AF211=3,IF($AF$2=2,(R211/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I211,Refurb_Poss_Tbl[%]))*AG211,IF($AF$2=3,(R211*AG211)-AV211,R211*AG211)),0)","v":0},{"$f":"IF(AF211=3,IF($AF$2=2,(S211/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I211,Refurb_Poss_Tbl[%]))*AG211,IF($AF$2=3,(S211*AG211)-AX211,S211*AG211)),0)","v":0},{"$f":"IF($AF211=3,IF($AF$2=2,(T211/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I211,Refurb_Poss_Tbl[%]))*AG211,T211*$AG211),0)","v":0},{"$f":"IF($AF211=3,IF($AF$2=2,(Q211/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I211,Refurb_Poss_Tbl[%]))*AG211,Q211*$AG211),0)","v":0},{"$f":"IF($AF211=3,IF($AF$2=2,(U211/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I211,Refurb_Poss_Tbl[%]))*AG211,U211*$AG211),0)","v":0},{"$f":"IF($AF211=3,IF($AF$2=2,(V211/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I211,Refurb_Poss_Tbl[%]))*AG211,IF($AF$2=3,(V211*AG211)-AW211,V211*AG211)),0)","v":0},{"$f":"IF($AF211=3,IF($AF$2=2,(W211/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I211,Refurb_Poss_Tbl[%]))*AG211,W211*$AG211),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,8,0,{"$f":"VLOOKUP(AE212,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.75941155621625056},0,0,0,0,0,0,0,0,4.1796142583654154E-2,{"$f":"IF(OR(AF212=3,AF212=2,AF212=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D212,FlatMaint!$Y$2:$Y$10000,AE212)*AG212,0)","v":67.265096662958058},{"$f":"IF(OR(AF212=3,AF212=2,AF212=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D212,FlatRepair!$Y$2:$Y$10000,AE212)*AG212,0)","v":67.265096662958058},0,134.57198946849977,0,0,0,0,0,134.57198946849977,0,{"$f":"IF($AF212=3,IF($AF$2=2,(R212/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I212,Refurb_Poss_Tbl[%]))*AG212,IF($AF$2=3,(R212*AG212)-AV212,R212*AG212)),0)","v":0},{"$f":"IF(AF212=3,IF($AF$2=2,(S212/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I212,Refurb_Poss_Tbl[%]))*AG212,IF($AF$2=3,(S212*AG212)-AX212,S212*AG212)),0)","v":0},{"$f":"IF($AF212=3,IF($AF$2=2,(T212/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I212,Refurb_Poss_Tbl[%]))*AG212,T212*$AG212),0)","v":0},{"$f":"IF($AF212=3,IF($AF$2=2,(Q212/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I212,Refurb_Poss_Tbl[%]))*AG212,Q212*$AG212),0)","v":0},{"$f":"IF($AF212=3,IF($AF$2=2,(U212/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I212,Refurb_Poss_Tbl[%]))*AG212,U212*$AG212),0)","v":0},{"$f":"IF($AF212=3,IF($AF$2=2,(V212/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I212,Refurb_Poss_Tbl[%]))*AG212,IF($AF$2=3,(V212*AG212)-AW212,V212*AG212)),0)","v":0},{"$f":"IF($AF212=3,IF($AF$2=2,(W212/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I212,Refurb_Poss_Tbl[%]))*AG212,W212*$AG212),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,9,0,{"$f":"VLOOKUP(AE213,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.73373097218961414},0,0,0,0,0,0,0,0,4.038274645763687E-2,{"$f":"IF(OR(AF213=3,AF213=2,AF213=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D213,FlatMaint!$Y$2:$Y$10000,AE213)*AG213,0)","v":64.99043155841359},{"$f":"IF(OR(AF213=3,AF213=2,AF213=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D213,FlatRepair!$Y$2:$Y$10000,AE213)*AG213,0)","v":0},0,65.030814304871228,0,0,0,0,0,65.030814304871228,0,{"$f":"IF($AF213=3,IF($AF$2=2,(R213/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I213,Refurb_Poss_Tbl[%]))*AG213,IF($AF$2=3,(R213*AG213)-AV213,R213*AG213)),0)","v":0},{"$f":"IF(AF213=3,IF($AF$2=2,(S213/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I213,Refurb_Poss_Tbl[%]))*AG213,IF($AF$2=3,(S213*AG213)-AX213,S213*AG213)),0)","v":0},{"$f":"IF($AF213=3,IF($AF$2=2,(T213/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I213,Refurb_Poss_Tbl[%]))*AG213,T213*$AG213),0)","v":0},{"$f":"IF($AF213=3,IF($AF$2=2,(Q213/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I213,Refurb_Poss_Tbl[%]))*AG213,Q213*$AG213),0)","v":0},{"$f":"IF($AF213=3,IF($AF$2=2,(U213/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I213,Refurb_Poss_Tbl[%]))*AG213,U213*$AG213),0)","v":0},{"$f":"IF($AF213=3,IF($AF$2=2,(V213/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I213,Refurb_Poss_Tbl[%]))*AG213,IF($AF$2=3,(V213*AG213)-AW213,V213*AG213)),0)","v":0},{"$f":"IF($AF213=3,IF($AF$2=2,(W213/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I213,Refurb_Poss_Tbl[%]))*AG213,W213*$AG213),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,10,0,{"$f":"VLOOKUP(AE214,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.70891881370977217},0,0,0,0,0,0,0,0,3.9017146335881034E-2,{"$f":"IF(OR(AF214=3,AF214=2,AF214=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D214,FlatMaint!$Y$2:$Y$10000,AE214)*AG214,0)","v":62.792687496051784},{"$f":"IF(OR(AF214=3,AF214=2,AF214=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D214,FlatRepair!$Y$2:$Y$10000,AE214)*AG214,0)","v":62.792687496051784},0,125.62439213843945,0,0,0,0,0,125.62439213843945,0,{"$f":"IF($AF214=3,IF($AF$2=2,(R214/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I214,Refurb_Poss_Tbl[%]))*AG214,IF($AF$2=3,(R214*AG214)-AV214,R214*AG214)),0)","v":0},{"$f":"IF(AF214=3,IF($AF$2=2,(S214/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I214,Refurb_Poss_Tbl[%]))*AG214,IF($AF$2=3,(S214*AG214)-AX214,S214*AG214)),0)","v":0},{"$f":"IF($AF214=3,IF($AF$2=2,(T214/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I214,Refurb_Poss_Tbl[%]))*AG214,T214*$AG214),0)","v":0},{"$f":"IF($AF214=3,IF($AF$2=2,(Q214/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I214,Refurb_Poss_Tbl[%]))*AG214,Q214*$AG214),0)","v":0},{"$f":"IF($AF214=3,IF($AF$2=2,(U214/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I214,Refurb_Poss_Tbl[%]))*AG214,U214*$AG214),0)","v":0},{"$f":"IF($AF214=3,IF($AF$2=2,(V214/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I214,Refurb_Poss_Tbl[%]))*AG214,IF($AF$2=3,(V214*AG214)-AW214,V214*AG214)),0)","v":0},{"$f":"IF($AF214=3,IF($AF$2=2,(W214/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I214,Refurb_Poss_Tbl[%]))*AG214,W214*$AG214),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,11,0,{"$f":"VLOOKUP(AE215,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.68494571372924851},0,0,0,0,0,0,0,0,3.7697725928387472E-2,{"$f":"IF(OR(AF215=3,AF215=2,AF215=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D215,FlatMaint!$Y$2:$Y$10000,AE215)*AG215,0)","v":60.669263281209453},{"$f":"IF(OR(AF215=3,AF215=2,AF215=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D215,FlatRepair!$Y$2:$Y$10000,AE215)*AG215,0)","v":0},0,60.706961007137842,0,0,0,0,0,60.706961007137842,0,{"$f":"IF($AF215=3,IF($AF$2=2,(R215/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I215,Refurb_Poss_Tbl[%]))*AG215,IF($AF$2=3,(R215*AG215)-AV215,R215*AG215)),0)","v":0},{"$f":"IF(AF215=3,IF($AF$2=2,(S215/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I215,Refurb_Poss_Tbl[%]))*AG215,IF($AF$2=3,(S215*AG215)-AX215,S215*AG215)),0)","v":0},{"$f":"IF($AF215=3,IF($AF$2=2,(T215/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I215,Refurb_Poss_Tbl[%]))*AG215,T215*$AG215),0)","v":0},{"$f":"IF($AF215=3,IF($AF$2=2,(Q215/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I215,Refurb_Poss_Tbl[%]))*AG215,Q215*$AG215),0)","v":0},{"$f":"IF($AF215=3,IF($AF$2=2,(U215/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I215,Refurb_Poss_Tbl[%]))*AG215,U215*$AG215),0)","v":0},{"$f":"IF($AF215=3,IF($AF$2=2,(V215/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I215,Refurb_Poss_Tbl[%]))*AG215,IF($AF$2=3,(V215*AG215)-AW215,V215*AG215)),0)","v":0},{"$f":"IF($AF215=3,IF($AF$2=2,(W215/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I215,Refurb_Poss_Tbl[%]))*AG215,W215*$AG215),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,12,0,{"$f":"VLOOKUP(AE216,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.66178329828912896},0,0,0,0,0,0,0,0,3.6422923602306735E-2,{"$f":"IF(OR(AF216=3,AF216=2,AF216=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D216,FlatMaint!$Y$2:$Y$10000,AE216)*AG216,0)","v":58.617645682327975},{"$f":"IF(OR(AF216=3,AF216=2,AF216=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D216,FlatRepair!$Y$2:$Y$10000,AE216)*AG216,0)","v":58.617645682327975},0,117.27171428825827,0,0,0,0,0,117.27171428825827,0,{"$f":"IF($AF216=3,IF($AF$2=2,(R216/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I216,Refurb_Poss_Tbl[%]))*AG216,IF($AF$2=3,(R216*AG216)-AV216,R216*AG216)),0)","v":0},{"$f":"IF(AF216=3,IF($AF$2=2,(S216/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I216,Refurb_Poss_Tbl[%]))*AG216,IF($AF$2=3,(S216*AG216)-AX216,S216*AG216)),0)","v":0},{"$f":"IF($AF216=3,IF($AF$2=2,(T216/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I216,Refurb_Poss_Tbl[%]))*AG216,T216*$AG216),0)","v":0},{"$f":"IF($AF216=3,IF($AF$2=2,(Q216/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I216,Refurb_Poss_Tbl[%]))*AG216,Q216*$AG216),0)","v":0},{"$f":"IF($AF216=3,IF($AF$2=2,(U216/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I216,Refurb_Poss_Tbl[%]))*AG216,U216*$AG216),0)","v":0},{"$f":"IF($AF216=3,IF($AF$2=2,(V216/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I216,Refurb_Poss_Tbl[%]))*AG216,IF($AF$2=3,(V216*AG216)-AW216,V216*AG216)),0)","v":0},{"$f":"IF($AF216=3,IF($AF$2=2,(W216/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I216,Refurb_Poss_Tbl[%]))*AG216,W216*$AG216),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,13,0,{"$f":"VLOOKUP(AE217,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.63940415293635666},0,0,0,0,0,0,0,0,3.5191230533629707E-2,{"$f":"IF(OR(AF217=3,AF217=2,AF217=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D217,FlatMaint!$Y$2:$Y$10000,AE217)*AG217,0)","v":56.635406456355547},{"$f":"IF(OR(AF217=3,AF217=2,AF217=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D217,FlatRepair!$Y$2:$Y$10000,AE217)*AG217,0)","v":0},0,56.670597686889174,0,0,0,0,0,56.670597686889174,0,{"$f":"IF($AF217=3,IF($AF$2=2,(R217/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I217,Refurb_Poss_Tbl[%]))*AG217,IF($AF$2=3,(R217*AG217)-AV217,R217*AG217)),0)","v":0},{"$f":"IF(AF217=3,IF($AF$2=2,(S217/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I217,Refurb_Poss_Tbl[%]))*AG217,IF($AF$2=3,(S217*AG217)-AX217,S217*AG217)),0)","v":0},{"$f":"IF($AF217=3,IF($AF$2=2,(T217/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I217,Refurb_Poss_Tbl[%]))*AG217,T217*$AG217),0)","v":0},{"$f":"IF($AF217=3,IF($AF$2=2,(Q217/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I217,Refurb_Poss_Tbl[%]))*AG217,Q217*$AG217),0)","v":0},{"$f":"IF($AF217=3,IF($AF$2=2,(U217/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I217,Refurb_Poss_Tbl[%]))*AG217,U217*$AG217),0)","v":0},{"$f":"IF($AF217=3,IF($AF$2=2,(V217/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I217,Refurb_Poss_Tbl[%]))*AG217,IF($AF$2=3,(V217*AG217)-AW217,V217*AG217)),0)","v":0},{"$f":"IF($AF217=3,IF($AF$2=2,(W217/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I217,Refurb_Poss_Tbl[%]))*AG217,W217*$AG217),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,14,0,{"$f":"VLOOKUP(AE218,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.61778179027667302},0,0,0,0,0,0,0,0,3.4001188921381355E-2,{"$f":"IF(OR(AF218=3,AF218=2,AF218=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D218,FlatMaint!$Y$2:$Y$10000,AE218)*AG218,0)","v":54.720199474739651},{"$f":"IF(OR(AF218=3,AF218=2,AF218=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D218,FlatRepair!$Y$2:$Y$10000,AE218)*AG218,0)","v":54.720199474739651},0,109.47440013840068,0,0,0,0,0,109.47440013840068,0,{"$f":"IF($AF218=3,IF($AF$2=2,(R218/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I218,Refurb_Poss_Tbl[%]))*AG218,IF($AF$2=3,(R218*AG218)-AV218,R218*AG218)),0)","v":0},{"$f":"IF(AF218=3,IF($AF$2=2,(S218/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I218,Refurb_Poss_Tbl[%]))*AG218,IF($AF$2=3,(S218*AG218)-AX218,S218*AG218)),0)","v":0},{"$f":"IF($AF218=3,IF($AF$2=2,(T218/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I218,Refurb_Poss_Tbl[%]))*AG218,T218*$AG218),0)","v":0},{"$f":"IF($AF218=3,IF($AF$2=2,(Q218/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I218,Refurb_Poss_Tbl[%]))*AG218,Q218*$AG218),0)","v":0},{"$f":"IF($AF218=3,IF($AF$2=2,(U218/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I218,Refurb_Poss_Tbl[%]))*AG218,U218*$AG218),0)","v":0},{"$f":"IF($AF218=3,IF($AF$2=2,(V218/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I218,Refurb_Poss_Tbl[%]))*AG218,IF($AF$2=3,(V218*AG218)-AW218,V218*AG218)),0)","v":0},{"$f":"IF($AF218=3,IF($AF$2=2,(W218/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I218,Refurb_Poss_Tbl[%]))*AG218,W218*$AG218),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,15,0,{"$f":"VLOOKUP(AE219,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.59689061862480497},0,0,0,0,0,0,0,0,3.2851390262204211E-2,{"$f":"IF(OR(AF219=3,AF219=2,AF219=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D219,FlatMaint!$Y$2:$Y$10000,AE219)*AG219,0)","v":52.869757946608367},{"$f":"IF(OR(AF219=3,AF219=2,AF219=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D219,FlatRepair!$Y$2:$Y$10000,AE219)*AG219,0)","v":0},0,52.902609336870569,0,0,0,0,0,52.902609336870569,0,{"$f":"IF($AF219=3,IF($AF$2=2,(R219/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I219,Refurb_Poss_Tbl[%]))*AG219,IF($AF$2=3,(R219*AG219)-AV219,R219*AG219)),0)","v":0},{"$f":"IF(AF219=3,IF($AF$2=2,(S219/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I219,Refurb_Poss_Tbl[%]))*AG219,IF($AF$2=3,(S219*AG219)-AX219,S219*AG219)),0)","v":0},{"$f":"IF($AF219=3,IF($AF$2=2,(T219/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I219,Refurb_Poss_Tbl[%]))*AG219,T219*$AG219),0)","v":0},{"$f":"IF($AF219=3,IF($AF$2=2,(Q219/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I219,Refurb_Poss_Tbl[%]))*AG219,Q219*$AG219),0)","v":0},{"$f":"IF($AF219=3,IF($AF$2=2,(U219/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I219,Refurb_Poss_Tbl[%]))*AG219,U219*$AG219),0)","v":0},{"$f":"IF($AF219=3,IF($AF$2=2,(V219/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I219,Refurb_Poss_Tbl[%]))*AG219,IF($AF$2=3,(V219*AG219)-AW219,V219*AG219)),0)","v":0},{"$f":"IF($AF219=3,IF($AF$2=2,(W219/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I219,Refurb_Poss_Tbl[%]))*AG219,W219*$AG219),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,16,0,{"$f":"VLOOKUP(AE220,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.57670591171478747},0,0,0,0,0,0,0,0,3.1740473683289097E-2,{"$f":"IF(OR(AF220=3,AF220=2,AF220=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D220,FlatMaint!$Y$2:$Y$10000,AE220)*AG220,0)","v":51.081891735853503},{"$f":"IF(OR(AF220=3,AF220=2,AF220=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D220,FlatRepair!$Y$2:$Y$10000,AE220)*AG220,0)","v":51.081891735853503},0,102.19552394539029,0,0,0,0,0,102.19552394539029,0,{"$f":"IF($AF220=3,IF($AF$2=2,(R220/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I220,Refurb_Poss_Tbl[%]))*AG220,IF($AF$2=3,(R220*AG220)-AV220,R220*AG220)),0)","v":0},{"$f":"IF(AF220=3,IF($AF$2=2,(S220/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I220,Refurb_Poss_Tbl[%]))*AG220,IF($AF$2=3,(S220*AG220)-AX220,S220*AG220)),0)","v":0},{"$f":"IF($AF220=3,IF($AF$2=2,(T220/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I220,Refurb_Poss_Tbl[%]))*AG220,T220*$AG220),0)","v":0},{"$f":"IF($AF220=3,IF($AF$2=2,(Q220/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I220,Refurb_Poss_Tbl[%]))*AG220,Q220*$AG220),0)","v":0},{"$f":"IF($AF220=3,IF($AF$2=2,(U220/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I220,Refurb_Poss_Tbl[%]))*AG220,U220*$AG220),0)","v":0},{"$f":"IF($AF220=3,IF($AF$2=2,(V220/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I220,Refurb_Poss_Tbl[%]))*AG220,IF($AF$2=3,(V220*AG220)-AW220,V220*AG220)),0)","v":0},{"$f":"IF($AF220=3,IF($AF$2=2,(W220/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I220,Refurb_Poss_Tbl[%]))*AG220,W220*$AG220),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,17,0,{"$f":"VLOOKUP(AE221,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.55720377943457733},0,0,0,0,0,0,0,0,3.0667124331680291E-2,{"$f":"IF(OR(AF221=3,AF221=2,AF221=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D221,FlatMaint!$Y$2:$Y$10000,AE221)*AG221,0)","v":49.354484768940587},{"$f":"IF(OR(AF221=3,AF221=2,AF221=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D221,FlatRepair!$Y$2:$Y$10000,AE221)*AG221,0)","v":0},0,49.385151893272266,0,0,0,0,0,49.385151893272266,0,{"$f":"IF($AF221=3,IF($AF$2=2,(R221/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I221,Refurb_Poss_Tbl[%]))*AG221,IF($AF$2=3,(R221*AG221)-AV221,R221*AG221)),0)","v":0},{"$f":"IF(AF221=3,IF($AF$2=2,(S221/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I221,Refurb_Poss_Tbl[%]))*AG221,IF($AF$2=3,(S221*AG221)-AX221,S221*AG221)),0)","v":0},{"$f":"IF($AF221=3,IF($AF$2=2,(T221/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I221,Refurb_Poss_Tbl[%]))*AG221,T221*$AG221),0)","v":0},{"$f":"IF($AF221=3,IF($AF$2=2,(Q221/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I221,Refurb_Poss_Tbl[%]))*AG221,Q221*$AG221),0)","v":0},{"$f":"IF($AF221=3,IF($AF$2=2,(U221/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I221,Refurb_Poss_Tbl[%]))*AG221,U221*$AG221),0)","v":0},{"$f":"IF($AF221=3,IF($AF$2=2,(V221/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I221,Refurb_Poss_Tbl[%]))*AG221,IF($AF$2=3,(V221*AG221)-AW221,V221*AG221)),0)","v":0},{"$f":"IF($AF221=3,IF($AF$2=2,(W221/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I221,Refurb_Poss_Tbl[%]))*AG221,W221*$AG221),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,18,0,{"$f":"VLOOKUP(AE222,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.53836113955031628},0,0,0,0,0,0,0,0,2.9630071818048592E-2,{"$f":"IF(OR(AF222=3,AF222=2,AF222=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D222,FlatMaint!$Y$2:$Y$10000,AE222)*AG222,0)","v":47.685492530377381},{"$f":"IF(OR(AF222=3,AF222=2,AF222=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D222,FlatRepair!$Y$2:$Y$10000,AE222)*AG222,0)","v":47.685492530377381},0,95.40061513257281,0,0,0,0,0,95.40061513257281,0,{"$f":"IF($AF222=3,IF($AF$2=2,(R222/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I222,Refurb_Poss_Tbl[%]))*AG222,IF($AF$2=3,(R222*AG222)-AV222,R222*AG222)),0)","v":0},{"$f":"IF(AF222=3,IF($AF$2=2,(S222/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I222,Refurb_Poss_Tbl[%]))*AG222,IF($AF$2=3,(S222*AG222)-AX222,S222*AG222)),0)","v":0},{"$f":"IF($AF222=3,IF($AF$2=2,(T222/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I222,Refurb_Poss_Tbl[%]))*AG222,T222*$AG222),0)","v":0},{"$f":"IF($AF222=3,IF($AF$2=2,(Q222/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I222,Refurb_Poss_Tbl[%]))*AG222,Q222*$AG222),0)","v":0},{"$f":"IF($AF222=3,IF($AF$2=2,(U222/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I222,Refurb_Poss_Tbl[%]))*AG222,U222*$AG222),0)","v":0},{"$f":"IF($AF222=3,IF($AF$2=2,(V222/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I222,Refurb_Poss_Tbl[%]))*AG222,IF($AF$2=3,(V222*AG222)-AW222,V222*AG222)),0)","v":0},{"$f":"IF($AF222=3,IF($AF$2=2,(W222/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I222,Refurb_Poss_Tbl[%]))*AG222,W222*$AG222),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,19,0,{"$f":"VLOOKUP(AE223,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.52015569038677911},0,0,0,0,0,0,0,0,2.8628088713090433E-2,{"$f":"IF(OR(AF223=3,AF223=2,AF223=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D223,FlatMaint!$Y$2:$Y$10000,AE223)*AG223,0)","v":46.072939642876705},{"$f":"IF(OR(AF223=3,AF223=2,AF223=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D223,FlatRepair!$Y$2:$Y$10000,AE223)*AG223,0)","v":0},0,46.101567731589796,0,0,0,0,0,46.101567731589796,0,{"$f":"IF($AF223=3,IF($AF$2=2,(R223/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I223,Refurb_Poss_Tbl[%]))*AG223,IF($AF$2=3,(R223*AG223)-AV223,R223*AG223)),0)","v":0},{"$f":"IF(AF223=3,IF($AF$2=2,(S223/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I223,Refurb_Poss_Tbl[%]))*AG223,IF($AF$2=3,(S223*AG223)-AX223,S223*AG223)),0)","v":0},{"$f":"IF($AF223=3,IF($AF$2=2,(T223/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I223,Refurb_Poss_Tbl[%]))*AG223,T223*$AG223),0)","v":0},{"$f":"IF($AF223=3,IF($AF$2=2,(Q223/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I223,Refurb_Poss_Tbl[%]))*AG223,Q223*$AG223),0)","v":0},{"$f":"IF($AF223=3,IF($AF$2=2,(U223/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I223,Refurb_Poss_Tbl[%]))*AG223,U223*$AG223),0)","v":0},{"$f":"IF($AF223=3,IF($AF$2=2,(V223/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I223,Refurb_Poss_Tbl[%]))*AG223,IF($AF$2=3,(V223*AG223)-AW223,V223*AG223)),0)","v":0},{"$f":"IF($AF223=3,IF($AF$2=2,(W223/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I223,Refurb_Poss_Tbl[%]))*AG223,W223*$AG223),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,20,0,{"$f":"VLOOKUP(AE224,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.50256588443167061},0,0,0,0,0,0,0,0,2.7659989094773362E-2,{"$f":"IF(OR(AF224=3,AF224=2,AF224=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D224,FlatMaint!$Y$2:$Y$10000,AE224)*AG224,0)","v":44.514917529349468},{"$f":"IF(OR(AF224=3,AF224=2,AF224=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D224,FlatRepair!$Y$2:$Y$10000,AE224)*AG224,0)","v":44.514917529349468},0,89.057495047793708,0,0,0,0,0,89.057495047793708,0,{"$f":"IF($AF224=3,IF($AF$2=2,(R224/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I224,Refurb_Poss_Tbl[%]))*AG224,IF($AF$2=3,(R224*AG224)-AV224,R224*AG224)),0)","v":0},{"$f":"IF(AF224=3,IF($AF$2=2,(S224/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I224,Refurb_Poss_Tbl[%]))*AG224,IF($AF$2=3,(S224*AG224)-AX224,S224*AG224)),0)","v":0},{"$f":"IF($AF224=3,IF($AF$2=2,(T224/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I224,Refurb_Poss_Tbl[%]))*AG224,T224*$AG224),0)","v":0},{"$f":"IF($AF224=3,IF($AF$2=2,(Q224/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I224,Refurb_Poss_Tbl[%]))*AG224,Q224*$AG224),0)","v":0},{"$f":"IF($AF224=3,IF($AF$2=2,(U224/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I224,Refurb_Poss_Tbl[%]))*AG224,U224*$AG224),0)","v":0},{"$f":"IF($AF224=3,IF($AF$2=2,(V224/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I224,Refurb_Poss_Tbl[%]))*AG224,IF($AF$2=3,(V224*AG224)-AW224,V224*AG224)),0)","v":0},{"$f":"IF($AF224=3,IF($AF$2=2,(W224/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I224,Refurb_Poss_Tbl[%]))*AG224,W224*$AG224),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,21,0,{"$f":"VLOOKUP(AE225,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.48557090283253213},0,0,0,0,0,0,0,0,2.6724627144708572E-2,{"$f":"IF(OR(AF225=3,AF225=2,AF225=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D225,FlatMaint!$Y$2:$Y$10000,AE225)*AG225,0)","v":43.009582153960849},{"$f":"IF(OR(AF225=3,AF225=2,AF225=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D225,FlatRepair!$Y$2:$Y$10000,AE225)*AG225,0)","v":0},0,43.036306781105559,0,0,0,0,0,43.036306781105559,0,{"$f":"IF($AF225=3,IF($AF$2=2,(R225/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I225,Refurb_Poss_Tbl[%]))*AG225,IF($AF$2=3,(R225*AG225)-AV225,R225*AG225)),0)","v":0},{"$f":"IF(AF225=3,IF($AF$2=2,(S225/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I225,Refurb_Poss_Tbl[%]))*AG225,IF($AF$2=3,(S225*AG225)-AX225,S225*AG225)),0)","v":0},{"$f":"IF($AF225=3,IF($AF$2=2,(T225/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I225,Refurb_Poss_Tbl[%]))*AG225,T225*$AG225),0)","v":0},{"$f":"IF($AF225=3,IF($AF$2=2,(Q225/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I225,Refurb_Poss_Tbl[%]))*AG225,Q225*$AG225),0)","v":0},{"$f":"IF($AF225=3,IF($AF$2=2,(U225/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I225,Refurb_Poss_Tbl[%]))*AG225,U225*$AG225),0)","v":0},{"$f":"IF($AF225=3,IF($AF$2=2,(V225/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I225,Refurb_Poss_Tbl[%]))*AG225,IF($AF$2=3,(V225*AG225)-AW225,V225*AG225)),0)","v":0},{"$f":"IF($AF225=3,IF($AF$2=2,(W225/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I225,Refurb_Poss_Tbl[%]))*AG225,W225*$AG225),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,22,0,{"$f":"VLOOKUP(AE226,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.46915063075606966},0,0,0,0,0,0,0,0,2.5820895791988957E-2,{"$f":"IF(OR(AF226=3,AF226=2,AF226=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D226,FlatMaint!$Y$2:$Y$10000,AE226)*AG226,0)","v":41.5551518395757},{"$f":"IF(OR(AF226=3,AF226=2,AF226=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D226,FlatRepair!$Y$2:$Y$10000,AE226)*AG226,0)","v":41.5551518395757},0,83.136124574943381,0,0,0,0,0,83.136124574943381,0,{"$f":"IF($AF226=3,IF($AF$2=2,(R226/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I226,Refurb_Poss_Tbl[%]))*AG226,IF($AF$2=3,(R226*AG226)-AV226,R226*AG226)),0)","v":0},{"$f":"IF(AF226=3,IF($AF$2=2,(S226/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I226,Refurb_Poss_Tbl[%]))*AG226,IF($AF$2=3,(S226*AG226)-AX226,S226*AG226)),0)","v":0},{"$f":"IF($AF226=3,IF($AF$2=2,(T226/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I226,Refurb_Poss_Tbl[%]))*AG226,T226*$AG226),0)","v":0},{"$f":"IF($AF226=3,IF($AF$2=2,(Q226/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I226,Refurb_Poss_Tbl[%]))*AG226,Q226*$AG226),0)","v":0},{"$f":"IF($AF226=3,IF($AF$2=2,(U226/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I226,Refurb_Poss_Tbl[%]))*AG226,U226*$AG226),0)","v":0},{"$f":"IF($AF226=3,IF($AF$2=2,(V226/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I226,Refurb_Poss_Tbl[%]))*AG226,IF($AF$2=3,(V226*AG226)-AW226,V226*AG226)),0)","v":0},{"$f":"IF($AF226=3,IF($AF$2=2,(W226/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I226,Refurb_Poss_Tbl[%]))*AG226,W226*$AG226),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,23,0,{"$f":"VLOOKUP(AE227,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.45328563358074364},0,0,0,0,0,0,0,0,2.494772540288788E-2,{"$f":"IF(OR(AF227=3,AF227=2,AF227=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D227,FlatMaint!$Y$2:$Y$10000,AE227)*AG227,0)","v":40.149905159010338},{"$f":"IF(OR(AF227=3,AF227=2,AF227=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D227,FlatRepair!$Y$2:$Y$10000,AE227)*AG227,0)","v":0},0,40.174852884413227,0,0,0,0,0,40.174852884413227,0,{"$f":"IF($AF227=3,IF($AF$2=2,(R227/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I227,Refurb_Poss_Tbl[%]))*AG227,IF($AF$2=3,(R227*AG227)-AV227,R227*AG227)),0)","v":0},{"$f":"IF(AF227=3,IF($AF$2=2,(S227/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I227,Refurb_Poss_Tbl[%]))*AG227,IF($AF$2=3,(S227*AG227)-AX227,S227*AG227)),0)","v":0},{"$f":"IF($AF227=3,IF($AF$2=2,(T227/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I227,Refurb_Poss_Tbl[%]))*AG227,T227*$AG227),0)","v":0},{"$f":"IF($AF227=3,IF($AF$2=2,(Q227/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I227,Refurb_Poss_Tbl[%]))*AG227,Q227*$AG227),0)","v":0},{"$f":"IF($AF227=3,IF($AF$2=2,(U227/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I227,Refurb_Poss_Tbl[%]))*AG227,U227*$AG227),0)","v":0},{"$f":"IF($AF227=3,IF($AF$2=2,(V227/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I227,Refurb_Poss_Tbl[%]))*AG227,IF($AF$2=3,(V227*AG227)-AW227,V227*AG227)),0)","v":0},{"$f":"IF($AF227=3,IF($AF$2=2,(W227/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I227,Refurb_Poss_Tbl[%]))*AG227,W227*$AG227),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,24,0,{"$f":"VLOOKUP(AE228,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.43795713389443841},0,0,0,0,0,0,0,0,2.4104082514867523E-2,{"$f":"IF(OR(AF228=3,AF228=2,AF228=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D228,FlatMaint!$Y$2:$Y$10000,AE228)*AG228,0)","v":38.792178897594539},{"$f":"IF(OR(AF228=3,AF228=2,AF228=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D228,FlatRepair!$Y$2:$Y$10000,AE228)*AG228,0)","v":38.792178897594539},0,77.608461877703945,0,0,0,0,0,77.608461877703945,0,{"$f":"IF($AF228=3,IF($AF$2=2,(R228/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I228,Refurb_Poss_Tbl[%]))*AG228,IF($AF$2=3,(R228*AG228)-AV228,R228*AG228)),0)","v":0},{"$f":"IF(AF228=3,IF($AF$2=2,(S228/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I228,Refurb_Poss_Tbl[%]))*AG228,IF($AF$2=3,(S228*AG228)-AX228,S228*AG228)),0)","v":0},{"$f":"IF($AF228=3,IF($AF$2=2,(T228/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I228,Refurb_Poss_Tbl[%]))*AG228,T228*$AG228),0)","v":0},{"$f":"IF($AF228=3,IF($AF$2=2,(Q228/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I228,Refurb_Poss_Tbl[%]))*AG228,Q228*$AG228),0)","v":0},{"$f":"IF($AF228=3,IF($AF$2=2,(U228/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I228,Refurb_Poss_Tbl[%]))*AG228,U228*$AG228),0)","v":0},{"$f":"IF($AF228=3,IF($AF$2=2,(V228/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I228,Refurb_Poss_Tbl[%]))*AG228,IF($AF$2=3,(V228*AG228)-AW228,V228*AG228)),0)","v":0},{"$f":"IF($AF228=3,IF($AF$2=2,(W228/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I228,Refurb_Poss_Tbl[%]))*AG228,W228*$AG228),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,25,0,{"$f":"VLOOKUP(AE229,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.42314698926998884},0,0,0,0,0,0,0,0,2.3288968613398575E-2,{"$f":"IF(OR(AF229=3,AF229=2,AF229=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D229,FlatMaint!$Y$2:$Y$10000,AE229)*AG229,0)","v":37.480366084632408},{"$f":"IF(OR(AF229=3,AF229=2,AF229=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D229,FlatRepair!$Y$2:$Y$10000,AE229)*AG229,0)","v":0},0,37.503655053245808,0,0,0,0,0,37.503655053245808,0,{"$f":"IF($AF229=3,IF($AF$2=2,(R229/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I229,Refurb_Poss_Tbl[%]))*AG229,IF($AF$2=3,(R229*AG229)-AV229,R229*AG229)),0)","v":0},{"$f":"IF(AF229=3,IF($AF$2=2,(S229/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I229,Refurb_Poss_Tbl[%]))*AG229,IF($AF$2=3,(S229*AG229)-AX229,S229*AG229)),0)","v":0},{"$f":"IF($AF229=3,IF($AF$2=2,(T229/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I229,Refurb_Poss_Tbl[%]))*AG229,T229*$AG229),0)","v":0},{"$f":"IF($AF229=3,IF($AF$2=2,(Q229/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I229,Refurb_Poss_Tbl[%]))*AG229,Q229*$AG229),0)","v":0},{"$f":"IF($AF229=3,IF($AF$2=2,(U229/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I229,Refurb_Poss_Tbl[%]))*AG229,U229*$AG229),0)","v":0},{"$f":"IF($AF229=3,IF($AF$2=2,(V229/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I229,Refurb_Poss_Tbl[%]))*AG229,IF($AF$2=3,(V229*AG229)-AW229,V229*AG229)),0)","v":0},{"$f":"IF($AF229=3,IF($AF$2=2,(W229/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I229,Refurb_Poss_Tbl[%]))*AG229,W229*$AG229),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,26,0,{"$f":"VLOOKUP(AE230,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.40883767079225974},0,0,0,0,0,0,0,0,2.2501418950143553E-2,{"$f":"IF(OR(AF230=3,AF230=2,AF230=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D230,FlatMaint!$Y$2:$Y$10000,AE230)*AG230,0)","v":36.212914091432282},{"$f":"IF(OR(AF230=3,AF230=2,AF230=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D230,FlatRepair!$Y$2:$Y$10000,AE230)*AG230,0)","v":36.212914091432282},0,72.448329601814706,0,0,0,0,0,72.448329601814706,0,{"$f":"IF($AF230=3,IF($AF$2=2,(R230/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I230,Refurb_Poss_Tbl[%]))*AG230,IF($AF$2=3,(R230*AG230)-AV230,R230*AG230)),0)","v":0},{"$f":"IF(AF230=3,IF($AF$2=2,(S230/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I230,Refurb_Poss_Tbl[%]))*AG230,IF($AF$2=3,(S230*AG230)-AX230,S230*AG230)),0)","v":0},{"$f":"IF($AF230=3,IF($AF$2=2,(T230/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I230,Refurb_Poss_Tbl[%]))*AG230,T230*$AG230),0)","v":0},{"$f":"IF($AF230=3,IF($AF$2=2,(Q230/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I230,Refurb_Poss_Tbl[%]))*AG230,Q230*$AG230),0)","v":0},{"$f":"IF($AF230=3,IF($AF$2=2,(U230/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I230,Refurb_Poss_Tbl[%]))*AG230,U230*$AG230),0)","v":0},{"$f":"IF($AF230=3,IF($AF$2=2,(V230/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I230,Refurb_Poss_Tbl[%]))*AG230,IF($AF$2=3,(V230*AG230)-AW230,V230*AG230)),0)","v":0},{"$f":"IF($AF230=3,IF($AF$2=2,(W230/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I230,Refurb_Poss_Tbl[%]))*AG230,W230*$AG230),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,27,0,{"$f":"VLOOKUP(AE231,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39501224231136206},0,0,0,0,0,0,0,0,2.1740501401104881E-2,{"$f":"IF(OR(AF231=3,AF231=2,AF231=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D231,FlatMaint!$Y$2:$Y$10000,AE231)*AG231,0)","v":34.988322793654376},{"$f":"IF(OR(AF231=3,AF231=2,AF231=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D231,FlatRepair!$Y$2:$Y$10000,AE231)*AG231,0)","v":0},0,35.010063295055481,0,0,0,0,0,35.010063295055481,0,{"$f":"IF($AF231=3,IF($AF$2=2,(R231/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I231,Refurb_Poss_Tbl[%]))*AG231,IF($AF$2=3,(R231*AG231)-AV231,R231*AG231)),0)","v":0},{"$f":"IF(AF231=3,IF($AF$2=2,(S231/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I231,Refurb_Poss_Tbl[%]))*AG231,IF($AF$2=3,(S231*AG231)-AX231,S231*AG231)),0)","v":0},{"$f":"IF($AF231=3,IF($AF$2=2,(T231/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I231,Refurb_Poss_Tbl[%]))*AG231,T231*$AG231),0)","v":0},{"$f":"IF($AF231=3,IF($AF$2=2,(Q231/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I231,Refurb_Poss_Tbl[%]))*AG231,Q231*$AG231),0)","v":0},{"$f":"IF($AF231=3,IF($AF$2=2,(U231/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I231,Refurb_Poss_Tbl[%]))*AG231,U231*$AG231),0)","v":0},{"$f":"IF($AF231=3,IF($AF$2=2,(V231/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I231,Refurb_Poss_Tbl[%]))*AG231,IF($AF$2=3,(V231*AG231)-AW231,V231*AG231)),0)","v":0},{"$f":"IF($AF231=3,IF($AF$2=2,(W231/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I231,Refurb_Poss_Tbl[%]))*AG231,W231*$AG231),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,28,0,{"$f":"VLOOKUP(AE232,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38165434039745127},0,0,0,0,0,0,0,0,2.1005315363386359E-2,{"$f":"IF(OR(AF232=3,AF232=2,AF232=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D232,FlatMaint!$Y$2:$Y$10000,AE232)*AG232,0)","v":33.805142795801331},{"$f":"IF(OR(AF232=3,AF232=2,AF232=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D232,FlatRepair!$Y$2:$Y$10000,AE232)*AG232,0)","v":33.805142795801331},0,67.631290906966058,0,0,0,0,0,67.631290906966058,0,{"$f":"IF($AF232=3,IF($AF$2=2,(R232/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I232,Refurb_Poss_Tbl[%]))*AG232,IF($AF$2=3,(R232*AG232)-AV232,R232*AG232)),0)","v":0},{"$f":"IF(AF232=3,IF($AF$2=2,(S232/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I232,Refurb_Poss_Tbl[%]))*AG232,IF($AF$2=3,(S232*AG232)-AX232,S232*AG232)),0)","v":0},{"$f":"IF($AF232=3,IF($AF$2=2,(T232/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I232,Refurb_Poss_Tbl[%]))*AG232,T232*$AG232),0)","v":0},{"$f":"IF($AF232=3,IF($AF$2=2,(Q232/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I232,Refurb_Poss_Tbl[%]))*AG232,Q232*$AG232),0)","v":0},{"$f":"IF($AF232=3,IF($AF$2=2,(U232/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I232,Refurb_Poss_Tbl[%]))*AG232,U232*$AG232),0)","v":0},{"$f":"IF($AF232=3,IF($AF$2=2,(V232/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I232,Refurb_Poss_Tbl[%]))*AG232,IF($AF$2=3,(V232*AG232)-AW232,V232*AG232)),0)","v":0},{"$f":"IF($AF232=3,IF($AF$2=2,(W232/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I232,Refurb_Poss_Tbl[%]))*AG232,W232*$AG232),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,29,0,{"$f":"VLOOKUP(AE233,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36874815497338298},0,0,0,0,0,0,0,0,2.0294990689262188E-2,{"$f":"IF(OR(AF233=3,AF233=2,AF233=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D233,FlatMaint!$Y$2:$Y$10000,AE233)*AG233,0)","v":32.661973715750086},{"$f":"IF(OR(AF233=3,AF233=2,AF233=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D233,FlatRepair!$Y$2:$Y$10000,AE233)*AG233,0)","v":0},0,32.682268706439352,0,0,0,0,0,32.682268706439352,0,{"$f":"IF($AF233=3,IF($AF$2=2,(R233/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I233,Refurb_Poss_Tbl[%]))*AG233,IF($AF$2=3,(R233*AG233)-AV233,R233*AG233)),0)","v":0},{"$f":"IF(AF233=3,IF($AF$2=2,(S233/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I233,Refurb_Poss_Tbl[%]))*AG233,IF($AF$2=3,(S233*AG233)-AX233,S233*AG233)),0)","v":0},{"$f":"IF($AF233=3,IF($AF$2=2,(T233/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I233,Refurb_Poss_Tbl[%]))*AG233,T233*$AG233),0)","v":0},{"$f":"IF($AF233=3,IF($AF$2=2,(Q233/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I233,Refurb_Poss_Tbl[%]))*AG233,Q233*$AG233),0)","v":0},{"$f":"IF($AF233=3,IF($AF$2=2,(U233/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I233,Refurb_Poss_Tbl[%]))*AG233,U233*$AG233),0)","v":0},{"$f":"IF($AF233=3,IF($AF$2=2,(V233/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I233,Refurb_Poss_Tbl[%]))*AG233,IF($AF$2=3,(V233*AG233)-AW233,V233*AG233)),0)","v":0},{"$f":"IF($AF233=3,IF($AF$2=2,(W233/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I233,Refurb_Poss_Tbl[%]))*AG233,W233*$AG233),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,30,0,{"$f":"VLOOKUP(AE234,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35627841060230236},0,0,0,0,0,0,0,0,1.9608686656291965E-2,{"$f":"IF(OR(AF234=3,AF234=2,AF234=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D234,FlatMaint!$Y$2:$Y$10000,AE234)*AG234,0)","v":31.557462527294767},{"$f":"IF(OR(AF234=3,AF234=2,AF234=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D234,FlatRepair!$Y$2:$Y$10000,AE234)*AG234,0)","v":31.557462527294767},0,63.134533741245825,0,0,0,0,0,63.134533741245825,0,{"$f":"IF($AF234=3,IF($AF$2=2,(R234/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I234,Refurb_Poss_Tbl[%]))*AG234,IF($AF$2=3,(R234*AG234)-AV234,R234*AG234)),0)","v":0},{"$f":"IF(AF234=3,IF($AF$2=2,(S234/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I234,Refurb_Poss_Tbl[%]))*AG234,IF($AF$2=3,(S234*AG234)-AX234,S234*AG234)),0)","v":0},{"$f":"IF($AF234=3,IF($AF$2=2,(T234/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I234,Refurb_Poss_Tbl[%]))*AG234,T234*$AG234),0)","v":0},{"$f":"IF($AF234=3,IF($AF$2=2,(Q234/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I234,Refurb_Poss_Tbl[%]))*AG234,Q234*$AG234),0)","v":0},{"$f":"IF($AF234=3,IF($AF$2=2,(U234/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I234,Refurb_Poss_Tbl[%]))*AG234,U234*$AG234),0)","v":0},{"$f":"IF($AF234=3,IF($AF$2=2,(V234/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I234,Refurb_Poss_Tbl[%]))*AG234,IF($AF$2=3,(V234*AG234)-AW234,V234*AG234)),0)","v":0},{"$f":"IF($AF234=3,IF($AF$2=2,(W234/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I234,Refurb_Poss_Tbl[%]))*AG234,W234*$AG234),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,31,0,{"$f":"VLOOKUP(AE235,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39998714516107459},0,0,0,0,0,0,0,0,2.2014307807057439E-2,{"$f":"IF(OR(AF235=3,AF235=2,AF235=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D235,FlatMaint!$Y$2:$Y$10000,AE235)*AG235,0)","v":35.428976242150817},{"$f":"IF(OR(AF235=3,AF235=2,AF235=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D235,FlatRepair!$Y$2:$Y$10000,AE235)*AG235,0)","v":0},0,35.450990549957872,0,0,0,0,0,35.450990549957872,0,{"$f":"IF($AF235=3,IF($AF$2=2,(R235/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I235,Refurb_Poss_Tbl[%]))*AG235,IF($AF$2=3,(R235*AG235)-AV235,R235*AG235)),0)","v":0},{"$f":"IF(AF235=3,IF($AF$2=2,(S235/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I235,Refurb_Poss_Tbl[%]))*AG235,IF($AF$2=3,(S235*AG235)-AX235,S235*AG235)),0)","v":0},{"$f":"IF($AF235=3,IF($AF$2=2,(T235/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I235,Refurb_Poss_Tbl[%]))*AG235,T235*$AG235),0)","v":0},{"$f":"IF($AF235=3,IF($AF$2=2,(Q235/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I235,Refurb_Poss_Tbl[%]))*AG235,Q235*$AG235),0)","v":0},{"$f":"IF($AF235=3,IF($AF$2=2,(U235/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I235,Refurb_Poss_Tbl[%]))*AG235,U235*$AG235),0)","v":0},{"$f":"IF($AF235=3,IF($AF$2=2,(V235/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I235,Refurb_Poss_Tbl[%]))*AG235,IF($AF$2=3,(V235*AG235)-AW235,V235*AG235)),0)","v":0},{"$f":"IF($AF235=3,IF($AF$2=2,(W235/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I235,Refurb_Poss_Tbl[%]))*AG235,W235*$AG235),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,32,0,{"$f":"VLOOKUP(AE236,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38833703413696569},0,0,0,0,0,0,0,0,2.1373114375783927E-2,{"$f":"IF(OR(AF236=3,AF236=2,AF236=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D236,FlatMaint!$Y$2:$Y$10000,AE236)*AG236,0)","v":34.397064312767789},{"$f":"IF(OR(AF236=3,AF236=2,AF236=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D236,FlatRepair!$Y$2:$Y$10000,AE236)*AG236,0)","v":34.397064312767789},0,68.815501739911355,0,0,0,0,0,68.815501739911355,0,{"$f":"IF($AF236=3,IF($AF$2=2,(R236/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I236,Refurb_Poss_Tbl[%]))*AG236,IF($AF$2=3,(R236*AG236)-AV236,R236*AG236)),0)","v":0},{"$f":"IF(AF236=3,IF($AF$2=2,(S236/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I236,Refurb_Poss_Tbl[%]))*AG236,IF($AF$2=3,(S236*AG236)-AX236,S236*AG236)),0)","v":0},{"$f":"IF($AF236=3,IF($AF$2=2,(T236/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I236,Refurb_Poss_Tbl[%]))*AG236,T236*$AG236),0)","v":0},{"$f":"IF($AF236=3,IF($AF$2=2,(Q236/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I236,Refurb_Poss_Tbl[%]))*AG236,Q236*$AG236),0)","v":0},{"$f":"IF($AF236=3,IF($AF$2=2,(U236/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I236,Refurb_Poss_Tbl[%]))*AG236,U236*$AG236),0)","v":0},{"$f":"IF($AF236=3,IF($AF$2=2,(V236/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I236,Refurb_Poss_Tbl[%]))*AG236,IF($AF$2=3,(V236*AG236)-AW236,V236*AG236)),0)","v":0},{"$f":"IF($AF236=3,IF($AF$2=2,(W236/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I236,Refurb_Poss_Tbl[%]))*AG236,W236*$AG236),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,33,0,{"$f":"VLOOKUP(AE237,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.37702624673491814},0,0,0,0,0,0,0,0,2.0750596481343617E-2,{"$f":"IF(OR(AF237=3,AF237=2,AF237=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D237,FlatMaint!$Y$2:$Y$10000,AE237)*AG237,0)","v":33.395208070648337},{"$f":"IF(OR(AF237=3,AF237=2,AF237=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D237,FlatRepair!$Y$2:$Y$10000,AE237)*AG237,0)","v":0},0,33.415958667129679,0,0,0,0,0,33.415958667129679,0,{"$f":"IF($AF237=3,IF($AF$2=2,(R237/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I237,Refurb_Poss_Tbl[%]))*AG237,IF($AF$2=3,(R237*AG237)-AV237,R237*AG237)),0)","v":0},{"$f":"IF(AF237=3,IF($AF$2=2,(S237/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I237,Refurb_Poss_Tbl[%]))*AG237,IF($AF$2=3,(S237*AG237)-AX237,S237*AG237)),0)","v":0},{"$f":"IF($AF237=3,IF($AF$2=2,(T237/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I237,Refurb_Poss_Tbl[%]))*AG237,T237*$AG237),0)","v":0},{"$f":"IF($AF237=3,IF($AF$2=2,(Q237/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I237,Refurb_Poss_Tbl[%]))*AG237,Q237*$AG237),0)","v":0},{"$f":"IF($AF237=3,IF($AF$2=2,(U237/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I237,Refurb_Poss_Tbl[%]))*AG237,U237*$AG237),0)","v":0},{"$f":"IF($AF237=3,IF($AF$2=2,(V237/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I237,Refurb_Poss_Tbl[%]))*AG237,IF($AF$2=3,(V237*AG237)-AW237,V237*AG237)),0)","v":0},{"$f":"IF($AF237=3,IF($AF$2=2,(W237/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I237,Refurb_Poss_Tbl[%]))*AG237,W237*$AG237),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,34,0,{"$f":"VLOOKUP(AE238,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36604489974263904},0,0,0,0,0,0,0,0,2.0146210176061767E-2,{"$f":"IF(OR(AF238=3,AF238=2,AF238=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D238,FlatMaint!$Y$2:$Y$10000,AE238)*AG238,0)","v":32.422532107425575},{"$f":"IF(OR(AF238=3,AF238=2,AF238=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D238,FlatRepair!$Y$2:$Y$10000,AE238)*AG238,0)","v":32.422532107425575},0,64.865210425027215,0,0,0,0,0,64.865210425027215,0,{"$f":"IF($AF238=3,IF($AF$2=2,(R238/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I238,Refurb_Poss_Tbl[%]))*AG238,IF($AF$2=3,(R238*AG238)-AV238,R238*AG238)),0)","v":0},{"$f":"IF(AF238=3,IF($AF$2=2,(S238/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I238,Refurb_Poss_Tbl[%]))*AG238,IF($AF$2=3,(S238*AG238)-AX238,S238*AG238)),0)","v":0},{"$f":"IF($AF238=3,IF($AF$2=2,(T238/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I238,Refurb_Poss_Tbl[%]))*AG238,T238*$AG238),0)","v":0},{"$f":"IF($AF238=3,IF($AF$2=2,(Q238/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I238,Refurb_Poss_Tbl[%]))*AG238,Q238*$AG238),0)","v":0},{"$f":"IF($AF238=3,IF($AF$2=2,(U238/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I238,Refurb_Poss_Tbl[%]))*AG238,U238*$AG238),0)","v":0},{"$f":"IF($AF238=3,IF($AF$2=2,(V238/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I238,Refurb_Poss_Tbl[%]))*AG238,IF($AF$2=3,(V238*AG238)-AW238,V238*AG238)),0)","v":0},{"$f":"IF($AF238=3,IF($AF$2=2,(W238/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I238,Refurb_Poss_Tbl[%]))*AG238,W238*$AG238),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,35,0,{"$f":"VLOOKUP(AE239,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35538339780838735},0,0,0,0,0,0,0,0,1.9559427355399769E-2,{"$f":"IF(OR(AF239=3,AF239=2,AF239=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D239,FlatMaint!$Y$2:$Y$10000,AE239)*AG239,0)","v":31.478186512063662},{"$f":"IF(OR(AF239=3,AF239=2,AF239=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D239,FlatRepair!$Y$2:$Y$10000,AE239)*AG239,0)","v":0},0,31.497745939419062,0,0,0,0,0,31.497745939419062,0,{"$f":"IF($AF239=3,IF($AF$2=2,(R239/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I239,Refurb_Poss_Tbl[%]))*AG239,IF($AF$2=3,(R239*AG239)-AV239,R239*AG239)),0)","v":0},{"$f":"IF(AF239=3,IF($AF$2=2,(S239/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I239,Refurb_Poss_Tbl[%]))*AG239,IF($AF$2=3,(S239*AG239)-AX239,S239*AG239)),0)","v":0},{"$f":"IF($AF239=3,IF($AF$2=2,(T239/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I239,Refurb_Poss_Tbl[%]))*AG239,T239*$AG239),0)","v":0},{"$f":"IF($AF239=3,IF($AF$2=2,(Q239/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I239,Refurb_Poss_Tbl[%]))*AG239,Q239*$AG239),0)","v":0},{"$f":"IF($AF239=3,IF($AF$2=2,(U239/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I239,Refurb_Poss_Tbl[%]))*AG239,U239*$AG239),0)","v":0},{"$f":"IF($AF239=3,IF($AF$2=2,(V239/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I239,Refurb_Poss_Tbl[%]))*AG239,IF($AF$2=3,(V239*AG239)-AW239,V239*AG239)),0)","v":0},{"$f":"IF($AF239=3,IF($AF$2=2,(W239/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I239,Refurb_Poss_Tbl[%]))*AG239,W239*$AG239),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,36,0,{"$f":"VLOOKUP(AE240,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.34503242505668674},0,0,0,0,0,0,0,0,1.8989735296504631E-2,{"$f":"IF(OR(AF240=3,AF240=2,AF240=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D240,FlatMaint!$Y$2:$Y$10000,AE240)*AG240,0)","v":30.561346128217146},{"$f":"IF(OR(AF240=3,AF240=2,AF240=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D240,FlatRepair!$Y$2:$Y$10000,AE240)*AG240,0)","v":30.561346128217146},0,61.141681991730792,0,0,0,0,0,61.141681991730792,0,{"$f":"IF($AF240=3,IF($AF$2=2,(R240/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I240,Refurb_Poss_Tbl[%]))*AG240,IF($AF$2=3,(R240*AG240)-AV240,R240*AG240)),0)","v":0},{"$f":"IF(AF240=3,IF($AF$2=2,(S240/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I240,Refurb_Poss_Tbl[%]))*AG240,IF($AF$2=3,(S240*AG240)-AX240,S240*AG240)),0)","v":0},{"$f":"IF($AF240=3,IF($AF$2=2,(T240/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I240,Refurb_Poss_Tbl[%]))*AG240,T240*$AG240),0)","v":0},{"$f":"IF($AF240=3,IF($AF$2=2,(Q240/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I240,Refurb_Poss_Tbl[%]))*AG240,Q240*$AG240),0)","v":0},{"$f":"IF($AF240=3,IF($AF$2=2,(U240/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I240,Refurb_Poss_Tbl[%]))*AG240,U240*$AG240),0)","v":0},{"$f":"IF($AF240=3,IF($AF$2=2,(V240/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I240,Refurb_Poss_Tbl[%]))*AG240,IF($AF$2=3,(V240*AG240)-AW240,V240*AG240)),0)","v":0},{"$f":"IF($AF240=3,IF($AF$2=2,(W240/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I240,Refurb_Poss_Tbl[%]))*AG240,W240*$AG240),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,37,0,{"$f":"VLOOKUP(AE241,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.33498293694823961},0,0,0,0,0,0,0,0,1.8436636210198674E-2,{"$f":"IF(OR(AF241=3,AF241=2,AF241=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D241,FlatMaint!$Y$2:$Y$10000,AE241)*AG241,0)","v":29.671209833220534},{"$f":"IF(OR(AF241=3,AF241=2,AF241=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D241,FlatRepair!$Y$2:$Y$10000,AE241)*AG241,0)","v":0},0,29.689646469430734,0,0,0,0,0,29.689646469430734,0,{"$f":"IF($AF241=3,IF($AF$2=2,(R241/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I241,Refurb_Poss_Tbl[%]))*AG241,IF($AF$2=3,(R241*AG241)-AV241,R241*AG241)),0)","v":0},{"$f":"IF(AF241=3,IF($AF$2=2,(S241/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I241,Refurb_Poss_Tbl[%]))*AG241,IF($AF$2=3,(S241*AG241)-AX241,S241*AG241)),0)","v":0},{"$f":"IF($AF241=3,IF($AF$2=2,(T241/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I241,Refurb_Poss_Tbl[%]))*AG241,T241*$AG241),0)","v":0},{"$f":"IF($AF241=3,IF($AF$2=2,(Q241/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I241,Refurb_Poss_Tbl[%]))*AG241,Q241*$AG241),0)","v":0},{"$f":"IF($AF241=3,IF($AF$2=2,(U241/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I241,Refurb_Poss_Tbl[%]))*AG241,U241*$AG241),0)","v":0},{"$f":"IF($AF241=3,IF($AF$2=2,(V241/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I241,Refurb_Poss_Tbl[%]))*AG241,IF($AF$2=3,(V241*AG241)-AW241,V241*AG241)),0)","v":0},{"$f":"IF($AF241=3,IF($AF$2=2,(W241/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I241,Refurb_Poss_Tbl[%]))*AG241,W241*$AG241),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,38,0,{"$f":"VLOOKUP(AE242,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.3252261523769317},0,0,0,0,0,0,0,0,1.7899646806018132E-2,{"$f":"IF(OR(AF242=3,AF242=2,AF242=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D242,FlatMaint!$Y$2:$Y$10000,AE242)*AG242,0)","v":28.806999838078191},{"$f":"IF(OR(AF242=3,AF242=2,AF242=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D242,FlatRepair!$Y$2:$Y$10000,AE242)*AG242,0)","v":28.806999838078191},0,57.631899322962397,0,0,0,0,0,57.631899322962397,0,{"$f":"IF($AF242=3,IF($AF$2=2,(R242/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I242,Refurb_Poss_Tbl[%]))*AG242,IF($AF$2=3,(R242*AG242)-AV242,R242*AG242)),0)","v":0},{"$f":"IF(AF242=3,IF($AF$2=2,(S242/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I242,Refurb_Poss_Tbl[%]))*AG242,IF($AF$2=3,(S242*AG242)-AX242,S242*AG242)),0)","v":0},{"$f":"IF($AF242=3,IF($AF$2=2,(T242/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I242,Refurb_Poss_Tbl[%]))*AG242,T242*$AG242),0)","v":0},{"$f":"IF($AF242=3,IF($AF$2=2,(Q242/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I242,Refurb_Poss_Tbl[%]))*AG242,Q242*$AG242),0)","v":0},{"$f":"IF($AF242=3,IF($AF$2=2,(U242/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I242,Refurb_Poss_Tbl[%]))*AG242,U242*$AG242),0)","v":0},{"$f":"IF($AF242=3,IF($AF$2=2,(V242/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I242,Refurb_Poss_Tbl[%]))*AG242,IF($AF$2=3,(V242*AG242)-AW242,V242*AG242)),0)","v":0},{"$f":"IF($AF242=3,IF($AF$2=2,(W242/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I242,Refurb_Poss_Tbl[%]))*AG242,W242*$AG242),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,39,0,{"$f":"VLOOKUP(AE243,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.31575354599702099},0,0,0,0,0,0,0,0,1.7378297869920515E-2,{"$f":"IF(OR(AF243=3,AF243=2,AF243=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D243,FlatMaint!$Y$2:$Y$10000,AE243)*AG243,0)","v":27.967961007842899},{"$f":"IF(OR(AF243=3,AF243=2,AF243=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D243,FlatRepair!$Y$2:$Y$10000,AE243)*AG243,0)","v":0},0,27.98533930571282,0,0,0,0,0,27.98533930571282,0,{"$f":"IF($AF243=3,IF($AF$2=2,(R243/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I243,Refurb_Poss_Tbl[%]))*AG243,IF($AF$2=3,(R243*AG243)-AV243,R243*AG243)),0)","v":0},{"$f":"IF(AF243=3,IF($AF$2=2,(S243/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I243,Refurb_Poss_Tbl[%]))*AG243,IF($AF$2=3,(S243*AG243)-AX243,S243*AG243)),0)","v":0},{"$f":"IF($AF243=3,IF($AF$2=2,(T243/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I243,Refurb_Poss_Tbl[%]))*AG243,T243*$AG243),0)","v":0},{"$f":"IF($AF243=3,IF($AF$2=2,(Q243/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I243,Refurb_Poss_Tbl[%]))*AG243,Q243*$AG243),0)","v":0},{"$f":"IF($AF243=3,IF($AF$2=2,(U243/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I243,Refurb_Poss_Tbl[%]))*AG243,U243*$AG243),0)","v":0},{"$f":"IF($AF243=3,IF($AF$2=2,(V243/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I243,Refurb_Poss_Tbl[%]))*AG243,IF($AF$2=3,(V243*AG243)-AW243,V243*AG243)),0)","v":0},{"$f":"IF($AF243=3,IF($AF$2=2,(W243/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I243,Refurb_Poss_Tbl[%]))*AG243,W243*$AG243),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,40,2,{"$f":"VLOOKUP(AE244,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.30655684077380685},0,0,0,0,0,0,0,0,1.6872133854291763E-2,{"$f":"IF(OR(AF244=3,AF244=2,AF244=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D244,FlatMaint!$Y$2:$Y$10000,AE244)*AG244,0)","v":27.153360201789226},{"$f":"IF(OR(AF244=3,AF244=2,AF244=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D244,FlatRepair!$Y$2:$Y$10000,AE244)*AG244,0)","v":27.153360201789226},0,54.323592537432745,27.482404163406333,0,0,0,0,81.805996700839074,0,{"$f":"IF($AF244=3,IF($AF$2=2,(R244/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I244,Refurb_Poss_Tbl[%]))*AG244,IF($AF$2=3,(R244*AG244)-AV244,R244*AG244)),0)","v":0},{"$f":"IF(AF244=3,IF($AF$2=2,(S244/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I244,Refurb_Poss_Tbl[%]))*AG244,IF($AF$2=3,(S244*AG244)-AX244,S244*AG244)),0)","v":0},{"$f":"IF($AF244=3,IF($AF$2=2,(T244/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I244,Refurb_Poss_Tbl[%]))*AG244,T244*$AG244),0)","v":0},{"$f":"IF($AF244=3,IF($AF$2=2,(Q244/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I244,Refurb_Poss_Tbl[%]))*AG244,Q244*$AG244),0)","v":0},{"$f":"IF($AF244=3,IF($AF$2=2,(U244/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I244,Refurb_Poss_Tbl[%]))*AG244,U244*$AG244),0)","v":0},{"$f":"IF($AF244=3,IF($AF$2=2,(V244/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I244,Refurb_Poss_Tbl[%]))*AG244,IF($AF$2=3,(V244*AG244)-AW244,V244*AG244)),0)","v":0},{"$f":"IF($AF244=3,IF($AF$2=2,(W244/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I244,Refurb_Poss_Tbl[%]))*AG244,W244*$AG244),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,41,0,{"$f":"VLOOKUP(AE245,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.29762800075126877},0,0,0,0,0,0,0,0,1.6380712479894914E-2,{"$f":"IF(OR(AF245=3,AF245=2,AF245=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D245,FlatMaint!$Y$2:$Y$10000,AE245)*AG245,0)","v":26.362485632805075},{"$f":"IF(OR(AF245=3,AF245=2,AF245=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D245,FlatRepair!$Y$2:$Y$10000,AE245)*AG245,0)","v":0},0,26.378866345284969,0,0,0,0,0,26.378866345284969,0,{"$f":"IF($AF245=3,IF($AF$2=2,(R245/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I245,Refurb_Poss_Tbl[%]))*AG245,IF($AF$2=3,(R245*AG245)-AV245,R245*AG245)),0)","v":0},{"$f":"IF(AF245=3,IF($AF$2=2,(S245/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I245,Refurb_Poss_Tbl[%]))*AG245,IF($AF$2=3,(S245*AG245)-AX245,S245*AG245)),0)","v":0},{"$f":"IF($AF245=3,IF($AF$2=2,(T245/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I245,Refurb_Poss_Tbl[%]))*AG245,T245*$AG245),0)","v":0},{"$f":"IF($AF245=3,IF($AF$2=2,(Q245/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I245,Refurb_Poss_Tbl[%]))*AG245,Q245*$AG245),0)","v":0},{"$f":"IF($AF245=3,IF($AF$2=2,(U245/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I245,Refurb_Poss_Tbl[%]))*AG245,U245*$AG245),0)","v":0},{"$f":"IF($AF245=3,IF($AF$2=2,(V245/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I245,Refurb_Poss_Tbl[%]))*AG245,IF($AF$2=3,(V245*AG245)-AW245,V245*AG245)),0)","v":0},{"$f":"IF($AF245=3,IF($AF$2=2,(W245/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I245,Refurb_Poss_Tbl[%]))*AG245,W245*$AG245),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,42,0,{"$f":"VLOOKUP(AE246,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28895922403035801},0,0,0,0,0,0,0,0,1.5903604349412539E-2,{"$f":"IF(OR(AF246=3,AF246=2,AF246=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D246,FlatMaint!$Y$2:$Y$10000,AE246)*AG246,0)","v":25.594646245441819},{"$f":"IF(OR(AF246=3,AF246=2,AF246=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D246,FlatRepair!$Y$2:$Y$10000,AE246)*AG246,0)","v":25.594646245441819},0,51.205196095233049,0,0,0,0,0,51.205196095233049,0,{"$f":"IF($AF246=3,IF($AF$2=2,(R246/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I246,Refurb_Poss_Tbl[%]))*AG246,IF($AF$2=3,(R246*AG246)-AV246,R246*AG246)),0)","v":0},{"$f":"IF(AF246=3,IF($AF$2=2,(S246/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I246,Refurb_Poss_Tbl[%]))*AG246,IF($AF$2=3,(S246*AG246)-AX246,S246*AG246)),0)","v":0},{"$f":"IF($AF246=3,IF($AF$2=2,(T246/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I246,Refurb_Poss_Tbl[%]))*AG246,T246*$AG246),0)","v":0},{"$f":"IF($AF246=3,IF($AF$2=2,(Q246/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I246,Refurb_Poss_Tbl[%]))*AG246,Q246*$AG246),0)","v":0},{"$f":"IF($AF246=3,IF($AF$2=2,(U246/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I246,Refurb_Poss_Tbl[%]))*AG246,U246*$AG246),0)","v":0},{"$f":"IF($AF246=3,IF($AF$2=2,(V246/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I246,Refurb_Poss_Tbl[%]))*AG246,IF($AF$2=3,(V246*AG246)-AW246,V246*AG246)),0)","v":0},{"$f":"IF($AF246=3,IF($AF$2=2,(W246/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I246,Refurb_Poss_Tbl[%]))*AG246,W246*$AG246),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,43,0,{"$f":"VLOOKUP(AE247,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28054293595180391},0,0,0,0,0,0,0,0,1.5440392572245184E-2,{"$f":"IF(OR(AF247=3,AF247=2,AF247=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D247,FlatMaint!$Y$2:$Y$10000,AE247)*AG247,0)","v":24.849171112079436},{"$f":"IF(OR(AF247=3,AF247=2,AF247=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D247,FlatRepair!$Y$2:$Y$10000,AE247)*AG247,0)","v":0},0,24.86461150465168,0,0,0,0,0,24.86461150465168,0,{"$f":"IF($AF247=3,IF($AF$2=2,(R247/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I247,Refurb_Poss_Tbl[%]))*AG247,IF($AF$2=3,(R247*AG247)-AV247,R247*AG247)),0)","v":0},{"$f":"IF(AF247=3,IF($AF$2=2,(S247/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I247,Refurb_Poss_Tbl[%]))*AG247,IF($AF$2=3,(S247*AG247)-AX247,S247*AG247)),0)","v":0},{"$f":"IF($AF247=3,IF($AF$2=2,(T247/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I247,Refurb_Poss_Tbl[%]))*AG247,T247*$AG247),0)","v":0},{"$f":"IF($AF247=3,IF($AF$2=2,(Q247/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I247,Refurb_Poss_Tbl[%]))*AG247,Q247*$AG247),0)","v":0},{"$f":"IF($AF247=3,IF($AF$2=2,(U247/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I247,Refurb_Poss_Tbl[%]))*AG247,U247*$AG247),0)","v":0},{"$f":"IF($AF247=3,IF($AF$2=2,(V247/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I247,Refurb_Poss_Tbl[%]))*AG247,IF($AF$2=3,(V247*AG247)-AW247,V247*AG247)),0)","v":0},{"$f":"IF($AF247=3,IF($AF$2=2,(W247/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I247,Refurb_Poss_Tbl[%]))*AG247,W247*$AG247),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,44,0,{"$f":"VLOOKUP(AE248,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.27237178247747956},0,0,0,0,0,0,0,0,1.4990672400238044E-2,{"$f":"IF(OR(AF248=3,AF248=2,AF248=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D248,FlatMaint!$Y$2:$Y$10000,AE248)*AG248,0)","v":24.125408846679068},{"$f":"IF(OR(AF248=3,AF248=2,AF248=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D248,FlatRepair!$Y$2:$Y$10000,AE248)*AG248,0)","v":24.125408846679068},0,48.265808365758375,0,0,0,0,0,48.265808365758375,0,{"$f":"IF($AF248=3,IF($AF$2=2,(R248/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I248,Refurb_Poss_Tbl[%]))*AG248,IF($AF$2=3,(R248*AG248)-AV248,R248*AG248)),0)","v":0},{"$f":"IF(AF248=3,IF($AF$2=2,(S248/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I248,Refurb_Poss_Tbl[%]))*AG248,IF($AF$2=3,(S248*AG248)-AX248,S248*AG248)),0)","v":0},{"$f":"IF($AF248=3,IF($AF$2=2,(T248/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I248,Refurb_Poss_Tbl[%]))*AG248,T248*$AG248),0)","v":0},{"$f":"IF($AF248=3,IF($AF$2=2,(Q248/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I248,Refurb_Poss_Tbl[%]))*AG248,Q248*$AG248),0)","v":0},{"$f":"IF($AF248=3,IF($AF$2=2,(U248/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I248,Refurb_Poss_Tbl[%]))*AG248,U248*$AG248),0)","v":0},{"$f":"IF($AF248=3,IF($AF$2=2,(V248/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I248,Refurb_Poss_Tbl[%]))*AG248,IF($AF$2=3,(V248*AG248)-AW248,V248*AG248)),0)","v":0},{"$f":"IF($AF248=3,IF($AF$2=2,(W248/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I248,Refurb_Poss_Tbl[%]))*AG248,W248*$AG248),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,45,0,{"$f":"VLOOKUP(AE249,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.26443862376454325},0,0,0,0,0,0,0,0,1.4554050874017519E-2,{"$f":"IF(OR(AF249=3,AF249=2,AF249=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D249,FlatMaint!$Y$2:$Y$10000,AE249)*AG249,0)","v":23.422727035610745},{"$f":"IF(OR(AF249=3,AF249=2,AF249=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D249,FlatRepair!$Y$2:$Y$10000,AE249)*AG249,0)","v":0},0,23.437281086484763,0,0,0,0,0,23.437281086484763,0,{"$f":"IF($AF249=3,IF($AF$2=2,(R249/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I249,Refurb_Poss_Tbl[%]))*AG249,IF($AF$2=3,(R249*AG249)-AV249,R249*AG249)),0)","v":0},{"$f":"IF(AF249=3,IF($AF$2=2,(S249/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I249,Refurb_Poss_Tbl[%]))*AG249,IF($AF$2=3,(S249*AG249)-AX249,S249*AG249)),0)","v":0},{"$f":"IF($AF249=3,IF($AF$2=2,(T249/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I249,Refurb_Poss_Tbl[%]))*AG249,T249*$AG249),0)","v":0},{"$f":"IF($AF249=3,IF($AF$2=2,(Q249/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I249,Refurb_Poss_Tbl[%]))*AG249,Q249*$AG249),0)","v":0},{"$f":"IF($AF249=3,IF($AF$2=2,(U249/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I249,Refurb_Poss_Tbl[%]))*AG249,U249*$AG249),0)","v":0},{"$f":"IF($AF249=3,IF($AF$2=2,(V249/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I249,Refurb_Poss_Tbl[%]))*AG249,IF($AF$2=3,(V249*AG249)-AW249,V249*AG249)),0)","v":0},{"$f":"IF($AF249=3,IF($AF$2=2,(W249/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I249,Refurb_Poss_Tbl[%]))*AG249,W249*$AG249),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,46,0,{"$f":"VLOOKUP(AE250,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.25673652792674101},0,0,0,0,0,0,0,0,1.4130146479628658E-2,{"$f":"IF(OR(AF250=3,AF250=2,AF250=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D250,FlatMaint!$Y$2:$Y$10000,AE250)*AG250,0)","v":22.740511685058973},{"$f":"IF(OR(AF250=3,AF250=2,AF250=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D250,FlatRepair!$Y$2:$Y$10000,AE250)*AG250,0)","v":22.740511685058973},0,45.495153516597576,0,0,0,0,0,45.495153516597576,0,{"$f":"IF($AF250=3,IF($AF$2=2,(R250/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I250,Refurb_Poss_Tbl[%]))*AG250,IF($AF$2=3,(R250*AG250)-AV250,R250*AG250)),0)","v":0},{"$f":"IF(AF250=3,IF($AF$2=2,(S250/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I250,Refurb_Poss_Tbl[%]))*AG250,IF($AF$2=3,(S250*AG250)-AX250,S250*AG250)),0)","v":0},{"$f":"IF($AF250=3,IF($AF$2=2,(T250/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I250,Refurb_Poss_Tbl[%]))*AG250,T250*$AG250),0)","v":0},{"$f":"IF($AF250=3,IF($AF$2=2,(Q250/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I250,Refurb_Poss_Tbl[%]))*AG250,Q250*$AG250),0)","v":0},{"$f":"IF($AF250=3,IF($AF$2=2,(U250/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I250,Refurb_Poss_Tbl[%]))*AG250,U250*$AG250),0)","v":0},{"$f":"IF($AF250=3,IF($AF$2=2,(V250/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I250,Refurb_Poss_Tbl[%]))*AG250,IF($AF$2=3,(V250*AG250)-AW250,V250*AG250)),0)","v":0},{"$f":"IF($AF250=3,IF($AF$2=2,(W250/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I250,Refurb_Poss_Tbl[%]))*AG250,W250*$AG250),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,47,0,{"$f":"VLOOKUP(AE251,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24925876497741845},0,0,0,0,0,0,0,0,1.3718588815173453E-2,{"$f":"IF(OR(AF251=3,AF251=2,AF251=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D251,FlatMaint!$Y$2:$Y$10000,AE251)*AG251,0)","v":22.078166684523275},{"$f":"IF(OR(AF251=3,AF251=2,AF251=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D251,FlatRepair!$Y$2:$Y$10000,AE251)*AG251,0)","v":0},0,22.091885273338448,0,0,0,0,0,22.091885273338448,0,{"$f":"IF($AF251=3,IF($AF$2=2,(R251/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I251,Refurb_Poss_Tbl[%]))*AG251,IF($AF$2=3,(R251*AG251)-AV251,R251*AG251)),0)","v":0},{"$f":"IF(AF251=3,IF($AF$2=2,(S251/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I251,Refurb_Poss_Tbl[%]))*AG251,IF($AF$2=3,(S251*AG251)-AX251,S251*AG251)),0)","v":0},{"$f":"IF($AF251=3,IF($AF$2=2,(T251/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I251,Refurb_Poss_Tbl[%]))*AG251,T251*$AG251),0)","v":0},{"$f":"IF($AF251=3,IF($AF$2=2,(Q251/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I251,Refurb_Poss_Tbl[%]))*AG251,Q251*$AG251),0)","v":0},{"$f":"IF($AF251=3,IF($AF$2=2,(U251/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I251,Refurb_Poss_Tbl[%]))*AG251,U251*$AG251),0)","v":0},{"$f":"IF($AF251=3,IF($AF$2=2,(V251/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I251,Refurb_Poss_Tbl[%]))*AG251,IF($AF$2=3,(V251*AG251)-AW251,V251*AG251)),0)","v":0},{"$f":"IF($AF251=3,IF($AF$2=2,(W251/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I251,Refurb_Poss_Tbl[%]))*AG251,W251*$AG251),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,48,0,{"$f":"VLOOKUP(AE252,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24199880094894996},0,0,0,0,0,0,0,0,1.3319018267158693E-2,{"$f":"IF(OR(AF252=3,AF252=2,AF252=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D252,FlatMaint!$Y$2:$Y$10000,AE252)*AG252,0)","v":21.435113285944929},{"$f":"IF(OR(AF252=3,AF252=2,AF252=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D252,FlatRepair!$Y$2:$Y$10000,AE252)*AG252,0)","v":21.435113285944929},0,42.883545590157013,0,0,0,0,0,42.883545590157013,0,{"$f":"IF($AF252=3,IF($AF$2=2,(R252/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I252,Refurb_Poss_Tbl[%]))*AG252,IF($AF$2=3,(R252*AG252)-AV252,R252*AG252)),0)","v":0},{"$f":"IF(AF252=3,IF($AF$2=2,(S252/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I252,Refurb_Poss_Tbl[%]))*AG252,IF($AF$2=3,(S252*AG252)-AX252,S252*AG252)),0)","v":0},{"$f":"IF($AF252=3,IF($AF$2=2,(T252/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I252,Refurb_Poss_Tbl[%]))*AG252,T252*$AG252),0)","v":0},{"$f":"IF($AF252=3,IF($AF$2=2,(Q252/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I252,Refurb_Poss_Tbl[%]))*AG252,Q252*$AG252),0)","v":0},{"$f":"IF($AF252=3,IF($AF$2=2,(U252/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I252,Refurb_Poss_Tbl[%]))*AG252,U252*$AG252),0)","v":0},{"$f":"IF($AF252=3,IF($AF$2=2,(V252/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I252,Refurb_Poss_Tbl[%]))*AG252,IF($AF$2=3,(V252*AG252)-AW252,V252*AG252)),0)","v":0},{"$f":"IF($AF252=3,IF($AF$2=2,(W252/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I252,Refurb_Poss_Tbl[%]))*AG252,W252*$AG252),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,49,0,{"$f":"VLOOKUP(AE253,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.2349502921834466},0,0,0,0,0,0,0,0,1.2931085696270578E-2,{"$f":"IF(OR(AF253=3,AF253=2,AF253=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D253,FlatMaint!$Y$2:$Y$10000,AE253)*AG253,0)","v":20.810789598004789},{"$f":"IF(OR(AF253=3,AF253=2,AF253=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D253,FlatRepair!$Y$2:$Y$10000,AE253)*AG253,0)","v":0},0,20.823720683701058,0,0,0,0,0,20.823720683701058,0,{"$f":"IF($AF253=3,IF($AF$2=2,(R253/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I253,Refurb_Poss_Tbl[%]))*AG253,IF($AF$2=3,(R253*AG253)-AV253,R253*AG253)),0)","v":0},{"$f":"IF(AF253=3,IF($AF$2=2,(S253/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I253,Refurb_Poss_Tbl[%]))*AG253,IF($AF$2=3,(S253*AG253)-AX253,S253*AG253)),0)","v":0},{"$f":"IF($AF253=3,IF($AF$2=2,(T253/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I253,Refurb_Poss_Tbl[%]))*AG253,T253*$AG253),0)","v":0},{"$f":"IF($AF253=3,IF($AF$2=2,(Q253/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I253,Refurb_Poss_Tbl[%]))*AG253,Q253*$AG253),0)","v":0},{"$f":"IF($AF253=3,IF($AF$2=2,(U253/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I253,Refurb_Poss_Tbl[%]))*AG253,U253*$AG253),0)","v":0},{"$f":"IF($AF253=3,IF($AF$2=2,(V253/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I253,Refurb_Poss_Tbl[%]))*AG253,IF($AF$2=3,(V253*AG253)-AW253,V253*AG253)),0)","v":0},{"$f":"IF($AF253=3,IF($AF$2=2,(W253/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I253,Refurb_Poss_Tbl[%]))*AG253,W253*$AG253),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,50,0,{"$f":"VLOOKUP(AE254,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22810707978975397},0,0,0,0,0,0,0,0,1.2554452132301532E-2,{"$f":"IF(OR(AF254=3,AF254=2,AF254=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D254,FlatMaint!$Y$2:$Y$10000,AE254)*AG254,0)","v":20.204650095150278},{"$f":"IF(OR(AF254=3,AF254=2,AF254=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D254,FlatRepair!$Y$2:$Y$10000,AE254)*AG254,0)","v":20.204650095150278},0,40.421854642432862,0,0,0,0,0,40.421854642432862,0,{"$f":"IF($AF254=3,IF($AF$2=2,(R254/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I254,Refurb_Poss_Tbl[%]))*AG254,IF($AF$2=3,(R254*AG254)-AV254,R254*AG254)),0)","v":0},{"$f":"IF(AF254=3,IF($AF$2=2,(S254/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I254,Refurb_Poss_Tbl[%]))*AG254,IF($AF$2=3,(S254*AG254)-AX254,S254*AG254)),0)","v":0},{"$f":"IF($AF254=3,IF($AF$2=2,(T254/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I254,Refurb_Poss_Tbl[%]))*AG254,T254*$AG254),0)","v":0},{"$f":"IF($AF254=3,IF($AF$2=2,(Q254/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I254,Refurb_Poss_Tbl[%]))*AG254,Q254*$AG254),0)","v":0},{"$f":"IF($AF254=3,IF($AF$2=2,(U254/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I254,Refurb_Poss_Tbl[%]))*AG254,U254*$AG254),0)","v":0},{"$f":"IF($AF254=3,IF($AF$2=2,(V254/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I254,Refurb_Poss_Tbl[%]))*AG254,IF($AF$2=3,(V254*AG254)-AW254,V254*AG254)),0)","v":0},{"$f":"IF($AF254=3,IF($AF$2=2,(W254/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I254,Refurb_Poss_Tbl[%]))*AG254,W254*$AG254),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,51,0,{"$f":"VLOOKUP(AE255,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22146318426189707},0,0,0,0,0,0,0,0,1.2188788477962653E-2,{"$f":"IF(OR(AF255=3,AF255=2,AF255=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D255,FlatMaint!$Y$2:$Y$10000,AE255)*AG255,0)","v":19.6161651409226},{"$f":"IF(OR(AF255=3,AF255=2,AF255=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D255,FlatRepair!$Y$2:$Y$10000,AE255)*AG255,0)","v":0},0,19.628353929400564,0,0,0,0,0,19.628353929400564,0,{"$f":"IF($AF255=3,IF($AF$2=2,(R255/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I255,Refurb_Poss_Tbl[%]))*AG255,IF($AF$2=3,(R255*AG255)-AV255,R255*AG255)),0)","v":0},{"$f":"IF(AF255=3,IF($AF$2=2,(S255/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I255,Refurb_Poss_Tbl[%]))*AG255,IF($AF$2=3,(S255*AG255)-AX255,S255*AG255)),0)","v":0},{"$f":"IF($AF255=3,IF($AF$2=2,(T255/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I255,Refurb_Poss_Tbl[%]))*AG255,T255*$AG255),0)","v":0},{"$f":"IF($AF255=3,IF($AF$2=2,(Q255/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I255,Refurb_Poss_Tbl[%]))*AG255,Q255*$AG255),0)","v":0},{"$f":"IF($AF255=3,IF($AF$2=2,(U255/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I255,Refurb_Poss_Tbl[%]))*AG255,U255*$AG255),0)","v":0},{"$f":"IF($AF255=3,IF($AF$2=2,(V255/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I255,Refurb_Poss_Tbl[%]))*AG255,IF($AF$2=3,(V255*AG255)-AW255,V255*AG255)),0)","v":0},{"$f":"IF($AF255=3,IF($AF$2=2,(W255/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I255,Refurb_Poss_Tbl[%]))*AG255,W255*$AG255),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,52,0,{"$f":"VLOOKUP(AE256,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.215012800254269},0,0,0,0,0,0,0,0,1.1833775221322965E-2,{"$f":"IF(OR(AF256=3,AF256=2,AF256=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D256,FlatMaint!$Y$2:$Y$10000,AE256)*AG256,0)","v":19.044820525167573},{"$f":"IF(OR(AF256=3,AF256=2,AF256=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D256,FlatRepair!$Y$2:$Y$10000,AE256)*AG256,0)","v":19.044820525167573},0,38.101474825556465,0,0,0,0,0,38.101474825556465,0,{"$f":"IF($AF256=3,IF($AF$2=2,(R256/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I256,Refurb_Poss_Tbl[%]))*AG256,IF($AF$2=3,(R256*AG256)-AV256,R256*AG256)),0)","v":0},{"$f":"IF(AF256=3,IF($AF$2=2,(S256/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I256,Refurb_Poss_Tbl[%]))*AG256,IF($AF$2=3,(S256*AG256)-AX256,S256*AG256)),0)","v":0},{"$f":"IF($AF256=3,IF($AF$2=2,(T256/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I256,Refurb_Poss_Tbl[%]))*AG256,T256*$AG256),0)","v":0},{"$f":"IF($AF256=3,IF($AF$2=2,(Q256/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I256,Refurb_Poss_Tbl[%]))*AG256,Q256*$AG256),0)","v":0},{"$f":"IF($AF256=3,IF($AF$2=2,(U256/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I256,Refurb_Poss_Tbl[%]))*AG256,U256*$AG256),0)","v":0},{"$f":"IF($AF256=3,IF($AF$2=2,(V256/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I256,Refurb_Poss_Tbl[%]))*AG256,IF($AF$2=3,(V256*AG256)-AW256,V256*AG256)),0)","v":0},{"$f":"IF($AF256=3,IF($AF$2=2,(W256/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I256,Refurb_Poss_Tbl[%]))*AG256,W256*$AG256),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,53,0,{"$f":"VLOOKUP(AE257,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20875029150899907},0,0,0,0,0,0,0,0,1.1489102156624239E-2,{"$f":"IF(OR(AF257=3,AF257=2,AF257=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D257,FlatMaint!$Y$2:$Y$10000,AE257)*AG257,0)","v":18.490117014725804},{"$f":"IF(OR(AF257=3,AF257=2,AF257=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D257,FlatRepair!$Y$2:$Y$10000,AE257)*AG257,0)","v":0},0,18.501606116882428,0,0,0,0,0,18.501606116882428,0,{"$f":"IF($AF257=3,IF($AF$2=2,(R257/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I257,Refurb_Poss_Tbl[%]))*AG257,IF($AF$2=3,(R257*AG257)-AV257,R257*AG257)),0)","v":0},{"$f":"IF(AF257=3,IF($AF$2=2,(S257/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I257,Refurb_Poss_Tbl[%]))*AG257,IF($AF$2=3,(S257*AG257)-AX257,S257*AG257)),0)","v":0},{"$f":"IF($AF257=3,IF($AF$2=2,(T257/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I257,Refurb_Poss_Tbl[%]))*AG257,T257*$AG257),0)","v":0},{"$f":"IF($AF257=3,IF($AF$2=2,(Q257/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I257,Refurb_Poss_Tbl[%]))*AG257,Q257*$AG257),0)","v":0},{"$f":"IF($AF257=3,IF($AF$2=2,(U257/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I257,Refurb_Poss_Tbl[%]))*AG257,U257*$AG257),0)","v":0},{"$f":"IF($AF257=3,IF($AF$2=2,(V257/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I257,Refurb_Poss_Tbl[%]))*AG257,IF($AF$2=3,(V257*AG257)-AW257,V257*AG257)),0)","v":0},{"$f":"IF($AF257=3,IF($AF$2=2,(W257/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I257,Refurb_Poss_Tbl[%]))*AG257,W257*$AG257),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,54,0,{"$f":"VLOOKUP(AE258,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20267018593106703},0,0,0,0,0,0,0,0,1.1154468113227416E-2,{"$f":"IF(OR(AF258=3,AF258=2,AF258=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D258,FlatMaint!$Y$2:$Y$10000,AE258)*AG258,0)","v":17.951569917209515},{"$f":"IF(OR(AF258=3,AF258=2,AF258=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D258,FlatRepair!$Y$2:$Y$10000,AE258)*AG258,0)","v":17.951569917209515},0,35.914294302532255,0,0,0,0,0,35.914294302532255,0,{"$f":"IF($AF258=3,IF($AF$2=2,(R258/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I258,Refurb_Poss_Tbl[%]))*AG258,IF($AF$2=3,(R258*AG258)-AV258,R258*AG258)),0)","v":0},{"$f":"IF(AF258=3,IF($AF$2=2,(S258/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I258,Refurb_Poss_Tbl[%]))*AG258,IF($AF$2=3,(S258*AG258)-AX258,S258*AG258)),0)","v":0},{"$f":"IF($AF258=3,IF($AF$2=2,(T258/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I258,Refurb_Poss_Tbl[%]))*AG258,T258*$AG258),0)","v":0},{"$f":"IF($AF258=3,IF($AF$2=2,(Q258/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I258,Refurb_Poss_Tbl[%]))*AG258,Q258*$AG258),0)","v":0},{"$f":"IF($AF258=3,IF($AF$2=2,(U258/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I258,Refurb_Poss_Tbl[%]))*AG258,U258*$AG258),0)","v":0},{"$f":"IF($AF258=3,IF($AF$2=2,(V258/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I258,Refurb_Poss_Tbl[%]))*AG258,IF($AF$2=3,(V258*AG258)-AW258,V258*AG258)),0)","v":0},{"$f":"IF($AF258=3,IF($AF$2=2,(W258/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I258,Refurb_Poss_Tbl[%]))*AG258,W258*$AG258),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,55,0,{"$f":"VLOOKUP(AE259,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19676717080686118},{"$f":"IF(AE259=0,Q259*AG259,0)","v":0},{"$f":"IF(AE259=0,R259*AG259,0)","v":0},{"$f":"IF(AE259=0,S259*AG259,0)","v":0},{"$f":"IF(AE259=0,T259*AG259,0)","v":0},{"$f":"IF(AE259=0,U259*AG259,0)","v":0},{"$f":"IF(AE259=0,V259*AG259,0)","v":0},{"$f":"IF(AE259=0,W259*AG259,0)","v":0},{"$f":"IF(AE259=0,AH259+AI259+AJ259+AK259+AL259+AM259+AN259,0)","v":0},{"$f":"IF(OR(AF259=3,AF259=2,AF259=0),Y259*AG259,0)","v":1.0829580692453801E-2},{"$f":"IF(OR(AF259=3,AF259=2,AF259=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D259,FlatMaint!$Y$2:$Y$10000,AE259)*AG259,0)","v":17.428708657484965},{"$f":"IF(OR(AF259=3,AF259=2,AF259=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D259,FlatRepair!$Y$2:$Y$10000,AE259)*AG259,0)","v":0},{"$f":"IF(OR(AF259=3,AF259=2,AF259=0),Z259*AG259,0)","v":0},{"$f":"AP259+AQ259+AR259+AS259","v":17.43953823817742},{"$f":"IF(AF259=2,AA259*AG259,0)","v":0},{"$f":"IF(AF259=3,AB259*AG259,0)","v":0},{"$f":"IF(AF259=3,AC259*AG259,0)","v":0},{"$f":"IF(AF259=3,AD259*AG259,0)","v":0},{"$f":"IF($AF$2=3,BB259+BC259+BD259+BE259+BF259+BG259+BH259,BB259+BC259+BD259+BE259+BF259+BG259+BH259)","v":0},{"$f":"AO259+AT259+AU259+AV259+AW259+AX259+AY259+BA259","v":17.43953823817742},{"$f":"IFERROR(IF(AE259=100,IF(O259=3,(N259/H259)*(X259*AG259)*-1,(N259/M259)*(X259*AG259)*-1),0),0)","v":0},{"$f":"IF($AF259=3,IF($AF$2=2,(R259/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I259,Refurb_Poss_Tbl[%]))*AG259,IF($AF$2=3,(R259*AG259)-AV259,R259*AG259)),0)","v":0},{"$f":"IF(AF259=3,IF($AF$2=2,(S259/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I259,Refurb_Poss_Tbl[%]))*AG259,IF($AF$2=3,(S259*AG259)-AX259,S259*AG259)),0)","v":0},{"$f":"IF($AF259=3,IF($AF$2=2,(T259/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I259,Refurb_Poss_Tbl[%]))*AG259,T259*$AG259),0)","v":0},{"$f":"IF($AF259=3,IF($AF$2=2,(Q259/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I259,Refurb_Poss_Tbl[%]))*AG259,Q259*$AG259),0)","v":0},{"$f":"IF($AF259=3,IF($AF$2=2,(U259/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I259,Refurb_Poss_Tbl[%]))*AG259,U259*$AG259),0)","v":0},{"$f":"IF($AF259=3,IF($AF$2=2,(V259/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I259,Refurb_Poss_Tbl[%]))*AG259,IF($AF$2=3,(V259*AG259)-AW259,V259*AG259)),0)","v":0},{"$f":"IF($AF259=3,IF($AF$2=2,(W259/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I259,Refurb_Poss_Tbl[%]))*AG259,W259*$AG259),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,56,0,{"$f":"VLOOKUP(AE260,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19103608816200118},0,0,0,0,0,0,0,0,1.051415601209107E-2,{"$f":"IF(OR(AF260=3,AF260=2,AF260=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D260,FlatMaint!$Y$2:$Y$10000,AE260)*AG260,0)","v":16.921076366490261},{"$f":"IF(OR(AF260=3,AF260=2,AF260=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D260,FlatRepair!$Y$2:$Y$10000,AE260)*AG260,0)","v":16.921076366490261},0,33.852666888992616,0,0,0,0,0,33.852666888992616,0,{"$f":"IF($AF260=3,IF($AF$2=2,(R260/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I260,Refurb_Poss_Tbl[%]))*AG260,IF($AF$2=3,(R260*AG260)-AV260,R260*AG260)),0)","v":0},{"$f":"IF(AF260=3,IF($AF$2=2,(S260/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I260,Refurb_Poss_Tbl[%]))*AG260,IF($AF$2=3,(S260*AG260)-AX260,S260*AG260)),0)","v":0},{"$f":"IF($AF260=3,IF($AF$2=2,(T260/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I260,Refurb_Poss_Tbl[%]))*AG260,T260*$AG260),0)","v":0},{"$f":"IF($AF260=3,IF($AF$2=2,(Q260/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I260,Refurb_Poss_Tbl[%]))*AG260,Q260*$AG260),0)","v":0},{"$f":"IF($AF260=3,IF($AF$2=2,(U260/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I260,Refurb_Poss_Tbl[%]))*AG260,U260*$AG260),0)","v":0},{"$f":"IF($AF260=3,IF($AF$2=2,(V260/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I260,Refurb_Poss_Tbl[%]))*AG260,IF($AF$2=3,(V260*AG260)-AW260,V260*AG260)),0)","v":0},{"$f":"IF($AF260=3,IF($AF$2=2,(W260/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I260,Refurb_Poss_Tbl[%]))*AG260,W260*$AG260),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,57,0,{"$f":"VLOOKUP(AE261,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18547193025437006},0,0,0,0,0,0,0,0,1.0207918458340844E-2,{"$f":"IF(OR(AF261=3,AF261=2,AF261=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D261,FlatMaint!$Y$2:$Y$10000,AE261)*AG261,0)","v":16.428229482029376},{"$f":"IF(OR(AF261=3,AF261=2,AF261=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D261,FlatRepair!$Y$2:$Y$10000,AE261)*AG261,0)","v":0},0,16.438437400487718,0,0,0,0,0,16.438437400487718,0,{"$f":"IF($AF261=3,IF($AF$2=2,(R261/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I261,Refurb_Poss_Tbl[%]))*AG261,IF($AF$2=3,(R261*AG261)-AV261,R261*AG261)),0)","v":0},{"$f":"IF(AF261=3,IF($AF$2=2,(S261/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I261,Refurb_Poss_Tbl[%]))*AG261,IF($AF$2=3,(S261*AG261)-AX261,S261*AG261)),0)","v":0},{"$f":"IF($AF261=3,IF($AF$2=2,(T261/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I261,Refurb_Poss_Tbl[%]))*AG261,T261*$AG261),0)","v":0},{"$f":"IF($AF261=3,IF($AF$2=2,(Q261/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I261,Refurb_Poss_Tbl[%]))*AG261,Q261*$AG261),0)","v":0},{"$f":"IF($AF261=3,IF($AF$2=2,(U261/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I261,Refurb_Poss_Tbl[%]))*AG261,U261*$AG261),0)","v":0},{"$f":"IF($AF261=3,IF($AF$2=2,(V261/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I261,Refurb_Poss_Tbl[%]))*AG261,IF($AF$2=3,(V261*AG261)-AW261,V261*AG261)),0)","v":0},{"$f":"IF($AF261=3,IF($AF$2=2,(W261/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I261,Refurb_Poss_Tbl[%]))*AG261,W261*$AG261),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,58,0,{"$f":"VLOOKUP(AE262,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18006983519841754},0,0,0,0,0,0,0,0,9.9106004449911102E-3,{"$f":"IF(OR(AF262=3,AF262=2,AF262=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D262,FlatMaint!$Y$2:$Y$10000,AE262)*AG262,0)","v":15.949737361193572},{"$f":"IF(OR(AF262=3,AF262=2,AF262=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D262,FlatRepair!$Y$2:$Y$10000,AE262)*AG262,0)","v":15.949737361193572},0,31.909385322832136,0,0,0,0,0,31.909385322832136,0,{"$f":"IF($AF262=3,IF($AF$2=2,(R262/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I262,Refurb_Poss_Tbl[%]))*AG262,IF($AF$2=3,(R262*AG262)-AV262,R262*AG262)),0)","v":0},{"$f":"IF(AF262=3,IF($AF$2=2,(S262/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I262,Refurb_Poss_Tbl[%]))*AG262,IF($AF$2=3,(S262*AG262)-AX262,S262*AG262)),0)","v":0},{"$f":"IF($AF262=3,IF($AF$2=2,(T262/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I262,Refurb_Poss_Tbl[%]))*AG262,T262*$AG262),0)","v":0},{"$f":"IF($AF262=3,IF($AF$2=2,(Q262/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I262,Refurb_Poss_Tbl[%]))*AG262,Q262*$AG262),0)","v":0},{"$f":"IF($AF262=3,IF($AF$2=2,(U262/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I262,Refurb_Poss_Tbl[%]))*AG262,U262*$AG262),0)","v":0},{"$f":"IF($AF262=3,IF($AF$2=2,(V262/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I262,Refurb_Poss_Tbl[%]))*AG262,IF($AF$2=3,(V262*AG262)-AW262,V262*AG262)),0)","v":0},{"$f":"IF($AF262=3,IF($AF$2=2,(W262/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I262,Refurb_Poss_Tbl[%]))*AG262,W262*$AG262),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,59,0,{"$f":"VLOOKUP(AE263,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.17482508271691022},0,0,0,0,0,0,0,0,9.6219421796030196E-3,{"$f":"IF(OR(AF263=3,AF263=2,AF263=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D263,FlatMaint!$Y$2:$Y$10000,AE263)*AG263,0)","v":15.485181904071426},{"$f":"IF(OR(AF263=3,AF263=2,AF263=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D263,FlatRepair!$Y$2:$Y$10000,AE263)*AG263,0)","v":0},0,15.494803846251029,0,0,0,0,0,15.494803846251029,0,{"$f":"IF($AF263=3,IF($AF$2=2,(R263/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I263,Refurb_Poss_Tbl[%]))*AG263,IF($AF$2=3,(R263*AG263)-AV263,R263*AG263)),0)","v":0},{"$f":"IF(AF263=3,IF($AF$2=2,(S263/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I263,Refurb_Poss_Tbl[%]))*AG263,IF($AF$2=3,(S263*AG263)-AX263,S263*AG263)),0)","v":0},{"$f":"IF($AF263=3,IF($AF$2=2,(T263/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I263,Refurb_Poss_Tbl[%]))*AG263,T263*$AG263),0)","v":0},{"$f":"IF($AF263=3,IF($AF$2=2,(Q263/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I263,Refurb_Poss_Tbl[%]))*AG263,Q263*$AG263),0)","v":0},{"$f":"IF($AF263=3,IF($AF$2=2,(U263/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I263,Refurb_Poss_Tbl[%]))*AG263,U263*$AG263),0)","v":0},{"$f":"IF($AF263=3,IF($AF$2=2,(V263/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I263,Refurb_Poss_Tbl[%]))*AG263,IF($AF$2=3,(V263*AG263)-AW263,V263*AG263)),0)","v":0},{"$f":"IF($AF263=3,IF($AF$2=2,(W263/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I263,Refurb_Poss_Tbl[%]))*AG263,W263*$AG263),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,60,3,{"$f":"VLOOKUP(AE264,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1697330900164177},0,0,0,0,0,0,0,0,9.3416914365077874E-3,{"$f":"IF(OR(AF264=3,AF264=2,AF264=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D264,FlatMaint!$Y$2:$Y$10000,AE264)*AG264,0)","v":15.034157188418863},{"$f":"IF(OR(AF264=3,AF264=2,AF264=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D264,FlatRepair!$Y$2:$Y$10000,AE264)*AG264,0)","v":15.034157188418863},0,30.077656068274234,0,9.998203777686579E-2,1.1011918601854059E-2,0.41704295575185918,152.16340852027673,182.76910150068156,0,{"$f":"IF($AF264=3,IF($AF$2=2,(R264/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I264,Refurb_Poss_Tbl[%]))*AG264,IF($AF$2=3,(R264*AG264)-AV264,R264*AG264)),0)","v":4.860883883256524E-2},{"$f":"IF(AF264=3,IF($AF$2=2,(S264/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I264,Refurb_Poss_Tbl[%]))*AG264,IF($AF$2=3,(S264*AG264)-AX264,S264*AG264)),0)","v":0.83408591150371669},{"$f":"IF($AF264=3,IF($AF$2=2,(T264/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I264,Refurb_Poss_Tbl[%]))*AG264,T264*$AG264),0)","v":2.2023837203708183E-2},{"$f":"IF($AF264=3,IF($AF$2=2,(Q264/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I264,Refurb_Poss_Tbl[%]))*AG264,Q264*$AG264),0)","v":150.31562451853952},{"$f":"IF($AF264=3,IF($AF$2=2,(U264/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I264,Refurb_Poss_Tbl[%]))*AG264,U264*$AG264),0)","v":0.93780320168264564},{"$f":"IF($AF264=3,IF($AF$2=2,(V264/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I264,Refurb_Poss_Tbl[%]))*AG264,IF($AF$2=3,(V264*AG264)-AW264,V264*AG264)),0)","v":0},{"$f":"IF($AF264=3,IF($AF$2=2,(W264/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I264,Refurb_Poss_Tbl[%]))*AG264,W264*$AG264),0)","v":5.2622125145718839E-3}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,61,0,{"$f":"VLOOKUP(AE265,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.16478940778292983},0,0,0,0,0,0,0,0,9.0696033364153286E-3,{"$f":"IF(OR(AF265=3,AF265=2,AF265=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D265,FlatMaint!$Y$2:$Y$10000,AE265)*AG265,0)","v":14.596269114969772},{"$f":"IF(OR(AF265=3,AF265=2,AF265=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D265,FlatRepair!$Y$2:$Y$10000,AE265)*AG265,0)","v":0},0,14.605338718306188,0,0,0,0,0,14.605338718306188,0,{"$f":"IF($AF265=3,IF($AF$2=2,(R265/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I265,Refurb_Poss_Tbl[%]))*AG265,IF($AF$2=3,(R265*AG265)-AV265,R265*AG265)),0)","v":0},{"$f":"IF(AF265=3,IF($AF$2=2,(S265/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I265,Refurb_Poss_Tbl[%]))*AG265,IF($AF$2=3,(S265*AG265)-AX265,S265*AG265)),0)","v":0},{"$f":"IF($AF265=3,IF($AF$2=2,(T265/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I265,Refurb_Poss_Tbl[%]))*AG265,T265*$AG265),0)","v":0},{"$f":"IF($AF265=3,IF($AF$2=2,(Q265/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I265,Refurb_Poss_Tbl[%]))*AG265,Q265*$AG265),0)","v":0},{"$f":"IF($AF265=3,IF($AF$2=2,(U265/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I265,Refurb_Poss_Tbl[%]))*AG265,U265*$AG265),0)","v":0},{"$f":"IF($AF265=3,IF($AF$2=2,(V265/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I265,Refurb_Poss_Tbl[%]))*AG265,IF($AF$2=3,(V265*AG265)-AW265,V265*AG265)),0)","v":0},{"$f":"IF($AF265=3,IF($AF$2=2,(W265/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I265,Refurb_Poss_Tbl[%]))*AG265,W265*$AG265),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,62,0,{"$f":"VLOOKUP(AE266,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15998971629410663},0,0,0,0,0,0,0,0,8.8054401324420654E-3,{"$f":"IF(OR(AF266=3,AF266=2,AF266=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D266,FlatMaint!$Y$2:$Y$10000,AE266)*AG266,0)","v":14.171135063077449},{"$f":"IF(OR(AF266=3,AF266=2,AF266=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D266,FlatRepair!$Y$2:$Y$10000,AE266)*AG266,0)","v":14.171135063077449},0,28.351075566287339,0,0,0,0,0,28.351075566287339,0,{"$f":"IF($AF266=3,IF($AF$2=2,(R266/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I266,Refurb_Poss_Tbl[%]))*AG266,IF($AF$2=3,(R266*AG266)-AV266,R266*AG266)),0)","v":0},{"$f":"IF(AF266=3,IF($AF$2=2,(S266/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I266,Refurb_Poss_Tbl[%]))*AG266,IF($AF$2=3,(S266*AG266)-AX266,S266*AG266)),0)","v":0},{"$f":"IF($AF266=3,IF($AF$2=2,(T266/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I266,Refurb_Poss_Tbl[%]))*AG266,T266*$AG266),0)","v":0},{"$f":"IF($AF266=3,IF($AF$2=2,(Q266/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I266,Refurb_Poss_Tbl[%]))*AG266,Q266*$AG266),0)","v":0},{"$f":"IF($AF266=3,IF($AF$2=2,(U266/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I266,Refurb_Poss_Tbl[%]))*AG266,U266*$AG266),0)","v":0},{"$f":"IF($AF266=3,IF($AF$2=2,(V266/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I266,Refurb_Poss_Tbl[%]))*AG266,IF($AF$2=3,(V266*AG266)-AW266,V266*AG266)),0)","v":0},{"$f":"IF($AF266=3,IF($AF$2=2,(W266/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I266,Refurb_Poss_Tbl[%]))*AG266,W266*$AG266),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,63,0,{"$f":"VLOOKUP(AE267,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15532982164476369},0,0,0,0,0,0,0,0,8.5489710023709357E-3,{"$f":"IF(OR(AF267=3,AF267=2,AF267=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D267,FlatMaint!$Y$2:$Y$10000,AE267)*AG267,0)","v":13.758383556385869},{"$f":"IF(OR(AF267=3,AF267=2,AF267=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D267,FlatRepair!$Y$2:$Y$10000,AE267)*AG267,0)","v":0},0,13.76693252738824,0,0,0,0,0,13.76693252738824,0,{"$f":"IF($AF267=3,IF($AF$2=2,(R267/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I267,Refurb_Poss_Tbl[%]))*AG267,IF($AF$2=3,(R267*AG267)-AV267,R267*AG267)),0)","v":0},{"$f":"IF(AF267=3,IF($AF$2=2,(S267/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I267,Refurb_Poss_Tbl[%]))*AG267,IF($AF$2=3,(S267*AG267)-AX267,S267*AG267)),0)","v":0},{"$f":"IF($AF267=3,IF($AF$2=2,(T267/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I267,Refurb_Poss_Tbl[%]))*AG267,T267*$AG267),0)","v":0},{"$f":"IF($AF267=3,IF($AF$2=2,(Q267/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I267,Refurb_Poss_Tbl[%]))*AG267,Q267*$AG267),0)","v":0},{"$f":"IF($AF267=3,IF($AF$2=2,(U267/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I267,Refurb_Poss_Tbl[%]))*AG267,U267*$AG267),0)","v":0},{"$f":"IF($AF267=3,IF($AF$2=2,(V267/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I267,Refurb_Poss_Tbl[%]))*AG267,IF($AF$2=3,(V267*AG267)-AW267,V267*AG267)),0)","v":0},{"$f":"IF($AF267=3,IF($AF$2=2,(W267/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I267,Refurb_Poss_Tbl[%]))*AG267,W267*$AG267),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,64,0,{"$f":"VLOOKUP(AE268,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15080565208229488},0,0,0,0,0,0,0,0,8.2999718469620766E-3,{"$f":"IF(OR(AF268=3,AF268=2,AF268=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D268,FlatMaint!$Y$2:$Y$10000,AE268)*AG268,0)","v":13.357653938238711},{"$f":"IF(OR(AF268=3,AF268=2,AF268=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D268,FlatRepair!$Y$2:$Y$10000,AE268)*AG268,0)","v":13.357653938238711},0,26.723607848324384,0,0,0,0,0,26.723607848324384,0,{"$f":"IF($AF268=3,IF($AF$2=2,(R268/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I268,Refurb_Poss_Tbl[%]))*AG268,IF($AF$2=3,(R268*AG268)-AV268,R268*AG268)),0)","v":0},{"$f":"IF(AF268=3,IF($AF$2=2,(S268/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I268,Refurb_Poss_Tbl[%]))*AG268,IF($AF$2=3,(S268*AG268)-AX268,S268*AG268)),0)","v":0},{"$f":"IF($AF268=3,IF($AF$2=2,(T268/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I268,Refurb_Poss_Tbl[%]))*AG268,T268*$AG268),0)","v":0},{"$f":"IF($AF268=3,IF($AF$2=2,(Q268/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I268,Refurb_Poss_Tbl[%]))*AG268,Q268*$AG268),0)","v":0},{"$f":"IF($AF268=3,IF($AF$2=2,(U268/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I268,Refurb_Poss_Tbl[%]))*AG268,U268*$AG268),0)","v":0},{"$f":"IF($AF268=3,IF($AF$2=2,(V268/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I268,Refurb_Poss_Tbl[%]))*AG268,IF($AF$2=3,(V268*AG268)-AW268,V268*AG268)),0)","v":0},{"$f":"IF($AF268=3,IF($AF$2=2,(W268/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I268,Refurb_Poss_Tbl[%]))*AG268,W268*$AG268),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,65,0,{"$f":"VLOOKUP(AE269,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14641325444882999},0,0,0,0,0,0,0,0,8.0582250941379392E-3,{"$f":"IF(OR(AF269=3,AF269=2,AF269=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D269,FlatMaint!$Y$2:$Y$10000,AE269)*AG269,0)","v":12.96859605654244},{"$f":"IF(OR(AF269=3,AF269=2,AF269=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D269,FlatRepair!$Y$2:$Y$10000,AE269)*AG269,0)","v":0},0,12.976654281636577,0,0,0,0,0,12.976654281636577,0,{"$f":"IF($AF269=3,IF($AF$2=2,(R269/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I269,Refurb_Poss_Tbl[%]))*AG269,IF($AF$2=3,(R269*AG269)-AV269,R269*AG269)),0)","v":0},{"$f":"IF(AF269=3,IF($AF$2=2,(S269/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I269,Refurb_Poss_Tbl[%]))*AG269,IF($AF$2=3,(S269*AG269)-AX269,S269*AG269)),0)","v":0},{"$f":"IF($AF269=3,IF($AF$2=2,(T269/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I269,Refurb_Poss_Tbl[%]))*AG269,T269*$AG269),0)","v":0},{"$f":"IF($AF269=3,IF($AF$2=2,(Q269/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I269,Refurb_Poss_Tbl[%]))*AG269,Q269*$AG269),0)","v":0},{"$f":"IF($AF269=3,IF($AF$2=2,(U269/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I269,Refurb_Poss_Tbl[%]))*AG269,U269*$AG269),0)","v":0},{"$f":"IF($AF269=3,IF($AF$2=2,(V269/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I269,Refurb_Poss_Tbl[%]))*AG269,IF($AF$2=3,(V269*AG269)-AW269,V269*AG269)),0)","v":0},{"$f":"IF($AF269=3,IF($AF$2=2,(W269/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I269,Refurb_Poss_Tbl[%]))*AG269,W269*$AG269),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,66,0,{"$f":"VLOOKUP(AE270,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14214879072701941},0,0,0,0,0,0,0,0,7.823519508871786E-3,{"$f":"IF(OR(AF270=3,AF270=2,AF270=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D270,FlatMaint!$Y$2:$Y$10000,AE270)*AG270,0)","v":12.590869957808193},{"$f":"IF(OR(AF270=3,AF270=2,AF270=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D270,FlatRepair!$Y$2:$Y$10000,AE270)*AG270,0)","v":12.590869957808193},0,25.189563435125258,0,0,0,0,0,25.189563435125258,0,{"$f":"IF($AF270=3,IF($AF$2=2,(R270/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I270,Refurb_Poss_Tbl[%]))*AG270,IF($AF$2=3,(R270*AG270)-AV270,R270*AG270)),0)","v":0},{"$f":"IF(AF270=3,IF($AF$2=2,(S270/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I270,Refurb_Poss_Tbl[%]))*AG270,IF($AF$2=3,(S270*AG270)-AX270,S270*AG270)),0)","v":0},{"$f":"IF($AF270=3,IF($AF$2=2,(T270/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I270,Refurb_Poss_Tbl[%]))*AG270,T270*$AG270),0)","v":0},{"$f":"IF($AF270=3,IF($AF$2=2,(Q270/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I270,Refurb_Poss_Tbl[%]))*AG270,Q270*$AG270),0)","v":0},{"$f":"IF($AF270=3,IF($AF$2=2,(U270/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I270,Refurb_Poss_Tbl[%]))*AG270,U270*$AG270),0)","v":0},{"$f":"IF($AF270=3,IF($AF$2=2,(V270/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I270,Refurb_Poss_Tbl[%]))*AG270,IF($AF$2=3,(V270*AG270)-AW270,V270*AG270)),0)","v":0},{"$f":"IF($AF270=3,IF($AF$2=2,(W270/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I270,Refurb_Poss_Tbl[%]))*AG270,W270*$AG270),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,67,0,{"$f":"VLOOKUP(AE271,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1380085346864266},0,0,0,0,0,0,0,0,7.5956500086133824E-3,{"$f":"IF(OR(AF271=3,AF271=2,AF271=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D271,FlatMaint!$Y$2:$Y$10000,AE271)*AG271,0)","v":12.22414559010504},{"$f":"IF(OR(AF271=3,AF271=2,AF271=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D271,FlatRepair!$Y$2:$Y$10000,AE271)*AG271,0)","v":0},0,12.231741240113653,0,0,0,0,0,12.231741240113653,0,{"$f":"IF($AF271=3,IF($AF$2=2,(R271/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I271,Refurb_Poss_Tbl[%]))*AG271,IF($AF$2=3,(R271*AG271)-AV271,R271*AG271)),0)","v":0},{"$f":"IF(AF271=3,IF($AF$2=2,(S271/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I271,Refurb_Poss_Tbl[%]))*AG271,IF($AF$2=3,(S271*AG271)-AX271,S271*AG271)),0)","v":0},{"$f":"IF($AF271=3,IF($AF$2=2,(T271/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I271,Refurb_Poss_Tbl[%]))*AG271,T271*$AG271),0)","v":0},{"$f":"IF($AF271=3,IF($AF$2=2,(Q271/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I271,Refurb_Poss_Tbl[%]))*AG271,Q271*$AG271),0)","v":0},{"$f":"IF($AF271=3,IF($AF$2=2,(U271/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I271,Refurb_Poss_Tbl[%]))*AG271,U271*$AG271),0)","v":0},{"$f":"IF($AF271=3,IF($AF$2=2,(V271/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I271,Refurb_Poss_Tbl[%]))*AG271,IF($AF$2=3,(V271*AG271)-AW271,V271*AG271)),0)","v":0},{"$f":"IF($AF271=3,IF($AF$2=2,(W271/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I271,Refurb_Poss_Tbl[%]))*AG271,W271*$AG271),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,68,0,{"$f":"VLOOKUP(AE272,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13398886862759865},0,0,0,0,0,0,0,0,7.3744174840906637E-3,{"$f":"IF(OR(AF272=3,AF272=2,AF272=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D272,FlatMaint!$Y$2:$Y$10000,AE272)*AG272,0)","v":11.86810251466509},{"$f":"IF(OR(AF272=3,AF272=2,AF272=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D272,FlatRepair!$Y$2:$Y$10000,AE272)*AG272,0)","v":11.86810251466509},0,23.74357944681427,0,0,0,0,0,23.74357944681427,0,{"$f":"IF($AF272=3,IF($AF$2=2,(R272/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I272,Refurb_Poss_Tbl[%]))*AG272,IF($AF$2=3,(R272*AG272)-AV272,R272*AG272)),0)","v":0},{"$f":"IF(AF272=3,IF($AF$2=2,(S272/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I272,Refurb_Poss_Tbl[%]))*AG272,IF($AF$2=3,(S272*AG272)-AX272,S272*AG272)),0)","v":0},{"$f":"IF($AF272=3,IF($AF$2=2,(T272/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I272,Refurb_Poss_Tbl[%]))*AG272,T272*$AG272),0)","v":0},{"$f":"IF($AF272=3,IF($AF$2=2,(Q272/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I272,Refurb_Poss_Tbl[%]))*AG272,Q272*$AG272),0)","v":0},{"$f":"IF($AF272=3,IF($AF$2=2,(U272/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I272,Refurb_Poss_Tbl[%]))*AG272,U272*$AG272),0)","v":0},{"$f":"IF($AF272=3,IF($AF$2=2,(V272/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I272,Refurb_Poss_Tbl[%]))*AG272,IF($AF$2=3,(V272*AG272)-AW272,V272*AG272)),0)","v":0},{"$f":"IF($AF272=3,IF($AF$2=2,(W272/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I272,Refurb_Poss_Tbl[%]))*AG272,W272*$AG272),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,69,0,{"$f":"VLOOKUP(AE273,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13008628022096957},0,0,0,0,0,0,0,0,7.1596286253307415E-3,{"$f":"IF(OR(AF273=3,AF273=2,AF273=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D273,FlatMaint!$Y$2:$Y$10000,AE273)*AG273,0)","v":11.522429625888437},{"$f":"IF(OR(AF273=3,AF273=2,AF273=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D273,FlatRepair!$Y$2:$Y$10000,AE273)*AG273,0)","v":0},0,11.529589254513768,0,0,0,0,0,11.529589254513768,0,{"$f":"IF($AF273=3,IF($AF$2=2,(R273/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I273,Refurb_Poss_Tbl[%]))*AG273,IF($AF$2=3,(R273*AG273)-AV273,R273*AG273)),0)","v":0},{"$f":"IF(AF273=3,IF($AF$2=2,(S273/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I273,Refurb_Poss_Tbl[%]))*AG273,IF($AF$2=3,(S273*AG273)-AX273,S273*AG273)),0)","v":0},{"$f":"IF($AF273=3,IF($AF$2=2,(T273/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I273,Refurb_Poss_Tbl[%]))*AG273,T273*$AG273),0)","v":0},{"$f":"IF($AF273=3,IF($AF$2=2,(Q273/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I273,Refurb_Poss_Tbl[%]))*AG273,Q273*$AG273),0)","v":0},{"$f":"IF($AF273=3,IF($AF$2=2,(U273/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I273,Refurb_Poss_Tbl[%]))*AG273,U273*$AG273),0)","v":0},{"$f":"IF($AF273=3,IF($AF$2=2,(V273/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I273,Refurb_Poss_Tbl[%]))*AG273,IF($AF$2=3,(V273*AG273)-AW273,V273*AG273)),0)","v":0},{"$f":"IF($AF273=3,IF($AF$2=2,(W273/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I273,Refurb_Poss_Tbl[%]))*AG273,W273*$AG273),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,70,0,{"$f":"VLOOKUP(AE274,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12629735943783454},0,0,0,0,0,0,0,0,6.9510957527482934E-3,{"$f":"IF(OR(AF274=3,AF274=2,AF274=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D274,FlatMaint!$Y$2:$Y$10000,AE274)*AG274,0)","v":11.186824879503337},{"$f":"IF(OR(AF274=3,AF274=2,AF274=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D274,FlatRepair!$Y$2:$Y$10000,AE274)*AG274,0)","v":11.186824879503337},0,22.380600854759422,0,0,0,0,0,22.380600854759422,0,{"$f":"IF($AF274=3,IF($AF$2=2,(R274/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I274,Refurb_Poss_Tbl[%]))*AG274,IF($AF$2=3,(R274*AG274)-AV274,R274*AG274)),0)","v":0},{"$f":"IF(AF274=3,IF($AF$2=2,(S274/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I274,Refurb_Poss_Tbl[%]))*AG274,IF($AF$2=3,(S274*AG274)-AX274,S274*AG274)),0)","v":0},{"$f":"IF($AF274=3,IF($AF$2=2,(T274/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I274,Refurb_Poss_Tbl[%]))*AG274,T274*$AG274),0)","v":0},{"$f":"IF($AF274=3,IF($AF$2=2,(Q274/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I274,Refurb_Poss_Tbl[%]))*AG274,Q274*$AG274),0)","v":0},{"$f":"IF($AF274=3,IF($AF$2=2,(U274/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I274,Refurb_Poss_Tbl[%]))*AG274,U274*$AG274),0)","v":0},{"$f":"IF($AF274=3,IF($AF$2=2,(V274/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I274,Refurb_Poss_Tbl[%]))*AG274,IF($AF$2=3,(V274*AG274)-AW274,V274*AG274)),0)","v":0},{"$f":"IF($AF274=3,IF($AF$2=2,(W274/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I274,Refurb_Poss_Tbl[%]))*AG274,W274*$AG274),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,71,0,{"$f":"VLOOKUP(AE275,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12261879557071313},0,0,0,0,0,0,0,0,6.7486366531536819E-3,{"$f":"IF(OR(AF275=3,AF275=2,AF275=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D275,FlatMaint!$Y$2:$Y$10000,AE275)*AG275,0)","v":10.860995028644016},{"$f":"IF(OR(AF275=3,AF275=2,AF275=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D275,FlatRepair!$Y$2:$Y$10000,AE275)*AG275,0)","v":0},0,10.867743665297169,0,0,0,0,0,10.867743665297169,0,{"$f":"IF($AF275=3,IF($AF$2=2,(R275/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I275,Refurb_Poss_Tbl[%]))*AG275,IF($AF$2=3,(R275*AG275)-AV275,R275*AG275)),0)","v":0},{"$f":"IF(AF275=3,IF($AF$2=2,(S275/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I275,Refurb_Poss_Tbl[%]))*AG275,IF($AF$2=3,(S275*AG275)-AX275,S275*AG275)),0)","v":0},{"$f":"IF($AF275=3,IF($AF$2=2,(T275/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I275,Refurb_Poss_Tbl[%]))*AG275,T275*$AG275),0)","v":0},{"$f":"IF($AF275=3,IF($AF$2=2,(Q275/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I275,Refurb_Poss_Tbl[%]))*AG275,Q275*$AG275),0)","v":0},{"$f":"IF($AF275=3,IF($AF$2=2,(U275/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I275,Refurb_Poss_Tbl[%]))*AG275,U275*$AG275),0)","v":0},{"$f":"IF($AF275=3,IF($AF$2=2,(V275/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I275,Refurb_Poss_Tbl[%]))*AG275,IF($AF$2=3,(V275*AG275)-AW275,V275*AG275)),0)","v":0},{"$f":"IF($AF275=3,IF($AF$2=2,(W275/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I275,Refurb_Poss_Tbl[%]))*AG275,W275*$AG275),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,72,0,{"$f":"VLOOKUP(AE276,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1190473743404982},0,0,0,0,0,0,0,0,6.5520744205375559E-3,{"$f":"IF(OR(AF276=3,AF276=2,AF276=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D276,FlatMaint!$Y$2:$Y$10000,AE276)*AG276,0)","v":10.544655367615549},{"$f":"IF(OR(AF276=3,AF276=2,AF276=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D276,FlatRepair!$Y$2:$Y$10000,AE276)*AG276,0)","v":10.544655367615549},0,21.095862809651635,0,0,0,0,0,21.095862809651635,0,{"$f":"IF($AF276=3,IF($AF$2=2,(R276/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I276,Refurb_Poss_Tbl[%]))*AG276,IF($AF$2=3,(R276*AG276)-AV276,R276*AG276)),0)","v":0},{"$f":"IF(AF276=3,IF($AF$2=2,(S276/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I276,Refurb_Poss_Tbl[%]))*AG276,IF($AF$2=3,(S276*AG276)-AX276,S276*AG276)),0)","v":0},{"$f":"IF($AF276=3,IF($AF$2=2,(T276/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I276,Refurb_Poss_Tbl[%]))*AG276,T276*$AG276),0)","v":0},{"$f":"IF($AF276=3,IF($AF$2=2,(Q276/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I276,Refurb_Poss_Tbl[%]))*AG276,Q276*$AG276),0)","v":0},{"$f":"IF($AF276=3,IF($AF$2=2,(U276/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I276,Refurb_Poss_Tbl[%]))*AG276,U276*$AG276),0)","v":0},{"$f":"IF($AF276=3,IF($AF$2=2,(V276/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I276,Refurb_Poss_Tbl[%]))*AG276,IF($AF$2=3,(V276*AG276)-AW276,V276*AG276)),0)","v":0},{"$f":"IF($AF276=3,IF($AF$2=2,(W276/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I276,Refurb_Poss_Tbl[%]))*AG276,W276*$AG276),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,73,0,{"$f":"VLOOKUP(AE277,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11557997508786232},0,0,0,0,0,0,0,0,6.3612373014927722E-3,{"$f":"IF(OR(AF277=3,AF277=2,AF277=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D277,FlatMaint!$Y$2:$Y$10000,AE277)*AG277,0)","v":10.237529483121891},{"$f":"IF(OR(AF277=3,AF277=2,AF277=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D277,FlatRepair!$Y$2:$Y$10000,AE277)*AG277,0)","v":0},0,10.243890720423384,0,0,0,0,0,10.243890720423384,0,{"$f":"IF($AF277=3,IF($AF$2=2,(R277/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I277,Refurb_Poss_Tbl[%]))*AG277,IF($AF$2=3,(R277*AG277)-AV277,R277*AG277)),0)","v":0},{"$f":"IF(AF277=3,IF($AF$2=2,(S277/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I277,Refurb_Poss_Tbl[%]))*AG277,IF($AF$2=3,(S277*AG277)-AX277,S277*AG277)),0)","v":0},{"$f":"IF($AF277=3,IF($AF$2=2,(T277/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I277,Refurb_Poss_Tbl[%]))*AG277,T277*$AG277),0)","v":0},{"$f":"IF($AF277=3,IF($AF$2=2,(Q277/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I277,Refurb_Poss_Tbl[%]))*AG277,Q277*$AG277),0)","v":0},{"$f":"IF($AF277=3,IF($AF$2=2,(U277/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I277,Refurb_Poss_Tbl[%]))*AG277,U277*$AG277),0)","v":0},{"$f":"IF($AF277=3,IF($AF$2=2,(V277/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I277,Refurb_Poss_Tbl[%]))*AG277,IF($AF$2=3,(V277*AG277)-AW277,V277*AG277)),0)","v":0},{"$f":"IF($AF277=3,IF($AF$2=2,(W277/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I277,Refurb_Poss_Tbl[%]))*AG277,W277*$AG277),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,74,0,{"$f":"VLOOKUP(AE278,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11221356804646829},0,0,0,0,0,0,0,0,6.1759585451386144E-3,{"$f":"IF(OR(AF278=3,AF278=2,AF278=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D278,FlatMaint!$Y$2:$Y$10000,AE278)*AG278,0)","v":9.9393490127397026},{"$f":"IF(OR(AF278=3,AF278=2,AF278=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D278,FlatRepair!$Y$2:$Y$10000,AE278)*AG278,0)","v":9.9393490127397026},0,19.884873984024544,0,0,0,0,0,19.884873984024544,0,{"$f":"IF($AF278=3,IF($AF$2=2,(R278/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I278,Refurb_Poss_Tbl[%]))*AG278,IF($AF$2=3,(R278*AG278)-AV278,R278*AG278)),0)","v":0},{"$f":"IF(AF278=3,IF($AF$2=2,(S278/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I278,Refurb_Poss_Tbl[%]))*AG278,IF($AF$2=3,(S278*AG278)-AX278,S278*AG278)),0)","v":0},{"$f":"IF($AF278=3,IF($AF$2=2,(T278/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I278,Refurb_Poss_Tbl[%]))*AG278,T278*$AG278),0)","v":0},{"$f":"IF($AF278=3,IF($AF$2=2,(Q278/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I278,Refurb_Poss_Tbl[%]))*AG278,Q278*$AG278),0)","v":0},{"$f":"IF($AF278=3,IF($AF$2=2,(U278/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I278,Refurb_Poss_Tbl[%]))*AG278,U278*$AG278),0)","v":0},{"$f":"IF($AF278=3,IF($AF$2=2,(V278/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I278,Refurb_Poss_Tbl[%]))*AG278,IF($AF$2=3,(V278*AG278)-AW278,V278*AG278)),0)","v":0},{"$f":"IF($AF278=3,IF($AF$2=2,(W278/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I278,Refurb_Poss_Tbl[%]))*AG278,W278*$AG278),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,75,0,{"$f":"VLOOKUP(AE279,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10894521169560026},0,0,0,0,0,0,0,0,5.9960762574161296E-3,{"$f":"IF(OR(AF279=3,AF279=2,AF279=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D279,FlatMaint!$Y$2:$Y$10000,AE279)*AG279,0)","v":9.6498534104268945},{"$f":"IF(OR(AF279=3,AF279=2,AF279=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D279,FlatRepair!$Y$2:$Y$10000,AE279)*AG279,0)","v":0},0,9.6558494866843105,0,0,0,0,0,9.6558494866843105,0,{"$f":"IF($AF279=3,IF($AF$2=2,(R279/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I279,Refurb_Poss_Tbl[%]))*AG279,IF($AF$2=3,(R279*AG279)-AV279,R279*AG279)),0)","v":0},{"$f":"IF(AF279=3,IF($AF$2=2,(S279/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I279,Refurb_Poss_Tbl[%]))*AG279,IF($AF$2=3,(S279*AG279)-AX279,S279*AG279)),0)","v":0},{"$f":"IF($AF279=3,IF($AF$2=2,(T279/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I279,Refurb_Poss_Tbl[%]))*AG279,T279*$AG279),0)","v":0},{"$f":"IF($AF279=3,IF($AF$2=2,(Q279/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I279,Refurb_Poss_Tbl[%]))*AG279,Q279*$AG279),0)","v":0},{"$f":"IF($AF279=3,IF($AF$2=2,(U279/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I279,Refurb_Poss_Tbl[%]))*AG279,U279*$AG279),0)","v":0},{"$f":"IF($AF279=3,IF($AF$2=2,(V279/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I279,Refurb_Poss_Tbl[%]))*AG279,IF($AF$2=3,(V279*AG279)-AW279,V279*AG279)),0)","v":0},{"$f":"IF($AF279=3,IF($AF$2=2,(W279/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I279,Refurb_Poss_Tbl[%]))*AG279,W279*$AG279),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,76,0,{"$f":"VLOOKUP(AE280,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15310389176729922},0,0,0,0,0,0,0,0,8.4264613015661884E-3,{"$f":"IF(OR(AF280=3,AF280=2,AF280=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D280,FlatMaint!$Y$2:$Y$10000,AE280)*AG280,0)","v":13.561221178295881},{"$f":"IF(OR(AF280=3,AF280=2,AF280=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D280,FlatRepair!$Y$2:$Y$10000,AE280)*AG280,0)","v":13.561221178295881},0,27.130868817893329,0,0,0,0,0,27.130868817893329,0,{"$f":"IF($AF280=3,IF($AF$2=2,(R280/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I280,Refurb_Poss_Tbl[%]))*AG280,IF($AF$2=3,(R280*AG280)-AV280,R280*AG280)),0)","v":0},{"$f":"IF(AF280=3,IF($AF$2=2,(S280/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I280,Refurb_Poss_Tbl[%]))*AG280,IF($AF$2=3,(S280*AG280)-AX280,S280*AG280)),0)","v":0},{"$f":"IF($AF280=3,IF($AF$2=2,(T280/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I280,Refurb_Poss_Tbl[%]))*AG280,T280*$AG280),0)","v":0},{"$f":"IF($AF280=3,IF($AF$2=2,(Q280/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I280,Refurb_Poss_Tbl[%]))*AG280,Q280*$AG280),0)","v":0},{"$f":"IF($AF280=3,IF($AF$2=2,(U280/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I280,Refurb_Poss_Tbl[%]))*AG280,U280*$AG280),0)","v":0},{"$f":"IF($AF280=3,IF($AF$2=2,(V280/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I280,Refurb_Poss_Tbl[%]))*AG280,IF($AF$2=3,(V280*AG280)-AW280,V280*AG280)),0)","v":0},{"$f":"IF($AF280=3,IF($AF$2=2,(W280/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I280,Refurb_Poss_Tbl[%]))*AG280,W280*$AG280),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,77,0,{"$f":"VLOOKUP(AE281,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14936965050468218},0,0,0,0,0,0,0,0,8.2209378551865268E-3,{"$f":"IF(OR(AF281=3,AF281=2,AF281=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D281,FlatMaint!$Y$2:$Y$10000,AE281)*AG281,0)","v":13.230459686142325},{"$f":"IF(OR(AF281=3,AF281=2,AF281=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D281,FlatRepair!$Y$2:$Y$10000,AE281)*AG281,0)","v":0},0,13.238680623997512,0,0,0,0,0,13.238680623997512,0,{"$f":"IF($AF281=3,IF($AF$2=2,(R281/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I281,Refurb_Poss_Tbl[%]))*AG281,IF($AF$2=3,(R281*AG281)-AV281,R281*AG281)),0)","v":0},{"$f":"IF(AF281=3,IF($AF$2=2,(S281/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I281,Refurb_Poss_Tbl[%]))*AG281,IF($AF$2=3,(S281*AG281)-AX281,S281*AG281)),0)","v":0},{"$f":"IF($AF281=3,IF($AF$2=2,(T281/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I281,Refurb_Poss_Tbl[%]))*AG281,T281*$AG281),0)","v":0},{"$f":"IF($AF281=3,IF($AF$2=2,(Q281/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I281,Refurb_Poss_Tbl[%]))*AG281,Q281*$AG281),0)","v":0},{"$f":"IF($AF281=3,IF($AF$2=2,(U281/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I281,Refurb_Poss_Tbl[%]))*AG281,U281*$AG281),0)","v":0},{"$f":"IF($AF281=3,IF($AF$2=2,(V281/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I281,Refurb_Poss_Tbl[%]))*AG281,IF($AF$2=3,(V281*AG281)-AW281,V281*AG281)),0)","v":0},{"$f":"IF($AF281=3,IF($AF$2=2,(W281/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I281,Refurb_Poss_Tbl[%]))*AG281,W281*$AG281),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,78,0,{"$f":"VLOOKUP(AE282,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14572648829725093},0,0,0,0,0,0,0,0,8.0204271757917337E-3,{"$f":"IF(OR(AF282=3,AF282=2,AF282=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D282,FlatMaint!$Y$2:$Y$10000,AE282)*AG282,0)","v":12.907765547455929},{"$f":"IF(OR(AF282=3,AF282=2,AF282=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D282,FlatRepair!$Y$2:$Y$10000,AE282)*AG282,0)","v":12.907765547455929},0,25.823551522087648,0,0,0,0,0,25.823551522087648,0,{"$f":"IF($AF282=3,IF($AF$2=2,(R282/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I282,Refurb_Poss_Tbl[%]))*AG282,IF($AF$2=3,(R282*AG282)-AV282,R282*AG282)),0)","v":0},{"$f":"IF(AF282=3,IF($AF$2=2,(S282/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I282,Refurb_Poss_Tbl[%]))*AG282,IF($AF$2=3,(S282*AG282)-AX282,S282*AG282)),0)","v":0},{"$f":"IF($AF282=3,IF($AF$2=2,(T282/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I282,Refurb_Poss_Tbl[%]))*AG282,T282*$AG282),0)","v":0},{"$f":"IF($AF282=3,IF($AF$2=2,(Q282/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I282,Refurb_Poss_Tbl[%]))*AG282,Q282*$AG282),0)","v":0},{"$f":"IF($AF282=3,IF($AF$2=2,(U282/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I282,Refurb_Poss_Tbl[%]))*AG282,U282*$AG282),0)","v":0},{"$f":"IF($AF282=3,IF($AF$2=2,(V282/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I282,Refurb_Poss_Tbl[%]))*AG282,IF($AF$2=3,(V282*AG282)-AW282,V282*AG282)),0)","v":0},{"$f":"IF($AF282=3,IF($AF$2=2,(W282/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I282,Refurb_Poss_Tbl[%]))*AG282,W282*$AG282),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,79,0,{"$f":"VLOOKUP(AE283,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14217218370463502},0,0,0,0,0,0,0,0,7.8248070007724217E-3,{"$f":"IF(OR(AF283=3,AF283=2,AF283=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D283,FlatMaint!$Y$2:$Y$10000,AE283)*AG283,0)","v":12.592941997517977},{"$f":"IF(OR(AF283=3,AF283=2,AF283=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D283,FlatRepair!$Y$2:$Y$10000,AE283)*AG283,0)","v":0},0,12.60076680451875,0,0,0,0,0,12.60076680451875,0,{"$f":"IF($AF283=3,IF($AF$2=2,(R283/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I283,Refurb_Poss_Tbl[%]))*AG283,IF($AF$2=3,(R283*AG283)-AV283,R283*AG283)),0)","v":0},{"$f":"IF(AF283=3,IF($AF$2=2,(S283/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I283,Refurb_Poss_Tbl[%]))*AG283,IF($AF$2=3,(S283*AG283)-AX283,S283*AG283)),0)","v":0},{"$f":"IF($AF283=3,IF($AF$2=2,(T283/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I283,Refurb_Poss_Tbl[%]))*AG283,T283*$AG283),0)","v":0},{"$f":"IF($AF283=3,IF($AF$2=2,(Q283/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I283,Refurb_Poss_Tbl[%]))*AG283,Q283*$AG283),0)","v":0},{"$f":"IF($AF283=3,IF($AF$2=2,(U283/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I283,Refurb_Poss_Tbl[%]))*AG283,U283*$AG283),0)","v":0},{"$f":"IF($AF283=3,IF($AF$2=2,(V283/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I283,Refurb_Poss_Tbl[%]))*AG283,IF($AF$2=3,(V283*AG283)-AW283,V283*AG283)),0)","v":0},{"$f":"IF($AF283=3,IF($AF$2=2,(W283/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I283,Refurb_Poss_Tbl[%]))*AG283,W283*$AG283),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,80,0,{"$f":"VLOOKUP(AE284,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13870456946793663},0,0,0,0,0,0,0,0,7.633958049534071E-3,{"$f":"IF(OR(AF284=3,AF284=2,AF284=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D284,FlatMaint!$Y$2:$Y$10000,AE284)*AG284,0)","v":12.285797070749247},{"$f":"IF(OR(AF284=3,AF284=2,AF284=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D284,FlatRepair!$Y$2:$Y$10000,AE284)*AG284,0)","v":12.285797070749247},0,24.579228099548025,0,0,0,0,0,24.579228099548025,0,{"$f":"IF($AF284=3,IF($AF$2=2,(R284/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I284,Refurb_Poss_Tbl[%]))*AG284,IF($AF$2=3,(R284*AG284)-AV284,R284*AG284)),0)","v":0},{"$f":"IF(AF284=3,IF($AF$2=2,(S284/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I284,Refurb_Poss_Tbl[%]))*AG284,IF($AF$2=3,(S284*AG284)-AX284,S284*AG284)),0)","v":0},{"$f":"IF($AF284=3,IF($AF$2=2,(T284/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I284,Refurb_Poss_Tbl[%]))*AG284,T284*$AG284),0)","v":0},{"$f":"IF($AF284=3,IF($AF$2=2,(Q284/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I284,Refurb_Poss_Tbl[%]))*AG284,Q284*$AG284),0)","v":0},{"$f":"IF($AF284=3,IF($AF$2=2,(U284/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I284,Refurb_Poss_Tbl[%]))*AG284,U284*$AG284),0)","v":0},{"$f":"IF($AF284=3,IF($AF$2=2,(V284/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I284,Refurb_Poss_Tbl[%]))*AG284,IF($AF$2=3,(V284*AG284)-AW284,V284*AG284)),0)","v":0},{"$f":"IF($AF284=3,IF($AF$2=2,(W284/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I284,Refurb_Poss_Tbl[%]))*AG284,W284*$AG284),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,81,0,{"$f":"VLOOKUP(AE285,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13532153118823087},0,0,0,0,0,0,0,0,7.4477639507649481E-3,{"$f":"IF(OR(AF285=3,AF285=2,AF285=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D285,FlatMaint!$Y$2:$Y$10000,AE285)*AG285,0)","v":11.986143483657804},{"$f":"IF(OR(AF285=3,AF285=2,AF285=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D285,FlatRepair!$Y$2:$Y$10000,AE285)*AG285,0)","v":0},0,11.993591247608569,0,0,0,0,0,11.993591247608569,0,{"$f":"IF($AF285=3,IF($AF$2=2,(R285/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I285,Refurb_Poss_Tbl[%]))*AG285,IF($AF$2=3,(R285*AG285)-AV285,R285*AG285)),0)","v":0},{"$f":"IF(AF285=3,IF($AF$2=2,(S285/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I285,Refurb_Poss_Tbl[%]))*AG285,IF($AF$2=3,(S285*AG285)-AX285,S285*AG285)),0)","v":0},{"$f":"IF($AF285=3,IF($AF$2=2,(T285/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I285,Refurb_Poss_Tbl[%]))*AG285,T285*$AG285),0)","v":0},{"$f":"IF($AF285=3,IF($AF$2=2,(Q285/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I285,Refurb_Poss_Tbl[%]))*AG285,Q285*$AG285),0)","v":0},{"$f":"IF($AF285=3,IF($AF$2=2,(U285/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I285,Refurb_Poss_Tbl[%]))*AG285,U285*$AG285),0)","v":0},{"$f":"IF($AF285=3,IF($AF$2=2,(V285/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I285,Refurb_Poss_Tbl[%]))*AG285,IF($AF$2=3,(V285*AG285)-AW285,V285*AG285)),0)","v":0},{"$f":"IF($AF285=3,IF($AF$2=2,(W285/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I285,Refurb_Poss_Tbl[%]))*AG285,W285*$AG285),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,82,0,{"$f":"VLOOKUP(AE286,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13202100603729841},0,0,0,0,0,0,0,0,7.266111171477998E-3,{"$f":"IF(OR(AF286=3,AF286=2,AF286=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D286,FlatMaint!$Y$2:$Y$10000,AE286)*AG286,0)","v":11.69379852064176},{"$f":"IF(OR(AF286=3,AF286=2,AF286=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D286,FlatRepair!$Y$2:$Y$10000,AE286)*AG286,0)","v":11.69379852064176},0,23.394863152454999,0,0,0,0,0,23.394863152454999,0,{"$f":"IF($AF286=3,IF($AF$2=2,(R286/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I286,Refurb_Poss_Tbl[%]))*AG286,IF($AF$2=3,(R286*AG286)-AV286,R286*AG286)),0)","v":0},{"$f":"IF(AF286=3,IF($AF$2=2,(S286/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I286,Refurb_Poss_Tbl[%]))*AG286,IF($AF$2=3,(S286*AG286)-AX286,S286*AG286)),0)","v":0},{"$f":"IF($AF286=3,IF($AF$2=2,(T286/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I286,Refurb_Poss_Tbl[%]))*AG286,T286*$AG286),0)","v":0},{"$f":"IF($AF286=3,IF($AF$2=2,(Q286/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I286,Refurb_Poss_Tbl[%]))*AG286,Q286*$AG286),0)","v":0},{"$f":"IF($AF286=3,IF($AF$2=2,(U286/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I286,Refurb_Poss_Tbl[%]))*AG286,U286*$AG286),0)","v":0},{"$f":"IF($AF286=3,IF($AF$2=2,(V286/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I286,Refurb_Poss_Tbl[%]))*AG286,IF($AF$2=3,(V286*AG286)-AW286,V286*AG286)),0)","v":0},{"$f":"IF($AF286=3,IF($AF$2=2,(W286/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I286,Refurb_Poss_Tbl[%]))*AG286,W286*$AG286),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,83,0,{"$f":"VLOOKUP(AE287,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12880098149980332},0,0,0,0,0,0,0,0,7.0888889477834123E-3,{"$f":"IF(OR(AF287=3,AF287=2,AF287=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D287,FlatMaint!$Y$2:$Y$10000,AE287)*AG287,0)","v":11.408583922577325},{"$f":"IF(OR(AF287=3,AF287=2,AF287=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D287,FlatRepair!$Y$2:$Y$10000,AE287)*AG287,0)","v":0},0,11.415672811525109,0,0,0,0,0,11.415672811525109,0,{"$f":"IF($AF287=3,IF($AF$2=2,(R287/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I287,Refurb_Poss_Tbl[%]))*AG287,IF($AF$2=3,(R287*AG287)-AV287,R287*AG287)),0)","v":0},{"$f":"IF(AF287=3,IF($AF$2=2,(S287/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I287,Refurb_Poss_Tbl[%]))*AG287,IF($AF$2=3,(S287*AG287)-AX287,S287*AG287)),0)","v":0},{"$f":"IF($AF287=3,IF($AF$2=2,(T287/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I287,Refurb_Poss_Tbl[%]))*AG287,T287*$AG287),0)","v":0},{"$f":"IF($AF287=3,IF($AF$2=2,(Q287/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I287,Refurb_Poss_Tbl[%]))*AG287,Q287*$AG287),0)","v":0},{"$f":"IF($AF287=3,IF($AF$2=2,(U287/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I287,Refurb_Poss_Tbl[%]))*AG287,U287*$AG287),0)","v":0},{"$f":"IF($AF287=3,IF($AF$2=2,(V287/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I287,Refurb_Poss_Tbl[%]))*AG287,IF($AF$2=3,(V287*AG287)-AW287,V287*AG287)),0)","v":0},{"$f":"IF($AF287=3,IF($AF$2=2,(W287/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I287,Refurb_Poss_Tbl[%]))*AG287,W287*$AG287),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,84,0,{"$f":"VLOOKUP(AE288,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1256594941461496},0,0,0,0,0,0,0,0,6.9159892173496721E-3,{"$f":"IF(OR(AF288=3,AF288=2,AF288=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D288,FlatMaint!$Y$2:$Y$10000,AE288)*AG288,0)","v":11.130325778124222},{"$f":"IF(OR(AF288=3,AF288=2,AF288=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D288,FlatRepair!$Y$2:$Y$10000,AE288)*AG288,0)","v":11.130325778124222},0,22.267567545465795,0,0,0,0,0,22.267567545465795,0,{"$f":"IF($AF288=3,IF($AF$2=2,(R288/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I288,Refurb_Poss_Tbl[%]))*AG288,IF($AF$2=3,(R288*AG288)-AV288,R288*AG288)),0)","v":0},{"$f":"IF(AF288=3,IF($AF$2=2,(S288/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I288,Refurb_Poss_Tbl[%]))*AG288,IF($AF$2=3,(S288*AG288)-AX288,S288*AG288)),0)","v":0},{"$f":"IF($AF288=3,IF($AF$2=2,(T288/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I288,Refurb_Poss_Tbl[%]))*AG288,T288*$AG288),0)","v":0},{"$f":"IF($AF288=3,IF($AF$2=2,(Q288/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I288,Refurb_Poss_Tbl[%]))*AG288,Q288*$AG288),0)","v":0},{"$f":"IF($AF288=3,IF($AF$2=2,(U288/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I288,Refurb_Poss_Tbl[%]))*AG288,U288*$AG288),0)","v":0},{"$f":"IF($AF288=3,IF($AF$2=2,(V288/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I288,Refurb_Poss_Tbl[%]))*AG288,IF($AF$2=3,(V288*AG288)-AW288,V288*AG288)),0)","v":0},{"$f":"IF($AF288=3,IF($AF$2=2,(W288/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I288,Refurb_Poss_Tbl[%]))*AG288,W288*$AG288),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,85,0,{"$f":"VLOOKUP(AE289,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1225946284352679},0,0,0,0,0,0,0,0,6.747306553511875E-3,{"$f":"IF(OR(AF289=3,AF289=2,AF289=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D289,FlatMaint!$Y$2:$Y$10000,AE289)*AG289,0)","v":10.858854417682167},{"$f":"IF(OR(AF289=3,AF289=2,AF289=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D289,FlatRepair!$Y$2:$Y$10000,AE289)*AG289,0)","v":0},0,10.865601724235679,0,0,0,0,0,10.865601724235679,0,{"$f":"IF($AF289=3,IF($AF$2=2,(R289/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I289,Refurb_Poss_Tbl[%]))*AG289,IF($AF$2=3,(R289*AG289)-AV289,R289*AG289)),0)","v":0},{"$f":"IF(AF289=3,IF($AF$2=2,(S289/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I289,Refurb_Poss_Tbl[%]))*AG289,IF($AF$2=3,(S289*AG289)-AX289,S289*AG289)),0)","v":0},{"$f":"IF($AF289=3,IF($AF$2=2,(T289/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I289,Refurb_Poss_Tbl[%]))*AG289,T289*$AG289),0)","v":0},{"$f":"IF($AF289=3,IF($AF$2=2,(Q289/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I289,Refurb_Poss_Tbl[%]))*AG289,Q289*$AG289),0)","v":0},{"$f":"IF($AF289=3,IF($AF$2=2,(U289/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I289,Refurb_Poss_Tbl[%]))*AG289,U289*$AG289),0)","v":0},{"$f":"IF($AF289=3,IF($AF$2=2,(V289/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I289,Refurb_Poss_Tbl[%]))*AG289,IF($AF$2=3,(V289*AG289)-AW289,V289*AG289)),0)","v":0},{"$f":"IF($AF289=3,IF($AF$2=2,(W289/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I289,Refurb_Poss_Tbl[%]))*AG289,W289*$AG289),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,86,0,{"$f":"VLOOKUP(AE290,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11960451554660284},0,0,0,0,0,0,0,0,6.5827381009871955E-3,{"$f":"IF(OR(AF290=3,AF290=2,AF290=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D290,FlatMaint!$Y$2:$Y$10000,AE290)*AG290,0)","v":10.594004309933823},{"$f":"IF(OR(AF290=3,AF290=2,AF290=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D290,FlatRepair!$Y$2:$Y$10000,AE290)*AG290,0)","v":10.594004309933823},0,21.194591357968633,0,0,0,0,0,21.194591357968633,0,{"$f":"IF($AF290=3,IF($AF$2=2,(R290/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I290,Refurb_Poss_Tbl[%]))*AG290,IF($AF$2=3,(R290*AG290)-AV290,R290*AG290)),0)","v":0},{"$f":"IF(AF290=3,IF($AF$2=2,(S290/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I290,Refurb_Poss_Tbl[%]))*AG290,IF($AF$2=3,(S290*AG290)-AX290,S290*AG290)),0)","v":0},{"$f":"IF($AF290=3,IF($AF$2=2,(T290/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I290,Refurb_Poss_Tbl[%]))*AG290,T290*$AG290),0)","v":0},{"$f":"IF($AF290=3,IF($AF$2=2,(Q290/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I290,Refurb_Poss_Tbl[%]))*AG290,Q290*$AG290),0)","v":0},{"$f":"IF($AF290=3,IF($AF$2=2,(U290/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I290,Refurb_Poss_Tbl[%]))*AG290,U290*$AG290),0)","v":0},{"$f":"IF($AF290=3,IF($AF$2=2,(V290/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I290,Refurb_Poss_Tbl[%]))*AG290,IF($AF$2=3,(V290*AG290)-AW290,V290*AG290)),0)","v":0},{"$f":"IF($AF290=3,IF($AF$2=2,(W290/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I290,Refurb_Poss_Tbl[%]))*AG290,W290*$AG290),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,87,0,{"$f":"VLOOKUP(AE291,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11668733224058814},0,0,0,0,0,0,0,0,6.4221835131582396E-3,{"$f":"IF(OR(AF291=3,AF291=2,AF291=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D291,FlatMaint!$Y$2:$Y$10000,AE291)*AG291,0)","v":10.335613960911047},{"$f":"IF(OR(AF291=3,AF291=2,AF291=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D291,FlatRepair!$Y$2:$Y$10000,AE291)*AG291,0)","v":0},0,10.342036144424206,0,0,0,0,0,10.342036144424206,0,{"$f":"IF($AF291=3,IF($AF$2=2,(R291/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I291,Refurb_Poss_Tbl[%]))*AG291,IF($AF$2=3,(R291*AG291)-AV291,R291*AG291)),0)","v":0},{"$f":"IF(AF291=3,IF($AF$2=2,(S291/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I291,Refurb_Poss_Tbl[%]))*AG291,IF($AF$2=3,(S291*AG291)-AX291,S291*AG291)),0)","v":0},{"$f":"IF($AF291=3,IF($AF$2=2,(T291/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I291,Refurb_Poss_Tbl[%]))*AG291,T291*$AG291),0)","v":0},{"$f":"IF($AF291=3,IF($AF$2=2,(Q291/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I291,Refurb_Poss_Tbl[%]))*AG291,Q291*$AG291),0)","v":0},{"$f":"IF($AF291=3,IF($AF$2=2,(U291/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I291,Refurb_Poss_Tbl[%]))*AG291,U291*$AG291),0)","v":0},{"$f":"IF($AF291=3,IF($AF$2=2,(V291/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I291,Refurb_Poss_Tbl[%]))*AG291,IF($AF$2=3,(V291*AG291)-AW291,V291*AG291)),0)","v":0},{"$f":"IF($AF291=3,IF($AF$2=2,(W291/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I291,Refurb_Poss_Tbl[%]))*AG291,W291*$AG291),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,88,0,{"$f":"VLOOKUP(AE292,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11384129974691526},0,0,0,0,0,0,0,0,6.2655448908860876E-3,{"$f":"IF(OR(AF292=3,AF292=2,AF292=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D292,FlatMaint!$Y$2:$Y$10000,AE292)*AG292,0)","v":10.083525815522973},{"$f":"IF(OR(AF292=3,AF292=2,AF292=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D292,FlatRepair!$Y$2:$Y$10000,AE292)*AG292,0)","v":10.083525815522973},0,20.17331717593683,0,0,0,0,0,20.17331717593683,0,{"$f":"IF($AF292=3,IF($AF$2=2,(R292/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I292,Refurb_Poss_Tbl[%]))*AG292,IF($AF$2=3,(R292*AG292)-AV292,R292*AG292)),0)","v":0},{"$f":"IF(AF292=3,IF($AF$2=2,(S292/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I292,Refurb_Poss_Tbl[%]))*AG292,IF($AF$2=3,(S292*AG292)-AX292,S292*AG292)),0)","v":0},{"$f":"IF($AF292=3,IF($AF$2=2,(T292/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I292,Refurb_Poss_Tbl[%]))*AG292,T292*$AG292),0)","v":0},{"$f":"IF($AF292=3,IF($AF$2=2,(Q292/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I292,Refurb_Poss_Tbl[%]))*AG292,Q292*$AG292),0)","v":0},{"$f":"IF($AF292=3,IF($AF$2=2,(U292/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I292,Refurb_Poss_Tbl[%]))*AG292,U292*$AG292),0)","v":0},{"$f":"IF($AF292=3,IF($AF$2=2,(V292/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I292,Refurb_Poss_Tbl[%]))*AG292,IF($AF$2=3,(V292*AG292)-AW292,V292*AG292)),0)","v":0},{"$f":"IF($AF292=3,IF($AF$2=2,(W292/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I292,Refurb_Poss_Tbl[%]))*AG292,W292*$AG292),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,89,0,{"$f":"VLOOKUP(AE293,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11106468267991736},0,0,0,0,0,0,0,0,6.1127267228156968E-3,{"$f":"IF(OR(AF293=3,AF293=2,AF293=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D293,FlatMaint!$Y$2:$Y$10000,AE293)*AG293,0)","v":9.8375861614858291},{"$f":"IF(OR(AF293=3,AF293=2,AF293=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D293,FlatRepair!$Y$2:$Y$10000,AE293)*AG293,0)","v":0},0,9.8436988882086442,0,0,0,0,0,9.8436988882086442,0,{"$f":"IF($AF293=3,IF($AF$2=2,(R293/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I293,Refurb_Poss_Tbl[%]))*AG293,IF($AF$2=3,(R293*AG293)-AV293,R293*AG293)),0)","v":0},{"$f":"IF(AF293=3,IF($AF$2=2,(S293/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I293,Refurb_Poss_Tbl[%]))*AG293,IF($AF$2=3,(S293*AG293)-AX293,S293*AG293)),0)","v":0},{"$f":"IF($AF293=3,IF($AF$2=2,(T293/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I293,Refurb_Poss_Tbl[%]))*AG293,T293*$AG293),0)","v":0},{"$f":"IF($AF293=3,IF($AF$2=2,(Q293/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I293,Refurb_Poss_Tbl[%]))*AG293,Q293*$AG293),0)","v":0},{"$f":"IF($AF293=3,IF($AF$2=2,(U293/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I293,Refurb_Poss_Tbl[%]))*AG293,U293*$AG293),0)","v":0},{"$f":"IF($AF293=3,IF($AF$2=2,(V293/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I293,Refurb_Poss_Tbl[%]))*AG293,IF($AF$2=3,(V293*AG293)-AW293,V293*AG293)),0)","v":0},{"$f":"IF($AF293=3,IF($AF$2=2,(W293/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I293,Refurb_Poss_Tbl[%]))*AG293,W293*$AG293),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,90,0,{"$f":"VLOOKUP(AE294,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10835578798040717},0,0,0,0,0,0,0,0,5.963635827137265E-3,{"$f":"IF(OR(AF294=3,AF294=2,AF294=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D294,FlatMaint!$Y$2:$Y$10000,AE294)*AG294,0)","v":9.5976450355959315},{"$f":"IF(OR(AF294=3,AF294=2,AF294=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D294,FlatRepair!$Y$2:$Y$10000,AE294)*AG294,0)","v":9.5976450355959315},0,19.201253707018999,0,0,0,0,0,19.201253707018999,0,{"$f":"IF($AF294=3,IF($AF$2=2,(R294/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I294,Refurb_Poss_Tbl[%]))*AG294,IF($AF$2=3,(R294*AG294)-AV294,R294*AG294)),0)","v":0},{"$f":"IF(AF294=3,IF($AF$2=2,(S294/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I294,Refurb_Poss_Tbl[%]))*AG294,IF($AF$2=3,(S294*AG294)-AX294,S294*AG294)),0)","v":0},{"$f":"IF($AF294=3,IF($AF$2=2,(T294/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I294,Refurb_Poss_Tbl[%]))*AG294,T294*$AG294),0)","v":0},{"$f":"IF($AF294=3,IF($AF$2=2,(Q294/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I294,Refurb_Poss_Tbl[%]))*AG294,Q294*$AG294),0)","v":0},{"$f":"IF($AF294=3,IF($AF$2=2,(U294/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I294,Refurb_Poss_Tbl[%]))*AG294,U294*$AG294),0)","v":0},{"$f":"IF($AF294=3,IF($AF$2=2,(V294/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I294,Refurb_Poss_Tbl[%]))*AG294,IF($AF$2=3,(V294*AG294)-AW294,V294*AG294)),0)","v":0},{"$f":"IF($AF294=3,IF($AF$2=2,(W294/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I294,Refurb_Poss_Tbl[%]))*AG294,W294*$AG294),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,91,0,{"$f":"VLOOKUP(AE295,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10571296388332406},0,0,0,0,0,0,0,0,5.8181812947680628E-3,{"$f":"IF(OR(AF295=3,AF295=2,AF295=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D295,FlatMaint!$Y$2:$Y$10000,AE295)*AG295,0)","v":9.3635561322887124},{"$f":"IF(OR(AF295=3,AF295=2,AF295=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D295,FlatRepair!$Y$2:$Y$10000,AE295)*AG295,0)","v":0},0,9.3693743135834797,0,0,0,0,0,9.3693743135834797,0,{"$f":"IF($AF295=3,IF($AF$2=2,(R295/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I295,Refurb_Poss_Tbl[%]))*AG295,IF($AF$2=3,(R295*AG295)-AV295,R295*AG295)),0)","v":0},{"$f":"IF(AF295=3,IF($AF$2=2,(S295/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I295,Refurb_Poss_Tbl[%]))*AG295,IF($AF$2=3,(S295*AG295)-AX295,S295*AG295)),0)","v":0},{"$f":"IF($AF295=3,IF($AF$2=2,(T295/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I295,Refurb_Poss_Tbl[%]))*AG295,T295*$AG295),0)","v":0},{"$f":"IF($AF295=3,IF($AF$2=2,(Q295/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I295,Refurb_Poss_Tbl[%]))*AG295,Q295*$AG295),0)","v":0},{"$f":"IF($AF295=3,IF($AF$2=2,(U295/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I295,Refurb_Poss_Tbl[%]))*AG295,U295*$AG295),0)","v":0},{"$f":"IF($AF295=3,IF($AF$2=2,(V295/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I295,Refurb_Poss_Tbl[%]))*AG295,IF($AF$2=3,(V295*AG295)-AW295,V295*AG295)),0)","v":0},{"$f":"IF($AF295=3,IF($AF$2=2,(W295/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I295,Refurb_Poss_Tbl[%]))*AG295,W295*$AG295),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,92,0,{"$f":"VLOOKUP(AE296,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10313459891056008},0,0,0,0,0,0,0,0,5.6762744339200625E-3,{"$f":"IF(OR(AF296=3,AF296=2,AF296=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D296,FlatMaint!$Y$2:$Y$10000,AE296)*AG296,0)","v":9.1351767144280132},{"$f":"IF(OR(AF296=3,AF296=2,AF296=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D296,FlatRepair!$Y$2:$Y$10000,AE296)*AG296,0)","v":9.1351767144280132},0,18.276029703289947,0,0,0,0,0,18.276029703289947,0,{"$f":"IF($AF296=3,IF($AF$2=2,(R296/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I296,Refurb_Poss_Tbl[%]))*AG296,IF($AF$2=3,(R296*AG296)-AV296,R296*AG296)),0)","v":0},{"$f":"IF(AF296=3,IF($AF$2=2,(S296/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I296,Refurb_Poss_Tbl[%]))*AG296,IF($AF$2=3,(S296*AG296)-AX296,S296*AG296)),0)","v":0},{"$f":"IF($AF296=3,IF($AF$2=2,(T296/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I296,Refurb_Poss_Tbl[%]))*AG296,T296*$AG296),0)","v":0},{"$f":"IF($AF296=3,IF($AF$2=2,(Q296/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I296,Refurb_Poss_Tbl[%]))*AG296,Q296*$AG296),0)","v":0},{"$f":"IF($AF296=3,IF($AF$2=2,(U296/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I296,Refurb_Poss_Tbl[%]))*AG296,U296*$AG296),0)","v":0},{"$f":"IF($AF296=3,IF($AF$2=2,(V296/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I296,Refurb_Poss_Tbl[%]))*AG296,IF($AF$2=3,(V296*AG296)-AW296,V296*AG296)),0)","v":0},{"$f":"IF($AF296=3,IF($AF$2=2,(W296/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I296,Refurb_Poss_Tbl[%]))*AG296,W296*$AG296),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,93,0,{"$f":"VLOOKUP(AE297,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10061912088835129},0,0,0,0,0,0,0,0,5.5378287160195725E-3,{"$f":"IF(OR(AF297=3,AF297=2,AF297=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D297,FlatMaint!$Y$2:$Y$10000,AE297)*AG297,0)","v":8.9123675262712325},{"$f":"IF(OR(AF297=3,AF297=2,AF297=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D297,FlatRepair!$Y$2:$Y$10000,AE297)*AG297,0)","v":0},0,8.9179053549872513,0,0,0,0,0,8.9179053549872513,0,{"$f":"IF($AF297=3,IF($AF$2=2,(R297/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I297,Refurb_Poss_Tbl[%]))*AG297,IF($AF$2=3,(R297*AG297)-AV297,R297*AG297)),0)","v":0},{"$f":"IF(AF297=3,IF($AF$2=2,(S297/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I297,Refurb_Poss_Tbl[%]))*AG297,IF($AF$2=3,(S297*AG297)-AX297,S297*AG297)),0)","v":0},{"$f":"IF($AF297=3,IF($AF$2=2,(T297/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I297,Refurb_Poss_Tbl[%]))*AG297,T297*$AG297),0)","v":0},{"$f":"IF($AF297=3,IF($AF$2=2,(Q297/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I297,Refurb_Poss_Tbl[%]))*AG297,Q297*$AG297),0)","v":0},{"$f":"IF($AF297=3,IF($AF$2=2,(U297/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I297,Refurb_Poss_Tbl[%]))*AG297,U297*$AG297),0)","v":0},{"$f":"IF($AF297=3,IF($AF$2=2,(V297/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I297,Refurb_Poss_Tbl[%]))*AG297,IF($AF$2=3,(V297*AG297)-AW297,V297*AG297)),0)","v":0},{"$f":"IF($AF297=3,IF($AF$2=2,(W297/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I297,Refurb_Poss_Tbl[%]))*AG297,W297*$AG297),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,94,0,{"$f":"VLOOKUP(AE298,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.8164995988635415E-2},0,0,0,0,0,0,0,0,5.4027597229459254E-3,{"$f":"IF(OR(AF298=3,AF298=2,AF298=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D298,FlatMaint!$Y$2:$Y$10000,AE298)*AG298,0)","v":8.6949927085573009},{"$f":"IF(OR(AF298=3,AF298=2,AF298=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D298,FlatRepair!$Y$2:$Y$10000,AE298)*AG298,0)","v":8.6949927085573009},0,17.39538817683755,0,0,0,0,0,17.39538817683755,0,{"$f":"IF($AF298=3,IF($AF$2=2,(R298/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I298,Refurb_Poss_Tbl[%]))*AG298,IF($AF$2=3,(R298*AG298)-AV298,R298*AG298)),0)","v":0},{"$f":"IF(AF298=3,IF($AF$2=2,(S298/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I298,Refurb_Poss_Tbl[%]))*AG298,IF($AF$2=3,(S298*AG298)-AX298,S298*AG298)),0)","v":0},{"$f":"IF($AF298=3,IF($AF$2=2,(T298/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I298,Refurb_Poss_Tbl[%]))*AG298,T298*$AG298),0)","v":0},{"$f":"IF($AF298=3,IF($AF$2=2,(Q298/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I298,Refurb_Poss_Tbl[%]))*AG298,Q298*$AG298),0)","v":0},{"$f":"IF($AF298=3,IF($AF$2=2,(U298/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I298,Refurb_Poss_Tbl[%]))*AG298,U298*$AG298),0)","v":0},{"$f":"IF($AF298=3,IF($AF$2=2,(V298/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I298,Refurb_Poss_Tbl[%]))*AG298,IF($AF$2=3,(V298*AG298)-AW298,V298*AG298)),0)","v":0},{"$f":"IF($AF298=3,IF($AF$2=2,(W298/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I298,Refurb_Poss_Tbl[%]))*AG298,W298*$AG298),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,95,0,{"$f":"VLOOKUP(AE299,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.577072779379063E-2},0,0,0,0,0,0,0,0,5.2709850955569995E-3,{"$f":"IF(OR(AF299=3,AF299=2,AF299=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D299,FlatMaint!$Y$2:$Y$10000,AE299)*AG299,0)","v":8.4829197156656573},{"$f":"IF(OR(AF299=3,AF299=2,AF299=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D299,FlatRepair!$Y$2:$Y$10000,AE299)*AG299,0)","v":0},0,8.4881907007612138,0,0,0,0,0,8.4881907007612138,0,{"$f":"IF($AF299=3,IF($AF$2=2,(R299/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I299,Refurb_Poss_Tbl[%]))*AG299,IF($AF$2=3,(R299*AG299)-AV299,R299*AG299)),0)","v":0},{"$f":"IF(AF299=3,IF($AF$2=2,(S299/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I299,Refurb_Poss_Tbl[%]))*AG299,IF($AF$2=3,(S299*AG299)-AX299,S299*AG299)),0)","v":0},{"$f":"IF($AF299=3,IF($AF$2=2,(T299/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I299,Refurb_Poss_Tbl[%]))*AG299,T299*$AG299),0)","v":0},{"$f":"IF($AF299=3,IF($AF$2=2,(Q299/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I299,Refurb_Poss_Tbl[%]))*AG299,Q299*$AG299),0)","v":0},{"$f":"IF($AF299=3,IF($AF$2=2,(U299/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I299,Refurb_Poss_Tbl[%]))*AG299,U299*$AG299),0)","v":0},{"$f":"IF($AF299=3,IF($AF$2=2,(V299/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I299,Refurb_Poss_Tbl[%]))*AG299,IF($AF$2=3,(V299*AG299)-AW299,V299*AG299)),0)","v":0},{"$f":"IF($AF299=3,IF($AF$2=2,(W299/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I299,Refurb_Poss_Tbl[%]))*AG299,W299*$AG299),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,96,0,{"$f":"VLOOKUP(AE300,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.3434856384185999E-2},0,0,0,0,0,0,0,0,5.1424244834702443E-3,{"$f":"IF(OR(AF300=3,AF300=2,AF300=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D300,FlatMaint!$Y$2:$Y$10000,AE300)*AG300,0)","v":8.2760192347957648},{"$f":"IF(OR(AF300=3,AF300=2,AF300=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D300,FlatRepair!$Y$2:$Y$10000,AE300)*AG300,0)","v":8.2760192347957648},0,16.557180894075,0,0,0,0,0,16.557180894075,0,{"$f":"IF($AF300=3,IF($AF$2=2,(R300/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I300,Refurb_Poss_Tbl[%]))*AG300,IF($AF$2=3,(R300*AG300)-AV300,R300*AG300)),0)","v":0},{"$f":"IF(AF300=3,IF($AF$2=2,(S300/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I300,Refurb_Poss_Tbl[%]))*AG300,IF($AF$2=3,(S300*AG300)-AX300,S300*AG300)),0)","v":0},{"$f":"IF($AF300=3,IF($AF$2=2,(T300/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I300,Refurb_Poss_Tbl[%]))*AG300,T300*$AG300),0)","v":0},{"$f":"IF($AF300=3,IF($AF$2=2,(Q300/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I300,Refurb_Poss_Tbl[%]))*AG300,Q300*$AG300),0)","v":0},{"$f":"IF($AF300=3,IF($AF$2=2,(U300/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I300,Refurb_Poss_Tbl[%]))*AG300,U300*$AG300),0)","v":0},{"$f":"IF($AF300=3,IF($AF$2=2,(V300/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I300,Refurb_Poss_Tbl[%]))*AG300,IF($AF$2=3,(V300*AG300)-AW300,V300*AG300)),0)","v":0},{"$f":"IF($AF300=3,IF($AF$2=2,(W300/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I300,Refurb_Poss_Tbl[%]))*AG300,W300*$AG300),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,97,0,{"$f":"VLOOKUP(AE301,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.1155957447986352E-2},0,0,0,0,0,0,0,0,5.0169994960685312E-3,{"$f":"IF(OR(AF301=3,AF301=2,AF301=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D301,FlatMaint!$Y$2:$Y$10000,AE301)*AG301,0)","v":8.0741651071178211},{"$f":"IF(OR(AF301=3,AF301=2,AF301=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D301,FlatRepair!$Y$2:$Y$10000,AE301)*AG301,0)","v":0},0,8.0791821066138905,0,0,0,0,0,8.0791821066138905,0,{"$f":"IF($AF301=3,IF($AF$2=2,(R301/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I301,Refurb_Poss_Tbl[%]))*AG301,IF($AF$2=3,(R301*AG301)-AV301,R301*AG301)),0)","v":0},{"$f":"IF(AF301=3,IF($AF$2=2,(S301/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I301,Refurb_Poss_Tbl[%]))*AG301,IF($AF$2=3,(S301*AG301)-AX301,S301*AG301)),0)","v":0},{"$f":"IF($AF301=3,IF($AF$2=2,(T301/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I301,Refurb_Poss_Tbl[%]))*AG301,T301*$AG301),0)","v":0},{"$f":"IF($AF301=3,IF($AF$2=2,(Q301/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I301,Refurb_Poss_Tbl[%]))*AG301,Q301*$AG301),0)","v":0},{"$f":"IF($AF301=3,IF($AF$2=2,(U301/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I301,Refurb_Poss_Tbl[%]))*AG301,U301*$AG301),0)","v":0},{"$f":"IF($AF301=3,IF($AF$2=2,(V301/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I301,Refurb_Poss_Tbl[%]))*AG301,IF($AF$2=3,(V301*AG301)-AW301,V301*AG301)),0)","v":0},{"$f":"IF($AF301=3,IF($AF$2=2,(W301/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I301,Refurb_Poss_Tbl[%]))*AG301,W301*$AG301),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,98,0,{"$f":"VLOOKUP(AE302,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.8932641412669614E-2},0,0,0,0,0,0,0,0,4.8946336547010067E-3,{"$f":"IF(OR(AF302=3,AF302=2,AF302=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D302,FlatMaint!$Y$2:$Y$10000,AE302)*AG302,0)","v":7.8772342508466542},{"$f":"IF(OR(AF302=3,AF302=2,AF302=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D302,FlatRepair!$Y$2:$Y$10000,AE302)*AG302,0)","v":7.8772342508466542},0,15.759363135348011,0,0,0,0,0,15.759363135348011,0,{"$f":"IF($AF302=3,IF($AF$2=2,(R302/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I302,Refurb_Poss_Tbl[%]))*AG302,IF($AF$2=3,(R302*AG302)-AV302,R302*AG302)),0)","v":0},{"$f":"IF(AF302=3,IF($AF$2=2,(S302/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I302,Refurb_Poss_Tbl[%]))*AG302,IF($AF$2=3,(S302*AG302)-AX302,S302*AG302)),0)","v":0},{"$f":"IF($AF302=3,IF($AF$2=2,(T302/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I302,Refurb_Poss_Tbl[%]))*AG302,T302*$AG302),0)","v":0},{"$f":"IF($AF302=3,IF($AF$2=2,(Q302/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I302,Refurb_Poss_Tbl[%]))*AG302,Q302*$AG302),0)","v":0},{"$f":"IF($AF302=3,IF($AF$2=2,(U302/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I302,Refurb_Poss_Tbl[%]))*AG302,U302*$AG302),0)","v":0},{"$f":"IF($AF302=3,IF($AF$2=2,(V302/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I302,Refurb_Poss_Tbl[%]))*AG302,IF($AF$2=3,(V302*AG302)-AW302,V302*AG302)),0)","v":0},{"$f":"IF($AF302=3,IF($AF$2=2,(W302/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I302,Refurb_Poss_Tbl[%]))*AG302,W302*$AG302),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,99,0,{"$f":"VLOOKUP(AE303,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.6763552597726459E-2},0,0,0,0,0,0,0,0,4.7752523460497624E-3,{"$f":"IF(OR(AF303=3,AF303=2,AF303=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D303,FlatMaint!$Y$2:$Y$10000,AE303)*AG303,0)","v":7.6851065861918588},{"$f":"IF(OR(AF303=3,AF303=2,AF303=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D303,FlatRepair!$Y$2:$Y$10000,AE303)*AG303,0)","v":0},0,7.6898818385379082,0,0,0,0,0,7.6898818385379082,0,{"$f":"IF($AF303=3,IF($AF$2=2,(R303/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I303,Refurb_Poss_Tbl[%]))*AG303,IF($AF$2=3,(R303*AG303)-AV303,R303*AG303)),0)","v":0},{"$f":"IF(AF303=3,IF($AF$2=2,(S303/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I303,Refurb_Poss_Tbl[%]))*AG303,IF($AF$2=3,(S303*AG303)-AX303,S303*AG303)),0)","v":0},{"$f":"IF($AF303=3,IF($AF$2=2,(T303/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I303,Refurb_Poss_Tbl[%]))*AG303,T303*$AG303),0)","v":0},{"$f":"IF($AF303=3,IF($AF$2=2,(Q303/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I303,Refurb_Poss_Tbl[%]))*AG303,Q303*$AG303),0)","v":0},{"$f":"IF($AF303=3,IF($AF$2=2,(U303/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I303,Refurb_Poss_Tbl[%]))*AG303,U303*$AG303),0)","v":0},{"$f":"IF($AF303=3,IF($AF$2=2,(V303/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I303,Refurb_Poss_Tbl[%]))*AG303,IF($AF$2=3,(V303*AG303)-AW303,V303*AG303)),0)","v":0},{"$f":"IF($AF303=3,IF($AF$2=2,(W303/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I303,Refurb_Poss_Tbl[%]))*AG303,W303*$AG303),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398575000001,4.9141031452561101,0.12975570763236499,5.5251642540174997,0,3.1002867585E-2,896.48640996024096,5.5037538264366699E-2,0,89.648640996024099,0.58905448411500005,6.4877853816182302E-2,2.45705157262806,100,2,{"$f":"VLOOKUP(AE304,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.4647368388025807E-2},0,0,0,0,0,0,0,0,4.6587827766339145E-3,{"$f":"IF(OR(AF304=3,AF304=2,AF304=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D304,FlatMaint!$Y$2:$Y$10000,AE304)*AG304,0)","v":7.4976649621383977},{"$f":"IF(OR(AF304=3,AF304=2,AF304=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D304,FlatRepair!$Y$2:$Y$10000,AE304)*AG304,0)","v":7.4976649621383977},0,14.999988707053429,7.5885215398763251,0,0,0,0,-59.00849555819201,-81.597005805121768,{"$f":"IF($AF304=3,IF($AF$2=2,(R304/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I304,Refurb_Poss_Tbl[%]))*AG304,IF($AF$2=3,(R304*AG304)-AV304,R304*AG304)),0)","v":0},{"$f":"IF(AF304=3,IF($AF$2=2,(S304/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I304,Refurb_Poss_Tbl[%]))*AG304,IF($AF$2=3,(S304*AG304)-AX304,S304*AG304)),0)","v":0},{"$f":"IF($AF304=3,IF($AF$2=2,(T304/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I304,Refurb_Poss_Tbl[%]))*AG304,T304*$AG304),0)","v":0},{"$f":"IF($AF304=3,IF($AF$2=2,(Q304/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I304,Refurb_Poss_Tbl[%]))*AG304,Q304*$AG304),0)","v":0},{"$f":"IF($AF304=3,IF($AF$2=2,(U304/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I304,Refurb_Poss_Tbl[%]))*AG304,U304*$AG304),0)","v":0},{"$f":"IF($AF304=3,IF($AF$2=2,(V304/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I304,Refurb_Poss_Tbl[%]))*AG304,IF($AF$2=3,(V304*AG304)-AW304,V304*AG304)),0)","v":0},{"$f":"IF($AF304=3,IF($AF$2=2,(W304/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I304,Refurb_Poss_Tbl[%]))*AG304,W304*$AG304),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,0,1,{"$f":"VLOOKUP(AE305,ValidationLists!$M$1:$N$102,2,FALSE)","v":1},9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551411,0,{"$f":"IF(OR(AF305=3,AF305=2,AF305=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D305,FlatMaint!$Y$2:$Y$10000,AE305)*AG305,0)","v":0},{"$f":"IF(OR(AF305=3,AF305=2,AF305=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D305,FlatRepair!$Y$2:$Y$10000,AE305)*AG305,0)","v":0},0,0,0,0,0,0,0,10.240910005551411,0,{"$f":"IF($AF305=3,IF($AF$2=2,(R305/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I305,Refurb_Poss_Tbl[%]))*AG305,IF($AF$2=3,(R305*AG305)-AV305,R305*AG305)),0)","v":0},{"$f":"IF(AF305=3,IF($AF$2=2,(S305/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I305,Refurb_Poss_Tbl[%]))*AG305,IF($AF$2=3,(S305*AG305)-AX305,S305*AG305)),0)","v":0},{"$f":"IF($AF305=3,IF($AF$2=2,(T305/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I305,Refurb_Poss_Tbl[%]))*AG305,T305*$AG305),0)","v":0},{"$f":"IF($AF305=3,IF($AF$2=2,(Q305/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I305,Refurb_Poss_Tbl[%]))*AG305,Q305*$AG305),0)","v":0},{"$f":"IF($AF305=3,IF($AF$2=2,(U305/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I305,Refurb_Poss_Tbl[%]))*AG305,U305*$AG305),0)","v":0},{"$f":"IF($AF305=3,IF($AF$2=2,(V305/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I305,Refurb_Poss_Tbl[%]))*AG305,IF($AF$2=3,(V305*AG305)-AW305,V305*AG305)),0)","v":0},{"$f":"IF($AF305=3,IF($AF$2=2,(W305/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I305,Refurb_Poss_Tbl[%]))*AG305,W305*$AG305),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,1,0,{"$f":"VLOOKUP(AE306,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.96618357487922713},0,0,0,0,0,0,0,0,6.0021561570267447E-4,{"$f":"IF(OR(AF306=3,AF306=2,AF306=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D306,FlatMaint!$Y$2:$Y$10000,AE306)*AG306,0)","v":9.6727412154589363},{"$f":"IF(OR(AF306=3,AF306=2,AF306=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D306,FlatRepair!$Y$2:$Y$10000,AE306)*AG306,0)","v":0},0,9.6733414310746397,0,0,0,0,0,9.6733414310746397,0,{"$f":"IF($AF306=3,IF($AF$2=2,(R306/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I306,Refurb_Poss_Tbl[%]))*AG306,IF($AF$2=3,(R306*AG306)-AV306,R306*AG306)),0)","v":0},{"$f":"IF(AF306=3,IF($AF$2=2,(S306/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I306,Refurb_Poss_Tbl[%]))*AG306,IF($AF$2=3,(S306*AG306)-AX306,S306*AG306)),0)","v":0},{"$f":"IF($AF306=3,IF($AF$2=2,(T306/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I306,Refurb_Poss_Tbl[%]))*AG306,T306*$AG306),0)","v":0},{"$f":"IF($AF306=3,IF($AF$2=2,(Q306/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I306,Refurb_Poss_Tbl[%]))*AG306,Q306*$AG306),0)","v":0},{"$f":"IF($AF306=3,IF($AF$2=2,(U306/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I306,Refurb_Poss_Tbl[%]))*AG306,U306*$AG306),0)","v":0},{"$f":"IF($AF306=3,IF($AF$2=2,(V306/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I306,Refurb_Poss_Tbl[%]))*AG306,IF($AF$2=3,(V306*AG306)-AW306,V306*AG306)),0)","v":0},{"$f":"IF($AF306=3,IF($AF$2=2,(W306/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I306,Refurb_Poss_Tbl[%]))*AG306,W306*$AG306),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,2,0,{"$f":"VLOOKUP(AE307,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.93351070036640305},0,0,0,0,0,0,0,0,5.7991846927794638E-4,{"$f":"IF(OR(AF307=3,AF307=2,AF307=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D307,FlatMaint!$Y$2:$Y$10000,AE307)*AG307,0)","v":9.3456436864337551},{"$f":"IF(OR(AF307=3,AF307=2,AF307=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D307,FlatRepair!$Y$2:$Y$10000,AE307)*AG307,0)","v":0},0,9.3462236049030327,0,0,0,0,0,9.3462236049030327,0,{"$f":"IF($AF307=3,IF($AF$2=2,(R307/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I307,Refurb_Poss_Tbl[%]))*AG307,IF($AF$2=3,(R307*AG307)-AV307,R307*AG307)),0)","v":0},{"$f":"IF(AF307=3,IF($AF$2=2,(S307/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I307,Refurb_Poss_Tbl[%]))*AG307,IF($AF$2=3,(S307*AG307)-AX307,S307*AG307)),0)","v":0},{"$f":"IF($AF307=3,IF($AF$2=2,(T307/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I307,Refurb_Poss_Tbl[%]))*AG307,T307*$AG307),0)","v":0},{"$f":"IF($AF307=3,IF($AF$2=2,(Q307/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I307,Refurb_Poss_Tbl[%]))*AG307,Q307*$AG307),0)","v":0},{"$f":"IF($AF307=3,IF($AF$2=2,(U307/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I307,Refurb_Poss_Tbl[%]))*AG307,U307*$AG307),0)","v":0},{"$f":"IF($AF307=3,IF($AF$2=2,(V307/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I307,Refurb_Poss_Tbl[%]))*AG307,IF($AF$2=3,(V307*AG307)-AW307,V307*AG307)),0)","v":0},{"$f":"IF($AF307=3,IF($AF$2=2,(W307/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I307,Refurb_Poss_Tbl[%]))*AG307,W307*$AG307),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,3,0,{"$f":"VLOOKUP(AE308,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.90194270566802237},0,0,0,0,0,0,0,0,5.6030769978545551E-4,{"$f":"IF(OR(AF308=3,AF308=2,AF308=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D308,FlatMaint!$Y$2:$Y$10000,AE308)*AG308,0)","v":9.0296074265060451},{"$f":"IF(OR(AF308=3,AF308=2,AF308=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D308,FlatRepair!$Y$2:$Y$10000,AE308)*AG308,0)","v":0},0,9.0301677342058309,0,0,0,0,0,9.0301677342058309,0,{"$f":"IF($AF308=3,IF($AF$2=2,(R308/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I308,Refurb_Poss_Tbl[%]))*AG308,IF($AF$2=3,(R308*AG308)-AV308,R308*AG308)),0)","v":0},{"$f":"IF(AF308=3,IF($AF$2=2,(S308/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I308,Refurb_Poss_Tbl[%]))*AG308,IF($AF$2=3,(S308*AG308)-AX308,S308*AG308)),0)","v":0},{"$f":"IF($AF308=3,IF($AF$2=2,(T308/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I308,Refurb_Poss_Tbl[%]))*AG308,T308*$AG308),0)","v":0},{"$f":"IF($AF308=3,IF($AF$2=2,(Q308/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I308,Refurb_Poss_Tbl[%]))*AG308,Q308*$AG308),0)","v":0},{"$f":"IF($AF308=3,IF($AF$2=2,(U308/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I308,Refurb_Poss_Tbl[%]))*AG308,U308*$AG308),0)","v":0},{"$f":"IF($AF308=3,IF($AF$2=2,(V308/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I308,Refurb_Poss_Tbl[%]))*AG308,IF($AF$2=3,(V308*AG308)-AW308,V308*AG308)),0)","v":0},{"$f":"IF($AF308=3,IF($AF$2=2,(W308/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I308,Refurb_Poss_Tbl[%]))*AG308,W308*$AG308),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,4,0,{"$f":"VLOOKUP(AE309,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.87144222769857238},0,0,0,0,0,0,0,0,5.413600964110681E-4,{"$f":"IF(OR(AF309=3,AF309=2,AF309=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D309,FlatMaint!$Y$2:$Y$10000,AE309)*AG309,0)","v":8.7242583830976272},{"$f":"IF(OR(AF309=3,AF309=2,AF309=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D309,FlatRepair!$Y$2:$Y$10000,AE309)*AG309,0)","v":0},0,8.7247997431940387,0,0,0,0,0,8.7247997431940387,0,{"$f":"IF($AF309=3,IF($AF$2=2,(R309/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I309,Refurb_Poss_Tbl[%]))*AG309,IF($AF$2=3,(R309*AG309)-AV309,R309*AG309)),0)","v":0},{"$f":"IF(AF309=3,IF($AF$2=2,(S309/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I309,Refurb_Poss_Tbl[%]))*AG309,IF($AF$2=3,(S309*AG309)-AX309,S309*AG309)),0)","v":0},{"$f":"IF($AF309=3,IF($AF$2=2,(T309/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I309,Refurb_Poss_Tbl[%]))*AG309,T309*$AG309),0)","v":0},{"$f":"IF($AF309=3,IF($AF$2=2,(Q309/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I309,Refurb_Poss_Tbl[%]))*AG309,Q309*$AG309),0)","v":0},{"$f":"IF($AF309=3,IF($AF$2=2,(U309/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I309,Refurb_Poss_Tbl[%]))*AG309,U309*$AG309),0)","v":0},{"$f":"IF($AF309=3,IF($AF$2=2,(V309/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I309,Refurb_Poss_Tbl[%]))*AG309,IF($AF$2=3,(V309*AG309)-AW309,V309*AG309)),0)","v":0},{"$f":"IF($AF309=3,IF($AF$2=2,(W309/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I309,Refurb_Poss_Tbl[%]))*AG309,W309*$AG309),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,5,0,{"$f":"VLOOKUP(AE310,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.84197316685852419},0,0,0,0,0,0,0,0,5.230532332474089E-4,{"$f":"IF(OR(AF310=3,AF310=2,AF310=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D310,FlatMaint!$Y$2:$Y$10000,AE310)*AG310,0)","v":8.4292351527513336},{"$f":"IF(OR(AF310=3,AF310=2,AF310=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D310,FlatRepair!$Y$2:$Y$10000,AE310)*AG310,0)","v":0},0,8.4297582059845801,0,0,0,0,0,8.4297582059845801,0,{"$f":"IF($AF310=3,IF($AF$2=2,(R310/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I310,Refurb_Poss_Tbl[%]))*AG310,IF($AF$2=3,(R310*AG310)-AV310,R310*AG310)),0)","v":0},{"$f":"IF(AF310=3,IF($AF$2=2,(S310/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I310,Refurb_Poss_Tbl[%]))*AG310,IF($AF$2=3,(S310*AG310)-AX310,S310*AG310)),0)","v":0},{"$f":"IF($AF310=3,IF($AF$2=2,(T310/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I310,Refurb_Poss_Tbl[%]))*AG310,T310*$AG310),0)","v":0},{"$f":"IF($AF310=3,IF($AF$2=2,(Q310/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I310,Refurb_Poss_Tbl[%]))*AG310,Q310*$AG310),0)","v":0},{"$f":"IF($AF310=3,IF($AF$2=2,(U310/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I310,Refurb_Poss_Tbl[%]))*AG310,U310*$AG310),0)","v":0},{"$f":"IF($AF310=3,IF($AF$2=2,(V310/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I310,Refurb_Poss_Tbl[%]))*AG310,IF($AF$2=3,(V310*AG310)-AW310,V310*AG310)),0)","v":0},{"$f":"IF($AF310=3,IF($AF$2=2,(W310/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I310,Refurb_Poss_Tbl[%]))*AG310,W310*$AG310),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,6,0,{"$f":"VLOOKUP(AE311,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.81350064430775282},0,0,0,0,0,0,0,0,5.0536544275111965E-4,{"$f":"IF(OR(AF311=3,AF311=2,AF311=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D311,FlatMaint!$Y$2:$Y$10000,AE311)*AG311,0)","v":8.1441885533829304},{"$f":"IF(OR(AF311=3,AF311=2,AF311=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D311,FlatRepair!$Y$2:$Y$10000,AE311)*AG311,0)","v":0},0,8.1446939188256806,0,0,0,0,0,8.1446939188256806,0,{"$f":"IF($AF311=3,IF($AF$2=2,(R311/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I311,Refurb_Poss_Tbl[%]))*AG311,IF($AF$2=3,(R311*AG311)-AV311,R311*AG311)),0)","v":0},{"$f":"IF(AF311=3,IF($AF$2=2,(S311/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I311,Refurb_Poss_Tbl[%]))*AG311,IF($AF$2=3,(S311*AG311)-AX311,S311*AG311)),0)","v":0},{"$f":"IF($AF311=3,IF($AF$2=2,(T311/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I311,Refurb_Poss_Tbl[%]))*AG311,T311*$AG311),0)","v":0},{"$f":"IF($AF311=3,IF($AF$2=2,(Q311/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I311,Refurb_Poss_Tbl[%]))*AG311,Q311*$AG311),0)","v":0},{"$f":"IF($AF311=3,IF($AF$2=2,(U311/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I311,Refurb_Poss_Tbl[%]))*AG311,U311*$AG311),0)","v":0},{"$f":"IF($AF311=3,IF($AF$2=2,(V311/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I311,Refurb_Poss_Tbl[%]))*AG311,IF($AF$2=3,(V311*AG311)-AW311,V311*AG311)),0)","v":0},{"$f":"IF($AF311=3,IF($AF$2=2,(W311/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I311,Refurb_Poss_Tbl[%]))*AG311,W311*$AG311),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,7,0,{"$f":"VLOOKUP(AE312,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.78599096068381913},0,0,0,0,0,0,0,0,4.8827579009770019E-4,{"$f":"IF(OR(AF312=3,AF312=2,AF312=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D312,FlatMaint!$Y$2:$Y$10000,AE312)*AG312,0)","v":7.8687812109979998},{"$f":"IF(OR(AF312=3,AF312=2,AF312=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D312,FlatRepair!$Y$2:$Y$10000,AE312)*AG312,0)","v":0},0,7.8692694867880979,0,0,0,0,0,7.8692694867880979,0,{"$f":"IF($AF312=3,IF($AF$2=2,(R312/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I312,Refurb_Poss_Tbl[%]))*AG312,IF($AF$2=3,(R312*AG312)-AV312,R312*AG312)),0)","v":0},{"$f":"IF(AF312=3,IF($AF$2=2,(S312/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I312,Refurb_Poss_Tbl[%]))*AG312,IF($AF$2=3,(S312*AG312)-AX312,S312*AG312)),0)","v":0},{"$f":"IF($AF312=3,IF($AF$2=2,(T312/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I312,Refurb_Poss_Tbl[%]))*AG312,T312*$AG312),0)","v":0},{"$f":"IF($AF312=3,IF($AF$2=2,(Q312/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I312,Refurb_Poss_Tbl[%]))*AG312,Q312*$AG312),0)","v":0},{"$f":"IF($AF312=3,IF($AF$2=2,(U312/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I312,Refurb_Poss_Tbl[%]))*AG312,U312*$AG312),0)","v":0},{"$f":"IF($AF312=3,IF($AF$2=2,(V312/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I312,Refurb_Poss_Tbl[%]))*AG312,IF($AF$2=3,(V312*AG312)-AW312,V312*AG312)),0)","v":0},{"$f":"IF($AF312=3,IF($AF$2=2,(W312/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I312,Refurb_Poss_Tbl[%]))*AG312,W312*$AG312),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,8,0,{"$f":"VLOOKUP(AE313,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.75941155621625056},0,0,0,0,0,0,0,0,4.7176404840357515E-4,{"$f":"IF(OR(AF313=3,AF313=2,AF313=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D313,FlatMaint!$Y$2:$Y$10000,AE313)*AG313,0)","v":7.6026871603845434},{"$f":"IF(OR(AF313=3,AF313=2,AF313=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D313,FlatRepair!$Y$2:$Y$10000,AE313)*AG313,0)","v":0},0,7.6031589244329467,0,0,0,0,0,7.6031589244329467,0,{"$f":"IF($AF313=3,IF($AF$2=2,(R313/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I313,Refurb_Poss_Tbl[%]))*AG313,IF($AF$2=3,(R313*AG313)-AV313,R313*AG313)),0)","v":0},{"$f":"IF(AF313=3,IF($AF$2=2,(S313/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I313,Refurb_Poss_Tbl[%]))*AG313,IF($AF$2=3,(S313*AG313)-AX313,S313*AG313)),0)","v":0},{"$f":"IF($AF313=3,IF($AF$2=2,(T313/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I313,Refurb_Poss_Tbl[%]))*AG313,T313*$AG313),0)","v":0},{"$f":"IF($AF313=3,IF($AF$2=2,(Q313/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I313,Refurb_Poss_Tbl[%]))*AG313,Q313*$AG313),0)","v":0},{"$f":"IF($AF313=3,IF($AF$2=2,(U313/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I313,Refurb_Poss_Tbl[%]))*AG313,U313*$AG313),0)","v":0},{"$f":"IF($AF313=3,IF($AF$2=2,(V313/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I313,Refurb_Poss_Tbl[%]))*AG313,IF($AF$2=3,(V313*AG313)-AW313,V313*AG313)),0)","v":0},{"$f":"IF($AF313=3,IF($AF$2=2,(W313/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I313,Refurb_Poss_Tbl[%]))*AG313,W313*$AG313),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,9,0,{"$f":"VLOOKUP(AE314,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.73373097218961414},0,0,0,0,0,0,0,0,4.5581067478606298E-4,{"$f":"IF(OR(AF314=3,AF314=2,AF314=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D314,FlatMaint!$Y$2:$Y$10000,AE314)*AG314,0)","v":7.3455914593087375},{"$f":"IF(OR(AF314=3,AF314=2,AF314=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D314,FlatRepair!$Y$2:$Y$10000,AE314)*AG314,0)","v":0},0,7.346047269983524,0,0,0,0,0,7.346047269983524,0,{"$f":"IF($AF314=3,IF($AF$2=2,(R314/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I314,Refurb_Poss_Tbl[%]))*AG314,IF($AF$2=3,(R314*AG314)-AV314,R314*AG314)),0)","v":0},{"$f":"IF(AF314=3,IF($AF$2=2,(S314/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I314,Refurb_Poss_Tbl[%]))*AG314,IF($AF$2=3,(S314*AG314)-AX314,S314*AG314)),0)","v":0},{"$f":"IF($AF314=3,IF($AF$2=2,(T314/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I314,Refurb_Poss_Tbl[%]))*AG314,T314*$AG314),0)","v":0},{"$f":"IF($AF314=3,IF($AF$2=2,(Q314/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I314,Refurb_Poss_Tbl[%]))*AG314,Q314*$AG314),0)","v":0},{"$f":"IF($AF314=3,IF($AF$2=2,(U314/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I314,Refurb_Poss_Tbl[%]))*AG314,U314*$AG314),0)","v":0},{"$f":"IF($AF314=3,IF($AF$2=2,(V314/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I314,Refurb_Poss_Tbl[%]))*AG314,IF($AF$2=3,(V314*AG314)-AW314,V314*AG314)),0)","v":0},{"$f":"IF($AF314=3,IF($AF$2=2,(W314/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I314,Refurb_Poss_Tbl[%]))*AG314,W314*$AG314),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,10,0,{"$f":"VLOOKUP(AE315,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.70891881370977217},0,0,0,0,0,0,0,0,4.4039678723291115E-4,{"$f":"IF(OR(AF315=3,AF315=2,AF315=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D315,FlatMaint!$Y$2:$Y$10000,AE315)*AG315,0)","v":7.0971898157572353},{"$f":"IF(OR(AF315=3,AF315=2,AF315=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D315,FlatRepair!$Y$2:$Y$10000,AE315)*AG315,0)","v":0},0,7.0976302125444679,0,0,0,0,0,7.0976302125444679,0,{"$f":"IF($AF315=3,IF($AF$2=2,(R315/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I315,Refurb_Poss_Tbl[%]))*AG315,IF($AF$2=3,(R315*AG315)-AV315,R315*AG315)),0)","v":0},{"$f":"IF(AF315=3,IF($AF$2=2,(S315/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I315,Refurb_Poss_Tbl[%]))*AG315,IF($AF$2=3,(S315*AG315)-AX315,S315*AG315)),0)","v":0},{"$f":"IF($AF315=3,IF($AF$2=2,(T315/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I315,Refurb_Poss_Tbl[%]))*AG315,T315*$AG315),0)","v":0},{"$f":"IF($AF315=3,IF($AF$2=2,(Q315/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I315,Refurb_Poss_Tbl[%]))*AG315,Q315*$AG315),0)","v":0},{"$f":"IF($AF315=3,IF($AF$2=2,(U315/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I315,Refurb_Poss_Tbl[%]))*AG315,U315*$AG315),0)","v":0},{"$f":"IF($AF315=3,IF($AF$2=2,(V315/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I315,Refurb_Poss_Tbl[%]))*AG315,IF($AF$2=3,(V315*AG315)-AW315,V315*AG315)),0)","v":0},{"$f":"IF($AF315=3,IF($AF$2=2,(W315/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I315,Refurb_Poss_Tbl[%]))*AG315,W315*$AG315),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,11,0,{"$f":"VLOOKUP(AE316,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.68494571372924851},0,0,0,0,0,0,0,0,4.2550414225402046E-4,{"$f":"IF(OR(AF316=3,AF316=2,AF316=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D316,FlatMaint!$Y$2:$Y$10000,AE316)*AG316,0)","v":6.8571882277847687},{"$f":"IF(OR(AF316=3,AF316=2,AF316=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D316,FlatRepair!$Y$2:$Y$10000,AE316)*AG316,0)","v":0},0,6.8576137319270227,0,0,0,0,0,6.8576137319270227,0,{"$f":"IF($AF316=3,IF($AF$2=2,(R316/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I316,Refurb_Poss_Tbl[%]))*AG316,IF($AF$2=3,(R316*AG316)-AV316,R316*AG316)),0)","v":0},{"$f":"IF(AF316=3,IF($AF$2=2,(S316/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I316,Refurb_Poss_Tbl[%]))*AG316,IF($AF$2=3,(S316*AG316)-AX316,S316*AG316)),0)","v":0},{"$f":"IF($AF316=3,IF($AF$2=2,(T316/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I316,Refurb_Poss_Tbl[%]))*AG316,T316*$AG316),0)","v":0},{"$f":"IF($AF316=3,IF($AF$2=2,(Q316/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I316,Refurb_Poss_Tbl[%]))*AG316,Q316*$AG316),0)","v":0},{"$f":"IF($AF316=3,IF($AF$2=2,(U316/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I316,Refurb_Poss_Tbl[%]))*AG316,U316*$AG316),0)","v":0},{"$f":"IF($AF316=3,IF($AF$2=2,(V316/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I316,Refurb_Poss_Tbl[%]))*AG316,IF($AF$2=3,(V316*AG316)-AW316,V316*AG316)),0)","v":0},{"$f":"IF($AF316=3,IF($AF$2=2,(W316/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I316,Refurb_Poss_Tbl[%]))*AG316,W316*$AG316),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,12,0,{"$f":"VLOOKUP(AE317,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.66178329828912896},0,0,0,0,0,0,0,0,4.1111511328890862E-4,{"$f":"IF(OR(AF317=3,AF317=2,AF317=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D317,FlatMaint!$Y$2:$Y$10000,AE317)*AG317,0)","v":6.6253026355408391},{"$f":"IF(OR(AF317=3,AF317=2,AF317=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D317,FlatRepair!$Y$2:$Y$10000,AE317)*AG317,0)","v":0},0,6.6257137506541284,0,0,0,0,0,6.6257137506541284,0,{"$f":"IF($AF317=3,IF($AF$2=2,(R317/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I317,Refurb_Poss_Tbl[%]))*AG317,IF($AF$2=3,(R317*AG317)-AV317,R317*AG317)),0)","v":0},{"$f":"IF(AF317=3,IF($AF$2=2,(S317/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I317,Refurb_Poss_Tbl[%]))*AG317,IF($AF$2=3,(S317*AG317)-AX317,S317*AG317)),0)","v":0},{"$f":"IF($AF317=3,IF($AF$2=2,(T317/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I317,Refurb_Poss_Tbl[%]))*AG317,T317*$AG317),0)","v":0},{"$f":"IF($AF317=3,IF($AF$2=2,(Q317/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I317,Refurb_Poss_Tbl[%]))*AG317,Q317*$AG317),0)","v":0},{"$f":"IF($AF317=3,IF($AF$2=2,(U317/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I317,Refurb_Poss_Tbl[%]))*AG317,U317*$AG317),0)","v":0},{"$f":"IF($AF317=3,IF($AF$2=2,(V317/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I317,Refurb_Poss_Tbl[%]))*AG317,IF($AF$2=3,(V317*AG317)-AW317,V317*AG317)),0)","v":0},{"$f":"IF($AF317=3,IF($AF$2=2,(W317/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I317,Refurb_Poss_Tbl[%]))*AG317,W317*$AG317),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,13,0,{"$f":"VLOOKUP(AE318,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.63940415293635666},0,0,0,0,0,0,0,0,3.9721266984435628E-4,{"$f":"IF(OR(AF318=3,AF318=2,AF318=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D318,FlatMaint!$Y$2:$Y$10000,AE318)*AG318,0)","v":6.4012585850636139},{"$f":"IF(OR(AF318=3,AF318=2,AF318=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D318,FlatRepair!$Y$2:$Y$10000,AE318)*AG318,0)","v":0},0,6.4016557977334578,0,0,0,0,0,6.4016557977334578,0,{"$f":"IF($AF318=3,IF($AF$2=2,(R318/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I318,Refurb_Poss_Tbl[%]))*AG318,IF($AF$2=3,(R318*AG318)-AV318,R318*AG318)),0)","v":0},{"$f":"IF(AF318=3,IF($AF$2=2,(S318/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I318,Refurb_Poss_Tbl[%]))*AG318,IF($AF$2=3,(S318*AG318)-AX318,S318*AG318)),0)","v":0},{"$f":"IF($AF318=3,IF($AF$2=2,(T318/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I318,Refurb_Poss_Tbl[%]))*AG318,T318*$AG318),0)","v":0},{"$f":"IF($AF318=3,IF($AF$2=2,(Q318/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I318,Refurb_Poss_Tbl[%]))*AG318,Q318*$AG318),0)","v":0},{"$f":"IF($AF318=3,IF($AF$2=2,(U318/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I318,Refurb_Poss_Tbl[%]))*AG318,U318*$AG318),0)","v":0},{"$f":"IF($AF318=3,IF($AF$2=2,(V318/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I318,Refurb_Poss_Tbl[%]))*AG318,IF($AF$2=3,(V318*AG318)-AW318,V318*AG318)),0)","v":0},{"$f":"IF($AF318=3,IF($AF$2=2,(W318/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I318,Refurb_Poss_Tbl[%]))*AG318,W318*$AG318),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,14,0,{"$f":"VLOOKUP(AE319,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.61778179027667302},0,0,0,0,0,0,0,0,3.8378035733754222E-4,{"$f":"IF(OR(AF319=3,AF319=2,AF319=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D319,FlatMaint!$Y$2:$Y$10000,AE319)*AG319,0)","v":6.1847909034431048},{"$f":"IF(OR(AF319=3,AF319=2,AF319=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D319,FlatRepair!$Y$2:$Y$10000,AE319)*AG319,0)","v":0},0,6.185174683800442,0,0,0,0,0,6.185174683800442,0,{"$f":"IF($AF319=3,IF($AF$2=2,(R319/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I319,Refurb_Poss_Tbl[%]))*AG319,IF($AF$2=3,(R319*AG319)-AV319,R319*AG319)),0)","v":0},{"$f":"IF(AF319=3,IF($AF$2=2,(S319/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I319,Refurb_Poss_Tbl[%]))*AG319,IF($AF$2=3,(S319*AG319)-AX319,S319*AG319)),0)","v":0},{"$f":"IF($AF319=3,IF($AF$2=2,(T319/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I319,Refurb_Poss_Tbl[%]))*AG319,T319*$AG319),0)","v":0},{"$f":"IF($AF319=3,IF($AF$2=2,(Q319/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I319,Refurb_Poss_Tbl[%]))*AG319,Q319*$AG319),0)","v":0},{"$f":"IF($AF319=3,IF($AF$2=2,(U319/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I319,Refurb_Poss_Tbl[%]))*AG319,U319*$AG319),0)","v":0},{"$f":"IF($AF319=3,IF($AF$2=2,(V319/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I319,Refurb_Poss_Tbl[%]))*AG319,IF($AF$2=3,(V319*AG319)-AW319,V319*AG319)),0)","v":0},{"$f":"IF($AF319=3,IF($AF$2=2,(W319/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I319,Refurb_Poss_Tbl[%]))*AG319,W319*$AG319),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,15,0,{"$f":"VLOOKUP(AE320,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.59689061862480497},0,0,0,0,0,0,0,0,3.7080227762081386E-4,{"$f":"IF(OR(AF320=3,AF320=2,AF320=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D320,FlatMaint!$Y$2:$Y$10000,AE320)*AG320,0)","v":5.9756433849691843},{"$f":"IF(OR(AF320=3,AF320=2,AF320=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D320,FlatRepair!$Y$2:$Y$10000,AE320)*AG320,0)","v":0},0,5.9760141872468049,0,0,0,0,0,5.9760141872468049,0,{"$f":"IF($AF320=3,IF($AF$2=2,(R320/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I320,Refurb_Poss_Tbl[%]))*AG320,IF($AF$2=3,(R320*AG320)-AV320,R320*AG320)),0)","v":0},{"$f":"IF(AF320=3,IF($AF$2=2,(S320/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I320,Refurb_Poss_Tbl[%]))*AG320,IF($AF$2=3,(S320*AG320)-AX320,S320*AG320)),0)","v":0},{"$f":"IF($AF320=3,IF($AF$2=2,(T320/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I320,Refurb_Poss_Tbl[%]))*AG320,T320*$AG320),0)","v":0},{"$f":"IF($AF320=3,IF($AF$2=2,(Q320/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I320,Refurb_Poss_Tbl[%]))*AG320,Q320*$AG320),0)","v":0},{"$f":"IF($AF320=3,IF($AF$2=2,(U320/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I320,Refurb_Poss_Tbl[%]))*AG320,U320*$AG320),0)","v":0},{"$f":"IF($AF320=3,IF($AF$2=2,(V320/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I320,Refurb_Poss_Tbl[%]))*AG320,IF($AF$2=3,(V320*AG320)-AW320,V320*AG320)),0)","v":0},{"$f":"IF($AF320=3,IF($AF$2=2,(W320/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I320,Refurb_Poss_Tbl[%]))*AG320,W320*$AG320),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,16,0,{"$f":"VLOOKUP(AE321,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.57670591171478747},0,0,0,0,0,0,0,0,3.5826307016503757E-4,{"$f":"IF(OR(AF321=3,AF321=2,AF321=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D321,FlatMaint!$Y$2:$Y$10000,AE321)*AG321,0)","v":5.7735684878929323},{"$f":"IF(OR(AF321=3,AF321=2,AF321=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D321,FlatRepair!$Y$2:$Y$10000,AE321)*AG321,0)","v":0},0,5.7739267509630974,0,0,0,0,0,5.7739267509630974,0,{"$f":"IF($AF321=3,IF($AF$2=2,(R321/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I321,Refurb_Poss_Tbl[%]))*AG321,IF($AF$2=3,(R321*AG321)-AV321,R321*AG321)),0)","v":0},{"$f":"IF(AF321=3,IF($AF$2=2,(S321/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I321,Refurb_Poss_Tbl[%]))*AG321,IF($AF$2=3,(S321*AG321)-AX321,S321*AG321)),0)","v":0},{"$f":"IF($AF321=3,IF($AF$2=2,(T321/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I321,Refurb_Poss_Tbl[%]))*AG321,T321*$AG321),0)","v":0},{"$f":"IF($AF321=3,IF($AF$2=2,(Q321/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I321,Refurb_Poss_Tbl[%]))*AG321,Q321*$AG321),0)","v":0},{"$f":"IF($AF321=3,IF($AF$2=2,(U321/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I321,Refurb_Poss_Tbl[%]))*AG321,U321*$AG321),0)","v":0},{"$f":"IF($AF321=3,IF($AF$2=2,(V321/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I321,Refurb_Poss_Tbl[%]))*AG321,IF($AF$2=3,(V321*AG321)-AW321,V321*AG321)),0)","v":0},{"$f":"IF($AF321=3,IF($AF$2=2,(W321/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I321,Refurb_Poss_Tbl[%]))*AG321,W321*$AG321),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,17,0,{"$f":"VLOOKUP(AE322,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.55720377943457733},0,0,0,0,0,0,0,0,3.4614789387926341E-4,{"$f":"IF(OR(AF322=3,AF322=2,AF322=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D322,FlatMaint!$Y$2:$Y$10000,AE322)*AG322,0)","v":5.5783270414424475},{"$f":"IF(OR(AF322=3,AF322=2,AF322=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D322,FlatRepair!$Y$2:$Y$10000,AE322)*AG322,0)","v":0},0,5.5786731893363264,0,0,0,0,0,5.5786731893363264,0,{"$f":"IF($AF322=3,IF($AF$2=2,(R322/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I322,Refurb_Poss_Tbl[%]))*AG322,IF($AF$2=3,(R322*AG322)-AV322,R322*AG322)),0)","v":0},{"$f":"IF(AF322=3,IF($AF$2=2,(S322/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I322,Refurb_Poss_Tbl[%]))*AG322,IF($AF$2=3,(S322*AG322)-AX322,S322*AG322)),0)","v":0},{"$f":"IF($AF322=3,IF($AF$2=2,(T322/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I322,Refurb_Poss_Tbl[%]))*AG322,T322*$AG322),0)","v":0},{"$f":"IF($AF322=3,IF($AF$2=2,(Q322/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I322,Refurb_Poss_Tbl[%]))*AG322,Q322*$AG322),0)","v":0},{"$f":"IF($AF322=3,IF($AF$2=2,(U322/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I322,Refurb_Poss_Tbl[%]))*AG322,U322*$AG322),0)","v":0},{"$f":"IF($AF322=3,IF($AF$2=2,(V322/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I322,Refurb_Poss_Tbl[%]))*AG322,IF($AF$2=3,(V322*AG322)-AW322,V322*AG322)),0)","v":0},{"$f":"IF($AF322=3,IF($AF$2=2,(W322/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I322,Refurb_Poss_Tbl[%]))*AG322,W322*$AG322),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,18,0,{"$f":"VLOOKUP(AE323,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.53836113955031628},{"$f":"IF(AE323=0,Q323*AG323,0)","v":0},{"$f":"IF(AE323=0,R323*AG323,0)","v":0},{"$f":"IF(AE323=0,S323*AG323,0)","v":0},{"$f":"IF(AE323=0,T323*AG323,0)","v":0},{"$f":"IF(AE323=0,U323*AG323,0)","v":0},{"$f":"IF(AE323=0,V323*AG323,0)","v":0},{"$f":"IF(AE323=0,W323*AG323,0)","v":0},{"$f":"IF(AE323=0,AH323+AI323+AJ323+AK323+AL323+AM323+AN323,0)","v":0},{"$f":"IF(OR(AF323=3,AF323=2,AF323=0),Y323*AG323,0)","v":3.3444240954518201E-4},{"$f":"IF(OR(AF323=3,AF323=2,AF323=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D323,FlatMaint!$Y$2:$Y$10000,AE323)*AG323,0)","v":5.3896879627463266},{"$f":"IF(OR(AF323=3,AF323=2,AF323=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D323,FlatRepair!$Y$2:$Y$10000,AE323)*AG323,0)","v":0},{"$f":"IF(OR(AF323=3,AF323=2,AF323=0),Z323*AG323,0)","v":0},{"$f":"AP323+AQ323+AR323+AS323","v":5.3900224051558716},{"$f":"IF(AF323=2,AA323*AG323,0)","v":0},{"$f":"IF(AF323=3,AB323*AG323,0)","v":0},{"$f":"IF(AF323=3,AC323*AG323,0)","v":0},{"$f":"IF(AF323=3,AD323*AG323,0)","v":0},{"$f":"IF($AF$2=3,BB323+BC323+BD323+BE323+BF323+BG323+BH323,BB323+BC323+BD323+BE323+BF323+BG323+BH323)","v":0},{"$f":"AO323+AT323+AU323+AV323+AW323+AX323+AY323+BA323","v":5.3900224051558716},{"$f":"IFERROR(IF(AE323=100,IF(O323=3,(N323/H323)*(X323*AG323)*-1,(N323/M323)*(X323*AG323)*-1),0),0)","v":0},{"$f":"IF($AF323=3,IF($AF$2=2,(R323/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I323,Refurb_Poss_Tbl[%]))*AG323,IF($AF$2=3,(R323*AG323)-AV323,R323*AG323)),0)","v":0},{"$f":"IF(AF323=3,IF($AF$2=2,(S323/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I323,Refurb_Poss_Tbl[%]))*AG323,IF($AF$2=3,(S323*AG323)-AX323,S323*AG323)),0)","v":0},{"$f":"IF($AF323=3,IF($AF$2=2,(T323/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I323,Refurb_Poss_Tbl[%]))*AG323,T323*$AG323),0)","v":0},{"$f":"IF($AF323=3,IF($AF$2=2,(Q323/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I323,Refurb_Poss_Tbl[%]))*AG323,Q323*$AG323),0)","v":0},{"$f":"IF($AF323=3,IF($AF$2=2,(U323/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I323,Refurb_Poss_Tbl[%]))*AG323,U323*$AG323),0)","v":0},{"$f":"IF($AF323=3,IF($AF$2=2,(V323/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I323,Refurb_Poss_Tbl[%]))*AG323,IF($AF$2=3,(V323*AG323)-AW323,V323*AG323)),0)","v":0},{"$f":"IF($AF323=3,IF($AF$2=2,(W323/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I323,Refurb_Poss_Tbl[%]))*AG323,W323*$AG323),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,19,0,{"$f":"VLOOKUP(AE324,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.52015569038677911},0,0,0,0,0,0,0,0,3.2313276284558657E-4,{"$f":"IF(OR(AF324=3,AF324=2,AF324=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D324,FlatMaint!$Y$2:$Y$10000,AE324)*AG324,0)","v":5.2074279833297847},{"$f":"IF(OR(AF324=3,AF324=2,AF324=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D324,FlatRepair!$Y$2:$Y$10000,AE324)*AG324,0)","v":0},0,5.2077511160926306,0,0,0,0,0,5.2077511160926306,0,{"$f":"IF($AF324=3,IF($AF$2=2,(R324/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I324,Refurb_Poss_Tbl[%]))*AG324,IF($AF$2=3,(R324*AG324)-AV324,R324*AG324)),0)","v":0},{"$f":"IF(AF324=3,IF($AF$2=2,(S324/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I324,Refurb_Poss_Tbl[%]))*AG324,IF($AF$2=3,(S324*AG324)-AX324,S324*AG324)),0)","v":0},{"$f":"IF($AF324=3,IF($AF$2=2,(T324/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I324,Refurb_Poss_Tbl[%]))*AG324,T324*$AG324),0)","v":0},{"$f":"IF($AF324=3,IF($AF$2=2,(Q324/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I324,Refurb_Poss_Tbl[%]))*AG324,Q324*$AG324),0)","v":0},{"$f":"IF($AF324=3,IF($AF$2=2,(U324/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I324,Refurb_Poss_Tbl[%]))*AG324,U324*$AG324),0)","v":0},{"$f":"IF($AF324=3,IF($AF$2=2,(V324/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I324,Refurb_Poss_Tbl[%]))*AG324,IF($AF$2=3,(V324*AG324)-AW324,V324*AG324)),0)","v":0},{"$f":"IF($AF324=3,IF($AF$2=2,(W324/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I324,Refurb_Poss_Tbl[%]))*AG324,W324*$AG324),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,20,0,{"$f":"VLOOKUP(AE325,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.50256588443167061},0,0,0,0,0,0,0,0,3.1220556796675026E-4,{"$f":"IF(OR(AF325=3,AF325=2,AF325=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D325,FlatMaint!$Y$2:$Y$10000,AE325)*AG325,0)","v":5.031331384859695},{"$f":"IF(OR(AF325=3,AF325=2,AF325=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D325,FlatRepair!$Y$2:$Y$10000,AE325)*AG325,0)","v":0},0,5.0316435904276622,0,0,0,0,0,5.0316435904276622,0,{"$f":"IF($AF325=3,IF($AF$2=2,(R325/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I325,Refurb_Poss_Tbl[%]))*AG325,IF($AF$2=3,(R325*AG325)-AV325,R325*AG325)),0)","v":0},{"$f":"IF(AF325=3,IF($AF$2=2,(S325/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I325,Refurb_Poss_Tbl[%]))*AG325,IF($AF$2=3,(S325*AG325)-AX325,S325*AG325)),0)","v":0},{"$f":"IF($AF325=3,IF($AF$2=2,(T325/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I325,Refurb_Poss_Tbl[%]))*AG325,T325*$AG325),0)","v":0},{"$f":"IF($AF325=3,IF($AF$2=2,(Q325/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I325,Refurb_Poss_Tbl[%]))*AG325,Q325*$AG325),0)","v":0},{"$f":"IF($AF325=3,IF($AF$2=2,(U325/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I325,Refurb_Poss_Tbl[%]))*AG325,U325*$AG325),0)","v":0},{"$f":"IF($AF325=3,IF($AF$2=2,(V325/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I325,Refurb_Poss_Tbl[%]))*AG325,IF($AF$2=3,(V325*AG325)-AW325,V325*AG325)),0)","v":0},{"$f":"IF($AF325=3,IF($AF$2=2,(W325/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I325,Refurb_Poss_Tbl[%]))*AG325,W325*$AG325),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,21,0,{"$f":"VLOOKUP(AE326,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.48557090283253213},0,0,0,0,0,0,0,0,3.0164789175531439E-4,{"$f":"IF(OR(AF326=3,AF326=2,AF326=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D326,FlatMaint!$Y$2:$Y$10000,AE326)*AG326,0)","v":4.8611897438257943},{"$f":"IF(OR(AF326=3,AF326=2,AF326=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D326,FlatRepair!$Y$2:$Y$10000,AE326)*AG326,0)","v":0},0,4.86149139171755,0,0,0,0,0,4.86149139171755,0,{"$f":"IF($AF326=3,IF($AF$2=2,(R326/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I326,Refurb_Poss_Tbl[%]))*AG326,IF($AF$2=3,(R326*AG326)-AV326,R326*AG326)),0)","v":0},{"$f":"IF(AF326=3,IF($AF$2=2,(S326/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I326,Refurb_Poss_Tbl[%]))*AG326,IF($AF$2=3,(S326*AG326)-AX326,S326*AG326)),0)","v":0},{"$f":"IF($AF326=3,IF($AF$2=2,(T326/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I326,Refurb_Poss_Tbl[%]))*AG326,T326*$AG326),0)","v":0},{"$f":"IF($AF326=3,IF($AF$2=2,(Q326/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I326,Refurb_Poss_Tbl[%]))*AG326,Q326*$AG326),0)","v":0},{"$f":"IF($AF326=3,IF($AF$2=2,(U326/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I326,Refurb_Poss_Tbl[%]))*AG326,U326*$AG326),0)","v":0},{"$f":"IF($AF326=3,IF($AF$2=2,(V326/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I326,Refurb_Poss_Tbl[%]))*AG326,IF($AF$2=3,(V326*AG326)-AW326,V326*AG326)),0)","v":0},{"$f":"IF($AF326=3,IF($AF$2=2,(W326/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I326,Refurb_Poss_Tbl[%]))*AG326,W326*$AG326),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,22,0,{"$f":"VLOOKUP(AE327,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.46915063075606966},0,0,0,0,0,0,0,0,2.9144723841093175E-4,{"$f":"IF(OR(AF327=3,AF327=2,AF327=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D327,FlatMaint!$Y$2:$Y$10000,AE327)*AG327,0)","v":4.6968016848558394},{"$f":"IF(OR(AF327=3,AF327=2,AF327=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D327,FlatRepair!$Y$2:$Y$10000,AE327)*AG327,0)","v":0},0,4.6970931320942499,0,0,0,0,0,4.6970931320942499,0,{"$f":"IF($AF327=3,IF($AF$2=2,(R327/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I327,Refurb_Poss_Tbl[%]))*AG327,IF($AF$2=3,(R327*AG327)-AV327,R327*AG327)),0)","v":0},{"$f":"IF(AF327=3,IF($AF$2=2,(S327/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I327,Refurb_Poss_Tbl[%]))*AG327,IF($AF$2=3,(S327*AG327)-AX327,S327*AG327)),0)","v":0},{"$f":"IF($AF327=3,IF($AF$2=2,(T327/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I327,Refurb_Poss_Tbl[%]))*AG327,T327*$AG327),0)","v":0},{"$f":"IF($AF327=3,IF($AF$2=2,(Q327/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I327,Refurb_Poss_Tbl[%]))*AG327,Q327*$AG327),0)","v":0},{"$f":"IF($AF327=3,IF($AF$2=2,(U327/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I327,Refurb_Poss_Tbl[%]))*AG327,U327*$AG327),0)","v":0},{"$f":"IF($AF327=3,IF($AF$2=2,(V327/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I327,Refurb_Poss_Tbl[%]))*AG327,IF($AF$2=3,(V327*AG327)-AW327,V327*AG327)),0)","v":0},{"$f":"IF($AF327=3,IF($AF$2=2,(W327/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I327,Refurb_Poss_Tbl[%]))*AG327,W327*$AG327),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,23,0,{"$f":"VLOOKUP(AE328,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.45328563358074364},0,0,0,0,0,0,0,0,2.8159153469655242E-4,{"$f":"IF(OR(AF328=3,AF328=2,AF328=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D328,FlatMaint!$Y$2:$Y$10000,AE328)*AG328,0)","v":4.5379726423727913},{"$f":"IF(OR(AF328=3,AF328=2,AF328=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D328,FlatRepair!$Y$2:$Y$10000,AE328)*AG328,0)","v":0},0,4.5382542339074883,0,0,0,0,0,4.5382542339074883,0,{"$f":"IF($AF328=3,IF($AF$2=2,(R328/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I328,Refurb_Poss_Tbl[%]))*AG328,IF($AF$2=3,(R328*AG328)-AV328,R328*AG328)),0)","v":0},{"$f":"IF(AF328=3,IF($AF$2=2,(S328/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I328,Refurb_Poss_Tbl[%]))*AG328,IF($AF$2=3,(S328*AG328)-AX328,S328*AG328)),0)","v":0},{"$f":"IF($AF328=3,IF($AF$2=2,(T328/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I328,Refurb_Poss_Tbl[%]))*AG328,T328*$AG328),0)","v":0},{"$f":"IF($AF328=3,IF($AF$2=2,(Q328/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I328,Refurb_Poss_Tbl[%]))*AG328,Q328*$AG328),0)","v":0},{"$f":"IF($AF328=3,IF($AF$2=2,(U328/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I328,Refurb_Poss_Tbl[%]))*AG328,U328*$AG328),0)","v":0},{"$f":"IF($AF328=3,IF($AF$2=2,(V328/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I328,Refurb_Poss_Tbl[%]))*AG328,IF($AF$2=3,(V328*AG328)-AW328,V328*AG328)),0)","v":0},{"$f":"IF($AF328=3,IF($AF$2=2,(W328/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I328,Refurb_Poss_Tbl[%]))*AG328,W328*$AG328),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,24,0,{"$f":"VLOOKUP(AE329,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.43795713389443841},0,0,0,0,0,0,0,0,2.7206911564884299E-4,{"$f":"IF(OR(AF329=3,AF329=2,AF329=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D329,FlatMaint!$Y$2:$Y$10000,AE329)*AG329,0)","v":4.3845146303118767},{"$f":"IF(OR(AF329=3,AF329=2,AF329=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D329,FlatRepair!$Y$2:$Y$10000,AE329)*AG329,0)","v":0},0,4.3847866994275257,0,0,0,0,0,4.3847866994275257,0,{"$f":"IF($AF329=3,IF($AF$2=2,(R329/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I329,Refurb_Poss_Tbl[%]))*AG329,IF($AF$2=3,(R329*AG329)-AV329,R329*AG329)),0)","v":0},{"$f":"IF(AF329=3,IF($AF$2=2,(S329/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I329,Refurb_Poss_Tbl[%]))*AG329,IF($AF$2=3,(S329*AG329)-AX329,S329*AG329)),0)","v":0},{"$f":"IF($AF329=3,IF($AF$2=2,(T329/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I329,Refurb_Poss_Tbl[%]))*AG329,T329*$AG329),0)","v":0},{"$f":"IF($AF329=3,IF($AF$2=2,(Q329/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I329,Refurb_Poss_Tbl[%]))*AG329,Q329*$AG329),0)","v":0},{"$f":"IF($AF329=3,IF($AF$2=2,(U329/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I329,Refurb_Poss_Tbl[%]))*AG329,U329*$AG329),0)","v":0},{"$f":"IF($AF329=3,IF($AF$2=2,(V329/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I329,Refurb_Poss_Tbl[%]))*AG329,IF($AF$2=3,(V329*AG329)-AW329,V329*AG329)),0)","v":0},{"$f":"IF($AF329=3,IF($AF$2=2,(W329/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I329,Refurb_Poss_Tbl[%]))*AG329,W329*$AG329),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,25,0,{"$f":"VLOOKUP(AE330,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.42314698926998884},0,0,0,0,0,0,0,0,2.6286871077182896E-4,{"$f":"IF(OR(AF330=3,AF330=2,AF330=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D330,FlatMaint!$Y$2:$Y$10000,AE330)*AG330,0)","v":4.2362460196250025},{"$f":"IF(OR(AF330=3,AF330=2,AF330=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D330,FlatRepair!$Y$2:$Y$10000,AE330)*AG330,0)","v":0},0,4.2365088883357744,0,0,0,0,0,4.2365088883357744,0,{"$f":"IF($AF330=3,IF($AF$2=2,(R330/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I330,Refurb_Poss_Tbl[%]))*AG330,IF($AF$2=3,(R330*AG330)-AV330,R330*AG330)),0)","v":0},{"$f":"IF(AF330=3,IF($AF$2=2,(S330/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I330,Refurb_Poss_Tbl[%]))*AG330,IF($AF$2=3,(S330*AG330)-AX330,S330*AG330)),0)","v":0},{"$f":"IF($AF330=3,IF($AF$2=2,(T330/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I330,Refurb_Poss_Tbl[%]))*AG330,T330*$AG330),0)","v":0},{"$f":"IF($AF330=3,IF($AF$2=2,(Q330/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I330,Refurb_Poss_Tbl[%]))*AG330,Q330*$AG330),0)","v":0},{"$f":"IF($AF330=3,IF($AF$2=2,(U330/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I330,Refurb_Poss_Tbl[%]))*AG330,U330*$AG330),0)","v":0},{"$f":"IF($AF330=3,IF($AF$2=2,(V330/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I330,Refurb_Poss_Tbl[%]))*AG330,IF($AF$2=3,(V330*AG330)-AW330,V330*AG330)),0)","v":0},{"$f":"IF($AF330=3,IF($AF$2=2,(W330/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I330,Refurb_Poss_Tbl[%]))*AG330,W330*$AG330),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,26,0,{"$f":"VLOOKUP(AE331,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.40883767079225974},0,0,0,0,0,0,0,0,2.5397943069741929E-4,{"$f":"IF(OR(AF331=3,AF331=2,AF331=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D331,FlatMaint!$Y$2:$Y$10000,AE331)*AG331,0)","v":4.0929913233091808},{"$f":"IF(OR(AF331=3,AF331=2,AF331=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D331,FlatRepair!$Y$2:$Y$10000,AE331)*AG331,0)","v":0},0,4.0932453027398781,0,0,0,0,0,4.0932453027398781,0,{"$f":"IF($AF331=3,IF($AF$2=2,(R331/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I331,Refurb_Poss_Tbl[%]))*AG331,IF($AF$2=3,(R331*AG331)-AV331,R331*AG331)),0)","v":0},{"$f":"IF(AF331=3,IF($AF$2=2,(S331/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I331,Refurb_Poss_Tbl[%]))*AG331,IF($AF$2=3,(S331*AG331)-AX331,S331*AG331)),0)","v":0},{"$f":"IF($AF331=3,IF($AF$2=2,(T331/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I331,Refurb_Poss_Tbl[%]))*AG331,T331*$AG331),0)","v":0},{"$f":"IF($AF331=3,IF($AF$2=2,(Q331/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I331,Refurb_Poss_Tbl[%]))*AG331,Q331*$AG331),0)","v":0},{"$f":"IF($AF331=3,IF($AF$2=2,(U331/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I331,Refurb_Poss_Tbl[%]))*AG331,U331*$AG331),0)","v":0},{"$f":"IF($AF331=3,IF($AF$2=2,(V331/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I331,Refurb_Poss_Tbl[%]))*AG331,IF($AF$2=3,(V331*AG331)-AW331,V331*AG331)),0)","v":0},{"$f":"IF($AF331=3,IF($AF$2=2,(W331/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I331,Refurb_Poss_Tbl[%]))*AG331,W331*$AG331),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,27,0,{"$f":"VLOOKUP(AE332,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39501224231136206},0,0,0,0,0,0,0,0,2.453907542970235E-4,{"$f":"IF(OR(AF332=3,AF332=2,AF332=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D332,FlatMaint!$Y$2:$Y$10000,AE332)*AG332,0)","v":3.9545809887045227},{"$f":"IF(OR(AF332=3,AF332=2,AF332=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D332,FlatRepair!$Y$2:$Y$10000,AE332)*AG332,0)","v":0},0,3.9548263794588197,0,0,0,0,0,3.9548263794588197,0,{"$f":"IF($AF332=3,IF($AF$2=2,(R332/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I332,Refurb_Poss_Tbl[%]))*AG332,IF($AF$2=3,(R332*AG332)-AV332,R332*AG332)),0)","v":0},{"$f":"IF(AF332=3,IF($AF$2=2,(S332/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I332,Refurb_Poss_Tbl[%]))*AG332,IF($AF$2=3,(S332*AG332)-AX332,S332*AG332)),0)","v":0},{"$f":"IF($AF332=3,IF($AF$2=2,(T332/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I332,Refurb_Poss_Tbl[%]))*AG332,T332*$AG332),0)","v":0},{"$f":"IF($AF332=3,IF($AF$2=2,(Q332/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I332,Refurb_Poss_Tbl[%]))*AG332,Q332*$AG332),0)","v":0},{"$f":"IF($AF332=3,IF($AF$2=2,(U332/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I332,Refurb_Poss_Tbl[%]))*AG332,U332*$AG332),0)","v":0},{"$f":"IF($AF332=3,IF($AF$2=2,(V332/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I332,Refurb_Poss_Tbl[%]))*AG332,IF($AF$2=3,(V332*AG332)-AW332,V332*AG332)),0)","v":0},{"$f":"IF($AF332=3,IF($AF$2=2,(W332/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I332,Refurb_Poss_Tbl[%]))*AG332,W332*$AG332),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,28,0,{"$f":"VLOOKUP(AE333,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38165434039745127},0,0,0,0,0,0,0,0,2.3709251622900819E-4,{"$f":"IF(OR(AF333=3,AF333=2,AF333=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D333,FlatMaint!$Y$2:$Y$10000,AE333)*AG333,0)","v":3.8208511968159637},{"$f":"IF(OR(AF333=3,AF333=2,AF333=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D333,FlatRepair!$Y$2:$Y$10000,AE333)*AG333,0)","v":0},0,3.8210882893321929,0,0,0,0,0,3.8210882893321929,0,{"$f":"IF($AF333=3,IF($AF$2=2,(R333/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I333,Refurb_Poss_Tbl[%]))*AG333,IF($AF$2=3,(R333*AG333)-AV333,R333*AG333)),0)","v":0},{"$f":"IF(AF333=3,IF($AF$2=2,(S333/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I333,Refurb_Poss_Tbl[%]))*AG333,IF($AF$2=3,(S333*AG333)-AX333,S333*AG333)),0)","v":0},{"$f":"IF($AF333=3,IF($AF$2=2,(T333/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I333,Refurb_Poss_Tbl[%]))*AG333,T333*$AG333),0)","v":0},{"$f":"IF($AF333=3,IF($AF$2=2,(Q333/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I333,Refurb_Poss_Tbl[%]))*AG333,Q333*$AG333),0)","v":0},{"$f":"IF($AF333=3,IF($AF$2=2,(U333/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I333,Refurb_Poss_Tbl[%]))*AG333,U333*$AG333),0)","v":0},{"$f":"IF($AF333=3,IF($AF$2=2,(V333/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I333,Refurb_Poss_Tbl[%]))*AG333,IF($AF$2=3,(V333*AG333)-AW333,V333*AG333)),0)","v":0},{"$f":"IF($AF333=3,IF($AF$2=2,(W333/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I333,Refurb_Poss_Tbl[%]))*AG333,W333*$AG333),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,29,0,{"$f":"VLOOKUP(AE334,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36874815497338298},0,0,0,0,0,0,0,0,2.2907489490725435E-4,{"$f":"IF(OR(AF334=3,AF334=2,AF334=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D334,FlatMaint!$Y$2:$Y$10000,AE334)*AG334,0)","v":3.6916436684212224},{"$f":"IF(OR(AF334=3,AF334=2,AF334=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D334,FlatRepair!$Y$2:$Y$10000,AE334)*AG334,0)","v":0},0,3.6918727433161296,0,0,0,0,0,3.6918727433161296,0,{"$f":"IF($AF334=3,IF($AF$2=2,(R334/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I334,Refurb_Poss_Tbl[%]))*AG334,IF($AF$2=3,(R334*AG334)-AV334,R334*AG334)),0)","v":0},{"$f":"IF(AF334=3,IF($AF$2=2,(S334/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I334,Refurb_Poss_Tbl[%]))*AG334,IF($AF$2=3,(S334*AG334)-AX334,S334*AG334)),0)","v":0},{"$f":"IF($AF334=3,IF($AF$2=2,(T334/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I334,Refurb_Poss_Tbl[%]))*AG334,T334*$AG334),0)","v":0},{"$f":"IF($AF334=3,IF($AF$2=2,(Q334/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I334,Refurb_Poss_Tbl[%]))*AG334,Q334*$AG334),0)","v":0},{"$f":"IF($AF334=3,IF($AF$2=2,(U334/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I334,Refurb_Poss_Tbl[%]))*AG334,U334*$AG334),0)","v":0},{"$f":"IF($AF334=3,IF($AF$2=2,(V334/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I334,Refurb_Poss_Tbl[%]))*AG334,IF($AF$2=3,(V334*AG334)-AW334,V334*AG334)),0)","v":0},{"$f":"IF($AF334=3,IF($AF$2=2,(W334/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I334,Refurb_Poss_Tbl[%]))*AG334,W334*$AG334),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,30,0,{"$f":"VLOOKUP(AE335,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35627841060230236},0,0,0,0,0,0,0,0,2.2132840087657425E-4,{"$f":"IF(OR(AF335=3,AF335=2,AF335=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D335,FlatMaint!$Y$2:$Y$10000,AE335)*AG335,0)","v":3.56680547673548},{"$f":"IF(OR(AF335=3,AF335=2,AF335=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D335,FlatRepair!$Y$2:$Y$10000,AE335)*AG335,0)","v":0},0,3.5670268051363565,0,0,0,0,0,3.5670268051363565,0,{"$f":"IF($AF335=3,IF($AF$2=2,(R335/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I335,Refurb_Poss_Tbl[%]))*AG335,IF($AF$2=3,(R335*AG335)-AV335,R335*AG335)),0)","v":0},{"$f":"IF(AF335=3,IF($AF$2=2,(S335/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I335,Refurb_Poss_Tbl[%]))*AG335,IF($AF$2=3,(S335*AG335)-AX335,S335*AG335)),0)","v":0},{"$f":"IF($AF335=3,IF($AF$2=2,(T335/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I335,Refurb_Poss_Tbl[%]))*AG335,T335*$AG335),0)","v":0},{"$f":"IF($AF335=3,IF($AF$2=2,(Q335/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I335,Refurb_Poss_Tbl[%]))*AG335,Q335*$AG335),0)","v":0},{"$f":"IF($AF335=3,IF($AF$2=2,(U335/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I335,Refurb_Poss_Tbl[%]))*AG335,U335*$AG335),0)","v":0},{"$f":"IF($AF335=3,IF($AF$2=2,(V335/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I335,Refurb_Poss_Tbl[%]))*AG335,IF($AF$2=3,(V335*AG335)-AW335,V335*AG335)),0)","v":0},{"$f":"IF($AF335=3,IF($AF$2=2,(W335/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I335,Refurb_Poss_Tbl[%]))*AG335,W335*$AG335),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,31,0,{"$f":"VLOOKUP(AE336,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39998714516107459},0,0,0,0,0,0,0,0,2.4848127917721969E-4,{"$f":"IF(OR(AF336=3,AF336=2,AF336=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D336,FlatMaint!$Y$2:$Y$10000,AE336)*AG336,0)","v":4.0043861697161471},{"$f":"IF(OR(AF336=3,AF336=2,AF336=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D336,FlatRepair!$Y$2:$Y$10000,AE336)*AG336,0)","v":0},0,4.0046346509953246,0,0,0,0,0,4.0046346509953246,0,{"$f":"IF($AF336=3,IF($AF$2=2,(R336/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I336,Refurb_Poss_Tbl[%]))*AG336,IF($AF$2=3,(R336*AG336)-AV336,R336*AG336)),0)","v":0},{"$f":"IF(AF336=3,IF($AF$2=2,(S336/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I336,Refurb_Poss_Tbl[%]))*AG336,IF($AF$2=3,(S336*AG336)-AX336,S336*AG336)),0)","v":0},{"$f":"IF($AF336=3,IF($AF$2=2,(T336/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I336,Refurb_Poss_Tbl[%]))*AG336,T336*$AG336),0)","v":0},{"$f":"IF($AF336=3,IF($AF$2=2,(Q336/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I336,Refurb_Poss_Tbl[%]))*AG336,Q336*$AG336),0)","v":0},{"$f":"IF($AF336=3,IF($AF$2=2,(U336/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I336,Refurb_Poss_Tbl[%]))*AG336,U336*$AG336),0)","v":0},{"$f":"IF($AF336=3,IF($AF$2=2,(V336/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I336,Refurb_Poss_Tbl[%]))*AG336,IF($AF$2=3,(V336*AG336)-AW336,V336*AG336)),0)","v":0},{"$f":"IF($AF336=3,IF($AF$2=2,(W336/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I336,Refurb_Poss_Tbl[%]))*AG336,W336*$AG336),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,32,0,{"$f":"VLOOKUP(AE337,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38833703413696569},0,0,0,0,0,0,0,0,2.4124396036623278E-4,{"$f":"IF(OR(AF337=3,AF337=2,AF337=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D337,FlatMaint!$Y$2:$Y$10000,AE337)*AG337,0)","v":3.8877535628312114},{"$f":"IF(OR(AF337=3,AF337=2,AF337=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D337,FlatRepair!$Y$2:$Y$10000,AE337)*AG337,0)","v":0},0,3.8879948067915775,0,0,0,0,0,3.8879948067915775,0,{"$f":"IF($AF337=3,IF($AF$2=2,(R337/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I337,Refurb_Poss_Tbl[%]))*AG337,IF($AF$2=3,(R337*AG337)-AV337,R337*AG337)),0)","v":0},{"$f":"IF(AF337=3,IF($AF$2=2,(S337/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I337,Refurb_Poss_Tbl[%]))*AG337,IF($AF$2=3,(S337*AG337)-AX337,S337*AG337)),0)","v":0},{"$f":"IF($AF337=3,IF($AF$2=2,(T337/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I337,Refurb_Poss_Tbl[%]))*AG337,T337*$AG337),0)","v":0},{"$f":"IF($AF337=3,IF($AF$2=2,(Q337/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I337,Refurb_Poss_Tbl[%]))*AG337,Q337*$AG337),0)","v":0},{"$f":"IF($AF337=3,IF($AF$2=2,(U337/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I337,Refurb_Poss_Tbl[%]))*AG337,U337*$AG337),0)","v":0},{"$f":"IF($AF337=3,IF($AF$2=2,(V337/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I337,Refurb_Poss_Tbl[%]))*AG337,IF($AF$2=3,(V337*AG337)-AW337,V337*AG337)),0)","v":0},{"$f":"IF($AF337=3,IF($AF$2=2,(W337/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I337,Refurb_Poss_Tbl[%]))*AG337,W337*$AG337),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,33,0,{"$f":"VLOOKUP(AE338,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.37702624673491814},0,0,0,0,0,0,0,0,2.3421743724876969E-4,{"$f":"IF(OR(AF338=3,AF338=2,AF338=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D338,FlatMaint!$Y$2:$Y$10000,AE338)*AG338,0)","v":3.7745180221662249},{"$f":"IF(OR(AF338=3,AF338=2,AF338=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D338,FlatRepair!$Y$2:$Y$10000,AE338)*AG338,0)","v":0},0,3.7747522396034738,0,0,0,0,0,3.7747522396034738,0,{"$f":"IF($AF338=3,IF($AF$2=2,(R338/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I338,Refurb_Poss_Tbl[%]))*AG338,IF($AF$2=3,(R338*AG338)-AV338,R338*AG338)),0)","v":0},{"$f":"IF(AF338=3,IF($AF$2=2,(S338/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I338,Refurb_Poss_Tbl[%]))*AG338,IF($AF$2=3,(S338*AG338)-AX338,S338*AG338)),0)","v":0},{"$f":"IF($AF338=3,IF($AF$2=2,(T338/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I338,Refurb_Poss_Tbl[%]))*AG338,T338*$AG338),0)","v":0},{"$f":"IF($AF338=3,IF($AF$2=2,(Q338/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I338,Refurb_Poss_Tbl[%]))*AG338,Q338*$AG338),0)","v":0},{"$f":"IF($AF338=3,IF($AF$2=2,(U338/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I338,Refurb_Poss_Tbl[%]))*AG338,U338*$AG338),0)","v":0},{"$f":"IF($AF338=3,IF($AF$2=2,(V338/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I338,Refurb_Poss_Tbl[%]))*AG338,IF($AF$2=3,(V338*AG338)-AW338,V338*AG338)),0)","v":0},{"$f":"IF($AF338=3,IF($AF$2=2,(W338/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I338,Refurb_Poss_Tbl[%]))*AG338,W338*$AG338),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,34,0,{"$f":"VLOOKUP(AE339,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36604489974263904},0,0,0,0,0,0,0,0,2.2739557014443663E-4,{"$f":"IF(OR(AF339=3,AF339=2,AF339=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D339,FlatMaint!$Y$2:$Y$10000,AE339)*AG339,0)","v":3.664580604044879},{"$f":"IF(OR(AF339=3,AF339=2,AF339=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D339,FlatRepair!$Y$2:$Y$10000,AE339)*AG339,0)","v":0},0,3.6648079996150233,0,0,0,0,0,3.6648079996150233,0,{"$f":"IF($AF339=3,IF($AF$2=2,(R339/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I339,Refurb_Poss_Tbl[%]))*AG339,IF($AF$2=3,(R339*AG339)-AV339,R339*AG339)),0)","v":0},{"$f":"IF(AF339=3,IF($AF$2=2,(S339/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I339,Refurb_Poss_Tbl[%]))*AG339,IF($AF$2=3,(S339*AG339)-AX339,S339*AG339)),0)","v":0},{"$f":"IF($AF339=3,IF($AF$2=2,(T339/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I339,Refurb_Poss_Tbl[%]))*AG339,T339*$AG339),0)","v":0},{"$f":"IF($AF339=3,IF($AF$2=2,(Q339/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I339,Refurb_Poss_Tbl[%]))*AG339,Q339*$AG339),0)","v":0},{"$f":"IF($AF339=3,IF($AF$2=2,(U339/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I339,Refurb_Poss_Tbl[%]))*AG339,U339*$AG339),0)","v":0},{"$f":"IF($AF339=3,IF($AF$2=2,(V339/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I339,Refurb_Poss_Tbl[%]))*AG339,IF($AF$2=3,(V339*AG339)-AW339,V339*AG339)),0)","v":0},{"$f":"IF($AF339=3,IF($AF$2=2,(W339/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I339,Refurb_Poss_Tbl[%]))*AG339,W339*$AG339),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,35,0,{"$f":"VLOOKUP(AE340,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35538339780838735},0,0,0,0,0,0,0,0,2.2077239819848213E-4,{"$f":"IF(OR(AF340=3,AF340=2,AF340=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D340,FlatMaint!$Y$2:$Y$10000,AE340)*AG340,0)","v":3.5578452466455128},{"$f":"IF(OR(AF340=3,AF340=2,AF340=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D340,FlatRepair!$Y$2:$Y$10000,AE340)*AG340,0)","v":0},0,3.5580660190437112,0,0,0,0,0,3.5580660190437112,0,{"$f":"IF($AF340=3,IF($AF$2=2,(R340/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I340,Refurb_Poss_Tbl[%]))*AG340,IF($AF$2=3,(R340*AG340)-AV340,R340*AG340)),0)","v":0},{"$f":"IF(AF340=3,IF($AF$2=2,(S340/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I340,Refurb_Poss_Tbl[%]))*AG340,IF($AF$2=3,(S340*AG340)-AX340,S340*AG340)),0)","v":0},{"$f":"IF($AF340=3,IF($AF$2=2,(T340/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I340,Refurb_Poss_Tbl[%]))*AG340,T340*$AG340),0)","v":0},{"$f":"IF($AF340=3,IF($AF$2=2,(Q340/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I340,Refurb_Poss_Tbl[%]))*AG340,Q340*$AG340),0)","v":0},{"$f":"IF($AF340=3,IF($AF$2=2,(U340/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I340,Refurb_Poss_Tbl[%]))*AG340,U340*$AG340),0)","v":0},{"$f":"IF($AF340=3,IF($AF$2=2,(V340/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I340,Refurb_Poss_Tbl[%]))*AG340,IF($AF$2=3,(V340*AG340)-AW340,V340*AG340)),0)","v":0},{"$f":"IF($AF340=3,IF($AF$2=2,(W340/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I340,Refurb_Poss_Tbl[%]))*AG340,W340*$AG340),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,36,0,{"$f":"VLOOKUP(AE341,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.34503242505668674},0,0,0,0,0,0,0,0,2.1434213417328361E-4,{"$f":"IF(OR(AF341=3,AF341=2,AF341=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D341,FlatMaint!$Y$2:$Y$10000,AE341)*AG341,0)","v":3.4542186860636046},{"$f":"IF(OR(AF341=3,AF341=2,AF341=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D341,FlatRepair!$Y$2:$Y$10000,AE341)*AG341,0)","v":0},0,3.4544330281977778,0,0,0,0,0,3.4544330281977778,0,{"$f":"IF($AF341=3,IF($AF$2=2,(R341/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I341,Refurb_Poss_Tbl[%]))*AG341,IF($AF$2=3,(R341*AG341)-AV341,R341*AG341)),0)","v":0},{"$f":"IF(AF341=3,IF($AF$2=2,(S341/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I341,Refurb_Poss_Tbl[%]))*AG341,IF($AF$2=3,(S341*AG341)-AX341,S341*AG341)),0)","v":0},{"$f":"IF($AF341=3,IF($AF$2=2,(T341/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I341,Refurb_Poss_Tbl[%]))*AG341,T341*$AG341),0)","v":0},{"$f":"IF($AF341=3,IF($AF$2=2,(Q341/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I341,Refurb_Poss_Tbl[%]))*AG341,Q341*$AG341),0)","v":0},{"$f":"IF($AF341=3,IF($AF$2=2,(U341/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I341,Refurb_Poss_Tbl[%]))*AG341,U341*$AG341),0)","v":0},{"$f":"IF($AF341=3,IF($AF$2=2,(V341/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I341,Refurb_Poss_Tbl[%]))*AG341,IF($AF$2=3,(V341*AG341)-AW341,V341*AG341)),0)","v":0},{"$f":"IF($AF341=3,IF($AF$2=2,(W341/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I341,Refurb_Poss_Tbl[%]))*AG341,W341*$AG341),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,37,0,{"$f":"VLOOKUP(AE342,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.33498293694823961},0,0,0,0,0,0,0,0,2.0809915939153751E-4,{"$f":"IF(OR(AF342=3,AF342=2,AF342=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D342,FlatMaint!$Y$2:$Y$10000,AE342)*AG342,0)","v":3.3536103748190342},{"$f":"IF(OR(AF342=3,AF342=2,AF342=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D342,FlatRepair!$Y$2:$Y$10000,AE342)*AG342,0)","v":0},0,3.3538184739784258,0,0,0,0,0,3.3538184739784258,0,{"$f":"IF($AF342=3,IF($AF$2=2,(R342/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I342,Refurb_Poss_Tbl[%]))*AG342,IF($AF$2=3,(R342*AG342)-AV342,R342*AG342)),0)","v":0},{"$f":"IF(AF342=3,IF($AF$2=2,(S342/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I342,Refurb_Poss_Tbl[%]))*AG342,IF($AF$2=3,(S342*AG342)-AX342,S342*AG342)),0)","v":0},{"$f":"IF($AF342=3,IF($AF$2=2,(T342/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I342,Refurb_Poss_Tbl[%]))*AG342,T342*$AG342),0)","v":0},{"$f":"IF($AF342=3,IF($AF$2=2,(Q342/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I342,Refurb_Poss_Tbl[%]))*AG342,Q342*$AG342),0)","v":0},{"$f":"IF($AF342=3,IF($AF$2=2,(U342/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I342,Refurb_Poss_Tbl[%]))*AG342,U342*$AG342),0)","v":0},{"$f":"IF($AF342=3,IF($AF$2=2,(V342/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I342,Refurb_Poss_Tbl[%]))*AG342,IF($AF$2=3,(V342*AG342)-AW342,V342*AG342)),0)","v":0},{"$f":"IF($AF342=3,IF($AF$2=2,(W342/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I342,Refurb_Poss_Tbl[%]))*AG342,W342*$AG342),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,38,0,{"$f":"VLOOKUP(AE343,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.3252261523769317},0,0,0,0,0,0,0,0,2.0203801882673548E-4,{"$f":"IF(OR(AF343=3,AF343=2,AF343=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D343,FlatMaint!$Y$2:$Y$10000,AE343)*AG343,0)","v":3.255932402736927},{"$f":"IF(OR(AF343=3,AF343=2,AF343=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D343,FlatRepair!$Y$2:$Y$10000,AE343)*AG343,0)","v":0},0,3.2561344407557535,0,0,0,0,0,3.2561344407557535,0,{"$f":"IF($AF343=3,IF($AF$2=2,(R343/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I343,Refurb_Poss_Tbl[%]))*AG343,IF($AF$2=3,(R343*AG343)-AV343,R343*AG343)),0)","v":0},{"$f":"IF(AF343=3,IF($AF$2=2,(S343/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I343,Refurb_Poss_Tbl[%]))*AG343,IF($AF$2=3,(S343*AG343)-AX343,S343*AG343)),0)","v":0},{"$f":"IF($AF343=3,IF($AF$2=2,(T343/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I343,Refurb_Poss_Tbl[%]))*AG343,T343*$AG343),0)","v":0},{"$f":"IF($AF343=3,IF($AF$2=2,(Q343/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I343,Refurb_Poss_Tbl[%]))*AG343,Q343*$AG343),0)","v":0},{"$f":"IF($AF343=3,IF($AF$2=2,(U343/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I343,Refurb_Poss_Tbl[%]))*AG343,U343*$AG343),0)","v":0},{"$f":"IF($AF343=3,IF($AF$2=2,(V343/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I343,Refurb_Poss_Tbl[%]))*AG343,IF($AF$2=3,(V343*AG343)-AW343,V343*AG343)),0)","v":0},{"$f":"IF($AF343=3,IF($AF$2=2,(W343/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I343,Refurb_Poss_Tbl[%]))*AG343,W343*$AG343),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,39,0,{"$f":"VLOOKUP(AE344,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.31575354599702099},0,0,0,0,0,0,0,0,1.9615341633663633E-4,{"$f":"IF(OR(AF344=3,AF344=2,AF344=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D344,FlatMaint!$Y$2:$Y$10000,AE344)*AG344,0)","v":3.1610994201329379},{"$f":"IF(OR(AF344=3,AF344=2,AF344=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D344,FlatRepair!$Y$2:$Y$10000,AE344)*AG344,0)","v":0},0,3.1612955735492747,0,0,0,0,0,3.1612955735492747,0,{"$f":"IF($AF344=3,IF($AF$2=2,(R344/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I344,Refurb_Poss_Tbl[%]))*AG344,IF($AF$2=3,(R344*AG344)-AV344,R344*AG344)),0)","v":0},{"$f":"IF(AF344=3,IF($AF$2=2,(S344/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I344,Refurb_Poss_Tbl[%]))*AG344,IF($AF$2=3,(S344*AG344)-AX344,S344*AG344)),0)","v":0},{"$f":"IF($AF344=3,IF($AF$2=2,(T344/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I344,Refurb_Poss_Tbl[%]))*AG344,T344*$AG344),0)","v":0},{"$f":"IF($AF344=3,IF($AF$2=2,(Q344/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I344,Refurb_Poss_Tbl[%]))*AG344,Q344*$AG344),0)","v":0},{"$f":"IF($AF344=3,IF($AF$2=2,(U344/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I344,Refurb_Poss_Tbl[%]))*AG344,U344*$AG344),0)","v":0},{"$f":"IF($AF344=3,IF($AF$2=2,(V344/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I344,Refurb_Poss_Tbl[%]))*AG344,IF($AF$2=3,(V344*AG344)-AW344,V344*AG344)),0)","v":0},{"$f":"IF($AF344=3,IF($AF$2=2,(W344/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I344,Refurb_Poss_Tbl[%]))*AG344,W344*$AG344),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,40,0,{"$f":"VLOOKUP(AE345,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.30655684077380685},0,0,0,0,0,0,0,0,1.9044021003556931E-4,{"$f":"IF(OR(AF345=3,AF345=2,AF345=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D345,FlatMaint!$Y$2:$Y$10000,AE345)*AG345,0)","v":3.0690285632358627},{"$f":"IF(OR(AF345=3,AF345=2,AF345=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D345,FlatRepair!$Y$2:$Y$10000,AE345)*AG345,0)","v":0},0,3.0692190034458982,0,0,0,0,0,3.0692190034458982,0,{"$f":"IF($AF345=3,IF($AF$2=2,(R345/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I345,Refurb_Poss_Tbl[%]))*AG345,IF($AF$2=3,(R345*AG345)-AV345,R345*AG345)),0)","v":0},{"$f":"IF(AF345=3,IF($AF$2=2,(S345/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I345,Refurb_Poss_Tbl[%]))*AG345,IF($AF$2=3,(S345*AG345)-AX345,S345*AG345)),0)","v":0},{"$f":"IF($AF345=3,IF($AF$2=2,(T345/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I345,Refurb_Poss_Tbl[%]))*AG345,T345*$AG345),0)","v":0},{"$f":"IF($AF345=3,IF($AF$2=2,(Q345/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I345,Refurb_Poss_Tbl[%]))*AG345,Q345*$AG345),0)","v":0},{"$f":"IF($AF345=3,IF($AF$2=2,(U345/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I345,Refurb_Poss_Tbl[%]))*AG345,U345*$AG345),0)","v":0},{"$f":"IF($AF345=3,IF($AF$2=2,(V345/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I345,Refurb_Poss_Tbl[%]))*AG345,IF($AF$2=3,(V345*AG345)-AW345,V345*AG345)),0)","v":0},{"$f":"IF($AF345=3,IF($AF$2=2,(W345/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I345,Refurb_Poss_Tbl[%]))*AG345,W345*$AG345),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,41,0,{"$f":"VLOOKUP(AE346,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.29762800075126877},0,0,0,0,0,0,0,0,1.8489340780152358E-4,{"$f":"IF(OR(AF346=3,AF346=2,AF346=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D346,FlatMaint!$Y$2:$Y$10000,AE346)*AG346,0)","v":2.9796393817823907},{"$f":"IF(OR(AF346=3,AF346=2,AF346=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D346,FlatRepair!$Y$2:$Y$10000,AE346)*AG346,0)","v":0},0,2.9798242751901922,0,0,0,0,0,2.9798242751901922,0,{"$f":"IF($AF346=3,IF($AF$2=2,(R346/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I346,Refurb_Poss_Tbl[%]))*AG346,IF($AF$2=3,(R346*AG346)-AV346,R346*AG346)),0)","v":0},{"$f":"IF(AF346=3,IF($AF$2=2,(S346/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I346,Refurb_Poss_Tbl[%]))*AG346,IF($AF$2=3,(S346*AG346)-AX346,S346*AG346)),0)","v":0},{"$f":"IF($AF346=3,IF($AF$2=2,(T346/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I346,Refurb_Poss_Tbl[%]))*AG346,T346*$AG346),0)","v":0},{"$f":"IF($AF346=3,IF($AF$2=2,(Q346/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I346,Refurb_Poss_Tbl[%]))*AG346,Q346*$AG346),0)","v":0},{"$f":"IF($AF346=3,IF($AF$2=2,(U346/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I346,Refurb_Poss_Tbl[%]))*AG346,U346*$AG346),0)","v":0},{"$f":"IF($AF346=3,IF($AF$2=2,(V346/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I346,Refurb_Poss_Tbl[%]))*AG346,IF($AF$2=3,(V346*AG346)-AW346,V346*AG346)),0)","v":0},{"$f":"IF($AF346=3,IF($AF$2=2,(W346/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I346,Refurb_Poss_Tbl[%]))*AG346,W346*$AG346),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,42,0,{"$f":"VLOOKUP(AE347,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28895922403035801},0,0,0,0,0,0,0,0,1.7950816291410055E-4,{"$f":"IF(OR(AF347=3,AF347=2,AF347=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D347,FlatMaint!$Y$2:$Y$10000,AE347)*AG347,0)","v":2.8928537687207676},{"$f":"IF(OR(AF347=3,AF347=2,AF347=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D347,FlatRepair!$Y$2:$Y$10000,AE347)*AG347,0)","v":0},0,2.8930332768836817,0,0,0,0,0,2.8930332768836817,0,{"$f":"IF($AF347=3,IF($AF$2=2,(R347/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I347,Refurb_Poss_Tbl[%]))*AG347,IF($AF$2=3,(R347*AG347)-AV347,R347*AG347)),0)","v":0},{"$f":"IF(AF347=3,IF($AF$2=2,(S347/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I347,Refurb_Poss_Tbl[%]))*AG347,IF($AF$2=3,(S347*AG347)-AX347,S347*AG347)),0)","v":0},{"$f":"IF($AF347=3,IF($AF$2=2,(T347/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I347,Refurb_Poss_Tbl[%]))*AG347,T347*$AG347),0)","v":0},{"$f":"IF($AF347=3,IF($AF$2=2,(Q347/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I347,Refurb_Poss_Tbl[%]))*AG347,Q347*$AG347),0)","v":0},{"$f":"IF($AF347=3,IF($AF$2=2,(U347/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I347,Refurb_Poss_Tbl[%]))*AG347,U347*$AG347),0)","v":0},{"$f":"IF($AF347=3,IF($AF$2=2,(V347/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I347,Refurb_Poss_Tbl[%]))*AG347,IF($AF$2=3,(V347*AG347)-AW347,V347*AG347)),0)","v":0},{"$f":"IF($AF347=3,IF($AF$2=2,(W347/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I347,Refurb_Poss_Tbl[%]))*AG347,W347*$AG347),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,43,0,{"$f":"VLOOKUP(AE348,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28054293595180391},0,0,0,0,0,0,0,0,1.742797698195151E-4,{"$f":"IF(OR(AF348=3,AF348=2,AF348=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D348,FlatMaint!$Y$2:$Y$10000,AE348)*AG348,0)","v":2.8085958919619105},{"$f":"IF(OR(AF348=3,AF348=2,AF348=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D348,FlatRepair!$Y$2:$Y$10000,AE348)*AG348,0)","v":0},0,2.8087701717317302,0,0,0,0,0,2.8087701717317302,0,{"$f":"IF($AF348=3,IF($AF$2=2,(R348/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I348,Refurb_Poss_Tbl[%]))*AG348,IF($AF$2=3,(R348*AG348)-AV348,R348*AG348)),0)","v":0},{"$f":"IF(AF348=3,IF($AF$2=2,(S348/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I348,Refurb_Poss_Tbl[%]))*AG348,IF($AF$2=3,(S348*AG348)-AX348,S348*AG348)),0)","v":0},{"$f":"IF($AF348=3,IF($AF$2=2,(T348/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I348,Refurb_Poss_Tbl[%]))*AG348,T348*$AG348),0)","v":0},{"$f":"IF($AF348=3,IF($AF$2=2,(Q348/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I348,Refurb_Poss_Tbl[%]))*AG348,Q348*$AG348),0)","v":0},{"$f":"IF($AF348=3,IF($AF$2=2,(U348/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I348,Refurb_Poss_Tbl[%]))*AG348,U348*$AG348),0)","v":0},{"$f":"IF($AF348=3,IF($AF$2=2,(V348/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I348,Refurb_Poss_Tbl[%]))*AG348,IF($AF$2=3,(V348*AG348)-AW348,V348*AG348)),0)","v":0},{"$f":"IF($AF348=3,IF($AF$2=2,(W348/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I348,Refurb_Poss_Tbl[%]))*AG348,W348*$AG348),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,44,0,{"$f":"VLOOKUP(AE349,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.27237178247747956},0,0,0,0,0,0,0,0,1.6920366001894674E-4,{"$f":"IF(OR(AF349=3,AF349=2,AF349=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D349,FlatMaint!$Y$2:$Y$10000,AE349)*AG349,0)","v":2.72679212811836},{"$f":"IF(OR(AF349=3,AF349=2,AF349=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D349,FlatRepair!$Y$2:$Y$10000,AE349)*AG349,0)","v":0},0,2.7269613317783792,0,0,0,0,0,2.7269613317783792,0,{"$f":"IF($AF349=3,IF($AF$2=2,(R349/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I349,Refurb_Poss_Tbl[%]))*AG349,IF($AF$2=3,(R349*AG349)-AV349,R349*AG349)),0)","v":0},{"$f":"IF(AF349=3,IF($AF$2=2,(S349/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I349,Refurb_Poss_Tbl[%]))*AG349,IF($AF$2=3,(S349*AG349)-AX349,S349*AG349)),0)","v":0},{"$f":"IF($AF349=3,IF($AF$2=2,(T349/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I349,Refurb_Poss_Tbl[%]))*AG349,T349*$AG349),0)","v":0},{"$f":"IF($AF349=3,IF($AF$2=2,(Q349/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I349,Refurb_Poss_Tbl[%]))*AG349,Q349*$AG349),0)","v":0},{"$f":"IF($AF349=3,IF($AF$2=2,(U349/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I349,Refurb_Poss_Tbl[%]))*AG349,U349*$AG349),0)","v":0},{"$f":"IF($AF349=3,IF($AF$2=2,(V349/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I349,Refurb_Poss_Tbl[%]))*AG349,IF($AF$2=3,(V349*AG349)-AW349,V349*AG349)),0)","v":0},{"$f":"IF($AF349=3,IF($AF$2=2,(W349/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I349,Refurb_Poss_Tbl[%]))*AG349,W349*$AG349),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,45,0,{"$f":"VLOOKUP(AE350,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.26443862376454325},0,0,0,0,0,0,0,0,1.642753980766473E-4,{"$f":"IF(OR(AF350=3,AF350=2,AF350=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D350,FlatMaint!$Y$2:$Y$10000,AE350)*AG350,0)","v":2.647370998173165},{"$f":"IF(OR(AF350=3,AF350=2,AF350=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D350,FlatRepair!$Y$2:$Y$10000,AE350)*AG350,0)","v":0},0,2.6475352735712416,0,0,0,0,0,2.6475352735712416,0,{"$f":"IF($AF350=3,IF($AF$2=2,(R350/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I350,Refurb_Poss_Tbl[%]))*AG350,IF($AF$2=3,(R350*AG350)-AV350,R350*AG350)),0)","v":0},{"$f":"IF(AF350=3,IF($AF$2=2,(S350/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I350,Refurb_Poss_Tbl[%]))*AG350,IF($AF$2=3,(S350*AG350)-AX350,S350*AG350)),0)","v":0},{"$f":"IF($AF350=3,IF($AF$2=2,(T350/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I350,Refurb_Poss_Tbl[%]))*AG350,T350*$AG350),0)","v":0},{"$f":"IF($AF350=3,IF($AF$2=2,(Q350/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I350,Refurb_Poss_Tbl[%]))*AG350,Q350*$AG350),0)","v":0},{"$f":"IF($AF350=3,IF($AF$2=2,(U350/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I350,Refurb_Poss_Tbl[%]))*AG350,U350*$AG350),0)","v":0},{"$f":"IF($AF350=3,IF($AF$2=2,(V350/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I350,Refurb_Poss_Tbl[%]))*AG350,IF($AF$2=3,(V350*AG350)-AW350,V350*AG350)),0)","v":0},{"$f":"IF($AF350=3,IF($AF$2=2,(W350/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I350,Refurb_Poss_Tbl[%]))*AG350,W350*$AG350),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,46,0,{"$f":"VLOOKUP(AE351,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.25673652792674101},0,0,0,0,0,0,0,0,1.5949067774431776E-4,{"$f":"IF(OR(AF351=3,AF351=2,AF351=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D351,FlatMaint!$Y$2:$Y$10000,AE351)*AG351,0)","v":2.57026310502249},{"$f":"IF(OR(AF351=3,AF351=2,AF351=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D351,FlatRepair!$Y$2:$Y$10000,AE351)*AG351,0)","v":0},0,2.5704225957002342,0,0,0,0,0,2.5704225957002342,0,{"$f":"IF($AF351=3,IF($AF$2=2,(R351/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I351,Refurb_Poss_Tbl[%]))*AG351,IF($AF$2=3,(R351*AG351)-AV351,R351*AG351)),0)","v":0},{"$f":"IF(AF351=3,IF($AF$2=2,(S351/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I351,Refurb_Poss_Tbl[%]))*AG351,IF($AF$2=3,(S351*AG351)-AX351,S351*AG351)),0)","v":0},{"$f":"IF($AF351=3,IF($AF$2=2,(T351/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I351,Refurb_Poss_Tbl[%]))*AG351,T351*$AG351),0)","v":0},{"$f":"IF($AF351=3,IF($AF$2=2,(Q351/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I351,Refurb_Poss_Tbl[%]))*AG351,Q351*$AG351),0)","v":0},{"$f":"IF($AF351=3,IF($AF$2=2,(U351/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I351,Refurb_Poss_Tbl[%]))*AG351,U351*$AG351),0)","v":0},{"$f":"IF($AF351=3,IF($AF$2=2,(V351/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I351,Refurb_Poss_Tbl[%]))*AG351,IF($AF$2=3,(V351*AG351)-AW351,V351*AG351)),0)","v":0},{"$f":"IF($AF351=3,IF($AF$2=2,(W351/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I351,Refurb_Poss_Tbl[%]))*AG351,W351*$AG351),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,47,0,{"$f":"VLOOKUP(AE352,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24925876497741845},0,0,0,0,0,0,0,0,1.5484531819836674E-4,{"$f":"IF(OR(AF352=3,AF352=2,AF352=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D352,FlatMaint!$Y$2:$Y$10000,AE352)*AG352,0)","v":2.4954010728373692},{"$f":"IF(OR(AF352=3,AF352=2,AF352=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D352,FlatRepair!$Y$2:$Y$10000,AE352)*AG352,0)","v":0},0,2.4955559181555675,0,0,0,0,0,2.4955559181555675,0,{"$f":"IF($AF352=3,IF($AF$2=2,(R352/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I352,Refurb_Poss_Tbl[%]))*AG352,IF($AF$2=3,(R352*AG352)-AV352,R352*AG352)),0)","v":0},{"$f":"IF(AF352=3,IF($AF$2=2,(S352/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I352,Refurb_Poss_Tbl[%]))*AG352,IF($AF$2=3,(S352*AG352)-AX352,S352*AG352)),0)","v":0},{"$f":"IF($AF352=3,IF($AF$2=2,(T352/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I352,Refurb_Poss_Tbl[%]))*AG352,T352*$AG352),0)","v":0},{"$f":"IF($AF352=3,IF($AF$2=2,(Q352/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I352,Refurb_Poss_Tbl[%]))*AG352,Q352*$AG352),0)","v":0},{"$f":"IF($AF352=3,IF($AF$2=2,(U352/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I352,Refurb_Poss_Tbl[%]))*AG352,U352*$AG352),0)","v":0},{"$f":"IF($AF352=3,IF($AF$2=2,(V352/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I352,Refurb_Poss_Tbl[%]))*AG352,IF($AF$2=3,(V352*AG352)-AW352,V352*AG352)),0)","v":0},{"$f":"IF($AF352=3,IF($AF$2=2,(W352/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I352,Refurb_Poss_Tbl[%]))*AG352,W352*$AG352),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,48,0,{"$f":"VLOOKUP(AE353,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24199880094894996},0,0,0,0,0,0,0,0,1.5033526038676386E-4,{"$f":"IF(OR(AF353=3,AF353=2,AF353=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D353,FlatMaint!$Y$2:$Y$10000,AE353)*AG353,0)","v":2.4227194881916203},{"$f":"IF(OR(AF353=3,AF353=2,AF353=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D353,FlatRepair!$Y$2:$Y$10000,AE353)*AG353,0)","v":0},0,2.422869823452007,0,0,0,0,0,2.422869823452007,0,{"$f":"IF($AF353=3,IF($AF$2=2,(R353/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I353,Refurb_Poss_Tbl[%]))*AG353,IF($AF$2=3,(R353*AG353)-AV353,R353*AG353)),0)","v":0},{"$f":"IF(AF353=3,IF($AF$2=2,(S353/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I353,Refurb_Poss_Tbl[%]))*AG353,IF($AF$2=3,(S353*AG353)-AX353,S353*AG353)),0)","v":0},{"$f":"IF($AF353=3,IF($AF$2=2,(T353/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I353,Refurb_Poss_Tbl[%]))*AG353,T353*$AG353),0)","v":0},{"$f":"IF($AF353=3,IF($AF$2=2,(Q353/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I353,Refurb_Poss_Tbl[%]))*AG353,Q353*$AG353),0)","v":0},{"$f":"IF($AF353=3,IF($AF$2=2,(U353/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I353,Refurb_Poss_Tbl[%]))*AG353,U353*$AG353),0)","v":0},{"$f":"IF($AF353=3,IF($AF$2=2,(V353/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I353,Refurb_Poss_Tbl[%]))*AG353,IF($AF$2=3,(V353*AG353)-AW353,V353*AG353)),0)","v":0},{"$f":"IF($AF353=3,IF($AF$2=2,(W353/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I353,Refurb_Poss_Tbl[%]))*AG353,W353*$AG353),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,49,0,{"$f":"VLOOKUP(AE354,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.2349502921834466},0,0,0,0,0,0,0,0,1.4595656348229501E-4,{"$f":"IF(OR(AF354=3,AF354=2,AF354=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D354,FlatMaint!$Y$2:$Y$10000,AE354)*AG354,0)","v":2.3521548429044863},{"$f":"IF(OR(AF354=3,AF354=2,AF354=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D354,FlatRepair!$Y$2:$Y$10000,AE354)*AG354,0)","v":0},0,2.3523007994679688,0,0,0,0,0,2.3523007994679688,0,{"$f":"IF($AF354=3,IF($AF$2=2,(R354/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I354,Refurb_Poss_Tbl[%]))*AG354,IF($AF$2=3,(R354*AG354)-AV354,R354*AG354)),0)","v":0},{"$f":"IF(AF354=3,IF($AF$2=2,(S354/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I354,Refurb_Poss_Tbl[%]))*AG354,IF($AF$2=3,(S354*AG354)-AX354,S354*AG354)),0)","v":0},{"$f":"IF($AF354=3,IF($AF$2=2,(T354/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I354,Refurb_Poss_Tbl[%]))*AG354,T354*$AG354),0)","v":0},{"$f":"IF($AF354=3,IF($AF$2=2,(Q354/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I354,Refurb_Poss_Tbl[%]))*AG354,Q354*$AG354),0)","v":0},{"$f":"IF($AF354=3,IF($AF$2=2,(U354/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I354,Refurb_Poss_Tbl[%]))*AG354,U354*$AG354),0)","v":0},{"$f":"IF($AF354=3,IF($AF$2=2,(V354/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I354,Refurb_Poss_Tbl[%]))*AG354,IF($AF$2=3,(V354*AG354)-AW354,V354*AG354)),0)","v":0},{"$f":"IF($AF354=3,IF($AF$2=2,(W354/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I354,Refurb_Poss_Tbl[%]))*AG354,W354*$AG354),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,50,0,{"$f":"VLOOKUP(AE355,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22810707978975397},0,0,0,0,0,0,0,0,1.4170540143912136E-4,{"$f":"IF(OR(AF355=3,AF355=2,AF355=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D355,FlatMaint!$Y$2:$Y$10000,AE355)*AG355,0)","v":2.2836454785480451},{"$f":"IF(OR(AF355=3,AF355=2,AF355=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D355,FlatRepair!$Y$2:$Y$10000,AE355)*AG355,0)","v":0},0,2.2837871839494843,0,0,0,0,0,2.2837871839494843,0,{"$f":"IF($AF355=3,IF($AF$2=2,(R355/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I355,Refurb_Poss_Tbl[%]))*AG355,IF($AF$2=3,(R355*AG355)-AV355,R355*AG355)),0)","v":0},{"$f":"IF(AF355=3,IF($AF$2=2,(S355/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I355,Refurb_Poss_Tbl[%]))*AG355,IF($AF$2=3,(S355*AG355)-AX355,S355*AG355)),0)","v":0},{"$f":"IF($AF355=3,IF($AF$2=2,(T355/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I355,Refurb_Poss_Tbl[%]))*AG355,T355*$AG355),0)","v":0},{"$f":"IF($AF355=3,IF($AF$2=2,(Q355/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I355,Refurb_Poss_Tbl[%]))*AG355,Q355*$AG355),0)","v":0},{"$f":"IF($AF355=3,IF($AF$2=2,(U355/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I355,Refurb_Poss_Tbl[%]))*AG355,U355*$AG355),0)","v":0},{"$f":"IF($AF355=3,IF($AF$2=2,(V355/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I355,Refurb_Poss_Tbl[%]))*AG355,IF($AF$2=3,(V355*AG355)-AW355,V355*AG355)),0)","v":0},{"$f":"IF($AF355=3,IF($AF$2=2,(W355/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I355,Refurb_Poss_Tbl[%]))*AG355,W355*$AG355),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,51,0,{"$f":"VLOOKUP(AE356,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22146318426189707},0,0,0,0,0,0,0,0,1.3757805964963242E-4,{"$f":"IF(OR(AF356=3,AF356=2,AF356=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D356,FlatMaint!$Y$2:$Y$10000,AE356)*AG356,0)","v":2.2171315325709173},{"$f":"IF(OR(AF356=3,AF356=2,AF356=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D356,FlatRepair!$Y$2:$Y$10000,AE356)*AG356,0)","v":0},0,2.2172691106305669,0,0,0,0,0,2.2172691106305669,0,{"$f":"IF($AF356=3,IF($AF$2=2,(R356/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I356,Refurb_Poss_Tbl[%]))*AG356,IF($AF$2=3,(R356*AG356)-AV356,R356*AG356)),0)","v":0},{"$f":"IF(AF356=3,IF($AF$2=2,(S356/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I356,Refurb_Poss_Tbl[%]))*AG356,IF($AF$2=3,(S356*AG356)-AX356,S356*AG356)),0)","v":0},{"$f":"IF($AF356=3,IF($AF$2=2,(T356/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I356,Refurb_Poss_Tbl[%]))*AG356,T356*$AG356),0)","v":0},{"$f":"IF($AF356=3,IF($AF$2=2,(Q356/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I356,Refurb_Poss_Tbl[%]))*AG356,Q356*$AG356),0)","v":0},{"$f":"IF($AF356=3,IF($AF$2=2,(U356/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I356,Refurb_Poss_Tbl[%]))*AG356,U356*$AG356),0)","v":0},{"$f":"IF($AF356=3,IF($AF$2=2,(V356/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I356,Refurb_Poss_Tbl[%]))*AG356,IF($AF$2=3,(V356*AG356)-AW356,V356*AG356)),0)","v":0},{"$f":"IF($AF356=3,IF($AF$2=2,(W356/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I356,Refurb_Poss_Tbl[%]))*AG356,W356*$AG356),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,52,0,{"$f":"VLOOKUP(AE357,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.215012800254269},0,0,0,0,0,0,0,0,1.3357093169867224E-4,{"$f":"IF(OR(AF357=3,AF357=2,AF357=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D357,FlatMaint!$Y$2:$Y$10000,AE357)*AG357,0)","v":2.1525548859911821},{"$f":"IF(OR(AF357=3,AF357=2,AF357=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D357,FlatRepair!$Y$2:$Y$10000,AE357)*AG357,0)","v":0},0,2.1526884569228808,0,0,0,0,0,2.1526884569228808,0,{"$f":"IF($AF357=3,IF($AF$2=2,(R357/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I357,Refurb_Poss_Tbl[%]))*AG357,IF($AF$2=3,(R357*AG357)-AV357,R357*AG357)),0)","v":0},{"$f":"IF(AF357=3,IF($AF$2=2,(S357/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I357,Refurb_Poss_Tbl[%]))*AG357,IF($AF$2=3,(S357*AG357)-AX357,S357*AG357)),0)","v":0},{"$f":"IF($AF357=3,IF($AF$2=2,(T357/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I357,Refurb_Poss_Tbl[%]))*AG357,T357*$AG357),0)","v":0},{"$f":"IF($AF357=3,IF($AF$2=2,(Q357/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I357,Refurb_Poss_Tbl[%]))*AG357,Q357*$AG357),0)","v":0},{"$f":"IF($AF357=3,IF($AF$2=2,(U357/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I357,Refurb_Poss_Tbl[%]))*AG357,U357*$AG357),0)","v":0},{"$f":"IF($AF357=3,IF($AF$2=2,(V357/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I357,Refurb_Poss_Tbl[%]))*AG357,IF($AF$2=3,(V357*AG357)-AW357,V357*AG357)),0)","v":0},{"$f":"IF($AF357=3,IF($AF$2=2,(W357/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I357,Refurb_Poss_Tbl[%]))*AG357,W357*$AG357),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,53,0,{"$f":"VLOOKUP(AE358,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20875029150899907},0,0,0,0,0,0,0,0,1.2968051621230317E-4,{"$f":"IF(OR(AF358=3,AF358=2,AF358=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D358,FlatMaint!$Y$2:$Y$10000,AE358)*AG358,0)","v":2.0898591126127983},{"$f":"IF(OR(AF358=3,AF358=2,AF358=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D358,FlatRepair!$Y$2:$Y$10000,AE358)*AG358,0)","v":0},0,2.0899887931290104,0,0,0,0,0,2.0899887931290104,0,{"$f":"IF($AF358=3,IF($AF$2=2,(R358/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I358,Refurb_Poss_Tbl[%]))*AG358,IF($AF$2=3,(R358*AG358)-AV358,R358*AG358)),0)","v":0},{"$f":"IF(AF358=3,IF($AF$2=2,(S358/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I358,Refurb_Poss_Tbl[%]))*AG358,IF($AF$2=3,(S358*AG358)-AX358,S358*AG358)),0)","v":0},{"$f":"IF($AF358=3,IF($AF$2=2,(T358/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I358,Refurb_Poss_Tbl[%]))*AG358,T358*$AG358),0)","v":0},{"$f":"IF($AF358=3,IF($AF$2=2,(Q358/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I358,Refurb_Poss_Tbl[%]))*AG358,Q358*$AG358),0)","v":0},{"$f":"IF($AF358=3,IF($AF$2=2,(U358/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I358,Refurb_Poss_Tbl[%]))*AG358,U358*$AG358),0)","v":0},{"$f":"IF($AF358=3,IF($AF$2=2,(V358/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I358,Refurb_Poss_Tbl[%]))*AG358,IF($AF$2=3,(V358*AG358)-AW358,V358*AG358)),0)","v":0},{"$f":"IF($AF358=3,IF($AF$2=2,(W358/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I358,Refurb_Poss_Tbl[%]))*AG358,W358*$AG358),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,54,0,{"$f":"VLOOKUP(AE359,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20267018593106703},0,0,0,0,0,0,0,0,1.2590341379835259E-4,{"$f":"IF(OR(AF359=3,AF359=2,AF359=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D359,FlatMaint!$Y$2:$Y$10000,AE359)*AG359,0)","v":2.0289894297211633},{"$f":"IF(OR(AF359=3,AF359=2,AF359=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D359,FlatRepair!$Y$2:$Y$10000,AE359)*AG359,0)","v":0},0,2.0291153331349614,0,0,0,0,0,2.0291153331349614,0,{"$f":"IF($AF359=3,IF($AF$2=2,(R359/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I359,Refurb_Poss_Tbl[%]))*AG359,IF($AF$2=3,(R359*AG359)-AV359,R359*AG359)),0)","v":0},{"$f":"IF(AF359=3,IF($AF$2=2,(S359/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I359,Refurb_Poss_Tbl[%]))*AG359,IF($AF$2=3,(S359*AG359)-AX359,S359*AG359)),0)","v":0},{"$f":"IF($AF359=3,IF($AF$2=2,(T359/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I359,Refurb_Poss_Tbl[%]))*AG359,T359*$AG359),0)","v":0},{"$f":"IF($AF359=3,IF($AF$2=2,(Q359/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I359,Refurb_Poss_Tbl[%]))*AG359,Q359*$AG359),0)","v":0},{"$f":"IF($AF359=3,IF($AF$2=2,(U359/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I359,Refurb_Poss_Tbl[%]))*AG359,U359*$AG359),0)","v":0},{"$f":"IF($AF359=3,IF($AF$2=2,(V359/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I359,Refurb_Poss_Tbl[%]))*AG359,IF($AF$2=3,(V359*AG359)-AW359,V359*AG359)),0)","v":0},{"$f":"IF($AF359=3,IF($AF$2=2,(W359/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I359,Refurb_Poss_Tbl[%]))*AG359,W359*$AG359),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,55,0,{"$f":"VLOOKUP(AE360,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19676717080686118},0,0,0,0,0,0,0,0,1.2223632407607046E-4,{"$f":"IF(OR(AF360=3,AF360=2,AF360=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D360,FlatMaint!$Y$2:$Y$10000,AE360)*AG360,0)","v":1.9698926502147216},{"$f":"IF(OR(AF360=3,AF360=2,AF360=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D360,FlatRepair!$Y$2:$Y$10000,AE360)*AG360,0)","v":0},0,1.9700148865387976,0,0,0,0,0,1.9700148865387976,0,{"$f":"IF($AF360=3,IF($AF$2=2,(R360/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I360,Refurb_Poss_Tbl[%]))*AG360,IF($AF$2=3,(R360*AG360)-AV360,R360*AG360)),0)","v":0},{"$f":"IF(AF360=3,IF($AF$2=2,(S360/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I360,Refurb_Poss_Tbl[%]))*AG360,IF($AF$2=3,(S360*AG360)-AX360,S360*AG360)),0)","v":0},{"$f":"IF($AF360=3,IF($AF$2=2,(T360/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I360,Refurb_Poss_Tbl[%]))*AG360,T360*$AG360),0)","v":0},{"$f":"IF($AF360=3,IF($AF$2=2,(Q360/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I360,Refurb_Poss_Tbl[%]))*AG360,Q360*$AG360),0)","v":0},{"$f":"IF($AF360=3,IF($AF$2=2,(U360/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I360,Refurb_Poss_Tbl[%]))*AG360,U360*$AG360),0)","v":0},{"$f":"IF($AF360=3,IF($AF$2=2,(V360/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I360,Refurb_Poss_Tbl[%]))*AG360,IF($AF$2=3,(V360*AG360)-AW360,V360*AG360)),0)","v":0},{"$f":"IF($AF360=3,IF($AF$2=2,(W360/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I360,Refurb_Poss_Tbl[%]))*AG360,W360*$AG360),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,56,0,{"$f":"VLOOKUP(AE361,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19103608816200118},0,0,0,0,0,0,0,0,1.1867604279230144E-4,{"$f":"IF(OR(AF361=3,AF361=2,AF361=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D361,FlatMaint!$Y$2:$Y$10000,AE361)*AG361,0)","v":1.912517136130798},{"$f":"IF(OR(AF361=3,AF361=2,AF361=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D361,FlatRepair!$Y$2:$Y$10000,AE361)*AG361,0)","v":0},0,1.9126358121735902,0,0,0,0,0,1.9126358121735902,0,{"$f":"IF($AF361=3,IF($AF$2=2,(R361/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I361,Refurb_Poss_Tbl[%]))*AG361,IF($AF$2=3,(R361*AG361)-AV361,R361*AG361)),0)","v":0},{"$f":"IF(AF361=3,IF($AF$2=2,(S361/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I361,Refurb_Poss_Tbl[%]))*AG361,IF($AF$2=3,(S361*AG361)-AX361,S361*AG361)),0)","v":0},{"$f":"IF($AF361=3,IF($AF$2=2,(T361/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I361,Refurb_Poss_Tbl[%]))*AG361,T361*$AG361),0)","v":0},{"$f":"IF($AF361=3,IF($AF$2=2,(Q361/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I361,Refurb_Poss_Tbl[%]))*AG361,Q361*$AG361),0)","v":0},{"$f":"IF($AF361=3,IF($AF$2=2,(U361/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I361,Refurb_Poss_Tbl[%]))*AG361,U361*$AG361),0)","v":0},{"$f":"IF($AF361=3,IF($AF$2=2,(V361/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I361,Refurb_Poss_Tbl[%]))*AG361,IF($AF$2=3,(V361*AG361)-AW361,V361*AG361)),0)","v":0},{"$f":"IF($AF361=3,IF($AF$2=2,(W361/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I361,Refurb_Poss_Tbl[%]))*AG361,W361*$AG361),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,57,0,{"$f":"VLOOKUP(AE362,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18547193025437006},0,0,0,0,0,0,0,0,1.1521945902165186E-4,{"$f":"IF(OR(AF362=3,AF362=2,AF362=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D362,FlatMaint!$Y$2:$Y$10000,AE362)*AG362,0)","v":1.8568127535250463},{"$f":"IF(OR(AF362=3,AF362=2,AF362=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D362,FlatRepair!$Y$2:$Y$10000,AE362)*AG362,0)","v":0},0,1.856927972984068,0,0,0,0,0,1.856927972984068,0,{"$f":"IF($AF362=3,IF($AF$2=2,(R362/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I362,Refurb_Poss_Tbl[%]))*AG362,IF($AF$2=3,(R362*AG362)-AV362,R362*AG362)),0)","v":0},{"$f":"IF(AF362=3,IF($AF$2=2,(S362/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I362,Refurb_Poss_Tbl[%]))*AG362,IF($AF$2=3,(S362*AG362)-AX362,S362*AG362)),0)","v":0},{"$f":"IF($AF362=3,IF($AF$2=2,(T362/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I362,Refurb_Poss_Tbl[%]))*AG362,T362*$AG362),0)","v":0},{"$f":"IF($AF362=3,IF($AF$2=2,(Q362/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I362,Refurb_Poss_Tbl[%]))*AG362,Q362*$AG362),0)","v":0},{"$f":"IF($AF362=3,IF($AF$2=2,(U362/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I362,Refurb_Poss_Tbl[%]))*AG362,U362*$AG362),0)","v":0},{"$f":"IF($AF362=3,IF($AF$2=2,(V362/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I362,Refurb_Poss_Tbl[%]))*AG362,IF($AF$2=3,(V362*AG362)-AW362,V362*AG362)),0)","v":0},{"$f":"IF($AF362=3,IF($AF$2=2,(W362/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I362,Refurb_Poss_Tbl[%]))*AG362,W362*$AG362),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,58,0,{"$f":"VLOOKUP(AE363,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18006983519841754},0,0,0,0,0,0,0,0,1.1186355244820571E-4,{"$f":"IF(OR(AF363=3,AF363=2,AF363=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D363,FlatMaint!$Y$2:$Y$10000,AE363)*AG363,0)","v":1.8027308286650936},{"$f":"IF(OR(AF363=3,AF363=2,AF363=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D363,FlatRepair!$Y$2:$Y$10000,AE363)*AG363,0)","v":0},0,1.8028426922175418,0,0,0,0,0,1.8028426922175418,0,{"$f":"IF($AF363=3,IF($AF$2=2,(R363/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I363,Refurb_Poss_Tbl[%]))*AG363,IF($AF$2=3,(R363*AG363)-AV363,R363*AG363)),0)","v":0},{"$f":"IF(AF363=3,IF($AF$2=2,(S363/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I363,Refurb_Poss_Tbl[%]))*AG363,IF($AF$2=3,(S363*AG363)-AX363,S363*AG363)),0)","v":0},{"$f":"IF($AF363=3,IF($AF$2=2,(T363/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I363,Refurb_Poss_Tbl[%]))*AG363,T363*$AG363),0)","v":0},{"$f":"IF($AF363=3,IF($AF$2=2,(Q363/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I363,Refurb_Poss_Tbl[%]))*AG363,Q363*$AG363),0)","v":0},{"$f":"IF($AF363=3,IF($AF$2=2,(U363/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I363,Refurb_Poss_Tbl[%]))*AG363,U363*$AG363),0)","v":0},{"$f":"IF($AF363=3,IF($AF$2=2,(V363/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I363,Refurb_Poss_Tbl[%]))*AG363,IF($AF$2=3,(V363*AG363)-AW363,V363*AG363)),0)","v":0},{"$f":"IF($AF363=3,IF($AF$2=2,(W363/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I363,Refurb_Poss_Tbl[%]))*AG363,W363*$AG363),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,59,0,{"$f":"VLOOKUP(AE364,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.17482508271691022},0,0,0,0,0,0,0,0,1.086053907264133E-4,{"$f":"IF(OR(AF364=3,AF364=2,AF364=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D364,FlatMaint!$Y$2:$Y$10000,AE364)*AG364,0)","v":1.7502241055000907},{"$f":"IF(OR(AF364=3,AF364=2,AF364=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D364,FlatRepair!$Y$2:$Y$10000,AE364)*AG364,0)","v":0},0,1.7503327108908171,0,0,0,0,0,1.7503327108908171,0,{"$f":"IF($AF364=3,IF($AF$2=2,(R364/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I364,Refurb_Poss_Tbl[%]))*AG364,IF($AF$2=3,(R364*AG364)-AV364,R364*AG364)),0)","v":0},{"$f":"IF(AF364=3,IF($AF$2=2,(S364/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I364,Refurb_Poss_Tbl[%]))*AG364,IF($AF$2=3,(S364*AG364)-AX364,S364*AG364)),0)","v":0},{"$f":"IF($AF364=3,IF($AF$2=2,(T364/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I364,Refurb_Poss_Tbl[%]))*AG364,T364*$AG364),0)","v":0},{"$f":"IF($AF364=3,IF($AF$2=2,(Q364/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I364,Refurb_Poss_Tbl[%]))*AG364,Q364*$AG364),0)","v":0},{"$f":"IF($AF364=3,IF($AF$2=2,(U364/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I364,Refurb_Poss_Tbl[%]))*AG364,U364*$AG364),0)","v":0},{"$f":"IF($AF364=3,IF($AF$2=2,(V364/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I364,Refurb_Poss_Tbl[%]))*AG364,IF($AF$2=3,(V364*AG364)-AW364,V364*AG364)),0)","v":0},{"$f":"IF($AF364=3,IF($AF$2=2,(W364/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I364,Refurb_Poss_Tbl[%]))*AG364,W364*$AG364),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,60,0,{"$f":"VLOOKUP(AE365,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1697330900164177},0,0,0,0,0,0,0,0,1.0544212691884787E-4,{"$f":"IF(OR(AF365=3,AF365=2,AF365=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D365,FlatMaint!$Y$2:$Y$10000,AE365)*AG365,0)","v":1.6992467043690203},{"$f":"IF(OR(AF365=3,AF365=2,AF365=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D365,FlatRepair!$Y$2:$Y$10000,AE365)*AG365,0)","v":0},0,1.6993521464959391,0,0,0,0,0,1.6993521464959391,0,{"$f":"IF($AF365=3,IF($AF$2=2,(R365/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I365,Refurb_Poss_Tbl[%]))*AG365,IF($AF$2=3,(R365*AG365)-AV365,R365*AG365)),0)","v":0},{"$f":"IF(AF365=3,IF($AF$2=2,(S365/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I365,Refurb_Poss_Tbl[%]))*AG365,IF($AF$2=3,(S365*AG365)-AX365,S365*AG365)),0)","v":0},{"$f":"IF($AF365=3,IF($AF$2=2,(T365/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I365,Refurb_Poss_Tbl[%]))*AG365,T365*$AG365),0)","v":0},{"$f":"IF($AF365=3,IF($AF$2=2,(Q365/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I365,Refurb_Poss_Tbl[%]))*AG365,Q365*$AG365),0)","v":0},{"$f":"IF($AF365=3,IF($AF$2=2,(U365/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I365,Refurb_Poss_Tbl[%]))*AG365,U365*$AG365),0)","v":0},{"$f":"IF($AF365=3,IF($AF$2=2,(V365/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I365,Refurb_Poss_Tbl[%]))*AG365,IF($AF$2=3,(V365*AG365)-AW365,V365*AG365)),0)","v":0},{"$f":"IF($AF365=3,IF($AF$2=2,(W365/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I365,Refurb_Poss_Tbl[%]))*AG365,W365*$AG365),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,61,0,{"$f":"VLOOKUP(AE366,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.16478940778292983},0,0,0,0,0,0,0,0,1.0237099700859017E-4,{"$f":"IF(OR(AF366=3,AF366=2,AF366=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D366,FlatMaint!$Y$2:$Y$10000,AE366)*AG366,0)","v":1.6497540819116703},{"$f":"IF(OR(AF366=3,AF366=2,AF366=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D366,FlatRepair!$Y$2:$Y$10000,AE366)*AG366,0)","v":0},0,1.6498564529086788,0,0,0,0,0,1.6498564529086788,0,{"$f":"IF($AF366=3,IF($AF$2=2,(R366/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I366,Refurb_Poss_Tbl[%]))*AG366,IF($AF$2=3,(R366*AG366)-AV366,R366*AG366)),0)","v":0},{"$f":"IF(AF366=3,IF($AF$2=2,(S366/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I366,Refurb_Poss_Tbl[%]))*AG366,IF($AF$2=3,(S366*AG366)-AX366,S366*AG366)),0)","v":0},{"$f":"IF($AF366=3,IF($AF$2=2,(T366/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I366,Refurb_Poss_Tbl[%]))*AG366,T366*$AG366),0)","v":0},{"$f":"IF($AF366=3,IF($AF$2=2,(Q366/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I366,Refurb_Poss_Tbl[%]))*AG366,Q366*$AG366),0)","v":0},{"$f":"IF($AF366=3,IF($AF$2=2,(U366/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I366,Refurb_Poss_Tbl[%]))*AG366,U366*$AG366),0)","v":0},{"$f":"IF($AF366=3,IF($AF$2=2,(V366/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I366,Refurb_Poss_Tbl[%]))*AG366,IF($AF$2=3,(V366*AG366)-AW366,V366*AG366)),0)","v":0},{"$f":"IF($AF366=3,IF($AF$2=2,(W366/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I366,Refurb_Poss_Tbl[%]))*AG366,W366*$AG366),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,62,0,{"$f":"VLOOKUP(AE367,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15998971629410663},0,0,0,0,0,0,0,0,9.9389317484068135E-5,{"$f":"IF(OR(AF367=3,AF367=2,AF367=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D367,FlatMaint!$Y$2:$Y$10000,AE367)*AG367,0)","v":1.6017029921472528},{"$f":"IF(OR(AF367=3,AF367=2,AF367=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D367,FlatRepair!$Y$2:$Y$10000,AE367)*AG367,0)","v":0},0,1.6018023814647369,0,0,0,0,0,1.6018023814647369,0,{"$f":"IF($AF367=3,IF($AF$2=2,(R367/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I367,Refurb_Poss_Tbl[%]))*AG367,IF($AF$2=3,(R367*AG367)-AV367,R367*AG367)),0)","v":0},{"$f":"IF(AF367=3,IF($AF$2=2,(S367/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I367,Refurb_Poss_Tbl[%]))*AG367,IF($AF$2=3,(S367*AG367)-AX367,S367*AG367)),0)","v":0},{"$f":"IF($AF367=3,IF($AF$2=2,(T367/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I367,Refurb_Poss_Tbl[%]))*AG367,T367*$AG367),0)","v":0},{"$f":"IF($AF367=3,IF($AF$2=2,(Q367/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I367,Refurb_Poss_Tbl[%]))*AG367,Q367*$AG367),0)","v":0},{"$f":"IF($AF367=3,IF($AF$2=2,(U367/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I367,Refurb_Poss_Tbl[%]))*AG367,U367*$AG367),0)","v":0},{"$f":"IF($AF367=3,IF($AF$2=2,(V367/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I367,Refurb_Poss_Tbl[%]))*AG367,IF($AF$2=3,(V367*AG367)-AW367,V367*AG367)),0)","v":0},{"$f":"IF($AF367=3,IF($AF$2=2,(W367/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I367,Refurb_Poss_Tbl[%]))*AG367,W367*$AG367),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,63,0,{"$f":"VLOOKUP(AE368,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15532982164476369},0,0,0,0,0,0,0,0,9.649448299424089E-5,{"$f":"IF(OR(AF368=3,AF368=2,AF368=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D368,FlatMaint!$Y$2:$Y$10000,AE368)*AG368,0)","v":1.5550514486866529},{"$f":"IF(OR(AF368=3,AF368=2,AF368=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D368,FlatRepair!$Y$2:$Y$10000,AE368)*AG368,0)","v":0},0,1.5551479431696471,0,0,0,0,0,1.5551479431696471,0,{"$f":"IF($AF368=3,IF($AF$2=2,(R368/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I368,Refurb_Poss_Tbl[%]))*AG368,IF($AF$2=3,(R368*AG368)-AV368,R368*AG368)),0)","v":0},{"$f":"IF(AF368=3,IF($AF$2=2,(S368/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I368,Refurb_Poss_Tbl[%]))*AG368,IF($AF$2=3,(S368*AG368)-AX368,S368*AG368)),0)","v":0},{"$f":"IF($AF368=3,IF($AF$2=2,(T368/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I368,Refurb_Poss_Tbl[%]))*AG368,T368*$AG368),0)","v":0},{"$f":"IF($AF368=3,IF($AF$2=2,(Q368/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I368,Refurb_Poss_Tbl[%]))*AG368,Q368*$AG368),0)","v":0},{"$f":"IF($AF368=3,IF($AF$2=2,(U368/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I368,Refurb_Poss_Tbl[%]))*AG368,U368*$AG368),0)","v":0},{"$f":"IF($AF368=3,IF($AF$2=2,(V368/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I368,Refurb_Poss_Tbl[%]))*AG368,IF($AF$2=3,(V368*AG368)-AW368,V368*AG368)),0)","v":0},{"$f":"IF($AF368=3,IF($AF$2=2,(W368/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I368,Refurb_Poss_Tbl[%]))*AG368,W368*$AG368),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,64,0,{"$f":"VLOOKUP(AE369,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15080565208229488},0,0,0,0,0,0,0,0,9.3683964072078548E-5,{"$f":"IF(OR(AF369=3,AF369=2,AF369=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D369,FlatMaint!$Y$2:$Y$10000,AE369)*AG369,0)","v":1.5097586880452945},{"$f":"IF(OR(AF369=3,AF369=2,AF369=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D369,FlatRepair!$Y$2:$Y$10000,AE369)*AG369,0)","v":0},0,1.5098523720093666,0,0,0,0,0,1.5098523720093666,0,{"$f":"IF($AF369=3,IF($AF$2=2,(R369/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I369,Refurb_Poss_Tbl[%]))*AG369,IF($AF$2=3,(R369*AG369)-AV369,R369*AG369)),0)","v":0},{"$f":"IF(AF369=3,IF($AF$2=2,(S369/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I369,Refurb_Poss_Tbl[%]))*AG369,IF($AF$2=3,(S369*AG369)-AX369,S369*AG369)),0)","v":0},{"$f":"IF($AF369=3,IF($AF$2=2,(T369/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I369,Refurb_Poss_Tbl[%]))*AG369,T369*$AG369),0)","v":0},{"$f":"IF($AF369=3,IF($AF$2=2,(Q369/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I369,Refurb_Poss_Tbl[%]))*AG369,Q369*$AG369),0)","v":0},{"$f":"IF($AF369=3,IF($AF$2=2,(U369/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I369,Refurb_Poss_Tbl[%]))*AG369,U369*$AG369),0)","v":0},{"$f":"IF($AF369=3,IF($AF$2=2,(V369/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I369,Refurb_Poss_Tbl[%]))*AG369,IF($AF$2=3,(V369*AG369)-AW369,V369*AG369)),0)","v":0},{"$f":"IF($AF369=3,IF($AF$2=2,(W369/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I369,Refurb_Poss_Tbl[%]))*AG369,W369*$AG369),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,65,0,{"$f":"VLOOKUP(AE370,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14641325444882999},0,0,0,0,0,0,0,0,9.0955304924348113E-5,{"$f":"IF(OR(AF370=3,AF370=2,AF370=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D370,FlatMaint!$Y$2:$Y$10000,AE370)*AG370,0)","v":1.4657851340245578},{"$f":"IF(OR(AF370=3,AF370=2,AF370=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D370,FlatRepair!$Y$2:$Y$10000,AE370)*AG370,0)","v":0},0,1.4658760893294822,0,0,0,0,0,1.4658760893294822,0,{"$f":"IF($AF370=3,IF($AF$2=2,(R370/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I370,Refurb_Poss_Tbl[%]))*AG370,IF($AF$2=3,(R370*AG370)-AV370,R370*AG370)),0)","v":0},{"$f":"IF(AF370=3,IF($AF$2=2,(S370/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I370,Refurb_Poss_Tbl[%]))*AG370,IF($AF$2=3,(S370*AG370)-AX370,S370*AG370)),0)","v":0},{"$f":"IF($AF370=3,IF($AF$2=2,(T370/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I370,Refurb_Poss_Tbl[%]))*AG370,T370*$AG370),0)","v":0},{"$f":"IF($AF370=3,IF($AF$2=2,(Q370/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I370,Refurb_Poss_Tbl[%]))*AG370,Q370*$AG370),0)","v":0},{"$f":"IF($AF370=3,IF($AF$2=2,(U370/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I370,Refurb_Poss_Tbl[%]))*AG370,U370*$AG370),0)","v":0},{"$f":"IF($AF370=3,IF($AF$2=2,(V370/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I370,Refurb_Poss_Tbl[%]))*AG370,IF($AF$2=3,(V370*AG370)-AW370,V370*AG370)),0)","v":0},{"$f":"IF($AF370=3,IF($AF$2=2,(W370/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I370,Refurb_Poss_Tbl[%]))*AG370,W370*$AG370),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,66,0,{"$f":"VLOOKUP(AE371,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14214879072701941},0,0,0,0,0,0,0,0,8.8306121285774871E-5,{"$f":"IF(OR(AF371=3,AF371=2,AF371=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D371,FlatMaint!$Y$2:$Y$10000,AE371)*AG371,0)","v":1.4230923631306387},{"$f":"IF(OR(AF371=3,AF371=2,AF371=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D371,FlatRepair!$Y$2:$Y$10000,AE371)*AG371,0)","v":0},0,1.4231806692519244,0,0,0,0,0,1.4231806692519244,0,{"$f":"IF($AF371=3,IF($AF$2=2,(R371/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I371,Refurb_Poss_Tbl[%]))*AG371,IF($AF$2=3,(R371*AG371)-AV371,R371*AG371)),0)","v":0},{"$f":"IF(AF371=3,IF($AF$2=2,(S371/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I371,Refurb_Poss_Tbl[%]))*AG371,IF($AF$2=3,(S371*AG371)-AX371,S371*AG371)),0)","v":0},{"$f":"IF($AF371=3,IF($AF$2=2,(T371/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I371,Refurb_Poss_Tbl[%]))*AG371,T371*$AG371),0)","v":0},{"$f":"IF($AF371=3,IF($AF$2=2,(Q371/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I371,Refurb_Poss_Tbl[%]))*AG371,Q371*$AG371),0)","v":0},{"$f":"IF($AF371=3,IF($AF$2=2,(U371/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I371,Refurb_Poss_Tbl[%]))*AG371,U371*$AG371),0)","v":0},{"$f":"IF($AF371=3,IF($AF$2=2,(V371/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I371,Refurb_Poss_Tbl[%]))*AG371,IF($AF$2=3,(V371*AG371)-AW371,V371*AG371)),0)","v":0},{"$f":"IF($AF371=3,IF($AF$2=2,(W371/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I371,Refurb_Poss_Tbl[%]))*AG371,W371*$AG371),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,67,0,{"$f":"VLOOKUP(AE372,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1380085346864266},0,0,0,0,0,0,0,0,8.5734098335703746E-5,{"$f":"IF(OR(AF372=3,AF372=2,AF372=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D372,FlatMaint!$Y$2:$Y$10000,AE372)*AG372,0)","v":1.38164307100062},{"$f":"IF(OR(AF372=3,AF372=2,AF372=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D372,FlatRepair!$Y$2:$Y$10000,AE372)*AG372,0)","v":0},0,1.3817288050989558,0,0,0,0,0,1.3817288050989558,0,{"$f":"IF($AF372=3,IF($AF$2=2,(R372/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I372,Refurb_Poss_Tbl[%]))*AG372,IF($AF$2=3,(R372*AG372)-AV372,R372*AG372)),0)","v":0},{"$f":"IF(AF372=3,IF($AF$2=2,(S372/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I372,Refurb_Poss_Tbl[%]))*AG372,IF($AF$2=3,(S372*AG372)-AX372,S372*AG372)),0)","v":0},{"$f":"IF($AF372=3,IF($AF$2=2,(T372/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I372,Refurb_Poss_Tbl[%]))*AG372,T372*$AG372),0)","v":0},{"$f":"IF($AF372=3,IF($AF$2=2,(Q372/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I372,Refurb_Poss_Tbl[%]))*AG372,Q372*$AG372),0)","v":0},{"$f":"IF($AF372=3,IF($AF$2=2,(U372/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I372,Refurb_Poss_Tbl[%]))*AG372,U372*$AG372),0)","v":0},{"$f":"IF($AF372=3,IF($AF$2=2,(V372/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I372,Refurb_Poss_Tbl[%]))*AG372,IF($AF$2=3,(V372*AG372)-AW372,V372*AG372)),0)","v":0},{"$f":"IF($AF372=3,IF($AF$2=2,(W372/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I372,Refurb_Poss_Tbl[%]))*AG372,W372*$AG372),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,68,0,{"$f":"VLOOKUP(AE373,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13398886862759865},0,0,0,0,0,0,0,0,8.3236988675440535E-5,{"$f":"IF(OR(AF373=3,AF373=2,AF373=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D373,FlatMaint!$Y$2:$Y$10000,AE373)*AG373,0)","v":1.3414010398064273},{"$f":"IF(OR(AF373=3,AF373=2,AF373=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D373,FlatRepair!$Y$2:$Y$10000,AE373)*AG373,0)","v":0},0,1.3414842767951027,0,0,0,0,0,1.3414842767951027,0,{"$f":"IF($AF373=3,IF($AF$2=2,(R373/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I373,Refurb_Poss_Tbl[%]))*AG373,IF($AF$2=3,(R373*AG373)-AV373,R373*AG373)),0)","v":0},{"$f":"IF(AF373=3,IF($AF$2=2,(S373/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I373,Refurb_Poss_Tbl[%]))*AG373,IF($AF$2=3,(S373*AG373)-AX373,S373*AG373)),0)","v":0},{"$f":"IF($AF373=3,IF($AF$2=2,(T373/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I373,Refurb_Poss_Tbl[%]))*AG373,T373*$AG373),0)","v":0},{"$f":"IF($AF373=3,IF($AF$2=2,(Q373/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I373,Refurb_Poss_Tbl[%]))*AG373,Q373*$AG373),0)","v":0},{"$f":"IF($AF373=3,IF($AF$2=2,(U373/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I373,Refurb_Poss_Tbl[%]))*AG373,U373*$AG373),0)","v":0},{"$f":"IF($AF373=3,IF($AF$2=2,(V373/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I373,Refurb_Poss_Tbl[%]))*AG373,IF($AF$2=3,(V373*AG373)-AW373,V373*AG373)),0)","v":0},{"$f":"IF($AF373=3,IF($AF$2=2,(W373/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I373,Refurb_Poss_Tbl[%]))*AG373,W373*$AG373),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,69,0,{"$f":"VLOOKUP(AE374,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13008628022096957},0,0,0,0,0,0,0,0,8.0812610364505382E-5,{"$f":"IF(OR(AF374=3,AF374=2,AF374=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D374,FlatMaint!$Y$2:$Y$10000,AE374)*AG374,0)","v":1.302331106608182},{"$f":"IF(OR(AF374=3,AF374=2,AF374=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D374,FlatRepair!$Y$2:$Y$10000,AE374)*AG374,0)","v":0},0,1.3024119192185464,0,0,0,0,0,1.3024119192185464,0,{"$f":"IF($AF374=3,IF($AF$2=2,(R374/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I374,Refurb_Poss_Tbl[%]))*AG374,IF($AF$2=3,(R374*AG374)-AV374,R374*AG374)),0)","v":0},{"$f":"IF(AF374=3,IF($AF$2=2,(S374/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I374,Refurb_Poss_Tbl[%]))*AG374,IF($AF$2=3,(S374*AG374)-AX374,S374*AG374)),0)","v":0},{"$f":"IF($AF374=3,IF($AF$2=2,(T374/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I374,Refurb_Poss_Tbl[%]))*AG374,T374*$AG374),0)","v":0},{"$f":"IF($AF374=3,IF($AF$2=2,(Q374/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I374,Refurb_Poss_Tbl[%]))*AG374,Q374*$AG374),0)","v":0},{"$f":"IF($AF374=3,IF($AF$2=2,(U374/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I374,Refurb_Poss_Tbl[%]))*AG374,U374*$AG374),0)","v":0},{"$f":"IF($AF374=3,IF($AF$2=2,(V374/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I374,Refurb_Poss_Tbl[%]))*AG374,IF($AF$2=3,(V374*AG374)-AW374,V374*AG374)),0)","v":0},{"$f":"IF($AF374=3,IF($AF$2=2,(W374/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I374,Refurb_Poss_Tbl[%]))*AG374,W374*$AG374),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,70,0,{"$f":"VLOOKUP(AE375,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12629735943783454},0,0,0,0,0,0,0,0,7.8458845014082903E-5,{"$f":"IF(OR(AF375=3,AF375=2,AF375=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D375,FlatMaint!$Y$2:$Y$10000,AE375)*AG375,0)","v":1.2643991326293029},{"$f":"IF(OR(AF375=3,AF375=2,AF375=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D375,FlatRepair!$Y$2:$Y$10000,AE375)*AG375,0)","v":0},0,1.2644775914743169,0,0,0,0,0,1.2644775914743169,0,{"$f":"IF($AF375=3,IF($AF$2=2,(R375/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I375,Refurb_Poss_Tbl[%]))*AG375,IF($AF$2=3,(R375*AG375)-AV375,R375*AG375)),0)","v":0},{"$f":"IF(AF375=3,IF($AF$2=2,(S375/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I375,Refurb_Poss_Tbl[%]))*AG375,IF($AF$2=3,(S375*AG375)-AX375,S375*AG375)),0)","v":0},{"$f":"IF($AF375=3,IF($AF$2=2,(T375/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I375,Refurb_Poss_Tbl[%]))*AG375,T375*$AG375),0)","v":0},{"$f":"IF($AF375=3,IF($AF$2=2,(Q375/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I375,Refurb_Poss_Tbl[%]))*AG375,Q375*$AG375),0)","v":0},{"$f":"IF($AF375=3,IF($AF$2=2,(U375/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I375,Refurb_Poss_Tbl[%]))*AG375,U375*$AG375),0)","v":0},{"$f":"IF($AF375=3,IF($AF$2=2,(V375/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I375,Refurb_Poss_Tbl[%]))*AG375,IF($AF$2=3,(V375*AG375)-AW375,V375*AG375)),0)","v":0},{"$f":"IF($AF375=3,IF($AF$2=2,(W375/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I375,Refurb_Poss_Tbl[%]))*AG375,W375*$AG375),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,71,0,{"$f":"VLOOKUP(AE376,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12261879557071313},0,0,0,0,0,0,0,0,7.6173635936002809E-5,{"$f":"IF(OR(AF376=3,AF376=2,AF376=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D376,FlatMaint!$Y$2:$Y$10000,AE376)*AG376,0)","v":1.2275719734265074},{"$f":"IF(OR(AF376=3,AF376=2,AF376=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D376,FlatRepair!$Y$2:$Y$10000,AE376)*AG376,0)","v":0},0,1.2276481470624434,0,0,0,0,0,1.2276481470624434,0,{"$f":"IF($AF376=3,IF($AF$2=2,(R376/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I376,Refurb_Poss_Tbl[%]))*AG376,IF($AF$2=3,(R376*AG376)-AV376,R376*AG376)),0)","v":0},{"$f":"IF(AF376=3,IF($AF$2=2,(S376/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I376,Refurb_Poss_Tbl[%]))*AG376,IF($AF$2=3,(S376*AG376)-AX376,S376*AG376)),0)","v":0},{"$f":"IF($AF376=3,IF($AF$2=2,(T376/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I376,Refurb_Poss_Tbl[%]))*AG376,T376*$AG376),0)","v":0},{"$f":"IF($AF376=3,IF($AF$2=2,(Q376/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I376,Refurb_Poss_Tbl[%]))*AG376,Q376*$AG376),0)","v":0},{"$f":"IF($AF376=3,IF($AF$2=2,(U376/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I376,Refurb_Poss_Tbl[%]))*AG376,U376*$AG376),0)","v":0},{"$f":"IF($AF376=3,IF($AF$2=2,(V376/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I376,Refurb_Poss_Tbl[%]))*AG376,IF($AF$2=3,(V376*AG376)-AW376,V376*AG376)),0)","v":0},{"$f":"IF($AF376=3,IF($AF$2=2,(W376/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I376,Refurb_Poss_Tbl[%]))*AG376,W376*$AG376),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,72,0,{"$f":"VLOOKUP(AE377,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1190473743404982},0,0,0,0,0,0,0,0,7.3954986345633794E-5,{"$f":"IF(OR(AF377=3,AF377=2,AF377=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D377,FlatMaint!$Y$2:$Y$10000,AE377)*AG377,0)","v":1.191817449928648},{"$f":"IF(OR(AF377=3,AF377=2,AF377=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D377,FlatRepair!$Y$2:$Y$10000,AE377)*AG377,0)","v":0},0,1.1918914049149936,0,0,0,0,0,1.1918914049149936,0,{"$f":"IF($AF377=3,IF($AF$2=2,(R377/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I377,Refurb_Poss_Tbl[%]))*AG377,IF($AF$2=3,(R377*AG377)-AV377,R377*AG377)),0)","v":0},{"$f":"IF(AF377=3,IF($AF$2=2,(S377/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I377,Refurb_Poss_Tbl[%]))*AG377,IF($AF$2=3,(S377*AG377)-AX377,S377*AG377)),0)","v":0},{"$f":"IF($AF377=3,IF($AF$2=2,(T377/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I377,Refurb_Poss_Tbl[%]))*AG377,T377*$AG377),0)","v":0},{"$f":"IF($AF377=3,IF($AF$2=2,(Q377/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I377,Refurb_Poss_Tbl[%]))*AG377,Q377*$AG377),0)","v":0},{"$f":"IF($AF377=3,IF($AF$2=2,(U377/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I377,Refurb_Poss_Tbl[%]))*AG377,U377*$AG377),0)","v":0},{"$f":"IF($AF377=3,IF($AF$2=2,(V377/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I377,Refurb_Poss_Tbl[%]))*AG377,IF($AF$2=3,(V377*AG377)-AW377,V377*AG377)),0)","v":0},{"$f":"IF($AF377=3,IF($AF$2=2,(W377/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I377,Refurb_Poss_Tbl[%]))*AG377,W377*$AG377),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,73,0,{"$f":"VLOOKUP(AE378,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11557997508786232},0,0,0,0,0,0,0,0,7.1800957617120187E-5,{"$f":"IF(OR(AF378=3,AF378=2,AF378=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D378,FlatMaint!$Y$2:$Y$10000,AE378)*AG378,0)","v":1.1571043203190756},{"$f":"IF(OR(AF378=3,AF378=2,AF378=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D378,FlatRepair!$Y$2:$Y$10000,AE378)*AG378,0)","v":0},0,1.1571761212766927,0,0,0,0,0,1.1571761212766927,0,{"$f":"IF($AF378=3,IF($AF$2=2,(R378/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I378,Refurb_Poss_Tbl[%]))*AG378,IF($AF$2=3,(R378*AG378)-AV378,R378*AG378)),0)","v":0},{"$f":"IF(AF378=3,IF($AF$2=2,(S378/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I378,Refurb_Poss_Tbl[%]))*AG378,IF($AF$2=3,(S378*AG378)-AX378,S378*AG378)),0)","v":0},{"$f":"IF($AF378=3,IF($AF$2=2,(T378/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I378,Refurb_Poss_Tbl[%]))*AG378,T378*$AG378),0)","v":0},{"$f":"IF($AF378=3,IF($AF$2=2,(Q378/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I378,Refurb_Poss_Tbl[%]))*AG378,Q378*$AG378),0)","v":0},{"$f":"IF($AF378=3,IF($AF$2=2,(U378/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I378,Refurb_Poss_Tbl[%]))*AG378,U378*$AG378),0)","v":0},{"$f":"IF($AF378=3,IF($AF$2=2,(V378/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I378,Refurb_Poss_Tbl[%]))*AG378,IF($AF$2=3,(V378*AG378)-AW378,V378*AG378)),0)","v":0},{"$f":"IF($AF378=3,IF($AF$2=2,(W378/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I378,Refurb_Poss_Tbl[%]))*AG378,W378*$AG378),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,74,0,{"$f":"VLOOKUP(AE379,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11221356804646829},0,0,0,0,0,0,0,0,6.9709667589437079E-5,{"$f":"IF(OR(AF379=3,AF379=2,AF379=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D379,FlatMaint!$Y$2:$Y$10000,AE379)*AG379,0)","v":1.1234022527369669},{"$f":"IF(OR(AF379=3,AF379=2,AF379=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D379,FlatRepair!$Y$2:$Y$10000,AE379)*AG379,0)","v":0},0,1.1234719624045564,0,0,0,0,0,1.1234719624045564,0,{"$f":"IF($AF379=3,IF($AF$2=2,(R379/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I379,Refurb_Poss_Tbl[%]))*AG379,IF($AF$2=3,(R379*AG379)-AV379,R379*AG379)),0)","v":0},{"$f":"IF(AF379=3,IF($AF$2=2,(S379/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I379,Refurb_Poss_Tbl[%]))*AG379,IF($AF$2=3,(S379*AG379)-AX379,S379*AG379)),0)","v":0},{"$f":"IF($AF379=3,IF($AF$2=2,(T379/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I379,Refurb_Poss_Tbl[%]))*AG379,T379*$AG379),0)","v":0},{"$f":"IF($AF379=3,IF($AF$2=2,(Q379/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I379,Refurb_Poss_Tbl[%]))*AG379,Q379*$AG379),0)","v":0},{"$f":"IF($AF379=3,IF($AF$2=2,(U379/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I379,Refurb_Poss_Tbl[%]))*AG379,U379*$AG379),0)","v":0},{"$f":"IF($AF379=3,IF($AF$2=2,(V379/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I379,Refurb_Poss_Tbl[%]))*AG379,IF($AF$2=3,(V379*AG379)-AW379,V379*AG379)),0)","v":0},{"$f":"IF($AF379=3,IF($AF$2=2,(W379/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I379,Refurb_Poss_Tbl[%]))*AG379,W379*$AG379),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,75,0,{"$f":"VLOOKUP(AE380,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10894521169560026},0,0,0,0,0,0,0,0,6.7679288921783566E-5,{"$f":"IF(OR(AF380=3,AF380=2,AF380=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D380,FlatMaint!$Y$2:$Y$10000,AE380)*AG380,0)","v":1.090681798773754},{"$f":"IF(OR(AF380=3,AF380=2,AF380=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D380,FlatRepair!$Y$2:$Y$10000,AE380)*AG380,0)","v":0},0,1.0907494780626759,0,0,0,0,0,1.0907494780626759,0,{"$f":"IF($AF380=3,IF($AF$2=2,(R380/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I380,Refurb_Poss_Tbl[%]))*AG380,IF($AF$2=3,(R380*AG380)-AV380,R380*AG380)),0)","v":0},{"$f":"IF(AF380=3,IF($AF$2=2,(S380/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I380,Refurb_Poss_Tbl[%]))*AG380,IF($AF$2=3,(S380*AG380)-AX380,S380*AG380)),0)","v":0},{"$f":"IF($AF380=3,IF($AF$2=2,(T380/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I380,Refurb_Poss_Tbl[%]))*AG380,T380*$AG380),0)","v":0},{"$f":"IF($AF380=3,IF($AF$2=2,(Q380/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I380,Refurb_Poss_Tbl[%]))*AG380,Q380*$AG380),0)","v":0},{"$f":"IF($AF380=3,IF($AF$2=2,(U380/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I380,Refurb_Poss_Tbl[%]))*AG380,U380*$AG380),0)","v":0},{"$f":"IF($AF380=3,IF($AF$2=2,(V380/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I380,Refurb_Poss_Tbl[%]))*AG380,IF($AF$2=3,(V380*AG380)-AW380,V380*AG380)),0)","v":0},{"$f":"IF($AF380=3,IF($AF$2=2,(W380/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I380,Refurb_Poss_Tbl[%]))*AG380,W380*$AG380),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,76,0,{"$f":"VLOOKUP(AE381,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15310389176729922},0,0,0,0,0,0,0,0,9.5111683796810602E-5,{"$f":"IF(OR(AF381=3,AF381=2,AF381=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D381,FlatMaint!$Y$2:$Y$10000,AE381)*AG381,0)","v":1.5327670254897843},{"$f":"IF(OR(AF381=3,AF381=2,AF381=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D381,FlatRepair!$Y$2:$Y$10000,AE381)*AG381,0)","v":0},0,1.5328621371735811,0,0,0,0,0,1.5328621371735811,0,{"$f":"IF($AF381=3,IF($AF$2=2,(R381/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I381,Refurb_Poss_Tbl[%]))*AG381,IF($AF$2=3,(R381*AG381)-AV381,R381*AG381)),0)","v":0},{"$f":"IF(AF381=3,IF($AF$2=2,(S381/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I381,Refurb_Poss_Tbl[%]))*AG381,IF($AF$2=3,(S381*AG381)-AX381,S381*AG381)),0)","v":0},{"$f":"IF($AF381=3,IF($AF$2=2,(T381/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I381,Refurb_Poss_Tbl[%]))*AG381,T381*$AG381),0)","v":0},{"$f":"IF($AF381=3,IF($AF$2=2,(Q381/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I381,Refurb_Poss_Tbl[%]))*AG381,Q381*$AG381),0)","v":0},{"$f":"IF($AF381=3,IF($AF$2=2,(U381/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I381,Refurb_Poss_Tbl[%]))*AG381,U381*$AG381),0)","v":0},{"$f":"IF($AF381=3,IF($AF$2=2,(V381/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I381,Refurb_Poss_Tbl[%]))*AG381,IF($AF$2=3,(V381*AG381)-AW381,V381*AG381)),0)","v":0},{"$f":"IF($AF381=3,IF($AF$2=2,(W381/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I381,Refurb_Poss_Tbl[%]))*AG381,W381*$AG381),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,77,0,{"$f":"VLOOKUP(AE382,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14936965050468218},0,0,0,0,0,0,0,0,9.2791886631034745E-5,{"$f":"IF(OR(AF382=3,AF382=2,AF382=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D382,FlatMaint!$Y$2:$Y$10000,AE382)*AG382,0)","v":1.4953824638924726},{"$f":"IF(OR(AF382=3,AF382=2,AF382=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D382,FlatRepair!$Y$2:$Y$10000,AE382)*AG382,0)","v":0},0,1.4954752557791038,0,0,0,0,0,1.4954752557791038,0,{"$f":"IF($AF382=3,IF($AF$2=2,(R382/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I382,Refurb_Poss_Tbl[%]))*AG382,IF($AF$2=3,(R382*AG382)-AV382,R382*AG382)),0)","v":0},{"$f":"IF(AF382=3,IF($AF$2=2,(S382/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I382,Refurb_Poss_Tbl[%]))*AG382,IF($AF$2=3,(S382*AG382)-AX382,S382*AG382)),0)","v":0},{"$f":"IF($AF382=3,IF($AF$2=2,(T382/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I382,Refurb_Poss_Tbl[%]))*AG382,T382*$AG382),0)","v":0},{"$f":"IF($AF382=3,IF($AF$2=2,(Q382/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I382,Refurb_Poss_Tbl[%]))*AG382,Q382*$AG382),0)","v":0},{"$f":"IF($AF382=3,IF($AF$2=2,(U382/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I382,Refurb_Poss_Tbl[%]))*AG382,U382*$AG382),0)","v":0},{"$f":"IF($AF382=3,IF($AF$2=2,(V382/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I382,Refurb_Poss_Tbl[%]))*AG382,IF($AF$2=3,(V382*AG382)-AW382,V382*AG382)),0)","v":0},{"$f":"IF($AF382=3,IF($AF$2=2,(W382/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I382,Refurb_Poss_Tbl[%]))*AG382,W382*$AG382),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,78,0,{"$f":"VLOOKUP(AE383,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14572648829725093},0,0,0,0,0,0,0,0,9.0528669883936351E-5,{"$f":"IF(OR(AF383=3,AF383=2,AF383=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D383,FlatMaint!$Y$2:$Y$10000,AE383)*AG383,0)","v":1.4589097208707054},{"$f":"IF(OR(AF383=3,AF383=2,AF383=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D383,FlatRepair!$Y$2:$Y$10000,AE383)*AG383,0)","v":0},0,1.4590002495405894,0,0,0,0,0,1.4590002495405894,0,{"$f":"IF($AF383=3,IF($AF$2=2,(R383/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I383,Refurb_Poss_Tbl[%]))*AG383,IF($AF$2=3,(R383*AG383)-AV383,R383*AG383)),0)","v":0},{"$f":"IF(AF383=3,IF($AF$2=2,(S383/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I383,Refurb_Poss_Tbl[%]))*AG383,IF($AF$2=3,(S383*AG383)-AX383,S383*AG383)),0)","v":0},{"$f":"IF($AF383=3,IF($AF$2=2,(T383/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I383,Refurb_Poss_Tbl[%]))*AG383,T383*$AG383),0)","v":0},{"$f":"IF($AF383=3,IF($AF$2=2,(Q383/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I383,Refurb_Poss_Tbl[%]))*AG383,Q383*$AG383),0)","v":0},{"$f":"IF($AF383=3,IF($AF$2=2,(U383/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I383,Refurb_Poss_Tbl[%]))*AG383,U383*$AG383),0)","v":0},{"$f":"IF($AF383=3,IF($AF$2=2,(V383/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I383,Refurb_Poss_Tbl[%]))*AG383,IF($AF$2=3,(V383*AG383)-AW383,V383*AG383)),0)","v":0},{"$f":"IF($AF383=3,IF($AF$2=2,(W383/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I383,Refurb_Poss_Tbl[%]))*AG383,W383*$AG383),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,79,0,{"$f":"VLOOKUP(AE384,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14217218370463502},0,0,0,0,0,0,0,0,8.8320653545303739E-5,{"$f":"IF(OR(AF384=3,AF384=2,AF384=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D384,FlatMaint!$Y$2:$Y$10000,AE384)*AG384,0)","v":1.4233265569470293},{"$f":"IF(OR(AF384=3,AF384=2,AF384=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D384,FlatRepair!$Y$2:$Y$10000,AE384)*AG384,0)","v":0},0,1.4234148776005746,0,0,0,0,0,1.4234148776005746,0,{"$f":"IF($AF384=3,IF($AF$2=2,(R384/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I384,Refurb_Poss_Tbl[%]))*AG384,IF($AF$2=3,(R384*AG384)-AV384,R384*AG384)),0)","v":0},{"$f":"IF(AF384=3,IF($AF$2=2,(S384/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I384,Refurb_Poss_Tbl[%]))*AG384,IF($AF$2=3,(S384*AG384)-AX384,S384*AG384)),0)","v":0},{"$f":"IF($AF384=3,IF($AF$2=2,(T384/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I384,Refurb_Poss_Tbl[%]))*AG384,T384*$AG384),0)","v":0},{"$f":"IF($AF384=3,IF($AF$2=2,(Q384/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I384,Refurb_Poss_Tbl[%]))*AG384,Q384*$AG384),0)","v":0},{"$f":"IF($AF384=3,IF($AF$2=2,(U384/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I384,Refurb_Poss_Tbl[%]))*AG384,U384*$AG384),0)","v":0},{"$f":"IF($AF384=3,IF($AF$2=2,(V384/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I384,Refurb_Poss_Tbl[%]))*AG384,IF($AF$2=3,(V384*AG384)-AW384,V384*AG384)),0)","v":0},{"$f":"IF($AF384=3,IF($AF$2=2,(W384/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I384,Refurb_Poss_Tbl[%]))*AG384,W384*$AG384),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,80,2,{"$f":"VLOOKUP(AE385,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13870456946793663},0,0,0,0,0,0,0,0,8.6166491263710973E-5,{"$f":"IF(OR(AF385=3,AF385=2,AF385=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D385,FlatMaint!$Y$2:$Y$10000,AE385)*AG385,0)","v":1.3886112750702726},{"$f":"IF(OR(AF385=3,AF385=2,AF385=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D385,FlatRepair!$Y$2:$Y$10000,AE385)*AG385,0)","v":0},0,1.3886974415615363,0.3551152533199729,0,0,0,0,1.7438126948815091,0,{"$f":"IF($AF385=3,IF($AF$2=2,(R385/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I385,Refurb_Poss_Tbl[%]))*AG385,IF($AF$2=3,(R385*AG385)-AV385,R385*AG385)),0)","v":0},{"$f":"IF(AF385=3,IF($AF$2=2,(S385/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I385,Refurb_Poss_Tbl[%]))*AG385,IF($AF$2=3,(S385*AG385)-AX385,S385*AG385)),0)","v":0},{"$f":"IF($AF385=3,IF($AF$2=2,(T385/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I385,Refurb_Poss_Tbl[%]))*AG385,T385*$AG385),0)","v":0},{"$f":"IF($AF385=3,IF($AF$2=2,(Q385/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I385,Refurb_Poss_Tbl[%]))*AG385,Q385*$AG385),0)","v":0},{"$f":"IF($AF385=3,IF($AF$2=2,(U385/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I385,Refurb_Poss_Tbl[%]))*AG385,U385*$AG385),0)","v":0},{"$f":"IF($AF385=3,IF($AF$2=2,(V385/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I385,Refurb_Poss_Tbl[%]))*AG385,IF($AF$2=3,(V385*AG385)-AW385,V385*AG385)),0)","v":0},{"$f":"IF($AF385=3,IF($AF$2=2,(W385/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I385,Refurb_Poss_Tbl[%]))*AG385,W385*$AG385),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,81,0,{"$f":"VLOOKUP(AE386,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13532153118823087},0,0,0,0,0,0,0,0,8.406486952557169E-5,{"$f":"IF(OR(AF386=3,AF386=2,AF386=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D386,FlatMaint!$Y$2:$Y$10000,AE386)*AG386,0)","v":1.354742707385632},{"$f":"IF(OR(AF386=3,AF386=2,AF386=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D386,FlatRepair!$Y$2:$Y$10000,AE386)*AG386,0)","v":0},0,1.3548267722551575,0,0,0,0,0,1.3548267722551575,0,{"$f":"IF($AF386=3,IF($AF$2=2,(R386/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I386,Refurb_Poss_Tbl[%]))*AG386,IF($AF$2=3,(R386*AG386)-AV386,R386*AG386)),0)","v":0},{"$f":"IF(AF386=3,IF($AF$2=2,(S386/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I386,Refurb_Poss_Tbl[%]))*AG386,IF($AF$2=3,(S386*AG386)-AX386,S386*AG386)),0)","v":0},{"$f":"IF($AF386=3,IF($AF$2=2,(T386/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I386,Refurb_Poss_Tbl[%]))*AG386,T386*$AG386),0)","v":0},{"$f":"IF($AF386=3,IF($AF$2=2,(Q386/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I386,Refurb_Poss_Tbl[%]))*AG386,Q386*$AG386),0)","v":0},{"$f":"IF($AF386=3,IF($AF$2=2,(U386/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I386,Refurb_Poss_Tbl[%]))*AG386,U386*$AG386),0)","v":0},{"$f":"IF($AF386=3,IF($AF$2=2,(V386/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I386,Refurb_Poss_Tbl[%]))*AG386,IF($AF$2=3,(V386*AG386)-AW386,V386*AG386)),0)","v":0},{"$f":"IF($AF386=3,IF($AF$2=2,(W386/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I386,Refurb_Poss_Tbl[%]))*AG386,W386*$AG386),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,82,0,{"$f":"VLOOKUP(AE387,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13202100603729841},{"$f":"IF(AE387=0,Q387*AG387,0)","v":0},{"$f":"IF(AE387=0,R387*AG387,0)","v":0},{"$f":"IF(AE387=0,S387*AG387,0)","v":0},{"$f":"IF(AE387=0,T387*AG387,0)","v":0},{"$f":"IF(AE387=0,U387*AG387,0)","v":0},{"$f":"IF(AE387=0,V387*AG387,0)","v":0},{"$f":"IF(AE387=0,W387*AG387,0)","v":0},{"$f":"IF(AE387=0,AH387+AI387+AJ387+AK387+AL387+AM387+AN387,0)","v":0},{"$f":"IF(OR(AF387=3,AF387=2,AF387=0),Y387*AG387,0)","v":8.201450685421629E-5},{"$f":"IF(OR(AF387=3,AF387=2,AF387=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D387,FlatMaint!$Y$2:$Y$10000,AE387)*AG387,0)","v":1.3217002023274458},{"$f":"IF(OR(AF387=3,AF387=2,AF387=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D387,FlatRepair!$Y$2:$Y$10000,AE387)*AG387,0)","v":0},{"$f":"IF(OR(AF387=3,AF387=2,AF387=0),Z387*AG387,0)","v":0},{"$f":"AP387+AQ387+AR387+AS387","v":1.3217822168343001},{"$f":"IF(AF387=2,AA387*AG387,0)","v":0},{"$f":"IF(AF387=3,AB387*AG387,0)","v":0},{"$f":"IF(AF387=3,AC387*AG387,0)","v":0},{"$f":"IF(AF387=3,AD387*AG387,0)","v":0},{"$f":"IF($AF$2=3,BB387+BC387+BD387+BE387+BF387+BG387+BH387,BB387+BC387+BD387+BE387+BF387+BG387+BH387)","v":0},{"$f":"AO387+AT387+AU387+AV387+AW387+AX387+AY387+BA387","v":1.3217822168343001},{"$f":"IFERROR(IF(AE387=100,IF(O387=3,(N387/H387)*(X387*AG387)*-1,(N387/M387)*(X387*AG387)*-1),0),0)","v":0},{"$f":"IF($AF387=3,IF($AF$2=2,(R387/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I387,Refurb_Poss_Tbl[%]))*AG387,IF($AF$2=3,(R387*AG387)-AV387,R387*AG387)),0)","v":0},{"$f":"IF(AF387=3,IF($AF$2=2,(S387/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I387,Refurb_Poss_Tbl[%]))*AG387,IF($AF$2=3,(S387*AG387)-AX387,S387*AG387)),0)","v":0},{"$f":"IF($AF387=3,IF($AF$2=2,(T387/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I387,Refurb_Poss_Tbl[%]))*AG387,T387*$AG387),0)","v":0},{"$f":"IF($AF387=3,IF($AF$2=2,(Q387/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I387,Refurb_Poss_Tbl[%]))*AG387,Q387*$AG387),0)","v":0},{"$f":"IF($AF387=3,IF($AF$2=2,(U387/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I387,Refurb_Poss_Tbl[%]))*AG387,U387*$AG387),0)","v":0},{"$f":"IF($AF387=3,IF($AF$2=2,(V387/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I387,Refurb_Poss_Tbl[%]))*AG387,IF($AF$2=3,(V387*AG387)-AW387,V387*AG387)),0)","v":0},{"$f":"IF($AF387=3,IF($AF$2=2,(W387/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I387,Refurb_Poss_Tbl[%]))*AG387,W387*$AG387),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,83,0,{"$f":"VLOOKUP(AE388,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12880098149980332},0,0,0,0,0,0,0,0,8.0014153028503684E-5,{"$f":"IF(OR(AF388=3,AF388=2,AF388=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D388,FlatMaint!$Y$2:$Y$10000,AE388)*AG388,0)","v":1.2894636120267764},{"$f":"IF(OR(AF388=3,AF388=2,AF388=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D388,FlatRepair!$Y$2:$Y$10000,AE388)*AG388,0)","v":0},0,1.289543626179805,0,0,0,0,0,1.289543626179805,0,{"$f":"IF($AF388=3,IF($AF$2=2,(R388/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I388,Refurb_Poss_Tbl[%]))*AG388,IF($AF$2=3,(R388*AG388)-AV388,R388*AG388)),0)","v":0},{"$f":"IF(AF388=3,IF($AF$2=2,(S388/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I388,Refurb_Poss_Tbl[%]))*AG388,IF($AF$2=3,(S388*AG388)-AX388,S388*AG388)),0)","v":0},{"$f":"IF($AF388=3,IF($AF$2=2,(T388/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I388,Refurb_Poss_Tbl[%]))*AG388,T388*$AG388),0)","v":0},{"$f":"IF($AF388=3,IF($AF$2=2,(Q388/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I388,Refurb_Poss_Tbl[%]))*AG388,Q388*$AG388),0)","v":0},{"$f":"IF($AF388=3,IF($AF$2=2,(U388/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I388,Refurb_Poss_Tbl[%]))*AG388,U388*$AG388),0)","v":0},{"$f":"IF($AF388=3,IF($AF$2=2,(V388/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I388,Refurb_Poss_Tbl[%]))*AG388,IF($AF$2=3,(V388*AG388)-AW388,V388*AG388)),0)","v":0},{"$f":"IF($AF388=3,IF($AF$2=2,(W388/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I388,Refurb_Poss_Tbl[%]))*AG388,W388*$AG388),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,84,0,{"$f":"VLOOKUP(AE389,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1256594941461496},0,0,0,0,0,0,0,0,7.8062588320491417E-5,{"$f":"IF(OR(AF389=3,AF389=2,AF389=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D389,FlatMaint!$Y$2:$Y$10000,AE389)*AG389,0)","v":1.2580132800261234},{"$f":"IF(OR(AF389=3,AF389=2,AF389=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D389,FlatRepair!$Y$2:$Y$10000,AE389)*AG389,0)","v":0},0,1.258091342614444,0,0,0,0,0,1.258091342614444,0,{"$f":"IF($AF389=3,IF($AF$2=2,(R389/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I389,Refurb_Poss_Tbl[%]))*AG389,IF($AF$2=3,(R389*AG389)-AV389,R389*AG389)),0)","v":0},{"$f":"IF(AF389=3,IF($AF$2=2,(S389/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I389,Refurb_Poss_Tbl[%]))*AG389,IF($AF$2=3,(S389*AG389)-AX389,S389*AG389)),0)","v":0},{"$f":"IF($AF389=3,IF($AF$2=2,(T389/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I389,Refurb_Poss_Tbl[%]))*AG389,T389*$AG389),0)","v":0},{"$f":"IF($AF389=3,IF($AF$2=2,(Q389/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I389,Refurb_Poss_Tbl[%]))*AG389,Q389*$AG389),0)","v":0},{"$f":"IF($AF389=3,IF($AF$2=2,(U389/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I389,Refurb_Poss_Tbl[%]))*AG389,U389*$AG389),0)","v":0},{"$f":"IF($AF389=3,IF($AF$2=2,(V389/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I389,Refurb_Poss_Tbl[%]))*AG389,IF($AF$2=3,(V389*AG389)-AW389,V389*AG389)),0)","v":0},{"$f":"IF($AF389=3,IF($AF$2=2,(W389/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I389,Refurb_Poss_Tbl[%]))*AG389,W389*$AG389),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,85,0,{"$f":"VLOOKUP(AE390,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1225946284352679},0,0,0,0,0,0,0,0,7.6158622751698935E-5,{"$f":"IF(OR(AF390=3,AF390=2,AF390=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D390,FlatMaint!$Y$2:$Y$10000,AE390)*AG390,0)","v":1.227330029293779},{"$f":"IF(OR(AF390=3,AF390=2,AF390=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D390,FlatRepair!$Y$2:$Y$10000,AE390)*AG390,0)","v":0},0,1.2274061879165308,0,0,0,0,0,1.2274061879165308,0,{"$f":"IF($AF390=3,IF($AF$2=2,(R390/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I390,Refurb_Poss_Tbl[%]))*AG390,IF($AF$2=3,(R390*AG390)-AV390,R390*AG390)),0)","v":0},{"$f":"IF(AF390=3,IF($AF$2=2,(S390/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I390,Refurb_Poss_Tbl[%]))*AG390,IF($AF$2=3,(S390*AG390)-AX390,S390*AG390)),0)","v":0},{"$f":"IF($AF390=3,IF($AF$2=2,(T390/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I390,Refurb_Poss_Tbl[%]))*AG390,T390*$AG390),0)","v":0},{"$f":"IF($AF390=3,IF($AF$2=2,(Q390/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I390,Refurb_Poss_Tbl[%]))*AG390,Q390*$AG390),0)","v":0},{"$f":"IF($AF390=3,IF($AF$2=2,(U390/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I390,Refurb_Poss_Tbl[%]))*AG390,U390*$AG390),0)","v":0},{"$f":"IF($AF390=3,IF($AF$2=2,(V390/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I390,Refurb_Poss_Tbl[%]))*AG390,IF($AF$2=3,(V390*AG390)-AW390,V390*AG390)),0)","v":0},{"$f":"IF($AF390=3,IF($AF$2=2,(W390/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I390,Refurb_Poss_Tbl[%]))*AG390,W390*$AG390),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,86,0,{"$f":"VLOOKUP(AE391,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11960451554660284},0,0,0,0,0,0,0,0,7.4301095367511162E-5,{"$f":"IF(OR(AF391=3,AF391=2,AF391=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D391,FlatMaint!$Y$2:$Y$10000,AE391)*AG391,0)","v":1.1973951505305163},{"$f":"IF(OR(AF391=3,AF391=2,AF391=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D391,FlatRepair!$Y$2:$Y$10000,AE391)*AG391,0)","v":0},0,1.1974694516258837,0,0,0,0,0,1.1974694516258837,0,{"$f":"IF($AF391=3,IF($AF$2=2,(R391/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I391,Refurb_Poss_Tbl[%]))*AG391,IF($AF$2=3,(R391*AG391)-AV391,R391*AG391)),0)","v":0},{"$f":"IF(AF391=3,IF($AF$2=2,(S391/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I391,Refurb_Poss_Tbl[%]))*AG391,IF($AF$2=3,(S391*AG391)-AX391,S391*AG391)),0)","v":0},{"$f":"IF($AF391=3,IF($AF$2=2,(T391/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I391,Refurb_Poss_Tbl[%]))*AG391,T391*$AG391),0)","v":0},{"$f":"IF($AF391=3,IF($AF$2=2,(Q391/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I391,Refurb_Poss_Tbl[%]))*AG391,Q391*$AG391),0)","v":0},{"$f":"IF($AF391=3,IF($AF$2=2,(U391/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I391,Refurb_Poss_Tbl[%]))*AG391,U391*$AG391),0)","v":0},{"$f":"IF($AF391=3,IF($AF$2=2,(V391/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I391,Refurb_Poss_Tbl[%]))*AG391,IF($AF$2=3,(V391*AG391)-AW391,V391*AG391)),0)","v":0},{"$f":"IF($AF391=3,IF($AF$2=2,(W391/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I391,Refurb_Poss_Tbl[%]))*AG391,W391*$AG391),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,87,0,{"$f":"VLOOKUP(AE392,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11668733224058814},0,0,0,0,0,0,0,0,7.2488873529279185E-5,{"$f":"IF(OR(AF392=3,AF392=2,AF392=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D392,FlatMaint!$Y$2:$Y$10000,AE392)*AG392,0)","v":1.1681903907614792},{"$f":"IF(OR(AF392=3,AF392=2,AF392=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D392,FlatRepair!$Y$2:$Y$10000,AE392)*AG392,0)","v":0},0,1.1682628796350085,0,0,0,0,0,1.1682628796350085,0,{"$f":"IF($AF392=3,IF($AF$2=2,(R392/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I392,Refurb_Poss_Tbl[%]))*AG392,IF($AF$2=3,(R392*AG392)-AV392,R392*AG392)),0)","v":0},{"$f":"IF(AF392=3,IF($AF$2=2,(S392/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I392,Refurb_Poss_Tbl[%]))*AG392,IF($AF$2=3,(S392*AG392)-AX392,S392*AG392)),0)","v":0},{"$f":"IF($AF392=3,IF($AF$2=2,(T392/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I392,Refurb_Poss_Tbl[%]))*AG392,T392*$AG392),0)","v":0},{"$f":"IF($AF392=3,IF($AF$2=2,(Q392/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I392,Refurb_Poss_Tbl[%]))*AG392,Q392*$AG392),0)","v":0},{"$f":"IF($AF392=3,IF($AF$2=2,(U392/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I392,Refurb_Poss_Tbl[%]))*AG392,U392*$AG392),0)","v":0},{"$f":"IF($AF392=3,IF($AF$2=2,(V392/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I392,Refurb_Poss_Tbl[%]))*AG392,IF($AF$2=3,(V392*AG392)-AW392,V392*AG392)),0)","v":0},{"$f":"IF($AF392=3,IF($AF$2=2,(W392/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I392,Refurb_Poss_Tbl[%]))*AG392,W392*$AG392),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,88,0,{"$f":"VLOOKUP(AE393,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11384129974691526},0,0,0,0,0,0,0,0,7.072085222368702E-5,{"$f":"IF(OR(AF393=3,AF393=2,AF393=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D393,FlatMaint!$Y$2:$Y$10000,AE393)*AG393,0)","v":1.1396979422063211},{"$f":"IF(OR(AF393=3,AF393=2,AF393=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D393,FlatRepair!$Y$2:$Y$10000,AE393)*AG393,0)","v":0},0,1.1397686630585449,0,0,0,0,0,1.1397686630585449,0,{"$f":"IF($AF393=3,IF($AF$2=2,(R393/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I393,Refurb_Poss_Tbl[%]))*AG393,IF($AF$2=3,(R393*AG393)-AV393,R393*AG393)),0)","v":0},{"$f":"IF(AF393=3,IF($AF$2=2,(S393/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I393,Refurb_Poss_Tbl[%]))*AG393,IF($AF$2=3,(S393*AG393)-AX393,S393*AG393)),0)","v":0},{"$f":"IF($AF393=3,IF($AF$2=2,(T393/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I393,Refurb_Poss_Tbl[%]))*AG393,T393*$AG393),0)","v":0},{"$f":"IF($AF393=3,IF($AF$2=2,(Q393/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I393,Refurb_Poss_Tbl[%]))*AG393,Q393*$AG393),0)","v":0},{"$f":"IF($AF393=3,IF($AF$2=2,(U393/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I393,Refurb_Poss_Tbl[%]))*AG393,U393*$AG393),0)","v":0},{"$f":"IF($AF393=3,IF($AF$2=2,(V393/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I393,Refurb_Poss_Tbl[%]))*AG393,IF($AF$2=3,(V393*AG393)-AW393,V393*AG393)),0)","v":0},{"$f":"IF($AF393=3,IF($AF$2=2,(W393/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I393,Refurb_Poss_Tbl[%]))*AG393,W393*$AG393),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,89,0,{"$f":"VLOOKUP(AE394,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11106468267991736},0,0,0,0,0,0,0,0,6.8995953388962963E-5,{"$f":"IF(OR(AF394=3,AF394=2,AF394=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D394,FlatMaint!$Y$2:$Y$10000,AE394)*AG394,0)","v":1.1119004314208014},{"$f":"IF(OR(AF394=3,AF394=2,AF394=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D394,FlatRepair!$Y$2:$Y$10000,AE394)*AG394,0)","v":0},0,1.1119694273741905,0,0,0,0,0,1.1119694273741905,0,{"$f":"IF($AF394=3,IF($AF$2=2,(R394/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I394,Refurb_Poss_Tbl[%]))*AG394,IF($AF$2=3,(R394*AG394)-AV394,R394*AG394)),0)","v":0},{"$f":"IF(AF394=3,IF($AF$2=2,(S394/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I394,Refurb_Poss_Tbl[%]))*AG394,IF($AF$2=3,(S394*AG394)-AX394,S394*AG394)),0)","v":0},{"$f":"IF($AF394=3,IF($AF$2=2,(T394/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I394,Refurb_Poss_Tbl[%]))*AG394,T394*$AG394),0)","v":0},{"$f":"IF($AF394=3,IF($AF$2=2,(Q394/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I394,Refurb_Poss_Tbl[%]))*AG394,Q394*$AG394),0)","v":0},{"$f":"IF($AF394=3,IF($AF$2=2,(U394/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I394,Refurb_Poss_Tbl[%]))*AG394,U394*$AG394),0)","v":0},{"$f":"IF($AF394=3,IF($AF$2=2,(V394/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I394,Refurb_Poss_Tbl[%]))*AG394,IF($AF$2=3,(V394*AG394)-AW394,V394*AG394)),0)","v":0},{"$f":"IF($AF394=3,IF($AF$2=2,(W394/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I394,Refurb_Poss_Tbl[%]))*AG394,W394*$AG394),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,90,0,{"$f":"VLOOKUP(AE395,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10835578798040717},0,0,0,0,0,0,0,0,6.7313125257524836E-5,{"$f":"IF(OR(AF395=3,AF395=2,AF395=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D395,FlatMaint!$Y$2:$Y$10000,AE395)*AG395,0)","v":1.0847809087032207},{"$f":"IF(OR(AF395=3,AF395=2,AF395=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D395,FlatRepair!$Y$2:$Y$10000,AE395)*AG395,0)","v":0},0,1.0848482218284783,0,0,0,0,0,1.0848482218284783,0,{"$f":"IF($AF395=3,IF($AF$2=2,(R395/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I395,Refurb_Poss_Tbl[%]))*AG395,IF($AF$2=3,(R395*AG395)-AV395,R395*AG395)),0)","v":0},{"$f":"IF(AF395=3,IF($AF$2=2,(S395/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I395,Refurb_Poss_Tbl[%]))*AG395,IF($AF$2=3,(S395*AG395)-AX395,S395*AG395)),0)","v":0},{"$f":"IF($AF395=3,IF($AF$2=2,(T395/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I395,Refurb_Poss_Tbl[%]))*AG395,T395*$AG395),0)","v":0},{"$f":"IF($AF395=3,IF($AF$2=2,(Q395/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I395,Refurb_Poss_Tbl[%]))*AG395,Q395*$AG395),0)","v":0},{"$f":"IF($AF395=3,IF($AF$2=2,(U395/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I395,Refurb_Poss_Tbl[%]))*AG395,U395*$AG395),0)","v":0},{"$f":"IF($AF395=3,IF($AF$2=2,(V395/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I395,Refurb_Poss_Tbl[%]))*AG395,IF($AF$2=3,(V395*AG395)-AW395,V395*AG395)),0)","v":0},{"$f":"IF($AF395=3,IF($AF$2=2,(W395/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I395,Refurb_Poss_Tbl[%]))*AG395,W395*$AG395),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,91,0,{"$f":"VLOOKUP(AE396,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10571296388332406},0,0,0,0,0,0,0,0,6.5671341714658375E-5,{"$f":"IF(OR(AF396=3,AF396=2,AF396=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D396,FlatMaint!$Y$2:$Y$10000,AE396)*AG396,0)","v":1.0583228377592397},{"$f":"IF(OR(AF396=3,AF396=2,AF396=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D396,FlatRepair!$Y$2:$Y$10000,AE396)*AG396,0)","v":0},0,1.0583885091009544,0,0,0,0,0,1.0583885091009544,0,{"$f":"IF($AF396=3,IF($AF$2=2,(R396/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I396,Refurb_Poss_Tbl[%]))*AG396,IF($AF$2=3,(R396*AG396)-AV396,R396*AG396)),0)","v":0},{"$f":"IF(AF396=3,IF($AF$2=2,(S396/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I396,Refurb_Poss_Tbl[%]))*AG396,IF($AF$2=3,(S396*AG396)-AX396,S396*AG396)),0)","v":0},{"$f":"IF($AF396=3,IF($AF$2=2,(T396/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I396,Refurb_Poss_Tbl[%]))*AG396,T396*$AG396),0)","v":0},{"$f":"IF($AF396=3,IF($AF$2=2,(Q396/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I396,Refurb_Poss_Tbl[%]))*AG396,Q396*$AG396),0)","v":0},{"$f":"IF($AF396=3,IF($AF$2=2,(U396/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I396,Refurb_Poss_Tbl[%]))*AG396,U396*$AG396),0)","v":0},{"$f":"IF($AF396=3,IF($AF$2=2,(V396/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I396,Refurb_Poss_Tbl[%]))*AG396,IF($AF$2=3,(V396*AG396)-AW396,V396*AG396)),0)","v":0},{"$f":"IF($AF396=3,IF($AF$2=2,(W396/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I396,Refurb_Poss_Tbl[%]))*AG396,W396*$AG396),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,92,0,{"$f":"VLOOKUP(AE397,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10313459891056008},0,0,0,0,0,0,0,0,6.4069601672837447E-5,{"$f":"IF(OR(AF397=3,AF397=2,AF397=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D397,FlatMaint!$Y$2:$Y$10000,AE397)*AG397,0)","v":1.0325100856187708},{"$f":"IF(OR(AF397=3,AF397=2,AF397=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D397,FlatRepair!$Y$2:$Y$10000,AE397)*AG397,0)","v":0},0,1.0325741552204437,0,0,0,0,0,1.0325741552204437,0,{"$f":"IF($AF397=3,IF($AF$2=2,(R397/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I397,Refurb_Poss_Tbl[%]))*AG397,IF($AF$2=3,(R397*AG397)-AV397,R397*AG397)),0)","v":0},{"$f":"IF(AF397=3,IF($AF$2=2,(S397/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I397,Refurb_Poss_Tbl[%]))*AG397,IF($AF$2=3,(S397*AG397)-AX397,S397*AG397)),0)","v":0},{"$f":"IF($AF397=3,IF($AF$2=2,(T397/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I397,Refurb_Poss_Tbl[%]))*AG397,T397*$AG397),0)","v":0},{"$f":"IF($AF397=3,IF($AF$2=2,(Q397/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I397,Refurb_Poss_Tbl[%]))*AG397,Q397*$AG397),0)","v":0},{"$f":"IF($AF397=3,IF($AF$2=2,(U397/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I397,Refurb_Poss_Tbl[%]))*AG397,U397*$AG397),0)","v":0},{"$f":"IF($AF397=3,IF($AF$2=2,(V397/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I397,Refurb_Poss_Tbl[%]))*AG397,IF($AF$2=3,(V397*AG397)-AW397,V397*AG397)),0)","v":0},{"$f":"IF($AF397=3,IF($AF$2=2,(W397/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I397,Refurb_Poss_Tbl[%]))*AG397,W397*$AG397),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,93,0,{"$f":"VLOOKUP(AE398,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10061912088835129},0,0,0,0,0,0,0,0,6.2506928461304815E-5,{"$f":"IF(OR(AF398=3,AF398=2,AF398=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D398,FlatMaint!$Y$2:$Y$10000,AE398)*AG398,0)","v":1.0073269127988007},{"$f":"IF(OR(AF398=3,AF398=2,AF398=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D398,FlatRepair!$Y$2:$Y$10000,AE398)*AG398,0)","v":0},0,1.0073894197272619,0,0,0,0,0,1.0073894197272619,0,{"$f":"IF($AF398=3,IF($AF$2=2,(R398/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I398,Refurb_Poss_Tbl[%]))*AG398,IF($AF$2=3,(R398*AG398)-AV398,R398*AG398)),0)","v":0},{"$f":"IF(AF398=3,IF($AF$2=2,(S398/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I398,Refurb_Poss_Tbl[%]))*AG398,IF($AF$2=3,(S398*AG398)-AX398,S398*AG398)),0)","v":0},{"$f":"IF($AF398=3,IF($AF$2=2,(T398/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I398,Refurb_Poss_Tbl[%]))*AG398,T398*$AG398),0)","v":0},{"$f":"IF($AF398=3,IF($AF$2=2,(Q398/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I398,Refurb_Poss_Tbl[%]))*AG398,Q398*$AG398),0)","v":0},{"$f":"IF($AF398=3,IF($AF$2=2,(U398/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I398,Refurb_Poss_Tbl[%]))*AG398,U398*$AG398),0)","v":0},{"$f":"IF($AF398=3,IF($AF$2=2,(V398/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I398,Refurb_Poss_Tbl[%]))*AG398,IF($AF$2=3,(V398*AG398)-AW398,V398*AG398)),0)","v":0},{"$f":"IF($AF398=3,IF($AF$2=2,(W398/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I398,Refurb_Poss_Tbl[%]))*AG398,W398*$AG398),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,94,0,{"$f":"VLOOKUP(AE399,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.8164995988635415E-2},0,0,0,0,0,0,0,0,6.0982369230541297E-5,{"$f":"IF(OR(AF399=3,AF399=2,AF399=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D399,FlatMaint!$Y$2:$Y$10000,AE399)*AG399,0)","v":0.9827579637061471},{"$f":"IF(OR(AF399=3,AF399=2,AF399=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D399,FlatRepair!$Y$2:$Y$10000,AE399)*AG399,0)","v":0},0,0.98281894607537768,0,0,0,0,0,0.98281894607537768,0,{"$f":"IF($AF399=3,IF($AF$2=2,(R399/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I399,Refurb_Poss_Tbl[%]))*AG399,IF($AF$2=3,(R399*AG399)-AV399,R399*AG399)),0)","v":0},{"$f":"IF(AF399=3,IF($AF$2=2,(S399/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I399,Refurb_Poss_Tbl[%]))*AG399,IF($AF$2=3,(S399*AG399)-AX399,S399*AG399)),0)","v":0},{"$f":"IF($AF399=3,IF($AF$2=2,(T399/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I399,Refurb_Poss_Tbl[%]))*AG399,T399*$AG399),0)","v":0},{"$f":"IF($AF399=3,IF($AF$2=2,(Q399/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I399,Refurb_Poss_Tbl[%]))*AG399,Q399*$AG399),0)","v":0},{"$f":"IF($AF399=3,IF($AF$2=2,(U399/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I399,Refurb_Poss_Tbl[%]))*AG399,U399*$AG399),0)","v":0},{"$f":"IF($AF399=3,IF($AF$2=2,(V399/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I399,Refurb_Poss_Tbl[%]))*AG399,IF($AF$2=3,(V399*AG399)-AW399,V399*AG399)),0)","v":0},{"$f":"IF($AF399=3,IF($AF$2=2,(W399/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I399,Refurb_Poss_Tbl[%]))*AG399,W399*$AG399),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,95,0,{"$f":"VLOOKUP(AE400,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.577072779379063E-2},0,0,0,0,0,0,0,0,5.9494994371259788E-5,{"$f":"IF(OR(AF400=3,AF400=2,AF400=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D400,FlatMaint!$Y$2:$Y$10000,AE400)*AG400,0)","v":0.95878825727428962},{"$f":"IF(OR(AF400=3,AF400=2,AF400=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D400,FlatRepair!$Y$2:$Y$10000,AE400)*AG400,0)","v":0},0,0.95884775226866092,0,0,0,0,0,0.95884775226866092,0,{"$f":"IF($AF400=3,IF($AF$2=2,(R400/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I400,Refurb_Poss_Tbl[%]))*AG400,IF($AF$2=3,(R400*AG400)-AV400,R400*AG400)),0)","v":0},{"$f":"IF(AF400=3,IF($AF$2=2,(S400/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I400,Refurb_Poss_Tbl[%]))*AG400,IF($AF$2=3,(S400*AG400)-AX400,S400*AG400)),0)","v":0},{"$f":"IF($AF400=3,IF($AF$2=2,(T400/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I400,Refurb_Poss_Tbl[%]))*AG400,T400*$AG400),0)","v":0},{"$f":"IF($AF400=3,IF($AF$2=2,(Q400/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I400,Refurb_Poss_Tbl[%]))*AG400,Q400*$AG400),0)","v":0},{"$f":"IF($AF400=3,IF($AF$2=2,(U400/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I400,Refurb_Poss_Tbl[%]))*AG400,U400*$AG400),0)","v":0},{"$f":"IF($AF400=3,IF($AF$2=2,(V400/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I400,Refurb_Poss_Tbl[%]))*AG400,IF($AF$2=3,(V400*AG400)-AW400,V400*AG400)),0)","v":0},{"$f":"IF($AF400=3,IF($AF$2=2,(W400/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I400,Refurb_Poss_Tbl[%]))*AG400,W400*$AG400),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,96,0,{"$f":"VLOOKUP(AE401,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.3434856384185999E-2},0,0,0,0,0,0,0,0,5.8043896947570538E-5,{"$f":"IF(OR(AF401=3,AF401=2,AF401=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D401,FlatMaint!$Y$2:$Y$10000,AE401)*AG401,0)","v":0.93540317782857541},{"$f":"IF(OR(AF401=3,AF401=2,AF401=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D401,FlatRepair!$Y$2:$Y$10000,AE401)*AG401,0)","v":0},0,0.93546122172552293,0,0,0,0,0,0.93546122172552293,0,{"$f":"IF($AF401=3,IF($AF$2=2,(R401/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I401,Refurb_Poss_Tbl[%]))*AG401,IF($AF$2=3,(R401*AG401)-AV401,R401*AG401)),0)","v":0},{"$f":"IF(AF401=3,IF($AF$2=2,(S401/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I401,Refurb_Poss_Tbl[%]))*AG401,IF($AF$2=3,(S401*AG401)-AX401,S401*AG401)),0)","v":0},{"$f":"IF($AF401=3,IF($AF$2=2,(T401/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I401,Refurb_Poss_Tbl[%]))*AG401,T401*$AG401),0)","v":0},{"$f":"IF($AF401=3,IF($AF$2=2,(Q401/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I401,Refurb_Poss_Tbl[%]))*AG401,Q401*$AG401),0)","v":0},{"$f":"IF($AF401=3,IF($AF$2=2,(U401/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I401,Refurb_Poss_Tbl[%]))*AG401,U401*$AG401),0)","v":0},{"$f":"IF($AF401=3,IF($AF$2=2,(V401/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I401,Refurb_Poss_Tbl[%]))*AG401,IF($AF$2=3,(V401*AG401)-AW401,V401*AG401)),0)","v":0},{"$f":"IF($AF401=3,IF($AF$2=2,(W401/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I401,Refurb_Poss_Tbl[%]))*AG401,W401*$AG401),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,97,0,{"$f":"VLOOKUP(AE402,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.1155957447986352E-2},0,0,0,0,0,0,0,0,5.6628192143971267E-5,{"$f":"IF(OR(AF402=3,AF402=2,AF402=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D402,FlatMaint!$Y$2:$Y$10000,AE402)*AG402,0)","v":0.91258846617422007},{"$f":"IF(OR(AF402=3,AF402=2,AF402=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D402,FlatRepair!$Y$2:$Y$10000,AE402)*AG402,0)","v":0},0,0.9126450943663641,0,0,0,0,0,0.9126450943663641,0,{"$f":"IF($AF402=3,IF($AF$2=2,(R402/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I402,Refurb_Poss_Tbl[%]))*AG402,IF($AF$2=3,(R402*AG402)-AV402,R402*AG402)),0)","v":0},{"$f":"IF(AF402=3,IF($AF$2=2,(S402/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I402,Refurb_Poss_Tbl[%]))*AG402,IF($AF$2=3,(S402*AG402)-AX402,S402*AG402)),0)","v":0},{"$f":"IF($AF402=3,IF($AF$2=2,(T402/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I402,Refurb_Poss_Tbl[%]))*AG402,T402*$AG402),0)","v":0},{"$f":"IF($AF402=3,IF($AF$2=2,(Q402/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I402,Refurb_Poss_Tbl[%]))*AG402,Q402*$AG402),0)","v":0},{"$f":"IF($AF402=3,IF($AF$2=2,(U402/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I402,Refurb_Poss_Tbl[%]))*AG402,U402*$AG402),0)","v":0},{"$f":"IF($AF402=3,IF($AF$2=2,(V402/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I402,Refurb_Poss_Tbl[%]))*AG402,IF($AF$2=3,(V402*AG402)-AW402,V402*AG402)),0)","v":0},{"$f":"IF($AF402=3,IF($AF$2=2,(W402/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I402,Refurb_Poss_Tbl[%]))*AG402,W402*$AG402),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,98,0,{"$f":"VLOOKUP(AE403,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.8932641412669614E-2},0,0,0,0,0,0,0,0,5.5247016725825621E-5,{"$f":"IF(OR(AF403=3,AF403=2,AF403=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D403,FlatMaint!$Y$2:$Y$10000,AE403)*AG403,0)","v":0.89033021090167808},{"$f":"IF(OR(AF403=3,AF403=2,AF403=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D403,FlatRepair!$Y$2:$Y$10000,AE403)*AG403,0)","v":0},0,0.89038545791840396,0,0,0,0,0,0.89038545791840396,0,{"$f":"IF($AF403=3,IF($AF$2=2,(R403/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I403,Refurb_Poss_Tbl[%]))*AG403,IF($AF$2=3,(R403*AG403)-AV403,R403*AG403)),0)","v":0},{"$f":"IF(AF403=3,IF($AF$2=2,(S403/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I403,Refurb_Poss_Tbl[%]))*AG403,IF($AF$2=3,(S403*AG403)-AX403,S403*AG403)),0)","v":0},{"$f":"IF($AF403=3,IF($AF$2=2,(T403/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I403,Refurb_Poss_Tbl[%]))*AG403,T403*$AG403),0)","v":0},{"$f":"IF($AF403=3,IF($AF$2=2,(Q403/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I403,Refurb_Poss_Tbl[%]))*AG403,Q403*$AG403),0)","v":0},{"$f":"IF($AF403=3,IF($AF$2=2,(U403/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I403,Refurb_Poss_Tbl[%]))*AG403,U403*$AG403),0)","v":0},{"$f":"IF($AF403=3,IF($AF$2=2,(V403/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I403,Refurb_Poss_Tbl[%]))*AG403,IF($AF$2=3,(V403*AG403)-AW403,V403*AG403)),0)","v":0},{"$f":"IF($AF403=3,IF($AF$2=2,(W403/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I403,Refurb_Poss_Tbl[%]))*AG403,W403*$AG403),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,99,0,{"$f":"VLOOKUP(AE404,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.6763552597726459E-2},0,0,0,0,0,0,0,0,5.389952851300061E-5,{"$f":"IF(OR(AF404=3,AF404=2,AF404=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D404,FlatMaint!$Y$2:$Y$10000,AE404)*AG404,0)","v":0.86861483990407629},{"$f":"IF(OR(AF404=3,AF404=2,AF404=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D404,FlatRepair!$Y$2:$Y$10000,AE404)*AG404,0)","v":0},0,0.86866873943258927,0,0,0,0,0,0.86866873943258927,0,{"$f":"IF($AF404=3,IF($AF$2=2,(R404/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I404,Refurb_Poss_Tbl[%]))*AG404,IF($AF$2=3,(R404*AG404)-AV404,R404*AG404)),0)","v":0},{"$f":"IF(AF404=3,IF($AF$2=2,(S404/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I404,Refurb_Poss_Tbl[%]))*AG404,IF($AF$2=3,(S404*AG404)-AX404,S404*AG404)),0)","v":0},{"$f":"IF($AF404=3,IF($AF$2=2,(T404/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I404,Refurb_Poss_Tbl[%]))*AG404,T404*$AG404),0)","v":0},{"$f":"IF($AF404=3,IF($AF$2=2,(Q404/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I404,Refurb_Poss_Tbl[%]))*AG404,Q404*$AG404),0)","v":0},{"$f":"IF($AF404=3,IF($AF$2=2,(U404/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I404,Refurb_Poss_Tbl[%]))*AG404,U404*$AG404),0)","v":0},{"$f":"IF($AF404=3,IF($AF$2=2,(V404/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I404,Refurb_Poss_Tbl[%]))*AG404,IF($AF$2=3,(V404*AG404)-AW404,V404*AG404)),0)","v":0},{"$f":"IF($AF404=3,IF($AF$2=2,(W404/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I404,Refurb_Poss_Tbl[%]))*AG404,W404*$AG404),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9960000000000004,9.9960000000000004,9.8487154300000004E-2,5.5466773983717299E-2,1.4645867812704599E-3,6.2363981349547098E-2,0,2.7127509136874998E-2,10.240910005551401,6.21223162252268E-4,0,2.5602275013878502,0.15372255177562499,7.3229339063522801E-4,2.7733386991858702E-2,100,0,{"$f":"VLOOKUP(AE405,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.4647368388025807E-2},0,0,0,0,0,0,0,0,5.2584905866342058E-5,{"$f":"IF(OR(AF405=3,AF405=2,AF405=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D405,FlatMaint!$Y$2:$Y$10000,AE405)*AG405,0)","v":0.84742911210153782},{"$f":"IF(OR(AF405=3,AF405=2,AF405=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D405,FlatRepair!$Y$2:$Y$10000,AE405)*AG405,0)","v":0},0,0.84748169700740417,0,0,0,0,0,0.84748169700740417,0,{"$f":"IF($AF405=3,IF($AF$2=2,(R405/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I405,Refurb_Poss_Tbl[%]))*AG405,IF($AF$2=3,(R405*AG405)-AV405,R405*AG405)),0)","v":0},{"$f":"IF(AF405=3,IF($AF$2=2,(S405/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I405,Refurb_Poss_Tbl[%]))*AG405,IF($AF$2=3,(S405*AG405)-AX405,S405*AG405)),0)","v":0},{"$f":"IF($AF405=3,IF($AF$2=2,(T405/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I405,Refurb_Poss_Tbl[%]))*AG405,T405*$AG405),0)","v":0},{"$f":"IF($AF405=3,IF($AF$2=2,(Q405/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I405,Refurb_Poss_Tbl[%]))*AG405,Q405*$AG405),0)","v":0},{"$f":"IF($AF405=3,IF($AF$2=2,(U405/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I405,Refurb_Poss_Tbl[%]))*AG405,U405*$AG405),0)","v":0},{"$f":"IF($AF405=3,IF($AF$2=2,(V405/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I405,Refurb_Poss_Tbl[%]))*AG405,IF($AF$2=3,(V405*AG405)-AW405,V405*AG405)),0)","v":0},{"$f":"IF($AF405=3,IF($AF$2=2,(W405/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I405,Refurb_Poss_Tbl[%]))*AG405,W405*$AG405),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,0,1,{"$f":"VLOOKUP(AE406,ValidationLists!$M$1:$N$102,2,FALSE)","v":1},3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.2131670570465869,0,{"$f":"IF(OR(AF406=3,AF406=2,AF406=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D406,FlatMaint!$Y$2:$Y$10000,AE406)*AG406,0)","v":0},{"$f":"IF(OR(AF406=3,AF406=2,AF406=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D406,FlatRepair!$Y$2:$Y$10000,AE406)*AG406,0)","v":0},0,0,0,0,0,0,0,3.2131670570465869,0,{"$f":"IF($AF406=3,IF($AF$2=2,(R406/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I406,Refurb_Poss_Tbl[%]))*AG406,IF($AF$2=3,(R406*AG406)-AV406,R406*AG406)),0)","v":0},{"$f":"IF(AF406=3,IF($AF$2=2,(S406/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I406,Refurb_Poss_Tbl[%]))*AG406,IF($AF$2=3,(S406*AG406)-AX406,S406*AG406)),0)","v":0},{"$f":"IF($AF406=3,IF($AF$2=2,(T406/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I406,Refurb_Poss_Tbl[%]))*AG406,T406*$AG406),0)","v":0},{"$f":"IF($AF406=3,IF($AF$2=2,(Q406/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I406,Refurb_Poss_Tbl[%]))*AG406,Q406*$AG406),0)","v":0},{"$f":"IF($AF406=3,IF($AF$2=2,(U406/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I406,Refurb_Poss_Tbl[%]))*AG406,U406*$AG406),0)","v":0},{"$f":"IF($AF406=3,IF($AF$2=2,(V406/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I406,Refurb_Poss_Tbl[%]))*AG406,IF($AF$2=3,(V406*AG406)-AW406,V406*AG406)),0)","v":0},{"$f":"IF($AF406=3,IF($AF$2=2,(W406/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I406,Refurb_Poss_Tbl[%]))*AG406,W406*$AG406),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,1,0,{"$f":"VLOOKUP(AE407,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.96618357487922713},0,0,0,0,0,0,0,0,1.8500043137054207E-4,{"$f":"IF(OR(AF407=3,AF407=2,AF407=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D407,FlatMaint!$Y$2:$Y$10000,AE407)*AG407,0)","v":0.31245136038647353},{"$f":"IF(OR(AF407=3,AF407=2,AF407=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D407,FlatRepair!$Y$2:$Y$10000,AE407)*AG407,0)","v":0},0,0.31263636081784407,0,0,0,0,0,0.31263636081784407,0,{"$f":"IF($AF407=3,IF($AF$2=2,(R407/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I407,Refurb_Poss_Tbl[%]))*AG407,IF($AF$2=3,(R407*AG407)-AV407,R407*AG407)),0)","v":0},{"$f":"IF(AF407=3,IF($AF$2=2,(S407/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I407,Refurb_Poss_Tbl[%]))*AG407,IF($AF$2=3,(S407*AG407)-AX407,S407*AG407)),0)","v":0},{"$f":"IF($AF407=3,IF($AF$2=2,(T407/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I407,Refurb_Poss_Tbl[%]))*AG407,T407*$AG407),0)","v":0},{"$f":"IF($AF407=3,IF($AF$2=2,(Q407/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I407,Refurb_Poss_Tbl[%]))*AG407,Q407*$AG407),0)","v":0},{"$f":"IF($AF407=3,IF($AF$2=2,(U407/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I407,Refurb_Poss_Tbl[%]))*AG407,U407*$AG407),0)","v":0},{"$f":"IF($AF407=3,IF($AF$2=2,(V407/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I407,Refurb_Poss_Tbl[%]))*AG407,IF($AF$2=3,(V407*AG407)-AW407,V407*AG407)),0)","v":0},{"$f":"IF($AF407=3,IF($AF$2=2,(W407/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I407,Refurb_Poss_Tbl[%]))*AG407,W407*$AG407),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,2,0,{"$f":"VLOOKUP(AE408,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.93351070036640305},0,0,0,0,0,0,0,0,1.7874437813578944E-4,{"$f":"IF(OR(AF408=3,AF408=2,AF408=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D408,FlatMaint!$Y$2:$Y$10000,AE408)*AG408,0)","v":0.30188537235408069},{"$f":"IF(OR(AF408=3,AF408=2,AF408=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D408,FlatRepair!$Y$2:$Y$10000,AE408)*AG408,0)","v":0},0,0.3020641167322165,0,0,0,0,0,0.3020641167322165,0,{"$f":"IF($AF408=3,IF($AF$2=2,(R408/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I408,Refurb_Poss_Tbl[%]))*AG408,IF($AF$2=3,(R408*AG408)-AV408,R408*AG408)),0)","v":0},{"$f":"IF(AF408=3,IF($AF$2=2,(S408/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I408,Refurb_Poss_Tbl[%]))*AG408,IF($AF$2=3,(S408*AG408)-AX408,S408*AG408)),0)","v":0},{"$f":"IF($AF408=3,IF($AF$2=2,(T408/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I408,Refurb_Poss_Tbl[%]))*AG408,T408*$AG408),0)","v":0},{"$f":"IF($AF408=3,IF($AF$2=2,(Q408/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I408,Refurb_Poss_Tbl[%]))*AG408,Q408*$AG408),0)","v":0},{"$f":"IF($AF408=3,IF($AF$2=2,(U408/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I408,Refurb_Poss_Tbl[%]))*AG408,U408*$AG408),0)","v":0},{"$f":"IF($AF408=3,IF($AF$2=2,(V408/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I408,Refurb_Poss_Tbl[%]))*AG408,IF($AF$2=3,(V408*AG408)-AW408,V408*AG408)),0)","v":0},{"$f":"IF($AF408=3,IF($AF$2=2,(W408/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I408,Refurb_Poss_Tbl[%]))*AG408,W408*$AG408),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,3,0,{"$f":"VLOOKUP(AE409,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.90194270566802237},0,0,0,0,0,0,0,0,1.726998822568014E-4,{"$f":"IF(OR(AF409=3,AF409=2,AF409=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D409,FlatMaint!$Y$2:$Y$10000,AE409)*AG409,0)","v":0.2916766882648123},{"$f":"IF(OR(AF409=3,AF409=2,AF409=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D409,FlatRepair!$Y$2:$Y$10000,AE409)*AG409,0)","v":0},0,0.29184938814706912,0,0,0,0,0,0.29184938814706912,0,{"$f":"IF($AF409=3,IF($AF$2=2,(R409/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I409,Refurb_Poss_Tbl[%]))*AG409,IF($AF$2=3,(R409*AG409)-AV409,R409*AG409)),0)","v":0},{"$f":"IF(AF409=3,IF($AF$2=2,(S409/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I409,Refurb_Poss_Tbl[%]))*AG409,IF($AF$2=3,(S409*AG409)-AX409,S409*AG409)),0)","v":0},{"$f":"IF($AF409=3,IF($AF$2=2,(T409/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I409,Refurb_Poss_Tbl[%]))*AG409,T409*$AG409),0)","v":0},{"$f":"IF($AF409=3,IF($AF$2=2,(Q409/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I409,Refurb_Poss_Tbl[%]))*AG409,Q409*$AG409),0)","v":0},{"$f":"IF($AF409=3,IF($AF$2=2,(U409/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I409,Refurb_Poss_Tbl[%]))*AG409,U409*$AG409),0)","v":0},{"$f":"IF($AF409=3,IF($AF$2=2,(V409/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I409,Refurb_Poss_Tbl[%]))*AG409,IF($AF$2=3,(V409*AG409)-AW409,V409*AG409)),0)","v":0},{"$f":"IF($AF409=3,IF($AF$2=2,(W409/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I409,Refurb_Poss_Tbl[%]))*AG409,W409*$AG409),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,4,0,{"$f":"VLOOKUP(AE410,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.87144222769857238},0,0,0,0,0,0,0,0,1.6685978962009798E-4,{"$f":"IF(OR(AF410=3,AF410=2,AF410=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D410,FlatMaint!$Y$2:$Y$10000,AE410)*AG410,0)","v":0.28181322537663028},{"$f":"IF(OR(AF410=3,AF410=2,AF410=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D410,FlatRepair!$Y$2:$Y$10000,AE410)*AG410,0)","v":0},0,0.28198008516625039,0,0,0,0,0,0.28198008516625039,0,{"$f":"IF($AF410=3,IF($AF$2=2,(R410/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I410,Refurb_Poss_Tbl[%]))*AG410,IF($AF$2=3,(R410*AG410)-AV410,R410*AG410)),0)","v":0},{"$f":"IF(AF410=3,IF($AF$2=2,(S410/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I410,Refurb_Poss_Tbl[%]))*AG410,IF($AF$2=3,(S410*AG410)-AX410,S410*AG410)),0)","v":0},{"$f":"IF($AF410=3,IF($AF$2=2,(T410/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I410,Refurb_Poss_Tbl[%]))*AG410,T410*$AG410),0)","v":0},{"$f":"IF($AF410=3,IF($AF$2=2,(Q410/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I410,Refurb_Poss_Tbl[%]))*AG410,Q410*$AG410),0)","v":0},{"$f":"IF($AF410=3,IF($AF$2=2,(U410/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I410,Refurb_Poss_Tbl[%]))*AG410,U410*$AG410),0)","v":0},{"$f":"IF($AF410=3,IF($AF$2=2,(V410/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I410,Refurb_Poss_Tbl[%]))*AG410,IF($AF$2=3,(V410*AG410)-AW410,V410*AG410)),0)","v":0},{"$f":"IF($AF410=3,IF($AF$2=2,(W410/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I410,Refurb_Poss_Tbl[%]))*AG410,W410*$AG410),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,5,0,{"$f":"VLOOKUP(AE411,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.84197316685852419},0,0,0,0,0,0,0,0,1.6121718803874203E-4,{"$f":"IF(OR(AF411=3,AF411=2,AF411=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D411,FlatMaint!$Y$2:$Y$10000,AE411)*AG411,0)","v":0.27228330954263796},{"$f":"IF(OR(AF411=3,AF411=2,AF411=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D411,FlatRepair!$Y$2:$Y$10000,AE411)*AG411,0)","v":0},0,0.27244452673067671,0,0,0,0,0,0.27244452673067671,0,{"$f":"IF($AF411=3,IF($AF$2=2,(R411/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I411,Refurb_Poss_Tbl[%]))*AG411,IF($AF$2=3,(R411*AG411)-AV411,R411*AG411)),0)","v":0},{"$f":"IF(AF411=3,IF($AF$2=2,(S411/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I411,Refurb_Poss_Tbl[%]))*AG411,IF($AF$2=3,(S411*AG411)-AX411,S411*AG411)),0)","v":0},{"$f":"IF($AF411=3,IF($AF$2=2,(T411/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I411,Refurb_Poss_Tbl[%]))*AG411,T411*$AG411),0)","v":0},{"$f":"IF($AF411=3,IF($AF$2=2,(Q411/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I411,Refurb_Poss_Tbl[%]))*AG411,Q411*$AG411),0)","v":0},{"$f":"IF($AF411=3,IF($AF$2=2,(U411/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I411,Refurb_Poss_Tbl[%]))*AG411,U411*$AG411),0)","v":0},{"$f":"IF($AF411=3,IF($AF$2=2,(V411/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I411,Refurb_Poss_Tbl[%]))*AG411,IF($AF$2=3,(V411*AG411)-AW411,V411*AG411)),0)","v":0},{"$f":"IF($AF411=3,IF($AF$2=2,(W411/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I411,Refurb_Poss_Tbl[%]))*AG411,W411*$AG411),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,6,0,{"$f":"VLOOKUP(AE412,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.81350064430775282},0,0,0,0,0,0,0,0,1.5576539907124833E-4,{"$f":"IF(OR(AF412=3,AF412=2,AF412=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D412,FlatMaint!$Y$2:$Y$10000,AE412)*AG412,0)","v":0.26307566139385313},{"$f":"IF(OR(AF412=3,AF412=2,AF412=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D412,FlatRepair!$Y$2:$Y$10000,AE412)*AG412,0)","v":0},0,0.26323142679292438,0,0,0,0,0,0.26323142679292438,0,{"$f":"IF($AF412=3,IF($AF$2=2,(R412/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I412,Refurb_Poss_Tbl[%]))*AG412,IF($AF$2=3,(R412*AG412)-AV412,R412*AG412)),0)","v":0},{"$f":"IF(AF412=3,IF($AF$2=2,(S412/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I412,Refurb_Poss_Tbl[%]))*AG412,IF($AF$2=3,(S412*AG412)-AX412,S412*AG412)),0)","v":0},{"$f":"IF($AF412=3,IF($AF$2=2,(T412/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I412,Refurb_Poss_Tbl[%]))*AG412,T412*$AG412),0)","v":0},{"$f":"IF($AF412=3,IF($AF$2=2,(Q412/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I412,Refurb_Poss_Tbl[%]))*AG412,Q412*$AG412),0)","v":0},{"$f":"IF($AF412=3,IF($AF$2=2,(U412/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I412,Refurb_Poss_Tbl[%]))*AG412,U412*$AG412),0)","v":0},{"$f":"IF($AF412=3,IF($AF$2=2,(V412/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I412,Refurb_Poss_Tbl[%]))*AG412,IF($AF$2=3,(V412*AG412)-AW412,V412*AG412)),0)","v":0},{"$f":"IF($AF412=3,IF($AF$2=2,(W412/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I412,Refurb_Poss_Tbl[%]))*AG412,W412*$AG412),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,7,0,{"$f":"VLOOKUP(AE413,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.78599096068381913},0,0,0,0,0,0,0,0,1.5049797011714816E-4,{"$f":"IF(OR(AF413=3,AF413=2,AF413=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D413,FlatMaint!$Y$2:$Y$10000,AE413)*AG413,0)","v":0.25417938298923004},{"$f":"IF(OR(AF413=3,AF413=2,AF413=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D413,FlatRepair!$Y$2:$Y$10000,AE413)*AG413,0)","v":0},0,0.25432988095934717,0,0,0,0,0,0.25432988095934717,0,{"$f":"IF($AF413=3,IF($AF$2=2,(R413/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I413,Refurb_Poss_Tbl[%]))*AG413,IF($AF$2=3,(R413*AG413)-AV413,R413*AG413)),0)","v":0},{"$f":"IF(AF413=3,IF($AF$2=2,(S413/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I413,Refurb_Poss_Tbl[%]))*AG413,IF($AF$2=3,(S413*AG413)-AX413,S413*AG413)),0)","v":0},{"$f":"IF($AF413=3,IF($AF$2=2,(T413/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I413,Refurb_Poss_Tbl[%]))*AG413,T413*$AG413),0)","v":0},{"$f":"IF($AF413=3,IF($AF$2=2,(Q413/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I413,Refurb_Poss_Tbl[%]))*AG413,Q413*$AG413),0)","v":0},{"$f":"IF($AF413=3,IF($AF$2=2,(U413/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I413,Refurb_Poss_Tbl[%]))*AG413,U413*$AG413),0)","v":0},{"$f":"IF($AF413=3,IF($AF$2=2,(V413/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I413,Refurb_Poss_Tbl[%]))*AG413,IF($AF$2=3,(V413*AG413)-AW413,V413*AG413)),0)","v":0},{"$f":"IF($AF413=3,IF($AF$2=2,(W413/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I413,Refurb_Poss_Tbl[%]))*AG413,W413*$AG413),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,8,0,{"$f":"VLOOKUP(AE414,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.75941155621625056},0,0,0,0,0,0,0,0,1.4540866677985334E-4,{"$f":"IF(OR(AF414=3,AF414=2,AF414=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D414,FlatMaint!$Y$2:$Y$10000,AE414)*AG414,0)","v":0.24558394491713054},{"$f":"IF(OR(AF414=3,AF414=2,AF414=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D414,FlatRepair!$Y$2:$Y$10000,AE414)*AG414,0)","v":0},0,0.2457293535839104,0,0,0,0,0,0.2457293535839104,0,{"$f":"IF($AF414=3,IF($AF$2=2,(R414/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I414,Refurb_Poss_Tbl[%]))*AG414,IF($AF$2=3,(R414*AG414)-AV414,R414*AG414)),0)","v":0},{"$f":"IF(AF414=3,IF($AF$2=2,(S414/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I414,Refurb_Poss_Tbl[%]))*AG414,IF($AF$2=3,(S414*AG414)-AX414,S414*AG414)),0)","v":0},{"$f":"IF($AF414=3,IF($AF$2=2,(T414/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I414,Refurb_Poss_Tbl[%]))*AG414,T414*$AG414),0)","v":0},{"$f":"IF($AF414=3,IF($AF$2=2,(Q414/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I414,Refurb_Poss_Tbl[%]))*AG414,Q414*$AG414),0)","v":0},{"$f":"IF($AF414=3,IF($AF$2=2,(U414/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I414,Refurb_Poss_Tbl[%]))*AG414,U414*$AG414),0)","v":0},{"$f":"IF($AF414=3,IF($AF$2=2,(V414/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I414,Refurb_Poss_Tbl[%]))*AG414,IF($AF$2=3,(V414*AG414)-AW414,V414*AG414)),0)","v":0},{"$f":"IF($AF414=3,IF($AF$2=2,(W414/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I414,Refurb_Poss_Tbl[%]))*AG414,W414*$AG414),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,9,0,{"$f":"VLOOKUP(AE415,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.73373097218961414},0,0,0,0,0,0,0,0,1.4049146548778099E-4,{"$f":"IF(OR(AF415=3,AF415=2,AF415=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D415,FlatMaint!$Y$2:$Y$10000,AE415)*AG415,0)","v":0.23727917383297639},{"$f":"IF(OR(AF415=3,AF415=2,AF415=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D415,FlatRepair!$Y$2:$Y$10000,AE415)*AG415,0)","v":0},0,0.23741966529846417,0,0,0,0,0,0.23741966529846417,0,{"$f":"IF($AF415=3,IF($AF$2=2,(R415/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I415,Refurb_Poss_Tbl[%]))*AG415,IF($AF$2=3,(R415*AG415)-AV415,R415*AG415)),0)","v":0},{"$f":"IF(AF415=3,IF($AF$2=2,(S415/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I415,Refurb_Poss_Tbl[%]))*AG415,IF($AF$2=3,(S415*AG415)-AX415,S415*AG415)),0)","v":0},{"$f":"IF($AF415=3,IF($AF$2=2,(T415/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I415,Refurb_Poss_Tbl[%]))*AG415,T415*$AG415),0)","v":0},{"$f":"IF($AF415=3,IF($AF$2=2,(Q415/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I415,Refurb_Poss_Tbl[%]))*AG415,Q415*$AG415),0)","v":0},{"$f":"IF($AF415=3,IF($AF$2=2,(U415/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I415,Refurb_Poss_Tbl[%]))*AG415,U415*$AG415),0)","v":0},{"$f":"IF($AF415=3,IF($AF$2=2,(V415/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I415,Refurb_Poss_Tbl[%]))*AG415,IF($AF$2=3,(V415*AG415)-AW415,V415*AG415)),0)","v":0},{"$f":"IF($AF415=3,IF($AF$2=2,(W415/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I415,Refurb_Poss_Tbl[%]))*AG415,W415*$AG415),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,10,0,{"$f":"VLOOKUP(AE416,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.70891881370977217},0,0,0,0,0,0,0,0,1.3574054636500581E-4,{"$f":"IF(OR(AF416=3,AF416=2,AF416=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D416,FlatMaint!$Y$2:$Y$10000,AE416)*AG416,0)","v":0.2292552404183347},{"$f":"IF(OR(AF416=3,AF416=2,AF416=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D416,FlatRepair!$Y$2:$Y$10000,AE416)*AG416,0)","v":0},0,0.2293909809646997,0,0,0,0,0,0.2293909809646997,0,{"$f":"IF($AF416=3,IF($AF$2=2,(R416/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I416,Refurb_Poss_Tbl[%]))*AG416,IF($AF$2=3,(R416*AG416)-AV416,R416*AG416)),0)","v":0},{"$f":"IF(AF416=3,IF($AF$2=2,(S416/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I416,Refurb_Poss_Tbl[%]))*AG416,IF($AF$2=3,(S416*AG416)-AX416,S416*AG416)),0)","v":0},{"$f":"IF($AF416=3,IF($AF$2=2,(T416/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I416,Refurb_Poss_Tbl[%]))*AG416,T416*$AG416),0)","v":0},{"$f":"IF($AF416=3,IF($AF$2=2,(Q416/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I416,Refurb_Poss_Tbl[%]))*AG416,Q416*$AG416),0)","v":0},{"$f":"IF($AF416=3,IF($AF$2=2,(U416/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I416,Refurb_Poss_Tbl[%]))*AG416,U416*$AG416),0)","v":0},{"$f":"IF($AF416=3,IF($AF$2=2,(V416/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I416,Refurb_Poss_Tbl[%]))*AG416,IF($AF$2=3,(V416*AG416)-AW416,V416*AG416)),0)","v":0},{"$f":"IF($AF416=3,IF($AF$2=2,(W416/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I416,Refurb_Poss_Tbl[%]))*AG416,W416*$AG416),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,11,0,{"$f":"VLOOKUP(AE417,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.68494571372924851},0,0,0,0,0,0,0,0,1.3115028634300079E-4,{"$f":"IF(OR(AF417=3,AF417=2,AF417=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D417,FlatMaint!$Y$2:$Y$10000,AE417)*AG417,0)","v":0.22150264774718331},{"$f":"IF(OR(AF417=3,AF417=2,AF417=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D417,FlatRepair!$Y$2:$Y$10000,AE417)*AG417,0)","v":0},0,0.22163379803352631,0,0,0,0,0,0.22163379803352631,0,{"$f":"IF($AF417=3,IF($AF$2=2,(R417/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I417,Refurb_Poss_Tbl[%]))*AG417,IF($AF$2=3,(R417*AG417)-AV417,R417*AG417)),0)","v":0},{"$f":"IF(AF417=3,IF($AF$2=2,(S417/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I417,Refurb_Poss_Tbl[%]))*AG417,IF($AF$2=3,(S417*AG417)-AX417,S417*AG417)),0)","v":0},{"$f":"IF($AF417=3,IF($AF$2=2,(T417/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I417,Refurb_Poss_Tbl[%]))*AG417,T417*$AG417),0)","v":0},{"$f":"IF($AF417=3,IF($AF$2=2,(Q417/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I417,Refurb_Poss_Tbl[%]))*AG417,Q417*$AG417),0)","v":0},{"$f":"IF($AF417=3,IF($AF$2=2,(U417/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I417,Refurb_Poss_Tbl[%]))*AG417,U417*$AG417),0)","v":0},{"$f":"IF($AF417=3,IF($AF$2=2,(V417/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I417,Refurb_Poss_Tbl[%]))*AG417,IF($AF$2=3,(V417*AG417)-AW417,V417*AG417)),0)","v":0},{"$f":"IF($AF417=3,IF($AF$2=2,(W417/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I417,Refurb_Poss_Tbl[%]))*AG417,W417*$AG417),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,12,0,{"$f":"VLOOKUP(AE418,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.66178329828912896},0,0,0,0,0,0,0,0,1.2671525250531476E-4,{"$f":"IF(OR(AF418=3,AF418=2,AF418=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D418,FlatMaint!$Y$2:$Y$10000,AE418)*AG418,0)","v":0.21401222004558773},{"$f":"IF(OR(AF418=3,AF418=2,AF418=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D418,FlatRepair!$Y$2:$Y$10000,AE418)*AG418,0)","v":0},0,0.21413893529809305,0,0,0,0,0,0.21413893529809305,0,{"$f":"IF($AF418=3,IF($AF$2=2,(R418/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I418,Refurb_Poss_Tbl[%]))*AG418,IF($AF$2=3,(R418*AG418)-AV418,R418*AG418)),0)","v":0},{"$f":"IF(AF418=3,IF($AF$2=2,(S418/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I418,Refurb_Poss_Tbl[%]))*AG418,IF($AF$2=3,(S418*AG418)-AX418,S418*AG418)),0)","v":0},{"$f":"IF($AF418=3,IF($AF$2=2,(T418/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I418,Refurb_Poss_Tbl[%]))*AG418,T418*$AG418),0)","v":0},{"$f":"IF($AF418=3,IF($AF$2=2,(Q418/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I418,Refurb_Poss_Tbl[%]))*AG418,Q418*$AG418),0)","v":0},{"$f":"IF($AF418=3,IF($AF$2=2,(U418/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I418,Refurb_Poss_Tbl[%]))*AG418,U418*$AG418),0)","v":0},{"$f":"IF($AF418=3,IF($AF$2=2,(V418/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I418,Refurb_Poss_Tbl[%]))*AG418,IF($AF$2=3,(V418*AG418)-AW418,V418*AG418)),0)","v":0},{"$f":"IF($AF418=3,IF($AF$2=2,(W418/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I418,Refurb_Poss_Tbl[%]))*AG418,W418*$AG418),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,13,0,{"$f":"VLOOKUP(AE419,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.63940415293635666},0,0,0,0,0,0,0,0,1.2243019565730899E-4,{"$f":"IF(OR(AF419=3,AF419=2,AF419=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D419,FlatMaint!$Y$2:$Y$10000,AE419)*AG419,0)","v":0.20677509183148576},{"$f":"IF(OR(AF419=3,AF419=2,AF419=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D419,FlatRepair!$Y$2:$Y$10000,AE419)*AG419,0)","v":0},0,0.20689752202714307,0,0,0,0,0,0.20689752202714307,0,{"$f":"IF($AF419=3,IF($AF$2=2,(R419/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I419,Refurb_Poss_Tbl[%]))*AG419,IF($AF$2=3,(R419*AG419)-AV419,R419*AG419)),0)","v":0},{"$f":"IF(AF419=3,IF($AF$2=2,(S419/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I419,Refurb_Poss_Tbl[%]))*AG419,IF($AF$2=3,(S419*AG419)-AX419,S419*AG419)),0)","v":0},{"$f":"IF($AF419=3,IF($AF$2=2,(T419/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I419,Refurb_Poss_Tbl[%]))*AG419,T419*$AG419),0)","v":0},{"$f":"IF($AF419=3,IF($AF$2=2,(Q419/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I419,Refurb_Poss_Tbl[%]))*AG419,Q419*$AG419),0)","v":0},{"$f":"IF($AF419=3,IF($AF$2=2,(U419/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I419,Refurb_Poss_Tbl[%]))*AG419,U419*$AG419),0)","v":0},{"$f":"IF($AF419=3,IF($AF$2=2,(V419/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I419,Refurb_Poss_Tbl[%]))*AG419,IF($AF$2=3,(V419*AG419)-AW419,V419*AG419)),0)","v":0},{"$f":"IF($AF419=3,IF($AF$2=2,(W419/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I419,Refurb_Poss_Tbl[%]))*AG419,W419*$AG419),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,14,0,{"$f":"VLOOKUP(AE420,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.61778179027667302},0,0,0,0,0,0,0,0,1.18290044113342E-4,{"$f":"IF(OR(AF420=3,AF420=2,AF420=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D420,FlatMaint!$Y$2:$Y$10000,AE420)*AG420,0)","v":0.19978269742172536},{"$f":"IF(OR(AF420=3,AF420=2,AF420=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D420,FlatRepair!$Y$2:$Y$10000,AE420)*AG420,0)","v":0},0,0.1999009874658387,0,0,0,0,0,0.1999009874658387,0,{"$f":"IF($AF420=3,IF($AF$2=2,(R420/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I420,Refurb_Poss_Tbl[%]))*AG420,IF($AF$2=3,(R420*AG420)-AV420,R420*AG420)),0)","v":0},{"$f":"IF(AF420=3,IF($AF$2=2,(S420/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I420,Refurb_Poss_Tbl[%]))*AG420,IF($AF$2=3,(S420*AG420)-AX420,S420*AG420)),0)","v":0},{"$f":"IF($AF420=3,IF($AF$2=2,(T420/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I420,Refurb_Poss_Tbl[%]))*AG420,T420*$AG420),0)","v":0},{"$f":"IF($AF420=3,IF($AF$2=2,(Q420/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I420,Refurb_Poss_Tbl[%]))*AG420,Q420*$AG420),0)","v":0},{"$f":"IF($AF420=3,IF($AF$2=2,(U420/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I420,Refurb_Poss_Tbl[%]))*AG420,U420*$AG420),0)","v":0},{"$f":"IF($AF420=3,IF($AF$2=2,(V420/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I420,Refurb_Poss_Tbl[%]))*AG420,IF($AF$2=3,(V420*AG420)-AW420,V420*AG420)),0)","v":0},{"$f":"IF($AF420=3,IF($AF$2=2,(W420/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I420,Refurb_Poss_Tbl[%]))*AG420,W420*$AG420),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,15,0,{"$f":"VLOOKUP(AE421,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.59689061862480497},0,0,0,0,0,0,0,0,1.1428989769405027E-4,{"$f":"IF(OR(AF421=3,AF421=2,AF421=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D421,FlatMaint!$Y$2:$Y$10000,AE421)*AG421,0)","v":0.19302676079393757},{"$f":"IF(OR(AF421=3,AF421=2,AF421=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D421,FlatRepair!$Y$2:$Y$10000,AE421)*AG421,0)","v":0},0,0.19314105069163162,0,0,0,0,0,0.19314105069163162,0,{"$f":"IF($AF421=3,IF($AF$2=2,(R421/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I421,Refurb_Poss_Tbl[%]))*AG421,IF($AF$2=3,(R421*AG421)-AV421,R421*AG421)),0)","v":0},{"$f":"IF(AF421=3,IF($AF$2=2,(S421/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I421,Refurb_Poss_Tbl[%]))*AG421,IF($AF$2=3,(S421*AG421)-AX421,S421*AG421)),0)","v":0},{"$f":"IF($AF421=3,IF($AF$2=2,(T421/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I421,Refurb_Poss_Tbl[%]))*AG421,T421*$AG421),0)","v":0},{"$f":"IF($AF421=3,IF($AF$2=2,(Q421/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I421,Refurb_Poss_Tbl[%]))*AG421,Q421*$AG421),0)","v":0},{"$f":"IF($AF421=3,IF($AF$2=2,(U421/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I421,Refurb_Poss_Tbl[%]))*AG421,U421*$AG421),0)","v":0},{"$f":"IF($AF421=3,IF($AF$2=2,(V421/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I421,Refurb_Poss_Tbl[%]))*AG421,IF($AF$2=3,(V421*AG421)-AW421,V421*AG421)),0)","v":0},{"$f":"IF($AF421=3,IF($AF$2=2,(W421/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I421,Refurb_Poss_Tbl[%]))*AG421,W421*$AG421),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,16,0,{"$f":"VLOOKUP(AE422,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.57670591171478747},0,0,0,0,0,0,0,0,1.1042502192661863E-4,{"$f":"IF(OR(AF422=3,AF422=2,AF422=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D422,FlatMaint!$Y$2:$Y$10000,AE422)*AG422,0)","v":0.18649928579124406},{"$f":"IF(OR(AF422=3,AF422=2,AF422=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D422,FlatRepair!$Y$2:$Y$10000,AE422)*AG422,0)","v":0},0,0.18660971081317068,0,0,0,0,0,0.18660971081317068,0,{"$f":"IF($AF422=3,IF($AF$2=2,(R422/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I422,Refurb_Poss_Tbl[%]))*AG422,IF($AF$2=3,(R422*AG422)-AV422,R422*AG422)),0)","v":0},{"$f":"IF(AF422=3,IF($AF$2=2,(S422/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I422,Refurb_Poss_Tbl[%]))*AG422,IF($AF$2=3,(S422*AG422)-AX422,S422*AG422)),0)","v":0},{"$f":"IF($AF422=3,IF($AF$2=2,(T422/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I422,Refurb_Poss_Tbl[%]))*AG422,T422*$AG422),0)","v":0},{"$f":"IF($AF422=3,IF($AF$2=2,(Q422/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I422,Refurb_Poss_Tbl[%]))*AG422,Q422*$AG422),0)","v":0},{"$f":"IF($AF422=3,IF($AF$2=2,(U422/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I422,Refurb_Poss_Tbl[%]))*AG422,U422*$AG422),0)","v":0},{"$f":"IF($AF422=3,IF($AF$2=2,(V422/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I422,Refurb_Poss_Tbl[%]))*AG422,IF($AF$2=3,(V422*AG422)-AW422,V422*AG422)),0)","v":0},{"$f":"IF($AF422=3,IF($AF$2=2,(W422/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I422,Refurb_Poss_Tbl[%]))*AG422,W422*$AG422),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,17,0,{"$f":"VLOOKUP(AE423,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.55720377943457733},0,0,0,0,0,0,0,0,1.0669084244117743E-4,{"$f":"IF(OR(AF423=3,AF423=2,AF423=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D423,FlatMaint!$Y$2:$Y$10000,AE423)*AG423,0)","v":0.18019254665820683},{"$f":"IF(OR(AF423=3,AF423=2,AF423=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D423,FlatRepair!$Y$2:$Y$10000,AE423)*AG423,0)","v":0},0,0.180299237500648,0,0,0,0,0,0.180299237500648,0,{"$f":"IF($AF423=3,IF($AF$2=2,(R423/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I423,Refurb_Poss_Tbl[%]))*AG423,IF($AF$2=3,(R423*AG423)-AV423,R423*AG423)),0)","v":0},{"$f":"IF(AF423=3,IF($AF$2=2,(S423/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I423,Refurb_Poss_Tbl[%]))*AG423,IF($AF$2=3,(S423*AG423)-AX423,S423*AG423)),0)","v":0},{"$f":"IF($AF423=3,IF($AF$2=2,(T423/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I423,Refurb_Poss_Tbl[%]))*AG423,T423*$AG423),0)","v":0},{"$f":"IF($AF423=3,IF($AF$2=2,(Q423/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I423,Refurb_Poss_Tbl[%]))*AG423,Q423*$AG423),0)","v":0},{"$f":"IF($AF423=3,IF($AF$2=2,(U423/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I423,Refurb_Poss_Tbl[%]))*AG423,U423*$AG423),0)","v":0},{"$f":"IF($AF423=3,IF($AF$2=2,(V423/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I423,Refurb_Poss_Tbl[%]))*AG423,IF($AF$2=3,(V423*AG423)-AW423,V423*AG423)),0)","v":0},{"$f":"IF($AF423=3,IF($AF$2=2,(W423/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I423,Refurb_Poss_Tbl[%]))*AG423,W423*$AG423),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,18,0,{"$f":"VLOOKUP(AE424,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.53836113955031628},0,0,0,0,0,0,0,0,1.0308293955669318E-4,{"$f":"IF(OR(AF424=3,AF424=2,AF424=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D424,FlatMaint!$Y$2:$Y$10000,AE424)*AG424,0)","v":0.17409907889681822},{"$f":"IF(OR(AF424=3,AF424=2,AF424=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D424,FlatRepair!$Y$2:$Y$10000,AE424)*AG424,0)","v":0},0,0.17420216183637491,0,0,0,0,0,0.17420216183637491,0,{"$f":"IF($AF424=3,IF($AF$2=2,(R424/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I424,Refurb_Poss_Tbl[%]))*AG424,IF($AF$2=3,(R424*AG424)-AV424,R424*AG424)),0)","v":0},{"$f":"IF(AF424=3,IF($AF$2=2,(S424/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I424,Refurb_Poss_Tbl[%]))*AG424,IF($AF$2=3,(S424*AG424)-AX424,S424*AG424)),0)","v":0},{"$f":"IF($AF424=3,IF($AF$2=2,(T424/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I424,Refurb_Poss_Tbl[%]))*AG424,T424*$AG424),0)","v":0},{"$f":"IF($AF424=3,IF($AF$2=2,(Q424/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I424,Refurb_Poss_Tbl[%]))*AG424,Q424*$AG424),0)","v":0},{"$f":"IF($AF424=3,IF($AF$2=2,(U424/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I424,Refurb_Poss_Tbl[%]))*AG424,U424*$AG424),0)","v":0},{"$f":"IF($AF424=3,IF($AF$2=2,(V424/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I424,Refurb_Poss_Tbl[%]))*AG424,IF($AF$2=3,(V424*AG424)-AW424,V424*AG424)),0)","v":0},{"$f":"IF($AF424=3,IF($AF$2=2,(W424/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I424,Refurb_Poss_Tbl[%]))*AG424,W424*$AG424),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,19,0,{"$f":"VLOOKUP(AE425,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.52015569038677911},0,0,0,0,0,0,0,0,9.9597043049945108E-5,{"$f":"IF(OR(AF425=3,AF425=2,AF425=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D425,FlatMaint!$Y$2:$Y$10000,AE425)*AG425,0)","v":0.16821167043170845},{"$f":"IF(OR(AF425=3,AF425=2,AF425=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D425,FlatRepair!$Y$2:$Y$10000,AE425)*AG425,0)","v":0},0,0.16831126747475839,0,0,0,0,0,0.16831126747475839,0,{"$f":"IF($AF425=3,IF($AF$2=2,(R425/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I425,Refurb_Poss_Tbl[%]))*AG425,IF($AF$2=3,(R425*AG425)-AV425,R425*AG425)),0)","v":0},{"$f":"IF(AF425=3,IF($AF$2=2,(S425/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I425,Refurb_Poss_Tbl[%]))*AG425,IF($AF$2=3,(S425*AG425)-AX425,S425*AG425)),0)","v":0},{"$f":"IF($AF425=3,IF($AF$2=2,(T425/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I425,Refurb_Poss_Tbl[%]))*AG425,T425*$AG425),0)","v":0},{"$f":"IF($AF425=3,IF($AF$2=2,(Q425/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I425,Refurb_Poss_Tbl[%]))*AG425,Q425*$AG425),0)","v":0},{"$f":"IF($AF425=3,IF($AF$2=2,(U425/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I425,Refurb_Poss_Tbl[%]))*AG425,U425*$AG425),0)","v":0},{"$f":"IF($AF425=3,IF($AF$2=2,(V425/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I425,Refurb_Poss_Tbl[%]))*AG425,IF($AF$2=3,(V425*AG425)-AW425,V425*AG425)),0)","v":0},{"$f":"IF($AF425=3,IF($AF$2=2,(W425/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I425,Refurb_Poss_Tbl[%]))*AG425,W425*$AG425),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,20,0,{"$f":"VLOOKUP(AE426,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.50256588443167061},0,0,0,0,0,0,0,0,9.6229027101396231E-5,{"$f":"IF(OR(AF426=3,AF426=2,AF426=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D426,FlatMaint!$Y$2:$Y$10000,AE426)*AG426,0)","v":0.16252335307411445},{"$f":"IF(OR(AF426=3,AF426=2,AF426=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D426,FlatRepair!$Y$2:$Y$10000,AE426)*AG426,0)","v":0},0,0.16261958210121585,0,0,0,0,0,0.16261958210121585,0,{"$f":"IF($AF426=3,IF($AF$2=2,(R426/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I426,Refurb_Poss_Tbl[%]))*AG426,IF($AF$2=3,(R426*AG426)-AV426,R426*AG426)),0)","v":0},{"$f":"IF(AF426=3,IF($AF$2=2,(S426/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I426,Refurb_Poss_Tbl[%]))*AG426,IF($AF$2=3,(S426*AG426)-AX426,S426*AG426)),0)","v":0},{"$f":"IF($AF426=3,IF($AF$2=2,(T426/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I426,Refurb_Poss_Tbl[%]))*AG426,T426*$AG426),0)","v":0},{"$f":"IF($AF426=3,IF($AF$2=2,(Q426/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I426,Refurb_Poss_Tbl[%]))*AG426,Q426*$AG426),0)","v":0},{"$f":"IF($AF426=3,IF($AF$2=2,(U426/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I426,Refurb_Poss_Tbl[%]))*AG426,U426*$AG426),0)","v":0},{"$f":"IF($AF426=3,IF($AF$2=2,(V426/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I426,Refurb_Poss_Tbl[%]))*AG426,IF($AF$2=3,(V426*AG426)-AW426,V426*AG426)),0)","v":0},{"$f":"IF($AF426=3,IF($AF$2=2,(W426/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I426,Refurb_Poss_Tbl[%]))*AG426,W426*$AG426),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,21,0,{"$f":"VLOOKUP(AE427,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.48557090283253213},0,0,0,0,0,0,0,0,9.2974905411977063E-5,{"$f":"IF(OR(AF427=3,AF427=2,AF427=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D427,FlatMaint!$Y$2:$Y$10000,AE427)*AG427,0)","v":0.15702739427450674},{"$f":"IF(OR(AF427=3,AF427=2,AF427=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D427,FlatRepair!$Y$2:$Y$10000,AE427)*AG427,0)","v":0},0,0.1571203691799187,0,0,0,0,0,0.1571203691799187,0,{"$f":"IF($AF427=3,IF($AF$2=2,(R427/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I427,Refurb_Poss_Tbl[%]))*AG427,IF($AF$2=3,(R427*AG427)-AV427,R427*AG427)),0)","v":0},{"$f":"IF(AF427=3,IF($AF$2=2,(S427/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I427,Refurb_Poss_Tbl[%]))*AG427,IF($AF$2=3,(S427*AG427)-AX427,S427*AG427)),0)","v":0},{"$f":"IF($AF427=3,IF($AF$2=2,(T427/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I427,Refurb_Poss_Tbl[%]))*AG427,T427*$AG427),0)","v":0},{"$f":"IF($AF427=3,IF($AF$2=2,(Q427/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I427,Refurb_Poss_Tbl[%]))*AG427,Q427*$AG427),0)","v":0},{"$f":"IF($AF427=3,IF($AF$2=2,(U427/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I427,Refurb_Poss_Tbl[%]))*AG427,U427*$AG427),0)","v":0},{"$f":"IF($AF427=3,IF($AF$2=2,(V427/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I427,Refurb_Poss_Tbl[%]))*AG427,IF($AF$2=3,(V427*AG427)-AW427,V427*AG427)),0)","v":0},{"$f":"IF($AF427=3,IF($AF$2=2,(W427/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I427,Refurb_Poss_Tbl[%]))*AG427,W427*$AG427),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,22,0,{"$f":"VLOOKUP(AE428,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.46915063075606966},0,0,0,0,0,0,0,0,8.9830826485001991E-5,{"$f":"IF(OR(AF428=3,AF428=2,AF428=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D428,FlatMaint!$Y$2:$Y$10000,AE428)*AG428,0)","v":0.15171728915411278},{"$f":"IF(OR(AF428=3,AF428=2,AF428=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D428,FlatRepair!$Y$2:$Y$10000,AE428)*AG428,0)","v":0},0,0.15180711998059779,0,0,0,0,0,0.15180711998059779,0,{"$f":"IF($AF428=3,IF($AF$2=2,(R428/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I428,Refurb_Poss_Tbl[%]))*AG428,IF($AF$2=3,(R428*AG428)-AV428,R428*AG428)),0)","v":0},{"$f":"IF(AF428=3,IF($AF$2=2,(S428/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I428,Refurb_Poss_Tbl[%]))*AG428,IF($AF$2=3,(S428*AG428)-AX428,S428*AG428)),0)","v":0},{"$f":"IF($AF428=3,IF($AF$2=2,(T428/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I428,Refurb_Poss_Tbl[%]))*AG428,T428*$AG428),0)","v":0},{"$f":"IF($AF428=3,IF($AF$2=2,(Q428/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I428,Refurb_Poss_Tbl[%]))*AG428,Q428*$AG428),0)","v":0},{"$f":"IF($AF428=3,IF($AF$2=2,(U428/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I428,Refurb_Poss_Tbl[%]))*AG428,U428*$AG428),0)","v":0},{"$f":"IF($AF428=3,IF($AF$2=2,(V428/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I428,Refurb_Poss_Tbl[%]))*AG428,IF($AF$2=3,(V428*AG428)-AW428,V428*AG428)),0)","v":0},{"$f":"IF($AF428=3,IF($AF$2=2,(W428/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I428,Refurb_Poss_Tbl[%]))*AG428,W428*$AG428),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,23,0,{"$f":"VLOOKUP(AE429,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.45328563358074364},0,0,0,0,0,0,0,0,8.679306906763477E-5,{"$f":"IF(OR(AF429=3,AF429=2,AF429=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D429,FlatMaint!$Y$2:$Y$10000,AE429)*AG429,0)","v":0.14658675280590608},{"$f":"IF(OR(AF429=3,AF429=2,AF429=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D429,FlatRepair!$Y$2:$Y$10000,AE429)*AG429,0)","v":0},0,0.14667354587497372,0,0,0,0,0,0.14667354587497372,0,{"$f":"IF($AF429=3,IF($AF$2=2,(R429/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I429,Refurb_Poss_Tbl[%]))*AG429,IF($AF$2=3,(R429*AG429)-AV429,R429*AG429)),0)","v":0},{"$f":"IF(AF429=3,IF($AF$2=2,(S429/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I429,Refurb_Poss_Tbl[%]))*AG429,IF($AF$2=3,(S429*AG429)-AX429,S429*AG429)),0)","v":0},{"$f":"IF($AF429=3,IF($AF$2=2,(T429/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I429,Refurb_Poss_Tbl[%]))*AG429,T429*$AG429),0)","v":0},{"$f":"IF($AF429=3,IF($AF$2=2,(Q429/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I429,Refurb_Poss_Tbl[%]))*AG429,Q429*$AG429),0)","v":0},{"$f":"IF($AF429=3,IF($AF$2=2,(U429/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I429,Refurb_Poss_Tbl[%]))*AG429,U429*$AG429),0)","v":0},{"$f":"IF($AF429=3,IF($AF$2=2,(V429/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I429,Refurb_Poss_Tbl[%]))*AG429,IF($AF$2=3,(V429*AG429)-AW429,V429*AG429)),0)","v":0},{"$f":"IF($AF429=3,IF($AF$2=2,(W429/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I429,Refurb_Poss_Tbl[%]))*AG429,W429*$AG429),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,24,0,{"$f":"VLOOKUP(AE430,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.43795713389443841},0,0,0,0,0,0,0,0,8.3858037746507047E-5,{"$f":"IF(OR(AF430=3,AF430=2,AF430=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D430,FlatMaint!$Y$2:$Y$10000,AE430)*AG430,0)","v":0.14162971285594794},{"$f":"IF(OR(AF430=3,AF430=2,AF430=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D430,FlatRepair!$Y$2:$Y$10000,AE430)*AG430,0)","v":0},0,0.14171357089369446,0,0,0,0,0,0.14171357089369446,0,{"$f":"IF($AF430=3,IF($AF$2=2,(R430/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I430,Refurb_Poss_Tbl[%]))*AG430,IF($AF$2=3,(R430*AG430)-AV430,R430*AG430)),0)","v":0},{"$f":"IF(AF430=3,IF($AF$2=2,(S430/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I430,Refurb_Poss_Tbl[%]))*AG430,IF($AF$2=3,(S430*AG430)-AX430,S430*AG430)),0)","v":0},{"$f":"IF($AF430=3,IF($AF$2=2,(T430/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I430,Refurb_Poss_Tbl[%]))*AG430,T430*$AG430),0)","v":0},{"$f":"IF($AF430=3,IF($AF$2=2,(Q430/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I430,Refurb_Poss_Tbl[%]))*AG430,Q430*$AG430),0)","v":0},{"$f":"IF($AF430=3,IF($AF$2=2,(U430/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I430,Refurb_Poss_Tbl[%]))*AG430,U430*$AG430),0)","v":0},{"$f":"IF($AF430=3,IF($AF$2=2,(V430/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I430,Refurb_Poss_Tbl[%]))*AG430,IF($AF$2=3,(V430*AG430)-AW430,V430*AG430)),0)","v":0},{"$f":"IF($AF430=3,IF($AF$2=2,(W430/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I430,Refurb_Poss_Tbl[%]))*AG430,W430*$AG430),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,25,0,{"$f":"VLOOKUP(AE431,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.42314698926998884},0,0,0,0,0,0,0,0,8.1022258692277355E-5,{"$f":"IF(OR(AF431=3,AF431=2,AF431=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D431,FlatMaint!$Y$2:$Y$10000,AE431)*AG431,0)","v":0.13684030227627822},{"$f":"IF(OR(AF431=3,AF431=2,AF431=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D431,FlatRepair!$Y$2:$Y$10000,AE431)*AG431,0)","v":0},0,0.1369213245349705,0,0,0,0,0,0.1369213245349705,0,{"$f":"IF($AF431=3,IF($AF$2=2,(R431/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I431,Refurb_Poss_Tbl[%]))*AG431,IF($AF$2=3,(R431*AG431)-AV431,R431*AG431)),0)","v":0},{"$f":"IF(AF431=3,IF($AF$2=2,(S431/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I431,Refurb_Poss_Tbl[%]))*AG431,IF($AF$2=3,(S431*AG431)-AX431,S431*AG431)),0)","v":0},{"$f":"IF($AF431=3,IF($AF$2=2,(T431/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I431,Refurb_Poss_Tbl[%]))*AG431,T431*$AG431),0)","v":0},{"$f":"IF($AF431=3,IF($AF$2=2,(Q431/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I431,Refurb_Poss_Tbl[%]))*AG431,Q431*$AG431),0)","v":0},{"$f":"IF($AF431=3,IF($AF$2=2,(U431/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I431,Refurb_Poss_Tbl[%]))*AG431,U431*$AG431),0)","v":0},{"$f":"IF($AF431=3,IF($AF$2=2,(V431/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I431,Refurb_Poss_Tbl[%]))*AG431,IF($AF$2=3,(V431*AG431)-AW431,V431*AG431)),0)","v":0},{"$f":"IF($AF431=3,IF($AF$2=2,(W431/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I431,Refurb_Poss_Tbl[%]))*AG431,W431*$AG431),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,26,0,{"$f":"VLOOKUP(AE432,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.40883767079225974},0,0,0,0,0,0,0,0,7.8282375548094054E-5,{"$f":"IF(OR(AF432=3,AF432=2,AF432=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D432,FlatMaint!$Y$2:$Y$10000,AE432)*AG432,0)","v":0.13221285244084852},{"$f":"IF(OR(AF432=3,AF432=2,AF432=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D432,FlatRepair!$Y$2:$Y$10000,AE432)*AG432,0)","v":0},0,0.13229113481639662,0,0,0,0,0,0.13229113481639662,0,{"$f":"IF($AF432=3,IF($AF$2=2,(R432/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I432,Refurb_Poss_Tbl[%]))*AG432,IF($AF$2=3,(R432*AG432)-AV432,R432*AG432)),0)","v":0},{"$f":"IF(AF432=3,IF($AF$2=2,(S432/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I432,Refurb_Poss_Tbl[%]))*AG432,IF($AF$2=3,(S432*AG432)-AX432,S432*AG432)),0)","v":0},{"$f":"IF($AF432=3,IF($AF$2=2,(T432/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I432,Refurb_Poss_Tbl[%]))*AG432,T432*$AG432),0)","v":0},{"$f":"IF($AF432=3,IF($AF$2=2,(Q432/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I432,Refurb_Poss_Tbl[%]))*AG432,Q432*$AG432),0)","v":0},{"$f":"IF($AF432=3,IF($AF$2=2,(U432/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I432,Refurb_Poss_Tbl[%]))*AG432,U432*$AG432),0)","v":0},{"$f":"IF($AF432=3,IF($AF$2=2,(V432/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I432,Refurb_Poss_Tbl[%]))*AG432,IF($AF$2=3,(V432*AG432)-AW432,V432*AG432)),0)","v":0},{"$f":"IF($AF432=3,IF($AF$2=2,(W432/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I432,Refurb_Poss_Tbl[%]))*AG432,W432*$AG432),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,27,0,{"$f":"VLOOKUP(AE433,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39501224231136206},0,0,0,0,0,0,0,0,7.5635145457095712E-5,{"$f":"IF(OR(AF433=3,AF433=2,AF433=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D433,FlatMaint!$Y$2:$Y$10000,AE433)*AG433,0)","v":0.12774188641627876},{"$f":"IF(OR(AF433=3,AF433=2,AF433=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D433,FlatRepair!$Y$2:$Y$10000,AE433)*AG433,0)","v":0},0,0.12781752156173587,0,0,0,0,0,0.12781752156173587,0,{"$f":"IF($AF433=3,IF($AF$2=2,(R433/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I433,Refurb_Poss_Tbl[%]))*AG433,IF($AF$2=3,(R433*AG433)-AV433,R433*AG433)),0)","v":0},{"$f":"IF(AF433=3,IF($AF$2=2,(S433/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I433,Refurb_Poss_Tbl[%]))*AG433,IF($AF$2=3,(S433*AG433)-AX433,S433*AG433)),0)","v":0},{"$f":"IF($AF433=3,IF($AF$2=2,(T433/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I433,Refurb_Poss_Tbl[%]))*AG433,T433*$AG433),0)","v":0},{"$f":"IF($AF433=3,IF($AF$2=2,(Q433/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I433,Refurb_Poss_Tbl[%]))*AG433,Q433*$AG433),0)","v":0},{"$f":"IF($AF433=3,IF($AF$2=2,(U433/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I433,Refurb_Poss_Tbl[%]))*AG433,U433*$AG433),0)","v":0},{"$f":"IF($AF433=3,IF($AF$2=2,(V433/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I433,Refurb_Poss_Tbl[%]))*AG433,IF($AF$2=3,(V433*AG433)-AW433,V433*AG433)),0)","v":0},{"$f":"IF($AF433=3,IF($AF$2=2,(W433/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I433,Refurb_Poss_Tbl[%]))*AG433,W433*$AG433),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,28,0,{"$f":"VLOOKUP(AE434,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38165434039745127},0,0,0,0,0,0,0,0,7.3077435224247055E-5,{"$f":"IF(OR(AF434=3,AF434=2,AF434=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D434,FlatMaint!$Y$2:$Y$10000,AE434)*AG434,0)","v":0.12342211247949639},{"$f":"IF(OR(AF434=3,AF434=2,AF434=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D434,FlatRepair!$Y$2:$Y$10000,AE434)*AG434,0)","v":0},0,0.12349518991472064,0,0,0,0,0,0.12349518991472064,0,{"$f":"IF($AF434=3,IF($AF$2=2,(R434/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I434,Refurb_Poss_Tbl[%]))*AG434,IF($AF$2=3,(R434*AG434)-AV434,R434*AG434)),0)","v":0},{"$f":"IF(AF434=3,IF($AF$2=2,(S434/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I434,Refurb_Poss_Tbl[%]))*AG434,IF($AF$2=3,(S434*AG434)-AX434,S434*AG434)),0)","v":0},{"$f":"IF($AF434=3,IF($AF$2=2,(T434/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I434,Refurb_Poss_Tbl[%]))*AG434,T434*$AG434),0)","v":0},{"$f":"IF($AF434=3,IF($AF$2=2,(Q434/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I434,Refurb_Poss_Tbl[%]))*AG434,Q434*$AG434),0)","v":0},{"$f":"IF($AF434=3,IF($AF$2=2,(U434/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I434,Refurb_Poss_Tbl[%]))*AG434,U434*$AG434),0)","v":0},{"$f":"IF($AF434=3,IF($AF$2=2,(V434/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I434,Refurb_Poss_Tbl[%]))*AG434,IF($AF$2=3,(V434*AG434)-AW434,V434*AG434)),0)","v":0},{"$f":"IF($AF434=3,IF($AF$2=2,(W434/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I434,Refurb_Poss_Tbl[%]))*AG434,W434*$AG434),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,29,0,{"$f":"VLOOKUP(AE435,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36874815497338298},0,0,0,0,0,0,0,0,7.0606217607968193E-5,{"$f":"IF(OR(AF435=3,AF435=2,AF435=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D435,FlatMaint!$Y$2:$Y$10000,AE435)*AG435,0)","v":0.11924841785458591},{"$f":"IF(OR(AF435=3,AF435=2,AF435=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D435,FlatRepair!$Y$2:$Y$10000,AE435)*AG435,0)","v":0},0,0.11931902407219389,0,0,0,0,0,0.11931902407219389,0,{"$f":"IF($AF435=3,IF($AF$2=2,(R435/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I435,Refurb_Poss_Tbl[%]))*AG435,IF($AF$2=3,(R435*AG435)-AV435,R435*AG435)),0)","v":0},{"$f":"IF(AF435=3,IF($AF$2=2,(S435/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I435,Refurb_Poss_Tbl[%]))*AG435,IF($AF$2=3,(S435*AG435)-AX435,S435*AG435)),0)","v":0},{"$f":"IF($AF435=3,IF($AF$2=2,(T435/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I435,Refurb_Poss_Tbl[%]))*AG435,T435*$AG435),0)","v":0},{"$f":"IF($AF435=3,IF($AF$2=2,(Q435/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I435,Refurb_Poss_Tbl[%]))*AG435,Q435*$AG435),0)","v":0},{"$f":"IF($AF435=3,IF($AF$2=2,(U435/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I435,Refurb_Poss_Tbl[%]))*AG435,U435*$AG435),0)","v":0},{"$f":"IF($AF435=3,IF($AF$2=2,(V435/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I435,Refurb_Poss_Tbl[%]))*AG435,IF($AF$2=3,(V435*AG435)-AW435,V435*AG435)),0)","v":0},{"$f":"IF($AF435=3,IF($AF$2=2,(W435/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I435,Refurb_Poss_Tbl[%]))*AG435,W435*$AG435),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,30,0,{"$f":"VLOOKUP(AE436,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35627841060230236},0,0,0,0,0,0,0,0,6.8218567737167327E-5,{"$f":"IF(OR(AF436=3,AF436=2,AF436=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D436,FlatMaint!$Y$2:$Y$10000,AE436)*AG436,0)","v":0.11521586266143566},{"$f":"IF(OR(AF436=3,AF436=2,AF436=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D436,FlatRepair!$Y$2:$Y$10000,AE436)*AG436,0)","v":0},0,0.11528408122917283,0,0,0,0,0,0.11528408122917283,0,{"$f":"IF($AF436=3,IF($AF$2=2,(R436/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I436,Refurb_Poss_Tbl[%]))*AG436,IF($AF$2=3,(R436*AG436)-AV436,R436*AG436)),0)","v":0},{"$f":"IF(AF436=3,IF($AF$2=2,(S436/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I436,Refurb_Poss_Tbl[%]))*AG436,IF($AF$2=3,(S436*AG436)-AX436,S436*AG436)),0)","v":0},{"$f":"IF($AF436=3,IF($AF$2=2,(T436/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I436,Refurb_Poss_Tbl[%]))*AG436,T436*$AG436),0)","v":0},{"$f":"IF($AF436=3,IF($AF$2=2,(Q436/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I436,Refurb_Poss_Tbl[%]))*AG436,Q436*$AG436),0)","v":0},{"$f":"IF($AF436=3,IF($AF$2=2,(U436/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I436,Refurb_Poss_Tbl[%]))*AG436,U436*$AG436),0)","v":0},{"$f":"IF($AF436=3,IF($AF$2=2,(V436/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I436,Refurb_Poss_Tbl[%]))*AG436,IF($AF$2=3,(V436*AG436)-AW436,V436*AG436)),0)","v":0},{"$f":"IF($AF436=3,IF($AF$2=2,(W436/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I436,Refurb_Poss_Tbl[%]))*AG436,W436*$AG436),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,31,0,{"$f":"VLOOKUP(AE437,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.39998714516107459},0,0,0,0,0,0,0,0,7.6587717201381878E-5,{"$f":"IF(OR(AF437=3,AF437=2,AF437=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D437,FlatMaint!$Y$2:$Y$10000,AE437)*AG437,0)","v":0.12935070611017338},{"$f":"IF(OR(AF437=3,AF437=2,AF437=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D437,FlatRepair!$Y$2:$Y$10000,AE437)*AG437,0)","v":0},0,0.12942729382737475,0,0,0,0,0,0.12942729382737475,0,{"$f":"IF($AF437=3,IF($AF$2=2,(R437/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I437,Refurb_Poss_Tbl[%]))*AG437,IF($AF$2=3,(R437*AG437)-AV437,R437*AG437)),0)","v":0},{"$f":"IF(AF437=3,IF($AF$2=2,(S437/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I437,Refurb_Poss_Tbl[%]))*AG437,IF($AF$2=3,(S437*AG437)-AX437,S437*AG437)),0)","v":0},{"$f":"IF($AF437=3,IF($AF$2=2,(T437/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I437,Refurb_Poss_Tbl[%]))*AG437,T437*$AG437),0)","v":0},{"$f":"IF($AF437=3,IF($AF$2=2,(Q437/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I437,Refurb_Poss_Tbl[%]))*AG437,Q437*$AG437),0)","v":0},{"$f":"IF($AF437=3,IF($AF$2=2,(U437/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I437,Refurb_Poss_Tbl[%]))*AG437,U437*$AG437),0)","v":0},{"$f":"IF($AF437=3,IF($AF$2=2,(V437/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I437,Refurb_Poss_Tbl[%]))*AG437,IF($AF$2=3,(V437*AG437)-AW437,V437*AG437)),0)","v":0},{"$f":"IF($AF437=3,IF($AF$2=2,(W437/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I437,Refurb_Poss_Tbl[%]))*AG437,W437*$AG437),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,32,0,{"$f":"VLOOKUP(AE438,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.38833703413696569},0,0,0,0,0,0,0,0,7.4357006991632906E-5,{"$f":"IF(OR(AF438=3,AF438=2,AF438=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D438,FlatMaint!$Y$2:$Y$10000,AE438)*AG438,0)","v":0.12558320981570234},{"$f":"IF(OR(AF438=3,AF438=2,AF438=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D438,FlatRepair!$Y$2:$Y$10000,AE438)*AG438,0)","v":0},0,0.12565756682269397,0,0,0,0,0,0.12565756682269397,0,{"$f":"IF($AF438=3,IF($AF$2=2,(R438/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I438,Refurb_Poss_Tbl[%]))*AG438,IF($AF$2=3,(R438*AG438)-AV438,R438*AG438)),0)","v":0},{"$f":"IF(AF438=3,IF($AF$2=2,(S438/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I438,Refurb_Poss_Tbl[%]))*AG438,IF($AF$2=3,(S438*AG438)-AX438,S438*AG438)),0)","v":0},{"$f":"IF($AF438=3,IF($AF$2=2,(T438/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I438,Refurb_Poss_Tbl[%]))*AG438,T438*$AG438),0)","v":0},{"$f":"IF($AF438=3,IF($AF$2=2,(Q438/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I438,Refurb_Poss_Tbl[%]))*AG438,Q438*$AG438),0)","v":0},{"$f":"IF($AF438=3,IF($AF$2=2,(U438/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I438,Refurb_Poss_Tbl[%]))*AG438,U438*$AG438),0)","v":0},{"$f":"IF($AF438=3,IF($AF$2=2,(V438/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I438,Refurb_Poss_Tbl[%]))*AG438,IF($AF$2=3,(V438*AG438)-AW438,V438*AG438)),0)","v":0},{"$f":"IF($AF438=3,IF($AF$2=2,(W438/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I438,Refurb_Poss_Tbl[%]))*AG438,W438*$AG438),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,33,0,{"$f":"VLOOKUP(AE439,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.37702624673491814},0,0,0,0,0,0,0,0,7.2191268923915445E-5,{"$f":"IF(OR(AF439=3,AF439=2,AF439=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D439,FlatMaint!$Y$2:$Y$10000,AE439)*AG439,0)","v":0.12192544642301198},{"$f":"IF(OR(AF439=3,AF439=2,AF439=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D439,FlatRepair!$Y$2:$Y$10000,AE439)*AG439,0)","v":0},0,0.12199763769193589,0,0,0,0,0,0.12199763769193589,0,{"$f":"IF($AF439=3,IF($AF$2=2,(R439/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I439,Refurb_Poss_Tbl[%]))*AG439,IF($AF$2=3,(R439*AG439)-AV439,R439*AG439)),0)","v":0},{"$f":"IF(AF439=3,IF($AF$2=2,(S439/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I439,Refurb_Poss_Tbl[%]))*AG439,IF($AF$2=3,(S439*AG439)-AX439,S439*AG439)),0)","v":0},{"$f":"IF($AF439=3,IF($AF$2=2,(T439/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I439,Refurb_Poss_Tbl[%]))*AG439,T439*$AG439),0)","v":0},{"$f":"IF($AF439=3,IF($AF$2=2,(Q439/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I439,Refurb_Poss_Tbl[%]))*AG439,Q439*$AG439),0)","v":0},{"$f":"IF($AF439=3,IF($AF$2=2,(U439/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I439,Refurb_Poss_Tbl[%]))*AG439,U439*$AG439),0)","v":0},{"$f":"IF($AF439=3,IF($AF$2=2,(V439/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I439,Refurb_Poss_Tbl[%]))*AG439,IF($AF$2=3,(V439*AG439)-AW439,V439*AG439)),0)","v":0},{"$f":"IF($AF439=3,IF($AF$2=2,(W439/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I439,Refurb_Poss_Tbl[%]))*AG439,W439*$AG439),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,34,0,{"$f":"VLOOKUP(AE440,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.36604489974263904},0,0,0,0,0,0,0,0,7.0088610605743157E-5,{"$f":"IF(OR(AF440=3,AF440=2,AF440=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D440,FlatMaint!$Y$2:$Y$10000,AE440)*AG440,0)","v":0.118374219828167},{"$f":"IF(OR(AF440=3,AF440=2,AF440=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D440,FlatRepair!$Y$2:$Y$10000,AE440)*AG440,0)","v":0},0,0.11844430843877274,0,0,0,0,0,0.11844430843877274,0,{"$f":"IF($AF440=3,IF($AF$2=2,(R440/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I440,Refurb_Poss_Tbl[%]))*AG440,IF($AF$2=3,(R440*AG440)-AV440,R440*AG440)),0)","v":0},{"$f":"IF(AF440=3,IF($AF$2=2,(S440/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I440,Refurb_Poss_Tbl[%]))*AG440,IF($AF$2=3,(S440*AG440)-AX440,S440*AG440)),0)","v":0},{"$f":"IF($AF440=3,IF($AF$2=2,(T440/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I440,Refurb_Poss_Tbl[%]))*AG440,T440*$AG440),0)","v":0},{"$f":"IF($AF440=3,IF($AF$2=2,(Q440/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I440,Refurb_Poss_Tbl[%]))*AG440,Q440*$AG440),0)","v":0},{"$f":"IF($AF440=3,IF($AF$2=2,(U440/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I440,Refurb_Poss_Tbl[%]))*AG440,U440*$AG440),0)","v":0},{"$f":"IF($AF440=3,IF($AF$2=2,(V440/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I440,Refurb_Poss_Tbl[%]))*AG440,IF($AF$2=3,(V440*AG440)-AW440,V440*AG440)),0)","v":0},{"$f":"IF($AF440=3,IF($AF$2=2,(W440/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I440,Refurb_Poss_Tbl[%]))*AG440,W440*$AG440),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,35,0,{"$f":"VLOOKUP(AE441,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.35538339780838735},0,0,0,0,0,0,0,0,6.804719476285742E-5,{"$f":"IF(OR(AF441=3,AF441=2,AF441=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D441,FlatMaint!$Y$2:$Y$10000,AE441)*AG441,0)","v":0.11492642701763783},{"$f":"IF(OR(AF441=3,AF441=2,AF441=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D441,FlatRepair!$Y$2:$Y$10000,AE441)*AG441,0)","v":0},0,0.11499447421240069,0,0,0,0,0,0.11499447421240069,0,{"$f":"IF($AF441=3,IF($AF$2=2,(R441/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I441,Refurb_Poss_Tbl[%]))*AG441,IF($AF$2=3,(R441*AG441)-AV441,R441*AG441)),0)","v":0},{"$f":"IF(AF441=3,IF($AF$2=2,(S441/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I441,Refurb_Poss_Tbl[%]))*AG441,IF($AF$2=3,(S441*AG441)-AX441,S441*AG441)),0)","v":0},{"$f":"IF($AF441=3,IF($AF$2=2,(T441/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I441,Refurb_Poss_Tbl[%]))*AG441,T441*$AG441),0)","v":0},{"$f":"IF($AF441=3,IF($AF$2=2,(Q441/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I441,Refurb_Poss_Tbl[%]))*AG441,Q441*$AG441),0)","v":0},{"$f":"IF($AF441=3,IF($AF$2=2,(U441/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I441,Refurb_Poss_Tbl[%]))*AG441,U441*$AG441),0)","v":0},{"$f":"IF($AF441=3,IF($AF$2=2,(V441/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I441,Refurb_Poss_Tbl[%]))*AG441,IF($AF$2=3,(V441*AG441)-AW441,V441*AG441)),0)","v":0},{"$f":"IF($AF441=3,IF($AF$2=2,(W441/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I441,Refurb_Poss_Tbl[%]))*AG441,W441*$AG441),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,36,0,{"$f":"VLOOKUP(AE442,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.34503242505668674},0,0,0,0,0,0,0,0,6.6065237633842154E-5,{"$f":"IF(OR(AF442=3,AF442=2,AF442=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D442,FlatMaint!$Y$2:$Y$10000,AE442)*AG442,0)","v":0.11157905535692994},{"$f":"IF(OR(AF442=3,AF442=2,AF442=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D442,FlatRepair!$Y$2:$Y$10000,AE442)*AG442,0)","v":0},0,0.11164512059456379,0,0,0,0,0,0.11164512059456379,0,{"$f":"IF($AF442=3,IF($AF$2=2,(R442/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I442,Refurb_Poss_Tbl[%]))*AG442,IF($AF$2=3,(R442*AG442)-AV442,R442*AG442)),0)","v":0},{"$f":"IF(AF442=3,IF($AF$2=2,(S442/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I442,Refurb_Poss_Tbl[%]))*AG442,IF($AF$2=3,(S442*AG442)-AX442,S442*AG442)),0)","v":0},{"$f":"IF($AF442=3,IF($AF$2=2,(T442/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I442,Refurb_Poss_Tbl[%]))*AG442,T442*$AG442),0)","v":0},{"$f":"IF($AF442=3,IF($AF$2=2,(Q442/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I442,Refurb_Poss_Tbl[%]))*AG442,Q442*$AG442),0)","v":0},{"$f":"IF($AF442=3,IF($AF$2=2,(U442/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I442,Refurb_Poss_Tbl[%]))*AG442,U442*$AG442),0)","v":0},{"$f":"IF($AF442=3,IF($AF$2=2,(V442/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I442,Refurb_Poss_Tbl[%]))*AG442,IF($AF$2=3,(V442*AG442)-AW442,V442*AG442)),0)","v":0},{"$f":"IF($AF442=3,IF($AF$2=2,(W442/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I442,Refurb_Poss_Tbl[%]))*AG442,W442*$AG442),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,37,0,{"$f":"VLOOKUP(AE443,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.33498293694823961},0,0,0,0,0,0,0,0,6.4141007411497246E-5,{"$f":"IF(OR(AF443=3,AF443=2,AF443=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D443,FlatMaint!$Y$2:$Y$10000,AE443)*AG443,0)","v":0.10832917995818442},{"$f":"IF(OR(AF443=3,AF443=2,AF443=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D443,FlatRepair!$Y$2:$Y$10000,AE443)*AG443,0)","v":0},0,0.10839332096559591,0,0,0,0,0,0.10839332096559591,0,{"$f":"IF($AF443=3,IF($AF$2=2,(R443/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I443,Refurb_Poss_Tbl[%]))*AG443,IF($AF$2=3,(R443*AG443)-AV443,R443*AG443)),0)","v":0},{"$f":"IF(AF443=3,IF($AF$2=2,(S443/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I443,Refurb_Poss_Tbl[%]))*AG443,IF($AF$2=3,(S443*AG443)-AX443,S443*AG443)),0)","v":0},{"$f":"IF($AF443=3,IF($AF$2=2,(T443/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I443,Refurb_Poss_Tbl[%]))*AG443,T443*$AG443),0)","v":0},{"$f":"IF($AF443=3,IF($AF$2=2,(Q443/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I443,Refurb_Poss_Tbl[%]))*AG443,Q443*$AG443),0)","v":0},{"$f":"IF($AF443=3,IF($AF$2=2,(U443/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I443,Refurb_Poss_Tbl[%]))*AG443,U443*$AG443),0)","v":0},{"$f":"IF($AF443=3,IF($AF$2=2,(V443/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I443,Refurb_Poss_Tbl[%]))*AG443,IF($AF$2=3,(V443*AG443)-AW443,V443*AG443)),0)","v":0},{"$f":"IF($AF443=3,IF($AF$2=2,(W443/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I443,Refurb_Poss_Tbl[%]))*AG443,W443*$AG443),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,38,0,{"$f":"VLOOKUP(AE444,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.3252261523769317},0,0,0,0,0,0,0,0,6.2272822729608985E-5,{"$f":"IF(OR(AF444=3,AF444=2,AF444=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D444,FlatMaint!$Y$2:$Y$10000,AE444)*AG444,0)","v":0.1051739611244509},{"$f":"IF(OR(AF444=3,AF444=2,AF444=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D444,FlatRepair!$Y$2:$Y$10000,AE444)*AG444,0)","v":0},0,0.10523623394718051,0,0,0,0,0,0.10523623394718051,0,{"$f":"IF($AF444=3,IF($AF$2=2,(R444/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I444,Refurb_Poss_Tbl[%]))*AG444,IF($AF$2=3,(R444*AG444)-AV444,R444*AG444)),0)","v":0},{"$f":"IF(AF444=3,IF($AF$2=2,(S444/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I444,Refurb_Poss_Tbl[%]))*AG444,IF($AF$2=3,(S444*AG444)-AX444,S444*AG444)),0)","v":0},{"$f":"IF($AF444=3,IF($AF$2=2,(T444/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I444,Refurb_Poss_Tbl[%]))*AG444,T444*$AG444),0)","v":0},{"$f":"IF($AF444=3,IF($AF$2=2,(Q444/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I444,Refurb_Poss_Tbl[%]))*AG444,Q444*$AG444),0)","v":0},{"$f":"IF($AF444=3,IF($AF$2=2,(U444/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I444,Refurb_Poss_Tbl[%]))*AG444,U444*$AG444),0)","v":0},{"$f":"IF($AF444=3,IF($AF$2=2,(V444/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I444,Refurb_Poss_Tbl[%]))*AG444,IF($AF$2=3,(V444*AG444)-AW444,V444*AG444)),0)","v":0},{"$f":"IF($AF444=3,IF($AF$2=2,(W444/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I444,Refurb_Poss_Tbl[%]))*AG444,W444*$AG444),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,39,0,{"$f":"VLOOKUP(AE445,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.31575354599702099},0,0,0,0,0,0,0,0,6.0459051193795119E-5,{"$f":"IF(OR(AF445=3,AF445=2,AF445=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D445,FlatMaint!$Y$2:$Y$10000,AE445)*AG445,0)","v":0.10211064186839891},{"$f":"IF(OR(AF445=3,AF445=2,AF445=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D445,FlatRepair!$Y$2:$Y$10000,AE445)*AG445,0)","v":0},0,0.10217110091959271,0,0,0,0,0,0.10217110091959271,0,{"$f":"IF($AF445=3,IF($AF$2=2,(R445/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I445,Refurb_Poss_Tbl[%]))*AG445,IF($AF$2=3,(R445*AG445)-AV445,R445*AG445)),0)","v":0},{"$f":"IF(AF445=3,IF($AF$2=2,(S445/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I445,Refurb_Poss_Tbl[%]))*AG445,IF($AF$2=3,(S445*AG445)-AX445,S445*AG445)),0)","v":0},{"$f":"IF($AF445=3,IF($AF$2=2,(T445/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I445,Refurb_Poss_Tbl[%]))*AG445,T445*$AG445),0)","v":0},{"$f":"IF($AF445=3,IF($AF$2=2,(Q445/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I445,Refurb_Poss_Tbl[%]))*AG445,Q445*$AG445),0)","v":0},{"$f":"IF($AF445=3,IF($AF$2=2,(U445/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I445,Refurb_Poss_Tbl[%]))*AG445,U445*$AG445),0)","v":0},{"$f":"IF($AF445=3,IF($AF$2=2,(V445/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I445,Refurb_Poss_Tbl[%]))*AG445,IF($AF$2=3,(V445*AG445)-AW445,V445*AG445)),0)","v":0},{"$f":"IF($AF445=3,IF($AF$2=2,(W445/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I445,Refurb_Poss_Tbl[%]))*AG445,W445*$AG445),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,40,0,{"$f":"VLOOKUP(AE446,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.30655684077380685},0,0,0,0,0,0,0,0,5.8698107955140906E-5,{"$f":"IF(OR(AF446=3,AF446=2,AF446=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D446,FlatMaint!$Y$2:$Y$10000,AE446)*AG446,0)","v":9.9136545503299936E-2},{"$f":"IF(OR(AF446=3,AF446=2,AF446=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D446,FlatRepair!$Y$2:$Y$10000,AE446)*AG446,0)","v":0},0,9.9195243611255077E-2,0,0,0,0,0,9.9195243611255077E-2,0,{"$f":"IF($AF446=3,IF($AF$2=2,(R446/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I446,Refurb_Poss_Tbl[%]))*AG446,IF($AF$2=3,(R446*AG446)-AV446,R446*AG446)),0)","v":0},{"$f":"IF(AF446=3,IF($AF$2=2,(S446/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I446,Refurb_Poss_Tbl[%]))*AG446,IF($AF$2=3,(S446*AG446)-AX446,S446*AG446)),0)","v":0},{"$f":"IF($AF446=3,IF($AF$2=2,(T446/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I446,Refurb_Poss_Tbl[%]))*AG446,T446*$AG446),0)","v":0},{"$f":"IF($AF446=3,IF($AF$2=2,(Q446/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I446,Refurb_Poss_Tbl[%]))*AG446,Q446*$AG446),0)","v":0},{"$f":"IF($AF446=3,IF($AF$2=2,(U446/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I446,Refurb_Poss_Tbl[%]))*AG446,U446*$AG446),0)","v":0},{"$f":"IF($AF446=3,IF($AF$2=2,(V446/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I446,Refurb_Poss_Tbl[%]))*AG446,IF($AF$2=3,(V446*AG446)-AW446,V446*AG446)),0)","v":0},{"$f":"IF($AF446=3,IF($AF$2=2,(W446/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I446,Refurb_Poss_Tbl[%]))*AG446,W446*$AG446),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,41,0,{"$f":"VLOOKUP(AE447,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.29762800075126877},0,0,0,0,0,0,0,0,5.698845432537952E-5,{"$f":"IF(OR(AF447=3,AF447=2,AF447=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D447,FlatMaint!$Y$2:$Y$10000,AE447)*AG447,0)","v":9.624907330417469E-2},{"$f":"IF(OR(AF447=3,AF447=2,AF447=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D447,FlatRepair!$Y$2:$Y$10000,AE447)*AG447,0)","v":0},0,9.6306061758500067E-2,0,0,0,0,0,9.6306061758500067E-2,0,{"$f":"IF($AF447=3,IF($AF$2=2,(R447/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I447,Refurb_Poss_Tbl[%]))*AG447,IF($AF$2=3,(R447*AG447)-AV447,R447*AG447)),0)","v":0},{"$f":"IF(AF447=3,IF($AF$2=2,(S447/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I447,Refurb_Poss_Tbl[%]))*AG447,IF($AF$2=3,(S447*AG447)-AX447,S447*AG447)),0)","v":0},{"$f":"IF($AF447=3,IF($AF$2=2,(T447/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I447,Refurb_Poss_Tbl[%]))*AG447,T447*$AG447),0)","v":0},{"$f":"IF($AF447=3,IF($AF$2=2,(Q447/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I447,Refurb_Poss_Tbl[%]))*AG447,Q447*$AG447),0)","v":0},{"$f":"IF($AF447=3,IF($AF$2=2,(U447/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I447,Refurb_Poss_Tbl[%]))*AG447,U447*$AG447),0)","v":0},{"$f":"IF($AF447=3,IF($AF$2=2,(V447/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I447,Refurb_Poss_Tbl[%]))*AG447,IF($AF$2=3,(V447*AG447)-AW447,V447*AG447)),0)","v":0},{"$f":"IF($AF447=3,IF($AF$2=2,(W447/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I447,Refurb_Poss_Tbl[%]))*AG447,W447*$AG447),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,42,0,{"$f":"VLOOKUP(AE448,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28895922403035801},0,0,0,0,0,0,0,0,5.5328596432407297E-5,{"$f":"IF(OR(AF448=3,AF448=2,AF448=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D448,FlatMaint!$Y$2:$Y$10000,AE448)*AG448,0)","v":9.3445702237062805E-2},{"$f":"IF(OR(AF448=3,AF448=2,AF448=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D448,FlatRepair!$Y$2:$Y$10000,AE448)*AG448,0)","v":0},0,9.3501030833495216E-2,0,0,0,0,0,9.3501030833495216E-2,0,{"$f":"IF($AF448=3,IF($AF$2=2,(R448/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I448,Refurb_Poss_Tbl[%]))*AG448,IF($AF$2=3,(R448*AG448)-AV448,R448*AG448)),0)","v":0},{"$f":"IF(AF448=3,IF($AF$2=2,(S448/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I448,Refurb_Poss_Tbl[%]))*AG448,IF($AF$2=3,(S448*AG448)-AX448,S448*AG448)),0)","v":0},{"$f":"IF($AF448=3,IF($AF$2=2,(T448/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I448,Refurb_Poss_Tbl[%]))*AG448,T448*$AG448),0)","v":0},{"$f":"IF($AF448=3,IF($AF$2=2,(Q448/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I448,Refurb_Poss_Tbl[%]))*AG448,Q448*$AG448),0)","v":0},{"$f":"IF($AF448=3,IF($AF$2=2,(U448/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I448,Refurb_Poss_Tbl[%]))*AG448,U448*$AG448),0)","v":0},{"$f":"IF($AF448=3,IF($AF$2=2,(V448/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I448,Refurb_Poss_Tbl[%]))*AG448,IF($AF$2=3,(V448*AG448)-AW448,V448*AG448)),0)","v":0},{"$f":"IF($AF448=3,IF($AF$2=2,(W448/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I448,Refurb_Poss_Tbl[%]))*AG448,W448*$AG448),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,43,0,{"$f":"VLOOKUP(AE449,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.28054293595180391},0,0,0,0,0,0,0,0,5.371708391495854E-5,{"$f":"IF(OR(AF449=3,AF449=2,AF449=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D449,FlatMaint!$Y$2:$Y$10000,AE449)*AG449,0)","v":9.0723982754429902E-2},{"$f":"IF(OR(AF449=3,AF449=2,AF449=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D449,FlatRepair!$Y$2:$Y$10000,AE449)*AG449,0)","v":0},0,9.0777699838344855E-2,0,0,0,0,0,9.0777699838344855E-2,0,{"$f":"IF($AF449=3,IF($AF$2=2,(R449/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I449,Refurb_Poss_Tbl[%]))*AG449,IF($AF$2=3,(R449*AG449)-AV449,R449*AG449)),0)","v":0},{"$f":"IF(AF449=3,IF($AF$2=2,(S449/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I449,Refurb_Poss_Tbl[%]))*AG449,IF($AF$2=3,(S449*AG449)-AX449,S449*AG449)),0)","v":0},{"$f":"IF($AF449=3,IF($AF$2=2,(T449/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I449,Refurb_Poss_Tbl[%]))*AG449,T449*$AG449),0)","v":0},{"$f":"IF($AF449=3,IF($AF$2=2,(Q449/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I449,Refurb_Poss_Tbl[%]))*AG449,Q449*$AG449),0)","v":0},{"$f":"IF($AF449=3,IF($AF$2=2,(U449/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I449,Refurb_Poss_Tbl[%]))*AG449,U449*$AG449),0)","v":0},{"$f":"IF($AF449=3,IF($AF$2=2,(V449/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I449,Refurb_Poss_Tbl[%]))*AG449,IF($AF$2=3,(V449*AG449)-AW449,V449*AG449)),0)","v":0},{"$f":"IF($AF449=3,IF($AF$2=2,(W449/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I449,Refurb_Poss_Tbl[%]))*AG449,W449*$AG449),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,44,0,{"$f":"VLOOKUP(AE450,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.27237178247747956},0,0,0,0,0,0,0,0,5.2152508655299566E-5,{"$f":"IF(OR(AF450=3,AF450=2,AF450=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D450,FlatMaint!$Y$2:$Y$10000,AE450)*AG450,0)","v":8.8081536654786338E-2},{"$f":"IF(OR(AF450=3,AF450=2,AF450=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D450,FlatRepair!$Y$2:$Y$10000,AE450)*AG450,0)","v":0},0,8.8133689163441636E-2,0,0,0,0,0,8.8133689163441636E-2,0,{"$f":"IF($AF450=3,IF($AF$2=2,(R450/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I450,Refurb_Poss_Tbl[%]))*AG450,IF($AF$2=3,(R450*AG450)-AV450,R450*AG450)),0)","v":0},{"$f":"IF(AF450=3,IF($AF$2=2,(S450/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I450,Refurb_Poss_Tbl[%]))*AG450,IF($AF$2=3,(S450*AG450)-AX450,S450*AG450)),0)","v":0},{"$f":"IF($AF450=3,IF($AF$2=2,(T450/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I450,Refurb_Poss_Tbl[%]))*AG450,T450*$AG450),0)","v":0},{"$f":"IF($AF450=3,IF($AF$2=2,(Q450/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I450,Refurb_Poss_Tbl[%]))*AG450,Q450*$AG450),0)","v":0},{"$f":"IF($AF450=3,IF($AF$2=2,(U450/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I450,Refurb_Poss_Tbl[%]))*AG450,U450*$AG450),0)","v":0},{"$f":"IF($AF450=3,IF($AF$2=2,(V450/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I450,Refurb_Poss_Tbl[%]))*AG450,IF($AF$2=3,(V450*AG450)-AW450,V450*AG450)),0)","v":0},{"$f":"IF($AF450=3,IF($AF$2=2,(W450/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I450,Refurb_Poss_Tbl[%]))*AG450,W450*$AG450),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,45,0,{"$f":"VLOOKUP(AE451,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.26443862376454325},{"$f":"IF(AE451=0,Q451*AG451,0)","v":0},{"$f":"IF(AE451=0,R451*AG451,0)","v":0},{"$f":"IF(AE451=0,S451*AG451,0)","v":0},{"$f":"IF(AE451=0,T451*AG451,0)","v":0},{"$f":"IF(AE451=0,U451*AG451,0)","v":0},{"$f":"IF(AE451=0,V451*AG451,0)","v":0},{"$f":"IF(AE451=0,W451*AG451,0)","v":0},{"$f":"IF(AE451=0,AH451+AI451+AJ451+AK451+AL451+AM451+AN451,0)","v":0},{"$f":"IF(OR(AF451=3,AF451=2,AF451=0),Y451*AG451,0)","v":5.0633503548834521E-5},{"$f":"IF(OR(AF451=3,AF451=2,AF451=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D451,FlatMaint!$Y$2:$Y$10000,AE451)*AG451,0)","v":8.5516055004646915E-2},{"$f":"IF(OR(AF451=3,AF451=2,AF451=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D451,FlatRepair!$Y$2:$Y$10000,AE451)*AG451,0)","v":0},{"$f":"IF(OR(AF451=3,AF451=2,AF451=0),Z451*AG451,0)","v":0},{"$f":"AP451+AQ451+AR451+AS451","v":8.5566688508195751E-2},{"$f":"IF(AF451=2,AA451*AG451,0)","v":0},{"$f":"IF(AF451=3,AB451*AG451,0)","v":0},{"$f":"IF(AF451=3,AC451*AG451,0)","v":0},{"$f":"IF(AF451=3,AD451*AG451,0)","v":0},{"$f":"IF($AF$2=3,BB451+BC451+BD451+BE451+BF451+BG451+BH451,BB451+BC451+BD451+BE451+BF451+BG451+BH451)","v":0},{"$f":"AO451+AT451+AU451+AV451+AW451+AX451+AY451+BA451","v":8.5566688508195751E-2},{"$f":"IFERROR(IF(AE451=100,IF(O451=3,(N451/H451)*(X451*AG451)*-1,(N451/M451)*(X451*AG451)*-1),0),0)","v":0},{"$f":"IF($AF451=3,IF($AF$2=2,(R451/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I451,Refurb_Poss_Tbl[%]))*AG451,IF($AF$2=3,(R451*AG451)-AV451,R451*AG451)),0)","v":0},{"$f":"IF(AF451=3,IF($AF$2=2,(S451/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I451,Refurb_Poss_Tbl[%]))*AG451,IF($AF$2=3,(S451*AG451)-AX451,S451*AG451)),0)","v":0},{"$f":"IF($AF451=3,IF($AF$2=2,(T451/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I451,Refurb_Poss_Tbl[%]))*AG451,T451*$AG451),0)","v":0},{"$f":"IF($AF451=3,IF($AF$2=2,(Q451/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I451,Refurb_Poss_Tbl[%]))*AG451,Q451*$AG451),0)","v":0},{"$f":"IF($AF451=3,IF($AF$2=2,(U451/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I451,Refurb_Poss_Tbl[%]))*AG451,U451*$AG451),0)","v":0},{"$f":"IF($AF451=3,IF($AF$2=2,(V451/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I451,Refurb_Poss_Tbl[%]))*AG451,IF($AF$2=3,(V451*AG451)-AW451,V451*AG451)),0)","v":0},{"$f":"IF($AF451=3,IF($AF$2=2,(W451/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I451,Refurb_Poss_Tbl[%]))*AG451,W451*$AG451),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,46,0,{"$f":"VLOOKUP(AE452,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.25673652792674101},0,0,0,0,0,0,0,0,4.9158741309548082E-5,{"$f":"IF(OR(AF452=3,AF452=2,AF452=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D452,FlatMaint!$Y$2:$Y$10000,AE452)*AG452,0)","v":8.3025296121016418E-2},{"$f":"IF(OR(AF452=3,AF452=2,AF452=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D452,FlatRepair!$Y$2:$Y$10000,AE452)*AG452,0)","v":0},0,8.3074454862325967E-2,0,0,0,0,0,8.3074454862325967E-2,0,{"$f":"IF($AF452=3,IF($AF$2=2,(R452/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I452,Refurb_Poss_Tbl[%]))*AG452,IF($AF$2=3,(R452*AG452)-AV452,R452*AG452)),0)","v":0},{"$f":"IF(AF452=3,IF($AF$2=2,(S452/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I452,Refurb_Poss_Tbl[%]))*AG452,IF($AF$2=3,(S452*AG452)-AX452,S452*AG452)),0)","v":0},{"$f":"IF($AF452=3,IF($AF$2=2,(T452/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I452,Refurb_Poss_Tbl[%]))*AG452,T452*$AG452),0)","v":0},{"$f":"IF($AF452=3,IF($AF$2=2,(Q452/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I452,Refurb_Poss_Tbl[%]))*AG452,Q452*$AG452),0)","v":0},{"$f":"IF($AF452=3,IF($AF$2=2,(U452/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I452,Refurb_Poss_Tbl[%]))*AG452,U452*$AG452),0)","v":0},{"$f":"IF($AF452=3,IF($AF$2=2,(V452/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I452,Refurb_Poss_Tbl[%]))*AG452,IF($AF$2=3,(V452*AG452)-AW452,V452*AG452)),0)","v":0},{"$f":"IF($AF452=3,IF($AF$2=2,(W452/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I452,Refurb_Poss_Tbl[%]))*AG452,W452*$AG452),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,47,0,{"$f":"VLOOKUP(AE453,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24925876497741845},0,0,0,0,0,0,0,0,4.7726933310240856E-5,{"$f":"IF(OR(AF453=3,AF453=2,AF453=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D453,FlatMaint!$Y$2:$Y$10000,AE453)*AG453,0)","v":8.0607083612637298E-2},{"$f":"IF(OR(AF453=3,AF453=2,AF453=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D453,FlatRepair!$Y$2:$Y$10000,AE453)*AG453,0)","v":0},0,8.0654810545947545E-2,0,0,0,0,0,8.0654810545947545E-2,0,{"$f":"IF($AF453=3,IF($AF$2=2,(R453/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I453,Refurb_Poss_Tbl[%]))*AG453,IF($AF$2=3,(R453*AG453)-AV453,R453*AG453)),0)","v":0},{"$f":"IF(AF453=3,IF($AF$2=2,(S453/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I453,Refurb_Poss_Tbl[%]))*AG453,IF($AF$2=3,(S453*AG453)-AX453,S453*AG453)),0)","v":0},{"$f":"IF($AF453=3,IF($AF$2=2,(T453/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I453,Refurb_Poss_Tbl[%]))*AG453,T453*$AG453),0)","v":0},{"$f":"IF($AF453=3,IF($AF$2=2,(Q453/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I453,Refurb_Poss_Tbl[%]))*AG453,Q453*$AG453),0)","v":0},{"$f":"IF($AF453=3,IF($AF$2=2,(U453/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I453,Refurb_Poss_Tbl[%]))*AG453,U453*$AG453),0)","v":0},{"$f":"IF($AF453=3,IF($AF$2=2,(V453/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I453,Refurb_Poss_Tbl[%]))*AG453,IF($AF$2=3,(V453*AG453)-AW453,V453*AG453)),0)","v":0},{"$f":"IF($AF453=3,IF($AF$2=2,(W453/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I453,Refurb_Poss_Tbl[%]))*AG453,W453*$AG453),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,48,0,{"$f":"VLOOKUP(AE454,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.24199880094894996},0,0,0,0,0,0,0,0,4.6336828456544521E-5,{"$f":"IF(OR(AF454=3,AF454=2,AF454=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D454,FlatMaint!$Y$2:$Y$10000,AE454)*AG454,0)","v":7.8259304478288647E-2},{"$f":"IF(OR(AF454=3,AF454=2,AF454=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D454,FlatRepair!$Y$2:$Y$10000,AE454)*AG454,0)","v":0},0,7.8305641306745194E-2,0,0,0,0,0,7.8305641306745194E-2,0,{"$f":"IF($AF454=3,IF($AF$2=2,(R454/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I454,Refurb_Poss_Tbl[%]))*AG454,IF($AF$2=3,(R454*AG454)-AV454,R454*AG454)),0)","v":0},{"$f":"IF(AF454=3,IF($AF$2=2,(S454/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I454,Refurb_Poss_Tbl[%]))*AG454,IF($AF$2=3,(S454*AG454)-AX454,S454*AG454)),0)","v":0},{"$f":"IF($AF454=3,IF($AF$2=2,(T454/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I454,Refurb_Poss_Tbl[%]))*AG454,T454*$AG454),0)","v":0},{"$f":"IF($AF454=3,IF($AF$2=2,(Q454/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I454,Refurb_Poss_Tbl[%]))*AG454,Q454*$AG454),0)","v":0},{"$f":"IF($AF454=3,IF($AF$2=2,(U454/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I454,Refurb_Poss_Tbl[%]))*AG454,U454*$AG454),0)","v":0},{"$f":"IF($AF454=3,IF($AF$2=2,(V454/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I454,Refurb_Poss_Tbl[%]))*AG454,IF($AF$2=3,(V454*AG454)-AW454,V454*AG454)),0)","v":0},{"$f":"IF($AF454=3,IF($AF$2=2,(W454/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I454,Refurb_Poss_Tbl[%]))*AG454,W454*$AG454),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,49,0,{"$f":"VLOOKUP(AE455,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.2349502921834466},0,0,0,0,0,0,0,0,4.4987212093732552E-5,{"$f":"IF(OR(AF455=3,AF455=2,AF455=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D455,FlatMaint!$Y$2:$Y$10000,AE455)*AG455,0)","v":7.5979907260474419E-2},{"$f":"IF(OR(AF455=3,AF455=2,AF455=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D455,FlatRepair!$Y$2:$Y$10000,AE455)*AG455,0)","v":0},0,7.6024894472568147E-2,0,0,0,0,0,7.6024894472568147E-2,0,{"$f":"IF($AF455=3,IF($AF$2=2,(R455/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I455,Refurb_Poss_Tbl[%]))*AG455,IF($AF$2=3,(R455*AG455)-AV455,R455*AG455)),0)","v":0},{"$f":"IF(AF455=3,IF($AF$2=2,(S455/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I455,Refurb_Poss_Tbl[%]))*AG455,IF($AF$2=3,(S455*AG455)-AX455,S455*AG455)),0)","v":0},{"$f":"IF($AF455=3,IF($AF$2=2,(T455/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I455,Refurb_Poss_Tbl[%]))*AG455,T455*$AG455),0)","v":0},{"$f":"IF($AF455=3,IF($AF$2=2,(Q455/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I455,Refurb_Poss_Tbl[%]))*AG455,Q455*$AG455),0)","v":0},{"$f":"IF($AF455=3,IF($AF$2=2,(U455/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I455,Refurb_Poss_Tbl[%]))*AG455,U455*$AG455),0)","v":0},{"$f":"IF($AF455=3,IF($AF$2=2,(V455/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I455,Refurb_Poss_Tbl[%]))*AG455,IF($AF$2=3,(V455*AG455)-AW455,V455*AG455)),0)","v":0},{"$f":"IF($AF455=3,IF($AF$2=2,(W455/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I455,Refurb_Poss_Tbl[%]))*AG455,W455*$AG455),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,50,0,{"$f":"VLOOKUP(AE456,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22810707978975397},0,0,0,0,0,0,0,0,4.3676904945371405E-5,{"$f":"IF(OR(AF456=3,AF456=2,AF456=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D456,FlatMaint!$Y$2:$Y$10000,AE456)*AG456,0)","v":7.376690025288779E-2},{"$f":"IF(OR(AF456=3,AF456=2,AF456=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D456,FlatRepair!$Y$2:$Y$10000,AE456)*AG456,0)","v":0},0,7.3810577157833165E-2,0,0,0,0,0,7.3810577157833165E-2,0,{"$f":"IF($AF456=3,IF($AF$2=2,(R456/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I456,Refurb_Poss_Tbl[%]))*AG456,IF($AF$2=3,(R456*AG456)-AV456,R456*AG456)),0)","v":0},{"$f":"IF(AF456=3,IF($AF$2=2,(S456/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I456,Refurb_Poss_Tbl[%]))*AG456,IF($AF$2=3,(S456*AG456)-AX456,S456*AG456)),0)","v":0},{"$f":"IF($AF456=3,IF($AF$2=2,(T456/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I456,Refurb_Poss_Tbl[%]))*AG456,T456*$AG456),0)","v":0},{"$f":"IF($AF456=3,IF($AF$2=2,(Q456/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I456,Refurb_Poss_Tbl[%]))*AG456,Q456*$AG456),0)","v":0},{"$f":"IF($AF456=3,IF($AF$2=2,(U456/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I456,Refurb_Poss_Tbl[%]))*AG456,U456*$AG456),0)","v":0},{"$f":"IF($AF456=3,IF($AF$2=2,(V456/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I456,Refurb_Poss_Tbl[%]))*AG456,IF($AF$2=3,(V456*AG456)-AW456,V456*AG456)),0)","v":0},{"$f":"IF($AF456=3,IF($AF$2=2,(W456/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I456,Refurb_Poss_Tbl[%]))*AG456,W456*$AG456),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,51,0,{"$f":"VLOOKUP(AE457,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.22146318426189707},0,0,0,0,0,0,0,0,4.2404762082884864E-5,{"$f":"IF(OR(AF457=3,AF457=2,AF457=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D457,FlatMaint!$Y$2:$Y$10000,AE457)*AG457,0)","v":7.1618349760085229E-2},{"$f":"IF(OR(AF457=3,AF457=2,AF457=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D457,FlatRepair!$Y$2:$Y$10000,AE457)*AG457,0)","v":0},0,7.1660754522168107E-2,0,0,0,0,0,7.1660754522168107E-2,0,{"$f":"IF($AF457=3,IF($AF$2=2,(R457/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I457,Refurb_Poss_Tbl[%]))*AG457,IF($AF$2=3,(R457*AG457)-AV457,R457*AG457)),0)","v":0},{"$f":"IF(AF457=3,IF($AF$2=2,(S457/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I457,Refurb_Poss_Tbl[%]))*AG457,IF($AF$2=3,(S457*AG457)-AX457,S457*AG457)),0)","v":0},{"$f":"IF($AF457=3,IF($AF$2=2,(T457/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I457,Refurb_Poss_Tbl[%]))*AG457,T457*$AG457),0)","v":0},{"$f":"IF($AF457=3,IF($AF$2=2,(Q457/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I457,Refurb_Poss_Tbl[%]))*AG457,Q457*$AG457),0)","v":0},{"$f":"IF($AF457=3,IF($AF$2=2,(U457/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I457,Refurb_Poss_Tbl[%]))*AG457,U457*$AG457),0)","v":0},{"$f":"IF($AF457=3,IF($AF$2=2,(V457/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I457,Refurb_Poss_Tbl[%]))*AG457,IF($AF$2=3,(V457*AG457)-AW457,V457*AG457)),0)","v":0},{"$f":"IF($AF457=3,IF($AF$2=2,(W457/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I457,Refurb_Poss_Tbl[%]))*AG457,W457*$AG457),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,52,0,{"$f":"VLOOKUP(AE458,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.215012800254269},0,0,0,0,0,0,0,0,4.1169671925130937E-5,{"$f":"IF(OR(AF458=3,AF458=2,AF458=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D458,FlatMaint!$Y$2:$Y$10000,AE458)*AG458,0)","v":6.9532378407849746E-2},{"$f":"IF(OR(AF458=3,AF458=2,AF458=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D458,FlatRepair!$Y$2:$Y$10000,AE458)*AG458,0)","v":0},0,6.957354807977488E-2,0,0,0,0,0,6.957354807977488E-2,0,{"$f":"IF($AF458=3,IF($AF$2=2,(R458/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I458,Refurb_Poss_Tbl[%]))*AG458,IF($AF$2=3,(R458*AG458)-AV458,R458*AG458)),0)","v":0},{"$f":"IF(AF458=3,IF($AF$2=2,(S458/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I458,Refurb_Poss_Tbl[%]))*AG458,IF($AF$2=3,(S458*AG458)-AX458,S458*AG458)),0)","v":0},{"$f":"IF($AF458=3,IF($AF$2=2,(T458/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I458,Refurb_Poss_Tbl[%]))*AG458,T458*$AG458),0)","v":0},{"$f":"IF($AF458=3,IF($AF$2=2,(Q458/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I458,Refurb_Poss_Tbl[%]))*AG458,Q458*$AG458),0)","v":0},{"$f":"IF($AF458=3,IF($AF$2=2,(U458/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I458,Refurb_Poss_Tbl[%]))*AG458,U458*$AG458),0)","v":0},{"$f":"IF($AF458=3,IF($AF$2=2,(V458/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I458,Refurb_Poss_Tbl[%]))*AG458,IF($AF$2=3,(V458*AG458)-AW458,V458*AG458)),0)","v":0},{"$f":"IF($AF458=3,IF($AF$2=2,(W458/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I458,Refurb_Poss_Tbl[%]))*AG458,W458*$AG458),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,53,0,{"$f":"VLOOKUP(AE459,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20875029150899907},0,0,0,0,0,0,0,0,3.997055526711742E-5,{"$f":"IF(OR(AF459=3,AF459=2,AF459=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D459,FlatMaint!$Y$2:$Y$10000,AE459)*AG459,0)","v":6.7507163502766754E-2},{"$f":"IF(OR(AF459=3,AF459=2,AF459=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D459,FlatRepair!$Y$2:$Y$10000,AE459)*AG459,0)","v":0},0,6.7547134058033878E-2,0,0,0,0,0,6.7547134058033878E-2,0,{"$f":"IF($AF459=3,IF($AF$2=2,(R459/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I459,Refurb_Poss_Tbl[%]))*AG459,IF($AF$2=3,(R459*AG459)-AV459,R459*AG459)),0)","v":0},{"$f":"IF(AF459=3,IF($AF$2=2,(S459/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I459,Refurb_Poss_Tbl[%]))*AG459,IF($AF$2=3,(S459*AG459)-AX459,S459*AG459)),0)","v":0},{"$f":"IF($AF459=3,IF($AF$2=2,(T459/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I459,Refurb_Poss_Tbl[%]))*AG459,T459*$AG459),0)","v":0},{"$f":"IF($AF459=3,IF($AF$2=2,(Q459/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I459,Refurb_Poss_Tbl[%]))*AG459,Q459*$AG459),0)","v":0},{"$f":"IF($AF459=3,IF($AF$2=2,(U459/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I459,Refurb_Poss_Tbl[%]))*AG459,U459*$AG459),0)","v":0},{"$f":"IF($AF459=3,IF($AF$2=2,(V459/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I459,Refurb_Poss_Tbl[%]))*AG459,IF($AF$2=3,(V459*AG459)-AW459,V459*AG459)),0)","v":0},{"$f":"IF($AF459=3,IF($AF$2=2,(W459/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I459,Refurb_Poss_Tbl[%]))*AG459,W459*$AG459),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,54,0,{"$f":"VLOOKUP(AE460,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.20267018593106703},0,0,0,0,0,0,0,0,3.8806364337007199E-5,{"$f":"IF(OR(AF460=3,AF460=2,AF460=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D460,FlatMaint!$Y$2:$Y$10000,AE460)*AG460,0)","v":6.5540935439579368E-2},{"$f":"IF(OR(AF460=3,AF460=2,AF460=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D460,FlatRepair!$Y$2:$Y$10000,AE460)*AG460,0)","v":0},0,6.5579741803916375E-2,0,0,0,0,0,6.5579741803916375E-2,0,{"$f":"IF($AF460=3,IF($AF$2=2,(R460/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I460,Refurb_Poss_Tbl[%]))*AG460,IF($AF$2=3,(R460*AG460)-AV460,R460*AG460)),0)","v":0},{"$f":"IF(AF460=3,IF($AF$2=2,(S460/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I460,Refurb_Poss_Tbl[%]))*AG460,IF($AF$2=3,(S460*AG460)-AX460,S460*AG460)),0)","v":0},{"$f":"IF($AF460=3,IF($AF$2=2,(T460/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I460,Refurb_Poss_Tbl[%]))*AG460,T460*$AG460),0)","v":0},{"$f":"IF($AF460=3,IF($AF$2=2,(Q460/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I460,Refurb_Poss_Tbl[%]))*AG460,Q460*$AG460),0)","v":0},{"$f":"IF($AF460=3,IF($AF$2=2,(U460/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I460,Refurb_Poss_Tbl[%]))*AG460,U460*$AG460),0)","v":0},{"$f":"IF($AF460=3,IF($AF$2=2,(V460/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I460,Refurb_Poss_Tbl[%]))*AG460,IF($AF$2=3,(V460*AG460)-AW460,V460*AG460)),0)","v":0},{"$f":"IF($AF460=3,IF($AF$2=2,(W460/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I460,Refurb_Poss_Tbl[%]))*AG460,W460*$AG460),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,55,0,{"$f":"VLOOKUP(AE461,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19676717080686118},0,0,0,0,0,0,0,0,3.7676081880589511E-5,{"$f":"IF(OR(AF461=3,AF461=2,AF461=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D461,FlatMaint!$Y$2:$Y$10000,AE461)*AG461,0)","v":6.3631976154931422E-2},{"$f":"IF(OR(AF461=3,AF461=2,AF461=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D461,FlatRepair!$Y$2:$Y$10000,AE461)*AG461,0)","v":0},0,6.3669652236812008E-2,0,0,0,0,0,6.3669652236812008E-2,0,{"$f":"IF($AF461=3,IF($AF$2=2,(R461/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I461,Refurb_Poss_Tbl[%]))*AG461,IF($AF$2=3,(R461*AG461)-AV461,R461*AG461)),0)","v":0},{"$f":"IF(AF461=3,IF($AF$2=2,(S461/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I461,Refurb_Poss_Tbl[%]))*AG461,IF($AF$2=3,(S461*AG461)-AX461,S461*AG461)),0)","v":0},{"$f":"IF($AF461=3,IF($AF$2=2,(T461/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I461,Refurb_Poss_Tbl[%]))*AG461,T461*$AG461),0)","v":0},{"$f":"IF($AF461=3,IF($AF$2=2,(Q461/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I461,Refurb_Poss_Tbl[%]))*AG461,Q461*$AG461),0)","v":0},{"$f":"IF($AF461=3,IF($AF$2=2,(U461/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I461,Refurb_Poss_Tbl[%]))*AG461,U461*$AG461),0)","v":0},{"$f":"IF($AF461=3,IF($AF$2=2,(V461/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I461,Refurb_Poss_Tbl[%]))*AG461,IF($AF$2=3,(V461*AG461)-AW461,V461*AG461)),0)","v":0},{"$f":"IF($AF461=3,IF($AF$2=2,(W461/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I461,Refurb_Poss_Tbl[%]))*AG461,W461*$AG461),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,56,0,{"$f":"VLOOKUP(AE462,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.19103608816200118},0,0,0,0,0,0,0,0,3.6578720272417008E-5,{"$f":"IF(OR(AF462=3,AF462=2,AF462=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D462,FlatMaint!$Y$2:$Y$10000,AE462)*AG462,0)","v":6.1778617626147017E-2},{"$f":"IF(OR(AF462=3,AF462=2,AF462=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D462,FlatRepair!$Y$2:$Y$10000,AE462)*AG462,0)","v":0},0,6.1815196346419431E-2,0,0,0,0,0,6.1815196346419431E-2,0,{"$f":"IF($AF462=3,IF($AF$2=2,(R462/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I462,Refurb_Poss_Tbl[%]))*AG462,IF($AF$2=3,(R462*AG462)-AV462,R462*AG462)),0)","v":0},{"$f":"IF(AF462=3,IF($AF$2=2,(S462/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I462,Refurb_Poss_Tbl[%]))*AG462,IF($AF$2=3,(S462*AG462)-AX462,S462*AG462)),0)","v":0},{"$f":"IF($AF462=3,IF($AF$2=2,(T462/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I462,Refurb_Poss_Tbl[%]))*AG462,T462*$AG462),0)","v":0},{"$f":"IF($AF462=3,IF($AF$2=2,(Q462/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I462,Refurb_Poss_Tbl[%]))*AG462,Q462*$AG462),0)","v":0},{"$f":"IF($AF462=3,IF($AF$2=2,(U462/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I462,Refurb_Poss_Tbl[%]))*AG462,U462*$AG462),0)","v":0},{"$f":"IF($AF462=3,IF($AF$2=2,(V462/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I462,Refurb_Poss_Tbl[%]))*AG462,IF($AF$2=3,(V462*AG462)-AW462,V462*AG462)),0)","v":0},{"$f":"IF($AF462=3,IF($AF$2=2,(W462/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I462,Refurb_Poss_Tbl[%]))*AG462,W462*$AG462),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,57,0,{"$f":"VLOOKUP(AE463,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18547193025437006},0,0,0,0,0,0,0,0,3.5513320652832042E-5,{"$f":"IF(OR(AF463=3,AF463=2,AF463=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D463,FlatMaint!$Y$2:$Y$10000,AE463)*AG463,0)","v":5.9979240413734959E-2},{"$f":"IF(OR(AF463=3,AF463=2,AF463=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D463,FlatRepair!$Y$2:$Y$10000,AE463)*AG463,0)","v":0},0,6.0014753734387791E-2,0,0,0,0,0,6.0014753734387791E-2,0,{"$f":"IF($AF463=3,IF($AF$2=2,(R463/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I463,Refurb_Poss_Tbl[%]))*AG463,IF($AF$2=3,(R463*AG463)-AV463,R463*AG463)),0)","v":0},{"$f":"IF(AF463=3,IF($AF$2=2,(S463/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I463,Refurb_Poss_Tbl[%]))*AG463,IF($AF$2=3,(S463*AG463)-AX463,S463*AG463)),0)","v":0},{"$f":"IF($AF463=3,IF($AF$2=2,(T463/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I463,Refurb_Poss_Tbl[%]))*AG463,T463*$AG463),0)","v":0},{"$f":"IF($AF463=3,IF($AF$2=2,(Q463/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I463,Refurb_Poss_Tbl[%]))*AG463,Q463*$AG463),0)","v":0},{"$f":"IF($AF463=3,IF($AF$2=2,(U463/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I463,Refurb_Poss_Tbl[%]))*AG463,U463*$AG463),0)","v":0},{"$f":"IF($AF463=3,IF($AF$2=2,(V463/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I463,Refurb_Poss_Tbl[%]))*AG463,IF($AF$2=3,(V463*AG463)-AW463,V463*AG463)),0)","v":0},{"$f":"IF($AF463=3,IF($AF$2=2,(W463/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I463,Refurb_Poss_Tbl[%]))*AG463,W463*$AG463),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,58,0,{"$f":"VLOOKUP(AE464,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.18006983519841754},0,0,0,0,0,0,0,0,3.4478952090128197E-5,{"$f":"IF(OR(AF464=3,AF464=2,AF464=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D464,FlatMaint!$Y$2:$Y$10000,AE464)*AG464,0)","v":5.8232272246344627E-2},{"$f":"IF(OR(AF464=3,AF464=2,AF464=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D464,FlatRepair!$Y$2:$Y$10000,AE464)*AG464,0)","v":0},0,5.8266751198434753E-2,0,0,0,0,0,5.8266751198434753E-2,0,{"$f":"IF($AF464=3,IF($AF$2=2,(R464/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I464,Refurb_Poss_Tbl[%]))*AG464,IF($AF$2=3,(R464*AG464)-AV464,R464*AG464)),0)","v":0},{"$f":"IF(AF464=3,IF($AF$2=2,(S464/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I464,Refurb_Poss_Tbl[%]))*AG464,IF($AF$2=3,(S464*AG464)-AX464,S464*AG464)),0)","v":0},{"$f":"IF($AF464=3,IF($AF$2=2,(T464/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I464,Refurb_Poss_Tbl[%]))*AG464,T464*$AG464),0)","v":0},{"$f":"IF($AF464=3,IF($AF$2=2,(Q464/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I464,Refurb_Poss_Tbl[%]))*AG464,Q464*$AG464),0)","v":0},{"$f":"IF($AF464=3,IF($AF$2=2,(U464/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I464,Refurb_Poss_Tbl[%]))*AG464,U464*$AG464),0)","v":0},{"$f":"IF($AF464=3,IF($AF$2=2,(V464/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I464,Refurb_Poss_Tbl[%]))*AG464,IF($AF$2=3,(V464*AG464)-AW464,V464*AG464)),0)","v":0},{"$f":"IF($AF464=3,IF($AF$2=2,(W464/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I464,Refurb_Poss_Tbl[%]))*AG464,W464*$AG464),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,59,0,{"$f":"VLOOKUP(AE465,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.17482508271691022},0,0,0,0,0,0,0,0,3.3474710767114752E-5,{"$f":"IF(OR(AF465=3,AF465=2,AF465=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D465,FlatMaint!$Y$2:$Y$10000,AE465)*AG465,0)","v":5.6536186646936527E-2},{"$f":"IF(OR(AF465=3,AF465=2,AF465=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D465,FlatRepair!$Y$2:$Y$10000,AE465)*AG465,0)","v":0},0,5.6569661357703645E-2,0,0,0,0,0,5.6569661357703645E-2,0,{"$f":"IF($AF465=3,IF($AF$2=2,(R465/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I465,Refurb_Poss_Tbl[%]))*AG465,IF($AF$2=3,(R465*AG465)-AV465,R465*AG465)),0)","v":0},{"$f":"IF(AF465=3,IF($AF$2=2,(S465/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I465,Refurb_Poss_Tbl[%]))*AG465,IF($AF$2=3,(S465*AG465)-AX465,S465*AG465)),0)","v":0},{"$f":"IF($AF465=3,IF($AF$2=2,(T465/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I465,Refurb_Poss_Tbl[%]))*AG465,T465*$AG465),0)","v":0},{"$f":"IF($AF465=3,IF($AF$2=2,(Q465/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I465,Refurb_Poss_Tbl[%]))*AG465,Q465*$AG465),0)","v":0},{"$f":"IF($AF465=3,IF($AF$2=2,(U465/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I465,Refurb_Poss_Tbl[%]))*AG465,U465*$AG465),0)","v":0},{"$f":"IF($AF465=3,IF($AF$2=2,(V465/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I465,Refurb_Poss_Tbl[%]))*AG465,IF($AF$2=3,(V465*AG465)-AW465,V465*AG465)),0)","v":0},{"$f":"IF($AF465=3,IF($AF$2=2,(W465/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I465,Refurb_Poss_Tbl[%]))*AG465,W465*$AG465),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,60,2,{"$f":"VLOOKUP(AE466,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1697330900164177},0,0,0,0,0,0,0,0,3.2499719191373551E-5,{"$f":"IF(OR(AF466=3,AF466=2,AF466=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D466,FlatMaint!$Y$2:$Y$10000,AE466)*AG466,0)","v":5.4889501598967508E-2},{"$f":"IF(OR(AF466=3,AF466=2,AF466=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D466,FlatRepair!$Y$2:$Y$10000,AE466)*AG466,0)","v":0},0,5.4922001318158879E-2,5.453807733314768E-2,0,0,0,0,0.10946007865130655,0,{"$f":"IF($AF466=3,IF($AF$2=2,(R466/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I466,Refurb_Poss_Tbl[%]))*AG466,IF($AF$2=3,(R466*AG466)-AV466,R466*AG466)),0)","v":0},{"$f":"IF(AF466=3,IF($AF$2=2,(S466/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I466,Refurb_Poss_Tbl[%]))*AG466,IF($AF$2=3,(S466*AG466)-AX466,S466*AG466)),0)","v":0},{"$f":"IF($AF466=3,IF($AF$2=2,(T466/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I466,Refurb_Poss_Tbl[%]))*AG466,T466*$AG466),0)","v":0},{"$f":"IF($AF466=3,IF($AF$2=2,(Q466/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I466,Refurb_Poss_Tbl[%]))*AG466,Q466*$AG466),0)","v":0},{"$f":"IF($AF466=3,IF($AF$2=2,(U466/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I466,Refurb_Poss_Tbl[%]))*AG466,U466*$AG466),0)","v":0},{"$f":"IF($AF466=3,IF($AF$2=2,(V466/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I466,Refurb_Poss_Tbl[%]))*AG466,IF($AF$2=3,(V466*AG466)-AW466,V466*AG466)),0)","v":0},{"$f":"IF($AF466=3,IF($AF$2=2,(W466/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I466,Refurb_Poss_Tbl[%]))*AG466,W466*$AG466),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,61,0,{"$f":"VLOOKUP(AE467,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.16478940778292983},0,0,0,0,0,0,0,0,3.155312542851801E-5,{"$f":"IF(OR(AF467=3,AF467=2,AF467=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D467,FlatMaint!$Y$2:$Y$10000,AE467)*AG467,0)","v":5.3290778251424767E-2},{"$f":"IF(OR(AF467=3,AF467=2,AF467=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D467,FlatRepair!$Y$2:$Y$10000,AE467)*AG467,0)","v":0},0,5.3322331376853285E-2,0,0,0,0,0,5.3322331376853285E-2,0,{"$f":"IF($AF467=3,IF($AF$2=2,(R467/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I467,Refurb_Poss_Tbl[%]))*AG467,IF($AF$2=3,(R467*AG467)-AV467,R467*AG467)),0)","v":0},{"$f":"IF(AF467=3,IF($AF$2=2,(S467/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I467,Refurb_Poss_Tbl[%]))*AG467,IF($AF$2=3,(S467*AG467)-AX467,S467*AG467)),0)","v":0},{"$f":"IF($AF467=3,IF($AF$2=2,(T467/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I467,Refurb_Poss_Tbl[%]))*AG467,T467*$AG467),0)","v":0},{"$f":"IF($AF467=3,IF($AF$2=2,(Q467/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I467,Refurb_Poss_Tbl[%]))*AG467,Q467*$AG467),0)","v":0},{"$f":"IF($AF467=3,IF($AF$2=2,(U467/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I467,Refurb_Poss_Tbl[%]))*AG467,U467*$AG467),0)","v":0},{"$f":"IF($AF467=3,IF($AF$2=2,(V467/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I467,Refurb_Poss_Tbl[%]))*AG467,IF($AF$2=3,(V467*AG467)-AW467,V467*AG467)),0)","v":0},{"$f":"IF($AF467=3,IF($AF$2=2,(W467/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I467,Refurb_Poss_Tbl[%]))*AG467,W467*$AG467),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,62,0,{"$f":"VLOOKUP(AE468,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15998971629410663},0,0,0,0,0,0,0,0,3.0634102357784478E-5,{"$f":"IF(OR(AF468=3,AF468=2,AF468=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D468,FlatMaint!$Y$2:$Y$10000,AE468)*AG468,0)","v":5.1738619661577445E-2},{"$f":"IF(OR(AF468=3,AF468=2,AF468=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D468,FlatRepair!$Y$2:$Y$10000,AE468)*AG468,0)","v":0},0,5.1769253763935229E-2,0,0,0,0,0,5.1769253763935229E-2,0,{"$f":"IF($AF468=3,IF($AF$2=2,(R468/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I468,Refurb_Poss_Tbl[%]))*AG468,IF($AF$2=3,(R468*AG468)-AV468,R468*AG468)),0)","v":0},{"$f":"IF(AF468=3,IF($AF$2=2,(S468/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I468,Refurb_Poss_Tbl[%]))*AG468,IF($AF$2=3,(S468*AG468)-AX468,S468*AG468)),0)","v":0},{"$f":"IF($AF468=3,IF($AF$2=2,(T468/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I468,Refurb_Poss_Tbl[%]))*AG468,T468*$AG468),0)","v":0},{"$f":"IF($AF468=3,IF($AF$2=2,(Q468/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I468,Refurb_Poss_Tbl[%]))*AG468,Q468*$AG468),0)","v":0},{"$f":"IF($AF468=3,IF($AF$2=2,(U468/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I468,Refurb_Poss_Tbl[%]))*AG468,U468*$AG468),0)","v":0},{"$f":"IF($AF468=3,IF($AF$2=2,(V468/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I468,Refurb_Poss_Tbl[%]))*AG468,IF($AF$2=3,(V468*AG468)-AW468,V468*AG468)),0)","v":0},{"$f":"IF($AF468=3,IF($AF$2=2,(W468/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I468,Refurb_Poss_Tbl[%]))*AG468,W468*$AG468),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,63,0,{"$f":"VLOOKUP(AE469,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15532982164476369},0,0,0,0,0,0,0,0,2.9741846949305314E-5,{"$f":"IF(OR(AF469=3,AF469=2,AF469=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D469,FlatMaint!$Y$2:$Y$10000,AE469)*AG469,0)","v":5.0231669574347028E-2},{"$f":"IF(OR(AF469=3,AF469=2,AF469=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D469,FlatRepair!$Y$2:$Y$10000,AE469)*AG469,0)","v":0},0,5.026141142129633E-2,0,0,0,0,0,5.026141142129633E-2,0,{"$f":"IF($AF469=3,IF($AF$2=2,(R469/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I469,Refurb_Poss_Tbl[%]))*AG469,IF($AF$2=3,(R469*AG469)-AV469,R469*AG469)),0)","v":0},{"$f":"IF(AF469=3,IF($AF$2=2,(S469/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I469,Refurb_Poss_Tbl[%]))*AG469,IF($AF$2=3,(S469*AG469)-AX469,S469*AG469)),0)","v":0},{"$f":"IF($AF469=3,IF($AF$2=2,(T469/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I469,Refurb_Poss_Tbl[%]))*AG469,T469*$AG469),0)","v":0},{"$f":"IF($AF469=3,IF($AF$2=2,(Q469/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I469,Refurb_Poss_Tbl[%]))*AG469,Q469*$AG469),0)","v":0},{"$f":"IF($AF469=3,IF($AF$2=2,(U469/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I469,Refurb_Poss_Tbl[%]))*AG469,U469*$AG469),0)","v":0},{"$f":"IF($AF469=3,IF($AF$2=2,(V469/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I469,Refurb_Poss_Tbl[%]))*AG469,IF($AF$2=3,(V469*AG469)-AW469,V469*AG469)),0)","v":0},{"$f":"IF($AF469=3,IF($AF$2=2,(W469/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I469,Refurb_Poss_Tbl[%]))*AG469,W469*$AG469),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,64,0,{"$f":"VLOOKUP(AE470,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15080565208229488},0,0,0,0,0,0,0,0,2.8875579562432348E-5,{"$f":"IF(OR(AF470=3,AF470=2,AF470=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D470,FlatMaint!$Y$2:$Y$10000,AE470)*AG470,0)","v":4.8768611237230135E-2},{"$f":"IF(OR(AF470=3,AF470=2,AF470=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D470,FlatRepair!$Y$2:$Y$10000,AE470)*AG470,0)","v":0},0,4.8797486816792565E-2,0,0,0,0,0,4.8797486816792565E-2,0,{"$f":"IF($AF470=3,IF($AF$2=2,(R470/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I470,Refurb_Poss_Tbl[%]))*AG470,IF($AF$2=3,(R470*AG470)-AV470,R470*AG470)),0)","v":0},{"$f":"IF(AF470=3,IF($AF$2=2,(S470/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I470,Refurb_Poss_Tbl[%]))*AG470,IF($AF$2=3,(S470*AG470)-AX470,S470*AG470)),0)","v":0},{"$f":"IF($AF470=3,IF($AF$2=2,(T470/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I470,Refurb_Poss_Tbl[%]))*AG470,T470*$AG470),0)","v":0},{"$f":"IF($AF470=3,IF($AF$2=2,(Q470/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I470,Refurb_Poss_Tbl[%]))*AG470,Q470*$AG470),0)","v":0},{"$f":"IF($AF470=3,IF($AF$2=2,(U470/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I470,Refurb_Poss_Tbl[%]))*AG470,U470*$AG470),0)","v":0},{"$f":"IF($AF470=3,IF($AF$2=2,(V470/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I470,Refurb_Poss_Tbl[%]))*AG470,IF($AF$2=3,(V470*AG470)-AW470,V470*AG470)),0)","v":0},{"$f":"IF($AF470=3,IF($AF$2=2,(W470/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I470,Refurb_Poss_Tbl[%]))*AG470,W470*$AG470),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,65,0,{"$f":"VLOOKUP(AE471,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14641325444882999},0,0,0,0,0,0,0,0,2.803454326449743E-5,{"$f":"IF(OR(AF471=3,AF471=2,AF471=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D471,FlatMaint!$Y$2:$Y$10000,AE471)*AG471,0)","v":4.7348166249737998E-2},{"$f":"IF(OR(AF471=3,AF471=2,AF471=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D471,FlatRepair!$Y$2:$Y$10000,AE471)*AG471,0)","v":0},0,4.7376200793002497E-2,0,0,0,0,0,4.7376200793002497E-2,0,{"$f":"IF($AF471=3,IF($AF$2=2,(R471/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I471,Refurb_Poss_Tbl[%]))*AG471,IF($AF$2=3,(R471*AG471)-AV471,R471*AG471)),0)","v":0},{"$f":"IF(AF471=3,IF($AF$2=2,(S471/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I471,Refurb_Poss_Tbl[%]))*AG471,IF($AF$2=3,(S471*AG471)-AX471,S471*AG471)),0)","v":0},{"$f":"IF($AF471=3,IF($AF$2=2,(T471/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I471,Refurb_Poss_Tbl[%]))*AG471,T471*$AG471),0)","v":0},{"$f":"IF($AF471=3,IF($AF$2=2,(Q471/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I471,Refurb_Poss_Tbl[%]))*AG471,Q471*$AG471),0)","v":0},{"$f":"IF($AF471=3,IF($AF$2=2,(U471/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I471,Refurb_Poss_Tbl[%]))*AG471,U471*$AG471),0)","v":0},{"$f":"IF($AF471=3,IF($AF$2=2,(V471/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I471,Refurb_Poss_Tbl[%]))*AG471,IF($AF$2=3,(V471*AG471)-AW471,V471*AG471)),0)","v":0},{"$f":"IF($AF471=3,IF($AF$2=2,(W471/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I471,Refurb_Poss_Tbl[%]))*AG471,W471*$AG471),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,66,0,{"$f":"VLOOKUP(AE472,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14214879072701941},0,0,0,0,0,0,0,0,2.7218003169414979E-5,{"$f":"IF(OR(AF472=3,AF472=2,AF472=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D472,FlatMaint!$Y$2:$Y$10000,AE472)*AG472,0)","v":4.5969093446347573E-2},{"$f":"IF(OR(AF472=3,AF472=2,AF472=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D472,FlatRepair!$Y$2:$Y$10000,AE472)*AG472,0)","v":0},0,4.5996311449516984E-2,0,0,0,0,0,4.5996311449516984E-2,0,{"$f":"IF($AF472=3,IF($AF$2=2,(R472/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I472,Refurb_Poss_Tbl[%]))*AG472,IF($AF$2=3,(R472*AG472)-AV472,R472*AG472)),0)","v":0},{"$f":"IF(AF472=3,IF($AF$2=2,(S472/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I472,Refurb_Poss_Tbl[%]))*AG472,IF($AF$2=3,(S472*AG472)-AX472,S472*AG472)),0)","v":0},{"$f":"IF($AF472=3,IF($AF$2=2,(T472/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I472,Refurb_Poss_Tbl[%]))*AG472,T472*$AG472),0)","v":0},{"$f":"IF($AF472=3,IF($AF$2=2,(Q472/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I472,Refurb_Poss_Tbl[%]))*AG472,Q472*$AG472),0)","v":0},{"$f":"IF($AF472=3,IF($AF$2=2,(U472/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I472,Refurb_Poss_Tbl[%]))*AG472,U472*$AG472),0)","v":0},{"$f":"IF($AF472=3,IF($AF$2=2,(V472/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I472,Refurb_Poss_Tbl[%]))*AG472,IF($AF$2=3,(V472*AG472)-AW472,V472*AG472)),0)","v":0},{"$f":"IF($AF472=3,IF($AF$2=2,(W472/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I472,Refurb_Poss_Tbl[%]))*AG472,W472*$AG472),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,67,0,{"$f":"VLOOKUP(AE473,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1380085346864266},0,0,0,0,0,0,0,0,2.6425245795548522E-5,{"$f":"IF(OR(AF473=3,AF473=2,AF473=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D473,FlatMaint!$Y$2:$Y$10000,AE473)*AG473,0)","v":4.463018781198793E-2},{"$f":"IF(OR(AF473=3,AF473=2,AF473=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D473,FlatRepair!$Y$2:$Y$10000,AE473)*AG473,0)","v":0},0,4.4656613057783477E-2,0,0,0,0,0,4.4656613057783477E-2,0,{"$f":"IF($AF473=3,IF($AF$2=2,(R473/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I473,Refurb_Poss_Tbl[%]))*AG473,IF($AF$2=3,(R473*AG473)-AV473,R473*AG473)),0)","v":0},{"$f":"IF(AF473=3,IF($AF$2=2,(S473/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I473,Refurb_Poss_Tbl[%]))*AG473,IF($AF$2=3,(S473*AG473)-AX473,S473*AG473)),0)","v":0},{"$f":"IF($AF473=3,IF($AF$2=2,(T473/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I473,Refurb_Poss_Tbl[%]))*AG473,T473*$AG473),0)","v":0},{"$f":"IF($AF473=3,IF($AF$2=2,(Q473/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I473,Refurb_Poss_Tbl[%]))*AG473,Q473*$AG473),0)","v":0},{"$f":"IF($AF473=3,IF($AF$2=2,(U473/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I473,Refurb_Poss_Tbl[%]))*AG473,U473*$AG473),0)","v":0},{"$f":"IF($AF473=3,IF($AF$2=2,(V473/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I473,Refurb_Poss_Tbl[%]))*AG473,IF($AF$2=3,(V473*AG473)-AW473,V473*AG473)),0)","v":0},{"$f":"IF($AF473=3,IF($AF$2=2,(W473/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I473,Refurb_Poss_Tbl[%]))*AG473,W473*$AG473),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,68,0,{"$f":"VLOOKUP(AE474,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13398886862759865},0,0,0,0,0,0,0,0,2.5655578442280119E-5,{"$f":"IF(OR(AF474=3,AF474=2,AF474=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D474,FlatMaint!$Y$2:$Y$10000,AE474)*AG474,0)","v":4.3330279429114493E-2},{"$f":"IF(OR(AF474=3,AF474=2,AF474=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D474,FlatRepair!$Y$2:$Y$10000,AE474)*AG474,0)","v":0},0,4.3355935007556773E-2,0,0,0,0,0,4.3355935007556773E-2,0,{"$f":"IF($AF474=3,IF($AF$2=2,(R474/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I474,Refurb_Poss_Tbl[%]))*AG474,IF($AF$2=3,(R474*AG474)-AV474,R474*AG474)),0)","v":0},{"$f":"IF(AF474=3,IF($AF$2=2,(S474/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I474,Refurb_Poss_Tbl[%]))*AG474,IF($AF$2=3,(S474*AG474)-AX474,S474*AG474)),0)","v":0},{"$f":"IF($AF474=3,IF($AF$2=2,(T474/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I474,Refurb_Poss_Tbl[%]))*AG474,T474*$AG474),0)","v":0},{"$f":"IF($AF474=3,IF($AF$2=2,(Q474/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I474,Refurb_Poss_Tbl[%]))*AG474,Q474*$AG474),0)","v":0},{"$f":"IF($AF474=3,IF($AF$2=2,(U474/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I474,Refurb_Poss_Tbl[%]))*AG474,U474*$AG474),0)","v":0},{"$f":"IF($AF474=3,IF($AF$2=2,(V474/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I474,Refurb_Poss_Tbl[%]))*AG474,IF($AF$2=3,(V474*AG474)-AW474,V474*AG474)),0)","v":0},{"$f":"IF($AF474=3,IF($AF$2=2,(W474/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I474,Refurb_Poss_Tbl[%]))*AG474,W474*$AG474),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,69,0,{"$f":"VLOOKUP(AE475,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13008628022096957},0,0,0,0,0,0,0,0,2.4908328584737984E-5,{"$f":"IF(OR(AF475=3,AF475=2,AF475=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D475,FlatMaint!$Y$2:$Y$10000,AE475)*AG475,0)","v":4.2068232455450973E-2},{"$f":"IF(OR(AF475=3,AF475=2,AF475=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D475,FlatRepair!$Y$2:$Y$10000,AE475)*AG475,0)","v":0},0,4.2093140784035712E-2,0,0,0,0,0,4.2093140784035712E-2,0,{"$f":"IF($AF475=3,IF($AF$2=2,(R475/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I475,Refurb_Poss_Tbl[%]))*AG475,IF($AF$2=3,(R475*AG475)-AV475,R475*AG475)),0)","v":0},{"$f":"IF(AF475=3,IF($AF$2=2,(S475/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I475,Refurb_Poss_Tbl[%]))*AG475,IF($AF$2=3,(S475*AG475)-AX475,S475*AG475)),0)","v":0},{"$f":"IF($AF475=3,IF($AF$2=2,(T475/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I475,Refurb_Poss_Tbl[%]))*AG475,T475*$AG475),0)","v":0},{"$f":"IF($AF475=3,IF($AF$2=2,(Q475/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I475,Refurb_Poss_Tbl[%]))*AG475,Q475*$AG475),0)","v":0},{"$f":"IF($AF475=3,IF($AF$2=2,(U475/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I475,Refurb_Poss_Tbl[%]))*AG475,U475*$AG475),0)","v":0},{"$f":"IF($AF475=3,IF($AF$2=2,(V475/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I475,Refurb_Poss_Tbl[%]))*AG475,IF($AF$2=3,(V475*AG475)-AW475,V475*AG475)),0)","v":0},{"$f":"IF($AF475=3,IF($AF$2=2,(W475/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I475,Refurb_Poss_Tbl[%]))*AG475,W475*$AG475),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,70,0,{"$f":"VLOOKUP(AE476,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12629735943783454},0,0,0,0,0,0,0,0,2.4182843286153384E-5,{"$f":"IF(OR(AF476=3,AF476=2,AF476=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D476,FlatMaint!$Y$2:$Y$10000,AE476)*AG476,0)","v":4.0842944131505798E-2},{"$f":"IF(OR(AF476=3,AF476=2,AF476=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D476,FlatRepair!$Y$2:$Y$10000,AE476)*AG476,0)","v":0},0,4.0867126974791952E-2,0,0,0,0,0,4.0867126974791952E-2,0,{"$f":"IF($AF476=3,IF($AF$2=2,(R476/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I476,Refurb_Poss_Tbl[%]))*AG476,IF($AF$2=3,(R476*AG476)-AV476,R476*AG476)),0)","v":0},{"$f":"IF(AF476=3,IF($AF$2=2,(S476/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I476,Refurb_Poss_Tbl[%]))*AG476,IF($AF$2=3,(S476*AG476)-AX476,S476*AG476)),0)","v":0},{"$f":"IF($AF476=3,IF($AF$2=2,(T476/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I476,Refurb_Poss_Tbl[%]))*AG476,T476*$AG476),0)","v":0},{"$f":"IF($AF476=3,IF($AF$2=2,(Q476/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I476,Refurb_Poss_Tbl[%]))*AG476,Q476*$AG476),0)","v":0},{"$f":"IF($AF476=3,IF($AF$2=2,(U476/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I476,Refurb_Poss_Tbl[%]))*AG476,U476*$AG476),0)","v":0},{"$f":"IF($AF476=3,IF($AF$2=2,(V476/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I476,Refurb_Poss_Tbl[%]))*AG476,IF($AF$2=3,(V476*AG476)-AW476,V476*AG476)),0)","v":0},{"$f":"IF($AF476=3,IF($AF$2=2,(W476/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I476,Refurb_Poss_Tbl[%]))*AG476,W476*$AG476),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,71,0,{"$f":"VLOOKUP(AE477,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12261879557071313},0,0,0,0,0,0,0,0,2.3478488627333376E-5,{"$f":"IF(OR(AF477=3,AF477=2,AF477=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D477,FlatMaint!$Y$2:$Y$10000,AE477)*AG477,0)","v":3.9653343816995916E-2},{"$f":"IF(OR(AF477=3,AF477=2,AF477=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D477,FlatRepair!$Y$2:$Y$10000,AE477)*AG477,0)","v":0},0,3.9676822305623249E-2,0,0,0,0,0,3.9676822305623249E-2,0,{"$f":"IF($AF477=3,IF($AF$2=2,(R477/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I477,Refurb_Poss_Tbl[%]))*AG477,IF($AF$2=3,(R477*AG477)-AV477,R477*AG477)),0)","v":0},{"$f":"IF(AF477=3,IF($AF$2=2,(S477/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I477,Refurb_Poss_Tbl[%]))*AG477,IF($AF$2=3,(S477*AG477)-AX477,S477*AG477)),0)","v":0},{"$f":"IF($AF477=3,IF($AF$2=2,(T477/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I477,Refurb_Poss_Tbl[%]))*AG477,T477*$AG477),0)","v":0},{"$f":"IF($AF477=3,IF($AF$2=2,(Q477/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I477,Refurb_Poss_Tbl[%]))*AG477,Q477*$AG477),0)","v":0},{"$f":"IF($AF477=3,IF($AF$2=2,(U477/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I477,Refurb_Poss_Tbl[%]))*AG477,U477*$AG477),0)","v":0},{"$f":"IF($AF477=3,IF($AF$2=2,(V477/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I477,Refurb_Poss_Tbl[%]))*AG477,IF($AF$2=3,(V477*AG477)-AW477,V477*AG477)),0)","v":0},{"$f":"IF($AF477=3,IF($AF$2=2,(W477/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I477,Refurb_Poss_Tbl[%]))*AG477,W477*$AG477),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,72,0,{"$f":"VLOOKUP(AE478,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1190473743404982},0,0,0,0,0,0,0,0,2.2794649152750853E-5,{"$f":"IF(OR(AF478=3,AF478=2,AF478=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D478,FlatMaint!$Y$2:$Y$10000,AE478)*AG478,0)","v":3.8498392055335846E-2},{"$f":"IF(OR(AF478=3,AF478=2,AF478=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D478,FlatRepair!$Y$2:$Y$10000,AE478)*AG478,0)","v":0},0,3.8521186704488598E-2,0,0,0,0,0,3.8521186704488598E-2,0,{"$f":"IF($AF478=3,IF($AF$2=2,(R478/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I478,Refurb_Poss_Tbl[%]))*AG478,IF($AF$2=3,(R478*AG478)-AV478,R478*AG478)),0)","v":0},{"$f":"IF(AF478=3,IF($AF$2=2,(S478/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I478,Refurb_Poss_Tbl[%]))*AG478,IF($AF$2=3,(S478*AG478)-AX478,S478*AG478)),0)","v":0},{"$f":"IF($AF478=3,IF($AF$2=2,(T478/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I478,Refurb_Poss_Tbl[%]))*AG478,T478*$AG478),0)","v":0},{"$f":"IF($AF478=3,IF($AF$2=2,(Q478/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I478,Refurb_Poss_Tbl[%]))*AG478,Q478*$AG478),0)","v":0},{"$f":"IF($AF478=3,IF($AF$2=2,(U478/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I478,Refurb_Poss_Tbl[%]))*AG478,U478*$AG478),0)","v":0},{"$f":"IF($AF478=3,IF($AF$2=2,(V478/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I478,Refurb_Poss_Tbl[%]))*AG478,IF($AF$2=3,(V478*AG478)-AW478,V478*AG478)),0)","v":0},{"$f":"IF($AF478=3,IF($AF$2=2,(W478/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I478,Refurb_Poss_Tbl[%]))*AG478,W478*$AG478),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,73,0,{"$f":"VLOOKUP(AE479,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11557997508786232},0,0,0,0,0,0,0,0,2.2130727332767819E-5,{"$f":"IF(OR(AF479=3,AF479=2,AF479=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D479,FlatMaint!$Y$2:$Y$10000,AE479)*AG479,0)","v":3.7377079665374603E-2},{"$f":"IF(OR(AF479=3,AF479=2,AF479=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D479,FlatRepair!$Y$2:$Y$10000,AE479)*AG479,0)","v":0},0,3.7399210392707369E-2,0,0,0,0,0,3.7399210392707369E-2,0,{"$f":"IF($AF479=3,IF($AF$2=2,(R479/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I479,Refurb_Poss_Tbl[%]))*AG479,IF($AF$2=3,(R479*AG479)-AV479,R479*AG479)),0)","v":0},{"$f":"IF(AF479=3,IF($AF$2=2,(S479/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I479,Refurb_Poss_Tbl[%]))*AG479,IF($AF$2=3,(S479*AG479)-AX479,S479*AG479)),0)","v":0},{"$f":"IF($AF479=3,IF($AF$2=2,(T479/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I479,Refurb_Poss_Tbl[%]))*AG479,T479*$AG479),0)","v":0},{"$f":"IF($AF479=3,IF($AF$2=2,(Q479/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I479,Refurb_Poss_Tbl[%]))*AG479,Q479*$AG479),0)","v":0},{"$f":"IF($AF479=3,IF($AF$2=2,(U479/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I479,Refurb_Poss_Tbl[%]))*AG479,U479*$AG479),0)","v":0},{"$f":"IF($AF479=3,IF($AF$2=2,(V479/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I479,Refurb_Poss_Tbl[%]))*AG479,IF($AF$2=3,(V479*AG479)-AW479,V479*AG479)),0)","v":0},{"$f":"IF($AF479=3,IF($AF$2=2,(W479/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I479,Refurb_Poss_Tbl[%]))*AG479,W479*$AG479),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,74,0,{"$f":"VLOOKUP(AE480,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11221356804646829},0,0,0,0,0,0,0,0,2.1486143041522157E-5,{"$f":"IF(OR(AF480=3,AF480=2,AF480=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D480,FlatMaint!$Y$2:$Y$10000,AE480)*AG480,0)","v":3.6288426859586997E-2},{"$f":"IF(OR(AF480=3,AF480=2,AF480=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D480,FlatRepair!$Y$2:$Y$10000,AE480)*AG480,0)","v":0},0,3.6309913002628522E-2,0,0,0,0,0,3.6309913002628522E-2,0,{"$f":"IF($AF480=3,IF($AF$2=2,(R480/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I480,Refurb_Poss_Tbl[%]))*AG480,IF($AF$2=3,(R480*AG480)-AV480,R480*AG480)),0)","v":0},{"$f":"IF(AF480=3,IF($AF$2=2,(S480/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I480,Refurb_Poss_Tbl[%]))*AG480,IF($AF$2=3,(S480*AG480)-AX480,S480*AG480)),0)","v":0},{"$f":"IF($AF480=3,IF($AF$2=2,(T480/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I480,Refurb_Poss_Tbl[%]))*AG480,T480*$AG480),0)","v":0},{"$f":"IF($AF480=3,IF($AF$2=2,(Q480/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I480,Refurb_Poss_Tbl[%]))*AG480,Q480*$AG480),0)","v":0},{"$f":"IF($AF480=3,IF($AF$2=2,(U480/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I480,Refurb_Poss_Tbl[%]))*AG480,U480*$AG480),0)","v":0},{"$f":"IF($AF480=3,IF($AF$2=2,(V480/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I480,Refurb_Poss_Tbl[%]))*AG480,IF($AF$2=3,(V480*AG480)-AW480,V480*AG480)),0)","v":0},{"$f":"IF($AF480=3,IF($AF$2=2,(W480/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I480,Refurb_Poss_Tbl[%]))*AG480,W480*$AG480),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,75,0,{"$f":"VLOOKUP(AE481,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10894521169560026},0,0,0,0,0,0,0,0,2.0860333050021508E-5,{"$f":"IF(OR(AF481=3,AF481=2,AF481=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D481,FlatMaint!$Y$2:$Y$10000,AE481)*AG481,0)","v":3.5231482387948536E-2},{"$f":"IF(OR(AF481=3,AF481=2,AF481=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D481,FlatRepair!$Y$2:$Y$10000,AE481)*AG481,0)","v":0},0,3.5252342720998558E-2,0,0,0,0,0,3.5252342720998558E-2,0,{"$f":"IF($AF481=3,IF($AF$2=2,(R481/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I481,Refurb_Poss_Tbl[%]))*AG481,IF($AF$2=3,(R481*AG481)-AV481,R481*AG481)),0)","v":0},{"$f":"IF(AF481=3,IF($AF$2=2,(S481/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I481,Refurb_Poss_Tbl[%]))*AG481,IF($AF$2=3,(S481*AG481)-AX481,S481*AG481)),0)","v":0},{"$f":"IF($AF481=3,IF($AF$2=2,(T481/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I481,Refurb_Poss_Tbl[%]))*AG481,T481*$AG481),0)","v":0},{"$f":"IF($AF481=3,IF($AF$2=2,(Q481/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I481,Refurb_Poss_Tbl[%]))*AG481,Q481*$AG481),0)","v":0},{"$f":"IF($AF481=3,IF($AF$2=2,(U481/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I481,Refurb_Poss_Tbl[%]))*AG481,U481*$AG481),0)","v":0},{"$f":"IF($AF481=3,IF($AF$2=2,(V481/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I481,Refurb_Poss_Tbl[%]))*AG481,IF($AF$2=3,(V481*AG481)-AW481,V481*AG481)),0)","v":0},{"$f":"IF($AF481=3,IF($AF$2=2,(W481/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I481,Refurb_Poss_Tbl[%]))*AG481,W481*$AG481),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,76,0,{"$f":"VLOOKUP(AE482,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.15310389176729922},0,0,0,0,0,0,0,0,2.9315636032210206E-5,{"$f":"IF(OR(AF482=3,AF482=2,AF482=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D482,FlatMaint!$Y$2:$Y$10000,AE482)*AG482,0)","v":4.9511832437366503E-2},{"$f":"IF(OR(AF482=3,AF482=2,AF482=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D482,FlatRepair!$Y$2:$Y$10000,AE482)*AG482,0)","v":0},0,4.9541148073398711E-2,0,0,0,0,0,4.9541148073398711E-2,0,{"$f":"IF($AF482=3,IF($AF$2=2,(R482/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I482,Refurb_Poss_Tbl[%]))*AG482,IF($AF$2=3,(R482*AG482)-AV482,R482*AG482)),0)","v":0},{"$f":"IF(AF482=3,IF($AF$2=2,(S482/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I482,Refurb_Poss_Tbl[%]))*AG482,IF($AF$2=3,(S482*AG482)-AX482,S482*AG482)),0)","v":0},{"$f":"IF($AF482=3,IF($AF$2=2,(T482/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I482,Refurb_Poss_Tbl[%]))*AG482,T482*$AG482),0)","v":0},{"$f":"IF($AF482=3,IF($AF$2=2,(Q482/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I482,Refurb_Poss_Tbl[%]))*AG482,Q482*$AG482),0)","v":0},{"$f":"IF($AF482=3,IF($AF$2=2,(U482/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I482,Refurb_Poss_Tbl[%]))*AG482,U482*$AG482),0)","v":0},{"$f":"IF($AF482=3,IF($AF$2=2,(V482/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I482,Refurb_Poss_Tbl[%]))*AG482,IF($AF$2=3,(V482*AG482)-AW482,V482*AG482)),0)","v":0},{"$f":"IF($AF482=3,IF($AF$2=2,(W482/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I482,Refurb_Poss_Tbl[%]))*AG482,W482*$AG482),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,77,0,{"$f":"VLOOKUP(AE483,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14936965050468218},0,0,0,0,0,0,0,0,2.8600620519229472E-5,{"$f":"IF(OR(AF483=3,AF483=2,AF483=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D483,FlatMaint!$Y$2:$Y$10000,AE483)*AG483,0)","v":4.8304226768162442E-2},{"$f":"IF(OR(AF483=3,AF483=2,AF483=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D483,FlatRepair!$Y$2:$Y$10000,AE483)*AG483,0)","v":0},0,4.8332827388681672E-2,0,0,0,0,0,4.8332827388681672E-2,0,{"$f":"IF($AF483=3,IF($AF$2=2,(R483/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I483,Refurb_Poss_Tbl[%]))*AG483,IF($AF$2=3,(R483*AG483)-AV483,R483*AG483)),0)","v":0},{"$f":"IF(AF483=3,IF($AF$2=2,(S483/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I483,Refurb_Poss_Tbl[%]))*AG483,IF($AF$2=3,(S483*AG483)-AX483,S483*AG483)),0)","v":0},{"$f":"IF($AF483=3,IF($AF$2=2,(T483/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I483,Refurb_Poss_Tbl[%]))*AG483,T483*$AG483),0)","v":0},{"$f":"IF($AF483=3,IF($AF$2=2,(Q483/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I483,Refurb_Poss_Tbl[%]))*AG483,Q483*$AG483),0)","v":0},{"$f":"IF($AF483=3,IF($AF$2=2,(U483/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I483,Refurb_Poss_Tbl[%]))*AG483,U483*$AG483),0)","v":0},{"$f":"IF($AF483=3,IF($AF$2=2,(V483/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I483,Refurb_Poss_Tbl[%]))*AG483,IF($AF$2=3,(V483*AG483)-AW483,V483*AG483)),0)","v":0},{"$f":"IF($AF483=3,IF($AF$2=2,(W483/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I483,Refurb_Poss_Tbl[%]))*AG483,W483*$AG483),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,78,0,{"$f":"VLOOKUP(AE484,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14572648829725093},0,0,0,0,0,0,0,0,2.7903044409004367E-5,{"$f":"IF(OR(AF484=3,AF484=2,AF484=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D484,FlatMaint!$Y$2:$Y$10000,AE484)*AG484,0)","v":4.7126074895768248E-2},{"$f":"IF(OR(AF484=3,AF484=2,AF484=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D484,FlatRepair!$Y$2:$Y$10000,AE484)*AG484,0)","v":0},0,4.7153977940177255E-2,0,0,0,0,0,4.7153977940177255E-2,0,{"$f":"IF($AF484=3,IF($AF$2=2,(R484/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I484,Refurb_Poss_Tbl[%]))*AG484,IF($AF$2=3,(R484*AG484)-AV484,R484*AG484)),0)","v":0},{"$f":"IF(AF484=3,IF($AF$2=2,(S484/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I484,Refurb_Poss_Tbl[%]))*AG484,IF($AF$2=3,(S484*AG484)-AX484,S484*AG484)),0)","v":0},{"$f":"IF($AF484=3,IF($AF$2=2,(T484/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I484,Refurb_Poss_Tbl[%]))*AG484,T484*$AG484),0)","v":0},{"$f":"IF($AF484=3,IF($AF$2=2,(Q484/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I484,Refurb_Poss_Tbl[%]))*AG484,Q484*$AG484),0)","v":0},{"$f":"IF($AF484=3,IF($AF$2=2,(U484/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I484,Refurb_Poss_Tbl[%]))*AG484,U484*$AG484),0)","v":0},{"$f":"IF($AF484=3,IF($AF$2=2,(V484/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I484,Refurb_Poss_Tbl[%]))*AG484,IF($AF$2=3,(V484*AG484)-AW484,V484*AG484)),0)","v":0},{"$f":"IF($AF484=3,IF($AF$2=2,(W484/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I484,Refurb_Poss_Tbl[%]))*AG484,W484*$AG484),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,79,0,{"$f":"VLOOKUP(AE485,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.14217218370463502},0,0,0,0,0,0,0,0,2.7222482350248157E-5,{"$f":"IF(OR(AF485=3,AF485=2,AF485=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D485,FlatMaint!$Y$2:$Y$10000,AE485)*AG485,0)","v":4.5976658434895838E-2},{"$f":"IF(OR(AF485=3,AF485=2,AF485=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D485,FlatRepair!$Y$2:$Y$10000,AE485)*AG485,0)","v":0},0,4.6003880917246089E-2,0,0,0,0,0,4.6003880917246089E-2,0,{"$f":"IF($AF485=3,IF($AF$2=2,(R485/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I485,Refurb_Poss_Tbl[%]))*AG485,IF($AF$2=3,(R485*AG485)-AV485,R485*AG485)),0)","v":0},{"$f":"IF(AF485=3,IF($AF$2=2,(S485/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I485,Refurb_Poss_Tbl[%]))*AG485,IF($AF$2=3,(S485*AG485)-AX485,S485*AG485)),0)","v":0},{"$f":"IF($AF485=3,IF($AF$2=2,(T485/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I485,Refurb_Poss_Tbl[%]))*AG485,T485*$AG485),0)","v":0},{"$f":"IF($AF485=3,IF($AF$2=2,(Q485/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I485,Refurb_Poss_Tbl[%]))*AG485,Q485*$AG485),0)","v":0},{"$f":"IF($AF485=3,IF($AF$2=2,(U485/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I485,Refurb_Poss_Tbl[%]))*AG485,U485*$AG485),0)","v":0},{"$f":"IF($AF485=3,IF($AF$2=2,(V485/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I485,Refurb_Poss_Tbl[%]))*AG485,IF($AF$2=3,(V485*AG485)-AW485,V485*AG485)),0)","v":0},{"$f":"IF($AF485=3,IF($AF$2=2,(W485/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I485,Refurb_Poss_Tbl[%]))*AG485,W485*$AG485),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,80,0,{"$f":"VLOOKUP(AE486,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13870456946793663},0,0,0,0,0,0,0,0,2.6558519366095766E-5,{"$f":"IF(OR(AF486=3,AF486=2,AF486=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D486,FlatMaint!$Y$2:$Y$10000,AE486)*AG486,0)","v":4.4855276521849612E-2},{"$f":"IF(OR(AF486=3,AF486=2,AF486=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D486,FlatRepair!$Y$2:$Y$10000,AE486)*AG486,0)","v":0},0,4.4881835041215706E-2,0,0,0,0,0,4.4881835041215706E-2,0,{"$f":"IF($AF486=3,IF($AF$2=2,(R486/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I486,Refurb_Poss_Tbl[%]))*AG486,IF($AF$2=3,(R486*AG486)-AV486,R486*AG486)),0)","v":0},{"$f":"IF(AF486=3,IF($AF$2=2,(S486/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I486,Refurb_Poss_Tbl[%]))*AG486,IF($AF$2=3,(S486*AG486)-AX486,S486*AG486)),0)","v":0},{"$f":"IF($AF486=3,IF($AF$2=2,(T486/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I486,Refurb_Poss_Tbl[%]))*AG486,T486*$AG486),0)","v":0},{"$f":"IF($AF486=3,IF($AF$2=2,(Q486/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I486,Refurb_Poss_Tbl[%]))*AG486,Q486*$AG486),0)","v":0},{"$f":"IF($AF486=3,IF($AF$2=2,(U486/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I486,Refurb_Poss_Tbl[%]))*AG486,U486*$AG486),0)","v":0},{"$f":"IF($AF486=3,IF($AF$2=2,(V486/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I486,Refurb_Poss_Tbl[%]))*AG486,IF($AF$2=3,(V486*AG486)-AW486,V486*AG486)),0)","v":0},{"$f":"IF($AF486=3,IF($AF$2=2,(W486/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I486,Refurb_Poss_Tbl[%]))*AG486,W486*$AG486),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,81,0,{"$f":"VLOOKUP(AE487,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13532153118823087},0,0,0,0,0,0,0,0,2.5910750601069043E-5,{"$f":"IF(OR(AF487=3,AF487=2,AF487=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D487,FlatMaint!$Y$2:$Y$10000,AE487)*AG487,0)","v":4.3761245387170356E-2},{"$f":"IF(OR(AF487=3,AF487=2,AF487=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D487,FlatRepair!$Y$2:$Y$10000,AE487)*AG487,0)","v":0},0,4.3787156137771427E-2,0,0,0,0,0,4.3787156137771427E-2,0,{"$f":"IF($AF487=3,IF($AF$2=2,(R487/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I487,Refurb_Poss_Tbl[%]))*AG487,IF($AF$2=3,(R487*AG487)-AV487,R487*AG487)),0)","v":0},{"$f":"IF(AF487=3,IF($AF$2=2,(S487/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I487,Refurb_Poss_Tbl[%]))*AG487,IF($AF$2=3,(S487*AG487)-AX487,S487*AG487)),0)","v":0},{"$f":"IF($AF487=3,IF($AF$2=2,(T487/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I487,Refurb_Poss_Tbl[%]))*AG487,T487*$AG487),0)","v":0},{"$f":"IF($AF487=3,IF($AF$2=2,(Q487/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I487,Refurb_Poss_Tbl[%]))*AG487,Q487*$AG487),0)","v":0},{"$f":"IF($AF487=3,IF($AF$2=2,(U487/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I487,Refurb_Poss_Tbl[%]))*AG487,U487*$AG487),0)","v":0},{"$f":"IF($AF487=3,IF($AF$2=2,(V487/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I487,Refurb_Poss_Tbl[%]))*AG487,IF($AF$2=3,(V487*AG487)-AW487,V487*AG487)),0)","v":0},{"$f":"IF($AF487=3,IF($AF$2=2,(W487/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I487,Refurb_Poss_Tbl[%]))*AG487,W487*$AG487),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,82,0,{"$f":"VLOOKUP(AE488,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.13202100603729841},0,0,0,0,0,0,0,0,2.52787810742137E-5,{"$f":"IF(OR(AF488=3,AF488=2,AF488=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D488,FlatMaint!$Y$2:$Y$10000,AE488)*AG488,0)","v":4.2693897938702784E-2},{"$f":"IF(OR(AF488=3,AF488=2,AF488=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D488,FlatRepair!$Y$2:$Y$10000,AE488)*AG488,0)","v":0},0,4.2719176719776999E-2,0,0,0,0,0,4.2719176719776999E-2,0,{"$f":"IF($AF488=3,IF($AF$2=2,(R488/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I488,Refurb_Poss_Tbl[%]))*AG488,IF($AF$2=3,(R488*AG488)-AV488,R488*AG488)),0)","v":0},{"$f":"IF(AF488=3,IF($AF$2=2,(S488/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I488,Refurb_Poss_Tbl[%]))*AG488,IF($AF$2=3,(S488*AG488)-AX488,S488*AG488)),0)","v":0},{"$f":"IF($AF488=3,IF($AF$2=2,(T488/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I488,Refurb_Poss_Tbl[%]))*AG488,T488*$AG488),0)","v":0},{"$f":"IF($AF488=3,IF($AF$2=2,(Q488/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I488,Refurb_Poss_Tbl[%]))*AG488,Q488*$AG488),0)","v":0},{"$f":"IF($AF488=3,IF($AF$2=2,(U488/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I488,Refurb_Poss_Tbl[%]))*AG488,U488*$AG488),0)","v":0},{"$f":"IF($AF488=3,IF($AF$2=2,(V488/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I488,Refurb_Poss_Tbl[%]))*AG488,IF($AF$2=3,(V488*AG488)-AW488,V488*AG488)),0)","v":0},{"$f":"IF($AF488=3,IF($AF$2=2,(W488/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I488,Refurb_Poss_Tbl[%]))*AG488,W488*$AG488),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,83,0,{"$f":"VLOOKUP(AE489,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.12880098149980332},0,0,0,0,0,0,0,0,2.4662225438257267E-5,{"$f":"IF(OR(AF489=3,AF489=2,AF489=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D489,FlatMaint!$Y$2:$Y$10000,AE489)*AG489,0)","v":4.1652583354831983E-2},{"$f":"IF(OR(AF489=3,AF489=2,AF489=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D489,FlatRepair!$Y$2:$Y$10000,AE489)*AG489,0)","v":0},0,4.1677245580270243E-2,0,0,0,0,0,4.1677245580270243E-2,0,{"$f":"IF($AF489=3,IF($AF$2=2,(R489/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I489,Refurb_Poss_Tbl[%]))*AG489,IF($AF$2=3,(R489*AG489)-AV489,R489*AG489)),0)","v":0},{"$f":"IF(AF489=3,IF($AF$2=2,(S489/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I489,Refurb_Poss_Tbl[%]))*AG489,IF($AF$2=3,(S489*AG489)-AX489,S489*AG489)),0)","v":0},{"$f":"IF($AF489=3,IF($AF$2=2,(T489/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I489,Refurb_Poss_Tbl[%]))*AG489,T489*$AG489),0)","v":0},{"$f":"IF($AF489=3,IF($AF$2=2,(Q489/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I489,Refurb_Poss_Tbl[%]))*AG489,Q489*$AG489),0)","v":0},{"$f":"IF($AF489=3,IF($AF$2=2,(U489/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I489,Refurb_Poss_Tbl[%]))*AG489,U489*$AG489),0)","v":0},{"$f":"IF($AF489=3,IF($AF$2=2,(V489/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I489,Refurb_Poss_Tbl[%]))*AG489,IF($AF$2=3,(V489*AG489)-AW489,V489*AG489)),0)","v":0},{"$f":"IF($AF489=3,IF($AF$2=2,(W489/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I489,Refurb_Poss_Tbl[%]))*AG489,W489*$AG489),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,84,0,{"$f":"VLOOKUP(AE490,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1256594941461496},0,0,0,0,0,0,0,0,2.406070774464124E-5,{"$f":"IF(OR(AF490=3,AF490=2,AF490=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D490,FlatMaint!$Y$2:$Y$10000,AE490)*AG490,0)","v":4.0636666687640967E-2},{"$f":"IF(OR(AF490=3,AF490=2,AF490=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D490,FlatRepair!$Y$2:$Y$10000,AE490)*AG490,0)","v":0},0,4.0660727395385607E-2,0,0,0,0,0,4.0660727395385607E-2,0,{"$f":"IF($AF490=3,IF($AF$2=2,(R490/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I490,Refurb_Poss_Tbl[%]))*AG490,IF($AF$2=3,(R490*AG490)-AV490,R490*AG490)),0)","v":0},{"$f":"IF(AF490=3,IF($AF$2=2,(S490/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I490,Refurb_Poss_Tbl[%]))*AG490,IF($AF$2=3,(S490*AG490)-AX490,S490*AG490)),0)","v":0},{"$f":"IF($AF490=3,IF($AF$2=2,(T490/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I490,Refurb_Poss_Tbl[%]))*AG490,T490*$AG490),0)","v":0},{"$f":"IF($AF490=3,IF($AF$2=2,(Q490/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I490,Refurb_Poss_Tbl[%]))*AG490,Q490*$AG490),0)","v":0},{"$f":"IF($AF490=3,IF($AF$2=2,(U490/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I490,Refurb_Poss_Tbl[%]))*AG490,U490*$AG490),0)","v":0},{"$f":"IF($AF490=3,IF($AF$2=2,(V490/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I490,Refurb_Poss_Tbl[%]))*AG490,IF($AF$2=3,(V490*AG490)-AW490,V490*AG490)),0)","v":0},{"$f":"IF($AF490=3,IF($AF$2=2,(W490/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I490,Refurb_Poss_Tbl[%]))*AG490,W490*$AG490),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,85,0,{"$f":"VLOOKUP(AE491,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.1225946284352679},0,0,0,0,0,0,0,0,2.3473861214284135E-5,{"$f":"IF(OR(AF491=3,AF491=2,AF491=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D491,FlatMaint!$Y$2:$Y$10000,AE491)*AG491,0)","v":3.9645528475747281E-2},{"$f":"IF(OR(AF491=3,AF491=2,AF491=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D491,FlatRepair!$Y$2:$Y$10000,AE491)*AG491,0)","v":0},0,3.9669002336961565E-2,0,0,0,0,0,3.9669002336961565E-2,0,{"$f":"IF($AF491=3,IF($AF$2=2,(R491/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I491,Refurb_Poss_Tbl[%]))*AG491,IF($AF$2=3,(R491*AG491)-AV491,R491*AG491)),0)","v":0},{"$f":"IF(AF491=3,IF($AF$2=2,(S491/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I491,Refurb_Poss_Tbl[%]))*AG491,IF($AF$2=3,(S491*AG491)-AX491,S491*AG491)),0)","v":0},{"$f":"IF($AF491=3,IF($AF$2=2,(T491/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I491,Refurb_Poss_Tbl[%]))*AG491,T491*$AG491),0)","v":0},{"$f":"IF($AF491=3,IF($AF$2=2,(Q491/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I491,Refurb_Poss_Tbl[%]))*AG491,Q491*$AG491),0)","v":0},{"$f":"IF($AF491=3,IF($AF$2=2,(U491/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I491,Refurb_Poss_Tbl[%]))*AG491,U491*$AG491),0)","v":0},{"$f":"IF($AF491=3,IF($AF$2=2,(V491/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I491,Refurb_Poss_Tbl[%]))*AG491,IF($AF$2=3,(V491*AG491)-AW491,V491*AG491)),0)","v":0},{"$f":"IF($AF491=3,IF($AF$2=2,(W491/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I491,Refurb_Poss_Tbl[%]))*AG491,W491*$AG491),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,86,0,{"$f":"VLOOKUP(AE492,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11960451554660284},0,0,0,0,0,0,0,0,2.2901328013935746E-5,{"$f":"IF(OR(AF492=3,AF492=2,AF492=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D492,FlatMaint!$Y$2:$Y$10000,AE492)*AG492,0)","v":3.8678564366582714E-2},{"$f":"IF(OR(AF492=3,AF492=2,AF492=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D492,FlatRepair!$Y$2:$Y$10000,AE492)*AG492,0)","v":0},0,3.8701465694596648E-2,0,0,0,0,0,3.8701465694596648E-2,0,{"$f":"IF($AF492=3,IF($AF$2=2,(R492/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I492,Refurb_Poss_Tbl[%]))*AG492,IF($AF$2=3,(R492*AG492)-AV492,R492*AG492)),0)","v":0},{"$f":"IF(AF492=3,IF($AF$2=2,(S492/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I492,Refurb_Poss_Tbl[%]))*AG492,IF($AF$2=3,(S492*AG492)-AX492,S492*AG492)),0)","v":0},{"$f":"IF($AF492=3,IF($AF$2=2,(T492/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I492,Refurb_Poss_Tbl[%]))*AG492,T492*$AG492),0)","v":0},{"$f":"IF($AF492=3,IF($AF$2=2,(Q492/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I492,Refurb_Poss_Tbl[%]))*AG492,Q492*$AG492),0)","v":0},{"$f":"IF($AF492=3,IF($AF$2=2,(U492/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I492,Refurb_Poss_Tbl[%]))*AG492,U492*$AG492),0)","v":0},{"$f":"IF($AF492=3,IF($AF$2=2,(V492/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I492,Refurb_Poss_Tbl[%]))*AG492,IF($AF$2=3,(V492*AG492)-AW492,V492*AG492)),0)","v":0},{"$f":"IF($AF492=3,IF($AF$2=2,(W492/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I492,Refurb_Poss_Tbl[%]))*AG492,W492*$AG492),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,87,0,{"$f":"VLOOKUP(AE493,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11668733224058814},0,0,0,0,0,0,0,0,2.2342759037986094E-5,{"$f":"IF(OR(AF493=3,AF493=2,AF493=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D493,FlatMaint!$Y$2:$Y$10000,AE493)*AG493,0)","v":3.7735184747885578E-2},{"$f":"IF(OR(AF493=3,AF493=2,AF493=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D493,FlatRepair!$Y$2:$Y$10000,AE493)*AG493,0)","v":0},0,3.7757527506923565E-2,0,0,0,0,0,3.7757527506923565E-2,0,{"$f":"IF($AF493=3,IF($AF$2=2,(R493/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I493,Refurb_Poss_Tbl[%]))*AG493,IF($AF$2=3,(R493*AG493)-AV493,R493*AG493)),0)","v":0},{"$f":"IF(AF493=3,IF($AF$2=2,(S493/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I493,Refurb_Poss_Tbl[%]))*AG493,IF($AF$2=3,(S493*AG493)-AX493,S493*AG493)),0)","v":0},{"$f":"IF($AF493=3,IF($AF$2=2,(T493/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I493,Refurb_Poss_Tbl[%]))*AG493,T493*$AG493),0)","v":0},{"$f":"IF($AF493=3,IF($AF$2=2,(Q493/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I493,Refurb_Poss_Tbl[%]))*AG493,Q493*$AG493),0)","v":0},{"$f":"IF($AF493=3,IF($AF$2=2,(U493/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I493,Refurb_Poss_Tbl[%]))*AG493,U493*$AG493),0)","v":0},{"$f":"IF($AF493=3,IF($AF$2=2,(V493/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I493,Refurb_Poss_Tbl[%]))*AG493,IF($AF$2=3,(V493*AG493)-AW493,V493*AG493)),0)","v":0},{"$f":"IF($AF493=3,IF($AF$2=2,(W493/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I493,Refurb_Poss_Tbl[%]))*AG493,W493*$AG493),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,88,0,{"$f":"VLOOKUP(AE494,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11384129974691526},0,0,0,0,0,0,0,0,2.1797813695596188E-5,{"$f":"IF(OR(AF494=3,AF494=2,AF494=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D494,FlatMaint!$Y$2:$Y$10000,AE494)*AG494,0)","v":3.6814814388181051E-2},{"$f":"IF(OR(AF494=3,AF494=2,AF494=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D494,FlatRepair!$Y$2:$Y$10000,AE494)*AG494,0)","v":0},0,3.6836612201876645E-2,0,0,0,0,0,3.6836612201876645E-2,0,{"$f":"IF($AF494=3,IF($AF$2=2,(R494/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I494,Refurb_Poss_Tbl[%]))*AG494,IF($AF$2=3,(R494*AG494)-AV494,R494*AG494)),0)","v":0},{"$f":"IF(AF494=3,IF($AF$2=2,(S494/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I494,Refurb_Poss_Tbl[%]))*AG494,IF($AF$2=3,(S494*AG494)-AX494,S494*AG494)),0)","v":0},{"$f":"IF($AF494=3,IF($AF$2=2,(T494/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I494,Refurb_Poss_Tbl[%]))*AG494,T494*$AG494),0)","v":0},{"$f":"IF($AF494=3,IF($AF$2=2,(Q494/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I494,Refurb_Poss_Tbl[%]))*AG494,Q494*$AG494),0)","v":0},{"$f":"IF($AF494=3,IF($AF$2=2,(U494/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I494,Refurb_Poss_Tbl[%]))*AG494,U494*$AG494),0)","v":0},{"$f":"IF($AF494=3,IF($AF$2=2,(V494/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I494,Refurb_Poss_Tbl[%]))*AG494,IF($AF$2=3,(V494*AG494)-AW494,V494*AG494)),0)","v":0},{"$f":"IF($AF494=3,IF($AF$2=2,(W494/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I494,Refurb_Poss_Tbl[%]))*AG494,W494*$AG494),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,89,0,{"$f":"VLOOKUP(AE495,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.11106468267991736},0,0,0,0,0,0,0,0,2.1266159703020678E-5,{"$f":"IF(OR(AF495=3,AF495=2,AF495=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D495,FlatMaint!$Y$2:$Y$10000,AE495)*AG495,0)","v":3.5916892086030307E-2},{"$f":"IF(OR(AF495=3,AF495=2,AF495=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D495,FlatRepair!$Y$2:$Y$10000,AE495)*AG495,0)","v":0},0,3.5938158245733327E-2,0,0,0,0,0,3.5938158245733327E-2,0,{"$f":"IF($AF495=3,IF($AF$2=2,(R495/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I495,Refurb_Poss_Tbl[%]))*AG495,IF($AF$2=3,(R495*AG495)-AV495,R495*AG495)),0)","v":0},{"$f":"IF(AF495=3,IF($AF$2=2,(S495/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I495,Refurb_Poss_Tbl[%]))*AG495,IF($AF$2=3,(S495*AG495)-AX495,S495*AG495)),0)","v":0},{"$f":"IF($AF495=3,IF($AF$2=2,(T495/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I495,Refurb_Poss_Tbl[%]))*AG495,T495*$AG495),0)","v":0},{"$f":"IF($AF495=3,IF($AF$2=2,(Q495/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I495,Refurb_Poss_Tbl[%]))*AG495,Q495*$AG495),0)","v":0},{"$f":"IF($AF495=3,IF($AF$2=2,(U495/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I495,Refurb_Poss_Tbl[%]))*AG495,U495*$AG495),0)","v":0},{"$f":"IF($AF495=3,IF($AF$2=2,(V495/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I495,Refurb_Poss_Tbl[%]))*AG495,IF($AF$2=3,(V495*AG495)-AW495,V495*AG495)),0)","v":0},{"$f":"IF($AF495=3,IF($AF$2=2,(W495/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I495,Refurb_Poss_Tbl[%]))*AG495,W495*$AG495),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,90,0,{"$f":"VLOOKUP(AE496,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10835578798040717},0,0,0,0,0,0,0,0,2.0747472880995781E-5,{"$f":"IF(OR(AF496=3,AF496=2,AF496=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D496,FlatMaint!$Y$2:$Y$10000,AE496)*AG496,0)","v":3.5040870327834442E-2},{"$f":"IF(OR(AF496=3,AF496=2,AF496=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D496,FlatRepair!$Y$2:$Y$10000,AE496)*AG496,0)","v":0},0,3.5061617800715435E-2,0,0,0,0,0,3.5061617800715435E-2,0,{"$f":"IF($AF496=3,IF($AF$2=2,(R496/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I496,Refurb_Poss_Tbl[%]))*AG496,IF($AF$2=3,(R496*AG496)-AV496,R496*AG496)),0)","v":0},{"$f":"IF(AF496=3,IF($AF$2=2,(S496/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I496,Refurb_Poss_Tbl[%]))*AG496,IF($AF$2=3,(S496*AG496)-AX496,S496*AG496)),0)","v":0},{"$f":"IF($AF496=3,IF($AF$2=2,(T496/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I496,Refurb_Poss_Tbl[%]))*AG496,T496*$AG496),0)","v":0},{"$f":"IF($AF496=3,IF($AF$2=2,(Q496/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I496,Refurb_Poss_Tbl[%]))*AG496,Q496*$AG496),0)","v":0},{"$f":"IF($AF496=3,IF($AF$2=2,(U496/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I496,Refurb_Poss_Tbl[%]))*AG496,U496*$AG496),0)","v":0},{"$f":"IF($AF496=3,IF($AF$2=2,(V496/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I496,Refurb_Poss_Tbl[%]))*AG496,IF($AF$2=3,(V496*AG496)-AW496,V496*AG496)),0)","v":0},{"$f":"IF($AF496=3,IF($AF$2=2,(W496/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I496,Refurb_Poss_Tbl[%]))*AG496,W496*$AG496),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,91,0,{"$f":"VLOOKUP(AE497,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10571296388332406},0,0,0,0,0,0,0,0,2.0241436957069054E-5,{"$f":"IF(OR(AF497=3,AF497=2,AF497=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D497,FlatMaint!$Y$2:$Y$10000,AE497)*AG497,0)","v":3.4186214953984821E-2},{"$f":"IF(OR(AF497=3,AF497=2,AF497=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D497,FlatRepair!$Y$2:$Y$10000,AE497)*AG497,0)","v":0},0,3.4206456390941893E-2,0,0,0,0,0,3.4206456390941893E-2,0,{"$f":"IF($AF497=3,IF($AF$2=2,(R497/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I497,Refurb_Poss_Tbl[%]))*AG497,IF($AF$2=3,(R497*AG497)-AV497,R497*AG497)),0)","v":0},{"$f":"IF(AF497=3,IF($AF$2=2,(S497/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I497,Refurb_Poss_Tbl[%]))*AG497,IF($AF$2=3,(S497*AG497)-AX497,S497*AG497)),0)","v":0},{"$f":"IF($AF497=3,IF($AF$2=2,(T497/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I497,Refurb_Poss_Tbl[%]))*AG497,T497*$AG497),0)","v":0},{"$f":"IF($AF497=3,IF($AF$2=2,(Q497/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I497,Refurb_Poss_Tbl[%]))*AG497,Q497*$AG497),0)","v":0},{"$f":"IF($AF497=3,IF($AF$2=2,(U497/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I497,Refurb_Poss_Tbl[%]))*AG497,U497*$AG497),0)","v":0},{"$f":"IF($AF497=3,IF($AF$2=2,(V497/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I497,Refurb_Poss_Tbl[%]))*AG497,IF($AF$2=3,(V497*AG497)-AW497,V497*AG497)),0)","v":0},{"$f":"IF($AF497=3,IF($AF$2=2,(W497/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I497,Refurb_Poss_Tbl[%]))*AG497,W497*$AG497),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,92,0,{"$f":"VLOOKUP(AE498,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10313459891056008},0,0,0,0,0,0,0,0,1.9747743372750301E-5,{"$f":"IF(OR(AF498=3,AF498=2,AF498=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D498,FlatMaint!$Y$2:$Y$10000,AE498)*AG498,0)","v":3.3352404833155928E-2},{"$f":"IF(OR(AF498=3,AF498=2,AF498=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D498,FlatRepair!$Y$2:$Y$10000,AE498)*AG498,0)","v":0},0,3.3372152576528681E-2,0,0,0,0,0,3.3372152576528681E-2,0,{"$f":"IF($AF498=3,IF($AF$2=2,(R498/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I498,Refurb_Poss_Tbl[%]))*AG498,IF($AF$2=3,(R498*AG498)-AV498,R498*AG498)),0)","v":0},{"$f":"IF(AF498=3,IF($AF$2=2,(S498/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I498,Refurb_Poss_Tbl[%]))*AG498,IF($AF$2=3,(S498*AG498)-AX498,S498*AG498)),0)","v":0},{"$f":"IF($AF498=3,IF($AF$2=2,(T498/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I498,Refurb_Poss_Tbl[%]))*AG498,T498*$AG498),0)","v":0},{"$f":"IF($AF498=3,IF($AF$2=2,(Q498/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I498,Refurb_Poss_Tbl[%]))*AG498,Q498*$AG498),0)","v":0},{"$f":"IF($AF498=3,IF($AF$2=2,(U498/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I498,Refurb_Poss_Tbl[%]))*AG498,U498*$AG498),0)","v":0},{"$f":"IF($AF498=3,IF($AF$2=2,(V498/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I498,Refurb_Poss_Tbl[%]))*AG498,IF($AF$2=3,(V498*AG498)-AW498,V498*AG498)),0)","v":0},{"$f":"IF($AF498=3,IF($AF$2=2,(W498/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I498,Refurb_Poss_Tbl[%]))*AG498,W498*$AG498),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,93,0,{"$f":"VLOOKUP(AE499,ValidationLists!$M$1:$N$102,2,FALSE)","v":0.10061912088835129},0,0,0,0,0,0,0,0,1.9266091095366146E-5,{"$f":"IF(OR(AF499=3,AF499=2,AF499=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D499,FlatMaint!$Y$2:$Y$10000,AE499)*AG499,0)","v":3.2538931544542363E-2},{"$f":"IF(OR(AF499=3,AF499=2,AF499=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D499,FlatRepair!$Y$2:$Y$10000,AE499)*AG499,0)","v":0},0,3.2558197635637727E-2,0,0,0,0,0,3.2558197635637727E-2,0,{"$f":"IF($AF499=3,IF($AF$2=2,(R499/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I499,Refurb_Poss_Tbl[%]))*AG499,IF($AF$2=3,(R499*AG499)-AV499,R499*AG499)),0)","v":0},{"$f":"IF(AF499=3,IF($AF$2=2,(S499/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I499,Refurb_Poss_Tbl[%]))*AG499,IF($AF$2=3,(S499*AG499)-AX499,S499*AG499)),0)","v":0},{"$f":"IF($AF499=3,IF($AF$2=2,(T499/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I499,Refurb_Poss_Tbl[%]))*AG499,T499*$AG499),0)","v":0},{"$f":"IF($AF499=3,IF($AF$2=2,(Q499/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I499,Refurb_Poss_Tbl[%]))*AG499,Q499*$AG499),0)","v":0},{"$f":"IF($AF499=3,IF($AF$2=2,(U499/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I499,Refurb_Poss_Tbl[%]))*AG499,U499*$AG499),0)","v":0},{"$f":"IF($AF499=3,IF($AF$2=2,(V499/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I499,Refurb_Poss_Tbl[%]))*AG499,IF($AF$2=3,(V499*AG499)-AW499,V499*AG499)),0)","v":0},{"$f":"IF($AF499=3,IF($AF$2=2,(W499/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I499,Refurb_Poss_Tbl[%]))*AG499,W499*$AG499),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,94,0,{"$f":"VLOOKUP(AE500,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.8164995988635415E-2},0,0,0,0,0,0,0,0,1.8796186434503558E-5,{"$f":"IF(OR(AF500=3,AF500=2,AF500=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D500,FlatMaint!$Y$2:$Y$10000,AE500)*AG500,0)","v":3.1745299067846212E-2},{"$f":"IF(OR(AF500=3,AF500=2,AF500=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D500,FlatRepair!$Y$2:$Y$10000,AE500)*AG500,0)","v":0},0,3.1764095254280714E-2,0,0,0,0,0,3.1764095254280714E-2,0,{"$f":"IF($AF500=3,IF($AF$2=2,(R500/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I500,Refurb_Poss_Tbl[%]))*AG500,IF($AF$2=3,(R500*AG500)-AV500,R500*AG500)),0)","v":0},{"$f":"IF(AF500=3,IF($AF$2=2,(S500/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I500,Refurb_Poss_Tbl[%]))*AG500,IF($AF$2=3,(S500*AG500)-AX500,S500*AG500)),0)","v":0},{"$f":"IF($AF500=3,IF($AF$2=2,(T500/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I500,Refurb_Poss_Tbl[%]))*AG500,T500*$AG500),0)","v":0},{"$f":"IF($AF500=3,IF($AF$2=2,(Q500/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I500,Refurb_Poss_Tbl[%]))*AG500,Q500*$AG500),0)","v":0},{"$f":"IF($AF500=3,IF($AF$2=2,(U500/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I500,Refurb_Poss_Tbl[%]))*AG500,U500*$AG500),0)","v":0},{"$f":"IF($AF500=3,IF($AF$2=2,(V500/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I500,Refurb_Poss_Tbl[%]))*AG500,IF($AF$2=3,(V500*AG500)-AW500,V500*AG500)),0)","v":0},{"$f":"IF($AF500=3,IF($AF$2=2,(W500/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I500,Refurb_Poss_Tbl[%]))*AG500,W500*$AG500),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,95,0,{"$f":"VLOOKUP(AE501,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.577072779379063E-2},0,0,0,0,0,0,0,0,1.8337742862930296E-5,{"$f":"IF(OR(AF501=3,AF501=2,AF501=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D501,FlatMaint!$Y$2:$Y$10000,AE501)*AG501,0)","v":3.0971023480825567E-2},{"$f":"IF(OR(AF501=3,AF501=2,AF501=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D501,FlatRepair!$Y$2:$Y$10000,AE501)*AG501,0)","v":0},0,3.0989361223688498E-2,0,0,0,0,0,3.0989361223688498E-2,0,{"$f":"IF($AF501=3,IF($AF$2=2,(R501/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I501,Refurb_Poss_Tbl[%]))*AG501,IF($AF$2=3,(R501*AG501)-AV501,R501*AG501)),0)","v":0},{"$f":"IF(AF501=3,IF($AF$2=2,(S501/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I501,Refurb_Poss_Tbl[%]))*AG501,IF($AF$2=3,(S501*AG501)-AX501,S501*AG501)),0)","v":0},{"$f":"IF($AF501=3,IF($AF$2=2,(T501/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I501,Refurb_Poss_Tbl[%]))*AG501,T501*$AG501),0)","v":0},{"$f":"IF($AF501=3,IF($AF$2=2,(Q501/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I501,Refurb_Poss_Tbl[%]))*AG501,Q501*$AG501),0)","v":0},{"$f":"IF($AF501=3,IF($AF$2=2,(U501/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I501,Refurb_Poss_Tbl[%]))*AG501,U501*$AG501),0)","v":0},{"$f":"IF($AF501=3,IF($AF$2=2,(V501/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I501,Refurb_Poss_Tbl[%]))*AG501,IF($AF$2=3,(V501*AG501)-AW501,V501*AG501)),0)","v":0},{"$f":"IF($AF501=3,IF($AF$2=2,(W501/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I501,Refurb_Poss_Tbl[%]))*AG501,W501*$AG501),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,96,0,{"$f":"VLOOKUP(AE502,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.3434856384185999E-2},0,0,0,0,0,0,0,0,1.789048084188322E-5,{"$f":"IF(OR(AF502=3,AF502=2,AF502=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D502,FlatMaint!$Y$2:$Y$10000,AE502)*AG502,0)","v":3.0215632664220074E-2},{"$f":"IF(OR(AF502=3,AF502=2,AF502=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D502,FlatRepair!$Y$2:$Y$10000,AE502)*AG502,0)","v":0},0,3.0233523145061957E-2,0,0,0,0,0,3.0233523145061957E-2,0,{"$f":"IF($AF502=3,IF($AF$2=2,(R502/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I502,Refurb_Poss_Tbl[%]))*AG502,IF($AF$2=3,(R502*AG502)-AV502,R502*AG502)),0)","v":0},{"$f":"IF(AF502=3,IF($AF$2=2,(S502/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I502,Refurb_Poss_Tbl[%]))*AG502,IF($AF$2=3,(S502*AG502)-AX502,S502*AG502)),0)","v":0},{"$f":"IF($AF502=3,IF($AF$2=2,(T502/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I502,Refurb_Poss_Tbl[%]))*AG502,T502*$AG502),0)","v":0},{"$f":"IF($AF502=3,IF($AF$2=2,(Q502/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I502,Refurb_Poss_Tbl[%]))*AG502,Q502*$AG502),0)","v":0},{"$f":"IF($AF502=3,IF($AF$2=2,(U502/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I502,Refurb_Poss_Tbl[%]))*AG502,U502*$AG502),0)","v":0},{"$f":"IF($AF502=3,IF($AF$2=2,(V502/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I502,Refurb_Poss_Tbl[%]))*AG502,IF($AF$2=3,(V502*AG502)-AW502,V502*AG502)),0)","v":0},{"$f":"IF($AF502=3,IF($AF$2=2,(W502/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I502,Refurb_Poss_Tbl[%]))*AG502,W502*$AG502),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,97,0,{"$f":"VLOOKUP(AE503,ValidationLists!$M$1:$N$102,2,FALSE)","v":9.1155957447986352E-2},0,0,0,0,0,0,0,0,1.7454127650617777E-5,{"$f":"IF(OR(AF503=3,AF503=2,AF503=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D503,FlatMaint!$Y$2:$Y$10000,AE503)*AG503,0)","v":2.9478666013873243E-2},{"$f":"IF(OR(AF503=3,AF503=2,AF503=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D503,FlatRepair!$Y$2:$Y$10000,AE503)*AG503,0)","v":0},0,2.9496120141523863E-2,0,0,0,0,0,2.9496120141523863E-2,0,{"$f":"IF($AF503=3,IF($AF$2=2,(R503/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I503,Refurb_Poss_Tbl[%]))*AG503,IF($AF$2=3,(R503*AG503)-AV503,R503*AG503)),0)","v":0},{"$f":"IF(AF503=3,IF($AF$2=2,(S503/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I503,Refurb_Poss_Tbl[%]))*AG503,IF($AF$2=3,(S503*AG503)-AX503,S503*AG503)),0)","v":0},{"$f":"IF($AF503=3,IF($AF$2=2,(T503/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I503,Refurb_Poss_Tbl[%]))*AG503,T503*$AG503),0)","v":0},{"$f":"IF($AF503=3,IF($AF$2=2,(Q503/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I503,Refurb_Poss_Tbl[%]))*AG503,Q503*$AG503),0)","v":0},{"$f":"IF($AF503=3,IF($AF$2=2,(U503/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I503,Refurb_Poss_Tbl[%]))*AG503,U503*$AG503),0)","v":0},{"$f":"IF($AF503=3,IF($AF$2=2,(V503/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I503,Refurb_Poss_Tbl[%]))*AG503,IF($AF$2=3,(V503*AG503)-AW503,V503*AG503)),0)","v":0},{"$f":"IF($AF503=3,IF($AF$2=2,(W503/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I503,Refurb_Poss_Tbl[%]))*AG503,W503*$AG503),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,98,0,{"$f":"VLOOKUP(AE504,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.8932641412669614E-2},0,0,0,0,0,0,0,0,1.7028417220114906E-5,{"$f":"IF(OR(AF504=3,AF504=2,AF504=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D504,FlatMaint!$Y$2:$Y$10000,AE504)*AG504,0)","v":2.8759674159876337E-2},{"$f":"IF(OR(AF504=3,AF504=2,AF504=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D504,FlatRepair!$Y$2:$Y$10000,AE504)*AG504,0)","v":0},0,2.8776702577096452E-2,0,0,0,0,0,2.8776702577096452E-2,0,{"$f":"IF($AF504=3,IF($AF$2=2,(R504/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I504,Refurb_Poss_Tbl[%]))*AG504,IF($AF$2=3,(R504*AG504)-AV504,R504*AG504)),0)","v":0},{"$f":"IF(AF504=3,IF($AF$2=2,(S504/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I504,Refurb_Poss_Tbl[%]))*AG504,IF($AF$2=3,(S504*AG504)-AX504,S504*AG504)),0)","v":0},{"$f":"IF($AF504=3,IF($AF$2=2,(T504/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I504,Refurb_Poss_Tbl[%]))*AG504,T504*$AG504),0)","v":0},{"$f":"IF($AF504=3,IF($AF$2=2,(Q504/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I504,Refurb_Poss_Tbl[%]))*AG504,Q504*$AG504),0)","v":0},{"$f":"IF($AF504=3,IF($AF$2=2,(U504/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I504,Refurb_Poss_Tbl[%]))*AG504,U504*$AG504),0)","v":0},{"$f":"IF($AF504=3,IF($AF$2=2,(V504/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I504,Refurb_Poss_Tbl[%]))*AG504,IF($AF$2=3,(V504*AG504)-AW504,V504*AG504)),0)","v":0},{"$f":"IF($AF504=3,IF($AF$2=2,(W504/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I504,Refurb_Poss_Tbl[%]))*AG504,W504*$AG504),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,99,0,{"$f":"VLOOKUP(AE505,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.6763552597726459E-2},0,0,0,0,0,0,0,0,1.6613089970843813E-5,{"$f":"IF(OR(AF505=3,AF505=2,AF505=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D505,FlatMaint!$Y$2:$Y$10000,AE505)*AG505,0)","v":2.8058218692562281E-2},{"$f":"IF(OR(AF505=3,AF505=2,AF505=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D505,FlatRepair!$Y$2:$Y$10000,AE505)*AG505,0)","v":0},0,2.8074831782533127E-2,0,0,0,0,0,2.8074831782533127E-2,0,{"$f":"IF($AF505=3,IF($AF$2=2,(R505/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I505,Refurb_Poss_Tbl[%]))*AG505,IF($AF$2=3,(R505*AG505)-AV505,R505*AG505)),0)","v":0},{"$f":"IF(AF505=3,IF($AF$2=2,(S505/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I505,Refurb_Poss_Tbl[%]))*AG505,IF($AF$2=3,(S505*AG505)-AX505,S505*AG505)),0)","v":0},{"$f":"IF($AF505=3,IF($AF$2=2,(T505/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I505,Refurb_Poss_Tbl[%]))*AG505,T505*$AG505),0)","v":0},{"$f":"IF($AF505=3,IF($AF$2=2,(Q505/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I505,Refurb_Poss_Tbl[%]))*AG505,Q505*$AG505),0)","v":0},{"$f":"IF($AF505=3,IF($AF$2=2,(U505/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I505,Refurb_Poss_Tbl[%]))*AG505,U505*$AG505),0)","v":0},{"$f":"IF($AF505=3,IF($AF$2=2,(V505/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I505,Refurb_Poss_Tbl[%]))*AG505,IF($AF$2=3,(V505*AG505)-AW505,V505*AG505)),0)","v":0},{"$f":"IF($AF505=3,IF($AF$2=2,(W505/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I505,Refurb_Poss_Tbl[%]))*AG505,W505*$AG505),0)","v":0}]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993299E-2,4.5141975521151197E-4,1.9222031466382E-2,0,0,3.21316705704659,1.9147544646851101E-4,0,0.32131670570465898,0,2.2570987760575599E-4,8.54807576249666E-3,100,0,{"$f":"VLOOKUP(AE506,ValidationLists!$M$1:$N$102,2,FALSE)","v":8.4647368388025807E-2},0,0,0,0,0,0,0,0,1.6207892654481768E-5,{"$f":"IF(OR(AF506=3,AF506=2,AF506=0),SUMIFS(FlatMaint!$Z$2:$Z$10000,FlatMaint!$A$2:$A$10000,D506,FlatMaint!$Y$2:$Y$10000,AE506)*AG506,0)","v":2.7373871895182714E-2},{"$f":"IF(OR(AF506=3,AF506=2,AF506=0),SUMIFS(FlatRepair!$Z$2:$Z$10000,FlatRepair!$A$2:$A$10000,D506,FlatRepair!$Y$2:$Y$10000,AE506)*AG506,0)","v":0},0,2.7390079787837196E-2,0,0,0,0,0,2.7390079787837196E-2,0,{"$f":"IF($AF506=3,IF($AF$2=2,(R506/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I506,Refurb_Poss_Tbl[%]))*AG506,IF($AF$2=3,(R506*AG506)-AV506,R506*AG506)),0)","v":0},{"$f":"IF(AF506=3,IF($AF$2=2,(S506/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I506,Refurb_Poss_Tbl[%]))*AG506,IF($AF$2=3,(S506*AG506)-AX506,S506*AG506)),0)","v":0},{"$f":"IF($AF506=3,IF($AF$2=2,(T506/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I506,Refurb_Poss_Tbl[%]))*AG506,T506*$AG506),0)","v":0},{"$f":"IF($AF506=3,IF($AF$2=2,(Q506/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I506,Refurb_Poss_Tbl[%]))*AG506,Q506*$AG506),0)","v":0},{"$f":"IF($AF506=3,IF($AF$2=2,(U506/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I506,Refurb_Poss_Tbl[%]))*AG506,U506*$AG506),0)","v":0},{"$f":"IF($AF506=3,IF($AF$2=2,(V506/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I506,Refurb_Poss_Tbl[%]))*AG506,IF($AF$2=3,(V506*AG506)-AW506,V506*AG506)),0)","v":0},{"$f":"IF($AF506=3,IF($AF$2=2,(W506/SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],I506,Refurb_Poss_Tbl[%]))*AG506,W506*$AG506),0)","v":0}]

{"sheet":"AssetDataExtract","index":3,"n_rows":6,"n_cols":131,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["Asset ID","Asset description","Asset class","Sub-Asset ref.","Sub-Asset description","Sub-Asset category","Standard life","Expected new build life","Refurbishment type","Expected refurbished Life","First intervention","Last Refurb","Last Replace","Remaining Life","Last intervention","Weighted Split","Materials","Materials Transport","People Transport","Plant Transport","Site Establishment","Plant use","Waste","New Build Co2e","Use","Energy","Refurbishment","Den - Material Waste","Dem - Plant use","Dem - People","0","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24","25","26","27","28","29","30","31","32","33","34","35","36","37","38","39","40","41","42","43","44","45","46","47","48","49","50","51","52","53","54","55","56","57","58","59","60","61","62","63","64","65","66","67","68","69","70","71","72","73","74","75","76","77","78","79","80","81","82","83","84","85","86","87","88","89","90","91","92","93","94","95","96","97","98","99","100"]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0333","Desk","Bridges",60,20,"Moderate Refurbishment",10,"New Build",113,123,100,3,883.50839999999994,883.50839999999994,1.0741763547000001,4.9024970723805268,0.1294492520789727,5.5121149839704069,0,0.12063990849013125,895.24727757161986,5.490755123293739E-2,0,223.81181939290497,2.2921582613124936,6.4724626039486352E-2,2.4512485361902634,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2,0,0,0,0,0,0,0,0,0,3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2,0,0,0,0,0,0,0,0,0,3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2,0,0,0,0,0,0,0,0,0,3,0,0,0,0,0,0,0,0,0,0]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0334","Abutment","Headwall",80,60,"Moderate Refurbishment",40,"New Build",93,133,100,3,27.229103999999996,27.229103999999996,0.22829150779999999,0.15109149233164604,3.989534392180724E-3,0.16987948519616625,0,7.3895334888847489E-2,27.856251354608833,1.6922118939751794E-3,0,6.9640628386522083,0.41874023103680236,1.994767196090362E-3,7.5545746165823019E-2,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,3]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0335","Handrail","Barriers",60,40,"Minor Refurbishment",20,"New Build",133,93,100,2,885.6,885.6,0.28638398574999996,4.914103145256111,0.1297557076323646,5.525164254017497,0,3.1002867585E-2,896.48640996024108,5.5037538264366651E-2,0,89.648640996024113,0.58905448411499983,6.4877853816182302E-2,2.4570515726280555,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0336","Concrete wingwall","Headwall",80,80,"Moderate Refurbishment",50,"New Build",113,0,100,2,9.9959999999999987,9.9959999999999987,9.8487154300000004E-2,5.5466773983717341E-2,1.4645867812704565E-3,6.2363981349547078E-2,0,2.7127509136874998E-2,10.24091000555141,6.2122316225226844E-4,0,2.5602275013878524,0.15372255177562497,7.3229339063522823E-4,2.773338699185867E-2,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BridEA03","Footbridge","Bridge - Pedestrian","BridEA0337","Erosion protection","Erosion Protection",60,60,"Minor Refurbishment",50,"New Build",93,0,100,2,3.081,3.081,9.5397454300000004E-2,1.7096151524993313E-2,4.5141975521151235E-4,1.922203146638201E-2,0,0,3.2131670570465869,1.9147544646851134E-4,0,0.3213167057046587,0,2.2570987760575618E-4,8.5480757624966566E-3,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"FlatMaint","index":4,"n_rows":809,"n_cols":26,"rows_kept":809,"cut":false,"hidden":true,"merged":[]}
["Sub-Asset Ref.","Sub-Asset description","Maintenance category","Maintenance description","Mode of transport","Return transport distance (km)","Materials","Plant","Waste","Overhead","Annual intervention fequency","Interventions per year","Exceptional intervention year","CO2e (t) per intervention","Material"," Plant","Transport","blank5","blank6","blank7","blank8","blank9","blank10","blank11","Year","Maint"]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",0]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",1,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",2,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",3,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",4,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",5,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",6,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",7,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",8,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",9,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",10,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",11,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",12,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",13,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",14,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",15,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",16,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",17,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",18,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",19,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",20,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",21,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",22,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",23,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",24,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",25,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",26,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",27,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",28,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",29,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",30,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",31,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",32,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",33,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",34,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",35,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",36,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",37,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",38,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",39,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",40,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",41,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",42,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",43,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",44,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",45,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",46,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",47,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",48,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",49,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",50,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",51,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",52,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",53,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",54,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",55,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",56,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",57,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",58,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",59,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",60,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",61,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",62,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",63,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",64,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",65,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",66,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",67,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",68,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",69,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",70,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",71,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",72,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",73,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",74,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",75,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",76,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",77,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",78,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",79,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",80,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",81,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",82,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",83,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",84,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",85,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",86,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",87,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",88,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",89,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",90,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",91,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",92,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",93,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",94,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",95,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",96,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",97,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",98,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",99,88.366127158000012]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.366127158","88.35084","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",100,88.366127158000012]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",0]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",1,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",2,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",3,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",4,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",5,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",6,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",7,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",8,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",9,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",10,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",11,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",12,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",13,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",14,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",15,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",16,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",17,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",18,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",19,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",20,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",21,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",22,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",23,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",24,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",25,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",26,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",27,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",28,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",29,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",30,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",31,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",32,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",33,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",34,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",35,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",36,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",37,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",38,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",39,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",40,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",41,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",42,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",43,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",44,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",45,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",46,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",47,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",48,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",49,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",50,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",51,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",52,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",53,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",54,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",55,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",56,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",57,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",58,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",59,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",60,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",61,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",62,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",63,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",64,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",65,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",66,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",67,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",68,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",69,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",70,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",71,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",72,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",73,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",74,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",75,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",76,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",77,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",78,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",79,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",80,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",81,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",82,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",83,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",84,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",85,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",86,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",87,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",88,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",89,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",90,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",91,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",92,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",93,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",94,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",95,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",96,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",97,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",98,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",99,27.244391157999996]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","27.244391158","27.229104","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",100,27.244391157999996]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",0]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",1,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",2,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",3,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",4,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",5,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",6,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",7,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",8,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",9,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",10,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",11,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",12,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",13,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",14,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",15,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",16,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",17,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",18,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",19,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",20,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",21,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",22,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",23,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",24,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",25,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",26,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",27,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",28,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",29,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",30,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",31,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",32,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",33,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",34,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",35,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",36,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",37,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",38,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",39,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",40,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",41,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",42,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",43,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",44,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",45,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",46,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",47,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",48,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",49,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",50,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",51,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",52,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",53,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",54,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",55,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",56,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",57,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",58,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",59,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",60,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",61,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",62,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",63,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",64,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",65,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",66,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",67,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",68,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",69,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",70,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",71,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",72,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",73,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",74,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",75,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",76,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",77,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",78,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",79,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",80,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",81,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",82,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",83,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",84,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",85,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",86,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",87,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",88,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",89,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",90,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",91,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",92,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",93,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",94,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",95,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",96,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",97,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",98,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",99,88.575287158000009]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",100,88.575287158000009]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",0]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",1,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",2,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",3,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",4,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",5,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",6,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",7,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",8,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",9,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",10,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",11,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",12,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",13,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",14,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",15,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",16,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",17,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",18,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",19,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",20,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",21,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",22,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",23,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",24,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",25,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",26,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",27,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",28,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",29,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",30,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",31,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",32,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",33,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",34,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",35,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",36,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",37,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",38,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",39,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",40,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",41,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",42,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",43,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",44,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",45,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",46,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",47,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",48,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",49,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",50,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",51,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",52,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",53,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",54,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",55,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",56,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",57,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",58,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",59,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",60,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",61,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",62,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",63,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",64,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",65,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",66,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",67,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",68,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",69,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",70,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",71,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",72,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",73,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",74,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",75,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",76,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",77,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",78,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",79,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",80,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",81,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",82,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",83,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",84,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",85,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",86,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",87,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",88,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",89,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",90,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",91,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",92,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",93,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",94,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",95,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",96,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",97,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",98,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",99,10.011287157999998]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van","50","Medium","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","10.011287158","9.996","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",100,10.011287157999998]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",1,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",2,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",3,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",4,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",5,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",6,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",7,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",8,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",9,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",10,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",11,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",12,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",13,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",14,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",15,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",16,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",17,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",18,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",19,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",20,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",21,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",22,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",23,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",24,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",25,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",26,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",27,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",28,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",29,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",30,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",31,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",32,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",33,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",34,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",35,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",36,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",37,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",38,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",39,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",40,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",41,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",42,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",43,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",44,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",45,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",46,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",47,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",48,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",49,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",50,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",51,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",52,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",53,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",54,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",55,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",56,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",57,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",58,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",59,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",60,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",61,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",62,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",63,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",64,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",65,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",66,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",67,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",68,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",69,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",70,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",71,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",72,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",73,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",74,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",75,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",76,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",77,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",78,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",79,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",80,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",81,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",82,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",83,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",84,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",85,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",86,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",87,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",88,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",89,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",90,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",91,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",92,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",93,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",94,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",95,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",96,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",97,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",98,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",99,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0.323387158","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",100,0.32338715800000006]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",1,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",2,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",3,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",4,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",5,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",6,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",7,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",8,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",9,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",10,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",11,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",12,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",13,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",14,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",15,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",16,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",17,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",18,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",19,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",20,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",21,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",22,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",23,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",24,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",25,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",26,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",27,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",28,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",29,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",30,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",31,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",32,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",33,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",34,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",35,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",36,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",37,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",38,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",39,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",40,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",41,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",42,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",43,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",44,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",45,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",46,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",47,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",48,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",49,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",50,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",51,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",52,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",53,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",54,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",55,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",56,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",57,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",58,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",59,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",60,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",61,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",62,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",63,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",64,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",65,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",66,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",67,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",68,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",69,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",70,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",71,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",72,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",73,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",74,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",75,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",76,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",77,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",78,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",79,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",80,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",81,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",82,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",83,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",84,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",85,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",86,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",87,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",88,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",89,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",90,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",91,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",92,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",93,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",94,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",95,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",96,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",97,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",98,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",99,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",100,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",1,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",2,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",3,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",4,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",5,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",6,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",7,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",8,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",9,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",10,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",11,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",12,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",13,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",14,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",15,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",16,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",17,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",18,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",19,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",20,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",21,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",22,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",23,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",24,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",25,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",26,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",27,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",28,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",29,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",30,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",31,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",32,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",33,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",34,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",35,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",36,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",37,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",38,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",39,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",40,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",41,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",42,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",43,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",44,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",45,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",46,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",47,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",48,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",49,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",50,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",51,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",52,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",53,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",54,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",55,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",56,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",57,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",58,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",59,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",60,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",61,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",62,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",63,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",64,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",65,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",66,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",67,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",68,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",69,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",70,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",71,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",72,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",73,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",74,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",75,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",76,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",77,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",78,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",79,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",80,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",81,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",82,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",83,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",84,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",85,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",86,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",87,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",88,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",89,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",90,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",91,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",92,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",93,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",94,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",95,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",96,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",97,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",98,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",99,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","0","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",100,0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",0]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",1]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",2]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",3]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",4]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",5]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",6]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",7]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",8]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",9]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",10]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",11]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",12]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",13]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",14]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",15]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",16]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",17]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",18]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",19]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",20]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",21]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",22]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",23]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",24]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",25]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",26]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",27]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",28]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",29]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",30]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",31]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",32]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",33]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",34]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",35]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",36]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",37]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",38]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",39]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",40]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",41]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",42]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",43]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",44]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",45]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",46]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",47]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",48]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",49]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",50]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",51]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",52]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",53]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",54]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",55]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",56]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",57]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",58]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",59]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",60]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",61]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",62]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",63]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",64]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",65]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",66]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",67]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",68]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",69]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",70]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",71]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",72]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",73]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",74]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",75]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",76]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",77]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",78]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",79]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",80]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",81]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",82]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",83]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",84]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",85]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",86]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",87]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",88]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",89]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",90]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",91]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",92]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",93]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",94]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",95]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",96]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",97]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",98]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",99]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van","50","Low","Low","Not used","Not used","Every year","Interventions per year","Exceptional intervention year","214.52047979","0.3081","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank10","blank11",100]

{"sheet":"FlatRepair","index":5,"n_rows":506,"n_cols":26,"rows_kept":506,"cut":false,"hidden":true,"merged":[]}
["Sub-Asset Ref.","Sub-Asset description","Repair category","Repair description","Mode of transport","Return transport distance (km)","Materials","Plant","Waste","Overhead","Annual intervention fequency","Interventions per year","Exceptional intervention year","CO2e (t) per intervention","Material"," Plant","Transport","blank5","blank6","blank7","blank8","blank9","blank92","blank10","Year","Repair"]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",1,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",2,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",3,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",4,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",5,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",6,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",7,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",8,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",9,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",10,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",11,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",12,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",13,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",14,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",15,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",16,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",17,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",18,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",19,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",20,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",21,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",22,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",23,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",24,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",25,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",26,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",27,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",28,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",29,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",30,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",31,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",32,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",33,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",34,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",35,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",36,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",37,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",38,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",39,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",40,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",41,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",42,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",43,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",44,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",45,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",46,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",47,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",48,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",49,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",50,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",51,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",52,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",53,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",54,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",55,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",56,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",57,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",58,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",59,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",60,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",61,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",62,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",63,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",64,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",65,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",66,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",67,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",68,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",69,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",70,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",71,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",72,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",73,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",74,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",75,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",76,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",77,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",78,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",79,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",80,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",81,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",82,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",83,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",84,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",85,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",86,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",87,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",88,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",89,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",90,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",91,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",92,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",93,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",94,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",95,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",96,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",97,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",98,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",99,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",100,88.575287158000009]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",1,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",2,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",3,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",4,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",5,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",6,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",7,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",8,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",9,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",10,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",11,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",12,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",13,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",14,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",15,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",16,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",17,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",18,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",19,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",20,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",21,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",22,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",23,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",24,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",25,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",26,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",27,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",28,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",29,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",30,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",31,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",32,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",33,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",34,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",35,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",36,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",37,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",38,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",39,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",40,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",41,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",42,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",43,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",44,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",45,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",46,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",47,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",48,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",49,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",50,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",51,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",52,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",53,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",54,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",55,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",56,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",57,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",58,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",59,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",60,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",61,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",62,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",63,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",64,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",65,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",66,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",67,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",68,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",69,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",70,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",71,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",72,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",73,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",74,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",75,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",76,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",77,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",78,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",79,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",80,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",81,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",82,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",83,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",84,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",85,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",86,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",87,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",88,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",89,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",90,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",91,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",92,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",93,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",94,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",95,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",96,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",97,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",98,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",99,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",100,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",1,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",2,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",3,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",4,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",5,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",6,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",7,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",8,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",9,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",10,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",11,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",12,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",13,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",14,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",15,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",16,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",17,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",18,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",19,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",20,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",21,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",22,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",23,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",24,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",25,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",26,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",27,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",28,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",29,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",30,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",31,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",32,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",33,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",34,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",35,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",36,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",37,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",38,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",39,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",40,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",41,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",42,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",43,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",44,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",45,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",46,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",47,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",48,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",49,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",50,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",51,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",52,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",53,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",54,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",55,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",56,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",57,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",58,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",59,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",60,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",61,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",62,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",63,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",64,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",65,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",66,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",67,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",68,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",69,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",70,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",71,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",72,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",73,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",74,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",75,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",76,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",77,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",78,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",79,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",80,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",81,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",82,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",83,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",84,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",85,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",86,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",87,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",88,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",89,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",90,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",91,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",92,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",93,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",94,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",95,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",96,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",97,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",98,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",99,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",100,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",1,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",2,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",3,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",4,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",5,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",6,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",7,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",8,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",9,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",10,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",11,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",12,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",13,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",14,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",15,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",16,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",17,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",18,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",19,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",20,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",21,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",22,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",23,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",24,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",25,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",26,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",27,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",28,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",29,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",30,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",31,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",32,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",33,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",34,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",35,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",36,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",37,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",38,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",39,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",40,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",41,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",42,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",43,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",44,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",45,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",46,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",47,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",48,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",49,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",50,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",51,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",52,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",53,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",54,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",55,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",56,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",57,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",58,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",59,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",60,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",61,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",62,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",63,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",64,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",65,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",66,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",67,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",68,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",69,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",70,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",71,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",72,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",73,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",74,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",75,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",76,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",77,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",78,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",79,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",80,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",81,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",82,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",83,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",84,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",85,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",86,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",87,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",88,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",89,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",90,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",91,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",92,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",93,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",94,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",95,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",96,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",97,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",98,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",99,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","0","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",100,0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",0]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",1]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",2]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",3]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",4]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",5]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",6]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",7]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",8]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",9]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",10]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",11]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",12]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",13]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",14]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",15]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",16]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",17]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",18]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",19]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",20]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",21]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",22]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",23]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",24]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",25]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",26]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",27]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",28]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",29]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",30]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",31]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",32]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",33]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",34]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",35]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",36]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",37]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",38]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",39]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",40]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",41]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",42]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",43]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",44]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",45]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",46]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",47]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",48]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",49]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",50]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",51]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",52]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",53]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",54]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",55]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",56]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",57]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",58]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",59]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",60]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",61]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",62]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",63]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",64]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",65]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",66]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",67]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",68]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",69]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",70]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",71]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",72]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",73]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",74]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",75]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",76]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",77]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",78]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",79]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",80]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",81]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",82]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",83]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",84]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",85]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",86]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",87]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",88]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",89]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",90]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",91]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",92]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",93]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",94]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",95]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",96]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",97]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",98]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",99]
["BridEA0335","Handrail","Not used","Damaged","Van","50","Low","Low","Not used","Not used","Every 2 years","Interventions per year","Exceptional intervention year","88.575287158","88.56","0","0.015287158","blank5","blank6","blank7","blank8","blank9","blank92","blank10",100]

{"sheet":"RepairData","index":6,"n_rows":6,"n_cols":125,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["Sub-Asset Ref.","Sub-Asset description","Repair category","Repair description","Mode of transport","Return transport distance (km)","Materials","Plant","Waste","Overhead","Annual intervention fequency","Interventions per year","Exceptional intervention year","CO2e (t) per intervention","Material"," Plant","Transport","blank5","blank6","blank7","blank8","blank9","blank92","blank10","0","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24","25","26","27","28","29","30","31","32","33","34","35","36","37","38","39","40","41","42","43","44","45","46","47","48","49","50","51","52","53","54","55","56","57","58","59","60","61","62","63","64","65","66","67","68","69","70","71","72","73","74","75","76","77","78","79","80","81","82","83","84","85","86","87","88","89","90","91","92","93","94","95","96","97","98","99","100"]
["BridEA0335","Handrail","Not used","Damaged","Van",50,"Low","Low","Not used","Not used","Every 2 years",null,null,88.575287158000009,88.56,0,1.5287157999999999E-2,null,null,null,null,null,null,null,null,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009,0,88.575287158000009]
["",null,"Not used",null,null,null,null,null,"Not used","Not used",null,null,null,0,"","","",null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["",null,"Not used",null,null,null,null,null,"Not used","Not used",null,null,null,0,"","","",null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["",null,"Not used",null,null,null,null,null,"Not used","Not used",null,null,null,0,"","","",null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,88.575287158000009]

{"sheet":"MaintData","index":7,"n_rows":9,"n_cols":125,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
["Sub-Asset Ref.","Sub-Asset description","Maintenance category","Maintenance description","Mode of transport","Return transport distance (km)","Materials","Plant","Waste","Overhead","Annual intervention fequency","Interventions per year","Exceptional intervention year","CO2e (t) per intervention","Material"," Plant","Transport","blank5","blank6","blank7","blank8","blank9","blank10","blank11","0","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24","25","26","27","28","29","30","31","32","33","34","35","36","37","38","39","40","41","42","43","44","45","46","47","48","49","50","51","52","53","54","55","56","57","58","59","60","61","62","63","64","65","66","67","68","69","70","71","72","73","74","75","76","77","78","79","80","81","82","83","84","85","86","87","88","89","90","91","92","93","94","95","96","97","98","99","100"]
["BridEA0333","Desk","Minimum Need","Safety Inspection","Van",50,"Low","Low","Not used","Not used","Every year",null,null,88.366127158000012,88.350840000000005,0,1.5287157999999999E-2,null,null,null,null,null,null,null,null,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012,88.366127158000012]
["BridEA0334","Abutment","Minimum Need","Special inspection","Van",50,"Medium","Low","Not used","Not used","Every year",null,null,27.244391157999996,27.229103999999996,0,1.5287157999999999E-2,null,null,null,null,null,null,null,null,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996,27.244391157999996]
["BridEA0335","Handrail","Minimum Need","Visual inspection","Van",50,"Low","Low","Not used","Not used","Every year",null,null,88.575287158000009,88.56,0,1.5287157999999999E-2,null,null,null,null,null,null,null,null,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009,88.575287158000009]
["BridEA0336","Concrete wingwall","Identified Need","Special inspection","Van",50,"Medium","Low","Not used","Not used","Every year",null,null,10.011287157999998,9.9959999999999987,0,1.5287157999999999E-2,null,null,null,null,null,null,null,null,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998,10.011287157999998]
["BridEA0337","Erosion protection","Identified Need","Vegetation maintenance","Van",50,"Low","Low","Not used","Not used","Every year",null,null,0.32338715800000006,0.30810000000000004,0,1.5287157999999999E-2,null,null,null,null,null,null,null,null,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006,0.32338715800000006]
["",null,null,null,null,null,null,null,"Not used","Not used",null,null,null,0,"","","",null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["",null,null,null,null,null,null,null,"Not used","Not used",null,null,null,0,"","","",null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,214.52047979]

{"sheet":"Calculator","index":8,"n_rows":202,"n_cols":133,"rows_kept":202,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[null,null,"Project details"]
[]
[null,null,"Date produced","Version","Produced by","Reviewed by","SOP","Project name","EA project manager"]
[null,null,42583,1,"VHJ",null,"IMSE50017","Oxford FAS","Heather Taylor"]
[]
[null,null," Total project cost","Total construction cost","Total salaries cost","Total consultant cost","Construction start date","Construction finish date","Gateway","Project Location"]
[null,null,600000,500000,20000,80000,42979,43101,"G1","West Midlands"]
[]
[]
[]
[null,null,"Assets"]
[]
[]
[null,null,"Asset ID","Asset class","Asset description","Asset measure","Asset unit","Asset value","1B1S Project ref.","Version","Gateway","Capital - Materials","Capital - Transport","Capital - Installation","Operational - Use","Operational - Maintenance","Operational -Repair","Operational - Energy","Replacement - Materials","Replacement - Transport","Replacement - Installation","Refurbishment","Demolition","Residual","Whole Life Carbon","Capital - New Build","Capital - Replacement","Capital -Refurbishment","Capital - Demolition","Lifecycle - Operational","Lifecycle - Replacement","Lifecycle - Refurbishment","Lifecycle - Demolition","General Item Material","General Item Material Transport","General Item Material Waste","General Item Plant use","Plant Transport","Non contractor People Transport","Contractor people transport","Site establishment","Plant use","Other Construction Waste","Use","Dem - General Item Waste"]
[null,null,{"$f":"IFERROR(IF(Form_Elements[[#This Row],[Asset class]]=\"\",\"\",INDEX(Assets[Element Id],MATCH(Form_Elements[[#This Row],[Asset class]],Assets[Element Description],0))),\"\")","v":"BridEA03"},"Bridge - Pedestrian","Footbridge",120,{"$f":"IF(Form_Elements[Asset class]=\"\",\"\",INDEX(Assets[Element Unit],MATCH(Form_Elements[Asset class],Assets[Element Description],0)))","v":"m2"},630000,{"$f":"IF(Form_Elements[[#This Row],[Asset ID]]=\"\",\"\",Form_Mod_1[SOP])","v":"IMSE50017"},{"$f":"Form_Mod_1[Version]","v":1},{"$f":"Form_Mod_2[Gateway]","v":"G1"},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AH$1:$AH$4800)","v":1809.4145040000001},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AI$1:$AI$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AJ$1:$AJ$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AK$1:$AK$4800)","v":12.088101592966996},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AL$1:$AL$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AM$1:$AM$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AN$1:$AN$4800)","v":11.541410356100858},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AP$1:$AP$4800)","v":3.5292202163767392},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AQ$1:$AQ$4800)","v":6732.681317044955},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AR$1:$AR$4800)","v":1369.8678143119284},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AS$1:$AS$4800)","v":0},{"$f":"SUMIFS(FlatData!$BE$1:$BE$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":713.0893246782565},{"$f":"SUMIFS(FlatData!$BB$1:$BB$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BD$1:$BD$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BC$1:$BC$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":4.8106945515317321},{"$f":"SUMIFS(FlatData!$BF$1:$BF$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BG$1:$BG$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BH$1:$BH$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":4.5369357596703406},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AU$1:$AU$4800)","v":231.23957849294123},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AV$1:$AV$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AW$1:$AW$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AX$1:$AX$4800)","v":3.6201670655063309},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$BA$1:$BA$4800)","v":-464.42856693723741},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AZ$1:$AZ$4800)","v":10431.990501132987},null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth (wtt)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[[Waste Co2e ]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",0,SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],\"GenEA1\",Form_Const_Ins_InsB[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",Form_TranPlantSum[Transport of plant]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),Form_Const_Tran_Plant[[#Totals],[CO2e (t)]]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0.26511050064000002},{"$f":"IFERROR(SUM(Form_Const_Tran_LabourA64[[EA staff]:[Consultants]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":1.2410040754769953},{"$f":"IFERROR(IF($D$62=\"Summary\",SUM(Form_Const_Tran_LabourA64[[Labour]:[Management staff]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),SUM(Form_Const_Tran_LabourB.1[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":8.7992505599999991},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_OnsiteA[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),(SUM(Form_Const_Ins_OnsiteB[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":11.288744736},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_InsA69[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Ins_ConsWaste[CO2e (t)])*Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_use[Asset Ref.],Form_Elements[[#This Row],[Asset ID]],Form_use_use[CO2e (t)]),0)","v":0.11245000000000001},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Dem -Waste Co2e])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Elements[[#This Row],[Asset class]]=\"\",\"\",INDEX(Assets[Element Id],MATCH(Form_Elements[[#This Row],[Asset class]],Assets[Element Description],0))),\"\")","v":""},null,null,null,{"$f":"IF(Form_Elements[Asset class]=\"\",\"\",INDEX(Assets[Element Unit],MATCH(Form_Elements[Asset class],Assets[Element Description],0)))","v":""},null,{"$f":"IF(Form_Elements[[#This Row],[Asset ID]]=\"\",\"\",Form_Mod_1[SOP])","v":""},{"$f":"Form_Mod_1[Version]","v":1},{"$f":"Form_Mod_2[Gateway]","v":"G1"},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AH$1:$AH$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AI$1:$AI$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AJ$1:$AJ$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AK$1:$AK$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AL$1:$AL$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AM$1:$AM$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AN$1:$AN$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AP$1:$AP$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AQ$1:$AQ$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AR$1:$AR$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AS$1:$AS$4800)","v":0},{"$f":"SUMIFS(FlatData!$BE$1:$BE$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BB$1:$BB$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BD$1:$BD$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BC$1:$BC$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BF$1:$BF$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BG$1:$BG$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BH$1:$BH$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AU$1:$AU$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AV$1:$AV$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AW$1:$AW$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AX$1:$AX$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$BA$1:$BA$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AZ$1:$AZ$4800)","v":0},null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth (wtt)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[[Waste Co2e ]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",0,SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],\"GenEA1\",Form_Const_Ins_InsB[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",Form_TranPlantSum[Transport of plant]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),Form_Const_Tran_Plant[[#Totals],[CO2e (t)]]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Tran_LabourA64[[EA staff]:[Consultants]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",SUM(Form_Const_Tran_LabourA64[[Labour]:[Management staff]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),SUM(Form_Const_Tran_LabourB.1[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_OnsiteA[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),(SUM(Form_Const_Ins_OnsiteB[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_InsA69[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Ins_ConsWaste[CO2e (t)])*Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_use[Asset Ref.],Form_Elements[[#This Row],[Asset ID]],Form_use_use[CO2e (t)]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Dem -Waste Co2e])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Elements[[#This Row],[Asset class]]=\"\",\"\",INDEX(Assets[Element Id],MATCH(Form_Elements[[#This Row],[Asset class]],Assets[Element Description],0))),\"\")","v":""},null,null,null,{"$f":"IF(Form_Elements[Asset class]=\"\",\"\",INDEX(Assets[Element Unit],MATCH(Form_Elements[Asset class],Assets[Element Description],0)))","v":""},null,{"$f":"IF(Form_Elements[[#This Row],[Asset ID]]=\"\",\"\",Form_Mod_1[SOP])","v":""},{"$f":"Form_Mod_1[Version]","v":1},{"$f":"Form_Mod_2[Gateway]","v":"G1"},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AH$1:$AH$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AI$1:$AI$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AJ$1:$AJ$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AK$1:$AK$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AL$1:$AL$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AM$1:$AM$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AN$1:$AN$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AP$1:$AP$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AQ$1:$AQ$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AR$1:$AR$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AS$1:$AS$4800)","v":0},{"$f":"SUMIFS(FlatData!$BE$1:$BE$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BB$1:$BB$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BD$1:$BD$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BC$1:$BC$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BF$1:$BF$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BG$1:$BG$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BH$1:$BH$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AU$1:$AU$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AV$1:$AV$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AW$1:$AW$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AX$1:$AX$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$BA$1:$BA$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AZ$1:$AZ$4800)","v":0},null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth (wtt)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[[Waste Co2e ]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",0,SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],\"GenEA1\",Form_Const_Ins_InsB[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",Form_TranPlantSum[Transport of plant]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),Form_Const_Tran_Plant[[#Totals],[CO2e (t)]]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Tran_LabourA64[[EA staff]:[Consultants]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",SUM(Form_Const_Tran_LabourA64[[Labour]:[Management staff]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),SUM(Form_Const_Tran_LabourB.1[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_OnsiteA[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),(SUM(Form_Const_Ins_OnsiteB[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_InsA69[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Ins_ConsWaste[CO2e (t)])*Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_use[Asset Ref.],Form_Elements[[#This Row],[Asset ID]],Form_use_use[CO2e (t)]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Dem -Waste Co2e])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Elements[[#This Row],[Asset class]]=\"\",\"\",INDEX(Assets[Element Id],MATCH(Form_Elements[[#This Row],[Asset class]],Assets[Element Description],0))),\"\")","v":""},null,null,null,{"$f":"IF(Form_Elements[Asset class]=\"\",\"\",INDEX(Assets[Element Unit],MATCH(Form_Elements[Asset class],Assets[Element Description],0)))","v":""},null,{"$f":"IF(Form_Elements[[#This Row],[Asset ID]]=\"\",\"\",Form_Mod_1[SOP])","v":""},{"$f":"Form_Mod_1[Version]","v":1},{"$f":"Form_Mod_2[Gateway]","v":"G1"},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AH$1:$AH$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AI$1:$AI$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AJ$1:$AJ$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AK$1:$AK$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AL$1:$AL$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AM$1:$AM$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AN$1:$AN$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AP$1:$AP$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AQ$1:$AQ$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AR$1:$AR$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AS$1:$AS$4800)","v":0},{"$f":"SUMIFS(FlatData!$BE$1:$BE$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BB$1:$BB$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BD$1:$BD$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BC$1:$BC$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BF$1:$BF$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BG$1:$BG$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BH$1:$BH$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AU$1:$AU$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AV$1:$AV$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AW$1:$AW$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AX$1:$AX$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$BA$1:$BA$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AZ$1:$AZ$4800)","v":0},null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth (wtt)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[[Waste Co2e ]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",0,SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],\"GenEA1\",Form_Const_Ins_InsB[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",Form_TranPlantSum[Transport of plant]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),Form_Const_Tran_Plant[[#Totals],[CO2e (t)]]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Tran_LabourA64[[EA staff]:[Consultants]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",SUM(Form_Const_Tran_LabourA64[[Labour]:[Management staff]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),SUM(Form_Const_Tran_LabourB.1[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_OnsiteA[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),(SUM(Form_Const_Ins_OnsiteB[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_InsA69[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Ins_ConsWaste[CO2e (t)])*Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_use[Asset Ref.],Form_Elements[[#This Row],[Asset ID]],Form_use_use[CO2e (t)]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Dem -Waste Co2e])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Elements[[#This Row],[Asset class]]=\"\",\"\",INDEX(Assets[Element Id],MATCH(Form_Elements[[#This Row],[Asset class]],Assets[Element Description],0))),\"\")","v":""},null,null,null,{"$f":"IF(Form_Elements[Asset class]=\"\",\"\",INDEX(Assets[Element Unit],MATCH(Form_Elements[Asset class],Assets[Element Description],0)))","v":""},null,{"$f":"IF(Form_Elements[[#This Row],[Asset ID]]=\"\",\"\",Form_Mod_1[SOP])","v":""},{"$f":"Form_Mod_1[Version]","v":1},{"$f":"Form_Mod_2[Gateway]","v":"G1"},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AH$1:$AH$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AI$1:$AI$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AJ$1:$AJ$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AK$1:$AK$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AL$1:$AL$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AM$1:$AM$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AN$1:$AN$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AP$1:$AP$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AQ$1:$AQ$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AR$1:$AR$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AS$1:$AS$4800)","v":0},{"$f":"SUMIFS(FlatData!$BE$1:$BE$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BB$1:$BB$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BD$1:$BD$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BC$1:$BC$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BF$1:$BF$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BG$1:$BG$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BH$1:$BH$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AU$1:$AU$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AV$1:$AV$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AW$1:$AW$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AX$1:$AX$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$BA$1:$BA$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AZ$1:$AZ$4800)","v":0},null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth (wtt)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[[Waste Co2e ]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",0,SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],\"GenEA1\",Form_Const_Ins_InsB[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",Form_TranPlantSum[Transport of plant]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),Form_Const_Tran_Plant[[#Totals],[CO2e (t)]]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Tran_LabourA64[[EA staff]:[Consultants]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",SUM(Form_Const_Tran_LabourA64[[Labour]:[Management staff]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),SUM(Form_Const_Tran_LabourB.1[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_OnsiteA[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),(SUM(Form_Const_Ins_OnsiteB[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_InsA69[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Ins_ConsWaste[CO2e (t)])*Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_use[Asset Ref.],Form_Elements[[#This Row],[Asset ID]],Form_use_use[CO2e (t)]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Dem -Waste Co2e])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Elements[[#This Row],[Asset class]]=\"\",\"\",INDEX(Assets[Element Id],MATCH(Form_Elements[[#This Row],[Asset class]],Assets[Element Description],0))),\"\")","v":""},null,null,null,{"$f":"IF(Form_Elements[Asset class]=\"\",\"\",INDEX(Assets[Element Unit],MATCH(Form_Elements[Asset class],Assets[Element Description],0)))","v":""},null,{"$f":"IF(Form_Elements[[#This Row],[Asset ID]]=\"\",\"\",Form_Mod_1[SOP])","v":""},{"$f":"Form_Mod_1[Version]","v":1},{"$f":"Form_Mod_2[Gateway]","v":"G1"},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AH$1:$AH$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AI$1:$AI$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AJ$1:$AJ$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AK$1:$AK$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AL$1:$AL$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AM$1:$AM$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AN$1:$AN$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AP$1:$AP$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AQ$1:$AQ$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AR$1:$AR$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AS$1:$AS$4800)","v":0},{"$f":"SUMIFS(FlatData!$BE$1:$BE$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BB$1:$BB$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BD$1:$BD$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BC$1:$BC$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIFS(FlatData!$BF$1:$BF$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BG$1:$BG$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)+SUMIFS(FlatData!$BH$1:$BH$4800,FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AF$1:$AF$4800,3)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AU$1:$AU$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AV$1:$AV$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AW$1:$AW$4800)+SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AX$1:$AX$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$BA$1:$BA$4800)","v":0},{"$f":"SUMIF(FlatData!$A$1:$A$4800,Form_Elements[[#This Row],[Asset ID]],FlatData!$AZ$1:$AZ$4800)","v":0},null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Total Oth (wtt)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[[Waste Co2e ]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",0,SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],\"GenEA1\",Form_Const_Ins_InsB[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",Form_TranPlantSum[Transport of plant]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),Form_Const_Tran_Plant[[#Totals],[CO2e (t)]]*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Tran_LabourA64[[EA staff]:[Consultants]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0},{"$f":"IFERROR(IF($D$62=\"Summary\",SUM(Form_Const_Tran_LabourA64[[Labour]:[Management staff]])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),SUM(Form_Const_Tran_LabourB.1[CO2e (t)])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_OnsiteA[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),(SUM(Form_Const_Ins_OnsiteB[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",(SUM(Form_Const_Ins_InsA69[CO2e (t)]))*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0),0)","v":0},{"$f":"IFERROR(SUM(Form_Const_Ins_ConsWaste[CO2e (t)])*Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_use[Asset Ref.],Form_Elements[[#This Row],[Asset ID]],Form_use_use[CO2e (t)]),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Product_Stage[Sub-Asset ref.],\"GenEA1\",Form_Product_Stage[Dem -Waste Co2e])*(Form_Elements[[#This Row],[Asset value]]/SUM(Form_Elements[Asset value])),0)","v":0}]
[]
[]
[null,null,"Sub-Assets"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a"]
[]
[null,null,"Asset ID","Asset description","Asset class","Sub-Asset ref.","Sub-Asset description","Sub-Asset category","Standard life","Expected new build life","Refurbishment type","Expected refurbished Life","First intervention","Last Refurb","Last Replace","Remaining Life","Last intervention","Weighted Split","Materials","Materials Transport","People Transport","Plant Transport","Site Establishment","Plant use","Waste","New Build Co2e","Use","Energy","Refurbishment","Den - Material Waste","Dem - Plant use","Dem - People","0","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24","25","26","27","28","29","30","31","32","33","34","35","36","37","38","39","40","41","42","43","44","45","46","47","48","49","50","51","52","53","54","55","56","57","58","59","60","61","62","63","64","65","66","67","68","69","70","71","72","73","74","75","76","77","78","79","80","81","82","83","84","85","86","87","88","89","90","91","92","93","94","95","96","97","98","99","100"]
[null,null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"BridEA03"},"Footbridge",{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset class],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"Bridge - Pedestrian"},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",Form_Asset[[#This Row],[Asset ID]]&ROW())","v":"BridEA0333"},"Desk","Bridges",{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",INDEX(AssetListTbl[Best Estimate Life (5)],(MATCH(Form_Asset[[#This Row],[Sub-Asset category]],AssetListTbl[Sub-Element Category],0))))","v":60},20,"Moderate Refurbishment",10,"New Build",{"$f":"MAX(COLUMN($AH33:EC33)*($AH33:EC33=2))","v":113},{"$f":"MAX(COLUMN($AH33:EC33)*($AH33:EC33=3))","v":123},{"$f":"IFERROR(100-(IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Replace]])),INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Refurb]])))),0)","v":100},{"$f":"IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],3,2)","v":3},{"$f":"SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Product_Stage[CO2e (t)])","v":883.50839999999994},{"$f":"IFERROR(SUM(Form_Elements[General Item Material])*(Form_Asset[[#This Row],[Weighted Split]]/SUM(Form_Asset[Weighted Split]))+Form_Asset[[#This Row],[Weighted Split]],0)","v":883.50839999999994},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth (wtt)]))+(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Transport]))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":1.0741763547000001},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Non contractor People Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Contractor people transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":4.9024970723805268},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0.1294492520789727},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Site establishment])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":5.5121149839704069},{"$f":"IFERROR(IF($D$88=\"Summary\",((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),(SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Const_Ins_InsB[CO2e (t)]))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Other Construction Waste])*Form_Asset[[#This Row],[Weighted Split]]/(SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[[Waste Co2e ]])+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0.12063990849013125},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New build\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]]),IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",(SUM(Form_Asset[[#This Row],[Materials]:[Waste]])-(SUM(Form_Asset[[#This Row],[Materials Transport]],Form_Asset[[#This Row],[People Transport]]*0.5,Form_Asset[[#This Row],[Plant Transport]]*0.5))),IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]])/(SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%])),0)))","v":895.24727757161986},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":5.490755123293739E-2},{"$f":"IFERROR(SUMIF(Form_use_energy[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_use_energy[CO2e (t)]),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset ref.]]=\"\",0,SUMIF(Form_Asset[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Asset[New Build Co2e])*SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%]))","v":223.81181939290497},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Dem - General Item Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Dem -Waste Co2e]),0)","v":2.2921582613124936},{"$f":"(Form_Asset[[#This Row],[Plant use]]+Form_Asset[[#This Row],[Plant Transport]])*50%","v":6.4724626039486352E-2},{"$f":"Form_Asset[[#This Row],[People Transport]]*50%","v":2.4512485361902634},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New Build\",1,IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",2,IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",3,IF(Form_Asset[[#This Row],[First intervention]]=\"Demolition\",4,\"\"))))","v":1},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AG33)*($AG33:AG33=1))>MAX(COLUMN($AG33:AG33)*($AG33:AG33=3)),MAX(COLUMN($AG33:AG33)*($AG33:AG33=1))>MAX(COLUMN($AG33:AG33)*($AG33:AG33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AH33)-MAX(COLUMN($AG33:AG33)*($AG33:AG33=1))=$J33,3,0),IF(COLUMN(AH33)-MAX(COLUMN($AG33:AG33)*($AG33:AG33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AG33)*($AG33:AG33=2))>MAX(COLUMN($AG33:AG33)*($AG33:AG33=3)),MAX(COLUMN($AG33:AG33)*($AG33:AG33=2))>MAX(COLUMN($AG33:AG33)*($AG33:AG33=1))),IF(COLUMN(AH33)-MAX(COLUMN($AG33:AG33)*($AG33:AG33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AH33)-MAX(COLUMN($AG33:AG33)*($AG33:AG33=3))=$J33,3,0),IF(COLUMN(AH33)-MAX(COLUMN($AG33:AG33)*($AG33:AG33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AH33)*($AG33:AH33=1))>MAX(COLUMN($AG33:AH33)*($AG33:AH33=3)),MAX(COLUMN($AG33:AH33)*($AG33:AH33=1))>MAX(COLUMN($AG33:AH33)*($AG33:AH33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AI33)-MAX(COLUMN($AG33:AH33)*($AG33:AH33=1))=$J33,3,0),IF(COLUMN(AI33)-MAX(COLUMN($AG33:AH33)*($AG33:AH33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AH33)*($AG33:AH33=2))>MAX(COLUMN($AG33:AH33)*($AG33:AH33=3)),MAX(COLUMN($AG33:AH33)*($AG33:AH33=2))>MAX(COLUMN($AG33:AH33)*($AG33:AH33=1))),IF(COLUMN(AI33)-MAX(COLUMN($AG33:AH33)*($AG33:AH33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AI33)-MAX(COLUMN($AG33:AH33)*($AG33:AH33=3))=$J33,3,0),IF(COLUMN(AI33)-MAX(COLUMN($AG33:AH33)*($AG33:AH33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AI33)*($AG33:AI33=1))>MAX(COLUMN($AG33:AI33)*($AG33:AI33=3)),MAX(COLUMN($AG33:AI33)*($AG33:AI33=1))>MAX(COLUMN($AG33:AI33)*($AG33:AI33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AJ33)-MAX(COLUMN($AG33:AI33)*($AG33:AI33=1))=$J33,3,0),IF(COLUMN(AJ33)-MAX(COLUMN($AG33:AI33)*($AG33:AI33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AI33)*($AG33:AI33=2))>MAX(COLUMN($AG33:AI33)*($AG33:AI33=3)),MAX(COLUMN($AG33:AI33)*($AG33:AI33=2))>MAX(COLUMN($AG33:AI33)*($AG33:AI33=1))),IF(COLUMN(AJ33)-MAX(COLUMN($AG33:AI33)*($AG33:AI33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AJ33)-MAX(COLUMN($AG33:AI33)*($AG33:AI33=3))=$J33,3,0),IF(COLUMN(AJ33)-MAX(COLUMN($AG33:AI33)*($AG33:AI33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=1))>MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=3)),MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=1))>MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AK33)-MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=1))=$J33,3,0),IF(COLUMN(AK33)-MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=2))>MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=3)),MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=2))>MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=1))),IF(COLUMN(AK33)-MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AK33)-MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=3))=$J33,3,0),IF(COLUMN(AK33)-MAX(COLUMN($AG33:AJ33)*($AG33:AJ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AK33)*($AG33:AK33=1))>MAX(COLUMN($AG33:AK33)*($AG33:AK33=3)),MAX(COLUMN($AG33:AK33)*($AG33:AK33=1))>MAX(COLUMN($AG33:AK33)*($AG33:AK33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AL33)-MAX(COLUMN($AG33:AK33)*($AG33:AK33=1))=$J33,3,0),IF(COLUMN(AL33)-MAX(COLUMN($AG33:AK33)*($AG33:AK33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AK33)*($AG33:AK33=2))>MAX(COLUMN($AG33:AK33)*($AG33:AK33=3)),MAX(COLUMN($AG33:AK33)*($AG33:AK33=2))>MAX(COLUMN($AG33:AK33)*($AG33:AK33=1))),IF(COLUMN(AL33)-MAX(COLUMN($AG33:AK33)*($AG33:AK33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AL33)-MAX(COLUMN($AG33:AK33)*($AG33:AK33=3))=$J33,3,0),IF(COLUMN(AL33)-MAX(COLUMN($AG33:AK33)*($AG33:AK33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AL33)*($AG33:AL33=1))>MAX(COLUMN($AG33:AL33)*($AG33:AL33=3)),MAX(COLUMN($AG33:AL33)*($AG33:AL33=1))>MAX(COLUMN($AG33:AL33)*($AG33:AL33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AM33)-MAX(COLUMN($AG33:AL33)*($AG33:AL33=1))=$J33,3,0),IF(COLUMN(AM33)-MAX(COLUMN($AG33:AL33)*($AG33:AL33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AL33)*($AG33:AL33=2))>MAX(COLUMN($AG33:AL33)*($AG33:AL33=3)),MAX(COLUMN($AG33:AL33)*($AG33:AL33=2))>MAX(COLUMN($AG33:AL33)*($AG33:AL33=1))),IF(COLUMN(AM33)-MAX(COLUMN($AG33:AL33)*($AG33:AL33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AM33)-MAX(COLUMN($AG33:AL33)*($AG33:AL33=3))=$J33,3,0),IF(COLUMN(AM33)-MAX(COLUMN($AG33:AL33)*($AG33:AL33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AM33)*($AG33:AM33=1))>MAX(COLUMN($AG33:AM33)*($AG33:AM33=3)),MAX(COLUMN($AG33:AM33)*($AG33:AM33=1))>MAX(COLUMN($AG33:AM33)*($AG33:AM33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AN33)-MAX(COLUMN($AG33:AM33)*($AG33:AM33=1))=$J33,3,0),IF(COLUMN(AN33)-MAX(COLUMN($AG33:AM33)*($AG33:AM33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AM33)*($AG33:AM33=2))>MAX(COLUMN($AG33:AM33)*($AG33:AM33=3)),MAX(COLUMN($AG33:AM33)*($AG33:AM33=2))>MAX(COLUMN($AG33:AM33)*($AG33:AM33=1))),IF(COLUMN(AN33)-MAX(COLUMN($AG33:AM33)*($AG33:AM33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AN33)-MAX(COLUMN($AG33:AM33)*($AG33:AM33=3))=$J33,3,0),IF(COLUMN(AN33)-MAX(COLUMN($AG33:AM33)*($AG33:AM33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AN33)*($AG33:AN33=1))>MAX(COLUMN($AG33:AN33)*($AG33:AN33=3)),MAX(COLUMN($AG33:AN33)*($AG33:AN33=1))>MAX(COLUMN($AG33:AN33)*($AG33:AN33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AO33)-MAX(COLUMN($AG33:AN33)*($AG33:AN33=1))=$J33,3,0),IF(COLUMN(AO33)-MAX(COLUMN($AG33:AN33)*($AG33:AN33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AN33)*($AG33:AN33=2))>MAX(COLUMN($AG33:AN33)*($AG33:AN33=3)),MAX(COLUMN($AG33:AN33)*($AG33:AN33=2))>MAX(COLUMN($AG33:AN33)*($AG33:AN33=1))),IF(COLUMN(AO33)-MAX(COLUMN($AG33:AN33)*($AG33:AN33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AO33)-MAX(COLUMN($AG33:AN33)*($AG33:AN33=3))=$J33,3,0),IF(COLUMN(AO33)-MAX(COLUMN($AG33:AN33)*($AG33:AN33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AO33)*($AG33:AO33=1))>MAX(COLUMN($AG33:AO33)*($AG33:AO33=3)),MAX(COLUMN($AG33:AO33)*($AG33:AO33=1))>MAX(COLUMN($AG33:AO33)*($AG33:AO33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AP33)-MAX(COLUMN($AG33:AO33)*($AG33:AO33=1))=$J33,3,0),IF(COLUMN(AP33)-MAX(COLUMN($AG33:AO33)*($AG33:AO33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AO33)*($AG33:AO33=2))>MAX(COLUMN($AG33:AO33)*($AG33:AO33=3)),MAX(COLUMN($AG33:AO33)*($AG33:AO33=2))>MAX(COLUMN($AG33:AO33)*($AG33:AO33=1))),IF(COLUMN(AP33)-MAX(COLUMN($AG33:AO33)*($AG33:AO33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AP33)-MAX(COLUMN($AG33:AO33)*($AG33:AO33=3))=$J33,3,0),IF(COLUMN(AP33)-MAX(COLUMN($AG33:AO33)*($AG33:AO33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AP33)*($AG33:AP33=1))>MAX(COLUMN($AG33:AP33)*($AG33:AP33=3)),MAX(COLUMN($AG33:AP33)*($AG33:AP33=1))>MAX(COLUMN($AG33:AP33)*($AG33:AP33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AQ33)-MAX(COLUMN($AG33:AP33)*($AG33:AP33=1))=$J33,3,0),IF(COLUMN(AQ33)-MAX(COLUMN($AG33:AP33)*($AG33:AP33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AP33)*($AG33:AP33=2))>MAX(COLUMN($AG33:AP33)*($AG33:AP33=3)),MAX(COLUMN($AG33:AP33)*($AG33:AP33=2))>MAX(COLUMN($AG33:AP33)*($AG33:AP33=1))),IF(COLUMN(AQ33)-MAX(COLUMN($AG33:AP33)*($AG33:AP33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AQ33)-MAX(COLUMN($AG33:AP33)*($AG33:AP33=3))=$J33,3,0),IF(COLUMN(AQ33)-MAX(COLUMN($AG33:AP33)*($AG33:AP33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=1))>MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=3)),MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=1))>MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AR33)-MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=1))=$J33,3,0),IF(COLUMN(AR33)-MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=2))>MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=3)),MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=2))>MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=1))),IF(COLUMN(AR33)-MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AR33)-MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=3))=$J33,3,0),IF(COLUMN(AR33)-MAX(COLUMN($AG33:AQ33)*($AG33:AQ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AR33)*($AG33:AR33=1))>MAX(COLUMN($AG33:AR33)*($AG33:AR33=3)),MAX(COLUMN($AG33:AR33)*($AG33:AR33=1))>MAX(COLUMN($AG33:AR33)*($AG33:AR33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AS33)-MAX(COLUMN($AG33:AR33)*($AG33:AR33=1))=$J33,3,0),IF(COLUMN(AS33)-MAX(COLUMN($AG33:AR33)*($AG33:AR33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AR33)*($AG33:AR33=2))>MAX(COLUMN($AG33:AR33)*($AG33:AR33=3)),MAX(COLUMN($AG33:AR33)*($AG33:AR33=2))>MAX(COLUMN($AG33:AR33)*($AG33:AR33=1))),IF(COLUMN(AS33)-MAX(COLUMN($AG33:AR33)*($AG33:AR33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AS33)-MAX(COLUMN($AG33:AR33)*($AG33:AR33=3))=$J33,3,0),IF(COLUMN(AS33)-MAX(COLUMN($AG33:AR33)*($AG33:AR33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AS33)*($AG33:AS33=1))>MAX(COLUMN($AG33:AS33)*($AG33:AS33=3)),MAX(COLUMN($AG33:AS33)*($AG33:AS33=1))>MAX(COLUMN($AG33:AS33)*($AG33:AS33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AT33)-MAX(COLUMN($AG33:AS33)*($AG33:AS33=1))=$J33,3,0),IF(COLUMN(AT33)-MAX(COLUMN($AG33:AS33)*($AG33:AS33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AS33)*($AG33:AS33=2))>MAX(COLUMN($AG33:AS33)*($AG33:AS33=3)),MAX(COLUMN($AG33:AS33)*($AG33:AS33=2))>MAX(COLUMN($AG33:AS33)*($AG33:AS33=1))),IF(COLUMN(AT33)-MAX(COLUMN($AG33:AS33)*($AG33:AS33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AT33)-MAX(COLUMN($AG33:AS33)*($AG33:AS33=3))=$J33,3,0),IF(COLUMN(AT33)-MAX(COLUMN($AG33:AS33)*($AG33:AS33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AT33)*($AG33:AT33=1))>MAX(COLUMN($AG33:AT33)*($AG33:AT33=3)),MAX(COLUMN($AG33:AT33)*($AG33:AT33=1))>MAX(COLUMN($AG33:AT33)*($AG33:AT33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AU33)-MAX(COLUMN($AG33:AT33)*($AG33:AT33=1))=$J33,3,0),IF(COLUMN(AU33)-MAX(COLUMN($AG33:AT33)*($AG33:AT33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AT33)*($AG33:AT33=2))>MAX(COLUMN($AG33:AT33)*($AG33:AT33=3)),MAX(COLUMN($AG33:AT33)*($AG33:AT33=2))>MAX(COLUMN($AG33:AT33)*($AG33:AT33=1))),IF(COLUMN(AU33)-MAX(COLUMN($AG33:AT33)*($AG33:AT33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AU33)-MAX(COLUMN($AG33:AT33)*($AG33:AT33=3))=$J33,3,0),IF(COLUMN(AU33)-MAX(COLUMN($AG33:AT33)*($AG33:AT33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AU33)*($AG33:AU33=1))>MAX(COLUMN($AG33:AU33)*($AG33:AU33=3)),MAX(COLUMN($AG33:AU33)*($AG33:AU33=1))>MAX(COLUMN($AG33:AU33)*($AG33:AU33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AV33)-MAX(COLUMN($AG33:AU33)*($AG33:AU33=1))=$J33,3,0),IF(COLUMN(AV33)-MAX(COLUMN($AG33:AU33)*($AG33:AU33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AU33)*($AG33:AU33=2))>MAX(COLUMN($AG33:AU33)*($AG33:AU33=3)),MAX(COLUMN($AG33:AU33)*($AG33:AU33=2))>MAX(COLUMN($AG33:AU33)*($AG33:AU33=1))),IF(COLUMN(AV33)-MAX(COLUMN($AG33:AU33)*($AG33:AU33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AV33)-MAX(COLUMN($AG33:AU33)*($AG33:AU33=3))=$J33,3,0),IF(COLUMN(AV33)-MAX(COLUMN($AG33:AU33)*($AG33:AU33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AV33)*($AG33:AV33=1))>MAX(COLUMN($AG33:AV33)*($AG33:AV33=3)),MAX(COLUMN($AG33:AV33)*($AG33:AV33=1))>MAX(COLUMN($AG33:AV33)*($AG33:AV33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AW33)-MAX(COLUMN($AG33:AV33)*($AG33:AV33=1))=$J33,3,0),IF(COLUMN(AW33)-MAX(COLUMN($AG33:AV33)*($AG33:AV33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AV33)*($AG33:AV33=2))>MAX(COLUMN($AG33:AV33)*($AG33:AV33=3)),MAX(COLUMN($AG33:AV33)*($AG33:AV33=2))>MAX(COLUMN($AG33:AV33)*($AG33:AV33=1))),IF(COLUMN(AW33)-MAX(COLUMN($AG33:AV33)*($AG33:AV33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AW33)-MAX(COLUMN($AG33:AV33)*($AG33:AV33=3))=$J33,3,0),IF(COLUMN(AW33)-MAX(COLUMN($AG33:AV33)*($AG33:AV33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AW33)*($AG33:AW33=1))>MAX(COLUMN($AG33:AW33)*($AG33:AW33=3)),MAX(COLUMN($AG33:AW33)*($AG33:AW33=1))>MAX(COLUMN($AG33:AW33)*($AG33:AW33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AX33)-MAX(COLUMN($AG33:AW33)*($AG33:AW33=1))=$J33,3,0),IF(COLUMN(AX33)-MAX(COLUMN($AG33:AW33)*($AG33:AW33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AW33)*($AG33:AW33=2))>MAX(COLUMN($AG33:AW33)*($AG33:AW33=3)),MAX(COLUMN($AG33:AW33)*($AG33:AW33=2))>MAX(COLUMN($AG33:AW33)*($AG33:AW33=1))),IF(COLUMN(AX33)-MAX(COLUMN($AG33:AW33)*($AG33:AW33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AX33)-MAX(COLUMN($AG33:AW33)*($AG33:AW33=3))=$J33,3,0),IF(COLUMN(AX33)-MAX(COLUMN($AG33:AW33)*($AG33:AW33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AX33)*($AG33:AX33=1))>MAX(COLUMN($AG33:AX33)*($AG33:AX33=3)),MAX(COLUMN($AG33:AX33)*($AG33:AX33=1))>MAX(COLUMN($AG33:AX33)*($AG33:AX33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AY33)-MAX(COLUMN($AG33:AX33)*($AG33:AX33=1))=$J33,3,0),IF(COLUMN(AY33)-MAX(COLUMN($AG33:AX33)*($AG33:AX33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AX33)*($AG33:AX33=2))>MAX(COLUMN($AG33:AX33)*($AG33:AX33=3)),MAX(COLUMN($AG33:AX33)*($AG33:AX33=2))>MAX(COLUMN($AG33:AX33)*($AG33:AX33=1))),IF(COLUMN(AY33)-MAX(COLUMN($AG33:AX33)*($AG33:AX33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AY33)-MAX(COLUMN($AG33:AX33)*($AG33:AX33=3))=$J33,3,0),IF(COLUMN(AY33)-MAX(COLUMN($AG33:AX33)*($AG33:AX33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AY33)*($AG33:AY33=1))>MAX(COLUMN($AG33:AY33)*($AG33:AY33=3)),MAX(COLUMN($AG33:AY33)*($AG33:AY33=1))>MAX(COLUMN($AG33:AY33)*($AG33:AY33=2))),IF($K33=\"Not Possible\",IF(COLUMN(AZ33)-MAX(COLUMN($AG33:AY33)*($AG33:AY33=1))=$J33,3,0),IF(COLUMN(AZ33)-MAX(COLUMN($AG33:AY33)*($AG33:AY33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AY33)*($AG33:AY33=2))>MAX(COLUMN($AG33:AY33)*($AG33:AY33=3)),MAX(COLUMN($AG33:AY33)*($AG33:AY33=2))>MAX(COLUMN($AG33:AY33)*($AG33:AY33=1))),IF(COLUMN(AZ33)-MAX(COLUMN($AG33:AY33)*($AG33:AY33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(AZ33)-MAX(COLUMN($AG33:AY33)*($AG33:AY33=3))=$J33,3,0),IF(COLUMN(AZ33)-MAX(COLUMN($AG33:AY33)*($AG33:AY33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=1))>MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=3)),MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=1))>MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BA33)-MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=1))=$J33,3,0),IF(COLUMN(BA33)-MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=2))>MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=3)),MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=2))>MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=1))),IF(COLUMN(BA33)-MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BA33)-MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=3))=$J33,3,0),IF(COLUMN(BA33)-MAX(COLUMN($AG33:AZ33)*($AG33:AZ33=3))=$J33,2,0)))))","v":2},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BA33)*($AG33:BA33=1))>MAX(COLUMN($AG33:BA33)*($AG33:BA33=3)),MAX(COLUMN($AG33:BA33)*($AG33:BA33=1))>MAX(COLUMN($AG33:BA33)*($AG33:BA33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BB33)-MAX(COLUMN($AG33:BA33)*($AG33:BA33=1))=$J33,3,0),IF(COLUMN(BB33)-MAX(COLUMN($AG33:BA33)*($AG33:BA33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BA33)*($AG33:BA33=2))>MAX(COLUMN($AG33:BA33)*($AG33:BA33=3)),MAX(COLUMN($AG33:BA33)*($AG33:BA33=2))>MAX(COLUMN($AG33:BA33)*($AG33:BA33=1))),IF(COLUMN(BB33)-MAX(COLUMN($AG33:BA33)*($AG33:BA33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BB33)-MAX(COLUMN($AG33:BA33)*($AG33:BA33=3))=$J33,3,0),IF(COLUMN(BB33)-MAX(COLUMN($AG33:BA33)*($AG33:BA33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BB33)*($AG33:BB33=1))>MAX(COLUMN($AG33:BB33)*($AG33:BB33=3)),MAX(COLUMN($AG33:BB33)*($AG33:BB33=1))>MAX(COLUMN($AG33:BB33)*($AG33:BB33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BC33)-MAX(COLUMN($AG33:BB33)*($AG33:BB33=1))=$J33,3,0),IF(COLUMN(BC33)-MAX(COLUMN($AG33:BB33)*($AG33:BB33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BB33)*($AG33:BB33=2))>MAX(COLUMN($AG33:BB33)*($AG33:BB33=3)),MAX(COLUMN($AG33:BB33)*($AG33:BB33=2))>MAX(COLUMN($AG33:BB33)*($AG33:BB33=1))),IF(COLUMN(BC33)-MAX(COLUMN($AG33:BB33)*($AG33:BB33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BC33)-MAX(COLUMN($AG33:BB33)*($AG33:BB33=3))=$J33,3,0),IF(COLUMN(BC33)-MAX(COLUMN($AG33:BB33)*($AG33:BB33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BC33)*($AG33:BC33=1))>MAX(COLUMN($AG33:BC33)*($AG33:BC33=3)),MAX(COLUMN($AG33:BC33)*($AG33:BC33=1))>MAX(COLUMN($AG33:BC33)*($AG33:BC33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BD33)-MAX(COLUMN($AG33:BC33)*($AG33:BC33=1))=$J33,3,0),IF(COLUMN(BD33)-MAX(COLUMN($AG33:BC33)*($AG33:BC33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BC33)*($AG33:BC33=2))>MAX(COLUMN($AG33:BC33)*($AG33:BC33=3)),MAX(COLUMN($AG33:BC33)*($AG33:BC33=2))>MAX(COLUMN($AG33:BC33)*($AG33:BC33=1))),IF(COLUMN(BD33)-MAX(COLUMN($AG33:BC33)*($AG33:BC33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BD33)-MAX(COLUMN($AG33:BC33)*($AG33:BC33=3))=$J33,3,0),IF(COLUMN(BD33)-MAX(COLUMN($AG33:BC33)*($AG33:BC33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BD33)*($AG33:BD33=1))>MAX(COLUMN($AG33:BD33)*($AG33:BD33=3)),MAX(COLUMN($AG33:BD33)*($AG33:BD33=1))>MAX(COLUMN($AG33:BD33)*($AG33:BD33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BE33)-MAX(COLUMN($AG33:BD33)*($AG33:BD33=1))=$J33,3,0),IF(COLUMN(BE33)-MAX(COLUMN($AG33:BD33)*($AG33:BD33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BD33)*($AG33:BD33=2))>MAX(COLUMN($AG33:BD33)*($AG33:BD33=3)),MAX(COLUMN($AG33:BD33)*($AG33:BD33=2))>MAX(COLUMN($AG33:BD33)*($AG33:BD33=1))),IF(COLUMN(BE33)-MAX(COLUMN($AG33:BD33)*($AG33:BD33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BE33)-MAX(COLUMN($AG33:BD33)*($AG33:BD33=3))=$J33,3,0),IF(COLUMN(BE33)-MAX(COLUMN($AG33:BD33)*($AG33:BD33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BE33)*($AG33:BE33=1))>MAX(COLUMN($AG33:BE33)*($AG33:BE33=3)),MAX(COLUMN($AG33:BE33)*($AG33:BE33=1))>MAX(COLUMN($AG33:BE33)*($AG33:BE33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BF33)-MAX(COLUMN($AG33:BE33)*($AG33:BE33=1))=$J33,3,0),IF(COLUMN(BF33)-MAX(COLUMN($AG33:BE33)*($AG33:BE33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BE33)*($AG33:BE33=2))>MAX(COLUMN($AG33:BE33)*($AG33:BE33=3)),MAX(COLUMN($AG33:BE33)*($AG33:BE33=2))>MAX(COLUMN($AG33:BE33)*($AG33:BE33=1))),IF(COLUMN(BF33)-MAX(COLUMN($AG33:BE33)*($AG33:BE33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BF33)-MAX(COLUMN($AG33:BE33)*($AG33:BE33=3))=$J33,3,0),IF(COLUMN(BF33)-MAX(COLUMN($AG33:BE33)*($AG33:BE33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BF33)*($AG33:BF33=1))>MAX(COLUMN($AG33:BF33)*($AG33:BF33=3)),MAX(COLUMN($AG33:BF33)*($AG33:BF33=1))>MAX(COLUMN($AG33:BF33)*($AG33:BF33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BG33)-MAX(COLUMN($AG33:BF33)*($AG33:BF33=1))=$J33,3,0),IF(COLUMN(BG33)-MAX(COLUMN($AG33:BF33)*($AG33:BF33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BF33)*($AG33:BF33=2))>MAX(COLUMN($AG33:BF33)*($AG33:BF33=3)),MAX(COLUMN($AG33:BF33)*($AG33:BF33=2))>MAX(COLUMN($AG33:BF33)*($AG33:BF33=1))),IF(COLUMN(BG33)-MAX(COLUMN($AG33:BF33)*($AG33:BF33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BG33)-MAX(COLUMN($AG33:BF33)*($AG33:BF33=3))=$J33,3,0),IF(COLUMN(BG33)-MAX(COLUMN($AG33:BF33)*($AG33:BF33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BG33)*($AG33:BG33=1))>MAX(COLUMN($AG33:BG33)*($AG33:BG33=3)),MAX(COLUMN($AG33:BG33)*($AG33:BG33=1))>MAX(COLUMN($AG33:BG33)*($AG33:BG33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BH33)-MAX(COLUMN($AG33:BG33)*($AG33:BG33=1))=$J33,3,0),IF(COLUMN(BH33)-MAX(COLUMN($AG33:BG33)*($AG33:BG33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BG33)*($AG33:BG33=2))>MAX(COLUMN($AG33:BG33)*($AG33:BG33=3)),MAX(COLUMN($AG33:BG33)*($AG33:BG33=2))>MAX(COLUMN($AG33:BG33)*($AG33:BG33=1))),IF(COLUMN(BH33)-MAX(COLUMN($AG33:BG33)*($AG33:BG33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BH33)-MAX(COLUMN($AG33:BG33)*($AG33:BG33=3))=$J33,3,0),IF(COLUMN(BH33)-MAX(COLUMN($AG33:BG33)*($AG33:BG33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BH33)*($AG33:BH33=1))>MAX(COLUMN($AG33:BH33)*($AG33:BH33=3)),MAX(COLUMN($AG33:BH33)*($AG33:BH33=1))>MAX(COLUMN($AG33:BH33)*($AG33:BH33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BI33)-MAX(COLUMN($AG33:BH33)*($AG33:BH33=1))=$J33,3,0),IF(COLUMN(BI33)-MAX(COLUMN($AG33:BH33)*($AG33:BH33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BH33)*($AG33:BH33=2))>MAX(COLUMN($AG33:BH33)*($AG33:BH33=3)),MAX(COLUMN($AG33:BH33)*($AG33:BH33=2))>MAX(COLUMN($AG33:BH33)*($AG33:BH33=1))),IF(COLUMN(BI33)-MAX(COLUMN($AG33:BH33)*($AG33:BH33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BI33)-MAX(COLUMN($AG33:BH33)*($AG33:BH33=3))=$J33,3,0),IF(COLUMN(BI33)-MAX(COLUMN($AG33:BH33)*($AG33:BH33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BI33)*($AG33:BI33=1))>MAX(COLUMN($AG33:BI33)*($AG33:BI33=3)),MAX(COLUMN($AG33:BI33)*($AG33:BI33=1))>MAX(COLUMN($AG33:BI33)*($AG33:BI33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BJ33)-MAX(COLUMN($AG33:BI33)*($AG33:BI33=1))=$J33,3,0),IF(COLUMN(BJ33)-MAX(COLUMN($AG33:BI33)*($AG33:BI33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BI33)*($AG33:BI33=2))>MAX(COLUMN($AG33:BI33)*($AG33:BI33=3)),MAX(COLUMN($AG33:BI33)*($AG33:BI33=2))>MAX(COLUMN($AG33:BI33)*($AG33:BI33=1))),IF(COLUMN(BJ33)-MAX(COLUMN($AG33:BI33)*($AG33:BI33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BJ33)-MAX(COLUMN($AG33:BI33)*($AG33:BI33=3))=$J33,3,0),IF(COLUMN(BJ33)-MAX(COLUMN($AG33:BI33)*($AG33:BI33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=1))>MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=3)),MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=1))>MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BK33)-MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=1))=$J33,3,0),IF(COLUMN(BK33)-MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=2))>MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=3)),MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=2))>MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=1))),IF(COLUMN(BK33)-MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BK33)-MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=3))=$J33,3,0),IF(COLUMN(BK33)-MAX(COLUMN($AG33:BJ33)*($AG33:BJ33=3))=$J33,2,0)))))","v":3},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BK33)*($AG33:BK33=1))>MAX(COLUMN($AG33:BK33)*($AG33:BK33=3)),MAX(COLUMN($AG33:BK33)*($AG33:BK33=1))>MAX(COLUMN($AG33:BK33)*($AG33:BK33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BL33)-MAX(COLUMN($AG33:BK33)*($AG33:BK33=1))=$J33,3,0),IF(COLUMN(BL33)-MAX(COLUMN($AG33:BK33)*($AG33:BK33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BK33)*($AG33:BK33=2))>MAX(COLUMN($AG33:BK33)*($AG33:BK33=3)),MAX(COLUMN($AG33:BK33)*($AG33:BK33=2))>MAX(COLUMN($AG33:BK33)*($AG33:BK33=1))),IF(COLUMN(BL33)-MAX(COLUMN($AG33:BK33)*($AG33:BK33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BL33)-MAX(COLUMN($AG33:BK33)*($AG33:BK33=3))=$J33,3,0),IF(COLUMN(BL33)-MAX(COLUMN($AG33:BK33)*($AG33:BK33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BL33)*($AG33:BL33=1))>MAX(COLUMN($AG33:BL33)*($AG33:BL33=3)),MAX(COLUMN($AG33:BL33)*($AG33:BL33=1))>MAX(COLUMN($AG33:BL33)*($AG33:BL33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BM33)-MAX(COLUMN($AG33:BL33)*($AG33:BL33=1))=$J33,3,0),IF(COLUMN(BM33)-MAX(COLUMN($AG33:BL33)*($AG33:BL33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BL33)*($AG33:BL33=2))>MAX(COLUMN($AG33:BL33)*($AG33:BL33=3)),MAX(COLUMN($AG33:BL33)*($AG33:BL33=2))>MAX(COLUMN($AG33:BL33)*($AG33:BL33=1))),IF(COLUMN(BM33)-MAX(COLUMN($AG33:BL33)*($AG33:BL33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BM33)-MAX(COLUMN($AG33:BL33)*($AG33:BL33=3))=$J33,3,0),IF(COLUMN(BM33)-MAX(COLUMN($AG33:BL33)*($AG33:BL33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BM33)*($AG33:BM33=1))>MAX(COLUMN($AG33:BM33)*($AG33:BM33=3)),MAX(COLUMN($AG33:BM33)*($AG33:BM33=1))>MAX(COLUMN($AG33:BM33)*($AG33:BM33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BN33)-MAX(COLUMN($AG33:BM33)*($AG33:BM33=1))=$J33,3,0),IF(COLUMN(BN33)-MAX(COLUMN($AG33:BM33)*($AG33:BM33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BM33)*($AG33:BM33=2))>MAX(COLUMN($AG33:BM33)*($AG33:BM33=3)),MAX(COLUMN($AG33:BM33)*($AG33:BM33=2))>MAX(COLUMN($AG33:BM33)*($AG33:BM33=1))),IF(COLUMN(BN33)-MAX(COLUMN($AG33:BM33)*($AG33:BM33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BN33)-MAX(COLUMN($AG33:BM33)*($AG33:BM33=3))=$J33,3,0),IF(COLUMN(BN33)-MAX(COLUMN($AG33:BM33)*($AG33:BM33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BN33)*($AG33:BN33=1))>MAX(COLUMN($AG33:BN33)*($AG33:BN33=3)),MAX(COLUMN($AG33:BN33)*($AG33:BN33=1))>MAX(COLUMN($AG33:BN33)*($AG33:BN33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BO33)-MAX(COLUMN($AG33:BN33)*($AG33:BN33=1))=$J33,3,0),IF(COLUMN(BO33)-MAX(COLUMN($AG33:BN33)*($AG33:BN33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BN33)*($AG33:BN33=2))>MAX(COLUMN($AG33:BN33)*($AG33:BN33=3)),MAX(COLUMN($AG33:BN33)*($AG33:BN33=2))>MAX(COLUMN($AG33:BN33)*($AG33:BN33=1))),IF(COLUMN(BO33)-MAX(COLUMN($AG33:BN33)*($AG33:BN33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BO33)-MAX(COLUMN($AG33:BN33)*($AG33:BN33=3))=$J33,3,0),IF(COLUMN(BO33)-MAX(COLUMN($AG33:BN33)*($AG33:BN33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BO33)*($AG33:BO33=1))>MAX(COLUMN($AG33:BO33)*($AG33:BO33=3)),MAX(COLUMN($AG33:BO33)*($AG33:BO33=1))>MAX(COLUMN($AG33:BO33)*($AG33:BO33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BP33)-MAX(COLUMN($AG33:BO33)*($AG33:BO33=1))=$J33,3,0),IF(COLUMN(BP33)-MAX(COLUMN($AG33:BO33)*($AG33:BO33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BO33)*($AG33:BO33=2))>MAX(COLUMN($AG33:BO33)*($AG33:BO33=3)),MAX(COLUMN($AG33:BO33)*($AG33:BO33=2))>MAX(COLUMN($AG33:BO33)*($AG33:BO33=1))),IF(COLUMN(BP33)-MAX(COLUMN($AG33:BO33)*($AG33:BO33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BP33)-MAX(COLUMN($AG33:BO33)*($AG33:BO33=3))=$J33,3,0),IF(COLUMN(BP33)-MAX(COLUMN($AG33:BO33)*($AG33:BO33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BP33)*($AG33:BP33=1))>MAX(COLUMN($AG33:BP33)*($AG33:BP33=3)),MAX(COLUMN($AG33:BP33)*($AG33:BP33=1))>MAX(COLUMN($AG33:BP33)*($AG33:BP33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BQ33)-MAX(COLUMN($AG33:BP33)*($AG33:BP33=1))=$J33,3,0),IF(COLUMN(BQ33)-MAX(COLUMN($AG33:BP33)*($AG33:BP33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BP33)*($AG33:BP33=2))>MAX(COLUMN($AG33:BP33)*($AG33:BP33=3)),MAX(COLUMN($AG33:BP33)*($AG33:BP33=2))>MAX(COLUMN($AG33:BP33)*($AG33:BP33=1))),IF(COLUMN(BQ33)-MAX(COLUMN($AG33:BP33)*($AG33:BP33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BQ33)-MAX(COLUMN($AG33:BP33)*($AG33:BP33=3))=$J33,3,0),IF(COLUMN(BQ33)-MAX(COLUMN($AG33:BP33)*($AG33:BP33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=1))>MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=3)),MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=1))>MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BR33)-MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=1))=$J33,3,0),IF(COLUMN(BR33)-MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=2))>MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=3)),MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=2))>MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=1))),IF(COLUMN(BR33)-MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BR33)-MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=3))=$J33,3,0),IF(COLUMN(BR33)-MAX(COLUMN($AG33:BQ33)*($AG33:BQ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BR33)*($AG33:BR33=1))>MAX(COLUMN($AG33:BR33)*($AG33:BR33=3)),MAX(COLUMN($AG33:BR33)*($AG33:BR33=1))>MAX(COLUMN($AG33:BR33)*($AG33:BR33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BS33)-MAX(COLUMN($AG33:BR33)*($AG33:BR33=1))=$J33,3,0),IF(COLUMN(BS33)-MAX(COLUMN($AG33:BR33)*($AG33:BR33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BR33)*($AG33:BR33=2))>MAX(COLUMN($AG33:BR33)*($AG33:BR33=3)),MAX(COLUMN($AG33:BR33)*($AG33:BR33=2))>MAX(COLUMN($AG33:BR33)*($AG33:BR33=1))),IF(COLUMN(BS33)-MAX(COLUMN($AG33:BR33)*($AG33:BR33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BS33)-MAX(COLUMN($AG33:BR33)*($AG33:BR33=3))=$J33,3,0),IF(COLUMN(BS33)-MAX(COLUMN($AG33:BR33)*($AG33:BR33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BS33)*($AG33:BS33=1))>MAX(COLUMN($AG33:BS33)*($AG33:BS33=3)),MAX(COLUMN($AG33:BS33)*($AG33:BS33=1))>MAX(COLUMN($AG33:BS33)*($AG33:BS33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BT33)-MAX(COLUMN($AG33:BS33)*($AG33:BS33=1))=$J33,3,0),IF(COLUMN(BT33)-MAX(COLUMN($AG33:BS33)*($AG33:BS33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BS33)*($AG33:BS33=2))>MAX(COLUMN($AG33:BS33)*($AG33:BS33=3)),MAX(COLUMN($AG33:BS33)*($AG33:BS33=2))>MAX(COLUMN($AG33:BS33)*($AG33:BS33=1))),IF(COLUMN(BT33)-MAX(COLUMN($AG33:BS33)*($AG33:BS33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BT33)-MAX(COLUMN($AG33:BS33)*($AG33:BS33=3))=$J33,3,0),IF(COLUMN(BT33)-MAX(COLUMN($AG33:BS33)*($AG33:BS33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BT33)*($AG33:BT33=1))>MAX(COLUMN($AG33:BT33)*($AG33:BT33=3)),MAX(COLUMN($AG33:BT33)*($AG33:BT33=1))>MAX(COLUMN($AG33:BT33)*($AG33:BT33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BU33)-MAX(COLUMN($AG33:BT33)*($AG33:BT33=1))=$J33,3,0),IF(COLUMN(BU33)-MAX(COLUMN($AG33:BT33)*($AG33:BT33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BT33)*($AG33:BT33=2))>MAX(COLUMN($AG33:BT33)*($AG33:BT33=3)),MAX(COLUMN($AG33:BT33)*($AG33:BT33=2))>MAX(COLUMN($AG33:BT33)*($AG33:BT33=1))),IF(COLUMN(BU33)-MAX(COLUMN($AG33:BT33)*($AG33:BT33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BU33)-MAX(COLUMN($AG33:BT33)*($AG33:BT33=3))=$J33,3,0),IF(COLUMN(BU33)-MAX(COLUMN($AG33:BT33)*($AG33:BT33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BU33)*($AG33:BU33=1))>MAX(COLUMN($AG33:BU33)*($AG33:BU33=3)),MAX(COLUMN($AG33:BU33)*($AG33:BU33=1))>MAX(COLUMN($AG33:BU33)*($AG33:BU33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BV33)-MAX(COLUMN($AG33:BU33)*($AG33:BU33=1))=$J33,3,0),IF(COLUMN(BV33)-MAX(COLUMN($AG33:BU33)*($AG33:BU33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BU33)*($AG33:BU33=2))>MAX(COLUMN($AG33:BU33)*($AG33:BU33=3)),MAX(COLUMN($AG33:BU33)*($AG33:BU33=2))>MAX(COLUMN($AG33:BU33)*($AG33:BU33=1))),IF(COLUMN(BV33)-MAX(COLUMN($AG33:BU33)*($AG33:BU33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BV33)-MAX(COLUMN($AG33:BU33)*($AG33:BU33=3))=$J33,3,0),IF(COLUMN(BV33)-MAX(COLUMN($AG33:BU33)*($AG33:BU33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BV33)*($AG33:BV33=1))>MAX(COLUMN($AG33:BV33)*($AG33:BV33=3)),MAX(COLUMN($AG33:BV33)*($AG33:BV33=1))>MAX(COLUMN($AG33:BV33)*($AG33:BV33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BW33)-MAX(COLUMN($AG33:BV33)*($AG33:BV33=1))=$J33,3,0),IF(COLUMN(BW33)-MAX(COLUMN($AG33:BV33)*($AG33:BV33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BV33)*($AG33:BV33=2))>MAX(COLUMN($AG33:BV33)*($AG33:BV33=3)),MAX(COLUMN($AG33:BV33)*($AG33:BV33=2))>MAX(COLUMN($AG33:BV33)*($AG33:BV33=1))),IF(COLUMN(BW33)-MAX(COLUMN($AG33:BV33)*($AG33:BV33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BW33)-MAX(COLUMN($AG33:BV33)*($AG33:BV33=3))=$J33,3,0),IF(COLUMN(BW33)-MAX(COLUMN($AG33:BV33)*($AG33:BV33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BW33)*($AG33:BW33=1))>MAX(COLUMN($AG33:BW33)*($AG33:BW33=3)),MAX(COLUMN($AG33:BW33)*($AG33:BW33=1))>MAX(COLUMN($AG33:BW33)*($AG33:BW33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BX33)-MAX(COLUMN($AG33:BW33)*($AG33:BW33=1))=$J33,3,0),IF(COLUMN(BX33)-MAX(COLUMN($AG33:BW33)*($AG33:BW33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BW33)*($AG33:BW33=2))>MAX(COLUMN($AG33:BW33)*($AG33:BW33=3)),MAX(COLUMN($AG33:BW33)*($AG33:BW33=2))>MAX(COLUMN($AG33:BW33)*($AG33:BW33=1))),IF(COLUMN(BX33)-MAX(COLUMN($AG33:BW33)*($AG33:BW33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BX33)-MAX(COLUMN($AG33:BW33)*($AG33:BW33=3))=$J33,3,0),IF(COLUMN(BX33)-MAX(COLUMN($AG33:BW33)*($AG33:BW33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BX33)*($AG33:BX33=1))>MAX(COLUMN($AG33:BX33)*($AG33:BX33=3)),MAX(COLUMN($AG33:BX33)*($AG33:BX33=1))>MAX(COLUMN($AG33:BX33)*($AG33:BX33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BY33)-MAX(COLUMN($AG33:BX33)*($AG33:BX33=1))=$J33,3,0),IF(COLUMN(BY33)-MAX(COLUMN($AG33:BX33)*($AG33:BX33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BX33)*($AG33:BX33=2))>MAX(COLUMN($AG33:BX33)*($AG33:BX33=3)),MAX(COLUMN($AG33:BX33)*($AG33:BX33=2))>MAX(COLUMN($AG33:BX33)*($AG33:BX33=1))),IF(COLUMN(BY33)-MAX(COLUMN($AG33:BX33)*($AG33:BX33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BY33)-MAX(COLUMN($AG33:BX33)*($AG33:BX33=3))=$J33,3,0),IF(COLUMN(BY33)-MAX(COLUMN($AG33:BX33)*($AG33:BX33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BY33)*($AG33:BY33=1))>MAX(COLUMN($AG33:BY33)*($AG33:BY33=3)),MAX(COLUMN($AG33:BY33)*($AG33:BY33=1))>MAX(COLUMN($AG33:BY33)*($AG33:BY33=2))),IF($K33=\"Not Possible\",IF(COLUMN(BZ33)-MAX(COLUMN($AG33:BY33)*($AG33:BY33=1))=$J33,3,0),IF(COLUMN(BZ33)-MAX(COLUMN($AG33:BY33)*($AG33:BY33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BY33)*($AG33:BY33=2))>MAX(COLUMN($AG33:BY33)*($AG33:BY33=3)),MAX(COLUMN($AG33:BY33)*($AG33:BY33=2))>MAX(COLUMN($AG33:BY33)*($AG33:BY33=1))),IF(COLUMN(BZ33)-MAX(COLUMN($AG33:BY33)*($AG33:BY33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(BZ33)-MAX(COLUMN($AG33:BY33)*($AG33:BY33=3))=$J33,3,0),IF(COLUMN(BZ33)-MAX(COLUMN($AG33:BY33)*($AG33:BY33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=1))>MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=3)),MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=1))>MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CA33)-MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=1))=$J33,3,0),IF(COLUMN(CA33)-MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=2))>MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=3)),MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=2))>MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=1))),IF(COLUMN(CA33)-MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CA33)-MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=3))=$J33,3,0),IF(COLUMN(CA33)-MAX(COLUMN($AG33:BZ33)*($AG33:BZ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CA33)*($AG33:CA33=1))>MAX(COLUMN($AG33:CA33)*($AG33:CA33=3)),MAX(COLUMN($AG33:CA33)*($AG33:CA33=1))>MAX(COLUMN($AG33:CA33)*($AG33:CA33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CB33)-MAX(COLUMN($AG33:CA33)*($AG33:CA33=1))=$J33,3,0),IF(COLUMN(CB33)-MAX(COLUMN($AG33:CA33)*($AG33:CA33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CA33)*($AG33:CA33=2))>MAX(COLUMN($AG33:CA33)*($AG33:CA33=3)),MAX(COLUMN($AG33:CA33)*($AG33:CA33=2))>MAX(COLUMN($AG33:CA33)*($AG33:CA33=1))),IF(COLUMN(CB33)-MAX(COLUMN($AG33:CA33)*($AG33:CA33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CB33)-MAX(COLUMN($AG33:CA33)*($AG33:CA33=3))=$J33,3,0),IF(COLUMN(CB33)-MAX(COLUMN($AG33:CA33)*($AG33:CA33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CB33)*($AG33:CB33=1))>MAX(COLUMN($AG33:CB33)*($AG33:CB33=3)),MAX(COLUMN($AG33:CB33)*($AG33:CB33=1))>MAX(COLUMN($AG33:CB33)*($AG33:CB33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CC33)-MAX(COLUMN($AG33:CB33)*($AG33:CB33=1))=$J33,3,0),IF(COLUMN(CC33)-MAX(COLUMN($AG33:CB33)*($AG33:CB33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CB33)*($AG33:CB33=2))>MAX(COLUMN($AG33:CB33)*($AG33:CB33=3)),MAX(COLUMN($AG33:CB33)*($AG33:CB33=2))>MAX(COLUMN($AG33:CB33)*($AG33:CB33=1))),IF(COLUMN(CC33)-MAX(COLUMN($AG33:CB33)*($AG33:CB33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CC33)-MAX(COLUMN($AG33:CB33)*($AG33:CB33=3))=$J33,3,0),IF(COLUMN(CC33)-MAX(COLUMN($AG33:CB33)*($AG33:CB33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CC33)*($AG33:CC33=1))>MAX(COLUMN($AG33:CC33)*($AG33:CC33=3)),MAX(COLUMN($AG33:CC33)*($AG33:CC33=1))>MAX(COLUMN($AG33:CC33)*($AG33:CC33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CD33)-MAX(COLUMN($AG33:CC33)*($AG33:CC33=1))=$J33,3,0),IF(COLUMN(CD33)-MAX(COLUMN($AG33:CC33)*($AG33:CC33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CC33)*($AG33:CC33=2))>MAX(COLUMN($AG33:CC33)*($AG33:CC33=3)),MAX(COLUMN($AG33:CC33)*($AG33:CC33=2))>MAX(COLUMN($AG33:CC33)*($AG33:CC33=1))),IF(COLUMN(CD33)-MAX(COLUMN($AG33:CC33)*($AG33:CC33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CD33)-MAX(COLUMN($AG33:CC33)*($AG33:CC33=3))=$J33,3,0),IF(COLUMN(CD33)-MAX(COLUMN($AG33:CC33)*($AG33:CC33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CD33)*($AG33:CD33=1))>MAX(COLUMN($AG33:CD33)*($AG33:CD33=3)),MAX(COLUMN($AG33:CD33)*($AG33:CD33=1))>MAX(COLUMN($AG33:CD33)*($AG33:CD33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CE33)-MAX(COLUMN($AG33:CD33)*($AG33:CD33=1))=$J33,3,0),IF(COLUMN(CE33)-MAX(COLUMN($AG33:CD33)*($AG33:CD33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CD33)*($AG33:CD33=2))>MAX(COLUMN($AG33:CD33)*($AG33:CD33=3)),MAX(COLUMN($AG33:CD33)*($AG33:CD33=2))>MAX(COLUMN($AG33:CD33)*($AG33:CD33=1))),IF(COLUMN(CE33)-MAX(COLUMN($AG33:CD33)*($AG33:CD33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CE33)-MAX(COLUMN($AG33:CD33)*($AG33:CD33=3))=$J33,3,0),IF(COLUMN(CE33)-MAX(COLUMN($AG33:CD33)*($AG33:CD33=3))=$J33,2,0)))))","v":2},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CE33)*($AG33:CE33=1))>MAX(COLUMN($AG33:CE33)*($AG33:CE33=3)),MAX(COLUMN($AG33:CE33)*($AG33:CE33=1))>MAX(COLUMN($AG33:CE33)*($AG33:CE33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CF33)-MAX(COLUMN($AG33:CE33)*($AG33:CE33=1))=$J33,3,0),IF(COLUMN(CF33)-MAX(COLUMN($AG33:CE33)*($AG33:CE33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CE33)*($AG33:CE33=2))>MAX(COLUMN($AG33:CE33)*($AG33:CE33=3)),MAX(COLUMN($AG33:CE33)*($AG33:CE33=2))>MAX(COLUMN($AG33:CE33)*($AG33:CE33=1))),IF(COLUMN(CF33)-MAX(COLUMN($AG33:CE33)*($AG33:CE33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CF33)-MAX(COLUMN($AG33:CE33)*($AG33:CE33=3))=$J33,3,0),IF(COLUMN(CF33)-MAX(COLUMN($AG33:CE33)*($AG33:CE33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CF33)*($AG33:CF33=1))>MAX(COLUMN($AG33:CF33)*($AG33:CF33=3)),MAX(COLUMN($AG33:CF33)*($AG33:CF33=1))>MAX(COLUMN($AG33:CF33)*($AG33:CF33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CG33)-MAX(COLUMN($AG33:CF33)*($AG33:CF33=1))=$J33,3,0),IF(COLUMN(CG33)-MAX(COLUMN($AG33:CF33)*($AG33:CF33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CF33)*($AG33:CF33=2))>MAX(COLUMN($AG33:CF33)*($AG33:CF33=3)),MAX(COLUMN($AG33:CF33)*($AG33:CF33=2))>MAX(COLUMN($AG33:CF33)*($AG33:CF33=1))),IF(COLUMN(CG33)-MAX(COLUMN($AG33:CF33)*($AG33:CF33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CG33)-MAX(COLUMN($AG33:CF33)*($AG33:CF33=3))=$J33,3,0),IF(COLUMN(CG33)-MAX(COLUMN($AG33:CF33)*($AG33:CF33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CG33)*($AG33:CG33=1))>MAX(COLUMN($AG33:CG33)*($AG33:CG33=3)),MAX(COLUMN($AG33:CG33)*($AG33:CG33=1))>MAX(COLUMN($AG33:CG33)*($AG33:CG33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CH33)-MAX(COLUMN($AG33:CG33)*($AG33:CG33=1))=$J33,3,0),IF(COLUMN(CH33)-MAX(COLUMN($AG33:CG33)*($AG33:CG33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CG33)*($AG33:CG33=2))>MAX(COLUMN($AG33:CG33)*($AG33:CG33=3)),MAX(COLUMN($AG33:CG33)*($AG33:CG33=2))>MAX(COLUMN($AG33:CG33)*($AG33:CG33=1))),IF(COLUMN(CH33)-MAX(COLUMN($AG33:CG33)*($AG33:CG33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CH33)-MAX(COLUMN($AG33:CG33)*($AG33:CG33=3))=$J33,3,0),IF(COLUMN(CH33)-MAX(COLUMN($AG33:CG33)*($AG33:CG33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CH33)*($AG33:CH33=1))>MAX(COLUMN($AG33:CH33)*($AG33:CH33=3)),MAX(COLUMN($AG33:CH33)*($AG33:CH33=1))>MAX(COLUMN($AG33:CH33)*($AG33:CH33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CI33)-MAX(COLUMN($AG33:CH33)*($AG33:CH33=1))=$J33,3,0),IF(COLUMN(CI33)-MAX(COLUMN($AG33:CH33)*($AG33:CH33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CH33)*($AG33:CH33=2))>MAX(COLUMN($AG33:CH33)*($AG33:CH33=3)),MAX(COLUMN($AG33:CH33)*($AG33:CH33=2))>MAX(COLUMN($AG33:CH33)*($AG33:CH33=1))),IF(COLUMN(CI33)-MAX(COLUMN($AG33:CH33)*($AG33:CH33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CI33)-MAX(COLUMN($AG33:CH33)*($AG33:CH33=3))=$J33,3,0),IF(COLUMN(CI33)-MAX(COLUMN($AG33:CH33)*($AG33:CH33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CI33)*($AG33:CI33=1))>MAX(COLUMN($AG33:CI33)*($AG33:CI33=3)),MAX(COLUMN($AG33:CI33)*($AG33:CI33=1))>MAX(COLUMN($AG33:CI33)*($AG33:CI33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CJ33)-MAX(COLUMN($AG33:CI33)*($AG33:CI33=1))=$J33,3,0),IF(COLUMN(CJ33)-MAX(COLUMN($AG33:CI33)*($AG33:CI33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CI33)*($AG33:CI33=2))>MAX(COLUMN($AG33:CI33)*($AG33:CI33=3)),MAX(COLUMN($AG33:CI33)*($AG33:CI33=2))>MAX(COLUMN($AG33:CI33)*($AG33:CI33=1))),IF(COLUMN(CJ33)-MAX(COLUMN($AG33:CI33)*($AG33:CI33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CJ33)-MAX(COLUMN($AG33:CI33)*($AG33:CI33=3))=$J33,3,0),IF(COLUMN(CJ33)-MAX(COLUMN($AG33:CI33)*($AG33:CI33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=1))>MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=3)),MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=1))>MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CK33)-MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=1))=$J33,3,0),IF(COLUMN(CK33)-MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=2))>MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=3)),MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=2))>MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=1))),IF(COLUMN(CK33)-MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CK33)-MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=3))=$J33,3,0),IF(COLUMN(CK33)-MAX(COLUMN($AG33:CJ33)*($AG33:CJ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CK33)*($AG33:CK33=1))>MAX(COLUMN($AG33:CK33)*($AG33:CK33=3)),MAX(COLUMN($AG33:CK33)*($AG33:CK33=1))>MAX(COLUMN($AG33:CK33)*($AG33:CK33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CL33)-MAX(COLUMN($AG33:CK33)*($AG33:CK33=1))=$J33,3,0),IF(COLUMN(CL33)-MAX(COLUMN($AG33:CK33)*($AG33:CK33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CK33)*($AG33:CK33=2))>MAX(COLUMN($AG33:CK33)*($AG33:CK33=3)),MAX(COLUMN($AG33:CK33)*($AG33:CK33=2))>MAX(COLUMN($AG33:CK33)*($AG33:CK33=1))),IF(COLUMN(CL33)-MAX(COLUMN($AG33:CK33)*($AG33:CK33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CL33)-MAX(COLUMN($AG33:CK33)*($AG33:CK33=3))=$J33,3,0),IF(COLUMN(CL33)-MAX(COLUMN($AG33:CK33)*($AG33:CK33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CL33)*($AG33:CL33=1))>MAX(COLUMN($AG33:CL33)*($AG33:CL33=3)),MAX(COLUMN($AG33:CL33)*($AG33:CL33=1))>MAX(COLUMN($AG33:CL33)*($AG33:CL33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CM33)-MAX(COLUMN($AG33:CL33)*($AG33:CL33=1))=$J33,3,0),IF(COLUMN(CM33)-MAX(COLUMN($AG33:CL33)*($AG33:CL33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CL33)*($AG33:CL33=2))>MAX(COLUMN($AG33:CL33)*($AG33:CL33=3)),MAX(COLUMN($AG33:CL33)*($AG33:CL33=2))>MAX(COLUMN($AG33:CL33)*($AG33:CL33=1))),IF(COLUMN(CM33)-MAX(COLUMN($AG33:CL33)*($AG33:CL33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CM33)-MAX(COLUMN($AG33:CL33)*($AG33:CL33=3))=$J33,3,0),IF(COLUMN(CM33)-MAX(COLUMN($AG33:CL33)*($AG33:CL33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CM33)*($AG33:CM33=1))>MAX(COLUMN($AG33:CM33)*($AG33:CM33=3)),MAX(COLUMN($AG33:CM33)*($AG33:CM33=1))>MAX(COLUMN($AG33:CM33)*($AG33:CM33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CN33)-MAX(COLUMN($AG33:CM33)*($AG33:CM33=1))=$J33,3,0),IF(COLUMN(CN33)-MAX(COLUMN($AG33:CM33)*($AG33:CM33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CM33)*($AG33:CM33=2))>MAX(COLUMN($AG33:CM33)*($AG33:CM33=3)),MAX(COLUMN($AG33:CM33)*($AG33:CM33=2))>MAX(COLUMN($AG33:CM33)*($AG33:CM33=1))),IF(COLUMN(CN33)-MAX(COLUMN($AG33:CM33)*($AG33:CM33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CN33)-MAX(COLUMN($AG33:CM33)*($AG33:CM33=3))=$J33,3,0),IF(COLUMN(CN33)-MAX(COLUMN($AG33:CM33)*($AG33:CM33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CN33)*($AG33:CN33=1))>MAX(COLUMN($AG33:CN33)*($AG33:CN33=3)),MAX(COLUMN($AG33:CN33)*($AG33:CN33=1))>MAX(COLUMN($AG33:CN33)*($AG33:CN33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CO33)-MAX(COLUMN($AG33:CN33)*($AG33:CN33=1))=$J33,3,0),IF(COLUMN(CO33)-MAX(COLUMN($AG33:CN33)*($AG33:CN33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CN33)*($AG33:CN33=2))>MAX(COLUMN($AG33:CN33)*($AG33:CN33=3)),MAX(COLUMN($AG33:CN33)*($AG33:CN33=2))>MAX(COLUMN($AG33:CN33)*($AG33:CN33=1))),IF(COLUMN(CO33)-MAX(COLUMN($AG33:CN33)*($AG33:CN33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CO33)-MAX(COLUMN($AG33:CN33)*($AG33:CN33=3))=$J33,3,0),IF(COLUMN(CO33)-MAX(COLUMN($AG33:CN33)*($AG33:CN33=3))=$J33,2,0)))))","v":3},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CO33)*($AG33:CO33=1))>MAX(COLUMN($AG33:CO33)*($AG33:CO33=3)),MAX(COLUMN($AG33:CO33)*($AG33:CO33=1))>MAX(COLUMN($AG33:CO33)*($AG33:CO33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CP33)-MAX(COLUMN($AG33:CO33)*($AG33:CO33=1))=$J33,3,0),IF(COLUMN(CP33)-MAX(COLUMN($AG33:CO33)*($AG33:CO33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CO33)*($AG33:CO33=2))>MAX(COLUMN($AG33:CO33)*($AG33:CO33=3)),MAX(COLUMN($AG33:CO33)*($AG33:CO33=2))>MAX(COLUMN($AG33:CO33)*($AG33:CO33=1))),IF(COLUMN(CP33)-MAX(COLUMN($AG33:CO33)*($AG33:CO33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CP33)-MAX(COLUMN($AG33:CO33)*($AG33:CO33=3))=$J33,3,0),IF(COLUMN(CP33)-MAX(COLUMN($AG33:CO33)*($AG33:CO33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CP33)*($AG33:CP33=1))>MAX(COLUMN($AG33:CP33)*($AG33:CP33=3)),MAX(COLUMN($AG33:CP33)*($AG33:CP33=1))>MAX(COLUMN($AG33:CP33)*($AG33:CP33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CQ33)-MAX(COLUMN($AG33:CP33)*($AG33:CP33=1))=$J33,3,0),IF(COLUMN(CQ33)-MAX(COLUMN($AG33:CP33)*($AG33:CP33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CP33)*($AG33:CP33=2))>MAX(COLUMN($AG33:CP33)*($AG33:CP33=3)),MAX(COLUMN($AG33:CP33)*($AG33:CP33=2))>MAX(COLUMN($AG33:CP33)*($AG33:CP33=1))),IF(COLUMN(CQ33)-MAX(COLUMN($AG33:CP33)*($AG33:CP33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CQ33)-MAX(COLUMN($AG33:CP33)*($AG33:CP33=3))=$J33,3,0),IF(COLUMN(CQ33)-MAX(COLUMN($AG33:CP33)*($AG33:CP33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=1))>MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=3)),MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=1))>MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CR33)-MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=1))=$J33,3,0),IF(COLUMN(CR33)-MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=2))>MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=3)),MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=2))>MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=1))),IF(COLUMN(CR33)-MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CR33)-MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=3))=$J33,3,0),IF(COLUMN(CR33)-MAX(COLUMN($AG33:CQ33)*($AG33:CQ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CR33)*($AG33:CR33=1))>MAX(COLUMN($AG33:CR33)*($AG33:CR33=3)),MAX(COLUMN($AG33:CR33)*($AG33:CR33=1))>MAX(COLUMN($AG33:CR33)*($AG33:CR33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CS33)-MAX(COLUMN($AG33:CR33)*($AG33:CR33=1))=$J33,3,0),IF(COLUMN(CS33)-MAX(COLUMN($AG33:CR33)*($AG33:CR33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CR33)*($AG33:CR33=2))>MAX(COLUMN($AG33:CR33)*($AG33:CR33=3)),MAX(COLUMN($AG33:CR33)*($AG33:CR33=2))>MAX(COLUMN($AG33:CR33)*($AG33:CR33=1))),IF(COLUMN(CS33)-MAX(COLUMN($AG33:CR33)*($AG33:CR33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CS33)-MAX(COLUMN($AG33:CR33)*($AG33:CR33=3))=$J33,3,0),IF(COLUMN(CS33)-MAX(COLUMN($AG33:CR33)*($AG33:CR33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CS33)*($AG33:CS33=1))>MAX(COLUMN($AG33:CS33)*($AG33:CS33=3)),MAX(COLUMN($AG33:CS33)*($AG33:CS33=1))>MAX(COLUMN($AG33:CS33)*($AG33:CS33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CT33)-MAX(COLUMN($AG33:CS33)*($AG33:CS33=1))=$J33,3,0),IF(COLUMN(CT33)-MAX(COLUMN($AG33:CS33)*($AG33:CS33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CS33)*($AG33:CS33=2))>MAX(COLUMN($AG33:CS33)*($AG33:CS33=3)),MAX(COLUMN($AG33:CS33)*($AG33:CS33=2))>MAX(COLUMN($AG33:CS33)*($AG33:CS33=1))),IF(COLUMN(CT33)-MAX(COLUMN($AG33:CS33)*($AG33:CS33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CT33)-MAX(COLUMN($AG33:CS33)*($AG33:CS33=3))=$J33,3,0),IF(COLUMN(CT33)-MAX(COLUMN($AG33:CS33)*($AG33:CS33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CT33)*($AG33:CT33=1))>MAX(COLUMN($AG33:CT33)*($AG33:CT33=3)),MAX(COLUMN($AG33:CT33)*($AG33:CT33=1))>MAX(COLUMN($AG33:CT33)*($AG33:CT33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CU33)-MAX(COLUMN($AG33:CT33)*($AG33:CT33=1))=$J33,3,0),IF(COLUMN(CU33)-MAX(COLUMN($AG33:CT33)*($AG33:CT33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CT33)*($AG33:CT33=2))>MAX(COLUMN($AG33:CT33)*($AG33:CT33=3)),MAX(COLUMN($AG33:CT33)*($AG33:CT33=2))>MAX(COLUMN($AG33:CT33)*($AG33:CT33=1))),IF(COLUMN(CU33)-MAX(COLUMN($AG33:CT33)*($AG33:CT33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CU33)-MAX(COLUMN($AG33:CT33)*($AG33:CT33=3))=$J33,3,0),IF(COLUMN(CU33)-MAX(COLUMN($AG33:CT33)*($AG33:CT33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CU33)*($AG33:CU33=1))>MAX(COLUMN($AG33:CU33)*($AG33:CU33=3)),MAX(COLUMN($AG33:CU33)*($AG33:CU33=1))>MAX(COLUMN($AG33:CU33)*($AG33:CU33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CV33)-MAX(COLUMN($AG33:CU33)*($AG33:CU33=1))=$J33,3,0),IF(COLUMN(CV33)-MAX(COLUMN($AG33:CU33)*($AG33:CU33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CU33)*($AG33:CU33=2))>MAX(COLUMN($AG33:CU33)*($AG33:CU33=3)),MAX(COLUMN($AG33:CU33)*($AG33:CU33=2))>MAX(COLUMN($AG33:CU33)*($AG33:CU33=1))),IF(COLUMN(CV33)-MAX(COLUMN($AG33:CU33)*($AG33:CU33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CV33)-MAX(COLUMN($AG33:CU33)*($AG33:CU33=3))=$J33,3,0),IF(COLUMN(CV33)-MAX(COLUMN($AG33:CU33)*($AG33:CU33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CV33)*($AG33:CV33=1))>MAX(COLUMN($AG33:CV33)*($AG33:CV33=3)),MAX(COLUMN($AG33:CV33)*($AG33:CV33=1))>MAX(COLUMN($AG33:CV33)*($AG33:CV33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CW33)-MAX(COLUMN($AG33:CV33)*($AG33:CV33=1))=$J33,3,0),IF(COLUMN(CW33)-MAX(COLUMN($AG33:CV33)*($AG33:CV33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CV33)*($AG33:CV33=2))>MAX(COLUMN($AG33:CV33)*($AG33:CV33=3)),MAX(COLUMN($AG33:CV33)*($AG33:CV33=2))>MAX(COLUMN($AG33:CV33)*($AG33:CV33=1))),IF(COLUMN(CW33)-MAX(COLUMN($AG33:CV33)*($AG33:CV33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CW33)-MAX(COLUMN($AG33:CV33)*($AG33:CV33=3))=$J33,3,0),IF(COLUMN(CW33)-MAX(COLUMN($AG33:CV33)*($AG33:CV33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CW33)*($AG33:CW33=1))>MAX(COLUMN($AG33:CW33)*($AG33:CW33=3)),MAX(COLUMN($AG33:CW33)*($AG33:CW33=1))>MAX(COLUMN($AG33:CW33)*($AG33:CW33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CX33)-MAX(COLUMN($AG33:CW33)*($AG33:CW33=1))=$J33,3,0),IF(COLUMN(CX33)-MAX(COLUMN($AG33:CW33)*($AG33:CW33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CW33)*($AG33:CW33=2))>MAX(COLUMN($AG33:CW33)*($AG33:CW33=3)),MAX(COLUMN($AG33:CW33)*($AG33:CW33=2))>MAX(COLUMN($AG33:CW33)*($AG33:CW33=1))),IF(COLUMN(CX33)-MAX(COLUMN($AG33:CW33)*($AG33:CW33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CX33)-MAX(COLUMN($AG33:CW33)*($AG33:CW33=3))=$J33,3,0),IF(COLUMN(CX33)-MAX(COLUMN($AG33:CW33)*($AG33:CW33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CX33)*($AG33:CX33=1))>MAX(COLUMN($AG33:CX33)*($AG33:CX33=3)),MAX(COLUMN($AG33:CX33)*($AG33:CX33=1))>MAX(COLUMN($AG33:CX33)*($AG33:CX33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CY33)-MAX(COLUMN($AG33:CX33)*($AG33:CX33=1))=$J33,3,0),IF(COLUMN(CY33)-MAX(COLUMN($AG33:CX33)*($AG33:CX33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CX33)*($AG33:CX33=2))>MAX(COLUMN($AG33:CX33)*($AG33:CX33=3)),MAX(COLUMN($AG33:CX33)*($AG33:CX33=2))>MAX(COLUMN($AG33:CX33)*($AG33:CX33=1))),IF(COLUMN(CY33)-MAX(COLUMN($AG33:CX33)*($AG33:CX33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CY33)-MAX(COLUMN($AG33:CX33)*($AG33:CX33=3))=$J33,3,0),IF(COLUMN(CY33)-MAX(COLUMN($AG33:CX33)*($AG33:CX33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CY33)*($AG33:CY33=1))>MAX(COLUMN($AG33:CY33)*($AG33:CY33=3)),MAX(COLUMN($AG33:CY33)*($AG33:CY33=1))>MAX(COLUMN($AG33:CY33)*($AG33:CY33=2))),IF($K33=\"Not Possible\",IF(COLUMN(CZ33)-MAX(COLUMN($AG33:CY33)*($AG33:CY33=1))=$J33,3,0),IF(COLUMN(CZ33)-MAX(COLUMN($AG33:CY33)*($AG33:CY33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CY33)*($AG33:CY33=2))>MAX(COLUMN($AG33:CY33)*($AG33:CY33=3)),MAX(COLUMN($AG33:CY33)*($AG33:CY33=2))>MAX(COLUMN($AG33:CY33)*($AG33:CY33=1))),IF(COLUMN(CZ33)-MAX(COLUMN($AG33:CY33)*($AG33:CY33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(CZ33)-MAX(COLUMN($AG33:CY33)*($AG33:CY33=3))=$J33,3,0),IF(COLUMN(CZ33)-MAX(COLUMN($AG33:CY33)*($AG33:CY33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=1))>MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=3)),MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=1))>MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DA33)-MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=1))=$J33,3,0),IF(COLUMN(DA33)-MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=2))>MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=3)),MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=2))>MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=1))),IF(COLUMN(DA33)-MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DA33)-MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=3))=$J33,3,0),IF(COLUMN(DA33)-MAX(COLUMN($AG33:CZ33)*($AG33:CZ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DA33)*($AG33:DA33=1))>MAX(COLUMN($AG33:DA33)*($AG33:DA33=3)),MAX(COLUMN($AG33:DA33)*($AG33:DA33=1))>MAX(COLUMN($AG33:DA33)*($AG33:DA33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DB33)-MAX(COLUMN($AG33:DA33)*($AG33:DA33=1))=$J33,3,0),IF(COLUMN(DB33)-MAX(COLUMN($AG33:DA33)*($AG33:DA33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DA33)*($AG33:DA33=2))>MAX(COLUMN($AG33:DA33)*($AG33:DA33=3)),MAX(COLUMN($AG33:DA33)*($AG33:DA33=2))>MAX(COLUMN($AG33:DA33)*($AG33:DA33=1))),IF(COLUMN(DB33)-MAX(COLUMN($AG33:DA33)*($AG33:DA33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DB33)-MAX(COLUMN($AG33:DA33)*($AG33:DA33=3))=$J33,3,0),IF(COLUMN(DB33)-MAX(COLUMN($AG33:DA33)*($AG33:DA33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DB33)*($AG33:DB33=1))>MAX(COLUMN($AG33:DB33)*($AG33:DB33=3)),MAX(COLUMN($AG33:DB33)*($AG33:DB33=1))>MAX(COLUMN($AG33:DB33)*($AG33:DB33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DC33)-MAX(COLUMN($AG33:DB33)*($AG33:DB33=1))=$J33,3,0),IF(COLUMN(DC33)-MAX(COLUMN($AG33:DB33)*($AG33:DB33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DB33)*($AG33:DB33=2))>MAX(COLUMN($AG33:DB33)*($AG33:DB33=3)),MAX(COLUMN($AG33:DB33)*($AG33:DB33=2))>MAX(COLUMN($AG33:DB33)*($AG33:DB33=1))),IF(COLUMN(DC33)-MAX(COLUMN($AG33:DB33)*($AG33:DB33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DC33)-MAX(COLUMN($AG33:DB33)*($AG33:DB33=3))=$J33,3,0),IF(COLUMN(DC33)-MAX(COLUMN($AG33:DB33)*($AG33:DB33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DC33)*($AG33:DC33=1))>MAX(COLUMN($AG33:DC33)*($AG33:DC33=3)),MAX(COLUMN($AG33:DC33)*($AG33:DC33=1))>MAX(COLUMN($AG33:DC33)*($AG33:DC33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DD33)-MAX(COLUMN($AG33:DC33)*($AG33:DC33=1))=$J33,3,0),IF(COLUMN(DD33)-MAX(COLUMN($AG33:DC33)*($AG33:DC33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DC33)*($AG33:DC33=2))>MAX(COLUMN($AG33:DC33)*($AG33:DC33=3)),MAX(COLUMN($AG33:DC33)*($AG33:DC33=2))>MAX(COLUMN($AG33:DC33)*($AG33:DC33=1))),IF(COLUMN(DD33)-MAX(COLUMN($AG33:DC33)*($AG33:DC33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DD33)-MAX(COLUMN($AG33:DC33)*($AG33:DC33=3))=$J33,3,0),IF(COLUMN(DD33)-MAX(COLUMN($AG33:DC33)*($AG33:DC33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DD33)*($AG33:DD33=1))>MAX(COLUMN($AG33:DD33)*($AG33:DD33=3)),MAX(COLUMN($AG33:DD33)*($AG33:DD33=1))>MAX(COLUMN($AG33:DD33)*($AG33:DD33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DE33)-MAX(COLUMN($AG33:DD33)*($AG33:DD33=1))=$J33,3,0),IF(COLUMN(DE33)-MAX(COLUMN($AG33:DD33)*($AG33:DD33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DD33)*($AG33:DD33=2))>MAX(COLUMN($AG33:DD33)*($AG33:DD33=3)),MAX(COLUMN($AG33:DD33)*($AG33:DD33=2))>MAX(COLUMN($AG33:DD33)*($AG33:DD33=1))),IF(COLUMN(DE33)-MAX(COLUMN($AG33:DD33)*($AG33:DD33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DE33)-MAX(COLUMN($AG33:DD33)*($AG33:DD33=3))=$J33,3,0),IF(COLUMN(DE33)-MAX(COLUMN($AG33:DD33)*($AG33:DD33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DE33)*($AG33:DE33=1))>MAX(COLUMN($AG33:DE33)*($AG33:DE33=3)),MAX(COLUMN($AG33:DE33)*($AG33:DE33=1))>MAX(COLUMN($AG33:DE33)*($AG33:DE33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DF33)-MAX(COLUMN($AG33:DE33)*($AG33:DE33=1))=$J33,3,0),IF(COLUMN(DF33)-MAX(COLUMN($AG33:DE33)*($AG33:DE33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DE33)*($AG33:DE33=2))>MAX(COLUMN($AG33:DE33)*($AG33:DE33=3)),MAX(COLUMN($AG33:DE33)*($AG33:DE33=2))>MAX(COLUMN($AG33:DE33)*($AG33:DE33=1))),IF(COLUMN(DF33)-MAX(COLUMN($AG33:DE33)*($AG33:DE33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DF33)-MAX(COLUMN($AG33:DE33)*($AG33:DE33=3))=$J33,3,0),IF(COLUMN(DF33)-MAX(COLUMN($AG33:DE33)*($AG33:DE33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DF33)*($AG33:DF33=1))>MAX(COLUMN($AG33:DF33)*($AG33:DF33=3)),MAX(COLUMN($AG33:DF33)*($AG33:DF33=1))>MAX(COLUMN($AG33:DF33)*($AG33:DF33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DG33)-MAX(COLUMN($AG33:DF33)*($AG33:DF33=1))=$J33,3,0),IF(COLUMN(DG33)-MAX(COLUMN($AG33:DF33)*($AG33:DF33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DF33)*($AG33:DF33=2))>MAX(COLUMN($AG33:DF33)*($AG33:DF33=3)),MAX(COLUMN($AG33:DF33)*($AG33:DF33=2))>MAX(COLUMN($AG33:DF33)*($AG33:DF33=1))),IF(COLUMN(DG33)-MAX(COLUMN($AG33:DF33)*($AG33:DF33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DG33)-MAX(COLUMN($AG33:DF33)*($AG33:DF33=3))=$J33,3,0),IF(COLUMN(DG33)-MAX(COLUMN($AG33:DF33)*($AG33:DF33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DG33)*($AG33:DG33=1))>MAX(COLUMN($AG33:DG33)*($AG33:DG33=3)),MAX(COLUMN($AG33:DG33)*($AG33:DG33=1))>MAX(COLUMN($AG33:DG33)*($AG33:DG33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DH33)-MAX(COLUMN($AG33:DG33)*($AG33:DG33=1))=$J33,3,0),IF(COLUMN(DH33)-MAX(COLUMN($AG33:DG33)*($AG33:DG33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DG33)*($AG33:DG33=2))>MAX(COLUMN($AG33:DG33)*($AG33:DG33=3)),MAX(COLUMN($AG33:DG33)*($AG33:DG33=2))>MAX(COLUMN($AG33:DG33)*($AG33:DG33=1))),IF(COLUMN(DH33)-MAX(COLUMN($AG33:DG33)*($AG33:DG33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DH33)-MAX(COLUMN($AG33:DG33)*($AG33:DG33=3))=$J33,3,0),IF(COLUMN(DH33)-MAX(COLUMN($AG33:DG33)*($AG33:DG33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DH33)*($AG33:DH33=1))>MAX(COLUMN($AG33:DH33)*($AG33:DH33=3)),MAX(COLUMN($AG33:DH33)*($AG33:DH33=1))>MAX(COLUMN($AG33:DH33)*($AG33:DH33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DI33)-MAX(COLUMN($AG33:DH33)*($AG33:DH33=1))=$J33,3,0),IF(COLUMN(DI33)-MAX(COLUMN($AG33:DH33)*($AG33:DH33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DH33)*($AG33:DH33=2))>MAX(COLUMN($AG33:DH33)*($AG33:DH33=3)),MAX(COLUMN($AG33:DH33)*($AG33:DH33=2))>MAX(COLUMN($AG33:DH33)*($AG33:DH33=1))),IF(COLUMN(DI33)-MAX(COLUMN($AG33:DH33)*($AG33:DH33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DI33)-MAX(COLUMN($AG33:DH33)*($AG33:DH33=3))=$J33,3,0),IF(COLUMN(DI33)-MAX(COLUMN($AG33:DH33)*($AG33:DH33=3))=$J33,2,0)))))","v":2},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DI33)*($AG33:DI33=1))>MAX(COLUMN($AG33:DI33)*($AG33:DI33=3)),MAX(COLUMN($AG33:DI33)*($AG33:DI33=1))>MAX(COLUMN($AG33:DI33)*($AG33:DI33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DJ33)-MAX(COLUMN($AG33:DI33)*($AG33:DI33=1))=$J33,3,0),IF(COLUMN(DJ33)-MAX(COLUMN($AG33:DI33)*($AG33:DI33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DI33)*($AG33:DI33=2))>MAX(COLUMN($AG33:DI33)*($AG33:DI33=3)),MAX(COLUMN($AG33:DI33)*($AG33:DI33=2))>MAX(COLUMN($AG33:DI33)*($AG33:DI33=1))),IF(COLUMN(DJ33)-MAX(COLUMN($AG33:DI33)*($AG33:DI33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DJ33)-MAX(COLUMN($AG33:DI33)*($AG33:DI33=3))=$J33,3,0),IF(COLUMN(DJ33)-MAX(COLUMN($AG33:DI33)*($AG33:DI33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=1))>MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=3)),MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=1))>MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DK33)-MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=1))=$J33,3,0),IF(COLUMN(DK33)-MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=2))>MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=3)),MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=2))>MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=1))),IF(COLUMN(DK33)-MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DK33)-MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=3))=$J33,3,0),IF(COLUMN(DK33)-MAX(COLUMN($AG33:DJ33)*($AG33:DJ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DK33)*($AG33:DK33=1))>MAX(COLUMN($AG33:DK33)*($AG33:DK33=3)),MAX(COLUMN($AG33:DK33)*($AG33:DK33=1))>MAX(COLUMN($AG33:DK33)*($AG33:DK33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DL33)-MAX(COLUMN($AG33:DK33)*($AG33:DK33=1))=$J33,3,0),IF(COLUMN(DL33)-MAX(COLUMN($AG33:DK33)*($AG33:DK33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DK33)*($AG33:DK33=2))>MAX(COLUMN($AG33:DK33)*($AG33:DK33=3)),MAX(COLUMN($AG33:DK33)*($AG33:DK33=2))>MAX(COLUMN($AG33:DK33)*($AG33:DK33=1))),IF(COLUMN(DL33)-MAX(COLUMN($AG33:DK33)*($AG33:DK33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DL33)-MAX(COLUMN($AG33:DK33)*($AG33:DK33=3))=$J33,3,0),IF(COLUMN(DL33)-MAX(COLUMN($AG33:DK33)*($AG33:DK33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DL33)*($AG33:DL33=1))>MAX(COLUMN($AG33:DL33)*($AG33:DL33=3)),MAX(COLUMN($AG33:DL33)*($AG33:DL33=1))>MAX(COLUMN($AG33:DL33)*($AG33:DL33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DM33)-MAX(COLUMN($AG33:DL33)*($AG33:DL33=1))=$J33,3,0),IF(COLUMN(DM33)-MAX(COLUMN($AG33:DL33)*($AG33:DL33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DL33)*($AG33:DL33=2))>MAX(COLUMN($AG33:DL33)*($AG33:DL33=3)),MAX(COLUMN($AG33:DL33)*($AG33:DL33=2))>MAX(COLUMN($AG33:DL33)*($AG33:DL33=1))),IF(COLUMN(DM33)-MAX(COLUMN($AG33:DL33)*($AG33:DL33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DM33)-MAX(COLUMN($AG33:DL33)*($AG33:DL33=3))=$J33,3,0),IF(COLUMN(DM33)-MAX(COLUMN($AG33:DL33)*($AG33:DL33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DM33)*($AG33:DM33=1))>MAX(COLUMN($AG33:DM33)*($AG33:DM33=3)),MAX(COLUMN($AG33:DM33)*($AG33:DM33=1))>MAX(COLUMN($AG33:DM33)*($AG33:DM33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DN33)-MAX(COLUMN($AG33:DM33)*($AG33:DM33=1))=$J33,3,0),IF(COLUMN(DN33)-MAX(COLUMN($AG33:DM33)*($AG33:DM33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DM33)*($AG33:DM33=2))>MAX(COLUMN($AG33:DM33)*($AG33:DM33=3)),MAX(COLUMN($AG33:DM33)*($AG33:DM33=2))>MAX(COLUMN($AG33:DM33)*($AG33:DM33=1))),IF(COLUMN(DN33)-MAX(COLUMN($AG33:DM33)*($AG33:DM33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DN33)-MAX(COLUMN($AG33:DM33)*($AG33:DM33=3))=$J33,3,0),IF(COLUMN(DN33)-MAX(COLUMN($AG33:DM33)*($AG33:DM33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DN33)*($AG33:DN33=1))>MAX(COLUMN($AG33:DN33)*($AG33:DN33=3)),MAX(COLUMN($AG33:DN33)*($AG33:DN33=1))>MAX(COLUMN($AG33:DN33)*($AG33:DN33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DO33)-MAX(COLUMN($AG33:DN33)*($AG33:DN33=1))=$J33,3,0),IF(COLUMN(DO33)-MAX(COLUMN($AG33:DN33)*($AG33:DN33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DN33)*($AG33:DN33=2))>MAX(COLUMN($AG33:DN33)*($AG33:DN33=3)),MAX(COLUMN($AG33:DN33)*($AG33:DN33=2))>MAX(COLUMN($AG33:DN33)*($AG33:DN33=1))),IF(COLUMN(DO33)-MAX(COLUMN($AG33:DN33)*($AG33:DN33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DO33)-MAX(COLUMN($AG33:DN33)*($AG33:DN33=3))=$J33,3,0),IF(COLUMN(DO33)-MAX(COLUMN($AG33:DN33)*($AG33:DN33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DO33)*($AG33:DO33=1))>MAX(COLUMN($AG33:DO33)*($AG33:DO33=3)),MAX(COLUMN($AG33:DO33)*($AG33:DO33=1))>MAX(COLUMN($AG33:DO33)*($AG33:DO33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DP33)-MAX(COLUMN($AG33:DO33)*($AG33:DO33=1))=$J33,3,0),IF(COLUMN(DP33)-MAX(COLUMN($AG33:DO33)*($AG33:DO33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DO33)*($AG33:DO33=2))>MAX(COLUMN($AG33:DO33)*($AG33:DO33=3)),MAX(COLUMN($AG33:DO33)*($AG33:DO33=2))>MAX(COLUMN($AG33:DO33)*($AG33:DO33=1))),IF(COLUMN(DP33)-MAX(COLUMN($AG33:DO33)*($AG33:DO33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DP33)-MAX(COLUMN($AG33:DO33)*($AG33:DO33=3))=$J33,3,0),IF(COLUMN(DP33)-MAX(COLUMN($AG33:DO33)*($AG33:DO33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DP33)*($AG33:DP33=1))>MAX(COLUMN($AG33:DP33)*($AG33:DP33=3)),MAX(COLUMN($AG33:DP33)*($AG33:DP33=1))>MAX(COLUMN($AG33:DP33)*($AG33:DP33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DQ33)-MAX(COLUMN($AG33:DP33)*($AG33:DP33=1))=$J33,3,0),IF(COLUMN(DQ33)-MAX(COLUMN($AG33:DP33)*($AG33:DP33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DP33)*($AG33:DP33=2))>MAX(COLUMN($AG33:DP33)*($AG33:DP33=3)),MAX(COLUMN($AG33:DP33)*($AG33:DP33=2))>MAX(COLUMN($AG33:DP33)*($AG33:DP33=1))),IF(COLUMN(DQ33)-MAX(COLUMN($AG33:DP33)*($AG33:DP33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DQ33)-MAX(COLUMN($AG33:DP33)*($AG33:DP33=3))=$J33,3,0),IF(COLUMN(DQ33)-MAX(COLUMN($AG33:DP33)*($AG33:DP33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=1))>MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=3)),MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=1))>MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DR33)-MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=1))=$J33,3,0),IF(COLUMN(DR33)-MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=2))>MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=3)),MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=2))>MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=1))),IF(COLUMN(DR33)-MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DR33)-MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=3))=$J33,3,0),IF(COLUMN(DR33)-MAX(COLUMN($AG33:DQ33)*($AG33:DQ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DR33)*($AG33:DR33=1))>MAX(COLUMN($AG33:DR33)*($AG33:DR33=3)),MAX(COLUMN($AG33:DR33)*($AG33:DR33=1))>MAX(COLUMN($AG33:DR33)*($AG33:DR33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DS33)-MAX(COLUMN($AG33:DR33)*($AG33:DR33=1))=$J33,3,0),IF(COLUMN(DS33)-MAX(COLUMN($AG33:DR33)*($AG33:DR33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DR33)*($AG33:DR33=2))>MAX(COLUMN($AG33:DR33)*($AG33:DR33=3)),MAX(COLUMN($AG33:DR33)*($AG33:DR33=2))>MAX(COLUMN($AG33:DR33)*($AG33:DR33=1))),IF(COLUMN(DS33)-MAX(COLUMN($AG33:DR33)*($AG33:DR33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DS33)-MAX(COLUMN($AG33:DR33)*($AG33:DR33=3))=$J33,3,0),IF(COLUMN(DS33)-MAX(COLUMN($AG33:DR33)*($AG33:DR33=3))=$J33,2,0)))))","v":3},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DS33)*($AG33:DS33=1))>MAX(COLUMN($AG33:DS33)*($AG33:DS33=3)),MAX(COLUMN($AG33:DS33)*($AG33:DS33=1))>MAX(COLUMN($AG33:DS33)*($AG33:DS33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DT33)-MAX(COLUMN($AG33:DS33)*($AG33:DS33=1))=$J33,3,0),IF(COLUMN(DT33)-MAX(COLUMN($AG33:DS33)*($AG33:DS33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DS33)*($AG33:DS33=2))>MAX(COLUMN($AG33:DS33)*($AG33:DS33=3)),MAX(COLUMN($AG33:DS33)*($AG33:DS33=2))>MAX(COLUMN($AG33:DS33)*($AG33:DS33=1))),IF(COLUMN(DT33)-MAX(COLUMN($AG33:DS33)*($AG33:DS33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DT33)-MAX(COLUMN($AG33:DS33)*($AG33:DS33=3))=$J33,3,0),IF(COLUMN(DT33)-MAX(COLUMN($AG33:DS33)*($AG33:DS33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DT33)*($AG33:DT33=1))>MAX(COLUMN($AG33:DT33)*($AG33:DT33=3)),MAX(COLUMN($AG33:DT33)*($AG33:DT33=1))>MAX(COLUMN($AG33:DT33)*($AG33:DT33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DU33)-MAX(COLUMN($AG33:DT33)*($AG33:DT33=1))=$J33,3,0),IF(COLUMN(DU33)-MAX(COLUMN($AG33:DT33)*($AG33:DT33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DT33)*($AG33:DT33=2))>MAX(COLUMN($AG33:DT33)*($AG33:DT33=3)),MAX(COLUMN($AG33:DT33)*($AG33:DT33=2))>MAX(COLUMN($AG33:DT33)*($AG33:DT33=1))),IF(COLUMN(DU33)-MAX(COLUMN($AG33:DT33)*($AG33:DT33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DU33)-MAX(COLUMN($AG33:DT33)*($AG33:DT33=3))=$J33,3,0),IF(COLUMN(DU33)-MAX(COLUMN($AG33:DT33)*($AG33:DT33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DU33)*($AG33:DU33=1))>MAX(COLUMN($AG33:DU33)*($AG33:DU33=3)),MAX(COLUMN($AG33:DU33)*($AG33:DU33=1))>MAX(COLUMN($AG33:DU33)*($AG33:DU33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DV33)-MAX(COLUMN($AG33:DU33)*($AG33:DU33=1))=$J33,3,0),IF(COLUMN(DV33)-MAX(COLUMN($AG33:DU33)*($AG33:DU33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DU33)*($AG33:DU33=2))>MAX(COLUMN($AG33:DU33)*($AG33:DU33=3)),MAX(COLUMN($AG33:DU33)*($AG33:DU33=2))>MAX(COLUMN($AG33:DU33)*($AG33:DU33=1))),IF(COLUMN(DV33)-MAX(COLUMN($AG33:DU33)*($AG33:DU33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DV33)-MAX(COLUMN($AG33:DU33)*($AG33:DU33=3))=$J33,3,0),IF(COLUMN(DV33)-MAX(COLUMN($AG33:DU33)*($AG33:DU33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DV33)*($AG33:DV33=1))>MAX(COLUMN($AG33:DV33)*($AG33:DV33=3)),MAX(COLUMN($AG33:DV33)*($AG33:DV33=1))>MAX(COLUMN($AG33:DV33)*($AG33:DV33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DW33)-MAX(COLUMN($AG33:DV33)*($AG33:DV33=1))=$J33,3,0),IF(COLUMN(DW33)-MAX(COLUMN($AG33:DV33)*($AG33:DV33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DV33)*($AG33:DV33=2))>MAX(COLUMN($AG33:DV33)*($AG33:DV33=3)),MAX(COLUMN($AG33:DV33)*($AG33:DV33=2))>MAX(COLUMN($AG33:DV33)*($AG33:DV33=1))),IF(COLUMN(DW33)-MAX(COLUMN($AG33:DV33)*($AG33:DV33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DW33)-MAX(COLUMN($AG33:DV33)*($AG33:DV33=3))=$J33,3,0),IF(COLUMN(DW33)-MAX(COLUMN($AG33:DV33)*($AG33:DV33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DW33)*($AG33:DW33=1))>MAX(COLUMN($AG33:DW33)*($AG33:DW33=3)),MAX(COLUMN($AG33:DW33)*($AG33:DW33=1))>MAX(COLUMN($AG33:DW33)*($AG33:DW33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DX33)-MAX(COLUMN($AG33:DW33)*($AG33:DW33=1))=$J33,3,0),IF(COLUMN(DX33)-MAX(COLUMN($AG33:DW33)*($AG33:DW33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DW33)*($AG33:DW33=2))>MAX(COLUMN($AG33:DW33)*($AG33:DW33=3)),MAX(COLUMN($AG33:DW33)*($AG33:DW33=2))>MAX(COLUMN($AG33:DW33)*($AG33:DW33=1))),IF(COLUMN(DX33)-MAX(COLUMN($AG33:DW33)*($AG33:DW33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DX33)-MAX(COLUMN($AG33:DW33)*($AG33:DW33=3))=$J33,3,0),IF(COLUMN(DX33)-MAX(COLUMN($AG33:DW33)*($AG33:DW33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DX33)*($AG33:DX33=1))>MAX(COLUMN($AG33:DX33)*($AG33:DX33=3)),MAX(COLUMN($AG33:DX33)*($AG33:DX33=1))>MAX(COLUMN($AG33:DX33)*($AG33:DX33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DY33)-MAX(COLUMN($AG33:DX33)*($AG33:DX33=1))=$J33,3,0),IF(COLUMN(DY33)-MAX(COLUMN($AG33:DX33)*($AG33:DX33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DX33)*($AG33:DX33=2))>MAX(COLUMN($AG33:DX33)*($AG33:DX33=3)),MAX(COLUMN($AG33:DX33)*($AG33:DX33=2))>MAX(COLUMN($AG33:DX33)*($AG33:DX33=1))),IF(COLUMN(DY33)-MAX(COLUMN($AG33:DX33)*($AG33:DX33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DY33)-MAX(COLUMN($AG33:DX33)*($AG33:DX33=3))=$J33,3,0),IF(COLUMN(DY33)-MAX(COLUMN($AG33:DX33)*($AG33:DX33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DY33)*($AG33:DY33=1))>MAX(COLUMN($AG33:DY33)*($AG33:DY33=3)),MAX(COLUMN($AG33:DY33)*($AG33:DY33=1))>MAX(COLUMN($AG33:DY33)*($AG33:DY33=2))),IF($K33=\"Not Possible\",IF(COLUMN(DZ33)-MAX(COLUMN($AG33:DY33)*($AG33:DY33=1))=$J33,3,0),IF(COLUMN(DZ33)-MAX(COLUMN($AG33:DY33)*($AG33:DY33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DY33)*($AG33:DY33=2))>MAX(COLUMN($AG33:DY33)*($AG33:DY33=3)),MAX(COLUMN($AG33:DY33)*($AG33:DY33=2))>MAX(COLUMN($AG33:DY33)*($AG33:DY33=1))),IF(COLUMN(DZ33)-MAX(COLUMN($AG33:DY33)*($AG33:DY33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(DZ33)-MAX(COLUMN($AG33:DY33)*($AG33:DY33=3))=$J33,3,0),IF(COLUMN(DZ33)-MAX(COLUMN($AG33:DY33)*($AG33:DY33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=1))>MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=3)),MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=1))>MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=2))),IF($K33=\"Not Possible\",IF(COLUMN(EA33)-MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=1))=$J33,3,0),IF(COLUMN(EA33)-MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=2))>MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=3)),MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=2))>MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=1))),IF(COLUMN(EA33)-MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(EA33)-MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=3))=$J33,3,0),IF(COLUMN(EA33)-MAX(COLUMN($AG33:DZ33)*($AG33:DZ33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:EA33)*($AG33:EA33=1))>MAX(COLUMN($AG33:EA33)*($AG33:EA33=3)),MAX(COLUMN($AG33:EA33)*($AG33:EA33=1))>MAX(COLUMN($AG33:EA33)*($AG33:EA33=2))),IF($K33=\"Not Possible\",IF(COLUMN(EB33)-MAX(COLUMN($AG33:EA33)*($AG33:EA33=1))=$J33,3,0),IF(COLUMN(EB33)-MAX(COLUMN($AG33:EA33)*($AG33:EA33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:EA33)*($AG33:EA33=2))>MAX(COLUMN($AG33:EA33)*($AG33:EA33=3)),MAX(COLUMN($AG33:EA33)*($AG33:EA33=2))>MAX(COLUMN($AG33:EA33)*($AG33:EA33=1))),IF(COLUMN(EB33)-MAX(COLUMN($AG33:EA33)*($AG33:EA33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(EB33)-MAX(COLUMN($AG33:EA33)*($AG33:EA33=3))=$J33,3,0),IF(COLUMN(EB33)-MAX(COLUMN($AG33:EA33)*($AG33:EA33=3))=$J33,2,0)))))","v":0},{"$f":"IF($AG33=4,0,IF(AND(MAX(COLUMN($AG33:EB33)*($AG33:EB33=1))>MAX(COLUMN($AG33:EB33)*($AG33:EB33=3)),MAX(COLUMN($AG33:EB33)*($AG33:EB33=1))>MAX(COLUMN($AG33:EB33)*($AG33:EB33=2))),IF($K33=\"Not Possible\",IF(COLUMN(EC33)-MAX(COLUMN($AG33:EB33)*($AG33:EB33=1))=$J33,3,0),IF(COLUMN(EC33)-MAX(COLUMN($AG33:EB33)*($AG33:EB33=1))=$J33,2,0)),IF(AND(MAX(COLUMN($AG33:EB33)*($AG33:EB33=2))>MAX(COLUMN($AG33:EB33)*($AG33:EB33=3)),MAX(COLUMN($AG33:EB33)*($AG33:EB33=2))>MAX(COLUMN($AG33:EB33)*($AG33:EB33=1))),IF(COLUMN(EC33)-MAX(COLUMN($AG33:EB33)*($AG33:EB33=2))=$L33,3,0),IF($K33=\"Not Possible\",IF(COLUMN(EC33)-MAX(COLUMN($AG33:EB33)*($AG33:EB33=3))=$J33,3,0),IF(COLUMN(EC33)-MAX(COLUMN($AG33:EB33)*($AG33:EB33=3))=$J33,2,0)))))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"BridEA03"},"Footbridge",{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset class],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"Bridge - Pedestrian"},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",Form_Asset[[#This Row],[Asset ID]]&ROW())","v":"BridEA0334"},"Abutment","Headwall",{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",INDEX(AssetListTbl[Best Estimate Life (5)],(MATCH(Form_Asset[[#This Row],[Sub-Asset category]],AssetListTbl[Sub-Element Category],0))))","v":80},60,"Moderate Refurbishment",40,"New Build",{"$f":"MAX(COLUMN($AH34:EC34)*($AH34:EC34=2))","v":93},{"$f":"MAX(COLUMN($AH34:EC34)*($AH34:EC34=3))","v":133},{"$f":"IFERROR(100-(IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Replace]])),INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Refurb]])))),0)","v":100},{"$f":"IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],3,2)","v":3},{"$f":"SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Product_Stage[CO2e (t)])","v":27.229103999999996},{"$f":"IFERROR(SUM(Form_Elements[General Item Material])*(Form_Asset[[#This Row],[Weighted Split]]/SUM(Form_Asset[Weighted Split]))+Form_Asset[[#This Row],[Weighted Split]],0)","v":27.229103999999996},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth (wtt)]))+(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Transport]))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0.22829150779999999},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Non contractor People Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Contractor people transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0.15109149233164604},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":3.989534392180724E-3},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Site establishment])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0.16987948519616625},{"$f":"IFERROR(IF($D$88=\"Summary\",((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),(SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Const_Ins_InsB[CO2e (t)]))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Other Construction Waste])*Form_Asset[[#This Row],[Weighted Split]]/(SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[[Waste Co2e ]])+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":7.3895334888847489E-2},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New build\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]]),IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",(SUM(Form_Asset[[#This Row],[Materials]:[Waste]])-(SUM(Form_Asset[[#This Row],[Materials Transport]],Form_Asset[[#This Row],[People Transport]]*0.5,Form_Asset[[#This Row],[Plant Transport]]*0.5))),IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]])/(SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%])),0)))","v":27.856251354608833},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":1.6922118939751794E-3},{"$f":"IFERROR(SUMIF(Form_use_energy[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_use_energy[CO2e (t)]),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset ref.]]=\"\",0,SUMIF(Form_Asset[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Asset[New Build Co2e])*SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%]))","v":6.9640628386522083},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Dem - General Item Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Dem -Waste Co2e]),0)","v":0.41874023103680236},{"$f":"(Form_Asset[[#This Row],[Plant use]]+Form_Asset[[#This Row],[Plant Transport]])*50%","v":1.994767196090362E-3},{"$f":"Form_Asset[[#This Row],[People Transport]]*50%","v":7.5545746165823019E-2},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New Build\",1,IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",2,IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",3,IF(Form_Asset[[#This Row],[First intervention]]=\"Demolition\",4,\"\"))))","v":1},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AG34)*($AG34:AG34=1))>MAX(COLUMN($AG34:AG34)*($AG34:AG34=3)),MAX(COLUMN($AG34:AG34)*($AG34:AG34=1))>MAX(COLUMN($AG34:AG34)*($AG34:AG34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AH34)-MAX(COLUMN($AG34:AG34)*($AG34:AG34=1))=$J34,3,0),IF(COLUMN(AH34)-MAX(COLUMN($AG34:AG34)*($AG34:AG34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AG34)*($AG34:AG34=2))>MAX(COLUMN($AG34:AG34)*($AG34:AG34=3)),MAX(COLUMN($AG34:AG34)*($AG34:AG34=2))>MAX(COLUMN($AG34:AG34)*($AG34:AG34=1))),IF(COLUMN(AH34)-MAX(COLUMN($AG34:AG34)*($AG34:AG34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AH34)-MAX(COLUMN($AG34:AG34)*($AG34:AG34=3))=$J34,3,0),IF(COLUMN(AH34)-MAX(COLUMN($AG34:AG34)*($AG34:AG34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AH34)*($AG34:AH34=1))>MAX(COLUMN($AG34:AH34)*($AG34:AH34=3)),MAX(COLUMN($AG34:AH34)*($AG34:AH34=1))>MAX(COLUMN($AG34:AH34)*($AG34:AH34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AI34)-MAX(COLUMN($AG34:AH34)*($AG34:AH34=1))=$J34,3,0),IF(COLUMN(AI34)-MAX(COLUMN($AG34:AH34)*($AG34:AH34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AH34)*($AG34:AH34=2))>MAX(COLUMN($AG34:AH34)*($AG34:AH34=3)),MAX(COLUMN($AG34:AH34)*($AG34:AH34=2))>MAX(COLUMN($AG34:AH34)*($AG34:AH34=1))),IF(COLUMN(AI34)-MAX(COLUMN($AG34:AH34)*($AG34:AH34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AI34)-MAX(COLUMN($AG34:AH34)*($AG34:AH34=3))=$J34,3,0),IF(COLUMN(AI34)-MAX(COLUMN($AG34:AH34)*($AG34:AH34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AI34)*($AG34:AI34=1))>MAX(COLUMN($AG34:AI34)*($AG34:AI34=3)),MAX(COLUMN($AG34:AI34)*($AG34:AI34=1))>MAX(COLUMN($AG34:AI34)*($AG34:AI34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AJ34)-MAX(COLUMN($AG34:AI34)*($AG34:AI34=1))=$J34,3,0),IF(COLUMN(AJ34)-MAX(COLUMN($AG34:AI34)*($AG34:AI34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AI34)*($AG34:AI34=2))>MAX(COLUMN($AG34:AI34)*($AG34:AI34=3)),MAX(COLUMN($AG34:AI34)*($AG34:AI34=2))>MAX(COLUMN($AG34:AI34)*($AG34:AI34=1))),IF(COLUMN(AJ34)-MAX(COLUMN($AG34:AI34)*($AG34:AI34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AJ34)-MAX(COLUMN($AG34:AI34)*($AG34:AI34=3))=$J34,3,0),IF(COLUMN(AJ34)-MAX(COLUMN($AG34:AI34)*($AG34:AI34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=1))>MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=3)),MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=1))>MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AK34)-MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=1))=$J34,3,0),IF(COLUMN(AK34)-MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=2))>MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=3)),MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=2))>MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=1))),IF(COLUMN(AK34)-MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AK34)-MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=3))=$J34,3,0),IF(COLUMN(AK34)-MAX(COLUMN($AG34:AJ34)*($AG34:AJ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AK34)*($AG34:AK34=1))>MAX(COLUMN($AG34:AK34)*($AG34:AK34=3)),MAX(COLUMN($AG34:AK34)*($AG34:AK34=1))>MAX(COLUMN($AG34:AK34)*($AG34:AK34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AL34)-MAX(COLUMN($AG34:AK34)*($AG34:AK34=1))=$J34,3,0),IF(COLUMN(AL34)-MAX(COLUMN($AG34:AK34)*($AG34:AK34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AK34)*($AG34:AK34=2))>MAX(COLUMN($AG34:AK34)*($AG34:AK34=3)),MAX(COLUMN($AG34:AK34)*($AG34:AK34=2))>MAX(COLUMN($AG34:AK34)*($AG34:AK34=1))),IF(COLUMN(AL34)-MAX(COLUMN($AG34:AK34)*($AG34:AK34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AL34)-MAX(COLUMN($AG34:AK34)*($AG34:AK34=3))=$J34,3,0),IF(COLUMN(AL34)-MAX(COLUMN($AG34:AK34)*($AG34:AK34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AL34)*($AG34:AL34=1))>MAX(COLUMN($AG34:AL34)*($AG34:AL34=3)),MAX(COLUMN($AG34:AL34)*($AG34:AL34=1))>MAX(COLUMN($AG34:AL34)*($AG34:AL34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AM34)-MAX(COLUMN($AG34:AL34)*($AG34:AL34=1))=$J34,3,0),IF(COLUMN(AM34)-MAX(COLUMN($AG34:AL34)*($AG34:AL34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AL34)*($AG34:AL34=2))>MAX(COLUMN($AG34:AL34)*($AG34:AL34=3)),MAX(COLUMN($AG34:AL34)*($AG34:AL34=2))>MAX(COLUMN($AG34:AL34)*($AG34:AL34=1))),IF(COLUMN(AM34)-MAX(COLUMN($AG34:AL34)*($AG34:AL34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AM34)-MAX(COLUMN($AG34:AL34)*($AG34:AL34=3))=$J34,3,0),IF(COLUMN(AM34)-MAX(COLUMN($AG34:AL34)*($AG34:AL34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AM34)*($AG34:AM34=1))>MAX(COLUMN($AG34:AM34)*($AG34:AM34=3)),MAX(COLUMN($AG34:AM34)*($AG34:AM34=1))>MAX(COLUMN($AG34:AM34)*($AG34:AM34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AN34)-MAX(COLUMN($AG34:AM34)*($AG34:AM34=1))=$J34,3,0),IF(COLUMN(AN34)-MAX(COLUMN($AG34:AM34)*($AG34:AM34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AM34)*($AG34:AM34=2))>MAX(COLUMN($AG34:AM34)*($AG34:AM34=3)),MAX(COLUMN($AG34:AM34)*($AG34:AM34=2))>MAX(COLUMN($AG34:AM34)*($AG34:AM34=1))),IF(COLUMN(AN34)-MAX(COLUMN($AG34:AM34)*($AG34:AM34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AN34)-MAX(COLUMN($AG34:AM34)*($AG34:AM34=3))=$J34,3,0),IF(COLUMN(AN34)-MAX(COLUMN($AG34:AM34)*($AG34:AM34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AN34)*($AG34:AN34=1))>MAX(COLUMN($AG34:AN34)*($AG34:AN34=3)),MAX(COLUMN($AG34:AN34)*($AG34:AN34=1))>MAX(COLUMN($AG34:AN34)*($AG34:AN34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AO34)-MAX(COLUMN($AG34:AN34)*($AG34:AN34=1))=$J34,3,0),IF(COLUMN(AO34)-MAX(COLUMN($AG34:AN34)*($AG34:AN34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AN34)*($AG34:AN34=2))>MAX(COLUMN($AG34:AN34)*($AG34:AN34=3)),MAX(COLUMN($AG34:AN34)*($AG34:AN34=2))>MAX(COLUMN($AG34:AN34)*($AG34:AN34=1))),IF(COLUMN(AO34)-MAX(COLUMN($AG34:AN34)*($AG34:AN34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AO34)-MAX(COLUMN($AG34:AN34)*($AG34:AN34=3))=$J34,3,0),IF(COLUMN(AO34)-MAX(COLUMN($AG34:AN34)*($AG34:AN34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AO34)*($AG34:AO34=1))>MAX(COLUMN($AG34:AO34)*($AG34:AO34=3)),MAX(COLUMN($AG34:AO34)*($AG34:AO34=1))>MAX(COLUMN($AG34:AO34)*($AG34:AO34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AP34)-MAX(COLUMN($AG34:AO34)*($AG34:AO34=1))=$J34,3,0),IF(COLUMN(AP34)-MAX(COLUMN($AG34:AO34)*($AG34:AO34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AO34)*($AG34:AO34=2))>MAX(COLUMN($AG34:AO34)*($AG34:AO34=3)),MAX(COLUMN($AG34:AO34)*($AG34:AO34=2))>MAX(COLUMN($AG34:AO34)*($AG34:AO34=1))),IF(COLUMN(AP34)-MAX(COLUMN($AG34:AO34)*($AG34:AO34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AP34)-MAX(COLUMN($AG34:AO34)*($AG34:AO34=3))=$J34,3,0),IF(COLUMN(AP34)-MAX(COLUMN($AG34:AO34)*($AG34:AO34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AP34)*($AG34:AP34=1))>MAX(COLUMN($AG34:AP34)*($AG34:AP34=3)),MAX(COLUMN($AG34:AP34)*($AG34:AP34=1))>MAX(COLUMN($AG34:AP34)*($AG34:AP34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AQ34)-MAX(COLUMN($AG34:AP34)*($AG34:AP34=1))=$J34,3,0),IF(COLUMN(AQ34)-MAX(COLUMN($AG34:AP34)*($AG34:AP34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AP34)*($AG34:AP34=2))>MAX(COLUMN($AG34:AP34)*($AG34:AP34=3)),MAX(COLUMN($AG34:AP34)*($AG34:AP34=2))>MAX(COLUMN($AG34:AP34)*($AG34:AP34=1))),IF(COLUMN(AQ34)-MAX(COLUMN($AG34:AP34)*($AG34:AP34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AQ34)-MAX(COLUMN($AG34:AP34)*($AG34:AP34=3))=$J34,3,0),IF(COLUMN(AQ34)-MAX(COLUMN($AG34:AP34)*($AG34:AP34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=1))>MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=3)),MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=1))>MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AR34)-MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=1))=$J34,3,0),IF(COLUMN(AR34)-MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=2))>MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=3)),MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=2))>MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=1))),IF(COLUMN(AR34)-MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AR34)-MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=3))=$J34,3,0),IF(COLUMN(AR34)-MAX(COLUMN($AG34:AQ34)*($AG34:AQ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AR34)*($AG34:AR34=1))>MAX(COLUMN($AG34:AR34)*($AG34:AR34=3)),MAX(COLUMN($AG34:AR34)*($AG34:AR34=1))>MAX(COLUMN($AG34:AR34)*($AG34:AR34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AS34)-MAX(COLUMN($AG34:AR34)*($AG34:AR34=1))=$J34,3,0),IF(COLUMN(AS34)-MAX(COLUMN($AG34:AR34)*($AG34:AR34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AR34)*($AG34:AR34=2))>MAX(COLUMN($AG34:AR34)*($AG34:AR34=3)),MAX(COLUMN($AG34:AR34)*($AG34:AR34=2))>MAX(COLUMN($AG34:AR34)*($AG34:AR34=1))),IF(COLUMN(AS34)-MAX(COLUMN($AG34:AR34)*($AG34:AR34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AS34)-MAX(COLUMN($AG34:AR34)*($AG34:AR34=3))=$J34,3,0),IF(COLUMN(AS34)-MAX(COLUMN($AG34:AR34)*($AG34:AR34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AS34)*($AG34:AS34=1))>MAX(COLUMN($AG34:AS34)*($AG34:AS34=3)),MAX(COLUMN($AG34:AS34)*($AG34:AS34=1))>MAX(COLUMN($AG34:AS34)*($AG34:AS34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AT34)-MAX(COLUMN($AG34:AS34)*($AG34:AS34=1))=$J34,3,0),IF(COLUMN(AT34)-MAX(COLUMN($AG34:AS34)*($AG34:AS34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AS34)*($AG34:AS34=2))>MAX(COLUMN($AG34:AS34)*($AG34:AS34=3)),MAX(COLUMN($AG34:AS34)*($AG34:AS34=2))>MAX(COLUMN($AG34:AS34)*($AG34:AS34=1))),IF(COLUMN(AT34)-MAX(COLUMN($AG34:AS34)*($AG34:AS34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AT34)-MAX(COLUMN($AG34:AS34)*($AG34:AS34=3))=$J34,3,0),IF(COLUMN(AT34)-MAX(COLUMN($AG34:AS34)*($AG34:AS34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AT34)*($AG34:AT34=1))>MAX(COLUMN($AG34:AT34)*($AG34:AT34=3)),MAX(COLUMN($AG34:AT34)*($AG34:AT34=1))>MAX(COLUMN($AG34:AT34)*($AG34:AT34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AU34)-MAX(COLUMN($AG34:AT34)*($AG34:AT34=1))=$J34,3,0),IF(COLUMN(AU34)-MAX(COLUMN($AG34:AT34)*($AG34:AT34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AT34)*($AG34:AT34=2))>MAX(COLUMN($AG34:AT34)*($AG34:AT34=3)),MAX(COLUMN($AG34:AT34)*($AG34:AT34=2))>MAX(COLUMN($AG34:AT34)*($AG34:AT34=1))),IF(COLUMN(AU34)-MAX(COLUMN($AG34:AT34)*($AG34:AT34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AU34)-MAX(COLUMN($AG34:AT34)*($AG34:AT34=3))=$J34,3,0),IF(COLUMN(AU34)-MAX(COLUMN($AG34:AT34)*($AG34:AT34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AU34)*($AG34:AU34=1))>MAX(COLUMN($AG34:AU34)*($AG34:AU34=3)),MAX(COLUMN($AG34:AU34)*($AG34:AU34=1))>MAX(COLUMN($AG34:AU34)*($AG34:AU34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AV34)-MAX(COLUMN($AG34:AU34)*($AG34:AU34=1))=$J34,3,0),IF(COLUMN(AV34)-MAX(COLUMN($AG34:AU34)*($AG34:AU34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AU34)*($AG34:AU34=2))>MAX(COLUMN($AG34:AU34)*($AG34:AU34=3)),MAX(COLUMN($AG34:AU34)*($AG34:AU34=2))>MAX(COLUMN($AG34:AU34)*($AG34:AU34=1))),IF(COLUMN(AV34)-MAX(COLUMN($AG34:AU34)*($AG34:AU34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AV34)-MAX(COLUMN($AG34:AU34)*($AG34:AU34=3))=$J34,3,0),IF(COLUMN(AV34)-MAX(COLUMN($AG34:AU34)*($AG34:AU34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AV34)*($AG34:AV34=1))>MAX(COLUMN($AG34:AV34)*($AG34:AV34=3)),MAX(COLUMN($AG34:AV34)*($AG34:AV34=1))>MAX(COLUMN($AG34:AV34)*($AG34:AV34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AW34)-MAX(COLUMN($AG34:AV34)*($AG34:AV34=1))=$J34,3,0),IF(COLUMN(AW34)-MAX(COLUMN($AG34:AV34)*($AG34:AV34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AV34)*($AG34:AV34=2))>MAX(COLUMN($AG34:AV34)*($AG34:AV34=3)),MAX(COLUMN($AG34:AV34)*($AG34:AV34=2))>MAX(COLUMN($AG34:AV34)*($AG34:AV34=1))),IF(COLUMN(AW34)-MAX(COLUMN($AG34:AV34)*($AG34:AV34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AW34)-MAX(COLUMN($AG34:AV34)*($AG34:AV34=3))=$J34,3,0),IF(COLUMN(AW34)-MAX(COLUMN($AG34:AV34)*($AG34:AV34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AW34)*($AG34:AW34=1))>MAX(COLUMN($AG34:AW34)*($AG34:AW34=3)),MAX(COLUMN($AG34:AW34)*($AG34:AW34=1))>MAX(COLUMN($AG34:AW34)*($AG34:AW34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AX34)-MAX(COLUMN($AG34:AW34)*($AG34:AW34=1))=$J34,3,0),IF(COLUMN(AX34)-MAX(COLUMN($AG34:AW34)*($AG34:AW34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AW34)*($AG34:AW34=2))>MAX(COLUMN($AG34:AW34)*($AG34:AW34=3)),MAX(COLUMN($AG34:AW34)*($AG34:AW34=2))>MAX(COLUMN($AG34:AW34)*($AG34:AW34=1))),IF(COLUMN(AX34)-MAX(COLUMN($AG34:AW34)*($AG34:AW34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AX34)-MAX(COLUMN($AG34:AW34)*($AG34:AW34=3))=$J34,3,0),IF(COLUMN(AX34)-MAX(COLUMN($AG34:AW34)*($AG34:AW34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AX34)*($AG34:AX34=1))>MAX(COLUMN($AG34:AX34)*($AG34:AX34=3)),MAX(COLUMN($AG34:AX34)*($AG34:AX34=1))>MAX(COLUMN($AG34:AX34)*($AG34:AX34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AY34)-MAX(COLUMN($AG34:AX34)*($AG34:AX34=1))=$J34,3,0),IF(COLUMN(AY34)-MAX(COLUMN($AG34:AX34)*($AG34:AX34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AX34)*($AG34:AX34=2))>MAX(COLUMN($AG34:AX34)*($AG34:AX34=3)),MAX(COLUMN($AG34:AX34)*($AG34:AX34=2))>MAX(COLUMN($AG34:AX34)*($AG34:AX34=1))),IF(COLUMN(AY34)-MAX(COLUMN($AG34:AX34)*($AG34:AX34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AY34)-MAX(COLUMN($AG34:AX34)*($AG34:AX34=3))=$J34,3,0),IF(COLUMN(AY34)-MAX(COLUMN($AG34:AX34)*($AG34:AX34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AY34)*($AG34:AY34=1))>MAX(COLUMN($AG34:AY34)*($AG34:AY34=3)),MAX(COLUMN($AG34:AY34)*($AG34:AY34=1))>MAX(COLUMN($AG34:AY34)*($AG34:AY34=2))),IF($K34=\"Not Possible\",IF(COLUMN(AZ34)-MAX(COLUMN($AG34:AY34)*($AG34:AY34=1))=$J34,3,0),IF(COLUMN(AZ34)-MAX(COLUMN($AG34:AY34)*($AG34:AY34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AY34)*($AG34:AY34=2))>MAX(COLUMN($AG34:AY34)*($AG34:AY34=3)),MAX(COLUMN($AG34:AY34)*($AG34:AY34=2))>MAX(COLUMN($AG34:AY34)*($AG34:AY34=1))),IF(COLUMN(AZ34)-MAX(COLUMN($AG34:AY34)*($AG34:AY34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(AZ34)-MAX(COLUMN($AG34:AY34)*($AG34:AY34=3))=$J34,3,0),IF(COLUMN(AZ34)-MAX(COLUMN($AG34:AY34)*($AG34:AY34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=1))>MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=3)),MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=1))>MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BA34)-MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=1))=$J34,3,0),IF(COLUMN(BA34)-MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=2))>MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=3)),MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=2))>MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=1))),IF(COLUMN(BA34)-MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BA34)-MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=3))=$J34,3,0),IF(COLUMN(BA34)-MAX(COLUMN($AG34:AZ34)*($AG34:AZ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BA34)*($AG34:BA34=1))>MAX(COLUMN($AG34:BA34)*($AG34:BA34=3)),MAX(COLUMN($AG34:BA34)*($AG34:BA34=1))>MAX(COLUMN($AG34:BA34)*($AG34:BA34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BB34)-MAX(COLUMN($AG34:BA34)*($AG34:BA34=1))=$J34,3,0),IF(COLUMN(BB34)-MAX(COLUMN($AG34:BA34)*($AG34:BA34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BA34)*($AG34:BA34=2))>MAX(COLUMN($AG34:BA34)*($AG34:BA34=3)),MAX(COLUMN($AG34:BA34)*($AG34:BA34=2))>MAX(COLUMN($AG34:BA34)*($AG34:BA34=1))),IF(COLUMN(BB34)-MAX(COLUMN($AG34:BA34)*($AG34:BA34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BB34)-MAX(COLUMN($AG34:BA34)*($AG34:BA34=3))=$J34,3,0),IF(COLUMN(BB34)-MAX(COLUMN($AG34:BA34)*($AG34:BA34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BB34)*($AG34:BB34=1))>MAX(COLUMN($AG34:BB34)*($AG34:BB34=3)),MAX(COLUMN($AG34:BB34)*($AG34:BB34=1))>MAX(COLUMN($AG34:BB34)*($AG34:BB34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BC34)-MAX(COLUMN($AG34:BB34)*($AG34:BB34=1))=$J34,3,0),IF(COLUMN(BC34)-MAX(COLUMN($AG34:BB34)*($AG34:BB34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BB34)*($AG34:BB34=2))>MAX(COLUMN($AG34:BB34)*($AG34:BB34=3)),MAX(COLUMN($AG34:BB34)*($AG34:BB34=2))>MAX(COLUMN($AG34:BB34)*($AG34:BB34=1))),IF(COLUMN(BC34)-MAX(COLUMN($AG34:BB34)*($AG34:BB34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BC34)-MAX(COLUMN($AG34:BB34)*($AG34:BB34=3))=$J34,3,0),IF(COLUMN(BC34)-MAX(COLUMN($AG34:BB34)*($AG34:BB34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BC34)*($AG34:BC34=1))>MAX(COLUMN($AG34:BC34)*($AG34:BC34=3)),MAX(COLUMN($AG34:BC34)*($AG34:BC34=1))>MAX(COLUMN($AG34:BC34)*($AG34:BC34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BD34)-MAX(COLUMN($AG34:BC34)*($AG34:BC34=1))=$J34,3,0),IF(COLUMN(BD34)-MAX(COLUMN($AG34:BC34)*($AG34:BC34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BC34)*($AG34:BC34=2))>MAX(COLUMN($AG34:BC34)*($AG34:BC34=3)),MAX(COLUMN($AG34:BC34)*($AG34:BC34=2))>MAX(COLUMN($AG34:BC34)*($AG34:BC34=1))),IF(COLUMN(BD34)-MAX(COLUMN($AG34:BC34)*($AG34:BC34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BD34)-MAX(COLUMN($AG34:BC34)*($AG34:BC34=3))=$J34,3,0),IF(COLUMN(BD34)-MAX(COLUMN($AG34:BC34)*($AG34:BC34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BD34)*($AG34:BD34=1))>MAX(COLUMN($AG34:BD34)*($AG34:BD34=3)),MAX(COLUMN($AG34:BD34)*($AG34:BD34=1))>MAX(COLUMN($AG34:BD34)*($AG34:BD34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BE34)-MAX(COLUMN($AG34:BD34)*($AG34:BD34=1))=$J34,3,0),IF(COLUMN(BE34)-MAX(COLUMN($AG34:BD34)*($AG34:BD34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BD34)*($AG34:BD34=2))>MAX(COLUMN($AG34:BD34)*($AG34:BD34=3)),MAX(COLUMN($AG34:BD34)*($AG34:BD34=2))>MAX(COLUMN($AG34:BD34)*($AG34:BD34=1))),IF(COLUMN(BE34)-MAX(COLUMN($AG34:BD34)*($AG34:BD34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BE34)-MAX(COLUMN($AG34:BD34)*($AG34:BD34=3))=$J34,3,0),IF(COLUMN(BE34)-MAX(COLUMN($AG34:BD34)*($AG34:BD34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BE34)*($AG34:BE34=1))>MAX(COLUMN($AG34:BE34)*($AG34:BE34=3)),MAX(COLUMN($AG34:BE34)*($AG34:BE34=1))>MAX(COLUMN($AG34:BE34)*($AG34:BE34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BF34)-MAX(COLUMN($AG34:BE34)*($AG34:BE34=1))=$J34,3,0),IF(COLUMN(BF34)-MAX(COLUMN($AG34:BE34)*($AG34:BE34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BE34)*($AG34:BE34=2))>MAX(COLUMN($AG34:BE34)*($AG34:BE34=3)),MAX(COLUMN($AG34:BE34)*($AG34:BE34=2))>MAX(COLUMN($AG34:BE34)*($AG34:BE34=1))),IF(COLUMN(BF34)-MAX(COLUMN($AG34:BE34)*($AG34:BE34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BF34)-MAX(COLUMN($AG34:BE34)*($AG34:BE34=3))=$J34,3,0),IF(COLUMN(BF34)-MAX(COLUMN($AG34:BE34)*($AG34:BE34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BF34)*($AG34:BF34=1))>MAX(COLUMN($AG34:BF34)*($AG34:BF34=3)),MAX(COLUMN($AG34:BF34)*($AG34:BF34=1))>MAX(COLUMN($AG34:BF34)*($AG34:BF34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BG34)-MAX(COLUMN($AG34:BF34)*($AG34:BF34=1))=$J34,3,0),IF(COLUMN(BG34)-MAX(COLUMN($AG34:BF34)*($AG34:BF34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BF34)*($AG34:BF34=2))>MAX(COLUMN($AG34:BF34)*($AG34:BF34=3)),MAX(COLUMN($AG34:BF34)*($AG34:BF34=2))>MAX(COLUMN($AG34:BF34)*($AG34:BF34=1))),IF(COLUMN(BG34)-MAX(COLUMN($AG34:BF34)*($AG34:BF34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BG34)-MAX(COLUMN($AG34:BF34)*($AG34:BF34=3))=$J34,3,0),IF(COLUMN(BG34)-MAX(COLUMN($AG34:BF34)*($AG34:BF34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BG34)*($AG34:BG34=1))>MAX(COLUMN($AG34:BG34)*($AG34:BG34=3)),MAX(COLUMN($AG34:BG34)*($AG34:BG34=1))>MAX(COLUMN($AG34:BG34)*($AG34:BG34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BH34)-MAX(COLUMN($AG34:BG34)*($AG34:BG34=1))=$J34,3,0),IF(COLUMN(BH34)-MAX(COLUMN($AG34:BG34)*($AG34:BG34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BG34)*($AG34:BG34=2))>MAX(COLUMN($AG34:BG34)*($AG34:BG34=3)),MAX(COLUMN($AG34:BG34)*($AG34:BG34=2))>MAX(COLUMN($AG34:BG34)*($AG34:BG34=1))),IF(COLUMN(BH34)-MAX(COLUMN($AG34:BG34)*($AG34:BG34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BH34)-MAX(COLUMN($AG34:BG34)*($AG34:BG34=3))=$J34,3,0),IF(COLUMN(BH34)-MAX(COLUMN($AG34:BG34)*($AG34:BG34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BH34)*($AG34:BH34=1))>MAX(COLUMN($AG34:BH34)*($AG34:BH34=3)),MAX(COLUMN($AG34:BH34)*($AG34:BH34=1))>MAX(COLUMN($AG34:BH34)*($AG34:BH34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BI34)-MAX(COLUMN($AG34:BH34)*($AG34:BH34=1))=$J34,3,0),IF(COLUMN(BI34)-MAX(COLUMN($AG34:BH34)*($AG34:BH34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BH34)*($AG34:BH34=2))>MAX(COLUMN($AG34:BH34)*($AG34:BH34=3)),MAX(COLUMN($AG34:BH34)*($AG34:BH34=2))>MAX(COLUMN($AG34:BH34)*($AG34:BH34=1))),IF(COLUMN(BI34)-MAX(COLUMN($AG34:BH34)*($AG34:BH34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BI34)-MAX(COLUMN($AG34:BH34)*($AG34:BH34=3))=$J34,3,0),IF(COLUMN(BI34)-MAX(COLUMN($AG34:BH34)*($AG34:BH34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BI34)*($AG34:BI34=1))>MAX(COLUMN($AG34:BI34)*($AG34:BI34=3)),MAX(COLUMN($AG34:BI34)*($AG34:BI34=1))>MAX(COLUMN($AG34:BI34)*($AG34:BI34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BJ34)-MAX(COLUMN($AG34:BI34)*($AG34:BI34=1))=$J34,3,0),IF(COLUMN(BJ34)-MAX(COLUMN($AG34:BI34)*($AG34:BI34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BI34)*($AG34:BI34=2))>MAX(COLUMN($AG34:BI34)*($AG34:BI34=3)),MAX(COLUMN($AG34:BI34)*($AG34:BI34=2))>MAX(COLUMN($AG34:BI34)*($AG34:BI34=1))),IF(COLUMN(BJ34)-MAX(COLUMN($AG34:BI34)*($AG34:BI34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BJ34)-MAX(COLUMN($AG34:BI34)*($AG34:BI34=3))=$J34,3,0),IF(COLUMN(BJ34)-MAX(COLUMN($AG34:BI34)*($AG34:BI34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=1))>MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=3)),MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=1))>MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BK34)-MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=1))=$J34,3,0),IF(COLUMN(BK34)-MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=2))>MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=3)),MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=2))>MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=1))),IF(COLUMN(BK34)-MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BK34)-MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=3))=$J34,3,0),IF(COLUMN(BK34)-MAX(COLUMN($AG34:BJ34)*($AG34:BJ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BK34)*($AG34:BK34=1))>MAX(COLUMN($AG34:BK34)*($AG34:BK34=3)),MAX(COLUMN($AG34:BK34)*($AG34:BK34=1))>MAX(COLUMN($AG34:BK34)*($AG34:BK34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BL34)-MAX(COLUMN($AG34:BK34)*($AG34:BK34=1))=$J34,3,0),IF(COLUMN(BL34)-MAX(COLUMN($AG34:BK34)*($AG34:BK34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BK34)*($AG34:BK34=2))>MAX(COLUMN($AG34:BK34)*($AG34:BK34=3)),MAX(COLUMN($AG34:BK34)*($AG34:BK34=2))>MAX(COLUMN($AG34:BK34)*($AG34:BK34=1))),IF(COLUMN(BL34)-MAX(COLUMN($AG34:BK34)*($AG34:BK34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BL34)-MAX(COLUMN($AG34:BK34)*($AG34:BK34=3))=$J34,3,0),IF(COLUMN(BL34)-MAX(COLUMN($AG34:BK34)*($AG34:BK34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BL34)*($AG34:BL34=1))>MAX(COLUMN($AG34:BL34)*($AG34:BL34=3)),MAX(COLUMN($AG34:BL34)*($AG34:BL34=1))>MAX(COLUMN($AG34:BL34)*($AG34:BL34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BM34)-MAX(COLUMN($AG34:BL34)*($AG34:BL34=1))=$J34,3,0),IF(COLUMN(BM34)-MAX(COLUMN($AG34:BL34)*($AG34:BL34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BL34)*($AG34:BL34=2))>MAX(COLUMN($AG34:BL34)*($AG34:BL34=3)),MAX(COLUMN($AG34:BL34)*($AG34:BL34=2))>MAX(COLUMN($AG34:BL34)*($AG34:BL34=1))),IF(COLUMN(BM34)-MAX(COLUMN($AG34:BL34)*($AG34:BL34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BM34)-MAX(COLUMN($AG34:BL34)*($AG34:BL34=3))=$J34,3,0),IF(COLUMN(BM34)-MAX(COLUMN($AG34:BL34)*($AG34:BL34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BM34)*($AG34:BM34=1))>MAX(COLUMN($AG34:BM34)*($AG34:BM34=3)),MAX(COLUMN($AG34:BM34)*($AG34:BM34=1))>MAX(COLUMN($AG34:BM34)*($AG34:BM34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BN34)-MAX(COLUMN($AG34:BM34)*($AG34:BM34=1))=$J34,3,0),IF(COLUMN(BN34)-MAX(COLUMN($AG34:BM34)*($AG34:BM34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BM34)*($AG34:BM34=2))>MAX(COLUMN($AG34:BM34)*($AG34:BM34=3)),MAX(COLUMN($AG34:BM34)*($AG34:BM34=2))>MAX(COLUMN($AG34:BM34)*($AG34:BM34=1))),IF(COLUMN(BN34)-MAX(COLUMN($AG34:BM34)*($AG34:BM34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BN34)-MAX(COLUMN($AG34:BM34)*($AG34:BM34=3))=$J34,3,0),IF(COLUMN(BN34)-MAX(COLUMN($AG34:BM34)*($AG34:BM34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BN34)*($AG34:BN34=1))>MAX(COLUMN($AG34:BN34)*($AG34:BN34=3)),MAX(COLUMN($AG34:BN34)*($AG34:BN34=1))>MAX(COLUMN($AG34:BN34)*($AG34:BN34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BO34)-MAX(COLUMN($AG34:BN34)*($AG34:BN34=1))=$J34,3,0),IF(COLUMN(BO34)-MAX(COLUMN($AG34:BN34)*($AG34:BN34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BN34)*($AG34:BN34=2))>MAX(COLUMN($AG34:BN34)*($AG34:BN34=3)),MAX(COLUMN($AG34:BN34)*($AG34:BN34=2))>MAX(COLUMN($AG34:BN34)*($AG34:BN34=1))),IF(COLUMN(BO34)-MAX(COLUMN($AG34:BN34)*($AG34:BN34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BO34)-MAX(COLUMN($AG34:BN34)*($AG34:BN34=3))=$J34,3,0),IF(COLUMN(BO34)-MAX(COLUMN($AG34:BN34)*($AG34:BN34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BO34)*($AG34:BO34=1))>MAX(COLUMN($AG34:BO34)*($AG34:BO34=3)),MAX(COLUMN($AG34:BO34)*($AG34:BO34=1))>MAX(COLUMN($AG34:BO34)*($AG34:BO34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BP34)-MAX(COLUMN($AG34:BO34)*($AG34:BO34=1))=$J34,3,0),IF(COLUMN(BP34)-MAX(COLUMN($AG34:BO34)*($AG34:BO34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BO34)*($AG34:BO34=2))>MAX(COLUMN($AG34:BO34)*($AG34:BO34=3)),MAX(COLUMN($AG34:BO34)*($AG34:BO34=2))>MAX(COLUMN($AG34:BO34)*($AG34:BO34=1))),IF(COLUMN(BP34)-MAX(COLUMN($AG34:BO34)*($AG34:BO34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BP34)-MAX(COLUMN($AG34:BO34)*($AG34:BO34=3))=$J34,3,0),IF(COLUMN(BP34)-MAX(COLUMN($AG34:BO34)*($AG34:BO34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BP34)*($AG34:BP34=1))>MAX(COLUMN($AG34:BP34)*($AG34:BP34=3)),MAX(COLUMN($AG34:BP34)*($AG34:BP34=1))>MAX(COLUMN($AG34:BP34)*($AG34:BP34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BQ34)-MAX(COLUMN($AG34:BP34)*($AG34:BP34=1))=$J34,3,0),IF(COLUMN(BQ34)-MAX(COLUMN($AG34:BP34)*($AG34:BP34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BP34)*($AG34:BP34=2))>MAX(COLUMN($AG34:BP34)*($AG34:BP34=3)),MAX(COLUMN($AG34:BP34)*($AG34:BP34=2))>MAX(COLUMN($AG34:BP34)*($AG34:BP34=1))),IF(COLUMN(BQ34)-MAX(COLUMN($AG34:BP34)*($AG34:BP34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BQ34)-MAX(COLUMN($AG34:BP34)*($AG34:BP34=3))=$J34,3,0),IF(COLUMN(BQ34)-MAX(COLUMN($AG34:BP34)*($AG34:BP34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=1))>MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=3)),MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=1))>MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BR34)-MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=1))=$J34,3,0),IF(COLUMN(BR34)-MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=2))>MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=3)),MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=2))>MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=1))),IF(COLUMN(BR34)-MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BR34)-MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=3))=$J34,3,0),IF(COLUMN(BR34)-MAX(COLUMN($AG34:BQ34)*($AG34:BQ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BR34)*($AG34:BR34=1))>MAX(COLUMN($AG34:BR34)*($AG34:BR34=3)),MAX(COLUMN($AG34:BR34)*($AG34:BR34=1))>MAX(COLUMN($AG34:BR34)*($AG34:BR34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BS34)-MAX(COLUMN($AG34:BR34)*($AG34:BR34=1))=$J34,3,0),IF(COLUMN(BS34)-MAX(COLUMN($AG34:BR34)*($AG34:BR34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BR34)*($AG34:BR34=2))>MAX(COLUMN($AG34:BR34)*($AG34:BR34=3)),MAX(COLUMN($AG34:BR34)*($AG34:BR34=2))>MAX(COLUMN($AG34:BR34)*($AG34:BR34=1))),IF(COLUMN(BS34)-MAX(COLUMN($AG34:BR34)*($AG34:BR34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BS34)-MAX(COLUMN($AG34:BR34)*($AG34:BR34=3))=$J34,3,0),IF(COLUMN(BS34)-MAX(COLUMN($AG34:BR34)*($AG34:BR34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BS34)*($AG34:BS34=1))>MAX(COLUMN($AG34:BS34)*($AG34:BS34=3)),MAX(COLUMN($AG34:BS34)*($AG34:BS34=1))>MAX(COLUMN($AG34:BS34)*($AG34:BS34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BT34)-MAX(COLUMN($AG34:BS34)*($AG34:BS34=1))=$J34,3,0),IF(COLUMN(BT34)-MAX(COLUMN($AG34:BS34)*($AG34:BS34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BS34)*($AG34:BS34=2))>MAX(COLUMN($AG34:BS34)*($AG34:BS34=3)),MAX(COLUMN($AG34:BS34)*($AG34:BS34=2))>MAX(COLUMN($AG34:BS34)*($AG34:BS34=1))),IF(COLUMN(BT34)-MAX(COLUMN($AG34:BS34)*($AG34:BS34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BT34)-MAX(COLUMN($AG34:BS34)*($AG34:BS34=3))=$J34,3,0),IF(COLUMN(BT34)-MAX(COLUMN($AG34:BS34)*($AG34:BS34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BT34)*($AG34:BT34=1))>MAX(COLUMN($AG34:BT34)*($AG34:BT34=3)),MAX(COLUMN($AG34:BT34)*($AG34:BT34=1))>MAX(COLUMN($AG34:BT34)*($AG34:BT34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BU34)-MAX(COLUMN($AG34:BT34)*($AG34:BT34=1))=$J34,3,0),IF(COLUMN(BU34)-MAX(COLUMN($AG34:BT34)*($AG34:BT34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BT34)*($AG34:BT34=2))>MAX(COLUMN($AG34:BT34)*($AG34:BT34=3)),MAX(COLUMN($AG34:BT34)*($AG34:BT34=2))>MAX(COLUMN($AG34:BT34)*($AG34:BT34=1))),IF(COLUMN(BU34)-MAX(COLUMN($AG34:BT34)*($AG34:BT34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BU34)-MAX(COLUMN($AG34:BT34)*($AG34:BT34=3))=$J34,3,0),IF(COLUMN(BU34)-MAX(COLUMN($AG34:BT34)*($AG34:BT34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BU34)*($AG34:BU34=1))>MAX(COLUMN($AG34:BU34)*($AG34:BU34=3)),MAX(COLUMN($AG34:BU34)*($AG34:BU34=1))>MAX(COLUMN($AG34:BU34)*($AG34:BU34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BV34)-MAX(COLUMN($AG34:BU34)*($AG34:BU34=1))=$J34,3,0),IF(COLUMN(BV34)-MAX(COLUMN($AG34:BU34)*($AG34:BU34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BU34)*($AG34:BU34=2))>MAX(COLUMN($AG34:BU34)*($AG34:BU34=3)),MAX(COLUMN($AG34:BU34)*($AG34:BU34=2))>MAX(COLUMN($AG34:BU34)*($AG34:BU34=1))),IF(COLUMN(BV34)-MAX(COLUMN($AG34:BU34)*($AG34:BU34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BV34)-MAX(COLUMN($AG34:BU34)*($AG34:BU34=3))=$J34,3,0),IF(COLUMN(BV34)-MAX(COLUMN($AG34:BU34)*($AG34:BU34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BV34)*($AG34:BV34=1))>MAX(COLUMN($AG34:BV34)*($AG34:BV34=3)),MAX(COLUMN($AG34:BV34)*($AG34:BV34=1))>MAX(COLUMN($AG34:BV34)*($AG34:BV34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BW34)-MAX(COLUMN($AG34:BV34)*($AG34:BV34=1))=$J34,3,0),IF(COLUMN(BW34)-MAX(COLUMN($AG34:BV34)*($AG34:BV34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BV34)*($AG34:BV34=2))>MAX(COLUMN($AG34:BV34)*($AG34:BV34=3)),MAX(COLUMN($AG34:BV34)*($AG34:BV34=2))>MAX(COLUMN($AG34:BV34)*($AG34:BV34=1))),IF(COLUMN(BW34)-MAX(COLUMN($AG34:BV34)*($AG34:BV34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BW34)-MAX(COLUMN($AG34:BV34)*($AG34:BV34=3))=$J34,3,0),IF(COLUMN(BW34)-MAX(COLUMN($AG34:BV34)*($AG34:BV34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BW34)*($AG34:BW34=1))>MAX(COLUMN($AG34:BW34)*($AG34:BW34=3)),MAX(COLUMN($AG34:BW34)*($AG34:BW34=1))>MAX(COLUMN($AG34:BW34)*($AG34:BW34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BX34)-MAX(COLUMN($AG34:BW34)*($AG34:BW34=1))=$J34,3,0),IF(COLUMN(BX34)-MAX(COLUMN($AG34:BW34)*($AG34:BW34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BW34)*($AG34:BW34=2))>MAX(COLUMN($AG34:BW34)*($AG34:BW34=3)),MAX(COLUMN($AG34:BW34)*($AG34:BW34=2))>MAX(COLUMN($AG34:BW34)*($AG34:BW34=1))),IF(COLUMN(BX34)-MAX(COLUMN($AG34:BW34)*($AG34:BW34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BX34)-MAX(COLUMN($AG34:BW34)*($AG34:BW34=3))=$J34,3,0),IF(COLUMN(BX34)-MAX(COLUMN($AG34:BW34)*($AG34:BW34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BX34)*($AG34:BX34=1))>MAX(COLUMN($AG34:BX34)*($AG34:BX34=3)),MAX(COLUMN($AG34:BX34)*($AG34:BX34=1))>MAX(COLUMN($AG34:BX34)*($AG34:BX34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BY34)-MAX(COLUMN($AG34:BX34)*($AG34:BX34=1))=$J34,3,0),IF(COLUMN(BY34)-MAX(COLUMN($AG34:BX34)*($AG34:BX34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BX34)*($AG34:BX34=2))>MAX(COLUMN($AG34:BX34)*($AG34:BX34=3)),MAX(COLUMN($AG34:BX34)*($AG34:BX34=2))>MAX(COLUMN($AG34:BX34)*($AG34:BX34=1))),IF(COLUMN(BY34)-MAX(COLUMN($AG34:BX34)*($AG34:BX34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BY34)-MAX(COLUMN($AG34:BX34)*($AG34:BX34=3))=$J34,3,0),IF(COLUMN(BY34)-MAX(COLUMN($AG34:BX34)*($AG34:BX34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BY34)*($AG34:BY34=1))>MAX(COLUMN($AG34:BY34)*($AG34:BY34=3)),MAX(COLUMN($AG34:BY34)*($AG34:BY34=1))>MAX(COLUMN($AG34:BY34)*($AG34:BY34=2))),IF($K34=\"Not Possible\",IF(COLUMN(BZ34)-MAX(COLUMN($AG34:BY34)*($AG34:BY34=1))=$J34,3,0),IF(COLUMN(BZ34)-MAX(COLUMN($AG34:BY34)*($AG34:BY34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BY34)*($AG34:BY34=2))>MAX(COLUMN($AG34:BY34)*($AG34:BY34=3)),MAX(COLUMN($AG34:BY34)*($AG34:BY34=2))>MAX(COLUMN($AG34:BY34)*($AG34:BY34=1))),IF(COLUMN(BZ34)-MAX(COLUMN($AG34:BY34)*($AG34:BY34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(BZ34)-MAX(COLUMN($AG34:BY34)*($AG34:BY34=3))=$J34,3,0),IF(COLUMN(BZ34)-MAX(COLUMN($AG34:BY34)*($AG34:BY34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=1))>MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=3)),MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=1))>MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CA34)-MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=1))=$J34,3,0),IF(COLUMN(CA34)-MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=2))>MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=3)),MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=2))>MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=1))),IF(COLUMN(CA34)-MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CA34)-MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=3))=$J34,3,0),IF(COLUMN(CA34)-MAX(COLUMN($AG34:BZ34)*($AG34:BZ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CA34)*($AG34:CA34=1))>MAX(COLUMN($AG34:CA34)*($AG34:CA34=3)),MAX(COLUMN($AG34:CA34)*($AG34:CA34=1))>MAX(COLUMN($AG34:CA34)*($AG34:CA34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CB34)-MAX(COLUMN($AG34:CA34)*($AG34:CA34=1))=$J34,3,0),IF(COLUMN(CB34)-MAX(COLUMN($AG34:CA34)*($AG34:CA34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CA34)*($AG34:CA34=2))>MAX(COLUMN($AG34:CA34)*($AG34:CA34=3)),MAX(COLUMN($AG34:CA34)*($AG34:CA34=2))>MAX(COLUMN($AG34:CA34)*($AG34:CA34=1))),IF(COLUMN(CB34)-MAX(COLUMN($AG34:CA34)*($AG34:CA34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CB34)-MAX(COLUMN($AG34:CA34)*($AG34:CA34=3))=$J34,3,0),IF(COLUMN(CB34)-MAX(COLUMN($AG34:CA34)*($AG34:CA34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CB34)*($AG34:CB34=1))>MAX(COLUMN($AG34:CB34)*($AG34:CB34=3)),MAX(COLUMN($AG34:CB34)*($AG34:CB34=1))>MAX(COLUMN($AG34:CB34)*($AG34:CB34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CC34)-MAX(COLUMN($AG34:CB34)*($AG34:CB34=1))=$J34,3,0),IF(COLUMN(CC34)-MAX(COLUMN($AG34:CB34)*($AG34:CB34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CB34)*($AG34:CB34=2))>MAX(COLUMN($AG34:CB34)*($AG34:CB34=3)),MAX(COLUMN($AG34:CB34)*($AG34:CB34=2))>MAX(COLUMN($AG34:CB34)*($AG34:CB34=1))),IF(COLUMN(CC34)-MAX(COLUMN($AG34:CB34)*($AG34:CB34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CC34)-MAX(COLUMN($AG34:CB34)*($AG34:CB34=3))=$J34,3,0),IF(COLUMN(CC34)-MAX(COLUMN($AG34:CB34)*($AG34:CB34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CC34)*($AG34:CC34=1))>MAX(COLUMN($AG34:CC34)*($AG34:CC34=3)),MAX(COLUMN($AG34:CC34)*($AG34:CC34=1))>MAX(COLUMN($AG34:CC34)*($AG34:CC34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CD34)-MAX(COLUMN($AG34:CC34)*($AG34:CC34=1))=$J34,3,0),IF(COLUMN(CD34)-MAX(COLUMN($AG34:CC34)*($AG34:CC34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CC34)*($AG34:CC34=2))>MAX(COLUMN($AG34:CC34)*($AG34:CC34=3)),MAX(COLUMN($AG34:CC34)*($AG34:CC34=2))>MAX(COLUMN($AG34:CC34)*($AG34:CC34=1))),IF(COLUMN(CD34)-MAX(COLUMN($AG34:CC34)*($AG34:CC34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CD34)-MAX(COLUMN($AG34:CC34)*($AG34:CC34=3))=$J34,3,0),IF(COLUMN(CD34)-MAX(COLUMN($AG34:CC34)*($AG34:CC34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CD34)*($AG34:CD34=1))>MAX(COLUMN($AG34:CD34)*($AG34:CD34=3)),MAX(COLUMN($AG34:CD34)*($AG34:CD34=1))>MAX(COLUMN($AG34:CD34)*($AG34:CD34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CE34)-MAX(COLUMN($AG34:CD34)*($AG34:CD34=1))=$J34,3,0),IF(COLUMN(CE34)-MAX(COLUMN($AG34:CD34)*($AG34:CD34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CD34)*($AG34:CD34=2))>MAX(COLUMN($AG34:CD34)*($AG34:CD34=3)),MAX(COLUMN($AG34:CD34)*($AG34:CD34=2))>MAX(COLUMN($AG34:CD34)*($AG34:CD34=1))),IF(COLUMN(CE34)-MAX(COLUMN($AG34:CD34)*($AG34:CD34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CE34)-MAX(COLUMN($AG34:CD34)*($AG34:CD34=3))=$J34,3,0),IF(COLUMN(CE34)-MAX(COLUMN($AG34:CD34)*($AG34:CD34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CE34)*($AG34:CE34=1))>MAX(COLUMN($AG34:CE34)*($AG34:CE34=3)),MAX(COLUMN($AG34:CE34)*($AG34:CE34=1))>MAX(COLUMN($AG34:CE34)*($AG34:CE34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CF34)-MAX(COLUMN($AG34:CE34)*($AG34:CE34=1))=$J34,3,0),IF(COLUMN(CF34)-MAX(COLUMN($AG34:CE34)*($AG34:CE34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CE34)*($AG34:CE34=2))>MAX(COLUMN($AG34:CE34)*($AG34:CE34=3)),MAX(COLUMN($AG34:CE34)*($AG34:CE34=2))>MAX(COLUMN($AG34:CE34)*($AG34:CE34=1))),IF(COLUMN(CF34)-MAX(COLUMN($AG34:CE34)*($AG34:CE34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CF34)-MAX(COLUMN($AG34:CE34)*($AG34:CE34=3))=$J34,3,0),IF(COLUMN(CF34)-MAX(COLUMN($AG34:CE34)*($AG34:CE34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CF34)*($AG34:CF34=1))>MAX(COLUMN($AG34:CF34)*($AG34:CF34=3)),MAX(COLUMN($AG34:CF34)*($AG34:CF34=1))>MAX(COLUMN($AG34:CF34)*($AG34:CF34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CG34)-MAX(COLUMN($AG34:CF34)*($AG34:CF34=1))=$J34,3,0),IF(COLUMN(CG34)-MAX(COLUMN($AG34:CF34)*($AG34:CF34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CF34)*($AG34:CF34=2))>MAX(COLUMN($AG34:CF34)*($AG34:CF34=3)),MAX(COLUMN($AG34:CF34)*($AG34:CF34=2))>MAX(COLUMN($AG34:CF34)*($AG34:CF34=1))),IF(COLUMN(CG34)-MAX(COLUMN($AG34:CF34)*($AG34:CF34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CG34)-MAX(COLUMN($AG34:CF34)*($AG34:CF34=3))=$J34,3,0),IF(COLUMN(CG34)-MAX(COLUMN($AG34:CF34)*($AG34:CF34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CG34)*($AG34:CG34=1))>MAX(COLUMN($AG34:CG34)*($AG34:CG34=3)),MAX(COLUMN($AG34:CG34)*($AG34:CG34=1))>MAX(COLUMN($AG34:CG34)*($AG34:CG34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CH34)-MAX(COLUMN($AG34:CG34)*($AG34:CG34=1))=$J34,3,0),IF(COLUMN(CH34)-MAX(COLUMN($AG34:CG34)*($AG34:CG34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CG34)*($AG34:CG34=2))>MAX(COLUMN($AG34:CG34)*($AG34:CG34=3)),MAX(COLUMN($AG34:CG34)*($AG34:CG34=2))>MAX(COLUMN($AG34:CG34)*($AG34:CG34=1))),IF(COLUMN(CH34)-MAX(COLUMN($AG34:CG34)*($AG34:CG34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CH34)-MAX(COLUMN($AG34:CG34)*($AG34:CG34=3))=$J34,3,0),IF(COLUMN(CH34)-MAX(COLUMN($AG34:CG34)*($AG34:CG34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CH34)*($AG34:CH34=1))>MAX(COLUMN($AG34:CH34)*($AG34:CH34=3)),MAX(COLUMN($AG34:CH34)*($AG34:CH34=1))>MAX(COLUMN($AG34:CH34)*($AG34:CH34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CI34)-MAX(COLUMN($AG34:CH34)*($AG34:CH34=1))=$J34,3,0),IF(COLUMN(CI34)-MAX(COLUMN($AG34:CH34)*($AG34:CH34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CH34)*($AG34:CH34=2))>MAX(COLUMN($AG34:CH34)*($AG34:CH34=3)),MAX(COLUMN($AG34:CH34)*($AG34:CH34=2))>MAX(COLUMN($AG34:CH34)*($AG34:CH34=1))),IF(COLUMN(CI34)-MAX(COLUMN($AG34:CH34)*($AG34:CH34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CI34)-MAX(COLUMN($AG34:CH34)*($AG34:CH34=3))=$J34,3,0),IF(COLUMN(CI34)-MAX(COLUMN($AG34:CH34)*($AG34:CH34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CI34)*($AG34:CI34=1))>MAX(COLUMN($AG34:CI34)*($AG34:CI34=3)),MAX(COLUMN($AG34:CI34)*($AG34:CI34=1))>MAX(COLUMN($AG34:CI34)*($AG34:CI34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CJ34)-MAX(COLUMN($AG34:CI34)*($AG34:CI34=1))=$J34,3,0),IF(COLUMN(CJ34)-MAX(COLUMN($AG34:CI34)*($AG34:CI34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CI34)*($AG34:CI34=2))>MAX(COLUMN($AG34:CI34)*($AG34:CI34=3)),MAX(COLUMN($AG34:CI34)*($AG34:CI34=2))>MAX(COLUMN($AG34:CI34)*($AG34:CI34=1))),IF(COLUMN(CJ34)-MAX(COLUMN($AG34:CI34)*($AG34:CI34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CJ34)-MAX(COLUMN($AG34:CI34)*($AG34:CI34=3))=$J34,3,0),IF(COLUMN(CJ34)-MAX(COLUMN($AG34:CI34)*($AG34:CI34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=1))>MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=3)),MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=1))>MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CK34)-MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=1))=$J34,3,0),IF(COLUMN(CK34)-MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=2))>MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=3)),MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=2))>MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=1))),IF(COLUMN(CK34)-MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CK34)-MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=3))=$J34,3,0),IF(COLUMN(CK34)-MAX(COLUMN($AG34:CJ34)*($AG34:CJ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CK34)*($AG34:CK34=1))>MAX(COLUMN($AG34:CK34)*($AG34:CK34=3)),MAX(COLUMN($AG34:CK34)*($AG34:CK34=1))>MAX(COLUMN($AG34:CK34)*($AG34:CK34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CL34)-MAX(COLUMN($AG34:CK34)*($AG34:CK34=1))=$J34,3,0),IF(COLUMN(CL34)-MAX(COLUMN($AG34:CK34)*($AG34:CK34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CK34)*($AG34:CK34=2))>MAX(COLUMN($AG34:CK34)*($AG34:CK34=3)),MAX(COLUMN($AG34:CK34)*($AG34:CK34=2))>MAX(COLUMN($AG34:CK34)*($AG34:CK34=1))),IF(COLUMN(CL34)-MAX(COLUMN($AG34:CK34)*($AG34:CK34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CL34)-MAX(COLUMN($AG34:CK34)*($AG34:CK34=3))=$J34,3,0),IF(COLUMN(CL34)-MAX(COLUMN($AG34:CK34)*($AG34:CK34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CL34)*($AG34:CL34=1))>MAX(COLUMN($AG34:CL34)*($AG34:CL34=3)),MAX(COLUMN($AG34:CL34)*($AG34:CL34=1))>MAX(COLUMN($AG34:CL34)*($AG34:CL34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CM34)-MAX(COLUMN($AG34:CL34)*($AG34:CL34=1))=$J34,3,0),IF(COLUMN(CM34)-MAX(COLUMN($AG34:CL34)*($AG34:CL34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CL34)*($AG34:CL34=2))>MAX(COLUMN($AG34:CL34)*($AG34:CL34=3)),MAX(COLUMN($AG34:CL34)*($AG34:CL34=2))>MAX(COLUMN($AG34:CL34)*($AG34:CL34=1))),IF(COLUMN(CM34)-MAX(COLUMN($AG34:CL34)*($AG34:CL34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CM34)-MAX(COLUMN($AG34:CL34)*($AG34:CL34=3))=$J34,3,0),IF(COLUMN(CM34)-MAX(COLUMN($AG34:CL34)*($AG34:CL34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CM34)*($AG34:CM34=1))>MAX(COLUMN($AG34:CM34)*($AG34:CM34=3)),MAX(COLUMN($AG34:CM34)*($AG34:CM34=1))>MAX(COLUMN($AG34:CM34)*($AG34:CM34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CN34)-MAX(COLUMN($AG34:CM34)*($AG34:CM34=1))=$J34,3,0),IF(COLUMN(CN34)-MAX(COLUMN($AG34:CM34)*($AG34:CM34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CM34)*($AG34:CM34=2))>MAX(COLUMN($AG34:CM34)*($AG34:CM34=3)),MAX(COLUMN($AG34:CM34)*($AG34:CM34=2))>MAX(COLUMN($AG34:CM34)*($AG34:CM34=1))),IF(COLUMN(CN34)-MAX(COLUMN($AG34:CM34)*($AG34:CM34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CN34)-MAX(COLUMN($AG34:CM34)*($AG34:CM34=3))=$J34,3,0),IF(COLUMN(CN34)-MAX(COLUMN($AG34:CM34)*($AG34:CM34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CN34)*($AG34:CN34=1))>MAX(COLUMN($AG34:CN34)*($AG34:CN34=3)),MAX(COLUMN($AG34:CN34)*($AG34:CN34=1))>MAX(COLUMN($AG34:CN34)*($AG34:CN34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CO34)-MAX(COLUMN($AG34:CN34)*($AG34:CN34=1))=$J34,3,0),IF(COLUMN(CO34)-MAX(COLUMN($AG34:CN34)*($AG34:CN34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CN34)*($AG34:CN34=2))>MAX(COLUMN($AG34:CN34)*($AG34:CN34=3)),MAX(COLUMN($AG34:CN34)*($AG34:CN34=2))>MAX(COLUMN($AG34:CN34)*($AG34:CN34=1))),IF(COLUMN(CO34)-MAX(COLUMN($AG34:CN34)*($AG34:CN34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CO34)-MAX(COLUMN($AG34:CN34)*($AG34:CN34=3))=$J34,3,0),IF(COLUMN(CO34)-MAX(COLUMN($AG34:CN34)*($AG34:CN34=3))=$J34,2,0)))))","v":2},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CO34)*($AG34:CO34=1))>MAX(COLUMN($AG34:CO34)*($AG34:CO34=3)),MAX(COLUMN($AG34:CO34)*($AG34:CO34=1))>MAX(COLUMN($AG34:CO34)*($AG34:CO34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CP34)-MAX(COLUMN($AG34:CO34)*($AG34:CO34=1))=$J34,3,0),IF(COLUMN(CP34)-MAX(COLUMN($AG34:CO34)*($AG34:CO34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CO34)*($AG34:CO34=2))>MAX(COLUMN($AG34:CO34)*($AG34:CO34=3)),MAX(COLUMN($AG34:CO34)*($AG34:CO34=2))>MAX(COLUMN($AG34:CO34)*($AG34:CO34=1))),IF(COLUMN(CP34)-MAX(COLUMN($AG34:CO34)*($AG34:CO34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CP34)-MAX(COLUMN($AG34:CO34)*($AG34:CO34=3))=$J34,3,0),IF(COLUMN(CP34)-MAX(COLUMN($AG34:CO34)*($AG34:CO34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CP34)*($AG34:CP34=1))>MAX(COLUMN($AG34:CP34)*($AG34:CP34=3)),MAX(COLUMN($AG34:CP34)*($AG34:CP34=1))>MAX(COLUMN($AG34:CP34)*($AG34:CP34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CQ34)-MAX(COLUMN($AG34:CP34)*($AG34:CP34=1))=$J34,3,0),IF(COLUMN(CQ34)-MAX(COLUMN($AG34:CP34)*($AG34:CP34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CP34)*($AG34:CP34=2))>MAX(COLUMN($AG34:CP34)*($AG34:CP34=3)),MAX(COLUMN($AG34:CP34)*($AG34:CP34=2))>MAX(COLUMN($AG34:CP34)*($AG34:CP34=1))),IF(COLUMN(CQ34)-MAX(COLUMN($AG34:CP34)*($AG34:CP34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CQ34)-MAX(COLUMN($AG34:CP34)*($AG34:CP34=3))=$J34,3,0),IF(COLUMN(CQ34)-MAX(COLUMN($AG34:CP34)*($AG34:CP34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=1))>MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=3)),MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=1))>MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CR34)-MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=1))=$J34,3,0),IF(COLUMN(CR34)-MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=2))>MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=3)),MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=2))>MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=1))),IF(COLUMN(CR34)-MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CR34)-MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=3))=$J34,3,0),IF(COLUMN(CR34)-MAX(COLUMN($AG34:CQ34)*($AG34:CQ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CR34)*($AG34:CR34=1))>MAX(COLUMN($AG34:CR34)*($AG34:CR34=3)),MAX(COLUMN($AG34:CR34)*($AG34:CR34=1))>MAX(COLUMN($AG34:CR34)*($AG34:CR34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CS34)-MAX(COLUMN($AG34:CR34)*($AG34:CR34=1))=$J34,3,0),IF(COLUMN(CS34)-MAX(COLUMN($AG34:CR34)*($AG34:CR34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CR34)*($AG34:CR34=2))>MAX(COLUMN($AG34:CR34)*($AG34:CR34=3)),MAX(COLUMN($AG34:CR34)*($AG34:CR34=2))>MAX(COLUMN($AG34:CR34)*($AG34:CR34=1))),IF(COLUMN(CS34)-MAX(COLUMN($AG34:CR34)*($AG34:CR34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CS34)-MAX(COLUMN($AG34:CR34)*($AG34:CR34=3))=$J34,3,0),IF(COLUMN(CS34)-MAX(COLUMN($AG34:CR34)*($AG34:CR34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CS34)*($AG34:CS34=1))>MAX(COLUMN($AG34:CS34)*($AG34:CS34=3)),MAX(COLUMN($AG34:CS34)*($AG34:CS34=1))>MAX(COLUMN($AG34:CS34)*($AG34:CS34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CT34)-MAX(COLUMN($AG34:CS34)*($AG34:CS34=1))=$J34,3,0),IF(COLUMN(CT34)-MAX(COLUMN($AG34:CS34)*($AG34:CS34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CS34)*($AG34:CS34=2))>MAX(COLUMN($AG34:CS34)*($AG34:CS34=3)),MAX(COLUMN($AG34:CS34)*($AG34:CS34=2))>MAX(COLUMN($AG34:CS34)*($AG34:CS34=1))),IF(COLUMN(CT34)-MAX(COLUMN($AG34:CS34)*($AG34:CS34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CT34)-MAX(COLUMN($AG34:CS34)*($AG34:CS34=3))=$J34,3,0),IF(COLUMN(CT34)-MAX(COLUMN($AG34:CS34)*($AG34:CS34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CT34)*($AG34:CT34=1))>MAX(COLUMN($AG34:CT34)*($AG34:CT34=3)),MAX(COLUMN($AG34:CT34)*($AG34:CT34=1))>MAX(COLUMN($AG34:CT34)*($AG34:CT34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CU34)-MAX(COLUMN($AG34:CT34)*($AG34:CT34=1))=$J34,3,0),IF(COLUMN(CU34)-MAX(COLUMN($AG34:CT34)*($AG34:CT34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CT34)*($AG34:CT34=2))>MAX(COLUMN($AG34:CT34)*($AG34:CT34=3)),MAX(COLUMN($AG34:CT34)*($AG34:CT34=2))>MAX(COLUMN($AG34:CT34)*($AG34:CT34=1))),IF(COLUMN(CU34)-MAX(COLUMN($AG34:CT34)*($AG34:CT34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CU34)-MAX(COLUMN($AG34:CT34)*($AG34:CT34=3))=$J34,3,0),IF(COLUMN(CU34)-MAX(COLUMN($AG34:CT34)*($AG34:CT34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CU34)*($AG34:CU34=1))>MAX(COLUMN($AG34:CU34)*($AG34:CU34=3)),MAX(COLUMN($AG34:CU34)*($AG34:CU34=1))>MAX(COLUMN($AG34:CU34)*($AG34:CU34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CV34)-MAX(COLUMN($AG34:CU34)*($AG34:CU34=1))=$J34,3,0),IF(COLUMN(CV34)-MAX(COLUMN($AG34:CU34)*($AG34:CU34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CU34)*($AG34:CU34=2))>MAX(COLUMN($AG34:CU34)*($AG34:CU34=3)),MAX(COLUMN($AG34:CU34)*($AG34:CU34=2))>MAX(COLUMN($AG34:CU34)*($AG34:CU34=1))),IF(COLUMN(CV34)-MAX(COLUMN($AG34:CU34)*($AG34:CU34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CV34)-MAX(COLUMN($AG34:CU34)*($AG34:CU34=3))=$J34,3,0),IF(COLUMN(CV34)-MAX(COLUMN($AG34:CU34)*($AG34:CU34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CV34)*($AG34:CV34=1))>MAX(COLUMN($AG34:CV34)*($AG34:CV34=3)),MAX(COLUMN($AG34:CV34)*($AG34:CV34=1))>MAX(COLUMN($AG34:CV34)*($AG34:CV34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CW34)-MAX(COLUMN($AG34:CV34)*($AG34:CV34=1))=$J34,3,0),IF(COLUMN(CW34)-MAX(COLUMN($AG34:CV34)*($AG34:CV34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CV34)*($AG34:CV34=2))>MAX(COLUMN($AG34:CV34)*($AG34:CV34=3)),MAX(COLUMN($AG34:CV34)*($AG34:CV34=2))>MAX(COLUMN($AG34:CV34)*($AG34:CV34=1))),IF(COLUMN(CW34)-MAX(COLUMN($AG34:CV34)*($AG34:CV34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CW34)-MAX(COLUMN($AG34:CV34)*($AG34:CV34=3))=$J34,3,0),IF(COLUMN(CW34)-MAX(COLUMN($AG34:CV34)*($AG34:CV34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CW34)*($AG34:CW34=1))>MAX(COLUMN($AG34:CW34)*($AG34:CW34=3)),MAX(COLUMN($AG34:CW34)*($AG34:CW34=1))>MAX(COLUMN($AG34:CW34)*($AG34:CW34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CX34)-MAX(COLUMN($AG34:CW34)*($AG34:CW34=1))=$J34,3,0),IF(COLUMN(CX34)-MAX(COLUMN($AG34:CW34)*($AG34:CW34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CW34)*($AG34:CW34=2))>MAX(COLUMN($AG34:CW34)*($AG34:CW34=3)),MAX(COLUMN($AG34:CW34)*($AG34:CW34=2))>MAX(COLUMN($AG34:CW34)*($AG34:CW34=1))),IF(COLUMN(CX34)-MAX(COLUMN($AG34:CW34)*($AG34:CW34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CX34)-MAX(COLUMN($AG34:CW34)*($AG34:CW34=3))=$J34,3,0),IF(COLUMN(CX34)-MAX(COLUMN($AG34:CW34)*($AG34:CW34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CX34)*($AG34:CX34=1))>MAX(COLUMN($AG34:CX34)*($AG34:CX34=3)),MAX(COLUMN($AG34:CX34)*($AG34:CX34=1))>MAX(COLUMN($AG34:CX34)*($AG34:CX34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CY34)-MAX(COLUMN($AG34:CX34)*($AG34:CX34=1))=$J34,3,0),IF(COLUMN(CY34)-MAX(COLUMN($AG34:CX34)*($AG34:CX34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CX34)*($AG34:CX34=2))>MAX(COLUMN($AG34:CX34)*($AG34:CX34=3)),MAX(COLUMN($AG34:CX34)*($AG34:CX34=2))>MAX(COLUMN($AG34:CX34)*($AG34:CX34=1))),IF(COLUMN(CY34)-MAX(COLUMN($AG34:CX34)*($AG34:CX34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CY34)-MAX(COLUMN($AG34:CX34)*($AG34:CX34=3))=$J34,3,0),IF(COLUMN(CY34)-MAX(COLUMN($AG34:CX34)*($AG34:CX34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CY34)*($AG34:CY34=1))>MAX(COLUMN($AG34:CY34)*($AG34:CY34=3)),MAX(COLUMN($AG34:CY34)*($AG34:CY34=1))>MAX(COLUMN($AG34:CY34)*($AG34:CY34=2))),IF($K34=\"Not Possible\",IF(COLUMN(CZ34)-MAX(COLUMN($AG34:CY34)*($AG34:CY34=1))=$J34,3,0),IF(COLUMN(CZ34)-MAX(COLUMN($AG34:CY34)*($AG34:CY34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CY34)*($AG34:CY34=2))>MAX(COLUMN($AG34:CY34)*($AG34:CY34=3)),MAX(COLUMN($AG34:CY34)*($AG34:CY34=2))>MAX(COLUMN($AG34:CY34)*($AG34:CY34=1))),IF(COLUMN(CZ34)-MAX(COLUMN($AG34:CY34)*($AG34:CY34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(CZ34)-MAX(COLUMN($AG34:CY34)*($AG34:CY34=3))=$J34,3,0),IF(COLUMN(CZ34)-MAX(COLUMN($AG34:CY34)*($AG34:CY34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=1))>MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=3)),MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=1))>MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DA34)-MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=1))=$J34,3,0),IF(COLUMN(DA34)-MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=2))>MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=3)),MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=2))>MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=1))),IF(COLUMN(DA34)-MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DA34)-MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=3))=$J34,3,0),IF(COLUMN(DA34)-MAX(COLUMN($AG34:CZ34)*($AG34:CZ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DA34)*($AG34:DA34=1))>MAX(COLUMN($AG34:DA34)*($AG34:DA34=3)),MAX(COLUMN($AG34:DA34)*($AG34:DA34=1))>MAX(COLUMN($AG34:DA34)*($AG34:DA34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DB34)-MAX(COLUMN($AG34:DA34)*($AG34:DA34=1))=$J34,3,0),IF(COLUMN(DB34)-MAX(COLUMN($AG34:DA34)*($AG34:DA34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DA34)*($AG34:DA34=2))>MAX(COLUMN($AG34:DA34)*($AG34:DA34=3)),MAX(COLUMN($AG34:DA34)*($AG34:DA34=2))>MAX(COLUMN($AG34:DA34)*($AG34:DA34=1))),IF(COLUMN(DB34)-MAX(COLUMN($AG34:DA34)*($AG34:DA34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DB34)-MAX(COLUMN($AG34:DA34)*($AG34:DA34=3))=$J34,3,0),IF(COLUMN(DB34)-MAX(COLUMN($AG34:DA34)*($AG34:DA34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DB34)*($AG34:DB34=1))>MAX(COLUMN($AG34:DB34)*($AG34:DB34=3)),MAX(COLUMN($AG34:DB34)*($AG34:DB34=1))>MAX(COLUMN($AG34:DB34)*($AG34:DB34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DC34)-MAX(COLUMN($AG34:DB34)*($AG34:DB34=1))=$J34,3,0),IF(COLUMN(DC34)-MAX(COLUMN($AG34:DB34)*($AG34:DB34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DB34)*($AG34:DB34=2))>MAX(COLUMN($AG34:DB34)*($AG34:DB34=3)),MAX(COLUMN($AG34:DB34)*($AG34:DB34=2))>MAX(COLUMN($AG34:DB34)*($AG34:DB34=1))),IF(COLUMN(DC34)-MAX(COLUMN($AG34:DB34)*($AG34:DB34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DC34)-MAX(COLUMN($AG34:DB34)*($AG34:DB34=3))=$J34,3,0),IF(COLUMN(DC34)-MAX(COLUMN($AG34:DB34)*($AG34:DB34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DC34)*($AG34:DC34=1))>MAX(COLUMN($AG34:DC34)*($AG34:DC34=3)),MAX(COLUMN($AG34:DC34)*($AG34:DC34=1))>MAX(COLUMN($AG34:DC34)*($AG34:DC34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DD34)-MAX(COLUMN($AG34:DC34)*($AG34:DC34=1))=$J34,3,0),IF(COLUMN(DD34)-MAX(COLUMN($AG34:DC34)*($AG34:DC34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DC34)*($AG34:DC34=2))>MAX(COLUMN($AG34:DC34)*($AG34:DC34=3)),MAX(COLUMN($AG34:DC34)*($AG34:DC34=2))>MAX(COLUMN($AG34:DC34)*($AG34:DC34=1))),IF(COLUMN(DD34)-MAX(COLUMN($AG34:DC34)*($AG34:DC34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DD34)-MAX(COLUMN($AG34:DC34)*($AG34:DC34=3))=$J34,3,0),IF(COLUMN(DD34)-MAX(COLUMN($AG34:DC34)*($AG34:DC34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DD34)*($AG34:DD34=1))>MAX(COLUMN($AG34:DD34)*($AG34:DD34=3)),MAX(COLUMN($AG34:DD34)*($AG34:DD34=1))>MAX(COLUMN($AG34:DD34)*($AG34:DD34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DE34)-MAX(COLUMN($AG34:DD34)*($AG34:DD34=1))=$J34,3,0),IF(COLUMN(DE34)-MAX(COLUMN($AG34:DD34)*($AG34:DD34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DD34)*($AG34:DD34=2))>MAX(COLUMN($AG34:DD34)*($AG34:DD34=3)),MAX(COLUMN($AG34:DD34)*($AG34:DD34=2))>MAX(COLUMN($AG34:DD34)*($AG34:DD34=1))),IF(COLUMN(DE34)-MAX(COLUMN($AG34:DD34)*($AG34:DD34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DE34)-MAX(COLUMN($AG34:DD34)*($AG34:DD34=3))=$J34,3,0),IF(COLUMN(DE34)-MAX(COLUMN($AG34:DD34)*($AG34:DD34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DE34)*($AG34:DE34=1))>MAX(COLUMN($AG34:DE34)*($AG34:DE34=3)),MAX(COLUMN($AG34:DE34)*($AG34:DE34=1))>MAX(COLUMN($AG34:DE34)*($AG34:DE34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DF34)-MAX(COLUMN($AG34:DE34)*($AG34:DE34=1))=$J34,3,0),IF(COLUMN(DF34)-MAX(COLUMN($AG34:DE34)*($AG34:DE34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DE34)*($AG34:DE34=2))>MAX(COLUMN($AG34:DE34)*($AG34:DE34=3)),MAX(COLUMN($AG34:DE34)*($AG34:DE34=2))>MAX(COLUMN($AG34:DE34)*($AG34:DE34=1))),IF(COLUMN(DF34)-MAX(COLUMN($AG34:DE34)*($AG34:DE34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DF34)-MAX(COLUMN($AG34:DE34)*($AG34:DE34=3))=$J34,3,0),IF(COLUMN(DF34)-MAX(COLUMN($AG34:DE34)*($AG34:DE34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DF34)*($AG34:DF34=1))>MAX(COLUMN($AG34:DF34)*($AG34:DF34=3)),MAX(COLUMN($AG34:DF34)*($AG34:DF34=1))>MAX(COLUMN($AG34:DF34)*($AG34:DF34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DG34)-MAX(COLUMN($AG34:DF34)*($AG34:DF34=1))=$J34,3,0),IF(COLUMN(DG34)-MAX(COLUMN($AG34:DF34)*($AG34:DF34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DF34)*($AG34:DF34=2))>MAX(COLUMN($AG34:DF34)*($AG34:DF34=3)),MAX(COLUMN($AG34:DF34)*($AG34:DF34=2))>MAX(COLUMN($AG34:DF34)*($AG34:DF34=1))),IF(COLUMN(DG34)-MAX(COLUMN($AG34:DF34)*($AG34:DF34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DG34)-MAX(COLUMN($AG34:DF34)*($AG34:DF34=3))=$J34,3,0),IF(COLUMN(DG34)-MAX(COLUMN($AG34:DF34)*($AG34:DF34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DG34)*($AG34:DG34=1))>MAX(COLUMN($AG34:DG34)*($AG34:DG34=3)),MAX(COLUMN($AG34:DG34)*($AG34:DG34=1))>MAX(COLUMN($AG34:DG34)*($AG34:DG34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DH34)-MAX(COLUMN($AG34:DG34)*($AG34:DG34=1))=$J34,3,0),IF(COLUMN(DH34)-MAX(COLUMN($AG34:DG34)*($AG34:DG34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DG34)*($AG34:DG34=2))>MAX(COLUMN($AG34:DG34)*($AG34:DG34=3)),MAX(COLUMN($AG34:DG34)*($AG34:DG34=2))>MAX(COLUMN($AG34:DG34)*($AG34:DG34=1))),IF(COLUMN(DH34)-MAX(COLUMN($AG34:DG34)*($AG34:DG34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DH34)-MAX(COLUMN($AG34:DG34)*($AG34:DG34=3))=$J34,3,0),IF(COLUMN(DH34)-MAX(COLUMN($AG34:DG34)*($AG34:DG34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DH34)*($AG34:DH34=1))>MAX(COLUMN($AG34:DH34)*($AG34:DH34=3)),MAX(COLUMN($AG34:DH34)*($AG34:DH34=1))>MAX(COLUMN($AG34:DH34)*($AG34:DH34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DI34)-MAX(COLUMN($AG34:DH34)*($AG34:DH34=1))=$J34,3,0),IF(COLUMN(DI34)-MAX(COLUMN($AG34:DH34)*($AG34:DH34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DH34)*($AG34:DH34=2))>MAX(COLUMN($AG34:DH34)*($AG34:DH34=3)),MAX(COLUMN($AG34:DH34)*($AG34:DH34=2))>MAX(COLUMN($AG34:DH34)*($AG34:DH34=1))),IF(COLUMN(DI34)-MAX(COLUMN($AG34:DH34)*($AG34:DH34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DI34)-MAX(COLUMN($AG34:DH34)*($AG34:DH34=3))=$J34,3,0),IF(COLUMN(DI34)-MAX(COLUMN($AG34:DH34)*($AG34:DH34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DI34)*($AG34:DI34=1))>MAX(COLUMN($AG34:DI34)*($AG34:DI34=3)),MAX(COLUMN($AG34:DI34)*($AG34:DI34=1))>MAX(COLUMN($AG34:DI34)*($AG34:DI34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DJ34)-MAX(COLUMN($AG34:DI34)*($AG34:DI34=1))=$J34,3,0),IF(COLUMN(DJ34)-MAX(COLUMN($AG34:DI34)*($AG34:DI34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DI34)*($AG34:DI34=2))>MAX(COLUMN($AG34:DI34)*($AG34:DI34=3)),MAX(COLUMN($AG34:DI34)*($AG34:DI34=2))>MAX(COLUMN($AG34:DI34)*($AG34:DI34=1))),IF(COLUMN(DJ34)-MAX(COLUMN($AG34:DI34)*($AG34:DI34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DJ34)-MAX(COLUMN($AG34:DI34)*($AG34:DI34=3))=$J34,3,0),IF(COLUMN(DJ34)-MAX(COLUMN($AG34:DI34)*($AG34:DI34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=1))>MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=3)),MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=1))>MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DK34)-MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=1))=$J34,3,0),IF(COLUMN(DK34)-MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=2))>MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=3)),MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=2))>MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=1))),IF(COLUMN(DK34)-MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DK34)-MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=3))=$J34,3,0),IF(COLUMN(DK34)-MAX(COLUMN($AG34:DJ34)*($AG34:DJ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DK34)*($AG34:DK34=1))>MAX(COLUMN($AG34:DK34)*($AG34:DK34=3)),MAX(COLUMN($AG34:DK34)*($AG34:DK34=1))>MAX(COLUMN($AG34:DK34)*($AG34:DK34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DL34)-MAX(COLUMN($AG34:DK34)*($AG34:DK34=1))=$J34,3,0),IF(COLUMN(DL34)-MAX(COLUMN($AG34:DK34)*($AG34:DK34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DK34)*($AG34:DK34=2))>MAX(COLUMN($AG34:DK34)*($AG34:DK34=3)),MAX(COLUMN($AG34:DK34)*($AG34:DK34=2))>MAX(COLUMN($AG34:DK34)*($AG34:DK34=1))),IF(COLUMN(DL34)-MAX(COLUMN($AG34:DK34)*($AG34:DK34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DL34)-MAX(COLUMN($AG34:DK34)*($AG34:DK34=3))=$J34,3,0),IF(COLUMN(DL34)-MAX(COLUMN($AG34:DK34)*($AG34:DK34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DL34)*($AG34:DL34=1))>MAX(COLUMN($AG34:DL34)*($AG34:DL34=3)),MAX(COLUMN($AG34:DL34)*($AG34:DL34=1))>MAX(COLUMN($AG34:DL34)*($AG34:DL34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DM34)-MAX(COLUMN($AG34:DL34)*($AG34:DL34=1))=$J34,3,0),IF(COLUMN(DM34)-MAX(COLUMN($AG34:DL34)*($AG34:DL34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DL34)*($AG34:DL34=2))>MAX(COLUMN($AG34:DL34)*($AG34:DL34=3)),MAX(COLUMN($AG34:DL34)*($AG34:DL34=2))>MAX(COLUMN($AG34:DL34)*($AG34:DL34=1))),IF(COLUMN(DM34)-MAX(COLUMN($AG34:DL34)*($AG34:DL34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DM34)-MAX(COLUMN($AG34:DL34)*($AG34:DL34=3))=$J34,3,0),IF(COLUMN(DM34)-MAX(COLUMN($AG34:DL34)*($AG34:DL34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DM34)*($AG34:DM34=1))>MAX(COLUMN($AG34:DM34)*($AG34:DM34=3)),MAX(COLUMN($AG34:DM34)*($AG34:DM34=1))>MAX(COLUMN($AG34:DM34)*($AG34:DM34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DN34)-MAX(COLUMN($AG34:DM34)*($AG34:DM34=1))=$J34,3,0),IF(COLUMN(DN34)-MAX(COLUMN($AG34:DM34)*($AG34:DM34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DM34)*($AG34:DM34=2))>MAX(COLUMN($AG34:DM34)*($AG34:DM34=3)),MAX(COLUMN($AG34:DM34)*($AG34:DM34=2))>MAX(COLUMN($AG34:DM34)*($AG34:DM34=1))),IF(COLUMN(DN34)-MAX(COLUMN($AG34:DM34)*($AG34:DM34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DN34)-MAX(COLUMN($AG34:DM34)*($AG34:DM34=3))=$J34,3,0),IF(COLUMN(DN34)-MAX(COLUMN($AG34:DM34)*($AG34:DM34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DN34)*($AG34:DN34=1))>MAX(COLUMN($AG34:DN34)*($AG34:DN34=3)),MAX(COLUMN($AG34:DN34)*($AG34:DN34=1))>MAX(COLUMN($AG34:DN34)*($AG34:DN34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DO34)-MAX(COLUMN($AG34:DN34)*($AG34:DN34=1))=$J34,3,0),IF(COLUMN(DO34)-MAX(COLUMN($AG34:DN34)*($AG34:DN34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DN34)*($AG34:DN34=2))>MAX(COLUMN($AG34:DN34)*($AG34:DN34=3)),MAX(COLUMN($AG34:DN34)*($AG34:DN34=2))>MAX(COLUMN($AG34:DN34)*($AG34:DN34=1))),IF(COLUMN(DO34)-MAX(COLUMN($AG34:DN34)*($AG34:DN34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DO34)-MAX(COLUMN($AG34:DN34)*($AG34:DN34=3))=$J34,3,0),IF(COLUMN(DO34)-MAX(COLUMN($AG34:DN34)*($AG34:DN34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DO34)*($AG34:DO34=1))>MAX(COLUMN($AG34:DO34)*($AG34:DO34=3)),MAX(COLUMN($AG34:DO34)*($AG34:DO34=1))>MAX(COLUMN($AG34:DO34)*($AG34:DO34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DP34)-MAX(COLUMN($AG34:DO34)*($AG34:DO34=1))=$J34,3,0),IF(COLUMN(DP34)-MAX(COLUMN($AG34:DO34)*($AG34:DO34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DO34)*($AG34:DO34=2))>MAX(COLUMN($AG34:DO34)*($AG34:DO34=3)),MAX(COLUMN($AG34:DO34)*($AG34:DO34=2))>MAX(COLUMN($AG34:DO34)*($AG34:DO34=1))),IF(COLUMN(DP34)-MAX(COLUMN($AG34:DO34)*($AG34:DO34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DP34)-MAX(COLUMN($AG34:DO34)*($AG34:DO34=3))=$J34,3,0),IF(COLUMN(DP34)-MAX(COLUMN($AG34:DO34)*($AG34:DO34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DP34)*($AG34:DP34=1))>MAX(COLUMN($AG34:DP34)*($AG34:DP34=3)),MAX(COLUMN($AG34:DP34)*($AG34:DP34=1))>MAX(COLUMN($AG34:DP34)*($AG34:DP34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DQ34)-MAX(COLUMN($AG34:DP34)*($AG34:DP34=1))=$J34,3,0),IF(COLUMN(DQ34)-MAX(COLUMN($AG34:DP34)*($AG34:DP34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DP34)*($AG34:DP34=2))>MAX(COLUMN($AG34:DP34)*($AG34:DP34=3)),MAX(COLUMN($AG34:DP34)*($AG34:DP34=2))>MAX(COLUMN($AG34:DP34)*($AG34:DP34=1))),IF(COLUMN(DQ34)-MAX(COLUMN($AG34:DP34)*($AG34:DP34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DQ34)-MAX(COLUMN($AG34:DP34)*($AG34:DP34=3))=$J34,3,0),IF(COLUMN(DQ34)-MAX(COLUMN($AG34:DP34)*($AG34:DP34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=1))>MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=3)),MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=1))>MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DR34)-MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=1))=$J34,3,0),IF(COLUMN(DR34)-MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=2))>MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=3)),MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=2))>MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=1))),IF(COLUMN(DR34)-MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DR34)-MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=3))=$J34,3,0),IF(COLUMN(DR34)-MAX(COLUMN($AG34:DQ34)*($AG34:DQ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DR34)*($AG34:DR34=1))>MAX(COLUMN($AG34:DR34)*($AG34:DR34=3)),MAX(COLUMN($AG34:DR34)*($AG34:DR34=1))>MAX(COLUMN($AG34:DR34)*($AG34:DR34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DS34)-MAX(COLUMN($AG34:DR34)*($AG34:DR34=1))=$J34,3,0),IF(COLUMN(DS34)-MAX(COLUMN($AG34:DR34)*($AG34:DR34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DR34)*($AG34:DR34=2))>MAX(COLUMN($AG34:DR34)*($AG34:DR34=3)),MAX(COLUMN($AG34:DR34)*($AG34:DR34=2))>MAX(COLUMN($AG34:DR34)*($AG34:DR34=1))),IF(COLUMN(DS34)-MAX(COLUMN($AG34:DR34)*($AG34:DR34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DS34)-MAX(COLUMN($AG34:DR34)*($AG34:DR34=3))=$J34,3,0),IF(COLUMN(DS34)-MAX(COLUMN($AG34:DR34)*($AG34:DR34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DS34)*($AG34:DS34=1))>MAX(COLUMN($AG34:DS34)*($AG34:DS34=3)),MAX(COLUMN($AG34:DS34)*($AG34:DS34=1))>MAX(COLUMN($AG34:DS34)*($AG34:DS34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DT34)-MAX(COLUMN($AG34:DS34)*($AG34:DS34=1))=$J34,3,0),IF(COLUMN(DT34)-MAX(COLUMN($AG34:DS34)*($AG34:DS34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DS34)*($AG34:DS34=2))>MAX(COLUMN($AG34:DS34)*($AG34:DS34=3)),MAX(COLUMN($AG34:DS34)*($AG34:DS34=2))>MAX(COLUMN($AG34:DS34)*($AG34:DS34=1))),IF(COLUMN(DT34)-MAX(COLUMN($AG34:DS34)*($AG34:DS34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DT34)-MAX(COLUMN($AG34:DS34)*($AG34:DS34=3))=$J34,3,0),IF(COLUMN(DT34)-MAX(COLUMN($AG34:DS34)*($AG34:DS34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DT34)*($AG34:DT34=1))>MAX(COLUMN($AG34:DT34)*($AG34:DT34=3)),MAX(COLUMN($AG34:DT34)*($AG34:DT34=1))>MAX(COLUMN($AG34:DT34)*($AG34:DT34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DU34)-MAX(COLUMN($AG34:DT34)*($AG34:DT34=1))=$J34,3,0),IF(COLUMN(DU34)-MAX(COLUMN($AG34:DT34)*($AG34:DT34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DT34)*($AG34:DT34=2))>MAX(COLUMN($AG34:DT34)*($AG34:DT34=3)),MAX(COLUMN($AG34:DT34)*($AG34:DT34=2))>MAX(COLUMN($AG34:DT34)*($AG34:DT34=1))),IF(COLUMN(DU34)-MAX(COLUMN($AG34:DT34)*($AG34:DT34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DU34)-MAX(COLUMN($AG34:DT34)*($AG34:DT34=3))=$J34,3,0),IF(COLUMN(DU34)-MAX(COLUMN($AG34:DT34)*($AG34:DT34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DU34)*($AG34:DU34=1))>MAX(COLUMN($AG34:DU34)*($AG34:DU34=3)),MAX(COLUMN($AG34:DU34)*($AG34:DU34=1))>MAX(COLUMN($AG34:DU34)*($AG34:DU34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DV34)-MAX(COLUMN($AG34:DU34)*($AG34:DU34=1))=$J34,3,0),IF(COLUMN(DV34)-MAX(COLUMN($AG34:DU34)*($AG34:DU34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DU34)*($AG34:DU34=2))>MAX(COLUMN($AG34:DU34)*($AG34:DU34=3)),MAX(COLUMN($AG34:DU34)*($AG34:DU34=2))>MAX(COLUMN($AG34:DU34)*($AG34:DU34=1))),IF(COLUMN(DV34)-MAX(COLUMN($AG34:DU34)*($AG34:DU34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DV34)-MAX(COLUMN($AG34:DU34)*($AG34:DU34=3))=$J34,3,0),IF(COLUMN(DV34)-MAX(COLUMN($AG34:DU34)*($AG34:DU34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DV34)*($AG34:DV34=1))>MAX(COLUMN($AG34:DV34)*($AG34:DV34=3)),MAX(COLUMN($AG34:DV34)*($AG34:DV34=1))>MAX(COLUMN($AG34:DV34)*($AG34:DV34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DW34)-MAX(COLUMN($AG34:DV34)*($AG34:DV34=1))=$J34,3,0),IF(COLUMN(DW34)-MAX(COLUMN($AG34:DV34)*($AG34:DV34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DV34)*($AG34:DV34=2))>MAX(COLUMN($AG34:DV34)*($AG34:DV34=3)),MAX(COLUMN($AG34:DV34)*($AG34:DV34=2))>MAX(COLUMN($AG34:DV34)*($AG34:DV34=1))),IF(COLUMN(DW34)-MAX(COLUMN($AG34:DV34)*($AG34:DV34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DW34)-MAX(COLUMN($AG34:DV34)*($AG34:DV34=3))=$J34,3,0),IF(COLUMN(DW34)-MAX(COLUMN($AG34:DV34)*($AG34:DV34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DW34)*($AG34:DW34=1))>MAX(COLUMN($AG34:DW34)*($AG34:DW34=3)),MAX(COLUMN($AG34:DW34)*($AG34:DW34=1))>MAX(COLUMN($AG34:DW34)*($AG34:DW34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DX34)-MAX(COLUMN($AG34:DW34)*($AG34:DW34=1))=$J34,3,0),IF(COLUMN(DX34)-MAX(COLUMN($AG34:DW34)*($AG34:DW34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DW34)*($AG34:DW34=2))>MAX(COLUMN($AG34:DW34)*($AG34:DW34=3)),MAX(COLUMN($AG34:DW34)*($AG34:DW34=2))>MAX(COLUMN($AG34:DW34)*($AG34:DW34=1))),IF(COLUMN(DX34)-MAX(COLUMN($AG34:DW34)*($AG34:DW34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DX34)-MAX(COLUMN($AG34:DW34)*($AG34:DW34=3))=$J34,3,0),IF(COLUMN(DX34)-MAX(COLUMN($AG34:DW34)*($AG34:DW34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DX34)*($AG34:DX34=1))>MAX(COLUMN($AG34:DX34)*($AG34:DX34=3)),MAX(COLUMN($AG34:DX34)*($AG34:DX34=1))>MAX(COLUMN($AG34:DX34)*($AG34:DX34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DY34)-MAX(COLUMN($AG34:DX34)*($AG34:DX34=1))=$J34,3,0),IF(COLUMN(DY34)-MAX(COLUMN($AG34:DX34)*($AG34:DX34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DX34)*($AG34:DX34=2))>MAX(COLUMN($AG34:DX34)*($AG34:DX34=3)),MAX(COLUMN($AG34:DX34)*($AG34:DX34=2))>MAX(COLUMN($AG34:DX34)*($AG34:DX34=1))),IF(COLUMN(DY34)-MAX(COLUMN($AG34:DX34)*($AG34:DX34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DY34)-MAX(COLUMN($AG34:DX34)*($AG34:DX34=3))=$J34,3,0),IF(COLUMN(DY34)-MAX(COLUMN($AG34:DX34)*($AG34:DX34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DY34)*($AG34:DY34=1))>MAX(COLUMN($AG34:DY34)*($AG34:DY34=3)),MAX(COLUMN($AG34:DY34)*($AG34:DY34=1))>MAX(COLUMN($AG34:DY34)*($AG34:DY34=2))),IF($K34=\"Not Possible\",IF(COLUMN(DZ34)-MAX(COLUMN($AG34:DY34)*($AG34:DY34=1))=$J34,3,0),IF(COLUMN(DZ34)-MAX(COLUMN($AG34:DY34)*($AG34:DY34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DY34)*($AG34:DY34=2))>MAX(COLUMN($AG34:DY34)*($AG34:DY34=3)),MAX(COLUMN($AG34:DY34)*($AG34:DY34=2))>MAX(COLUMN($AG34:DY34)*($AG34:DY34=1))),IF(COLUMN(DZ34)-MAX(COLUMN($AG34:DY34)*($AG34:DY34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(DZ34)-MAX(COLUMN($AG34:DY34)*($AG34:DY34=3))=$J34,3,0),IF(COLUMN(DZ34)-MAX(COLUMN($AG34:DY34)*($AG34:DY34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=1))>MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=3)),MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=1))>MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=2))),IF($K34=\"Not Possible\",IF(COLUMN(EA34)-MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=1))=$J34,3,0),IF(COLUMN(EA34)-MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=2))>MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=3)),MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=2))>MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=1))),IF(COLUMN(EA34)-MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(EA34)-MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=3))=$J34,3,0),IF(COLUMN(EA34)-MAX(COLUMN($AG34:DZ34)*($AG34:DZ34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:EA34)*($AG34:EA34=1))>MAX(COLUMN($AG34:EA34)*($AG34:EA34=3)),MAX(COLUMN($AG34:EA34)*($AG34:EA34=1))>MAX(COLUMN($AG34:EA34)*($AG34:EA34=2))),IF($K34=\"Not Possible\",IF(COLUMN(EB34)-MAX(COLUMN($AG34:EA34)*($AG34:EA34=1))=$J34,3,0),IF(COLUMN(EB34)-MAX(COLUMN($AG34:EA34)*($AG34:EA34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:EA34)*($AG34:EA34=2))>MAX(COLUMN($AG34:EA34)*($AG34:EA34=3)),MAX(COLUMN($AG34:EA34)*($AG34:EA34=2))>MAX(COLUMN($AG34:EA34)*($AG34:EA34=1))),IF(COLUMN(EB34)-MAX(COLUMN($AG34:EA34)*($AG34:EA34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(EB34)-MAX(COLUMN($AG34:EA34)*($AG34:EA34=3))=$J34,3,0),IF(COLUMN(EB34)-MAX(COLUMN($AG34:EA34)*($AG34:EA34=3))=$J34,2,0)))))","v":0},{"$f":"IF($AG34=4,0,IF(AND(MAX(COLUMN($AG34:EB34)*($AG34:EB34=1))>MAX(COLUMN($AG34:EB34)*($AG34:EB34=3)),MAX(COLUMN($AG34:EB34)*($AG34:EB34=1))>MAX(COLUMN($AG34:EB34)*($AG34:EB34=2))),IF($K34=\"Not Possible\",IF(COLUMN(EC34)-MAX(COLUMN($AG34:EB34)*($AG34:EB34=1))=$J34,3,0),IF(COLUMN(EC34)-MAX(COLUMN($AG34:EB34)*($AG34:EB34=1))=$J34,2,0)),IF(AND(MAX(COLUMN($AG34:EB34)*($AG34:EB34=2))>MAX(COLUMN($AG34:EB34)*($AG34:EB34=3)),MAX(COLUMN($AG34:EB34)*($AG34:EB34=2))>MAX(COLUMN($AG34:EB34)*($AG34:EB34=1))),IF(COLUMN(EC34)-MAX(COLUMN($AG34:EB34)*($AG34:EB34=2))=$L34,3,0),IF($K34=\"Not Possible\",IF(COLUMN(EC34)-MAX(COLUMN($AG34:EB34)*($AG34:EB34=3))=$J34,3,0),IF(COLUMN(EC34)-MAX(COLUMN($AG34:EB34)*($AG34:EB34=3))=$J34,2,0)))))","v":3}]
[null,null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"BridEA03"},"Footbridge",{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset class],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"Bridge - Pedestrian"},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",Form_Asset[[#This Row],[Asset ID]]&ROW())","v":"BridEA0335"},"Handrail","Barriers",{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",INDEX(AssetListTbl[Best Estimate Life (5)],(MATCH(Form_Asset[[#This Row],[Sub-Asset category]],AssetListTbl[Sub-Element Category],0))))","v":60},40,"Minor Refurbishment",20,"New Build",{"$f":"MAX(COLUMN($AH35:EC35)*($AH35:EC35=2))","v":133},{"$f":"MAX(COLUMN($AH35:EC35)*($AH35:EC35=3))","v":93},{"$f":"IFERROR(100-(IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Replace]])),INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Refurb]])))),0)","v":100},{"$f":"IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],3,2)","v":2},{"$f":"SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Product_Stage[CO2e (t)])","v":885.6},{"$f":"IFERROR(SUM(Form_Elements[General Item Material])*(Form_Asset[[#This Row],[Weighted Split]]/SUM(Form_Asset[Weighted Split]))+Form_Asset[[#This Row],[Weighted Split]],0)","v":885.6},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth (wtt)]))+(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Transport]))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0.28638398574999996},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Non contractor People Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Contractor people transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":4.914103145256111},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0.1297557076323646},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Site establishment])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":5.525164254017497},{"$f":"IFERROR(IF($D$88=\"Summary\",((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),(SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Const_Ins_InsB[CO2e (t)]))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Other Construction Waste])*Form_Asset[[#This Row],[Weighted Split]]/(SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[[Waste Co2e ]])+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":3.1002867585E-2},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New build\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]]),IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",(SUM(Form_Asset[[#This Row],[Materials]:[Waste]])-(SUM(Form_Asset[[#This Row],[Materials Transport]],Form_Asset[[#This Row],[People Transport]]*0.5,Form_Asset[[#This Row],[Plant Transport]]*0.5))),IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]])/(SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%])),0)))","v":896.48640996024108},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":5.5037538264366651E-2},{"$f":"IFERROR(SUMIF(Form_use_energy[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_use_energy[CO2e (t)]),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset ref.]]=\"\",0,SUMIF(Form_Asset[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Asset[New Build Co2e])*SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%]))","v":89.648640996024113},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Dem - General Item Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Dem -Waste Co2e]),0)","v":0.58905448411499983},{"$f":"(Form_Asset[[#This Row],[Plant use]]+Form_Asset[[#This Row],[Plant Transport]])*50%","v":6.4877853816182302E-2},{"$f":"Form_Asset[[#This Row],[People Transport]]*50%","v":2.4570515726280555},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New Build\",1,IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",2,IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",3,IF(Form_Asset[[#This Row],[First intervention]]=\"Demolition\",4,\"\"))))","v":1},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AG35)*($AG35:AG35=1))>MAX(COLUMN($AG35:AG35)*($AG35:AG35=3)),MAX(COLUMN($AG35:AG35)*($AG35:AG35=1))>MAX(COLUMN($AG35:AG35)*($AG35:AG35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AH35)-MAX(COLUMN($AG35:AG35)*($AG35:AG35=1))=$J35,3,0),IF(COLUMN(AH35)-MAX(COLUMN($AG35:AG35)*($AG35:AG35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AG35)*($AG35:AG35=2))>MAX(COLUMN($AG35:AG35)*($AG35:AG35=3)),MAX(COLUMN($AG35:AG35)*($AG35:AG35=2))>MAX(COLUMN($AG35:AG35)*($AG35:AG35=1))),IF(COLUMN(AH35)-MAX(COLUMN($AG35:AG35)*($AG35:AG35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AH35)-MAX(COLUMN($AG35:AG35)*($AG35:AG35=3))=$J35,3,0),IF(COLUMN(AH35)-MAX(COLUMN($AG35:AG35)*($AG35:AG35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AH35)*($AG35:AH35=1))>MAX(COLUMN($AG35:AH35)*($AG35:AH35=3)),MAX(COLUMN($AG35:AH35)*($AG35:AH35=1))>MAX(COLUMN($AG35:AH35)*($AG35:AH35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AI35)-MAX(COLUMN($AG35:AH35)*($AG35:AH35=1))=$J35,3,0),IF(COLUMN(AI35)-MAX(COLUMN($AG35:AH35)*($AG35:AH35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AH35)*($AG35:AH35=2))>MAX(COLUMN($AG35:AH35)*($AG35:AH35=3)),MAX(COLUMN($AG35:AH35)*($AG35:AH35=2))>MAX(COLUMN($AG35:AH35)*($AG35:AH35=1))),IF(COLUMN(AI35)-MAX(COLUMN($AG35:AH35)*($AG35:AH35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AI35)-MAX(COLUMN($AG35:AH35)*($AG35:AH35=3))=$J35,3,0),IF(COLUMN(AI35)-MAX(COLUMN($AG35:AH35)*($AG35:AH35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AI35)*($AG35:AI35=1))>MAX(COLUMN($AG35:AI35)*($AG35:AI35=3)),MAX(COLUMN($AG35:AI35)*($AG35:AI35=1))>MAX(COLUMN($AG35:AI35)*($AG35:AI35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AJ35)-MAX(COLUMN($AG35:AI35)*($AG35:AI35=1))=$J35,3,0),IF(COLUMN(AJ35)-MAX(COLUMN($AG35:AI35)*($AG35:AI35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AI35)*($AG35:AI35=2))>MAX(COLUMN($AG35:AI35)*($AG35:AI35=3)),MAX(COLUMN($AG35:AI35)*($AG35:AI35=2))>MAX(COLUMN($AG35:AI35)*($AG35:AI35=1))),IF(COLUMN(AJ35)-MAX(COLUMN($AG35:AI35)*($AG35:AI35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AJ35)-MAX(COLUMN($AG35:AI35)*($AG35:AI35=3))=$J35,3,0),IF(COLUMN(AJ35)-MAX(COLUMN($AG35:AI35)*($AG35:AI35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=1))>MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=3)),MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=1))>MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AK35)-MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=1))=$J35,3,0),IF(COLUMN(AK35)-MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=2))>MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=3)),MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=2))>MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=1))),IF(COLUMN(AK35)-MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AK35)-MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=3))=$J35,3,0),IF(COLUMN(AK35)-MAX(COLUMN($AG35:AJ35)*($AG35:AJ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AK35)*($AG35:AK35=1))>MAX(COLUMN($AG35:AK35)*($AG35:AK35=3)),MAX(COLUMN($AG35:AK35)*($AG35:AK35=1))>MAX(COLUMN($AG35:AK35)*($AG35:AK35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AL35)-MAX(COLUMN($AG35:AK35)*($AG35:AK35=1))=$J35,3,0),IF(COLUMN(AL35)-MAX(COLUMN($AG35:AK35)*($AG35:AK35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AK35)*($AG35:AK35=2))>MAX(COLUMN($AG35:AK35)*($AG35:AK35=3)),MAX(COLUMN($AG35:AK35)*($AG35:AK35=2))>MAX(COLUMN($AG35:AK35)*($AG35:AK35=1))),IF(COLUMN(AL35)-MAX(COLUMN($AG35:AK35)*($AG35:AK35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AL35)-MAX(COLUMN($AG35:AK35)*($AG35:AK35=3))=$J35,3,0),IF(COLUMN(AL35)-MAX(COLUMN($AG35:AK35)*($AG35:AK35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AL35)*($AG35:AL35=1))>MAX(COLUMN($AG35:AL35)*($AG35:AL35=3)),MAX(COLUMN($AG35:AL35)*($AG35:AL35=1))>MAX(COLUMN($AG35:AL35)*($AG35:AL35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AM35)-MAX(COLUMN($AG35:AL35)*($AG35:AL35=1))=$J35,3,0),IF(COLUMN(AM35)-MAX(COLUMN($AG35:AL35)*($AG35:AL35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AL35)*($AG35:AL35=2))>MAX(COLUMN($AG35:AL35)*($AG35:AL35=3)),MAX(COLUMN($AG35:AL35)*($AG35:AL35=2))>MAX(COLUMN($AG35:AL35)*($AG35:AL35=1))),IF(COLUMN(AM35)-MAX(COLUMN($AG35:AL35)*($AG35:AL35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AM35)-MAX(COLUMN($AG35:AL35)*($AG35:AL35=3))=$J35,3,0),IF(COLUMN(AM35)-MAX(COLUMN($AG35:AL35)*($AG35:AL35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AM35)*($AG35:AM35=1))>MAX(COLUMN($AG35:AM35)*($AG35:AM35=3)),MAX(COLUMN($AG35:AM35)*($AG35:AM35=1))>MAX(COLUMN($AG35:AM35)*($AG35:AM35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AN35)-MAX(COLUMN($AG35:AM35)*($AG35:AM35=1))=$J35,3,0),IF(COLUMN(AN35)-MAX(COLUMN($AG35:AM35)*($AG35:AM35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AM35)*($AG35:AM35=2))>MAX(COLUMN($AG35:AM35)*($AG35:AM35=3)),MAX(COLUMN($AG35:AM35)*($AG35:AM35=2))>MAX(COLUMN($AG35:AM35)*($AG35:AM35=1))),IF(COLUMN(AN35)-MAX(COLUMN($AG35:AM35)*($AG35:AM35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AN35)-MAX(COLUMN($AG35:AM35)*($AG35:AM35=3))=$J35,3,0),IF(COLUMN(AN35)-MAX(COLUMN($AG35:AM35)*($AG35:AM35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AN35)*($AG35:AN35=1))>MAX(COLUMN($AG35:AN35)*($AG35:AN35=3)),MAX(COLUMN($AG35:AN35)*($AG35:AN35=1))>MAX(COLUMN($AG35:AN35)*($AG35:AN35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AO35)-MAX(COLUMN($AG35:AN35)*($AG35:AN35=1))=$J35,3,0),IF(COLUMN(AO35)-MAX(COLUMN($AG35:AN35)*($AG35:AN35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AN35)*($AG35:AN35=2))>MAX(COLUMN($AG35:AN35)*($AG35:AN35=3)),MAX(COLUMN($AG35:AN35)*($AG35:AN35=2))>MAX(COLUMN($AG35:AN35)*($AG35:AN35=1))),IF(COLUMN(AO35)-MAX(COLUMN($AG35:AN35)*($AG35:AN35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AO35)-MAX(COLUMN($AG35:AN35)*($AG35:AN35=3))=$J35,3,0),IF(COLUMN(AO35)-MAX(COLUMN($AG35:AN35)*($AG35:AN35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AO35)*($AG35:AO35=1))>MAX(COLUMN($AG35:AO35)*($AG35:AO35=3)),MAX(COLUMN($AG35:AO35)*($AG35:AO35=1))>MAX(COLUMN($AG35:AO35)*($AG35:AO35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AP35)-MAX(COLUMN($AG35:AO35)*($AG35:AO35=1))=$J35,3,0),IF(COLUMN(AP35)-MAX(COLUMN($AG35:AO35)*($AG35:AO35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AO35)*($AG35:AO35=2))>MAX(COLUMN($AG35:AO35)*($AG35:AO35=3)),MAX(COLUMN($AG35:AO35)*($AG35:AO35=2))>MAX(COLUMN($AG35:AO35)*($AG35:AO35=1))),IF(COLUMN(AP35)-MAX(COLUMN($AG35:AO35)*($AG35:AO35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AP35)-MAX(COLUMN($AG35:AO35)*($AG35:AO35=3))=$J35,3,0),IF(COLUMN(AP35)-MAX(COLUMN($AG35:AO35)*($AG35:AO35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AP35)*($AG35:AP35=1))>MAX(COLUMN($AG35:AP35)*($AG35:AP35=3)),MAX(COLUMN($AG35:AP35)*($AG35:AP35=1))>MAX(COLUMN($AG35:AP35)*($AG35:AP35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AQ35)-MAX(COLUMN($AG35:AP35)*($AG35:AP35=1))=$J35,3,0),IF(COLUMN(AQ35)-MAX(COLUMN($AG35:AP35)*($AG35:AP35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AP35)*($AG35:AP35=2))>MAX(COLUMN($AG35:AP35)*($AG35:AP35=3)),MAX(COLUMN($AG35:AP35)*($AG35:AP35=2))>MAX(COLUMN($AG35:AP35)*($AG35:AP35=1))),IF(COLUMN(AQ35)-MAX(COLUMN($AG35:AP35)*($AG35:AP35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AQ35)-MAX(COLUMN($AG35:AP35)*($AG35:AP35=3))=$J35,3,0),IF(COLUMN(AQ35)-MAX(COLUMN($AG35:AP35)*($AG35:AP35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=1))>MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=3)),MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=1))>MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AR35)-MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=1))=$J35,3,0),IF(COLUMN(AR35)-MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=2))>MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=3)),MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=2))>MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=1))),IF(COLUMN(AR35)-MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AR35)-MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=3))=$J35,3,0),IF(COLUMN(AR35)-MAX(COLUMN($AG35:AQ35)*($AG35:AQ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AR35)*($AG35:AR35=1))>MAX(COLUMN($AG35:AR35)*($AG35:AR35=3)),MAX(COLUMN($AG35:AR35)*($AG35:AR35=1))>MAX(COLUMN($AG35:AR35)*($AG35:AR35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AS35)-MAX(COLUMN($AG35:AR35)*($AG35:AR35=1))=$J35,3,0),IF(COLUMN(AS35)-MAX(COLUMN($AG35:AR35)*($AG35:AR35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AR35)*($AG35:AR35=2))>MAX(COLUMN($AG35:AR35)*($AG35:AR35=3)),MAX(COLUMN($AG35:AR35)*($AG35:AR35=2))>MAX(COLUMN($AG35:AR35)*($AG35:AR35=1))),IF(COLUMN(AS35)-MAX(COLUMN($AG35:AR35)*($AG35:AR35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AS35)-MAX(COLUMN($AG35:AR35)*($AG35:AR35=3))=$J35,3,0),IF(COLUMN(AS35)-MAX(COLUMN($AG35:AR35)*($AG35:AR35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AS35)*($AG35:AS35=1))>MAX(COLUMN($AG35:AS35)*($AG35:AS35=3)),MAX(COLUMN($AG35:AS35)*($AG35:AS35=1))>MAX(COLUMN($AG35:AS35)*($AG35:AS35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AT35)-MAX(COLUMN($AG35:AS35)*($AG35:AS35=1))=$J35,3,0),IF(COLUMN(AT35)-MAX(COLUMN($AG35:AS35)*($AG35:AS35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AS35)*($AG35:AS35=2))>MAX(COLUMN($AG35:AS35)*($AG35:AS35=3)),MAX(COLUMN($AG35:AS35)*($AG35:AS35=2))>MAX(COLUMN($AG35:AS35)*($AG35:AS35=1))),IF(COLUMN(AT35)-MAX(COLUMN($AG35:AS35)*($AG35:AS35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AT35)-MAX(COLUMN($AG35:AS35)*($AG35:AS35=3))=$J35,3,0),IF(COLUMN(AT35)-MAX(COLUMN($AG35:AS35)*($AG35:AS35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AT35)*($AG35:AT35=1))>MAX(COLUMN($AG35:AT35)*($AG35:AT35=3)),MAX(COLUMN($AG35:AT35)*($AG35:AT35=1))>MAX(COLUMN($AG35:AT35)*($AG35:AT35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AU35)-MAX(COLUMN($AG35:AT35)*($AG35:AT35=1))=$J35,3,0),IF(COLUMN(AU35)-MAX(COLUMN($AG35:AT35)*($AG35:AT35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AT35)*($AG35:AT35=2))>MAX(COLUMN($AG35:AT35)*($AG35:AT35=3)),MAX(COLUMN($AG35:AT35)*($AG35:AT35=2))>MAX(COLUMN($AG35:AT35)*($AG35:AT35=1))),IF(COLUMN(AU35)-MAX(COLUMN($AG35:AT35)*($AG35:AT35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AU35)-MAX(COLUMN($AG35:AT35)*($AG35:AT35=3))=$J35,3,0),IF(COLUMN(AU35)-MAX(COLUMN($AG35:AT35)*($AG35:AT35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AU35)*($AG35:AU35=1))>MAX(COLUMN($AG35:AU35)*($AG35:AU35=3)),MAX(COLUMN($AG35:AU35)*($AG35:AU35=1))>MAX(COLUMN($AG35:AU35)*($AG35:AU35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AV35)-MAX(COLUMN($AG35:AU35)*($AG35:AU35=1))=$J35,3,0),IF(COLUMN(AV35)-MAX(COLUMN($AG35:AU35)*($AG35:AU35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AU35)*($AG35:AU35=2))>MAX(COLUMN($AG35:AU35)*($AG35:AU35=3)),MAX(COLUMN($AG35:AU35)*($AG35:AU35=2))>MAX(COLUMN($AG35:AU35)*($AG35:AU35=1))),IF(COLUMN(AV35)-MAX(COLUMN($AG35:AU35)*($AG35:AU35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AV35)-MAX(COLUMN($AG35:AU35)*($AG35:AU35=3))=$J35,3,0),IF(COLUMN(AV35)-MAX(COLUMN($AG35:AU35)*($AG35:AU35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AV35)*($AG35:AV35=1))>MAX(COLUMN($AG35:AV35)*($AG35:AV35=3)),MAX(COLUMN($AG35:AV35)*($AG35:AV35=1))>MAX(COLUMN($AG35:AV35)*($AG35:AV35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AW35)-MAX(COLUMN($AG35:AV35)*($AG35:AV35=1))=$J35,3,0),IF(COLUMN(AW35)-MAX(COLUMN($AG35:AV35)*($AG35:AV35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AV35)*($AG35:AV35=2))>MAX(COLUMN($AG35:AV35)*($AG35:AV35=3)),MAX(COLUMN($AG35:AV35)*($AG35:AV35=2))>MAX(COLUMN($AG35:AV35)*($AG35:AV35=1))),IF(COLUMN(AW35)-MAX(COLUMN($AG35:AV35)*($AG35:AV35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AW35)-MAX(COLUMN($AG35:AV35)*($AG35:AV35=3))=$J35,3,0),IF(COLUMN(AW35)-MAX(COLUMN($AG35:AV35)*($AG35:AV35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AW35)*($AG35:AW35=1))>MAX(COLUMN($AG35:AW35)*($AG35:AW35=3)),MAX(COLUMN($AG35:AW35)*($AG35:AW35=1))>MAX(COLUMN($AG35:AW35)*($AG35:AW35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AX35)-MAX(COLUMN($AG35:AW35)*($AG35:AW35=1))=$J35,3,0),IF(COLUMN(AX35)-MAX(COLUMN($AG35:AW35)*($AG35:AW35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AW35)*($AG35:AW35=2))>MAX(COLUMN($AG35:AW35)*($AG35:AW35=3)),MAX(COLUMN($AG35:AW35)*($AG35:AW35=2))>MAX(COLUMN($AG35:AW35)*($AG35:AW35=1))),IF(COLUMN(AX35)-MAX(COLUMN($AG35:AW35)*($AG35:AW35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AX35)-MAX(COLUMN($AG35:AW35)*($AG35:AW35=3))=$J35,3,0),IF(COLUMN(AX35)-MAX(COLUMN($AG35:AW35)*($AG35:AW35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AX35)*($AG35:AX35=1))>MAX(COLUMN($AG35:AX35)*($AG35:AX35=3)),MAX(COLUMN($AG35:AX35)*($AG35:AX35=1))>MAX(COLUMN($AG35:AX35)*($AG35:AX35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AY35)-MAX(COLUMN($AG35:AX35)*($AG35:AX35=1))=$J35,3,0),IF(COLUMN(AY35)-MAX(COLUMN($AG35:AX35)*($AG35:AX35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AX35)*($AG35:AX35=2))>MAX(COLUMN($AG35:AX35)*($AG35:AX35=3)),MAX(COLUMN($AG35:AX35)*($AG35:AX35=2))>MAX(COLUMN($AG35:AX35)*($AG35:AX35=1))),IF(COLUMN(AY35)-MAX(COLUMN($AG35:AX35)*($AG35:AX35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AY35)-MAX(COLUMN($AG35:AX35)*($AG35:AX35=3))=$J35,3,0),IF(COLUMN(AY35)-MAX(COLUMN($AG35:AX35)*($AG35:AX35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AY35)*($AG35:AY35=1))>MAX(COLUMN($AG35:AY35)*($AG35:AY35=3)),MAX(COLUMN($AG35:AY35)*($AG35:AY35=1))>MAX(COLUMN($AG35:AY35)*($AG35:AY35=2))),IF($K35=\"Not Possible\",IF(COLUMN(AZ35)-MAX(COLUMN($AG35:AY35)*($AG35:AY35=1))=$J35,3,0),IF(COLUMN(AZ35)-MAX(COLUMN($AG35:AY35)*($AG35:AY35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AY35)*($AG35:AY35=2))>MAX(COLUMN($AG35:AY35)*($AG35:AY35=3)),MAX(COLUMN($AG35:AY35)*($AG35:AY35=2))>MAX(COLUMN($AG35:AY35)*($AG35:AY35=1))),IF(COLUMN(AZ35)-MAX(COLUMN($AG35:AY35)*($AG35:AY35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(AZ35)-MAX(COLUMN($AG35:AY35)*($AG35:AY35=3))=$J35,3,0),IF(COLUMN(AZ35)-MAX(COLUMN($AG35:AY35)*($AG35:AY35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=1))>MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=3)),MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=1))>MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BA35)-MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=1))=$J35,3,0),IF(COLUMN(BA35)-MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=2))>MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=3)),MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=2))>MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=1))),IF(COLUMN(BA35)-MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BA35)-MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=3))=$J35,3,0),IF(COLUMN(BA35)-MAX(COLUMN($AG35:AZ35)*($AG35:AZ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BA35)*($AG35:BA35=1))>MAX(COLUMN($AG35:BA35)*($AG35:BA35=3)),MAX(COLUMN($AG35:BA35)*($AG35:BA35=1))>MAX(COLUMN($AG35:BA35)*($AG35:BA35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BB35)-MAX(COLUMN($AG35:BA35)*($AG35:BA35=1))=$J35,3,0),IF(COLUMN(BB35)-MAX(COLUMN($AG35:BA35)*($AG35:BA35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BA35)*($AG35:BA35=2))>MAX(COLUMN($AG35:BA35)*($AG35:BA35=3)),MAX(COLUMN($AG35:BA35)*($AG35:BA35=2))>MAX(COLUMN($AG35:BA35)*($AG35:BA35=1))),IF(COLUMN(BB35)-MAX(COLUMN($AG35:BA35)*($AG35:BA35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BB35)-MAX(COLUMN($AG35:BA35)*($AG35:BA35=3))=$J35,3,0),IF(COLUMN(BB35)-MAX(COLUMN($AG35:BA35)*($AG35:BA35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BB35)*($AG35:BB35=1))>MAX(COLUMN($AG35:BB35)*($AG35:BB35=3)),MAX(COLUMN($AG35:BB35)*($AG35:BB35=1))>MAX(COLUMN($AG35:BB35)*($AG35:BB35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BC35)-MAX(COLUMN($AG35:BB35)*($AG35:BB35=1))=$J35,3,0),IF(COLUMN(BC35)-MAX(COLUMN($AG35:BB35)*($AG35:BB35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BB35)*($AG35:BB35=2))>MAX(COLUMN($AG35:BB35)*($AG35:BB35=3)),MAX(COLUMN($AG35:BB35)*($AG35:BB35=2))>MAX(COLUMN($AG35:BB35)*($AG35:BB35=1))),IF(COLUMN(BC35)-MAX(COLUMN($AG35:BB35)*($AG35:BB35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BC35)-MAX(COLUMN($AG35:BB35)*($AG35:BB35=3))=$J35,3,0),IF(COLUMN(BC35)-MAX(COLUMN($AG35:BB35)*($AG35:BB35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BC35)*($AG35:BC35=1))>MAX(COLUMN($AG35:BC35)*($AG35:BC35=3)),MAX(COLUMN($AG35:BC35)*($AG35:BC35=1))>MAX(COLUMN($AG35:BC35)*($AG35:BC35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BD35)-MAX(COLUMN($AG35:BC35)*($AG35:BC35=1))=$J35,3,0),IF(COLUMN(BD35)-MAX(COLUMN($AG35:BC35)*($AG35:BC35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BC35)*($AG35:BC35=2))>MAX(COLUMN($AG35:BC35)*($AG35:BC35=3)),MAX(COLUMN($AG35:BC35)*($AG35:BC35=2))>MAX(COLUMN($AG35:BC35)*($AG35:BC35=1))),IF(COLUMN(BD35)-MAX(COLUMN($AG35:BC35)*($AG35:BC35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BD35)-MAX(COLUMN($AG35:BC35)*($AG35:BC35=3))=$J35,3,0),IF(COLUMN(BD35)-MAX(COLUMN($AG35:BC35)*($AG35:BC35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BD35)*($AG35:BD35=1))>MAX(COLUMN($AG35:BD35)*($AG35:BD35=3)),MAX(COLUMN($AG35:BD35)*($AG35:BD35=1))>MAX(COLUMN($AG35:BD35)*($AG35:BD35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BE35)-MAX(COLUMN($AG35:BD35)*($AG35:BD35=1))=$J35,3,0),IF(COLUMN(BE35)-MAX(COLUMN($AG35:BD35)*($AG35:BD35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BD35)*($AG35:BD35=2))>MAX(COLUMN($AG35:BD35)*($AG35:BD35=3)),MAX(COLUMN($AG35:BD35)*($AG35:BD35=2))>MAX(COLUMN($AG35:BD35)*($AG35:BD35=1))),IF(COLUMN(BE35)-MAX(COLUMN($AG35:BD35)*($AG35:BD35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BE35)-MAX(COLUMN($AG35:BD35)*($AG35:BD35=3))=$J35,3,0),IF(COLUMN(BE35)-MAX(COLUMN($AG35:BD35)*($AG35:BD35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BE35)*($AG35:BE35=1))>MAX(COLUMN($AG35:BE35)*($AG35:BE35=3)),MAX(COLUMN($AG35:BE35)*($AG35:BE35=1))>MAX(COLUMN($AG35:BE35)*($AG35:BE35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BF35)-MAX(COLUMN($AG35:BE35)*($AG35:BE35=1))=$J35,3,0),IF(COLUMN(BF35)-MAX(COLUMN($AG35:BE35)*($AG35:BE35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BE35)*($AG35:BE35=2))>MAX(COLUMN($AG35:BE35)*($AG35:BE35=3)),MAX(COLUMN($AG35:BE35)*($AG35:BE35=2))>MAX(COLUMN($AG35:BE35)*($AG35:BE35=1))),IF(COLUMN(BF35)-MAX(COLUMN($AG35:BE35)*($AG35:BE35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BF35)-MAX(COLUMN($AG35:BE35)*($AG35:BE35=3))=$J35,3,0),IF(COLUMN(BF35)-MAX(COLUMN($AG35:BE35)*($AG35:BE35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BF35)*($AG35:BF35=1))>MAX(COLUMN($AG35:BF35)*($AG35:BF35=3)),MAX(COLUMN($AG35:BF35)*($AG35:BF35=1))>MAX(COLUMN($AG35:BF35)*($AG35:BF35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BG35)-MAX(COLUMN($AG35:BF35)*($AG35:BF35=1))=$J35,3,0),IF(COLUMN(BG35)-MAX(COLUMN($AG35:BF35)*($AG35:BF35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BF35)*($AG35:BF35=2))>MAX(COLUMN($AG35:BF35)*($AG35:BF35=3)),MAX(COLUMN($AG35:BF35)*($AG35:BF35=2))>MAX(COLUMN($AG35:BF35)*($AG35:BF35=1))),IF(COLUMN(BG35)-MAX(COLUMN($AG35:BF35)*($AG35:BF35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BG35)-MAX(COLUMN($AG35:BF35)*($AG35:BF35=3))=$J35,3,0),IF(COLUMN(BG35)-MAX(COLUMN($AG35:BF35)*($AG35:BF35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BG35)*($AG35:BG35=1))>MAX(COLUMN($AG35:BG35)*($AG35:BG35=3)),MAX(COLUMN($AG35:BG35)*($AG35:BG35=1))>MAX(COLUMN($AG35:BG35)*($AG35:BG35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BH35)-MAX(COLUMN($AG35:BG35)*($AG35:BG35=1))=$J35,3,0),IF(COLUMN(BH35)-MAX(COLUMN($AG35:BG35)*($AG35:BG35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BG35)*($AG35:BG35=2))>MAX(COLUMN($AG35:BG35)*($AG35:BG35=3)),MAX(COLUMN($AG35:BG35)*($AG35:BG35=2))>MAX(COLUMN($AG35:BG35)*($AG35:BG35=1))),IF(COLUMN(BH35)-MAX(COLUMN($AG35:BG35)*($AG35:BG35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BH35)-MAX(COLUMN($AG35:BG35)*($AG35:BG35=3))=$J35,3,0),IF(COLUMN(BH35)-MAX(COLUMN($AG35:BG35)*($AG35:BG35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BH35)*($AG35:BH35=1))>MAX(COLUMN($AG35:BH35)*($AG35:BH35=3)),MAX(COLUMN($AG35:BH35)*($AG35:BH35=1))>MAX(COLUMN($AG35:BH35)*($AG35:BH35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BI35)-MAX(COLUMN($AG35:BH35)*($AG35:BH35=1))=$J35,3,0),IF(COLUMN(BI35)-MAX(COLUMN($AG35:BH35)*($AG35:BH35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BH35)*($AG35:BH35=2))>MAX(COLUMN($AG35:BH35)*($AG35:BH35=3)),MAX(COLUMN($AG35:BH35)*($AG35:BH35=2))>MAX(COLUMN($AG35:BH35)*($AG35:BH35=1))),IF(COLUMN(BI35)-MAX(COLUMN($AG35:BH35)*($AG35:BH35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BI35)-MAX(COLUMN($AG35:BH35)*($AG35:BH35=3))=$J35,3,0),IF(COLUMN(BI35)-MAX(COLUMN($AG35:BH35)*($AG35:BH35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BI35)*($AG35:BI35=1))>MAX(COLUMN($AG35:BI35)*($AG35:BI35=3)),MAX(COLUMN($AG35:BI35)*($AG35:BI35=1))>MAX(COLUMN($AG35:BI35)*($AG35:BI35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BJ35)-MAX(COLUMN($AG35:BI35)*($AG35:BI35=1))=$J35,3,0),IF(COLUMN(BJ35)-MAX(COLUMN($AG35:BI35)*($AG35:BI35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BI35)*($AG35:BI35=2))>MAX(COLUMN($AG35:BI35)*($AG35:BI35=3)),MAX(COLUMN($AG35:BI35)*($AG35:BI35=2))>MAX(COLUMN($AG35:BI35)*($AG35:BI35=1))),IF(COLUMN(BJ35)-MAX(COLUMN($AG35:BI35)*($AG35:BI35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BJ35)-MAX(COLUMN($AG35:BI35)*($AG35:BI35=3))=$J35,3,0),IF(COLUMN(BJ35)-MAX(COLUMN($AG35:BI35)*($AG35:BI35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=1))>MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=3)),MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=1))>MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BK35)-MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=1))=$J35,3,0),IF(COLUMN(BK35)-MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=2))>MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=3)),MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=2))>MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=1))),IF(COLUMN(BK35)-MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BK35)-MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=3))=$J35,3,0),IF(COLUMN(BK35)-MAX(COLUMN($AG35:BJ35)*($AG35:BJ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BK35)*($AG35:BK35=1))>MAX(COLUMN($AG35:BK35)*($AG35:BK35=3)),MAX(COLUMN($AG35:BK35)*($AG35:BK35=1))>MAX(COLUMN($AG35:BK35)*($AG35:BK35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BL35)-MAX(COLUMN($AG35:BK35)*($AG35:BK35=1))=$J35,3,0),IF(COLUMN(BL35)-MAX(COLUMN($AG35:BK35)*($AG35:BK35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BK35)*($AG35:BK35=2))>MAX(COLUMN($AG35:BK35)*($AG35:BK35=3)),MAX(COLUMN($AG35:BK35)*($AG35:BK35=2))>MAX(COLUMN($AG35:BK35)*($AG35:BK35=1))),IF(COLUMN(BL35)-MAX(COLUMN($AG35:BK35)*($AG35:BK35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BL35)-MAX(COLUMN($AG35:BK35)*($AG35:BK35=3))=$J35,3,0),IF(COLUMN(BL35)-MAX(COLUMN($AG35:BK35)*($AG35:BK35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BL35)*($AG35:BL35=1))>MAX(COLUMN($AG35:BL35)*($AG35:BL35=3)),MAX(COLUMN($AG35:BL35)*($AG35:BL35=1))>MAX(COLUMN($AG35:BL35)*($AG35:BL35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BM35)-MAX(COLUMN($AG35:BL35)*($AG35:BL35=1))=$J35,3,0),IF(COLUMN(BM35)-MAX(COLUMN($AG35:BL35)*($AG35:BL35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BL35)*($AG35:BL35=2))>MAX(COLUMN($AG35:BL35)*($AG35:BL35=3)),MAX(COLUMN($AG35:BL35)*($AG35:BL35=2))>MAX(COLUMN($AG35:BL35)*($AG35:BL35=1))),IF(COLUMN(BM35)-MAX(COLUMN($AG35:BL35)*($AG35:BL35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BM35)-MAX(COLUMN($AG35:BL35)*($AG35:BL35=3))=$J35,3,0),IF(COLUMN(BM35)-MAX(COLUMN($AG35:BL35)*($AG35:BL35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BM35)*($AG35:BM35=1))>MAX(COLUMN($AG35:BM35)*($AG35:BM35=3)),MAX(COLUMN($AG35:BM35)*($AG35:BM35=1))>MAX(COLUMN($AG35:BM35)*($AG35:BM35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BN35)-MAX(COLUMN($AG35:BM35)*($AG35:BM35=1))=$J35,3,0),IF(COLUMN(BN35)-MAX(COLUMN($AG35:BM35)*($AG35:BM35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BM35)*($AG35:BM35=2))>MAX(COLUMN($AG35:BM35)*($AG35:BM35=3)),MAX(COLUMN($AG35:BM35)*($AG35:BM35=2))>MAX(COLUMN($AG35:BM35)*($AG35:BM35=1))),IF(COLUMN(BN35)-MAX(COLUMN($AG35:BM35)*($AG35:BM35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BN35)-MAX(COLUMN($AG35:BM35)*($AG35:BM35=3))=$J35,3,0),IF(COLUMN(BN35)-MAX(COLUMN($AG35:BM35)*($AG35:BM35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BN35)*($AG35:BN35=1))>MAX(COLUMN($AG35:BN35)*($AG35:BN35=3)),MAX(COLUMN($AG35:BN35)*($AG35:BN35=1))>MAX(COLUMN($AG35:BN35)*($AG35:BN35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BO35)-MAX(COLUMN($AG35:BN35)*($AG35:BN35=1))=$J35,3,0),IF(COLUMN(BO35)-MAX(COLUMN($AG35:BN35)*($AG35:BN35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BN35)*($AG35:BN35=2))>MAX(COLUMN($AG35:BN35)*($AG35:BN35=3)),MAX(COLUMN($AG35:BN35)*($AG35:BN35=2))>MAX(COLUMN($AG35:BN35)*($AG35:BN35=1))),IF(COLUMN(BO35)-MAX(COLUMN($AG35:BN35)*($AG35:BN35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BO35)-MAX(COLUMN($AG35:BN35)*($AG35:BN35=3))=$J35,3,0),IF(COLUMN(BO35)-MAX(COLUMN($AG35:BN35)*($AG35:BN35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BO35)*($AG35:BO35=1))>MAX(COLUMN($AG35:BO35)*($AG35:BO35=3)),MAX(COLUMN($AG35:BO35)*($AG35:BO35=1))>MAX(COLUMN($AG35:BO35)*($AG35:BO35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BP35)-MAX(COLUMN($AG35:BO35)*($AG35:BO35=1))=$J35,3,0),IF(COLUMN(BP35)-MAX(COLUMN($AG35:BO35)*($AG35:BO35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BO35)*($AG35:BO35=2))>MAX(COLUMN($AG35:BO35)*($AG35:BO35=3)),MAX(COLUMN($AG35:BO35)*($AG35:BO35=2))>MAX(COLUMN($AG35:BO35)*($AG35:BO35=1))),IF(COLUMN(BP35)-MAX(COLUMN($AG35:BO35)*($AG35:BO35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BP35)-MAX(COLUMN($AG35:BO35)*($AG35:BO35=3))=$J35,3,0),IF(COLUMN(BP35)-MAX(COLUMN($AG35:BO35)*($AG35:BO35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BP35)*($AG35:BP35=1))>MAX(COLUMN($AG35:BP35)*($AG35:BP35=3)),MAX(COLUMN($AG35:BP35)*($AG35:BP35=1))>MAX(COLUMN($AG35:BP35)*($AG35:BP35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BQ35)-MAX(COLUMN($AG35:BP35)*($AG35:BP35=1))=$J35,3,0),IF(COLUMN(BQ35)-MAX(COLUMN($AG35:BP35)*($AG35:BP35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BP35)*($AG35:BP35=2))>MAX(COLUMN($AG35:BP35)*($AG35:BP35=3)),MAX(COLUMN($AG35:BP35)*($AG35:BP35=2))>MAX(COLUMN($AG35:BP35)*($AG35:BP35=1))),IF(COLUMN(BQ35)-MAX(COLUMN($AG35:BP35)*($AG35:BP35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BQ35)-MAX(COLUMN($AG35:BP35)*($AG35:BP35=3))=$J35,3,0),IF(COLUMN(BQ35)-MAX(COLUMN($AG35:BP35)*($AG35:BP35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=1))>MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=3)),MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=1))>MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BR35)-MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=1))=$J35,3,0),IF(COLUMN(BR35)-MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=2))>MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=3)),MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=2))>MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=1))),IF(COLUMN(BR35)-MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BR35)-MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=3))=$J35,3,0),IF(COLUMN(BR35)-MAX(COLUMN($AG35:BQ35)*($AG35:BQ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BR35)*($AG35:BR35=1))>MAX(COLUMN($AG35:BR35)*($AG35:BR35=3)),MAX(COLUMN($AG35:BR35)*($AG35:BR35=1))>MAX(COLUMN($AG35:BR35)*($AG35:BR35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BS35)-MAX(COLUMN($AG35:BR35)*($AG35:BR35=1))=$J35,3,0),IF(COLUMN(BS35)-MAX(COLUMN($AG35:BR35)*($AG35:BR35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BR35)*($AG35:BR35=2))>MAX(COLUMN($AG35:BR35)*($AG35:BR35=3)),MAX(COLUMN($AG35:BR35)*($AG35:BR35=2))>MAX(COLUMN($AG35:BR35)*($AG35:BR35=1))),IF(COLUMN(BS35)-MAX(COLUMN($AG35:BR35)*($AG35:BR35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BS35)-MAX(COLUMN($AG35:BR35)*($AG35:BR35=3))=$J35,3,0),IF(COLUMN(BS35)-MAX(COLUMN($AG35:BR35)*($AG35:BR35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BS35)*($AG35:BS35=1))>MAX(COLUMN($AG35:BS35)*($AG35:BS35=3)),MAX(COLUMN($AG35:BS35)*($AG35:BS35=1))>MAX(COLUMN($AG35:BS35)*($AG35:BS35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BT35)-MAX(COLUMN($AG35:BS35)*($AG35:BS35=1))=$J35,3,0),IF(COLUMN(BT35)-MAX(COLUMN($AG35:BS35)*($AG35:BS35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BS35)*($AG35:BS35=2))>MAX(COLUMN($AG35:BS35)*($AG35:BS35=3)),MAX(COLUMN($AG35:BS35)*($AG35:BS35=2))>MAX(COLUMN($AG35:BS35)*($AG35:BS35=1))),IF(COLUMN(BT35)-MAX(COLUMN($AG35:BS35)*($AG35:BS35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BT35)-MAX(COLUMN($AG35:BS35)*($AG35:BS35=3))=$J35,3,0),IF(COLUMN(BT35)-MAX(COLUMN($AG35:BS35)*($AG35:BS35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BT35)*($AG35:BT35=1))>MAX(COLUMN($AG35:BT35)*($AG35:BT35=3)),MAX(COLUMN($AG35:BT35)*($AG35:BT35=1))>MAX(COLUMN($AG35:BT35)*($AG35:BT35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BU35)-MAX(COLUMN($AG35:BT35)*($AG35:BT35=1))=$J35,3,0),IF(COLUMN(BU35)-MAX(COLUMN($AG35:BT35)*($AG35:BT35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BT35)*($AG35:BT35=2))>MAX(COLUMN($AG35:BT35)*($AG35:BT35=3)),MAX(COLUMN($AG35:BT35)*($AG35:BT35=2))>MAX(COLUMN($AG35:BT35)*($AG35:BT35=1))),IF(COLUMN(BU35)-MAX(COLUMN($AG35:BT35)*($AG35:BT35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BU35)-MAX(COLUMN($AG35:BT35)*($AG35:BT35=3))=$J35,3,0),IF(COLUMN(BU35)-MAX(COLUMN($AG35:BT35)*($AG35:BT35=3))=$J35,2,0)))))","v":2},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BU35)*($AG35:BU35=1))>MAX(COLUMN($AG35:BU35)*($AG35:BU35=3)),MAX(COLUMN($AG35:BU35)*($AG35:BU35=1))>MAX(COLUMN($AG35:BU35)*($AG35:BU35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BV35)-MAX(COLUMN($AG35:BU35)*($AG35:BU35=1))=$J35,3,0),IF(COLUMN(BV35)-MAX(COLUMN($AG35:BU35)*($AG35:BU35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BU35)*($AG35:BU35=2))>MAX(COLUMN($AG35:BU35)*($AG35:BU35=3)),MAX(COLUMN($AG35:BU35)*($AG35:BU35=2))>MAX(COLUMN($AG35:BU35)*($AG35:BU35=1))),IF(COLUMN(BV35)-MAX(COLUMN($AG35:BU35)*($AG35:BU35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BV35)-MAX(COLUMN($AG35:BU35)*($AG35:BU35=3))=$J35,3,0),IF(COLUMN(BV35)-MAX(COLUMN($AG35:BU35)*($AG35:BU35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BV35)*($AG35:BV35=1))>MAX(COLUMN($AG35:BV35)*($AG35:BV35=3)),MAX(COLUMN($AG35:BV35)*($AG35:BV35=1))>MAX(COLUMN($AG35:BV35)*($AG35:BV35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BW35)-MAX(COLUMN($AG35:BV35)*($AG35:BV35=1))=$J35,3,0),IF(COLUMN(BW35)-MAX(COLUMN($AG35:BV35)*($AG35:BV35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BV35)*($AG35:BV35=2))>MAX(COLUMN($AG35:BV35)*($AG35:BV35=3)),MAX(COLUMN($AG35:BV35)*($AG35:BV35=2))>MAX(COLUMN($AG35:BV35)*($AG35:BV35=1))),IF(COLUMN(BW35)-MAX(COLUMN($AG35:BV35)*($AG35:BV35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BW35)-MAX(COLUMN($AG35:BV35)*($AG35:BV35=3))=$J35,3,0),IF(COLUMN(BW35)-MAX(COLUMN($AG35:BV35)*($AG35:BV35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BW35)*($AG35:BW35=1))>MAX(COLUMN($AG35:BW35)*($AG35:BW35=3)),MAX(COLUMN($AG35:BW35)*($AG35:BW35=1))>MAX(COLUMN($AG35:BW35)*($AG35:BW35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BX35)-MAX(COLUMN($AG35:BW35)*($AG35:BW35=1))=$J35,3,0),IF(COLUMN(BX35)-MAX(COLUMN($AG35:BW35)*($AG35:BW35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BW35)*($AG35:BW35=2))>MAX(COLUMN($AG35:BW35)*($AG35:BW35=3)),MAX(COLUMN($AG35:BW35)*($AG35:BW35=2))>MAX(COLUMN($AG35:BW35)*($AG35:BW35=1))),IF(COLUMN(BX35)-MAX(COLUMN($AG35:BW35)*($AG35:BW35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BX35)-MAX(COLUMN($AG35:BW35)*($AG35:BW35=3))=$J35,3,0),IF(COLUMN(BX35)-MAX(COLUMN($AG35:BW35)*($AG35:BW35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BX35)*($AG35:BX35=1))>MAX(COLUMN($AG35:BX35)*($AG35:BX35=3)),MAX(COLUMN($AG35:BX35)*($AG35:BX35=1))>MAX(COLUMN($AG35:BX35)*($AG35:BX35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BY35)-MAX(COLUMN($AG35:BX35)*($AG35:BX35=1))=$J35,3,0),IF(COLUMN(BY35)-MAX(COLUMN($AG35:BX35)*($AG35:BX35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BX35)*($AG35:BX35=2))>MAX(COLUMN($AG35:BX35)*($AG35:BX35=3)),MAX(COLUMN($AG35:BX35)*($AG35:BX35=2))>MAX(COLUMN($AG35:BX35)*($AG35:BX35=1))),IF(COLUMN(BY35)-MAX(COLUMN($AG35:BX35)*($AG35:BX35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BY35)-MAX(COLUMN($AG35:BX35)*($AG35:BX35=3))=$J35,3,0),IF(COLUMN(BY35)-MAX(COLUMN($AG35:BX35)*($AG35:BX35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BY35)*($AG35:BY35=1))>MAX(COLUMN($AG35:BY35)*($AG35:BY35=3)),MAX(COLUMN($AG35:BY35)*($AG35:BY35=1))>MAX(COLUMN($AG35:BY35)*($AG35:BY35=2))),IF($K35=\"Not Possible\",IF(COLUMN(BZ35)-MAX(COLUMN($AG35:BY35)*($AG35:BY35=1))=$J35,3,0),IF(COLUMN(BZ35)-MAX(COLUMN($AG35:BY35)*($AG35:BY35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BY35)*($AG35:BY35=2))>MAX(COLUMN($AG35:BY35)*($AG35:BY35=3)),MAX(COLUMN($AG35:BY35)*($AG35:BY35=2))>MAX(COLUMN($AG35:BY35)*($AG35:BY35=1))),IF(COLUMN(BZ35)-MAX(COLUMN($AG35:BY35)*($AG35:BY35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(BZ35)-MAX(COLUMN($AG35:BY35)*($AG35:BY35=3))=$J35,3,0),IF(COLUMN(BZ35)-MAX(COLUMN($AG35:BY35)*($AG35:BY35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=1))>MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=3)),MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=1))>MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CA35)-MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=1))=$J35,3,0),IF(COLUMN(CA35)-MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=2))>MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=3)),MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=2))>MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=1))),IF(COLUMN(CA35)-MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CA35)-MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=3))=$J35,3,0),IF(COLUMN(CA35)-MAX(COLUMN($AG35:BZ35)*($AG35:BZ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CA35)*($AG35:CA35=1))>MAX(COLUMN($AG35:CA35)*($AG35:CA35=3)),MAX(COLUMN($AG35:CA35)*($AG35:CA35=1))>MAX(COLUMN($AG35:CA35)*($AG35:CA35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CB35)-MAX(COLUMN($AG35:CA35)*($AG35:CA35=1))=$J35,3,0),IF(COLUMN(CB35)-MAX(COLUMN($AG35:CA35)*($AG35:CA35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CA35)*($AG35:CA35=2))>MAX(COLUMN($AG35:CA35)*($AG35:CA35=3)),MAX(COLUMN($AG35:CA35)*($AG35:CA35=2))>MAX(COLUMN($AG35:CA35)*($AG35:CA35=1))),IF(COLUMN(CB35)-MAX(COLUMN($AG35:CA35)*($AG35:CA35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CB35)-MAX(COLUMN($AG35:CA35)*($AG35:CA35=3))=$J35,3,0),IF(COLUMN(CB35)-MAX(COLUMN($AG35:CA35)*($AG35:CA35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CB35)*($AG35:CB35=1))>MAX(COLUMN($AG35:CB35)*($AG35:CB35=3)),MAX(COLUMN($AG35:CB35)*($AG35:CB35=1))>MAX(COLUMN($AG35:CB35)*($AG35:CB35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CC35)-MAX(COLUMN($AG35:CB35)*($AG35:CB35=1))=$J35,3,0),IF(COLUMN(CC35)-MAX(COLUMN($AG35:CB35)*($AG35:CB35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CB35)*($AG35:CB35=2))>MAX(COLUMN($AG35:CB35)*($AG35:CB35=3)),MAX(COLUMN($AG35:CB35)*($AG35:CB35=2))>MAX(COLUMN($AG35:CB35)*($AG35:CB35=1))),IF(COLUMN(CC35)-MAX(COLUMN($AG35:CB35)*($AG35:CB35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CC35)-MAX(COLUMN($AG35:CB35)*($AG35:CB35=3))=$J35,3,0),IF(COLUMN(CC35)-MAX(COLUMN($AG35:CB35)*($AG35:CB35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CC35)*($AG35:CC35=1))>MAX(COLUMN($AG35:CC35)*($AG35:CC35=3)),MAX(COLUMN($AG35:CC35)*($AG35:CC35=1))>MAX(COLUMN($AG35:CC35)*($AG35:CC35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CD35)-MAX(COLUMN($AG35:CC35)*($AG35:CC35=1))=$J35,3,0),IF(COLUMN(CD35)-MAX(COLUMN($AG35:CC35)*($AG35:CC35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CC35)*($AG35:CC35=2))>MAX(COLUMN($AG35:CC35)*($AG35:CC35=3)),MAX(COLUMN($AG35:CC35)*($AG35:CC35=2))>MAX(COLUMN($AG35:CC35)*($AG35:CC35=1))),IF(COLUMN(CD35)-MAX(COLUMN($AG35:CC35)*($AG35:CC35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CD35)-MAX(COLUMN($AG35:CC35)*($AG35:CC35=3))=$J35,3,0),IF(COLUMN(CD35)-MAX(COLUMN($AG35:CC35)*($AG35:CC35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CD35)*($AG35:CD35=1))>MAX(COLUMN($AG35:CD35)*($AG35:CD35=3)),MAX(COLUMN($AG35:CD35)*($AG35:CD35=1))>MAX(COLUMN($AG35:CD35)*($AG35:CD35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CE35)-MAX(COLUMN($AG35:CD35)*($AG35:CD35=1))=$J35,3,0),IF(COLUMN(CE35)-MAX(COLUMN($AG35:CD35)*($AG35:CD35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CD35)*($AG35:CD35=2))>MAX(COLUMN($AG35:CD35)*($AG35:CD35=3)),MAX(COLUMN($AG35:CD35)*($AG35:CD35=2))>MAX(COLUMN($AG35:CD35)*($AG35:CD35=1))),IF(COLUMN(CE35)-MAX(COLUMN($AG35:CD35)*($AG35:CD35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CE35)-MAX(COLUMN($AG35:CD35)*($AG35:CD35=3))=$J35,3,0),IF(COLUMN(CE35)-MAX(COLUMN($AG35:CD35)*($AG35:CD35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CE35)*($AG35:CE35=1))>MAX(COLUMN($AG35:CE35)*($AG35:CE35=3)),MAX(COLUMN($AG35:CE35)*($AG35:CE35=1))>MAX(COLUMN($AG35:CE35)*($AG35:CE35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CF35)-MAX(COLUMN($AG35:CE35)*($AG35:CE35=1))=$J35,3,0),IF(COLUMN(CF35)-MAX(COLUMN($AG35:CE35)*($AG35:CE35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CE35)*($AG35:CE35=2))>MAX(COLUMN($AG35:CE35)*($AG35:CE35=3)),MAX(COLUMN($AG35:CE35)*($AG35:CE35=2))>MAX(COLUMN($AG35:CE35)*($AG35:CE35=1))),IF(COLUMN(CF35)-MAX(COLUMN($AG35:CE35)*($AG35:CE35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CF35)-MAX(COLUMN($AG35:CE35)*($AG35:CE35=3))=$J35,3,0),IF(COLUMN(CF35)-MAX(COLUMN($AG35:CE35)*($AG35:CE35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CF35)*($AG35:CF35=1))>MAX(COLUMN($AG35:CF35)*($AG35:CF35=3)),MAX(COLUMN($AG35:CF35)*($AG35:CF35=1))>MAX(COLUMN($AG35:CF35)*($AG35:CF35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CG35)-MAX(COLUMN($AG35:CF35)*($AG35:CF35=1))=$J35,3,0),IF(COLUMN(CG35)-MAX(COLUMN($AG35:CF35)*($AG35:CF35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CF35)*($AG35:CF35=2))>MAX(COLUMN($AG35:CF35)*($AG35:CF35=3)),MAX(COLUMN($AG35:CF35)*($AG35:CF35=2))>MAX(COLUMN($AG35:CF35)*($AG35:CF35=1))),IF(COLUMN(CG35)-MAX(COLUMN($AG35:CF35)*($AG35:CF35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CG35)-MAX(COLUMN($AG35:CF35)*($AG35:CF35=3))=$J35,3,0),IF(COLUMN(CG35)-MAX(COLUMN($AG35:CF35)*($AG35:CF35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CG35)*($AG35:CG35=1))>MAX(COLUMN($AG35:CG35)*($AG35:CG35=3)),MAX(COLUMN($AG35:CG35)*($AG35:CG35=1))>MAX(COLUMN($AG35:CG35)*($AG35:CG35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CH35)-MAX(COLUMN($AG35:CG35)*($AG35:CG35=1))=$J35,3,0),IF(COLUMN(CH35)-MAX(COLUMN($AG35:CG35)*($AG35:CG35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CG35)*($AG35:CG35=2))>MAX(COLUMN($AG35:CG35)*($AG35:CG35=3)),MAX(COLUMN($AG35:CG35)*($AG35:CG35=2))>MAX(COLUMN($AG35:CG35)*($AG35:CG35=1))),IF(COLUMN(CH35)-MAX(COLUMN($AG35:CG35)*($AG35:CG35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CH35)-MAX(COLUMN($AG35:CG35)*($AG35:CG35=3))=$J35,3,0),IF(COLUMN(CH35)-MAX(COLUMN($AG35:CG35)*($AG35:CG35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CH35)*($AG35:CH35=1))>MAX(COLUMN($AG35:CH35)*($AG35:CH35=3)),MAX(COLUMN($AG35:CH35)*($AG35:CH35=1))>MAX(COLUMN($AG35:CH35)*($AG35:CH35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CI35)-MAX(COLUMN($AG35:CH35)*($AG35:CH35=1))=$J35,3,0),IF(COLUMN(CI35)-MAX(COLUMN($AG35:CH35)*($AG35:CH35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CH35)*($AG35:CH35=2))>MAX(COLUMN($AG35:CH35)*($AG35:CH35=3)),MAX(COLUMN($AG35:CH35)*($AG35:CH35=2))>MAX(COLUMN($AG35:CH35)*($AG35:CH35=1))),IF(COLUMN(CI35)-MAX(COLUMN($AG35:CH35)*($AG35:CH35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CI35)-MAX(COLUMN($AG35:CH35)*($AG35:CH35=3))=$J35,3,0),IF(COLUMN(CI35)-MAX(COLUMN($AG35:CH35)*($AG35:CH35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CI35)*($AG35:CI35=1))>MAX(COLUMN($AG35:CI35)*($AG35:CI35=3)),MAX(COLUMN($AG35:CI35)*($AG35:CI35=1))>MAX(COLUMN($AG35:CI35)*($AG35:CI35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CJ35)-MAX(COLUMN($AG35:CI35)*($AG35:CI35=1))=$J35,3,0),IF(COLUMN(CJ35)-MAX(COLUMN($AG35:CI35)*($AG35:CI35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CI35)*($AG35:CI35=2))>MAX(COLUMN($AG35:CI35)*($AG35:CI35=3)),MAX(COLUMN($AG35:CI35)*($AG35:CI35=2))>MAX(COLUMN($AG35:CI35)*($AG35:CI35=1))),IF(COLUMN(CJ35)-MAX(COLUMN($AG35:CI35)*($AG35:CI35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CJ35)-MAX(COLUMN($AG35:CI35)*($AG35:CI35=3))=$J35,3,0),IF(COLUMN(CJ35)-MAX(COLUMN($AG35:CI35)*($AG35:CI35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=1))>MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=3)),MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=1))>MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CK35)-MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=1))=$J35,3,0),IF(COLUMN(CK35)-MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=2))>MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=3)),MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=2))>MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=1))),IF(COLUMN(CK35)-MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CK35)-MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=3))=$J35,3,0),IF(COLUMN(CK35)-MAX(COLUMN($AG35:CJ35)*($AG35:CJ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CK35)*($AG35:CK35=1))>MAX(COLUMN($AG35:CK35)*($AG35:CK35=3)),MAX(COLUMN($AG35:CK35)*($AG35:CK35=1))>MAX(COLUMN($AG35:CK35)*($AG35:CK35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CL35)-MAX(COLUMN($AG35:CK35)*($AG35:CK35=1))=$J35,3,0),IF(COLUMN(CL35)-MAX(COLUMN($AG35:CK35)*($AG35:CK35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CK35)*($AG35:CK35=2))>MAX(COLUMN($AG35:CK35)*($AG35:CK35=3)),MAX(COLUMN($AG35:CK35)*($AG35:CK35=2))>MAX(COLUMN($AG35:CK35)*($AG35:CK35=1))),IF(COLUMN(CL35)-MAX(COLUMN($AG35:CK35)*($AG35:CK35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CL35)-MAX(COLUMN($AG35:CK35)*($AG35:CK35=3))=$J35,3,0),IF(COLUMN(CL35)-MAX(COLUMN($AG35:CK35)*($AG35:CK35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CL35)*($AG35:CL35=1))>MAX(COLUMN($AG35:CL35)*($AG35:CL35=3)),MAX(COLUMN($AG35:CL35)*($AG35:CL35=1))>MAX(COLUMN($AG35:CL35)*($AG35:CL35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CM35)-MAX(COLUMN($AG35:CL35)*($AG35:CL35=1))=$J35,3,0),IF(COLUMN(CM35)-MAX(COLUMN($AG35:CL35)*($AG35:CL35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CL35)*($AG35:CL35=2))>MAX(COLUMN($AG35:CL35)*($AG35:CL35=3)),MAX(COLUMN($AG35:CL35)*($AG35:CL35=2))>MAX(COLUMN($AG35:CL35)*($AG35:CL35=1))),IF(COLUMN(CM35)-MAX(COLUMN($AG35:CL35)*($AG35:CL35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CM35)-MAX(COLUMN($AG35:CL35)*($AG35:CL35=3))=$J35,3,0),IF(COLUMN(CM35)-MAX(COLUMN($AG35:CL35)*($AG35:CL35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CM35)*($AG35:CM35=1))>MAX(COLUMN($AG35:CM35)*($AG35:CM35=3)),MAX(COLUMN($AG35:CM35)*($AG35:CM35=1))>MAX(COLUMN($AG35:CM35)*($AG35:CM35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CN35)-MAX(COLUMN($AG35:CM35)*($AG35:CM35=1))=$J35,3,0),IF(COLUMN(CN35)-MAX(COLUMN($AG35:CM35)*($AG35:CM35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CM35)*($AG35:CM35=2))>MAX(COLUMN($AG35:CM35)*($AG35:CM35=3)),MAX(COLUMN($AG35:CM35)*($AG35:CM35=2))>MAX(COLUMN($AG35:CM35)*($AG35:CM35=1))),IF(COLUMN(CN35)-MAX(COLUMN($AG35:CM35)*($AG35:CM35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CN35)-MAX(COLUMN($AG35:CM35)*($AG35:CM35=3))=$J35,3,0),IF(COLUMN(CN35)-MAX(COLUMN($AG35:CM35)*($AG35:CM35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CN35)*($AG35:CN35=1))>MAX(COLUMN($AG35:CN35)*($AG35:CN35=3)),MAX(COLUMN($AG35:CN35)*($AG35:CN35=1))>MAX(COLUMN($AG35:CN35)*($AG35:CN35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CO35)-MAX(COLUMN($AG35:CN35)*($AG35:CN35=1))=$J35,3,0),IF(COLUMN(CO35)-MAX(COLUMN($AG35:CN35)*($AG35:CN35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CN35)*($AG35:CN35=2))>MAX(COLUMN($AG35:CN35)*($AG35:CN35=3)),MAX(COLUMN($AG35:CN35)*($AG35:CN35=2))>MAX(COLUMN($AG35:CN35)*($AG35:CN35=1))),IF(COLUMN(CO35)-MAX(COLUMN($AG35:CN35)*($AG35:CN35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CO35)-MAX(COLUMN($AG35:CN35)*($AG35:CN35=3))=$J35,3,0),IF(COLUMN(CO35)-MAX(COLUMN($AG35:CN35)*($AG35:CN35=3))=$J35,2,0)))))","v":3},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CO35)*($AG35:CO35=1))>MAX(COLUMN($AG35:CO35)*($AG35:CO35=3)),MAX(COLUMN($AG35:CO35)*($AG35:CO35=1))>MAX(COLUMN($AG35:CO35)*($AG35:CO35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CP35)-MAX(COLUMN($AG35:CO35)*($AG35:CO35=1))=$J35,3,0),IF(COLUMN(CP35)-MAX(COLUMN($AG35:CO35)*($AG35:CO35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CO35)*($AG35:CO35=2))>MAX(COLUMN($AG35:CO35)*($AG35:CO35=3)),MAX(COLUMN($AG35:CO35)*($AG35:CO35=2))>MAX(COLUMN($AG35:CO35)*($AG35:CO35=1))),IF(COLUMN(CP35)-MAX(COLUMN($AG35:CO35)*($AG35:CO35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CP35)-MAX(COLUMN($AG35:CO35)*($AG35:CO35=3))=$J35,3,0),IF(COLUMN(CP35)-MAX(COLUMN($AG35:CO35)*($AG35:CO35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CP35)*($AG35:CP35=1))>MAX(COLUMN($AG35:CP35)*($AG35:CP35=3)),MAX(COLUMN($AG35:CP35)*($AG35:CP35=1))>MAX(COLUMN($AG35:CP35)*($AG35:CP35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CQ35)-MAX(COLUMN($AG35:CP35)*($AG35:CP35=1))=$J35,3,0),IF(COLUMN(CQ35)-MAX(COLUMN($AG35:CP35)*($AG35:CP35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CP35)*($AG35:CP35=2))>MAX(COLUMN($AG35:CP35)*($AG35:CP35=3)),MAX(COLUMN($AG35:CP35)*($AG35:CP35=2))>MAX(COLUMN($AG35:CP35)*($AG35:CP35=1))),IF(COLUMN(CQ35)-MAX(COLUMN($AG35:CP35)*($AG35:CP35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CQ35)-MAX(COLUMN($AG35:CP35)*($AG35:CP35=3))=$J35,3,0),IF(COLUMN(CQ35)-MAX(COLUMN($AG35:CP35)*($AG35:CP35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=1))>MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=3)),MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=1))>MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CR35)-MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=1))=$J35,3,0),IF(COLUMN(CR35)-MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=2))>MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=3)),MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=2))>MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=1))),IF(COLUMN(CR35)-MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CR35)-MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=3))=$J35,3,0),IF(COLUMN(CR35)-MAX(COLUMN($AG35:CQ35)*($AG35:CQ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CR35)*($AG35:CR35=1))>MAX(COLUMN($AG35:CR35)*($AG35:CR35=3)),MAX(COLUMN($AG35:CR35)*($AG35:CR35=1))>MAX(COLUMN($AG35:CR35)*($AG35:CR35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CS35)-MAX(COLUMN($AG35:CR35)*($AG35:CR35=1))=$J35,3,0),IF(COLUMN(CS35)-MAX(COLUMN($AG35:CR35)*($AG35:CR35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CR35)*($AG35:CR35=2))>MAX(COLUMN($AG35:CR35)*($AG35:CR35=3)),MAX(COLUMN($AG35:CR35)*($AG35:CR35=2))>MAX(COLUMN($AG35:CR35)*($AG35:CR35=1))),IF(COLUMN(CS35)-MAX(COLUMN($AG35:CR35)*($AG35:CR35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CS35)-MAX(COLUMN($AG35:CR35)*($AG35:CR35=3))=$J35,3,0),IF(COLUMN(CS35)-MAX(COLUMN($AG35:CR35)*($AG35:CR35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CS35)*($AG35:CS35=1))>MAX(COLUMN($AG35:CS35)*($AG35:CS35=3)),MAX(COLUMN($AG35:CS35)*($AG35:CS35=1))>MAX(COLUMN($AG35:CS35)*($AG35:CS35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CT35)-MAX(COLUMN($AG35:CS35)*($AG35:CS35=1))=$J35,3,0),IF(COLUMN(CT35)-MAX(COLUMN($AG35:CS35)*($AG35:CS35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CS35)*($AG35:CS35=2))>MAX(COLUMN($AG35:CS35)*($AG35:CS35=3)),MAX(COLUMN($AG35:CS35)*($AG35:CS35=2))>MAX(COLUMN($AG35:CS35)*($AG35:CS35=1))),IF(COLUMN(CT35)-MAX(COLUMN($AG35:CS35)*($AG35:CS35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CT35)-MAX(COLUMN($AG35:CS35)*($AG35:CS35=3))=$J35,3,0),IF(COLUMN(CT35)-MAX(COLUMN($AG35:CS35)*($AG35:CS35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CT35)*($AG35:CT35=1))>MAX(COLUMN($AG35:CT35)*($AG35:CT35=3)),MAX(COLUMN($AG35:CT35)*($AG35:CT35=1))>MAX(COLUMN($AG35:CT35)*($AG35:CT35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CU35)-MAX(COLUMN($AG35:CT35)*($AG35:CT35=1))=$J35,3,0),IF(COLUMN(CU35)-MAX(COLUMN($AG35:CT35)*($AG35:CT35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CT35)*($AG35:CT35=2))>MAX(COLUMN($AG35:CT35)*($AG35:CT35=3)),MAX(COLUMN($AG35:CT35)*($AG35:CT35=2))>MAX(COLUMN($AG35:CT35)*($AG35:CT35=1))),IF(COLUMN(CU35)-MAX(COLUMN($AG35:CT35)*($AG35:CT35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CU35)-MAX(COLUMN($AG35:CT35)*($AG35:CT35=3))=$J35,3,0),IF(COLUMN(CU35)-MAX(COLUMN($AG35:CT35)*($AG35:CT35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CU35)*($AG35:CU35=1))>MAX(COLUMN($AG35:CU35)*($AG35:CU35=3)),MAX(COLUMN($AG35:CU35)*($AG35:CU35=1))>MAX(COLUMN($AG35:CU35)*($AG35:CU35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CV35)-MAX(COLUMN($AG35:CU35)*($AG35:CU35=1))=$J35,3,0),IF(COLUMN(CV35)-MAX(COLUMN($AG35:CU35)*($AG35:CU35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CU35)*($AG35:CU35=2))>MAX(COLUMN($AG35:CU35)*($AG35:CU35=3)),MAX(COLUMN($AG35:CU35)*($AG35:CU35=2))>MAX(COLUMN($AG35:CU35)*($AG35:CU35=1))),IF(COLUMN(CV35)-MAX(COLUMN($AG35:CU35)*($AG35:CU35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CV35)-MAX(COLUMN($AG35:CU35)*($AG35:CU35=3))=$J35,3,0),IF(COLUMN(CV35)-MAX(COLUMN($AG35:CU35)*($AG35:CU35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CV35)*($AG35:CV35=1))>MAX(COLUMN($AG35:CV35)*($AG35:CV35=3)),MAX(COLUMN($AG35:CV35)*($AG35:CV35=1))>MAX(COLUMN($AG35:CV35)*($AG35:CV35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CW35)-MAX(COLUMN($AG35:CV35)*($AG35:CV35=1))=$J35,3,0),IF(COLUMN(CW35)-MAX(COLUMN($AG35:CV35)*($AG35:CV35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CV35)*($AG35:CV35=2))>MAX(COLUMN($AG35:CV35)*($AG35:CV35=3)),MAX(COLUMN($AG35:CV35)*($AG35:CV35=2))>MAX(COLUMN($AG35:CV35)*($AG35:CV35=1))),IF(COLUMN(CW35)-MAX(COLUMN($AG35:CV35)*($AG35:CV35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CW35)-MAX(COLUMN($AG35:CV35)*($AG35:CV35=3))=$J35,3,0),IF(COLUMN(CW35)-MAX(COLUMN($AG35:CV35)*($AG35:CV35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CW35)*($AG35:CW35=1))>MAX(COLUMN($AG35:CW35)*($AG35:CW35=3)),MAX(COLUMN($AG35:CW35)*($AG35:CW35=1))>MAX(COLUMN($AG35:CW35)*($AG35:CW35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CX35)-MAX(COLUMN($AG35:CW35)*($AG35:CW35=1))=$J35,3,0),IF(COLUMN(CX35)-MAX(COLUMN($AG35:CW35)*($AG35:CW35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CW35)*($AG35:CW35=2))>MAX(COLUMN($AG35:CW35)*($AG35:CW35=3)),MAX(COLUMN($AG35:CW35)*($AG35:CW35=2))>MAX(COLUMN($AG35:CW35)*($AG35:CW35=1))),IF(COLUMN(CX35)-MAX(COLUMN($AG35:CW35)*($AG35:CW35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CX35)-MAX(COLUMN($AG35:CW35)*($AG35:CW35=3))=$J35,3,0),IF(COLUMN(CX35)-MAX(COLUMN($AG35:CW35)*($AG35:CW35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CX35)*($AG35:CX35=1))>MAX(COLUMN($AG35:CX35)*($AG35:CX35=3)),MAX(COLUMN($AG35:CX35)*($AG35:CX35=1))>MAX(COLUMN($AG35:CX35)*($AG35:CX35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CY35)-MAX(COLUMN($AG35:CX35)*($AG35:CX35=1))=$J35,3,0),IF(COLUMN(CY35)-MAX(COLUMN($AG35:CX35)*($AG35:CX35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CX35)*($AG35:CX35=2))>MAX(COLUMN($AG35:CX35)*($AG35:CX35=3)),MAX(COLUMN($AG35:CX35)*($AG35:CX35=2))>MAX(COLUMN($AG35:CX35)*($AG35:CX35=1))),IF(COLUMN(CY35)-MAX(COLUMN($AG35:CX35)*($AG35:CX35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CY35)-MAX(COLUMN($AG35:CX35)*($AG35:CX35=3))=$J35,3,0),IF(COLUMN(CY35)-MAX(COLUMN($AG35:CX35)*($AG35:CX35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CY35)*($AG35:CY35=1))>MAX(COLUMN($AG35:CY35)*($AG35:CY35=3)),MAX(COLUMN($AG35:CY35)*($AG35:CY35=1))>MAX(COLUMN($AG35:CY35)*($AG35:CY35=2))),IF($K35=\"Not Possible\",IF(COLUMN(CZ35)-MAX(COLUMN($AG35:CY35)*($AG35:CY35=1))=$J35,3,0),IF(COLUMN(CZ35)-MAX(COLUMN($AG35:CY35)*($AG35:CY35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CY35)*($AG35:CY35=2))>MAX(COLUMN($AG35:CY35)*($AG35:CY35=3)),MAX(COLUMN($AG35:CY35)*($AG35:CY35=2))>MAX(COLUMN($AG35:CY35)*($AG35:CY35=1))),IF(COLUMN(CZ35)-MAX(COLUMN($AG35:CY35)*($AG35:CY35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(CZ35)-MAX(COLUMN($AG35:CY35)*($AG35:CY35=3))=$J35,3,0),IF(COLUMN(CZ35)-MAX(COLUMN($AG35:CY35)*($AG35:CY35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=1))>MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=3)),MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=1))>MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DA35)-MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=1))=$J35,3,0),IF(COLUMN(DA35)-MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=2))>MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=3)),MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=2))>MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=1))),IF(COLUMN(DA35)-MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DA35)-MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=3))=$J35,3,0),IF(COLUMN(DA35)-MAX(COLUMN($AG35:CZ35)*($AG35:CZ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DA35)*($AG35:DA35=1))>MAX(COLUMN($AG35:DA35)*($AG35:DA35=3)),MAX(COLUMN($AG35:DA35)*($AG35:DA35=1))>MAX(COLUMN($AG35:DA35)*($AG35:DA35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DB35)-MAX(COLUMN($AG35:DA35)*($AG35:DA35=1))=$J35,3,0),IF(COLUMN(DB35)-MAX(COLUMN($AG35:DA35)*($AG35:DA35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DA35)*($AG35:DA35=2))>MAX(COLUMN($AG35:DA35)*($AG35:DA35=3)),MAX(COLUMN($AG35:DA35)*($AG35:DA35=2))>MAX(COLUMN($AG35:DA35)*($AG35:DA35=1))),IF(COLUMN(DB35)-MAX(COLUMN($AG35:DA35)*($AG35:DA35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DB35)-MAX(COLUMN($AG35:DA35)*($AG35:DA35=3))=$J35,3,0),IF(COLUMN(DB35)-MAX(COLUMN($AG35:DA35)*($AG35:DA35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DB35)*($AG35:DB35=1))>MAX(COLUMN($AG35:DB35)*($AG35:DB35=3)),MAX(COLUMN($AG35:DB35)*($AG35:DB35=1))>MAX(COLUMN($AG35:DB35)*($AG35:DB35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DC35)-MAX(COLUMN($AG35:DB35)*($AG35:DB35=1))=$J35,3,0),IF(COLUMN(DC35)-MAX(COLUMN($AG35:DB35)*($AG35:DB35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DB35)*($AG35:DB35=2))>MAX(COLUMN($AG35:DB35)*($AG35:DB35=3)),MAX(COLUMN($AG35:DB35)*($AG35:DB35=2))>MAX(COLUMN($AG35:DB35)*($AG35:DB35=1))),IF(COLUMN(DC35)-MAX(COLUMN($AG35:DB35)*($AG35:DB35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DC35)-MAX(COLUMN($AG35:DB35)*($AG35:DB35=3))=$J35,3,0),IF(COLUMN(DC35)-MAX(COLUMN($AG35:DB35)*($AG35:DB35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DC35)*($AG35:DC35=1))>MAX(COLUMN($AG35:DC35)*($AG35:DC35=3)),MAX(COLUMN($AG35:DC35)*($AG35:DC35=1))>MAX(COLUMN($AG35:DC35)*($AG35:DC35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DD35)-MAX(COLUMN($AG35:DC35)*($AG35:DC35=1))=$J35,3,0),IF(COLUMN(DD35)-MAX(COLUMN($AG35:DC35)*($AG35:DC35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DC35)*($AG35:DC35=2))>MAX(COLUMN($AG35:DC35)*($AG35:DC35=3)),MAX(COLUMN($AG35:DC35)*($AG35:DC35=2))>MAX(COLUMN($AG35:DC35)*($AG35:DC35=1))),IF(COLUMN(DD35)-MAX(COLUMN($AG35:DC35)*($AG35:DC35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DD35)-MAX(COLUMN($AG35:DC35)*($AG35:DC35=3))=$J35,3,0),IF(COLUMN(DD35)-MAX(COLUMN($AG35:DC35)*($AG35:DC35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DD35)*($AG35:DD35=1))>MAX(COLUMN($AG35:DD35)*($AG35:DD35=3)),MAX(COLUMN($AG35:DD35)*($AG35:DD35=1))>MAX(COLUMN($AG35:DD35)*($AG35:DD35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DE35)-MAX(COLUMN($AG35:DD35)*($AG35:DD35=1))=$J35,3,0),IF(COLUMN(DE35)-MAX(COLUMN($AG35:DD35)*($AG35:DD35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DD35)*($AG35:DD35=2))>MAX(COLUMN($AG35:DD35)*($AG35:DD35=3)),MAX(COLUMN($AG35:DD35)*($AG35:DD35=2))>MAX(COLUMN($AG35:DD35)*($AG35:DD35=1))),IF(COLUMN(DE35)-MAX(COLUMN($AG35:DD35)*($AG35:DD35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DE35)-MAX(COLUMN($AG35:DD35)*($AG35:DD35=3))=$J35,3,0),IF(COLUMN(DE35)-MAX(COLUMN($AG35:DD35)*($AG35:DD35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DE35)*($AG35:DE35=1))>MAX(COLUMN($AG35:DE35)*($AG35:DE35=3)),MAX(COLUMN($AG35:DE35)*($AG35:DE35=1))>MAX(COLUMN($AG35:DE35)*($AG35:DE35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DF35)-MAX(COLUMN($AG35:DE35)*($AG35:DE35=1))=$J35,3,0),IF(COLUMN(DF35)-MAX(COLUMN($AG35:DE35)*($AG35:DE35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DE35)*($AG35:DE35=2))>MAX(COLUMN($AG35:DE35)*($AG35:DE35=3)),MAX(COLUMN($AG35:DE35)*($AG35:DE35=2))>MAX(COLUMN($AG35:DE35)*($AG35:DE35=1))),IF(COLUMN(DF35)-MAX(COLUMN($AG35:DE35)*($AG35:DE35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DF35)-MAX(COLUMN($AG35:DE35)*($AG35:DE35=3))=$J35,3,0),IF(COLUMN(DF35)-MAX(COLUMN($AG35:DE35)*($AG35:DE35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DF35)*($AG35:DF35=1))>MAX(COLUMN($AG35:DF35)*($AG35:DF35=3)),MAX(COLUMN($AG35:DF35)*($AG35:DF35=1))>MAX(COLUMN($AG35:DF35)*($AG35:DF35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DG35)-MAX(COLUMN($AG35:DF35)*($AG35:DF35=1))=$J35,3,0),IF(COLUMN(DG35)-MAX(COLUMN($AG35:DF35)*($AG35:DF35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DF35)*($AG35:DF35=2))>MAX(COLUMN($AG35:DF35)*($AG35:DF35=3)),MAX(COLUMN($AG35:DF35)*($AG35:DF35=2))>MAX(COLUMN($AG35:DF35)*($AG35:DF35=1))),IF(COLUMN(DG35)-MAX(COLUMN($AG35:DF35)*($AG35:DF35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DG35)-MAX(COLUMN($AG35:DF35)*($AG35:DF35=3))=$J35,3,0),IF(COLUMN(DG35)-MAX(COLUMN($AG35:DF35)*($AG35:DF35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DG35)*($AG35:DG35=1))>MAX(COLUMN($AG35:DG35)*($AG35:DG35=3)),MAX(COLUMN($AG35:DG35)*($AG35:DG35=1))>MAX(COLUMN($AG35:DG35)*($AG35:DG35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DH35)-MAX(COLUMN($AG35:DG35)*($AG35:DG35=1))=$J35,3,0),IF(COLUMN(DH35)-MAX(COLUMN($AG35:DG35)*($AG35:DG35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DG35)*($AG35:DG35=2))>MAX(COLUMN($AG35:DG35)*($AG35:DG35=3)),MAX(COLUMN($AG35:DG35)*($AG35:DG35=2))>MAX(COLUMN($AG35:DG35)*($AG35:DG35=1))),IF(COLUMN(DH35)-MAX(COLUMN($AG35:DG35)*($AG35:DG35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DH35)-MAX(COLUMN($AG35:DG35)*($AG35:DG35=3))=$J35,3,0),IF(COLUMN(DH35)-MAX(COLUMN($AG35:DG35)*($AG35:DG35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DH35)*($AG35:DH35=1))>MAX(COLUMN($AG35:DH35)*($AG35:DH35=3)),MAX(COLUMN($AG35:DH35)*($AG35:DH35=1))>MAX(COLUMN($AG35:DH35)*($AG35:DH35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DI35)-MAX(COLUMN($AG35:DH35)*($AG35:DH35=1))=$J35,3,0),IF(COLUMN(DI35)-MAX(COLUMN($AG35:DH35)*($AG35:DH35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DH35)*($AG35:DH35=2))>MAX(COLUMN($AG35:DH35)*($AG35:DH35=3)),MAX(COLUMN($AG35:DH35)*($AG35:DH35=2))>MAX(COLUMN($AG35:DH35)*($AG35:DH35=1))),IF(COLUMN(DI35)-MAX(COLUMN($AG35:DH35)*($AG35:DH35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DI35)-MAX(COLUMN($AG35:DH35)*($AG35:DH35=3))=$J35,3,0),IF(COLUMN(DI35)-MAX(COLUMN($AG35:DH35)*($AG35:DH35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DI35)*($AG35:DI35=1))>MAX(COLUMN($AG35:DI35)*($AG35:DI35=3)),MAX(COLUMN($AG35:DI35)*($AG35:DI35=1))>MAX(COLUMN($AG35:DI35)*($AG35:DI35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DJ35)-MAX(COLUMN($AG35:DI35)*($AG35:DI35=1))=$J35,3,0),IF(COLUMN(DJ35)-MAX(COLUMN($AG35:DI35)*($AG35:DI35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DI35)*($AG35:DI35=2))>MAX(COLUMN($AG35:DI35)*($AG35:DI35=3)),MAX(COLUMN($AG35:DI35)*($AG35:DI35=2))>MAX(COLUMN($AG35:DI35)*($AG35:DI35=1))),IF(COLUMN(DJ35)-MAX(COLUMN($AG35:DI35)*($AG35:DI35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DJ35)-MAX(COLUMN($AG35:DI35)*($AG35:DI35=3))=$J35,3,0),IF(COLUMN(DJ35)-MAX(COLUMN($AG35:DI35)*($AG35:DI35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=1))>MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=3)),MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=1))>MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DK35)-MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=1))=$J35,3,0),IF(COLUMN(DK35)-MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=2))>MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=3)),MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=2))>MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=1))),IF(COLUMN(DK35)-MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DK35)-MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=3))=$J35,3,0),IF(COLUMN(DK35)-MAX(COLUMN($AG35:DJ35)*($AG35:DJ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DK35)*($AG35:DK35=1))>MAX(COLUMN($AG35:DK35)*($AG35:DK35=3)),MAX(COLUMN($AG35:DK35)*($AG35:DK35=1))>MAX(COLUMN($AG35:DK35)*($AG35:DK35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DL35)-MAX(COLUMN($AG35:DK35)*($AG35:DK35=1))=$J35,3,0),IF(COLUMN(DL35)-MAX(COLUMN($AG35:DK35)*($AG35:DK35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DK35)*($AG35:DK35=2))>MAX(COLUMN($AG35:DK35)*($AG35:DK35=3)),MAX(COLUMN($AG35:DK35)*($AG35:DK35=2))>MAX(COLUMN($AG35:DK35)*($AG35:DK35=1))),IF(COLUMN(DL35)-MAX(COLUMN($AG35:DK35)*($AG35:DK35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DL35)-MAX(COLUMN($AG35:DK35)*($AG35:DK35=3))=$J35,3,0),IF(COLUMN(DL35)-MAX(COLUMN($AG35:DK35)*($AG35:DK35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DL35)*($AG35:DL35=1))>MAX(COLUMN($AG35:DL35)*($AG35:DL35=3)),MAX(COLUMN($AG35:DL35)*($AG35:DL35=1))>MAX(COLUMN($AG35:DL35)*($AG35:DL35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DM35)-MAX(COLUMN($AG35:DL35)*($AG35:DL35=1))=$J35,3,0),IF(COLUMN(DM35)-MAX(COLUMN($AG35:DL35)*($AG35:DL35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DL35)*($AG35:DL35=2))>MAX(COLUMN($AG35:DL35)*($AG35:DL35=3)),MAX(COLUMN($AG35:DL35)*($AG35:DL35=2))>MAX(COLUMN($AG35:DL35)*($AG35:DL35=1))),IF(COLUMN(DM35)-MAX(COLUMN($AG35:DL35)*($AG35:DL35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DM35)-MAX(COLUMN($AG35:DL35)*($AG35:DL35=3))=$J35,3,0),IF(COLUMN(DM35)-MAX(COLUMN($AG35:DL35)*($AG35:DL35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DM35)*($AG35:DM35=1))>MAX(COLUMN($AG35:DM35)*($AG35:DM35=3)),MAX(COLUMN($AG35:DM35)*($AG35:DM35=1))>MAX(COLUMN($AG35:DM35)*($AG35:DM35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DN35)-MAX(COLUMN($AG35:DM35)*($AG35:DM35=1))=$J35,3,0),IF(COLUMN(DN35)-MAX(COLUMN($AG35:DM35)*($AG35:DM35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DM35)*($AG35:DM35=2))>MAX(COLUMN($AG35:DM35)*($AG35:DM35=3)),MAX(COLUMN($AG35:DM35)*($AG35:DM35=2))>MAX(COLUMN($AG35:DM35)*($AG35:DM35=1))),IF(COLUMN(DN35)-MAX(COLUMN($AG35:DM35)*($AG35:DM35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DN35)-MAX(COLUMN($AG35:DM35)*($AG35:DM35=3))=$J35,3,0),IF(COLUMN(DN35)-MAX(COLUMN($AG35:DM35)*($AG35:DM35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DN35)*($AG35:DN35=1))>MAX(COLUMN($AG35:DN35)*($AG35:DN35=3)),MAX(COLUMN($AG35:DN35)*($AG35:DN35=1))>MAX(COLUMN($AG35:DN35)*($AG35:DN35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DO35)-MAX(COLUMN($AG35:DN35)*($AG35:DN35=1))=$J35,3,0),IF(COLUMN(DO35)-MAX(COLUMN($AG35:DN35)*($AG35:DN35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DN35)*($AG35:DN35=2))>MAX(COLUMN($AG35:DN35)*($AG35:DN35=3)),MAX(COLUMN($AG35:DN35)*($AG35:DN35=2))>MAX(COLUMN($AG35:DN35)*($AG35:DN35=1))),IF(COLUMN(DO35)-MAX(COLUMN($AG35:DN35)*($AG35:DN35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DO35)-MAX(COLUMN($AG35:DN35)*($AG35:DN35=3))=$J35,3,0),IF(COLUMN(DO35)-MAX(COLUMN($AG35:DN35)*($AG35:DN35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DO35)*($AG35:DO35=1))>MAX(COLUMN($AG35:DO35)*($AG35:DO35=3)),MAX(COLUMN($AG35:DO35)*($AG35:DO35=1))>MAX(COLUMN($AG35:DO35)*($AG35:DO35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DP35)-MAX(COLUMN($AG35:DO35)*($AG35:DO35=1))=$J35,3,0),IF(COLUMN(DP35)-MAX(COLUMN($AG35:DO35)*($AG35:DO35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DO35)*($AG35:DO35=2))>MAX(COLUMN($AG35:DO35)*($AG35:DO35=3)),MAX(COLUMN($AG35:DO35)*($AG35:DO35=2))>MAX(COLUMN($AG35:DO35)*($AG35:DO35=1))),IF(COLUMN(DP35)-MAX(COLUMN($AG35:DO35)*($AG35:DO35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DP35)-MAX(COLUMN($AG35:DO35)*($AG35:DO35=3))=$J35,3,0),IF(COLUMN(DP35)-MAX(COLUMN($AG35:DO35)*($AG35:DO35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DP35)*($AG35:DP35=1))>MAX(COLUMN($AG35:DP35)*($AG35:DP35=3)),MAX(COLUMN($AG35:DP35)*($AG35:DP35=1))>MAX(COLUMN($AG35:DP35)*($AG35:DP35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DQ35)-MAX(COLUMN($AG35:DP35)*($AG35:DP35=1))=$J35,3,0),IF(COLUMN(DQ35)-MAX(COLUMN($AG35:DP35)*($AG35:DP35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DP35)*($AG35:DP35=2))>MAX(COLUMN($AG35:DP35)*($AG35:DP35=3)),MAX(COLUMN($AG35:DP35)*($AG35:DP35=2))>MAX(COLUMN($AG35:DP35)*($AG35:DP35=1))),IF(COLUMN(DQ35)-MAX(COLUMN($AG35:DP35)*($AG35:DP35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DQ35)-MAX(COLUMN($AG35:DP35)*($AG35:DP35=3))=$J35,3,0),IF(COLUMN(DQ35)-MAX(COLUMN($AG35:DP35)*($AG35:DP35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=1))>MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=3)),MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=1))>MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DR35)-MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=1))=$J35,3,0),IF(COLUMN(DR35)-MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=2))>MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=3)),MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=2))>MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=1))),IF(COLUMN(DR35)-MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DR35)-MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=3))=$J35,3,0),IF(COLUMN(DR35)-MAX(COLUMN($AG35:DQ35)*($AG35:DQ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DR35)*($AG35:DR35=1))>MAX(COLUMN($AG35:DR35)*($AG35:DR35=3)),MAX(COLUMN($AG35:DR35)*($AG35:DR35=1))>MAX(COLUMN($AG35:DR35)*($AG35:DR35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DS35)-MAX(COLUMN($AG35:DR35)*($AG35:DR35=1))=$J35,3,0),IF(COLUMN(DS35)-MAX(COLUMN($AG35:DR35)*($AG35:DR35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DR35)*($AG35:DR35=2))>MAX(COLUMN($AG35:DR35)*($AG35:DR35=3)),MAX(COLUMN($AG35:DR35)*($AG35:DR35=2))>MAX(COLUMN($AG35:DR35)*($AG35:DR35=1))),IF(COLUMN(DS35)-MAX(COLUMN($AG35:DR35)*($AG35:DR35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DS35)-MAX(COLUMN($AG35:DR35)*($AG35:DR35=3))=$J35,3,0),IF(COLUMN(DS35)-MAX(COLUMN($AG35:DR35)*($AG35:DR35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DS35)*($AG35:DS35=1))>MAX(COLUMN($AG35:DS35)*($AG35:DS35=3)),MAX(COLUMN($AG35:DS35)*($AG35:DS35=1))>MAX(COLUMN($AG35:DS35)*($AG35:DS35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DT35)-MAX(COLUMN($AG35:DS35)*($AG35:DS35=1))=$J35,3,0),IF(COLUMN(DT35)-MAX(COLUMN($AG35:DS35)*($AG35:DS35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DS35)*($AG35:DS35=2))>MAX(COLUMN($AG35:DS35)*($AG35:DS35=3)),MAX(COLUMN($AG35:DS35)*($AG35:DS35=2))>MAX(COLUMN($AG35:DS35)*($AG35:DS35=1))),IF(COLUMN(DT35)-MAX(COLUMN($AG35:DS35)*($AG35:DS35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DT35)-MAX(COLUMN($AG35:DS35)*($AG35:DS35=3))=$J35,3,0),IF(COLUMN(DT35)-MAX(COLUMN($AG35:DS35)*($AG35:DS35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DT35)*($AG35:DT35=1))>MAX(COLUMN($AG35:DT35)*($AG35:DT35=3)),MAX(COLUMN($AG35:DT35)*($AG35:DT35=1))>MAX(COLUMN($AG35:DT35)*($AG35:DT35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DU35)-MAX(COLUMN($AG35:DT35)*($AG35:DT35=1))=$J35,3,0),IF(COLUMN(DU35)-MAX(COLUMN($AG35:DT35)*($AG35:DT35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DT35)*($AG35:DT35=2))>MAX(COLUMN($AG35:DT35)*($AG35:DT35=3)),MAX(COLUMN($AG35:DT35)*($AG35:DT35=2))>MAX(COLUMN($AG35:DT35)*($AG35:DT35=1))),IF(COLUMN(DU35)-MAX(COLUMN($AG35:DT35)*($AG35:DT35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DU35)-MAX(COLUMN($AG35:DT35)*($AG35:DT35=3))=$J35,3,0),IF(COLUMN(DU35)-MAX(COLUMN($AG35:DT35)*($AG35:DT35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DU35)*($AG35:DU35=1))>MAX(COLUMN($AG35:DU35)*($AG35:DU35=3)),MAX(COLUMN($AG35:DU35)*($AG35:DU35=1))>MAX(COLUMN($AG35:DU35)*($AG35:DU35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DV35)-MAX(COLUMN($AG35:DU35)*($AG35:DU35=1))=$J35,3,0),IF(COLUMN(DV35)-MAX(COLUMN($AG35:DU35)*($AG35:DU35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DU35)*($AG35:DU35=2))>MAX(COLUMN($AG35:DU35)*($AG35:DU35=3)),MAX(COLUMN($AG35:DU35)*($AG35:DU35=2))>MAX(COLUMN($AG35:DU35)*($AG35:DU35=1))),IF(COLUMN(DV35)-MAX(COLUMN($AG35:DU35)*($AG35:DU35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DV35)-MAX(COLUMN($AG35:DU35)*($AG35:DU35=3))=$J35,3,0),IF(COLUMN(DV35)-MAX(COLUMN($AG35:DU35)*($AG35:DU35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DV35)*($AG35:DV35=1))>MAX(COLUMN($AG35:DV35)*($AG35:DV35=3)),MAX(COLUMN($AG35:DV35)*($AG35:DV35=1))>MAX(COLUMN($AG35:DV35)*($AG35:DV35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DW35)-MAX(COLUMN($AG35:DV35)*($AG35:DV35=1))=$J35,3,0),IF(COLUMN(DW35)-MAX(COLUMN($AG35:DV35)*($AG35:DV35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DV35)*($AG35:DV35=2))>MAX(COLUMN($AG35:DV35)*($AG35:DV35=3)),MAX(COLUMN($AG35:DV35)*($AG35:DV35=2))>MAX(COLUMN($AG35:DV35)*($AG35:DV35=1))),IF(COLUMN(DW35)-MAX(COLUMN($AG35:DV35)*($AG35:DV35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DW35)-MAX(COLUMN($AG35:DV35)*($AG35:DV35=3))=$J35,3,0),IF(COLUMN(DW35)-MAX(COLUMN($AG35:DV35)*($AG35:DV35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DW35)*($AG35:DW35=1))>MAX(COLUMN($AG35:DW35)*($AG35:DW35=3)),MAX(COLUMN($AG35:DW35)*($AG35:DW35=1))>MAX(COLUMN($AG35:DW35)*($AG35:DW35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DX35)-MAX(COLUMN($AG35:DW35)*($AG35:DW35=1))=$J35,3,0),IF(COLUMN(DX35)-MAX(COLUMN($AG35:DW35)*($AG35:DW35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DW35)*($AG35:DW35=2))>MAX(COLUMN($AG35:DW35)*($AG35:DW35=3)),MAX(COLUMN($AG35:DW35)*($AG35:DW35=2))>MAX(COLUMN($AG35:DW35)*($AG35:DW35=1))),IF(COLUMN(DX35)-MAX(COLUMN($AG35:DW35)*($AG35:DW35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DX35)-MAX(COLUMN($AG35:DW35)*($AG35:DW35=3))=$J35,3,0),IF(COLUMN(DX35)-MAX(COLUMN($AG35:DW35)*($AG35:DW35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DX35)*($AG35:DX35=1))>MAX(COLUMN($AG35:DX35)*($AG35:DX35=3)),MAX(COLUMN($AG35:DX35)*($AG35:DX35=1))>MAX(COLUMN($AG35:DX35)*($AG35:DX35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DY35)-MAX(COLUMN($AG35:DX35)*($AG35:DX35=1))=$J35,3,0),IF(COLUMN(DY35)-MAX(COLUMN($AG35:DX35)*($AG35:DX35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DX35)*($AG35:DX35=2))>MAX(COLUMN($AG35:DX35)*($AG35:DX35=3)),MAX(COLUMN($AG35:DX35)*($AG35:DX35=2))>MAX(COLUMN($AG35:DX35)*($AG35:DX35=1))),IF(COLUMN(DY35)-MAX(COLUMN($AG35:DX35)*($AG35:DX35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DY35)-MAX(COLUMN($AG35:DX35)*($AG35:DX35=3))=$J35,3,0),IF(COLUMN(DY35)-MAX(COLUMN($AG35:DX35)*($AG35:DX35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DY35)*($AG35:DY35=1))>MAX(COLUMN($AG35:DY35)*($AG35:DY35=3)),MAX(COLUMN($AG35:DY35)*($AG35:DY35=1))>MAX(COLUMN($AG35:DY35)*($AG35:DY35=2))),IF($K35=\"Not Possible\",IF(COLUMN(DZ35)-MAX(COLUMN($AG35:DY35)*($AG35:DY35=1))=$J35,3,0),IF(COLUMN(DZ35)-MAX(COLUMN($AG35:DY35)*($AG35:DY35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DY35)*($AG35:DY35=2))>MAX(COLUMN($AG35:DY35)*($AG35:DY35=3)),MAX(COLUMN($AG35:DY35)*($AG35:DY35=2))>MAX(COLUMN($AG35:DY35)*($AG35:DY35=1))),IF(COLUMN(DZ35)-MAX(COLUMN($AG35:DY35)*($AG35:DY35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(DZ35)-MAX(COLUMN($AG35:DY35)*($AG35:DY35=3))=$J35,3,0),IF(COLUMN(DZ35)-MAX(COLUMN($AG35:DY35)*($AG35:DY35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=1))>MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=3)),MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=1))>MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=2))),IF($K35=\"Not Possible\",IF(COLUMN(EA35)-MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=1))=$J35,3,0),IF(COLUMN(EA35)-MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=2))>MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=3)),MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=2))>MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=1))),IF(COLUMN(EA35)-MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(EA35)-MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=3))=$J35,3,0),IF(COLUMN(EA35)-MAX(COLUMN($AG35:DZ35)*($AG35:DZ35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:EA35)*($AG35:EA35=1))>MAX(COLUMN($AG35:EA35)*($AG35:EA35=3)),MAX(COLUMN($AG35:EA35)*($AG35:EA35=1))>MAX(COLUMN($AG35:EA35)*($AG35:EA35=2))),IF($K35=\"Not Possible\",IF(COLUMN(EB35)-MAX(COLUMN($AG35:EA35)*($AG35:EA35=1))=$J35,3,0),IF(COLUMN(EB35)-MAX(COLUMN($AG35:EA35)*($AG35:EA35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:EA35)*($AG35:EA35=2))>MAX(COLUMN($AG35:EA35)*($AG35:EA35=3)),MAX(COLUMN($AG35:EA35)*($AG35:EA35=2))>MAX(COLUMN($AG35:EA35)*($AG35:EA35=1))),IF(COLUMN(EB35)-MAX(COLUMN($AG35:EA35)*($AG35:EA35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(EB35)-MAX(COLUMN($AG35:EA35)*($AG35:EA35=3))=$J35,3,0),IF(COLUMN(EB35)-MAX(COLUMN($AG35:EA35)*($AG35:EA35=3))=$J35,2,0)))))","v":0},{"$f":"IF($AG35=4,0,IF(AND(MAX(COLUMN($AG35:EB35)*($AG35:EB35=1))>MAX(COLUMN($AG35:EB35)*($AG35:EB35=3)),MAX(COLUMN($AG35:EB35)*($AG35:EB35=1))>MAX(COLUMN($AG35:EB35)*($AG35:EB35=2))),IF($K35=\"Not Possible\",IF(COLUMN(EC35)-MAX(COLUMN($AG35:EB35)*($AG35:EB35=1))=$J35,3,0),IF(COLUMN(EC35)-MAX(COLUMN($AG35:EB35)*($AG35:EB35=1))=$J35,2,0)),IF(AND(MAX(COLUMN($AG35:EB35)*($AG35:EB35=2))>MAX(COLUMN($AG35:EB35)*($AG35:EB35=3)),MAX(COLUMN($AG35:EB35)*($AG35:EB35=2))>MAX(COLUMN($AG35:EB35)*($AG35:EB35=1))),IF(COLUMN(EC35)-MAX(COLUMN($AG35:EB35)*($AG35:EB35=2))=$L35,3,0),IF($K35=\"Not Possible\",IF(COLUMN(EC35)-MAX(COLUMN($AG35:EB35)*($AG35:EB35=3))=$J35,3,0),IF(COLUMN(EC35)-MAX(COLUMN($AG35:EB35)*($AG35:EB35=3))=$J35,2,0)))))","v":2}]
[null,null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"BridEA03"},"Footbridge",{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset class],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"Bridge - Pedestrian"},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",Form_Asset[[#This Row],[Asset ID]]&ROW())","v":"BridEA0336"},"Concrete wingwall","Headwall",{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",INDEX(AssetListTbl[Best Estimate Life (5)],(MATCH(Form_Asset[[#This Row],[Sub-Asset category]],AssetListTbl[Sub-Element Category],0))))","v":80},80,"Moderate Refurbishment",50,"New Build",{"$f":"MAX(COLUMN($AH36:EC36)*($AH36:EC36=2))","v":113},{"$f":"MAX(COLUMN($AH36:EC36)*($AH36:EC36=3))","v":0},{"$f":"IFERROR(100-(IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Replace]])),INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Refurb]])))),0)","v":100},{"$f":"IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],3,2)","v":2},{"$f":"SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Product_Stage[CO2e (t)])","v":9.9959999999999987},{"$f":"IFERROR(SUM(Form_Elements[General Item Material])*(Form_Asset[[#This Row],[Weighted Split]]/SUM(Form_Asset[Weighted Split]))+Form_Asset[[#This Row],[Weighted Split]],0)","v":9.9959999999999987},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth (wtt)]))+(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Transport]))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":9.8487154300000004E-2},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Non contractor People Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Contractor people transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":5.5466773983717341E-2},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":1.4645867812704565E-3},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Site establishment])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":6.2363981349547078E-2},{"$f":"IFERROR(IF($D$88=\"Summary\",((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),(SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Const_Ins_InsB[CO2e (t)]))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Other Construction Waste])*Form_Asset[[#This Row],[Weighted Split]]/(SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[[Waste Co2e ]])+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":2.7127509136874998E-2},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New build\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]]),IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",(SUM(Form_Asset[[#This Row],[Materials]:[Waste]])-(SUM(Form_Asset[[#This Row],[Materials Transport]],Form_Asset[[#This Row],[People Transport]]*0.5,Form_Asset[[#This Row],[Plant Transport]]*0.5))),IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]])/(SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%])),0)))","v":10.24091000555141},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":6.2122316225226844E-4},{"$f":"IFERROR(SUMIF(Form_use_energy[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_use_energy[CO2e (t)]),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset ref.]]=\"\",0,SUMIF(Form_Asset[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Asset[New Build Co2e])*SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%]))","v":2.5602275013878524},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Dem - General Item Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Dem -Waste Co2e]),0)","v":0.15372255177562497},{"$f":"(Form_Asset[[#This Row],[Plant use]]+Form_Asset[[#This Row],[Plant Transport]])*50%","v":7.3229339063522823E-4},{"$f":"Form_Asset[[#This Row],[People Transport]]*50%","v":2.773338699185867E-2},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New Build\",1,IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",2,IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",3,IF(Form_Asset[[#This Row],[First intervention]]=\"Demolition\",4,\"\"))))","v":1},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AG36)*($AG36:AG36=1))>MAX(COLUMN($AG36:AG36)*($AG36:AG36=3)),MAX(COLUMN($AG36:AG36)*($AG36:AG36=1))>MAX(COLUMN($AG36:AG36)*($AG36:AG36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AH36)-MAX(COLUMN($AG36:AG36)*($AG36:AG36=1))=$J36,3,0),IF(COLUMN(AH36)-MAX(COLUMN($AG36:AG36)*($AG36:AG36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AG36)*($AG36:AG36=2))>MAX(COLUMN($AG36:AG36)*($AG36:AG36=3)),MAX(COLUMN($AG36:AG36)*($AG36:AG36=2))>MAX(COLUMN($AG36:AG36)*($AG36:AG36=1))),IF(COLUMN(AH36)-MAX(COLUMN($AG36:AG36)*($AG36:AG36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AH36)-MAX(COLUMN($AG36:AG36)*($AG36:AG36=3))=$J36,3,0),IF(COLUMN(AH36)-MAX(COLUMN($AG36:AG36)*($AG36:AG36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AH36)*($AG36:AH36=1))>MAX(COLUMN($AG36:AH36)*($AG36:AH36=3)),MAX(COLUMN($AG36:AH36)*($AG36:AH36=1))>MAX(COLUMN($AG36:AH36)*($AG36:AH36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AI36)-MAX(COLUMN($AG36:AH36)*($AG36:AH36=1))=$J36,3,0),IF(COLUMN(AI36)-MAX(COLUMN($AG36:AH36)*($AG36:AH36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AH36)*($AG36:AH36=2))>MAX(COLUMN($AG36:AH36)*($AG36:AH36=3)),MAX(COLUMN($AG36:AH36)*($AG36:AH36=2))>MAX(COLUMN($AG36:AH36)*($AG36:AH36=1))),IF(COLUMN(AI36)-MAX(COLUMN($AG36:AH36)*($AG36:AH36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AI36)-MAX(COLUMN($AG36:AH36)*($AG36:AH36=3))=$J36,3,0),IF(COLUMN(AI36)-MAX(COLUMN($AG36:AH36)*($AG36:AH36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AI36)*($AG36:AI36=1))>MAX(COLUMN($AG36:AI36)*($AG36:AI36=3)),MAX(COLUMN($AG36:AI36)*($AG36:AI36=1))>MAX(COLUMN($AG36:AI36)*($AG36:AI36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AJ36)-MAX(COLUMN($AG36:AI36)*($AG36:AI36=1))=$J36,3,0),IF(COLUMN(AJ36)-MAX(COLUMN($AG36:AI36)*($AG36:AI36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AI36)*($AG36:AI36=2))>MAX(COLUMN($AG36:AI36)*($AG36:AI36=3)),MAX(COLUMN($AG36:AI36)*($AG36:AI36=2))>MAX(COLUMN($AG36:AI36)*($AG36:AI36=1))),IF(COLUMN(AJ36)-MAX(COLUMN($AG36:AI36)*($AG36:AI36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AJ36)-MAX(COLUMN($AG36:AI36)*($AG36:AI36=3))=$J36,3,0),IF(COLUMN(AJ36)-MAX(COLUMN($AG36:AI36)*($AG36:AI36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=1))>MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=3)),MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=1))>MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AK36)-MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=1))=$J36,3,0),IF(COLUMN(AK36)-MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=2))>MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=3)),MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=2))>MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=1))),IF(COLUMN(AK36)-MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AK36)-MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=3))=$J36,3,0),IF(COLUMN(AK36)-MAX(COLUMN($AG36:AJ36)*($AG36:AJ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AK36)*($AG36:AK36=1))>MAX(COLUMN($AG36:AK36)*($AG36:AK36=3)),MAX(COLUMN($AG36:AK36)*($AG36:AK36=1))>MAX(COLUMN($AG36:AK36)*($AG36:AK36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AL36)-MAX(COLUMN($AG36:AK36)*($AG36:AK36=1))=$J36,3,0),IF(COLUMN(AL36)-MAX(COLUMN($AG36:AK36)*($AG36:AK36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AK36)*($AG36:AK36=2))>MAX(COLUMN($AG36:AK36)*($AG36:AK36=3)),MAX(COLUMN($AG36:AK36)*($AG36:AK36=2))>MAX(COLUMN($AG36:AK36)*($AG36:AK36=1))),IF(COLUMN(AL36)-MAX(COLUMN($AG36:AK36)*($AG36:AK36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AL36)-MAX(COLUMN($AG36:AK36)*($AG36:AK36=3))=$J36,3,0),IF(COLUMN(AL36)-MAX(COLUMN($AG36:AK36)*($AG36:AK36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AL36)*($AG36:AL36=1))>MAX(COLUMN($AG36:AL36)*($AG36:AL36=3)),MAX(COLUMN($AG36:AL36)*($AG36:AL36=1))>MAX(COLUMN($AG36:AL36)*($AG36:AL36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AM36)-MAX(COLUMN($AG36:AL36)*($AG36:AL36=1))=$J36,3,0),IF(COLUMN(AM36)-MAX(COLUMN($AG36:AL36)*($AG36:AL36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AL36)*($AG36:AL36=2))>MAX(COLUMN($AG36:AL36)*($AG36:AL36=3)),MAX(COLUMN($AG36:AL36)*($AG36:AL36=2))>MAX(COLUMN($AG36:AL36)*($AG36:AL36=1))),IF(COLUMN(AM36)-MAX(COLUMN($AG36:AL36)*($AG36:AL36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AM36)-MAX(COLUMN($AG36:AL36)*($AG36:AL36=3))=$J36,3,0),IF(COLUMN(AM36)-MAX(COLUMN($AG36:AL36)*($AG36:AL36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AM36)*($AG36:AM36=1))>MAX(COLUMN($AG36:AM36)*($AG36:AM36=3)),MAX(COLUMN($AG36:AM36)*($AG36:AM36=1))>MAX(COLUMN($AG36:AM36)*($AG36:AM36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AN36)-MAX(COLUMN($AG36:AM36)*($AG36:AM36=1))=$J36,3,0),IF(COLUMN(AN36)-MAX(COLUMN($AG36:AM36)*($AG36:AM36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AM36)*($AG36:AM36=2))>MAX(COLUMN($AG36:AM36)*($AG36:AM36=3)),MAX(COLUMN($AG36:AM36)*($AG36:AM36=2))>MAX(COLUMN($AG36:AM36)*($AG36:AM36=1))),IF(COLUMN(AN36)-MAX(COLUMN($AG36:AM36)*($AG36:AM36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AN36)-MAX(COLUMN($AG36:AM36)*($AG36:AM36=3))=$J36,3,0),IF(COLUMN(AN36)-MAX(COLUMN($AG36:AM36)*($AG36:AM36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AN36)*($AG36:AN36=1))>MAX(COLUMN($AG36:AN36)*($AG36:AN36=3)),MAX(COLUMN($AG36:AN36)*($AG36:AN36=1))>MAX(COLUMN($AG36:AN36)*($AG36:AN36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AO36)-MAX(COLUMN($AG36:AN36)*($AG36:AN36=1))=$J36,3,0),IF(COLUMN(AO36)-MAX(COLUMN($AG36:AN36)*($AG36:AN36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AN36)*($AG36:AN36=2))>MAX(COLUMN($AG36:AN36)*($AG36:AN36=3)),MAX(COLUMN($AG36:AN36)*($AG36:AN36=2))>MAX(COLUMN($AG36:AN36)*($AG36:AN36=1))),IF(COLUMN(AO36)-MAX(COLUMN($AG36:AN36)*($AG36:AN36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AO36)-MAX(COLUMN($AG36:AN36)*($AG36:AN36=3))=$J36,3,0),IF(COLUMN(AO36)-MAX(COLUMN($AG36:AN36)*($AG36:AN36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AO36)*($AG36:AO36=1))>MAX(COLUMN($AG36:AO36)*($AG36:AO36=3)),MAX(COLUMN($AG36:AO36)*($AG36:AO36=1))>MAX(COLUMN($AG36:AO36)*($AG36:AO36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AP36)-MAX(COLUMN($AG36:AO36)*($AG36:AO36=1))=$J36,3,0),IF(COLUMN(AP36)-MAX(COLUMN($AG36:AO36)*($AG36:AO36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AO36)*($AG36:AO36=2))>MAX(COLUMN($AG36:AO36)*($AG36:AO36=3)),MAX(COLUMN($AG36:AO36)*($AG36:AO36=2))>MAX(COLUMN($AG36:AO36)*($AG36:AO36=1))),IF(COLUMN(AP36)-MAX(COLUMN($AG36:AO36)*($AG36:AO36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AP36)-MAX(COLUMN($AG36:AO36)*($AG36:AO36=3))=$J36,3,0),IF(COLUMN(AP36)-MAX(COLUMN($AG36:AO36)*($AG36:AO36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AP36)*($AG36:AP36=1))>MAX(COLUMN($AG36:AP36)*($AG36:AP36=3)),MAX(COLUMN($AG36:AP36)*($AG36:AP36=1))>MAX(COLUMN($AG36:AP36)*($AG36:AP36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AQ36)-MAX(COLUMN($AG36:AP36)*($AG36:AP36=1))=$J36,3,0),IF(COLUMN(AQ36)-MAX(COLUMN($AG36:AP36)*($AG36:AP36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AP36)*($AG36:AP36=2))>MAX(COLUMN($AG36:AP36)*($AG36:AP36=3)),MAX(COLUMN($AG36:AP36)*($AG36:AP36=2))>MAX(COLUMN($AG36:AP36)*($AG36:AP36=1))),IF(COLUMN(AQ36)-MAX(COLUMN($AG36:AP36)*($AG36:AP36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AQ36)-MAX(COLUMN($AG36:AP36)*($AG36:AP36=3))=$J36,3,0),IF(COLUMN(AQ36)-MAX(COLUMN($AG36:AP36)*($AG36:AP36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=1))>MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=3)),MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=1))>MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AR36)-MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=1))=$J36,3,0),IF(COLUMN(AR36)-MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=2))>MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=3)),MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=2))>MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=1))),IF(COLUMN(AR36)-MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AR36)-MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=3))=$J36,3,0),IF(COLUMN(AR36)-MAX(COLUMN($AG36:AQ36)*($AG36:AQ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AR36)*($AG36:AR36=1))>MAX(COLUMN($AG36:AR36)*($AG36:AR36=3)),MAX(COLUMN($AG36:AR36)*($AG36:AR36=1))>MAX(COLUMN($AG36:AR36)*($AG36:AR36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AS36)-MAX(COLUMN($AG36:AR36)*($AG36:AR36=1))=$J36,3,0),IF(COLUMN(AS36)-MAX(COLUMN($AG36:AR36)*($AG36:AR36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AR36)*($AG36:AR36=2))>MAX(COLUMN($AG36:AR36)*($AG36:AR36=3)),MAX(COLUMN($AG36:AR36)*($AG36:AR36=2))>MAX(COLUMN($AG36:AR36)*($AG36:AR36=1))),IF(COLUMN(AS36)-MAX(COLUMN($AG36:AR36)*($AG36:AR36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AS36)-MAX(COLUMN($AG36:AR36)*($AG36:AR36=3))=$J36,3,0),IF(COLUMN(AS36)-MAX(COLUMN($AG36:AR36)*($AG36:AR36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AS36)*($AG36:AS36=1))>MAX(COLUMN($AG36:AS36)*($AG36:AS36=3)),MAX(COLUMN($AG36:AS36)*($AG36:AS36=1))>MAX(COLUMN($AG36:AS36)*($AG36:AS36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AT36)-MAX(COLUMN($AG36:AS36)*($AG36:AS36=1))=$J36,3,0),IF(COLUMN(AT36)-MAX(COLUMN($AG36:AS36)*($AG36:AS36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AS36)*($AG36:AS36=2))>MAX(COLUMN($AG36:AS36)*($AG36:AS36=3)),MAX(COLUMN($AG36:AS36)*($AG36:AS36=2))>MAX(COLUMN($AG36:AS36)*($AG36:AS36=1))),IF(COLUMN(AT36)-MAX(COLUMN($AG36:AS36)*($AG36:AS36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AT36)-MAX(COLUMN($AG36:AS36)*($AG36:AS36=3))=$J36,3,0),IF(COLUMN(AT36)-MAX(COLUMN($AG36:AS36)*($AG36:AS36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AT36)*($AG36:AT36=1))>MAX(COLUMN($AG36:AT36)*($AG36:AT36=3)),MAX(COLUMN($AG36:AT36)*($AG36:AT36=1))>MAX(COLUMN($AG36:AT36)*($AG36:AT36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AU36)-MAX(COLUMN($AG36:AT36)*($AG36:AT36=1))=$J36,3,0),IF(COLUMN(AU36)-MAX(COLUMN($AG36:AT36)*($AG36:AT36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AT36)*($AG36:AT36=2))>MAX(COLUMN($AG36:AT36)*($AG36:AT36=3)),MAX(COLUMN($AG36:AT36)*($AG36:AT36=2))>MAX(COLUMN($AG36:AT36)*($AG36:AT36=1))),IF(COLUMN(AU36)-MAX(COLUMN($AG36:AT36)*($AG36:AT36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AU36)-MAX(COLUMN($AG36:AT36)*($AG36:AT36=3))=$J36,3,0),IF(COLUMN(AU36)-MAX(COLUMN($AG36:AT36)*($AG36:AT36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AU36)*($AG36:AU36=1))>MAX(COLUMN($AG36:AU36)*($AG36:AU36=3)),MAX(COLUMN($AG36:AU36)*($AG36:AU36=1))>MAX(COLUMN($AG36:AU36)*($AG36:AU36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AV36)-MAX(COLUMN($AG36:AU36)*($AG36:AU36=1))=$J36,3,0),IF(COLUMN(AV36)-MAX(COLUMN($AG36:AU36)*($AG36:AU36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AU36)*($AG36:AU36=2))>MAX(COLUMN($AG36:AU36)*($AG36:AU36=3)),MAX(COLUMN($AG36:AU36)*($AG36:AU36=2))>MAX(COLUMN($AG36:AU36)*($AG36:AU36=1))),IF(COLUMN(AV36)-MAX(COLUMN($AG36:AU36)*($AG36:AU36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AV36)-MAX(COLUMN($AG36:AU36)*($AG36:AU36=3))=$J36,3,0),IF(COLUMN(AV36)-MAX(COLUMN($AG36:AU36)*($AG36:AU36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AV36)*($AG36:AV36=1))>MAX(COLUMN($AG36:AV36)*($AG36:AV36=3)),MAX(COLUMN($AG36:AV36)*($AG36:AV36=1))>MAX(COLUMN($AG36:AV36)*($AG36:AV36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AW36)-MAX(COLUMN($AG36:AV36)*($AG36:AV36=1))=$J36,3,0),IF(COLUMN(AW36)-MAX(COLUMN($AG36:AV36)*($AG36:AV36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AV36)*($AG36:AV36=2))>MAX(COLUMN($AG36:AV36)*($AG36:AV36=3)),MAX(COLUMN($AG36:AV36)*($AG36:AV36=2))>MAX(COLUMN($AG36:AV36)*($AG36:AV36=1))),IF(COLUMN(AW36)-MAX(COLUMN($AG36:AV36)*($AG36:AV36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AW36)-MAX(COLUMN($AG36:AV36)*($AG36:AV36=3))=$J36,3,0),IF(COLUMN(AW36)-MAX(COLUMN($AG36:AV36)*($AG36:AV36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AW36)*($AG36:AW36=1))>MAX(COLUMN($AG36:AW36)*($AG36:AW36=3)),MAX(COLUMN($AG36:AW36)*($AG36:AW36=1))>MAX(COLUMN($AG36:AW36)*($AG36:AW36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AX36)-MAX(COLUMN($AG36:AW36)*($AG36:AW36=1))=$J36,3,0),IF(COLUMN(AX36)-MAX(COLUMN($AG36:AW36)*($AG36:AW36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AW36)*($AG36:AW36=2))>MAX(COLUMN($AG36:AW36)*($AG36:AW36=3)),MAX(COLUMN($AG36:AW36)*($AG36:AW36=2))>MAX(COLUMN($AG36:AW36)*($AG36:AW36=1))),IF(COLUMN(AX36)-MAX(COLUMN($AG36:AW36)*($AG36:AW36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AX36)-MAX(COLUMN($AG36:AW36)*($AG36:AW36=3))=$J36,3,0),IF(COLUMN(AX36)-MAX(COLUMN($AG36:AW36)*($AG36:AW36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AX36)*($AG36:AX36=1))>MAX(COLUMN($AG36:AX36)*($AG36:AX36=3)),MAX(COLUMN($AG36:AX36)*($AG36:AX36=1))>MAX(COLUMN($AG36:AX36)*($AG36:AX36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AY36)-MAX(COLUMN($AG36:AX36)*($AG36:AX36=1))=$J36,3,0),IF(COLUMN(AY36)-MAX(COLUMN($AG36:AX36)*($AG36:AX36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AX36)*($AG36:AX36=2))>MAX(COLUMN($AG36:AX36)*($AG36:AX36=3)),MAX(COLUMN($AG36:AX36)*($AG36:AX36=2))>MAX(COLUMN($AG36:AX36)*($AG36:AX36=1))),IF(COLUMN(AY36)-MAX(COLUMN($AG36:AX36)*($AG36:AX36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AY36)-MAX(COLUMN($AG36:AX36)*($AG36:AX36=3))=$J36,3,0),IF(COLUMN(AY36)-MAX(COLUMN($AG36:AX36)*($AG36:AX36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AY36)*($AG36:AY36=1))>MAX(COLUMN($AG36:AY36)*($AG36:AY36=3)),MAX(COLUMN($AG36:AY36)*($AG36:AY36=1))>MAX(COLUMN($AG36:AY36)*($AG36:AY36=2))),IF($K36=\"Not Possible\",IF(COLUMN(AZ36)-MAX(COLUMN($AG36:AY36)*($AG36:AY36=1))=$J36,3,0),IF(COLUMN(AZ36)-MAX(COLUMN($AG36:AY36)*($AG36:AY36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AY36)*($AG36:AY36=2))>MAX(COLUMN($AG36:AY36)*($AG36:AY36=3)),MAX(COLUMN($AG36:AY36)*($AG36:AY36=2))>MAX(COLUMN($AG36:AY36)*($AG36:AY36=1))),IF(COLUMN(AZ36)-MAX(COLUMN($AG36:AY36)*($AG36:AY36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(AZ36)-MAX(COLUMN($AG36:AY36)*($AG36:AY36=3))=$J36,3,0),IF(COLUMN(AZ36)-MAX(COLUMN($AG36:AY36)*($AG36:AY36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=1))>MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=3)),MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=1))>MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BA36)-MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=1))=$J36,3,0),IF(COLUMN(BA36)-MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=2))>MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=3)),MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=2))>MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=1))),IF(COLUMN(BA36)-MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BA36)-MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=3))=$J36,3,0),IF(COLUMN(BA36)-MAX(COLUMN($AG36:AZ36)*($AG36:AZ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BA36)*($AG36:BA36=1))>MAX(COLUMN($AG36:BA36)*($AG36:BA36=3)),MAX(COLUMN($AG36:BA36)*($AG36:BA36=1))>MAX(COLUMN($AG36:BA36)*($AG36:BA36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BB36)-MAX(COLUMN($AG36:BA36)*($AG36:BA36=1))=$J36,3,0),IF(COLUMN(BB36)-MAX(COLUMN($AG36:BA36)*($AG36:BA36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BA36)*($AG36:BA36=2))>MAX(COLUMN($AG36:BA36)*($AG36:BA36=3)),MAX(COLUMN($AG36:BA36)*($AG36:BA36=2))>MAX(COLUMN($AG36:BA36)*($AG36:BA36=1))),IF(COLUMN(BB36)-MAX(COLUMN($AG36:BA36)*($AG36:BA36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BB36)-MAX(COLUMN($AG36:BA36)*($AG36:BA36=3))=$J36,3,0),IF(COLUMN(BB36)-MAX(COLUMN($AG36:BA36)*($AG36:BA36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BB36)*($AG36:BB36=1))>MAX(COLUMN($AG36:BB36)*($AG36:BB36=3)),MAX(COLUMN($AG36:BB36)*($AG36:BB36=1))>MAX(COLUMN($AG36:BB36)*($AG36:BB36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BC36)-MAX(COLUMN($AG36:BB36)*($AG36:BB36=1))=$J36,3,0),IF(COLUMN(BC36)-MAX(COLUMN($AG36:BB36)*($AG36:BB36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BB36)*($AG36:BB36=2))>MAX(COLUMN($AG36:BB36)*($AG36:BB36=3)),MAX(COLUMN($AG36:BB36)*($AG36:BB36=2))>MAX(COLUMN($AG36:BB36)*($AG36:BB36=1))),IF(COLUMN(BC36)-MAX(COLUMN($AG36:BB36)*($AG36:BB36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BC36)-MAX(COLUMN($AG36:BB36)*($AG36:BB36=3))=$J36,3,0),IF(COLUMN(BC36)-MAX(COLUMN($AG36:BB36)*($AG36:BB36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BC36)*($AG36:BC36=1))>MAX(COLUMN($AG36:BC36)*($AG36:BC36=3)),MAX(COLUMN($AG36:BC36)*($AG36:BC36=1))>MAX(COLUMN($AG36:BC36)*($AG36:BC36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BD36)-MAX(COLUMN($AG36:BC36)*($AG36:BC36=1))=$J36,3,0),IF(COLUMN(BD36)-MAX(COLUMN($AG36:BC36)*($AG36:BC36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BC36)*($AG36:BC36=2))>MAX(COLUMN($AG36:BC36)*($AG36:BC36=3)),MAX(COLUMN($AG36:BC36)*($AG36:BC36=2))>MAX(COLUMN($AG36:BC36)*($AG36:BC36=1))),IF(COLUMN(BD36)-MAX(COLUMN($AG36:BC36)*($AG36:BC36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BD36)-MAX(COLUMN($AG36:BC36)*($AG36:BC36=3))=$J36,3,0),IF(COLUMN(BD36)-MAX(COLUMN($AG36:BC36)*($AG36:BC36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BD36)*($AG36:BD36=1))>MAX(COLUMN($AG36:BD36)*($AG36:BD36=3)),MAX(COLUMN($AG36:BD36)*($AG36:BD36=1))>MAX(COLUMN($AG36:BD36)*($AG36:BD36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BE36)-MAX(COLUMN($AG36:BD36)*($AG36:BD36=1))=$J36,3,0),IF(COLUMN(BE36)-MAX(COLUMN($AG36:BD36)*($AG36:BD36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BD36)*($AG36:BD36=2))>MAX(COLUMN($AG36:BD36)*($AG36:BD36=3)),MAX(COLUMN($AG36:BD36)*($AG36:BD36=2))>MAX(COLUMN($AG36:BD36)*($AG36:BD36=1))),IF(COLUMN(BE36)-MAX(COLUMN($AG36:BD36)*($AG36:BD36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BE36)-MAX(COLUMN($AG36:BD36)*($AG36:BD36=3))=$J36,3,0),IF(COLUMN(BE36)-MAX(COLUMN($AG36:BD36)*($AG36:BD36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BE36)*($AG36:BE36=1))>MAX(COLUMN($AG36:BE36)*($AG36:BE36=3)),MAX(COLUMN($AG36:BE36)*($AG36:BE36=1))>MAX(COLUMN($AG36:BE36)*($AG36:BE36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BF36)-MAX(COLUMN($AG36:BE36)*($AG36:BE36=1))=$J36,3,0),IF(COLUMN(BF36)-MAX(COLUMN($AG36:BE36)*($AG36:BE36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BE36)*($AG36:BE36=2))>MAX(COLUMN($AG36:BE36)*($AG36:BE36=3)),MAX(COLUMN($AG36:BE36)*($AG36:BE36=2))>MAX(COLUMN($AG36:BE36)*($AG36:BE36=1))),IF(COLUMN(BF36)-MAX(COLUMN($AG36:BE36)*($AG36:BE36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BF36)-MAX(COLUMN($AG36:BE36)*($AG36:BE36=3))=$J36,3,0),IF(COLUMN(BF36)-MAX(COLUMN($AG36:BE36)*($AG36:BE36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BF36)*($AG36:BF36=1))>MAX(COLUMN($AG36:BF36)*($AG36:BF36=3)),MAX(COLUMN($AG36:BF36)*($AG36:BF36=1))>MAX(COLUMN($AG36:BF36)*($AG36:BF36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BG36)-MAX(COLUMN($AG36:BF36)*($AG36:BF36=1))=$J36,3,0),IF(COLUMN(BG36)-MAX(COLUMN($AG36:BF36)*($AG36:BF36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BF36)*($AG36:BF36=2))>MAX(COLUMN($AG36:BF36)*($AG36:BF36=3)),MAX(COLUMN($AG36:BF36)*($AG36:BF36=2))>MAX(COLUMN($AG36:BF36)*($AG36:BF36=1))),IF(COLUMN(BG36)-MAX(COLUMN($AG36:BF36)*($AG36:BF36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BG36)-MAX(COLUMN($AG36:BF36)*($AG36:BF36=3))=$J36,3,0),IF(COLUMN(BG36)-MAX(COLUMN($AG36:BF36)*($AG36:BF36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BG36)*($AG36:BG36=1))>MAX(COLUMN($AG36:BG36)*($AG36:BG36=3)),MAX(COLUMN($AG36:BG36)*($AG36:BG36=1))>MAX(COLUMN($AG36:BG36)*($AG36:BG36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BH36)-MAX(COLUMN($AG36:BG36)*($AG36:BG36=1))=$J36,3,0),IF(COLUMN(BH36)-MAX(COLUMN($AG36:BG36)*($AG36:BG36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BG36)*($AG36:BG36=2))>MAX(COLUMN($AG36:BG36)*($AG36:BG36=3)),MAX(COLUMN($AG36:BG36)*($AG36:BG36=2))>MAX(COLUMN($AG36:BG36)*($AG36:BG36=1))),IF(COLUMN(BH36)-MAX(COLUMN($AG36:BG36)*($AG36:BG36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BH36)-MAX(COLUMN($AG36:BG36)*($AG36:BG36=3))=$J36,3,0),IF(COLUMN(BH36)-MAX(COLUMN($AG36:BG36)*($AG36:BG36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BH36)*($AG36:BH36=1))>MAX(COLUMN($AG36:BH36)*($AG36:BH36=3)),MAX(COLUMN($AG36:BH36)*($AG36:BH36=1))>MAX(COLUMN($AG36:BH36)*($AG36:BH36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BI36)-MAX(COLUMN($AG36:BH36)*($AG36:BH36=1))=$J36,3,0),IF(COLUMN(BI36)-MAX(COLUMN($AG36:BH36)*($AG36:BH36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BH36)*($AG36:BH36=2))>MAX(COLUMN($AG36:BH36)*($AG36:BH36=3)),MAX(COLUMN($AG36:BH36)*($AG36:BH36=2))>MAX(COLUMN($AG36:BH36)*($AG36:BH36=1))),IF(COLUMN(BI36)-MAX(COLUMN($AG36:BH36)*($AG36:BH36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BI36)-MAX(COLUMN($AG36:BH36)*($AG36:BH36=3))=$J36,3,0),IF(COLUMN(BI36)-MAX(COLUMN($AG36:BH36)*($AG36:BH36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BI36)*($AG36:BI36=1))>MAX(COLUMN($AG36:BI36)*($AG36:BI36=3)),MAX(COLUMN($AG36:BI36)*($AG36:BI36=1))>MAX(COLUMN($AG36:BI36)*($AG36:BI36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BJ36)-MAX(COLUMN($AG36:BI36)*($AG36:BI36=1))=$J36,3,0),IF(COLUMN(BJ36)-MAX(COLUMN($AG36:BI36)*($AG36:BI36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BI36)*($AG36:BI36=2))>MAX(COLUMN($AG36:BI36)*($AG36:BI36=3)),MAX(COLUMN($AG36:BI36)*($AG36:BI36=2))>MAX(COLUMN($AG36:BI36)*($AG36:BI36=1))),IF(COLUMN(BJ36)-MAX(COLUMN($AG36:BI36)*($AG36:BI36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BJ36)-MAX(COLUMN($AG36:BI36)*($AG36:BI36=3))=$J36,3,0),IF(COLUMN(BJ36)-MAX(COLUMN($AG36:BI36)*($AG36:BI36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=1))>MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=3)),MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=1))>MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BK36)-MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=1))=$J36,3,0),IF(COLUMN(BK36)-MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=2))>MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=3)),MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=2))>MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=1))),IF(COLUMN(BK36)-MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BK36)-MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=3))=$J36,3,0),IF(COLUMN(BK36)-MAX(COLUMN($AG36:BJ36)*($AG36:BJ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BK36)*($AG36:BK36=1))>MAX(COLUMN($AG36:BK36)*($AG36:BK36=3)),MAX(COLUMN($AG36:BK36)*($AG36:BK36=1))>MAX(COLUMN($AG36:BK36)*($AG36:BK36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BL36)-MAX(COLUMN($AG36:BK36)*($AG36:BK36=1))=$J36,3,0),IF(COLUMN(BL36)-MAX(COLUMN($AG36:BK36)*($AG36:BK36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BK36)*($AG36:BK36=2))>MAX(COLUMN($AG36:BK36)*($AG36:BK36=3)),MAX(COLUMN($AG36:BK36)*($AG36:BK36=2))>MAX(COLUMN($AG36:BK36)*($AG36:BK36=1))),IF(COLUMN(BL36)-MAX(COLUMN($AG36:BK36)*($AG36:BK36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BL36)-MAX(COLUMN($AG36:BK36)*($AG36:BK36=3))=$J36,3,0),IF(COLUMN(BL36)-MAX(COLUMN($AG36:BK36)*($AG36:BK36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BL36)*($AG36:BL36=1))>MAX(COLUMN($AG36:BL36)*($AG36:BL36=3)),MAX(COLUMN($AG36:BL36)*($AG36:BL36=1))>MAX(COLUMN($AG36:BL36)*($AG36:BL36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BM36)-MAX(COLUMN($AG36:BL36)*($AG36:BL36=1))=$J36,3,0),IF(COLUMN(BM36)-MAX(COLUMN($AG36:BL36)*($AG36:BL36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BL36)*($AG36:BL36=2))>MAX(COLUMN($AG36:BL36)*($AG36:BL36=3)),MAX(COLUMN($AG36:BL36)*($AG36:BL36=2))>MAX(COLUMN($AG36:BL36)*($AG36:BL36=1))),IF(COLUMN(BM36)-MAX(COLUMN($AG36:BL36)*($AG36:BL36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BM36)-MAX(COLUMN($AG36:BL36)*($AG36:BL36=3))=$J36,3,0),IF(COLUMN(BM36)-MAX(COLUMN($AG36:BL36)*($AG36:BL36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BM36)*($AG36:BM36=1))>MAX(COLUMN($AG36:BM36)*($AG36:BM36=3)),MAX(COLUMN($AG36:BM36)*($AG36:BM36=1))>MAX(COLUMN($AG36:BM36)*($AG36:BM36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BN36)-MAX(COLUMN($AG36:BM36)*($AG36:BM36=1))=$J36,3,0),IF(COLUMN(BN36)-MAX(COLUMN($AG36:BM36)*($AG36:BM36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BM36)*($AG36:BM36=2))>MAX(COLUMN($AG36:BM36)*($AG36:BM36=3)),MAX(COLUMN($AG36:BM36)*($AG36:BM36=2))>MAX(COLUMN($AG36:BM36)*($AG36:BM36=1))),IF(COLUMN(BN36)-MAX(COLUMN($AG36:BM36)*($AG36:BM36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BN36)-MAX(COLUMN($AG36:BM36)*($AG36:BM36=3))=$J36,3,0),IF(COLUMN(BN36)-MAX(COLUMN($AG36:BM36)*($AG36:BM36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BN36)*($AG36:BN36=1))>MAX(COLUMN($AG36:BN36)*($AG36:BN36=3)),MAX(COLUMN($AG36:BN36)*($AG36:BN36=1))>MAX(COLUMN($AG36:BN36)*($AG36:BN36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BO36)-MAX(COLUMN($AG36:BN36)*($AG36:BN36=1))=$J36,3,0),IF(COLUMN(BO36)-MAX(COLUMN($AG36:BN36)*($AG36:BN36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BN36)*($AG36:BN36=2))>MAX(COLUMN($AG36:BN36)*($AG36:BN36=3)),MAX(COLUMN($AG36:BN36)*($AG36:BN36=2))>MAX(COLUMN($AG36:BN36)*($AG36:BN36=1))),IF(COLUMN(BO36)-MAX(COLUMN($AG36:BN36)*($AG36:BN36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BO36)-MAX(COLUMN($AG36:BN36)*($AG36:BN36=3))=$J36,3,0),IF(COLUMN(BO36)-MAX(COLUMN($AG36:BN36)*($AG36:BN36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BO36)*($AG36:BO36=1))>MAX(COLUMN($AG36:BO36)*($AG36:BO36=3)),MAX(COLUMN($AG36:BO36)*($AG36:BO36=1))>MAX(COLUMN($AG36:BO36)*($AG36:BO36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BP36)-MAX(COLUMN($AG36:BO36)*($AG36:BO36=1))=$J36,3,0),IF(COLUMN(BP36)-MAX(COLUMN($AG36:BO36)*($AG36:BO36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BO36)*($AG36:BO36=2))>MAX(COLUMN($AG36:BO36)*($AG36:BO36=3)),MAX(COLUMN($AG36:BO36)*($AG36:BO36=2))>MAX(COLUMN($AG36:BO36)*($AG36:BO36=1))),IF(COLUMN(BP36)-MAX(COLUMN($AG36:BO36)*($AG36:BO36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BP36)-MAX(COLUMN($AG36:BO36)*($AG36:BO36=3))=$J36,3,0),IF(COLUMN(BP36)-MAX(COLUMN($AG36:BO36)*($AG36:BO36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BP36)*($AG36:BP36=1))>MAX(COLUMN($AG36:BP36)*($AG36:BP36=3)),MAX(COLUMN($AG36:BP36)*($AG36:BP36=1))>MAX(COLUMN($AG36:BP36)*($AG36:BP36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BQ36)-MAX(COLUMN($AG36:BP36)*($AG36:BP36=1))=$J36,3,0),IF(COLUMN(BQ36)-MAX(COLUMN($AG36:BP36)*($AG36:BP36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BP36)*($AG36:BP36=2))>MAX(COLUMN($AG36:BP36)*($AG36:BP36=3)),MAX(COLUMN($AG36:BP36)*($AG36:BP36=2))>MAX(COLUMN($AG36:BP36)*($AG36:BP36=1))),IF(COLUMN(BQ36)-MAX(COLUMN($AG36:BP36)*($AG36:BP36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BQ36)-MAX(COLUMN($AG36:BP36)*($AG36:BP36=3))=$J36,3,0),IF(COLUMN(BQ36)-MAX(COLUMN($AG36:BP36)*($AG36:BP36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=1))>MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=3)),MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=1))>MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BR36)-MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=1))=$J36,3,0),IF(COLUMN(BR36)-MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=2))>MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=3)),MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=2))>MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=1))),IF(COLUMN(BR36)-MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BR36)-MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=3))=$J36,3,0),IF(COLUMN(BR36)-MAX(COLUMN($AG36:BQ36)*($AG36:BQ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BR36)*($AG36:BR36=1))>MAX(COLUMN($AG36:BR36)*($AG36:BR36=3)),MAX(COLUMN($AG36:BR36)*($AG36:BR36=1))>MAX(COLUMN($AG36:BR36)*($AG36:BR36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BS36)-MAX(COLUMN($AG36:BR36)*($AG36:BR36=1))=$J36,3,0),IF(COLUMN(BS36)-MAX(COLUMN($AG36:BR36)*($AG36:BR36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BR36)*($AG36:BR36=2))>MAX(COLUMN($AG36:BR36)*($AG36:BR36=3)),MAX(COLUMN($AG36:BR36)*($AG36:BR36=2))>MAX(COLUMN($AG36:BR36)*($AG36:BR36=1))),IF(COLUMN(BS36)-MAX(COLUMN($AG36:BR36)*($AG36:BR36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BS36)-MAX(COLUMN($AG36:BR36)*($AG36:BR36=3))=$J36,3,0),IF(COLUMN(BS36)-MAX(COLUMN($AG36:BR36)*($AG36:BR36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BS36)*($AG36:BS36=1))>MAX(COLUMN($AG36:BS36)*($AG36:BS36=3)),MAX(COLUMN($AG36:BS36)*($AG36:BS36=1))>MAX(COLUMN($AG36:BS36)*($AG36:BS36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BT36)-MAX(COLUMN($AG36:BS36)*($AG36:BS36=1))=$J36,3,0),IF(COLUMN(BT36)-MAX(COLUMN($AG36:BS36)*($AG36:BS36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BS36)*($AG36:BS36=2))>MAX(COLUMN($AG36:BS36)*($AG36:BS36=3)),MAX(COLUMN($AG36:BS36)*($AG36:BS36=2))>MAX(COLUMN($AG36:BS36)*($AG36:BS36=1))),IF(COLUMN(BT36)-MAX(COLUMN($AG36:BS36)*($AG36:BS36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BT36)-MAX(COLUMN($AG36:BS36)*($AG36:BS36=3))=$J36,3,0),IF(COLUMN(BT36)-MAX(COLUMN($AG36:BS36)*($AG36:BS36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BT36)*($AG36:BT36=1))>MAX(COLUMN($AG36:BT36)*($AG36:BT36=3)),MAX(COLUMN($AG36:BT36)*($AG36:BT36=1))>MAX(COLUMN($AG36:BT36)*($AG36:BT36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BU36)-MAX(COLUMN($AG36:BT36)*($AG36:BT36=1))=$J36,3,0),IF(COLUMN(BU36)-MAX(COLUMN($AG36:BT36)*($AG36:BT36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BT36)*($AG36:BT36=2))>MAX(COLUMN($AG36:BT36)*($AG36:BT36=3)),MAX(COLUMN($AG36:BT36)*($AG36:BT36=2))>MAX(COLUMN($AG36:BT36)*($AG36:BT36=1))),IF(COLUMN(BU36)-MAX(COLUMN($AG36:BT36)*($AG36:BT36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BU36)-MAX(COLUMN($AG36:BT36)*($AG36:BT36=3))=$J36,3,0),IF(COLUMN(BU36)-MAX(COLUMN($AG36:BT36)*($AG36:BT36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BU36)*($AG36:BU36=1))>MAX(COLUMN($AG36:BU36)*($AG36:BU36=3)),MAX(COLUMN($AG36:BU36)*($AG36:BU36=1))>MAX(COLUMN($AG36:BU36)*($AG36:BU36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BV36)-MAX(COLUMN($AG36:BU36)*($AG36:BU36=1))=$J36,3,0),IF(COLUMN(BV36)-MAX(COLUMN($AG36:BU36)*($AG36:BU36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BU36)*($AG36:BU36=2))>MAX(COLUMN($AG36:BU36)*($AG36:BU36=3)),MAX(COLUMN($AG36:BU36)*($AG36:BU36=2))>MAX(COLUMN($AG36:BU36)*($AG36:BU36=1))),IF(COLUMN(BV36)-MAX(COLUMN($AG36:BU36)*($AG36:BU36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BV36)-MAX(COLUMN($AG36:BU36)*($AG36:BU36=3))=$J36,3,0),IF(COLUMN(BV36)-MAX(COLUMN($AG36:BU36)*($AG36:BU36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BV36)*($AG36:BV36=1))>MAX(COLUMN($AG36:BV36)*($AG36:BV36=3)),MAX(COLUMN($AG36:BV36)*($AG36:BV36=1))>MAX(COLUMN($AG36:BV36)*($AG36:BV36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BW36)-MAX(COLUMN($AG36:BV36)*($AG36:BV36=1))=$J36,3,0),IF(COLUMN(BW36)-MAX(COLUMN($AG36:BV36)*($AG36:BV36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BV36)*($AG36:BV36=2))>MAX(COLUMN($AG36:BV36)*($AG36:BV36=3)),MAX(COLUMN($AG36:BV36)*($AG36:BV36=2))>MAX(COLUMN($AG36:BV36)*($AG36:BV36=1))),IF(COLUMN(BW36)-MAX(COLUMN($AG36:BV36)*($AG36:BV36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BW36)-MAX(COLUMN($AG36:BV36)*($AG36:BV36=3))=$J36,3,0),IF(COLUMN(BW36)-MAX(COLUMN($AG36:BV36)*($AG36:BV36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BW36)*($AG36:BW36=1))>MAX(COLUMN($AG36:BW36)*($AG36:BW36=3)),MAX(COLUMN($AG36:BW36)*($AG36:BW36=1))>MAX(COLUMN($AG36:BW36)*($AG36:BW36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BX36)-MAX(COLUMN($AG36:BW36)*($AG36:BW36=1))=$J36,3,0),IF(COLUMN(BX36)-MAX(COLUMN($AG36:BW36)*($AG36:BW36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BW36)*($AG36:BW36=2))>MAX(COLUMN($AG36:BW36)*($AG36:BW36=3)),MAX(COLUMN($AG36:BW36)*($AG36:BW36=2))>MAX(COLUMN($AG36:BW36)*($AG36:BW36=1))),IF(COLUMN(BX36)-MAX(COLUMN($AG36:BW36)*($AG36:BW36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BX36)-MAX(COLUMN($AG36:BW36)*($AG36:BW36=3))=$J36,3,0),IF(COLUMN(BX36)-MAX(COLUMN($AG36:BW36)*($AG36:BW36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BX36)*($AG36:BX36=1))>MAX(COLUMN($AG36:BX36)*($AG36:BX36=3)),MAX(COLUMN($AG36:BX36)*($AG36:BX36=1))>MAX(COLUMN($AG36:BX36)*($AG36:BX36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BY36)-MAX(COLUMN($AG36:BX36)*($AG36:BX36=1))=$J36,3,0),IF(COLUMN(BY36)-MAX(COLUMN($AG36:BX36)*($AG36:BX36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BX36)*($AG36:BX36=2))>MAX(COLUMN($AG36:BX36)*($AG36:BX36=3)),MAX(COLUMN($AG36:BX36)*($AG36:BX36=2))>MAX(COLUMN($AG36:BX36)*($AG36:BX36=1))),IF(COLUMN(BY36)-MAX(COLUMN($AG36:BX36)*($AG36:BX36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BY36)-MAX(COLUMN($AG36:BX36)*($AG36:BX36=3))=$J36,3,0),IF(COLUMN(BY36)-MAX(COLUMN($AG36:BX36)*($AG36:BX36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BY36)*($AG36:BY36=1))>MAX(COLUMN($AG36:BY36)*($AG36:BY36=3)),MAX(COLUMN($AG36:BY36)*($AG36:BY36=1))>MAX(COLUMN($AG36:BY36)*($AG36:BY36=2))),IF($K36=\"Not Possible\",IF(COLUMN(BZ36)-MAX(COLUMN($AG36:BY36)*($AG36:BY36=1))=$J36,3,0),IF(COLUMN(BZ36)-MAX(COLUMN($AG36:BY36)*($AG36:BY36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BY36)*($AG36:BY36=2))>MAX(COLUMN($AG36:BY36)*($AG36:BY36=3)),MAX(COLUMN($AG36:BY36)*($AG36:BY36=2))>MAX(COLUMN($AG36:BY36)*($AG36:BY36=1))),IF(COLUMN(BZ36)-MAX(COLUMN($AG36:BY36)*($AG36:BY36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(BZ36)-MAX(COLUMN($AG36:BY36)*($AG36:BY36=3))=$J36,3,0),IF(COLUMN(BZ36)-MAX(COLUMN($AG36:BY36)*($AG36:BY36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=1))>MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=3)),MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=1))>MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CA36)-MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=1))=$J36,3,0),IF(COLUMN(CA36)-MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=2))>MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=3)),MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=2))>MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=1))),IF(COLUMN(CA36)-MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CA36)-MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=3))=$J36,3,0),IF(COLUMN(CA36)-MAX(COLUMN($AG36:BZ36)*($AG36:BZ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CA36)*($AG36:CA36=1))>MAX(COLUMN($AG36:CA36)*($AG36:CA36=3)),MAX(COLUMN($AG36:CA36)*($AG36:CA36=1))>MAX(COLUMN($AG36:CA36)*($AG36:CA36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CB36)-MAX(COLUMN($AG36:CA36)*($AG36:CA36=1))=$J36,3,0),IF(COLUMN(CB36)-MAX(COLUMN($AG36:CA36)*($AG36:CA36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CA36)*($AG36:CA36=2))>MAX(COLUMN($AG36:CA36)*($AG36:CA36=3)),MAX(COLUMN($AG36:CA36)*($AG36:CA36=2))>MAX(COLUMN($AG36:CA36)*($AG36:CA36=1))),IF(COLUMN(CB36)-MAX(COLUMN($AG36:CA36)*($AG36:CA36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CB36)-MAX(COLUMN($AG36:CA36)*($AG36:CA36=3))=$J36,3,0),IF(COLUMN(CB36)-MAX(COLUMN($AG36:CA36)*($AG36:CA36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CB36)*($AG36:CB36=1))>MAX(COLUMN($AG36:CB36)*($AG36:CB36=3)),MAX(COLUMN($AG36:CB36)*($AG36:CB36=1))>MAX(COLUMN($AG36:CB36)*($AG36:CB36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CC36)-MAX(COLUMN($AG36:CB36)*($AG36:CB36=1))=$J36,3,0),IF(COLUMN(CC36)-MAX(COLUMN($AG36:CB36)*($AG36:CB36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CB36)*($AG36:CB36=2))>MAX(COLUMN($AG36:CB36)*($AG36:CB36=3)),MAX(COLUMN($AG36:CB36)*($AG36:CB36=2))>MAX(COLUMN($AG36:CB36)*($AG36:CB36=1))),IF(COLUMN(CC36)-MAX(COLUMN($AG36:CB36)*($AG36:CB36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CC36)-MAX(COLUMN($AG36:CB36)*($AG36:CB36=3))=$J36,3,0),IF(COLUMN(CC36)-MAX(COLUMN($AG36:CB36)*($AG36:CB36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CC36)*($AG36:CC36=1))>MAX(COLUMN($AG36:CC36)*($AG36:CC36=3)),MAX(COLUMN($AG36:CC36)*($AG36:CC36=1))>MAX(COLUMN($AG36:CC36)*($AG36:CC36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CD36)-MAX(COLUMN($AG36:CC36)*($AG36:CC36=1))=$J36,3,0),IF(COLUMN(CD36)-MAX(COLUMN($AG36:CC36)*($AG36:CC36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CC36)*($AG36:CC36=2))>MAX(COLUMN($AG36:CC36)*($AG36:CC36=3)),MAX(COLUMN($AG36:CC36)*($AG36:CC36=2))>MAX(COLUMN($AG36:CC36)*($AG36:CC36=1))),IF(COLUMN(CD36)-MAX(COLUMN($AG36:CC36)*($AG36:CC36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CD36)-MAX(COLUMN($AG36:CC36)*($AG36:CC36=3))=$J36,3,0),IF(COLUMN(CD36)-MAX(COLUMN($AG36:CC36)*($AG36:CC36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CD36)*($AG36:CD36=1))>MAX(COLUMN($AG36:CD36)*($AG36:CD36=3)),MAX(COLUMN($AG36:CD36)*($AG36:CD36=1))>MAX(COLUMN($AG36:CD36)*($AG36:CD36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CE36)-MAX(COLUMN($AG36:CD36)*($AG36:CD36=1))=$J36,3,0),IF(COLUMN(CE36)-MAX(COLUMN($AG36:CD36)*($AG36:CD36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CD36)*($AG36:CD36=2))>MAX(COLUMN($AG36:CD36)*($AG36:CD36=3)),MAX(COLUMN($AG36:CD36)*($AG36:CD36=2))>MAX(COLUMN($AG36:CD36)*($AG36:CD36=1))),IF(COLUMN(CE36)-MAX(COLUMN($AG36:CD36)*($AG36:CD36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CE36)-MAX(COLUMN($AG36:CD36)*($AG36:CD36=3))=$J36,3,0),IF(COLUMN(CE36)-MAX(COLUMN($AG36:CD36)*($AG36:CD36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CE36)*($AG36:CE36=1))>MAX(COLUMN($AG36:CE36)*($AG36:CE36=3)),MAX(COLUMN($AG36:CE36)*($AG36:CE36=1))>MAX(COLUMN($AG36:CE36)*($AG36:CE36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CF36)-MAX(COLUMN($AG36:CE36)*($AG36:CE36=1))=$J36,3,0),IF(COLUMN(CF36)-MAX(COLUMN($AG36:CE36)*($AG36:CE36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CE36)*($AG36:CE36=2))>MAX(COLUMN($AG36:CE36)*($AG36:CE36=3)),MAX(COLUMN($AG36:CE36)*($AG36:CE36=2))>MAX(COLUMN($AG36:CE36)*($AG36:CE36=1))),IF(COLUMN(CF36)-MAX(COLUMN($AG36:CE36)*($AG36:CE36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CF36)-MAX(COLUMN($AG36:CE36)*($AG36:CE36=3))=$J36,3,0),IF(COLUMN(CF36)-MAX(COLUMN($AG36:CE36)*($AG36:CE36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CF36)*($AG36:CF36=1))>MAX(COLUMN($AG36:CF36)*($AG36:CF36=3)),MAX(COLUMN($AG36:CF36)*($AG36:CF36=1))>MAX(COLUMN($AG36:CF36)*($AG36:CF36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CG36)-MAX(COLUMN($AG36:CF36)*($AG36:CF36=1))=$J36,3,0),IF(COLUMN(CG36)-MAX(COLUMN($AG36:CF36)*($AG36:CF36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CF36)*($AG36:CF36=2))>MAX(COLUMN($AG36:CF36)*($AG36:CF36=3)),MAX(COLUMN($AG36:CF36)*($AG36:CF36=2))>MAX(COLUMN($AG36:CF36)*($AG36:CF36=1))),IF(COLUMN(CG36)-MAX(COLUMN($AG36:CF36)*($AG36:CF36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CG36)-MAX(COLUMN($AG36:CF36)*($AG36:CF36=3))=$J36,3,0),IF(COLUMN(CG36)-MAX(COLUMN($AG36:CF36)*($AG36:CF36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CG36)*($AG36:CG36=1))>MAX(COLUMN($AG36:CG36)*($AG36:CG36=3)),MAX(COLUMN($AG36:CG36)*($AG36:CG36=1))>MAX(COLUMN($AG36:CG36)*($AG36:CG36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CH36)-MAX(COLUMN($AG36:CG36)*($AG36:CG36=1))=$J36,3,0),IF(COLUMN(CH36)-MAX(COLUMN($AG36:CG36)*($AG36:CG36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CG36)*($AG36:CG36=2))>MAX(COLUMN($AG36:CG36)*($AG36:CG36=3)),MAX(COLUMN($AG36:CG36)*($AG36:CG36=2))>MAX(COLUMN($AG36:CG36)*($AG36:CG36=1))),IF(COLUMN(CH36)-MAX(COLUMN($AG36:CG36)*($AG36:CG36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CH36)-MAX(COLUMN($AG36:CG36)*($AG36:CG36=3))=$J36,3,0),IF(COLUMN(CH36)-MAX(COLUMN($AG36:CG36)*($AG36:CG36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CH36)*($AG36:CH36=1))>MAX(COLUMN($AG36:CH36)*($AG36:CH36=3)),MAX(COLUMN($AG36:CH36)*($AG36:CH36=1))>MAX(COLUMN($AG36:CH36)*($AG36:CH36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CI36)-MAX(COLUMN($AG36:CH36)*($AG36:CH36=1))=$J36,3,0),IF(COLUMN(CI36)-MAX(COLUMN($AG36:CH36)*($AG36:CH36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CH36)*($AG36:CH36=2))>MAX(COLUMN($AG36:CH36)*($AG36:CH36=3)),MAX(COLUMN($AG36:CH36)*($AG36:CH36=2))>MAX(COLUMN($AG36:CH36)*($AG36:CH36=1))),IF(COLUMN(CI36)-MAX(COLUMN($AG36:CH36)*($AG36:CH36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CI36)-MAX(COLUMN($AG36:CH36)*($AG36:CH36=3))=$J36,3,0),IF(COLUMN(CI36)-MAX(COLUMN($AG36:CH36)*($AG36:CH36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CI36)*($AG36:CI36=1))>MAX(COLUMN($AG36:CI36)*($AG36:CI36=3)),MAX(COLUMN($AG36:CI36)*($AG36:CI36=1))>MAX(COLUMN($AG36:CI36)*($AG36:CI36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CJ36)-MAX(COLUMN($AG36:CI36)*($AG36:CI36=1))=$J36,3,0),IF(COLUMN(CJ36)-MAX(COLUMN($AG36:CI36)*($AG36:CI36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CI36)*($AG36:CI36=2))>MAX(COLUMN($AG36:CI36)*($AG36:CI36=3)),MAX(COLUMN($AG36:CI36)*($AG36:CI36=2))>MAX(COLUMN($AG36:CI36)*($AG36:CI36=1))),IF(COLUMN(CJ36)-MAX(COLUMN($AG36:CI36)*($AG36:CI36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CJ36)-MAX(COLUMN($AG36:CI36)*($AG36:CI36=3))=$J36,3,0),IF(COLUMN(CJ36)-MAX(COLUMN($AG36:CI36)*($AG36:CI36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=1))>MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=3)),MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=1))>MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CK36)-MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=1))=$J36,3,0),IF(COLUMN(CK36)-MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=2))>MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=3)),MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=2))>MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=1))),IF(COLUMN(CK36)-MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CK36)-MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=3))=$J36,3,0),IF(COLUMN(CK36)-MAX(COLUMN($AG36:CJ36)*($AG36:CJ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CK36)*($AG36:CK36=1))>MAX(COLUMN($AG36:CK36)*($AG36:CK36=3)),MAX(COLUMN($AG36:CK36)*($AG36:CK36=1))>MAX(COLUMN($AG36:CK36)*($AG36:CK36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CL36)-MAX(COLUMN($AG36:CK36)*($AG36:CK36=1))=$J36,3,0),IF(COLUMN(CL36)-MAX(COLUMN($AG36:CK36)*($AG36:CK36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CK36)*($AG36:CK36=2))>MAX(COLUMN($AG36:CK36)*($AG36:CK36=3)),MAX(COLUMN($AG36:CK36)*($AG36:CK36=2))>MAX(COLUMN($AG36:CK36)*($AG36:CK36=1))),IF(COLUMN(CL36)-MAX(COLUMN($AG36:CK36)*($AG36:CK36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CL36)-MAX(COLUMN($AG36:CK36)*($AG36:CK36=3))=$J36,3,0),IF(COLUMN(CL36)-MAX(COLUMN($AG36:CK36)*($AG36:CK36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CL36)*($AG36:CL36=1))>MAX(COLUMN($AG36:CL36)*($AG36:CL36=3)),MAX(COLUMN($AG36:CL36)*($AG36:CL36=1))>MAX(COLUMN($AG36:CL36)*($AG36:CL36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CM36)-MAX(COLUMN($AG36:CL36)*($AG36:CL36=1))=$J36,3,0),IF(COLUMN(CM36)-MAX(COLUMN($AG36:CL36)*($AG36:CL36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CL36)*($AG36:CL36=2))>MAX(COLUMN($AG36:CL36)*($AG36:CL36=3)),MAX(COLUMN($AG36:CL36)*($AG36:CL36=2))>MAX(COLUMN($AG36:CL36)*($AG36:CL36=1))),IF(COLUMN(CM36)-MAX(COLUMN($AG36:CL36)*($AG36:CL36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CM36)-MAX(COLUMN($AG36:CL36)*($AG36:CL36=3))=$J36,3,0),IF(COLUMN(CM36)-MAX(COLUMN($AG36:CL36)*($AG36:CL36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CM36)*($AG36:CM36=1))>MAX(COLUMN($AG36:CM36)*($AG36:CM36=3)),MAX(COLUMN($AG36:CM36)*($AG36:CM36=1))>MAX(COLUMN($AG36:CM36)*($AG36:CM36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CN36)-MAX(COLUMN($AG36:CM36)*($AG36:CM36=1))=$J36,3,0),IF(COLUMN(CN36)-MAX(COLUMN($AG36:CM36)*($AG36:CM36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CM36)*($AG36:CM36=2))>MAX(COLUMN($AG36:CM36)*($AG36:CM36=3)),MAX(COLUMN($AG36:CM36)*($AG36:CM36=2))>MAX(COLUMN($AG36:CM36)*($AG36:CM36=1))),IF(COLUMN(CN36)-MAX(COLUMN($AG36:CM36)*($AG36:CM36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CN36)-MAX(COLUMN($AG36:CM36)*($AG36:CM36=3))=$J36,3,0),IF(COLUMN(CN36)-MAX(COLUMN($AG36:CM36)*($AG36:CM36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CN36)*($AG36:CN36=1))>MAX(COLUMN($AG36:CN36)*($AG36:CN36=3)),MAX(COLUMN($AG36:CN36)*($AG36:CN36=1))>MAX(COLUMN($AG36:CN36)*($AG36:CN36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CO36)-MAX(COLUMN($AG36:CN36)*($AG36:CN36=1))=$J36,3,0),IF(COLUMN(CO36)-MAX(COLUMN($AG36:CN36)*($AG36:CN36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CN36)*($AG36:CN36=2))>MAX(COLUMN($AG36:CN36)*($AG36:CN36=3)),MAX(COLUMN($AG36:CN36)*($AG36:CN36=2))>MAX(COLUMN($AG36:CN36)*($AG36:CN36=1))),IF(COLUMN(CO36)-MAX(COLUMN($AG36:CN36)*($AG36:CN36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CO36)-MAX(COLUMN($AG36:CN36)*($AG36:CN36=3))=$J36,3,0),IF(COLUMN(CO36)-MAX(COLUMN($AG36:CN36)*($AG36:CN36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CO36)*($AG36:CO36=1))>MAX(COLUMN($AG36:CO36)*($AG36:CO36=3)),MAX(COLUMN($AG36:CO36)*($AG36:CO36=1))>MAX(COLUMN($AG36:CO36)*($AG36:CO36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CP36)-MAX(COLUMN($AG36:CO36)*($AG36:CO36=1))=$J36,3,0),IF(COLUMN(CP36)-MAX(COLUMN($AG36:CO36)*($AG36:CO36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CO36)*($AG36:CO36=2))>MAX(COLUMN($AG36:CO36)*($AG36:CO36=3)),MAX(COLUMN($AG36:CO36)*($AG36:CO36=2))>MAX(COLUMN($AG36:CO36)*($AG36:CO36=1))),IF(COLUMN(CP36)-MAX(COLUMN($AG36:CO36)*($AG36:CO36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CP36)-MAX(COLUMN($AG36:CO36)*($AG36:CO36=3))=$J36,3,0),IF(COLUMN(CP36)-MAX(COLUMN($AG36:CO36)*($AG36:CO36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CP36)*($AG36:CP36=1))>MAX(COLUMN($AG36:CP36)*($AG36:CP36=3)),MAX(COLUMN($AG36:CP36)*($AG36:CP36=1))>MAX(COLUMN($AG36:CP36)*($AG36:CP36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CQ36)-MAX(COLUMN($AG36:CP36)*($AG36:CP36=1))=$J36,3,0),IF(COLUMN(CQ36)-MAX(COLUMN($AG36:CP36)*($AG36:CP36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CP36)*($AG36:CP36=2))>MAX(COLUMN($AG36:CP36)*($AG36:CP36=3)),MAX(COLUMN($AG36:CP36)*($AG36:CP36=2))>MAX(COLUMN($AG36:CP36)*($AG36:CP36=1))),IF(COLUMN(CQ36)-MAX(COLUMN($AG36:CP36)*($AG36:CP36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CQ36)-MAX(COLUMN($AG36:CP36)*($AG36:CP36=3))=$J36,3,0),IF(COLUMN(CQ36)-MAX(COLUMN($AG36:CP36)*($AG36:CP36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=1))>MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=3)),MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=1))>MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CR36)-MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=1))=$J36,3,0),IF(COLUMN(CR36)-MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=2))>MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=3)),MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=2))>MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=1))),IF(COLUMN(CR36)-MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CR36)-MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=3))=$J36,3,0),IF(COLUMN(CR36)-MAX(COLUMN($AG36:CQ36)*($AG36:CQ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CR36)*($AG36:CR36=1))>MAX(COLUMN($AG36:CR36)*($AG36:CR36=3)),MAX(COLUMN($AG36:CR36)*($AG36:CR36=1))>MAX(COLUMN($AG36:CR36)*($AG36:CR36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CS36)-MAX(COLUMN($AG36:CR36)*($AG36:CR36=1))=$J36,3,0),IF(COLUMN(CS36)-MAX(COLUMN($AG36:CR36)*($AG36:CR36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CR36)*($AG36:CR36=2))>MAX(COLUMN($AG36:CR36)*($AG36:CR36=3)),MAX(COLUMN($AG36:CR36)*($AG36:CR36=2))>MAX(COLUMN($AG36:CR36)*($AG36:CR36=1))),IF(COLUMN(CS36)-MAX(COLUMN($AG36:CR36)*($AG36:CR36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CS36)-MAX(COLUMN($AG36:CR36)*($AG36:CR36=3))=$J36,3,0),IF(COLUMN(CS36)-MAX(COLUMN($AG36:CR36)*($AG36:CR36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CS36)*($AG36:CS36=1))>MAX(COLUMN($AG36:CS36)*($AG36:CS36=3)),MAX(COLUMN($AG36:CS36)*($AG36:CS36=1))>MAX(COLUMN($AG36:CS36)*($AG36:CS36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CT36)-MAX(COLUMN($AG36:CS36)*($AG36:CS36=1))=$J36,3,0),IF(COLUMN(CT36)-MAX(COLUMN($AG36:CS36)*($AG36:CS36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CS36)*($AG36:CS36=2))>MAX(COLUMN($AG36:CS36)*($AG36:CS36=3)),MAX(COLUMN($AG36:CS36)*($AG36:CS36=2))>MAX(COLUMN($AG36:CS36)*($AG36:CS36=1))),IF(COLUMN(CT36)-MAX(COLUMN($AG36:CS36)*($AG36:CS36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CT36)-MAX(COLUMN($AG36:CS36)*($AG36:CS36=3))=$J36,3,0),IF(COLUMN(CT36)-MAX(COLUMN($AG36:CS36)*($AG36:CS36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CT36)*($AG36:CT36=1))>MAX(COLUMN($AG36:CT36)*($AG36:CT36=3)),MAX(COLUMN($AG36:CT36)*($AG36:CT36=1))>MAX(COLUMN($AG36:CT36)*($AG36:CT36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CU36)-MAX(COLUMN($AG36:CT36)*($AG36:CT36=1))=$J36,3,0),IF(COLUMN(CU36)-MAX(COLUMN($AG36:CT36)*($AG36:CT36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CT36)*($AG36:CT36=2))>MAX(COLUMN($AG36:CT36)*($AG36:CT36=3)),MAX(COLUMN($AG36:CT36)*($AG36:CT36=2))>MAX(COLUMN($AG36:CT36)*($AG36:CT36=1))),IF(COLUMN(CU36)-MAX(COLUMN($AG36:CT36)*($AG36:CT36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CU36)-MAX(COLUMN($AG36:CT36)*($AG36:CT36=3))=$J36,3,0),IF(COLUMN(CU36)-MAX(COLUMN($AG36:CT36)*($AG36:CT36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CU36)*($AG36:CU36=1))>MAX(COLUMN($AG36:CU36)*($AG36:CU36=3)),MAX(COLUMN($AG36:CU36)*($AG36:CU36=1))>MAX(COLUMN($AG36:CU36)*($AG36:CU36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CV36)-MAX(COLUMN($AG36:CU36)*($AG36:CU36=1))=$J36,3,0),IF(COLUMN(CV36)-MAX(COLUMN($AG36:CU36)*($AG36:CU36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CU36)*($AG36:CU36=2))>MAX(COLUMN($AG36:CU36)*($AG36:CU36=3)),MAX(COLUMN($AG36:CU36)*($AG36:CU36=2))>MAX(COLUMN($AG36:CU36)*($AG36:CU36=1))),IF(COLUMN(CV36)-MAX(COLUMN($AG36:CU36)*($AG36:CU36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CV36)-MAX(COLUMN($AG36:CU36)*($AG36:CU36=3))=$J36,3,0),IF(COLUMN(CV36)-MAX(COLUMN($AG36:CU36)*($AG36:CU36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CV36)*($AG36:CV36=1))>MAX(COLUMN($AG36:CV36)*($AG36:CV36=3)),MAX(COLUMN($AG36:CV36)*($AG36:CV36=1))>MAX(COLUMN($AG36:CV36)*($AG36:CV36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CW36)-MAX(COLUMN($AG36:CV36)*($AG36:CV36=1))=$J36,3,0),IF(COLUMN(CW36)-MAX(COLUMN($AG36:CV36)*($AG36:CV36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CV36)*($AG36:CV36=2))>MAX(COLUMN($AG36:CV36)*($AG36:CV36=3)),MAX(COLUMN($AG36:CV36)*($AG36:CV36=2))>MAX(COLUMN($AG36:CV36)*($AG36:CV36=1))),IF(COLUMN(CW36)-MAX(COLUMN($AG36:CV36)*($AG36:CV36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CW36)-MAX(COLUMN($AG36:CV36)*($AG36:CV36=3))=$J36,3,0),IF(COLUMN(CW36)-MAX(COLUMN($AG36:CV36)*($AG36:CV36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CW36)*($AG36:CW36=1))>MAX(COLUMN($AG36:CW36)*($AG36:CW36=3)),MAX(COLUMN($AG36:CW36)*($AG36:CW36=1))>MAX(COLUMN($AG36:CW36)*($AG36:CW36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CX36)-MAX(COLUMN($AG36:CW36)*($AG36:CW36=1))=$J36,3,0),IF(COLUMN(CX36)-MAX(COLUMN($AG36:CW36)*($AG36:CW36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CW36)*($AG36:CW36=2))>MAX(COLUMN($AG36:CW36)*($AG36:CW36=3)),MAX(COLUMN($AG36:CW36)*($AG36:CW36=2))>MAX(COLUMN($AG36:CW36)*($AG36:CW36=1))),IF(COLUMN(CX36)-MAX(COLUMN($AG36:CW36)*($AG36:CW36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CX36)-MAX(COLUMN($AG36:CW36)*($AG36:CW36=3))=$J36,3,0),IF(COLUMN(CX36)-MAX(COLUMN($AG36:CW36)*($AG36:CW36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CX36)*($AG36:CX36=1))>MAX(COLUMN($AG36:CX36)*($AG36:CX36=3)),MAX(COLUMN($AG36:CX36)*($AG36:CX36=1))>MAX(COLUMN($AG36:CX36)*($AG36:CX36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CY36)-MAX(COLUMN($AG36:CX36)*($AG36:CX36=1))=$J36,3,0),IF(COLUMN(CY36)-MAX(COLUMN($AG36:CX36)*($AG36:CX36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CX36)*($AG36:CX36=2))>MAX(COLUMN($AG36:CX36)*($AG36:CX36=3)),MAX(COLUMN($AG36:CX36)*($AG36:CX36=2))>MAX(COLUMN($AG36:CX36)*($AG36:CX36=1))),IF(COLUMN(CY36)-MAX(COLUMN($AG36:CX36)*($AG36:CX36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CY36)-MAX(COLUMN($AG36:CX36)*($AG36:CX36=3))=$J36,3,0),IF(COLUMN(CY36)-MAX(COLUMN($AG36:CX36)*($AG36:CX36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CY36)*($AG36:CY36=1))>MAX(COLUMN($AG36:CY36)*($AG36:CY36=3)),MAX(COLUMN($AG36:CY36)*($AG36:CY36=1))>MAX(COLUMN($AG36:CY36)*($AG36:CY36=2))),IF($K36=\"Not Possible\",IF(COLUMN(CZ36)-MAX(COLUMN($AG36:CY36)*($AG36:CY36=1))=$J36,3,0),IF(COLUMN(CZ36)-MAX(COLUMN($AG36:CY36)*($AG36:CY36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CY36)*($AG36:CY36=2))>MAX(COLUMN($AG36:CY36)*($AG36:CY36=3)),MAX(COLUMN($AG36:CY36)*($AG36:CY36=2))>MAX(COLUMN($AG36:CY36)*($AG36:CY36=1))),IF(COLUMN(CZ36)-MAX(COLUMN($AG36:CY36)*($AG36:CY36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(CZ36)-MAX(COLUMN($AG36:CY36)*($AG36:CY36=3))=$J36,3,0),IF(COLUMN(CZ36)-MAX(COLUMN($AG36:CY36)*($AG36:CY36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=1))>MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=3)),MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=1))>MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DA36)-MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=1))=$J36,3,0),IF(COLUMN(DA36)-MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=2))>MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=3)),MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=2))>MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=1))),IF(COLUMN(DA36)-MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DA36)-MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=3))=$J36,3,0),IF(COLUMN(DA36)-MAX(COLUMN($AG36:CZ36)*($AG36:CZ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DA36)*($AG36:DA36=1))>MAX(COLUMN($AG36:DA36)*($AG36:DA36=3)),MAX(COLUMN($AG36:DA36)*($AG36:DA36=1))>MAX(COLUMN($AG36:DA36)*($AG36:DA36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DB36)-MAX(COLUMN($AG36:DA36)*($AG36:DA36=1))=$J36,3,0),IF(COLUMN(DB36)-MAX(COLUMN($AG36:DA36)*($AG36:DA36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DA36)*($AG36:DA36=2))>MAX(COLUMN($AG36:DA36)*($AG36:DA36=3)),MAX(COLUMN($AG36:DA36)*($AG36:DA36=2))>MAX(COLUMN($AG36:DA36)*($AG36:DA36=1))),IF(COLUMN(DB36)-MAX(COLUMN($AG36:DA36)*($AG36:DA36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DB36)-MAX(COLUMN($AG36:DA36)*($AG36:DA36=3))=$J36,3,0),IF(COLUMN(DB36)-MAX(COLUMN($AG36:DA36)*($AG36:DA36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DB36)*($AG36:DB36=1))>MAX(COLUMN($AG36:DB36)*($AG36:DB36=3)),MAX(COLUMN($AG36:DB36)*($AG36:DB36=1))>MAX(COLUMN($AG36:DB36)*($AG36:DB36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DC36)-MAX(COLUMN($AG36:DB36)*($AG36:DB36=1))=$J36,3,0),IF(COLUMN(DC36)-MAX(COLUMN($AG36:DB36)*($AG36:DB36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DB36)*($AG36:DB36=2))>MAX(COLUMN($AG36:DB36)*($AG36:DB36=3)),MAX(COLUMN($AG36:DB36)*($AG36:DB36=2))>MAX(COLUMN($AG36:DB36)*($AG36:DB36=1))),IF(COLUMN(DC36)-MAX(COLUMN($AG36:DB36)*($AG36:DB36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DC36)-MAX(COLUMN($AG36:DB36)*($AG36:DB36=3))=$J36,3,0),IF(COLUMN(DC36)-MAX(COLUMN($AG36:DB36)*($AG36:DB36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DC36)*($AG36:DC36=1))>MAX(COLUMN($AG36:DC36)*($AG36:DC36=3)),MAX(COLUMN($AG36:DC36)*($AG36:DC36=1))>MAX(COLUMN($AG36:DC36)*($AG36:DC36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DD36)-MAX(COLUMN($AG36:DC36)*($AG36:DC36=1))=$J36,3,0),IF(COLUMN(DD36)-MAX(COLUMN($AG36:DC36)*($AG36:DC36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DC36)*($AG36:DC36=2))>MAX(COLUMN($AG36:DC36)*($AG36:DC36=3)),MAX(COLUMN($AG36:DC36)*($AG36:DC36=2))>MAX(COLUMN($AG36:DC36)*($AG36:DC36=1))),IF(COLUMN(DD36)-MAX(COLUMN($AG36:DC36)*($AG36:DC36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DD36)-MAX(COLUMN($AG36:DC36)*($AG36:DC36=3))=$J36,3,0),IF(COLUMN(DD36)-MAX(COLUMN($AG36:DC36)*($AG36:DC36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DD36)*($AG36:DD36=1))>MAX(COLUMN($AG36:DD36)*($AG36:DD36=3)),MAX(COLUMN($AG36:DD36)*($AG36:DD36=1))>MAX(COLUMN($AG36:DD36)*($AG36:DD36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DE36)-MAX(COLUMN($AG36:DD36)*($AG36:DD36=1))=$J36,3,0),IF(COLUMN(DE36)-MAX(COLUMN($AG36:DD36)*($AG36:DD36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DD36)*($AG36:DD36=2))>MAX(COLUMN($AG36:DD36)*($AG36:DD36=3)),MAX(COLUMN($AG36:DD36)*($AG36:DD36=2))>MAX(COLUMN($AG36:DD36)*($AG36:DD36=1))),IF(COLUMN(DE36)-MAX(COLUMN($AG36:DD36)*($AG36:DD36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DE36)-MAX(COLUMN($AG36:DD36)*($AG36:DD36=3))=$J36,3,0),IF(COLUMN(DE36)-MAX(COLUMN($AG36:DD36)*($AG36:DD36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DE36)*($AG36:DE36=1))>MAX(COLUMN($AG36:DE36)*($AG36:DE36=3)),MAX(COLUMN($AG36:DE36)*($AG36:DE36=1))>MAX(COLUMN($AG36:DE36)*($AG36:DE36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DF36)-MAX(COLUMN($AG36:DE36)*($AG36:DE36=1))=$J36,3,0),IF(COLUMN(DF36)-MAX(COLUMN($AG36:DE36)*($AG36:DE36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DE36)*($AG36:DE36=2))>MAX(COLUMN($AG36:DE36)*($AG36:DE36=3)),MAX(COLUMN($AG36:DE36)*($AG36:DE36=2))>MAX(COLUMN($AG36:DE36)*($AG36:DE36=1))),IF(COLUMN(DF36)-MAX(COLUMN($AG36:DE36)*($AG36:DE36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DF36)-MAX(COLUMN($AG36:DE36)*($AG36:DE36=3))=$J36,3,0),IF(COLUMN(DF36)-MAX(COLUMN($AG36:DE36)*($AG36:DE36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DF36)*($AG36:DF36=1))>MAX(COLUMN($AG36:DF36)*($AG36:DF36=3)),MAX(COLUMN($AG36:DF36)*($AG36:DF36=1))>MAX(COLUMN($AG36:DF36)*($AG36:DF36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DG36)-MAX(COLUMN($AG36:DF36)*($AG36:DF36=1))=$J36,3,0),IF(COLUMN(DG36)-MAX(COLUMN($AG36:DF36)*($AG36:DF36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DF36)*($AG36:DF36=2))>MAX(COLUMN($AG36:DF36)*($AG36:DF36=3)),MAX(COLUMN($AG36:DF36)*($AG36:DF36=2))>MAX(COLUMN($AG36:DF36)*($AG36:DF36=1))),IF(COLUMN(DG36)-MAX(COLUMN($AG36:DF36)*($AG36:DF36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DG36)-MAX(COLUMN($AG36:DF36)*($AG36:DF36=3))=$J36,3,0),IF(COLUMN(DG36)-MAX(COLUMN($AG36:DF36)*($AG36:DF36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DG36)*($AG36:DG36=1))>MAX(COLUMN($AG36:DG36)*($AG36:DG36=3)),MAX(COLUMN($AG36:DG36)*($AG36:DG36=1))>MAX(COLUMN($AG36:DG36)*($AG36:DG36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DH36)-MAX(COLUMN($AG36:DG36)*($AG36:DG36=1))=$J36,3,0),IF(COLUMN(DH36)-MAX(COLUMN($AG36:DG36)*($AG36:DG36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DG36)*($AG36:DG36=2))>MAX(COLUMN($AG36:DG36)*($AG36:DG36=3)),MAX(COLUMN($AG36:DG36)*($AG36:DG36=2))>MAX(COLUMN($AG36:DG36)*($AG36:DG36=1))),IF(COLUMN(DH36)-MAX(COLUMN($AG36:DG36)*($AG36:DG36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DH36)-MAX(COLUMN($AG36:DG36)*($AG36:DG36=3))=$J36,3,0),IF(COLUMN(DH36)-MAX(COLUMN($AG36:DG36)*($AG36:DG36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DH36)*($AG36:DH36=1))>MAX(COLUMN($AG36:DH36)*($AG36:DH36=3)),MAX(COLUMN($AG36:DH36)*($AG36:DH36=1))>MAX(COLUMN($AG36:DH36)*($AG36:DH36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DI36)-MAX(COLUMN($AG36:DH36)*($AG36:DH36=1))=$J36,3,0),IF(COLUMN(DI36)-MAX(COLUMN($AG36:DH36)*($AG36:DH36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DH36)*($AG36:DH36=2))>MAX(COLUMN($AG36:DH36)*($AG36:DH36=3)),MAX(COLUMN($AG36:DH36)*($AG36:DH36=2))>MAX(COLUMN($AG36:DH36)*($AG36:DH36=1))),IF(COLUMN(DI36)-MAX(COLUMN($AG36:DH36)*($AG36:DH36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DI36)-MAX(COLUMN($AG36:DH36)*($AG36:DH36=3))=$J36,3,0),IF(COLUMN(DI36)-MAX(COLUMN($AG36:DH36)*($AG36:DH36=3))=$J36,2,0)))))","v":2},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DI36)*($AG36:DI36=1))>MAX(COLUMN($AG36:DI36)*($AG36:DI36=3)),MAX(COLUMN($AG36:DI36)*($AG36:DI36=1))>MAX(COLUMN($AG36:DI36)*($AG36:DI36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DJ36)-MAX(COLUMN($AG36:DI36)*($AG36:DI36=1))=$J36,3,0),IF(COLUMN(DJ36)-MAX(COLUMN($AG36:DI36)*($AG36:DI36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DI36)*($AG36:DI36=2))>MAX(COLUMN($AG36:DI36)*($AG36:DI36=3)),MAX(COLUMN($AG36:DI36)*($AG36:DI36=2))>MAX(COLUMN($AG36:DI36)*($AG36:DI36=1))),IF(COLUMN(DJ36)-MAX(COLUMN($AG36:DI36)*($AG36:DI36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DJ36)-MAX(COLUMN($AG36:DI36)*($AG36:DI36=3))=$J36,3,0),IF(COLUMN(DJ36)-MAX(COLUMN($AG36:DI36)*($AG36:DI36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=1))>MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=3)),MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=1))>MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DK36)-MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=1))=$J36,3,0),IF(COLUMN(DK36)-MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=2))>MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=3)),MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=2))>MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=1))),IF(COLUMN(DK36)-MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DK36)-MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=3))=$J36,3,0),IF(COLUMN(DK36)-MAX(COLUMN($AG36:DJ36)*($AG36:DJ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DK36)*($AG36:DK36=1))>MAX(COLUMN($AG36:DK36)*($AG36:DK36=3)),MAX(COLUMN($AG36:DK36)*($AG36:DK36=1))>MAX(COLUMN($AG36:DK36)*($AG36:DK36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DL36)-MAX(COLUMN($AG36:DK36)*($AG36:DK36=1))=$J36,3,0),IF(COLUMN(DL36)-MAX(COLUMN($AG36:DK36)*($AG36:DK36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DK36)*($AG36:DK36=2))>MAX(COLUMN($AG36:DK36)*($AG36:DK36=3)),MAX(COLUMN($AG36:DK36)*($AG36:DK36=2))>MAX(COLUMN($AG36:DK36)*($AG36:DK36=1))),IF(COLUMN(DL36)-MAX(COLUMN($AG36:DK36)*($AG36:DK36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DL36)-MAX(COLUMN($AG36:DK36)*($AG36:DK36=3))=$J36,3,0),IF(COLUMN(DL36)-MAX(COLUMN($AG36:DK36)*($AG36:DK36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DL36)*($AG36:DL36=1))>MAX(COLUMN($AG36:DL36)*($AG36:DL36=3)),MAX(COLUMN($AG36:DL36)*($AG36:DL36=1))>MAX(COLUMN($AG36:DL36)*($AG36:DL36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DM36)-MAX(COLUMN($AG36:DL36)*($AG36:DL36=1))=$J36,3,0),IF(COLUMN(DM36)-MAX(COLUMN($AG36:DL36)*($AG36:DL36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DL36)*($AG36:DL36=2))>MAX(COLUMN($AG36:DL36)*($AG36:DL36=3)),MAX(COLUMN($AG36:DL36)*($AG36:DL36=2))>MAX(COLUMN($AG36:DL36)*($AG36:DL36=1))),IF(COLUMN(DM36)-MAX(COLUMN($AG36:DL36)*($AG36:DL36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DM36)-MAX(COLUMN($AG36:DL36)*($AG36:DL36=3))=$J36,3,0),IF(COLUMN(DM36)-MAX(COLUMN($AG36:DL36)*($AG36:DL36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DM36)*($AG36:DM36=1))>MAX(COLUMN($AG36:DM36)*($AG36:DM36=3)),MAX(COLUMN($AG36:DM36)*($AG36:DM36=1))>MAX(COLUMN($AG36:DM36)*($AG36:DM36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DN36)-MAX(COLUMN($AG36:DM36)*($AG36:DM36=1))=$J36,3,0),IF(COLUMN(DN36)-MAX(COLUMN($AG36:DM36)*($AG36:DM36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DM36)*($AG36:DM36=2))>MAX(COLUMN($AG36:DM36)*($AG36:DM36=3)),MAX(COLUMN($AG36:DM36)*($AG36:DM36=2))>MAX(COLUMN($AG36:DM36)*($AG36:DM36=1))),IF(COLUMN(DN36)-MAX(COLUMN($AG36:DM36)*($AG36:DM36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DN36)-MAX(COLUMN($AG36:DM36)*($AG36:DM36=3))=$J36,3,0),IF(COLUMN(DN36)-MAX(COLUMN($AG36:DM36)*($AG36:DM36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DN36)*($AG36:DN36=1))>MAX(COLUMN($AG36:DN36)*($AG36:DN36=3)),MAX(COLUMN($AG36:DN36)*($AG36:DN36=1))>MAX(COLUMN($AG36:DN36)*($AG36:DN36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DO36)-MAX(COLUMN($AG36:DN36)*($AG36:DN36=1))=$J36,3,0),IF(COLUMN(DO36)-MAX(COLUMN($AG36:DN36)*($AG36:DN36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DN36)*($AG36:DN36=2))>MAX(COLUMN($AG36:DN36)*($AG36:DN36=3)),MAX(COLUMN($AG36:DN36)*($AG36:DN36=2))>MAX(COLUMN($AG36:DN36)*($AG36:DN36=1))),IF(COLUMN(DO36)-MAX(COLUMN($AG36:DN36)*($AG36:DN36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DO36)-MAX(COLUMN($AG36:DN36)*($AG36:DN36=3))=$J36,3,0),IF(COLUMN(DO36)-MAX(COLUMN($AG36:DN36)*($AG36:DN36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DO36)*($AG36:DO36=1))>MAX(COLUMN($AG36:DO36)*($AG36:DO36=3)),MAX(COLUMN($AG36:DO36)*($AG36:DO36=1))>MAX(COLUMN($AG36:DO36)*($AG36:DO36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DP36)-MAX(COLUMN($AG36:DO36)*($AG36:DO36=1))=$J36,3,0),IF(COLUMN(DP36)-MAX(COLUMN($AG36:DO36)*($AG36:DO36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DO36)*($AG36:DO36=2))>MAX(COLUMN($AG36:DO36)*($AG36:DO36=3)),MAX(COLUMN($AG36:DO36)*($AG36:DO36=2))>MAX(COLUMN($AG36:DO36)*($AG36:DO36=1))),IF(COLUMN(DP36)-MAX(COLUMN($AG36:DO36)*($AG36:DO36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DP36)-MAX(COLUMN($AG36:DO36)*($AG36:DO36=3))=$J36,3,0),IF(COLUMN(DP36)-MAX(COLUMN($AG36:DO36)*($AG36:DO36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DP36)*($AG36:DP36=1))>MAX(COLUMN($AG36:DP36)*($AG36:DP36=3)),MAX(COLUMN($AG36:DP36)*($AG36:DP36=1))>MAX(COLUMN($AG36:DP36)*($AG36:DP36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DQ36)-MAX(COLUMN($AG36:DP36)*($AG36:DP36=1))=$J36,3,0),IF(COLUMN(DQ36)-MAX(COLUMN($AG36:DP36)*($AG36:DP36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DP36)*($AG36:DP36=2))>MAX(COLUMN($AG36:DP36)*($AG36:DP36=3)),MAX(COLUMN($AG36:DP36)*($AG36:DP36=2))>MAX(COLUMN($AG36:DP36)*($AG36:DP36=1))),IF(COLUMN(DQ36)-MAX(COLUMN($AG36:DP36)*($AG36:DP36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DQ36)-MAX(COLUMN($AG36:DP36)*($AG36:DP36=3))=$J36,3,0),IF(COLUMN(DQ36)-MAX(COLUMN($AG36:DP36)*($AG36:DP36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=1))>MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=3)),MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=1))>MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DR36)-MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=1))=$J36,3,0),IF(COLUMN(DR36)-MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=2))>MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=3)),MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=2))>MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=1))),IF(COLUMN(DR36)-MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DR36)-MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=3))=$J36,3,0),IF(COLUMN(DR36)-MAX(COLUMN($AG36:DQ36)*($AG36:DQ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DR36)*($AG36:DR36=1))>MAX(COLUMN($AG36:DR36)*($AG36:DR36=3)),MAX(COLUMN($AG36:DR36)*($AG36:DR36=1))>MAX(COLUMN($AG36:DR36)*($AG36:DR36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DS36)-MAX(COLUMN($AG36:DR36)*($AG36:DR36=1))=$J36,3,0),IF(COLUMN(DS36)-MAX(COLUMN($AG36:DR36)*($AG36:DR36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DR36)*($AG36:DR36=2))>MAX(COLUMN($AG36:DR36)*($AG36:DR36=3)),MAX(COLUMN($AG36:DR36)*($AG36:DR36=2))>MAX(COLUMN($AG36:DR36)*($AG36:DR36=1))),IF(COLUMN(DS36)-MAX(COLUMN($AG36:DR36)*($AG36:DR36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DS36)-MAX(COLUMN($AG36:DR36)*($AG36:DR36=3))=$J36,3,0),IF(COLUMN(DS36)-MAX(COLUMN($AG36:DR36)*($AG36:DR36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DS36)*($AG36:DS36=1))>MAX(COLUMN($AG36:DS36)*($AG36:DS36=3)),MAX(COLUMN($AG36:DS36)*($AG36:DS36=1))>MAX(COLUMN($AG36:DS36)*($AG36:DS36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DT36)-MAX(COLUMN($AG36:DS36)*($AG36:DS36=1))=$J36,3,0),IF(COLUMN(DT36)-MAX(COLUMN($AG36:DS36)*($AG36:DS36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DS36)*($AG36:DS36=2))>MAX(COLUMN($AG36:DS36)*($AG36:DS36=3)),MAX(COLUMN($AG36:DS36)*($AG36:DS36=2))>MAX(COLUMN($AG36:DS36)*($AG36:DS36=1))),IF(COLUMN(DT36)-MAX(COLUMN($AG36:DS36)*($AG36:DS36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DT36)-MAX(COLUMN($AG36:DS36)*($AG36:DS36=3))=$J36,3,0),IF(COLUMN(DT36)-MAX(COLUMN($AG36:DS36)*($AG36:DS36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DT36)*($AG36:DT36=1))>MAX(COLUMN($AG36:DT36)*($AG36:DT36=3)),MAX(COLUMN($AG36:DT36)*($AG36:DT36=1))>MAX(COLUMN($AG36:DT36)*($AG36:DT36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DU36)-MAX(COLUMN($AG36:DT36)*($AG36:DT36=1))=$J36,3,0),IF(COLUMN(DU36)-MAX(COLUMN($AG36:DT36)*($AG36:DT36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DT36)*($AG36:DT36=2))>MAX(COLUMN($AG36:DT36)*($AG36:DT36=3)),MAX(COLUMN($AG36:DT36)*($AG36:DT36=2))>MAX(COLUMN($AG36:DT36)*($AG36:DT36=1))),IF(COLUMN(DU36)-MAX(COLUMN($AG36:DT36)*($AG36:DT36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DU36)-MAX(COLUMN($AG36:DT36)*($AG36:DT36=3))=$J36,3,0),IF(COLUMN(DU36)-MAX(COLUMN($AG36:DT36)*($AG36:DT36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DU36)*($AG36:DU36=1))>MAX(COLUMN($AG36:DU36)*($AG36:DU36=3)),MAX(COLUMN($AG36:DU36)*($AG36:DU36=1))>MAX(COLUMN($AG36:DU36)*($AG36:DU36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DV36)-MAX(COLUMN($AG36:DU36)*($AG36:DU36=1))=$J36,3,0),IF(COLUMN(DV36)-MAX(COLUMN($AG36:DU36)*($AG36:DU36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DU36)*($AG36:DU36=2))>MAX(COLUMN($AG36:DU36)*($AG36:DU36=3)),MAX(COLUMN($AG36:DU36)*($AG36:DU36=2))>MAX(COLUMN($AG36:DU36)*($AG36:DU36=1))),IF(COLUMN(DV36)-MAX(COLUMN($AG36:DU36)*($AG36:DU36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DV36)-MAX(COLUMN($AG36:DU36)*($AG36:DU36=3))=$J36,3,0),IF(COLUMN(DV36)-MAX(COLUMN($AG36:DU36)*($AG36:DU36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DV36)*($AG36:DV36=1))>MAX(COLUMN($AG36:DV36)*($AG36:DV36=3)),MAX(COLUMN($AG36:DV36)*($AG36:DV36=1))>MAX(COLUMN($AG36:DV36)*($AG36:DV36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DW36)-MAX(COLUMN($AG36:DV36)*($AG36:DV36=1))=$J36,3,0),IF(COLUMN(DW36)-MAX(COLUMN($AG36:DV36)*($AG36:DV36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DV36)*($AG36:DV36=2))>MAX(COLUMN($AG36:DV36)*($AG36:DV36=3)),MAX(COLUMN($AG36:DV36)*($AG36:DV36=2))>MAX(COLUMN($AG36:DV36)*($AG36:DV36=1))),IF(COLUMN(DW36)-MAX(COLUMN($AG36:DV36)*($AG36:DV36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DW36)-MAX(COLUMN($AG36:DV36)*($AG36:DV36=3))=$J36,3,0),IF(COLUMN(DW36)-MAX(COLUMN($AG36:DV36)*($AG36:DV36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DW36)*($AG36:DW36=1))>MAX(COLUMN($AG36:DW36)*($AG36:DW36=3)),MAX(COLUMN($AG36:DW36)*($AG36:DW36=1))>MAX(COLUMN($AG36:DW36)*($AG36:DW36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DX36)-MAX(COLUMN($AG36:DW36)*($AG36:DW36=1))=$J36,3,0),IF(COLUMN(DX36)-MAX(COLUMN($AG36:DW36)*($AG36:DW36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DW36)*($AG36:DW36=2))>MAX(COLUMN($AG36:DW36)*($AG36:DW36=3)),MAX(COLUMN($AG36:DW36)*($AG36:DW36=2))>MAX(COLUMN($AG36:DW36)*($AG36:DW36=1))),IF(COLUMN(DX36)-MAX(COLUMN($AG36:DW36)*($AG36:DW36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DX36)-MAX(COLUMN($AG36:DW36)*($AG36:DW36=3))=$J36,3,0),IF(COLUMN(DX36)-MAX(COLUMN($AG36:DW36)*($AG36:DW36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DX36)*($AG36:DX36=1))>MAX(COLUMN($AG36:DX36)*($AG36:DX36=3)),MAX(COLUMN($AG36:DX36)*($AG36:DX36=1))>MAX(COLUMN($AG36:DX36)*($AG36:DX36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DY36)-MAX(COLUMN($AG36:DX36)*($AG36:DX36=1))=$J36,3,0),IF(COLUMN(DY36)-MAX(COLUMN($AG36:DX36)*($AG36:DX36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DX36)*($AG36:DX36=2))>MAX(COLUMN($AG36:DX36)*($AG36:DX36=3)),MAX(COLUMN($AG36:DX36)*($AG36:DX36=2))>MAX(COLUMN($AG36:DX36)*($AG36:DX36=1))),IF(COLUMN(DY36)-MAX(COLUMN($AG36:DX36)*($AG36:DX36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DY36)-MAX(COLUMN($AG36:DX36)*($AG36:DX36=3))=$J36,3,0),IF(COLUMN(DY36)-MAX(COLUMN($AG36:DX36)*($AG36:DX36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DY36)*($AG36:DY36=1))>MAX(COLUMN($AG36:DY36)*($AG36:DY36=3)),MAX(COLUMN($AG36:DY36)*($AG36:DY36=1))>MAX(COLUMN($AG36:DY36)*($AG36:DY36=2))),IF($K36=\"Not Possible\",IF(COLUMN(DZ36)-MAX(COLUMN($AG36:DY36)*($AG36:DY36=1))=$J36,3,0),IF(COLUMN(DZ36)-MAX(COLUMN($AG36:DY36)*($AG36:DY36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DY36)*($AG36:DY36=2))>MAX(COLUMN($AG36:DY36)*($AG36:DY36=3)),MAX(COLUMN($AG36:DY36)*($AG36:DY36=2))>MAX(COLUMN($AG36:DY36)*($AG36:DY36=1))),IF(COLUMN(DZ36)-MAX(COLUMN($AG36:DY36)*($AG36:DY36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(DZ36)-MAX(COLUMN($AG36:DY36)*($AG36:DY36=3))=$J36,3,0),IF(COLUMN(DZ36)-MAX(COLUMN($AG36:DY36)*($AG36:DY36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=1))>MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=3)),MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=1))>MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=2))),IF($K36=\"Not Possible\",IF(COLUMN(EA36)-MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=1))=$J36,3,0),IF(COLUMN(EA36)-MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=2))>MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=3)),MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=2))>MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=1))),IF(COLUMN(EA36)-MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(EA36)-MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=3))=$J36,3,0),IF(COLUMN(EA36)-MAX(COLUMN($AG36:DZ36)*($AG36:DZ36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:EA36)*($AG36:EA36=1))>MAX(COLUMN($AG36:EA36)*($AG36:EA36=3)),MAX(COLUMN($AG36:EA36)*($AG36:EA36=1))>MAX(COLUMN($AG36:EA36)*($AG36:EA36=2))),IF($K36=\"Not Possible\",IF(COLUMN(EB36)-MAX(COLUMN($AG36:EA36)*($AG36:EA36=1))=$J36,3,0),IF(COLUMN(EB36)-MAX(COLUMN($AG36:EA36)*($AG36:EA36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:EA36)*($AG36:EA36=2))>MAX(COLUMN($AG36:EA36)*($AG36:EA36=3)),MAX(COLUMN($AG36:EA36)*($AG36:EA36=2))>MAX(COLUMN($AG36:EA36)*($AG36:EA36=1))),IF(COLUMN(EB36)-MAX(COLUMN($AG36:EA36)*($AG36:EA36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(EB36)-MAX(COLUMN($AG36:EA36)*($AG36:EA36=3))=$J36,3,0),IF(COLUMN(EB36)-MAX(COLUMN($AG36:EA36)*($AG36:EA36=3))=$J36,2,0)))))","v":0},{"$f":"IF($AG36=4,0,IF(AND(MAX(COLUMN($AG36:EB36)*($AG36:EB36=1))>MAX(COLUMN($AG36:EB36)*($AG36:EB36=3)),MAX(COLUMN($AG36:EB36)*($AG36:EB36=1))>MAX(COLUMN($AG36:EB36)*($AG36:EB36=2))),IF($K36=\"Not Possible\",IF(COLUMN(EC36)-MAX(COLUMN($AG36:EB36)*($AG36:EB36=1))=$J36,3,0),IF(COLUMN(EC36)-MAX(COLUMN($AG36:EB36)*($AG36:EB36=1))=$J36,2,0)),IF(AND(MAX(COLUMN($AG36:EB36)*($AG36:EB36=2))>MAX(COLUMN($AG36:EB36)*($AG36:EB36=3)),MAX(COLUMN($AG36:EB36)*($AG36:EB36=2))>MAX(COLUMN($AG36:EB36)*($AG36:EB36=1))),IF(COLUMN(EC36)-MAX(COLUMN($AG36:EB36)*($AG36:EB36=2))=$L36,3,0),IF($K36=\"Not Possible\",IF(COLUMN(EC36)-MAX(COLUMN($AG36:EB36)*($AG36:EB36=3))=$J36,3,0),IF(COLUMN(EC36)-MAX(COLUMN($AG36:EB36)*($AG36:EB36=3))=$J36,2,0)))))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"BridEA03"},"Footbridge",{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset class],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":"Bridge - Pedestrian"},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",Form_Asset[[#This Row],[Asset ID]]&ROW())","v":"BridEA0337"},"Erosion protection","Erosion Protection",{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",INDEX(AssetListTbl[Best Estimate Life (5)],(MATCH(Form_Asset[[#This Row],[Sub-Asset category]],AssetListTbl[Sub-Element Category],0))))","v":60},60,"Minor Refurbishment",50,"New Build",{"$f":"MAX(COLUMN($AH37:EC37)*($AH37:EC37=2))","v":93},{"$f":"MAX(COLUMN($AH37:EC37)*($AH37:EC37=3))","v":0},{"$f":"IFERROR(100-(IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Replace]])),INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Refurb]])))),0)","v":100},{"$f":"IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],3,2)","v":2},{"$f":"SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Product_Stage[CO2e (t)])","v":3.081},{"$f":"IFERROR(SUM(Form_Elements[General Item Material])*(Form_Asset[[#This Row],[Weighted Split]]/SUM(Form_Asset[Weighted Split]))+Form_Asset[[#This Row],[Weighted Split]],0)","v":3.081},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth (wtt)]))+(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Transport]))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":9.5397454300000004E-2},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Non contractor People Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Contractor people transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":1.7096151524993313E-2},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":4.5141975521151235E-4},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Site establishment])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":1.922203146638201E-2},{"$f":"IFERROR(IF($D$88=\"Summary\",((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),(SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Const_Ins_InsB[CO2e (t)]))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Other Construction Waste])*Form_Asset[[#This Row],[Weighted Split]]/(SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[[Waste Co2e ]])+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New build\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]]),IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",(SUM(Form_Asset[[#This Row],[Materials]:[Waste]])-(SUM(Form_Asset[[#This Row],[Materials Transport]],Form_Asset[[#This Row],[People Transport]]*0.5,Form_Asset[[#This Row],[Plant Transport]]*0.5))),IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]])/(SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%])),0)))","v":3.2131670570465869},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":1.9147544646851134E-4},{"$f":"IFERROR(SUMIF(Form_use_energy[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_use_energy[CO2e (t)]),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset ref.]]=\"\",0,SUMIF(Form_Asset[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Asset[New Build Co2e])*SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%]))","v":0.3213167057046587},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Dem - General Item Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Dem -Waste Co2e]),0)","v":0},{"$f":"(Form_Asset[[#This Row],[Plant use]]+Form_Asset[[#This Row],[Plant Transport]])*50%","v":2.2570987760575618E-4},{"$f":"Form_Asset[[#This Row],[People Transport]]*50%","v":8.5480757624966566E-3},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New Build\",1,IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",2,IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",3,IF(Form_Asset[[#This Row],[First intervention]]=\"Demolition\",4,\"\"))))","v":1},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AG37)*($AG37:AG37=1))>MAX(COLUMN($AG37:AG37)*($AG37:AG37=3)),MAX(COLUMN($AG37:AG37)*($AG37:AG37=1))>MAX(COLUMN($AG37:AG37)*($AG37:AG37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AH37)-MAX(COLUMN($AG37:AG37)*($AG37:AG37=1))=$J37,3,0),IF(COLUMN(AH37)-MAX(COLUMN($AG37:AG37)*($AG37:AG37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AG37)*($AG37:AG37=2))>MAX(COLUMN($AG37:AG37)*($AG37:AG37=3)),MAX(COLUMN($AG37:AG37)*($AG37:AG37=2))>MAX(COLUMN($AG37:AG37)*($AG37:AG37=1))),IF(COLUMN(AH37)-MAX(COLUMN($AG37:AG37)*($AG37:AG37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AH37)-MAX(COLUMN($AG37:AG37)*($AG37:AG37=3))=$J37,3,0),IF(COLUMN(AH37)-MAX(COLUMN($AG37:AG37)*($AG37:AG37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AH37)*($AG37:AH37=1))>MAX(COLUMN($AG37:AH37)*($AG37:AH37=3)),MAX(COLUMN($AG37:AH37)*($AG37:AH37=1))>MAX(COLUMN($AG37:AH37)*($AG37:AH37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AI37)-MAX(COLUMN($AG37:AH37)*($AG37:AH37=1))=$J37,3,0),IF(COLUMN(AI37)-MAX(COLUMN($AG37:AH37)*($AG37:AH37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AH37)*($AG37:AH37=2))>MAX(COLUMN($AG37:AH37)*($AG37:AH37=3)),MAX(COLUMN($AG37:AH37)*($AG37:AH37=2))>MAX(COLUMN($AG37:AH37)*($AG37:AH37=1))),IF(COLUMN(AI37)-MAX(COLUMN($AG37:AH37)*($AG37:AH37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AI37)-MAX(COLUMN($AG37:AH37)*($AG37:AH37=3))=$J37,3,0),IF(COLUMN(AI37)-MAX(COLUMN($AG37:AH37)*($AG37:AH37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AI37)*($AG37:AI37=1))>MAX(COLUMN($AG37:AI37)*($AG37:AI37=3)),MAX(COLUMN($AG37:AI37)*($AG37:AI37=1))>MAX(COLUMN($AG37:AI37)*($AG37:AI37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AJ37)-MAX(COLUMN($AG37:AI37)*($AG37:AI37=1))=$J37,3,0),IF(COLUMN(AJ37)-MAX(COLUMN($AG37:AI37)*($AG37:AI37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AI37)*($AG37:AI37=2))>MAX(COLUMN($AG37:AI37)*($AG37:AI37=3)),MAX(COLUMN($AG37:AI37)*($AG37:AI37=2))>MAX(COLUMN($AG37:AI37)*($AG37:AI37=1))),IF(COLUMN(AJ37)-MAX(COLUMN($AG37:AI37)*($AG37:AI37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AJ37)-MAX(COLUMN($AG37:AI37)*($AG37:AI37=3))=$J37,3,0),IF(COLUMN(AJ37)-MAX(COLUMN($AG37:AI37)*($AG37:AI37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=1))>MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=3)),MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=1))>MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AK37)-MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=1))=$J37,3,0),IF(COLUMN(AK37)-MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=2))>MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=3)),MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=2))>MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=1))),IF(COLUMN(AK37)-MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AK37)-MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=3))=$J37,3,0),IF(COLUMN(AK37)-MAX(COLUMN($AG37:AJ37)*($AG37:AJ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AK37)*($AG37:AK37=1))>MAX(COLUMN($AG37:AK37)*($AG37:AK37=3)),MAX(COLUMN($AG37:AK37)*($AG37:AK37=1))>MAX(COLUMN($AG37:AK37)*($AG37:AK37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AL37)-MAX(COLUMN($AG37:AK37)*($AG37:AK37=1))=$J37,3,0),IF(COLUMN(AL37)-MAX(COLUMN($AG37:AK37)*($AG37:AK37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AK37)*($AG37:AK37=2))>MAX(COLUMN($AG37:AK37)*($AG37:AK37=3)),MAX(COLUMN($AG37:AK37)*($AG37:AK37=2))>MAX(COLUMN($AG37:AK37)*($AG37:AK37=1))),IF(COLUMN(AL37)-MAX(COLUMN($AG37:AK37)*($AG37:AK37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AL37)-MAX(COLUMN($AG37:AK37)*($AG37:AK37=3))=$J37,3,0),IF(COLUMN(AL37)-MAX(COLUMN($AG37:AK37)*($AG37:AK37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AL37)*($AG37:AL37=1))>MAX(COLUMN($AG37:AL37)*($AG37:AL37=3)),MAX(COLUMN($AG37:AL37)*($AG37:AL37=1))>MAX(COLUMN($AG37:AL37)*($AG37:AL37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AM37)-MAX(COLUMN($AG37:AL37)*($AG37:AL37=1))=$J37,3,0),IF(COLUMN(AM37)-MAX(COLUMN($AG37:AL37)*($AG37:AL37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AL37)*($AG37:AL37=2))>MAX(COLUMN($AG37:AL37)*($AG37:AL37=3)),MAX(COLUMN($AG37:AL37)*($AG37:AL37=2))>MAX(COLUMN($AG37:AL37)*($AG37:AL37=1))),IF(COLUMN(AM37)-MAX(COLUMN($AG37:AL37)*($AG37:AL37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AM37)-MAX(COLUMN($AG37:AL37)*($AG37:AL37=3))=$J37,3,0),IF(COLUMN(AM37)-MAX(COLUMN($AG37:AL37)*($AG37:AL37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AM37)*($AG37:AM37=1))>MAX(COLUMN($AG37:AM37)*($AG37:AM37=3)),MAX(COLUMN($AG37:AM37)*($AG37:AM37=1))>MAX(COLUMN($AG37:AM37)*($AG37:AM37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AN37)-MAX(COLUMN($AG37:AM37)*($AG37:AM37=1))=$J37,3,0),IF(COLUMN(AN37)-MAX(COLUMN($AG37:AM37)*($AG37:AM37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AM37)*($AG37:AM37=2))>MAX(COLUMN($AG37:AM37)*($AG37:AM37=3)),MAX(COLUMN($AG37:AM37)*($AG37:AM37=2))>MAX(COLUMN($AG37:AM37)*($AG37:AM37=1))),IF(COLUMN(AN37)-MAX(COLUMN($AG37:AM37)*($AG37:AM37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AN37)-MAX(COLUMN($AG37:AM37)*($AG37:AM37=3))=$J37,3,0),IF(COLUMN(AN37)-MAX(COLUMN($AG37:AM37)*($AG37:AM37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AN37)*($AG37:AN37=1))>MAX(COLUMN($AG37:AN37)*($AG37:AN37=3)),MAX(COLUMN($AG37:AN37)*($AG37:AN37=1))>MAX(COLUMN($AG37:AN37)*($AG37:AN37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AO37)-MAX(COLUMN($AG37:AN37)*($AG37:AN37=1))=$J37,3,0),IF(COLUMN(AO37)-MAX(COLUMN($AG37:AN37)*($AG37:AN37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AN37)*($AG37:AN37=2))>MAX(COLUMN($AG37:AN37)*($AG37:AN37=3)),MAX(COLUMN($AG37:AN37)*($AG37:AN37=2))>MAX(COLUMN($AG37:AN37)*($AG37:AN37=1))),IF(COLUMN(AO37)-MAX(COLUMN($AG37:AN37)*($AG37:AN37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AO37)-MAX(COLUMN($AG37:AN37)*($AG37:AN37=3))=$J37,3,0),IF(COLUMN(AO37)-MAX(COLUMN($AG37:AN37)*($AG37:AN37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AO37)*($AG37:AO37=1))>MAX(COLUMN($AG37:AO37)*($AG37:AO37=3)),MAX(COLUMN($AG37:AO37)*($AG37:AO37=1))>MAX(COLUMN($AG37:AO37)*($AG37:AO37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AP37)-MAX(COLUMN($AG37:AO37)*($AG37:AO37=1))=$J37,3,0),IF(COLUMN(AP37)-MAX(COLUMN($AG37:AO37)*($AG37:AO37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AO37)*($AG37:AO37=2))>MAX(COLUMN($AG37:AO37)*($AG37:AO37=3)),MAX(COLUMN($AG37:AO37)*($AG37:AO37=2))>MAX(COLUMN($AG37:AO37)*($AG37:AO37=1))),IF(COLUMN(AP37)-MAX(COLUMN($AG37:AO37)*($AG37:AO37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AP37)-MAX(COLUMN($AG37:AO37)*($AG37:AO37=3))=$J37,3,0),IF(COLUMN(AP37)-MAX(COLUMN($AG37:AO37)*($AG37:AO37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AP37)*($AG37:AP37=1))>MAX(COLUMN($AG37:AP37)*($AG37:AP37=3)),MAX(COLUMN($AG37:AP37)*($AG37:AP37=1))>MAX(COLUMN($AG37:AP37)*($AG37:AP37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AQ37)-MAX(COLUMN($AG37:AP37)*($AG37:AP37=1))=$J37,3,0),IF(COLUMN(AQ37)-MAX(COLUMN($AG37:AP37)*($AG37:AP37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AP37)*($AG37:AP37=2))>MAX(COLUMN($AG37:AP37)*($AG37:AP37=3)),MAX(COLUMN($AG37:AP37)*($AG37:AP37=2))>MAX(COLUMN($AG37:AP37)*($AG37:AP37=1))),IF(COLUMN(AQ37)-MAX(COLUMN($AG37:AP37)*($AG37:AP37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AQ37)-MAX(COLUMN($AG37:AP37)*($AG37:AP37=3))=$J37,3,0),IF(COLUMN(AQ37)-MAX(COLUMN($AG37:AP37)*($AG37:AP37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=1))>MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=3)),MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=1))>MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AR37)-MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=1))=$J37,3,0),IF(COLUMN(AR37)-MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=2))>MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=3)),MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=2))>MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=1))),IF(COLUMN(AR37)-MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AR37)-MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=3))=$J37,3,0),IF(COLUMN(AR37)-MAX(COLUMN($AG37:AQ37)*($AG37:AQ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AR37)*($AG37:AR37=1))>MAX(COLUMN($AG37:AR37)*($AG37:AR37=3)),MAX(COLUMN($AG37:AR37)*($AG37:AR37=1))>MAX(COLUMN($AG37:AR37)*($AG37:AR37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AS37)-MAX(COLUMN($AG37:AR37)*($AG37:AR37=1))=$J37,3,0),IF(COLUMN(AS37)-MAX(COLUMN($AG37:AR37)*($AG37:AR37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AR37)*($AG37:AR37=2))>MAX(COLUMN($AG37:AR37)*($AG37:AR37=3)),MAX(COLUMN($AG37:AR37)*($AG37:AR37=2))>MAX(COLUMN($AG37:AR37)*($AG37:AR37=1))),IF(COLUMN(AS37)-MAX(COLUMN($AG37:AR37)*($AG37:AR37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AS37)-MAX(COLUMN($AG37:AR37)*($AG37:AR37=3))=$J37,3,0),IF(COLUMN(AS37)-MAX(COLUMN($AG37:AR37)*($AG37:AR37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AS37)*($AG37:AS37=1))>MAX(COLUMN($AG37:AS37)*($AG37:AS37=3)),MAX(COLUMN($AG37:AS37)*($AG37:AS37=1))>MAX(COLUMN($AG37:AS37)*($AG37:AS37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AT37)-MAX(COLUMN($AG37:AS37)*($AG37:AS37=1))=$J37,3,0),IF(COLUMN(AT37)-MAX(COLUMN($AG37:AS37)*($AG37:AS37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AS37)*($AG37:AS37=2))>MAX(COLUMN($AG37:AS37)*($AG37:AS37=3)),MAX(COLUMN($AG37:AS37)*($AG37:AS37=2))>MAX(COLUMN($AG37:AS37)*($AG37:AS37=1))),IF(COLUMN(AT37)-MAX(COLUMN($AG37:AS37)*($AG37:AS37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AT37)-MAX(COLUMN($AG37:AS37)*($AG37:AS37=3))=$J37,3,0),IF(COLUMN(AT37)-MAX(COLUMN($AG37:AS37)*($AG37:AS37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AT37)*($AG37:AT37=1))>MAX(COLUMN($AG37:AT37)*($AG37:AT37=3)),MAX(COLUMN($AG37:AT37)*($AG37:AT37=1))>MAX(COLUMN($AG37:AT37)*($AG37:AT37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AU37)-MAX(COLUMN($AG37:AT37)*($AG37:AT37=1))=$J37,3,0),IF(COLUMN(AU37)-MAX(COLUMN($AG37:AT37)*($AG37:AT37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AT37)*($AG37:AT37=2))>MAX(COLUMN($AG37:AT37)*($AG37:AT37=3)),MAX(COLUMN($AG37:AT37)*($AG37:AT37=2))>MAX(COLUMN($AG37:AT37)*($AG37:AT37=1))),IF(COLUMN(AU37)-MAX(COLUMN($AG37:AT37)*($AG37:AT37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AU37)-MAX(COLUMN($AG37:AT37)*($AG37:AT37=3))=$J37,3,0),IF(COLUMN(AU37)-MAX(COLUMN($AG37:AT37)*($AG37:AT37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AU37)*($AG37:AU37=1))>MAX(COLUMN($AG37:AU37)*($AG37:AU37=3)),MAX(COLUMN($AG37:AU37)*($AG37:AU37=1))>MAX(COLUMN($AG37:AU37)*($AG37:AU37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AV37)-MAX(COLUMN($AG37:AU37)*($AG37:AU37=1))=$J37,3,0),IF(COLUMN(AV37)-MAX(COLUMN($AG37:AU37)*($AG37:AU37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AU37)*($AG37:AU37=2))>MAX(COLUMN($AG37:AU37)*($AG37:AU37=3)),MAX(COLUMN($AG37:AU37)*($AG37:AU37=2))>MAX(COLUMN($AG37:AU37)*($AG37:AU37=1))),IF(COLUMN(AV37)-MAX(COLUMN($AG37:AU37)*($AG37:AU37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AV37)-MAX(COLUMN($AG37:AU37)*($AG37:AU37=3))=$J37,3,0),IF(COLUMN(AV37)-MAX(COLUMN($AG37:AU37)*($AG37:AU37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AV37)*($AG37:AV37=1))>MAX(COLUMN($AG37:AV37)*($AG37:AV37=3)),MAX(COLUMN($AG37:AV37)*($AG37:AV37=1))>MAX(COLUMN($AG37:AV37)*($AG37:AV37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AW37)-MAX(COLUMN($AG37:AV37)*($AG37:AV37=1))=$J37,3,0),IF(COLUMN(AW37)-MAX(COLUMN($AG37:AV37)*($AG37:AV37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AV37)*($AG37:AV37=2))>MAX(COLUMN($AG37:AV37)*($AG37:AV37=3)),MAX(COLUMN($AG37:AV37)*($AG37:AV37=2))>MAX(COLUMN($AG37:AV37)*($AG37:AV37=1))),IF(COLUMN(AW37)-MAX(COLUMN($AG37:AV37)*($AG37:AV37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AW37)-MAX(COLUMN($AG37:AV37)*($AG37:AV37=3))=$J37,3,0),IF(COLUMN(AW37)-MAX(COLUMN($AG37:AV37)*($AG37:AV37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AW37)*($AG37:AW37=1))>MAX(COLUMN($AG37:AW37)*($AG37:AW37=3)),MAX(COLUMN($AG37:AW37)*($AG37:AW37=1))>MAX(COLUMN($AG37:AW37)*($AG37:AW37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AX37)-MAX(COLUMN($AG37:AW37)*($AG37:AW37=1))=$J37,3,0),IF(COLUMN(AX37)-MAX(COLUMN($AG37:AW37)*($AG37:AW37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AW37)*($AG37:AW37=2))>MAX(COLUMN($AG37:AW37)*($AG37:AW37=3)),MAX(COLUMN($AG37:AW37)*($AG37:AW37=2))>MAX(COLUMN($AG37:AW37)*($AG37:AW37=1))),IF(COLUMN(AX37)-MAX(COLUMN($AG37:AW37)*($AG37:AW37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AX37)-MAX(COLUMN($AG37:AW37)*($AG37:AW37=3))=$J37,3,0),IF(COLUMN(AX37)-MAX(COLUMN($AG37:AW37)*($AG37:AW37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AX37)*($AG37:AX37=1))>MAX(COLUMN($AG37:AX37)*($AG37:AX37=3)),MAX(COLUMN($AG37:AX37)*($AG37:AX37=1))>MAX(COLUMN($AG37:AX37)*($AG37:AX37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AY37)-MAX(COLUMN($AG37:AX37)*($AG37:AX37=1))=$J37,3,0),IF(COLUMN(AY37)-MAX(COLUMN($AG37:AX37)*($AG37:AX37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AX37)*($AG37:AX37=2))>MAX(COLUMN($AG37:AX37)*($AG37:AX37=3)),MAX(COLUMN($AG37:AX37)*($AG37:AX37=2))>MAX(COLUMN($AG37:AX37)*($AG37:AX37=1))),IF(COLUMN(AY37)-MAX(COLUMN($AG37:AX37)*($AG37:AX37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AY37)-MAX(COLUMN($AG37:AX37)*($AG37:AX37=3))=$J37,3,0),IF(COLUMN(AY37)-MAX(COLUMN($AG37:AX37)*($AG37:AX37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AY37)*($AG37:AY37=1))>MAX(COLUMN($AG37:AY37)*($AG37:AY37=3)),MAX(COLUMN($AG37:AY37)*($AG37:AY37=1))>MAX(COLUMN($AG37:AY37)*($AG37:AY37=2))),IF($K37=\"Not Possible\",IF(COLUMN(AZ37)-MAX(COLUMN($AG37:AY37)*($AG37:AY37=1))=$J37,3,0),IF(COLUMN(AZ37)-MAX(COLUMN($AG37:AY37)*($AG37:AY37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AY37)*($AG37:AY37=2))>MAX(COLUMN($AG37:AY37)*($AG37:AY37=3)),MAX(COLUMN($AG37:AY37)*($AG37:AY37=2))>MAX(COLUMN($AG37:AY37)*($AG37:AY37=1))),IF(COLUMN(AZ37)-MAX(COLUMN($AG37:AY37)*($AG37:AY37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(AZ37)-MAX(COLUMN($AG37:AY37)*($AG37:AY37=3))=$J37,3,0),IF(COLUMN(AZ37)-MAX(COLUMN($AG37:AY37)*($AG37:AY37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=1))>MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=3)),MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=1))>MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BA37)-MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=1))=$J37,3,0),IF(COLUMN(BA37)-MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=2))>MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=3)),MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=2))>MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=1))),IF(COLUMN(BA37)-MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BA37)-MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=3))=$J37,3,0),IF(COLUMN(BA37)-MAX(COLUMN($AG37:AZ37)*($AG37:AZ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BA37)*($AG37:BA37=1))>MAX(COLUMN($AG37:BA37)*($AG37:BA37=3)),MAX(COLUMN($AG37:BA37)*($AG37:BA37=1))>MAX(COLUMN($AG37:BA37)*($AG37:BA37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BB37)-MAX(COLUMN($AG37:BA37)*($AG37:BA37=1))=$J37,3,0),IF(COLUMN(BB37)-MAX(COLUMN($AG37:BA37)*($AG37:BA37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BA37)*($AG37:BA37=2))>MAX(COLUMN($AG37:BA37)*($AG37:BA37=3)),MAX(COLUMN($AG37:BA37)*($AG37:BA37=2))>MAX(COLUMN($AG37:BA37)*($AG37:BA37=1))),IF(COLUMN(BB37)-MAX(COLUMN($AG37:BA37)*($AG37:BA37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BB37)-MAX(COLUMN($AG37:BA37)*($AG37:BA37=3))=$J37,3,0),IF(COLUMN(BB37)-MAX(COLUMN($AG37:BA37)*($AG37:BA37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BB37)*($AG37:BB37=1))>MAX(COLUMN($AG37:BB37)*($AG37:BB37=3)),MAX(COLUMN($AG37:BB37)*($AG37:BB37=1))>MAX(COLUMN($AG37:BB37)*($AG37:BB37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BC37)-MAX(COLUMN($AG37:BB37)*($AG37:BB37=1))=$J37,3,0),IF(COLUMN(BC37)-MAX(COLUMN($AG37:BB37)*($AG37:BB37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BB37)*($AG37:BB37=2))>MAX(COLUMN($AG37:BB37)*($AG37:BB37=3)),MAX(COLUMN($AG37:BB37)*($AG37:BB37=2))>MAX(COLUMN($AG37:BB37)*($AG37:BB37=1))),IF(COLUMN(BC37)-MAX(COLUMN($AG37:BB37)*($AG37:BB37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BC37)-MAX(COLUMN($AG37:BB37)*($AG37:BB37=3))=$J37,3,0),IF(COLUMN(BC37)-MAX(COLUMN($AG37:BB37)*($AG37:BB37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BC37)*($AG37:BC37=1))>MAX(COLUMN($AG37:BC37)*($AG37:BC37=3)),MAX(COLUMN($AG37:BC37)*($AG37:BC37=1))>MAX(COLUMN($AG37:BC37)*($AG37:BC37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BD37)-MAX(COLUMN($AG37:BC37)*($AG37:BC37=1))=$J37,3,0),IF(COLUMN(BD37)-MAX(COLUMN($AG37:BC37)*($AG37:BC37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BC37)*($AG37:BC37=2))>MAX(COLUMN($AG37:BC37)*($AG37:BC37=3)),MAX(COLUMN($AG37:BC37)*($AG37:BC37=2))>MAX(COLUMN($AG37:BC37)*($AG37:BC37=1))),IF(COLUMN(BD37)-MAX(COLUMN($AG37:BC37)*($AG37:BC37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BD37)-MAX(COLUMN($AG37:BC37)*($AG37:BC37=3))=$J37,3,0),IF(COLUMN(BD37)-MAX(COLUMN($AG37:BC37)*($AG37:BC37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BD37)*($AG37:BD37=1))>MAX(COLUMN($AG37:BD37)*($AG37:BD37=3)),MAX(COLUMN($AG37:BD37)*($AG37:BD37=1))>MAX(COLUMN($AG37:BD37)*($AG37:BD37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BE37)-MAX(COLUMN($AG37:BD37)*($AG37:BD37=1))=$J37,3,0),IF(COLUMN(BE37)-MAX(COLUMN($AG37:BD37)*($AG37:BD37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BD37)*($AG37:BD37=2))>MAX(COLUMN($AG37:BD37)*($AG37:BD37=3)),MAX(COLUMN($AG37:BD37)*($AG37:BD37=2))>MAX(COLUMN($AG37:BD37)*($AG37:BD37=1))),IF(COLUMN(BE37)-MAX(COLUMN($AG37:BD37)*($AG37:BD37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BE37)-MAX(COLUMN($AG37:BD37)*($AG37:BD37=3))=$J37,3,0),IF(COLUMN(BE37)-MAX(COLUMN($AG37:BD37)*($AG37:BD37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BE37)*($AG37:BE37=1))>MAX(COLUMN($AG37:BE37)*($AG37:BE37=3)),MAX(COLUMN($AG37:BE37)*($AG37:BE37=1))>MAX(COLUMN($AG37:BE37)*($AG37:BE37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BF37)-MAX(COLUMN($AG37:BE37)*($AG37:BE37=1))=$J37,3,0),IF(COLUMN(BF37)-MAX(COLUMN($AG37:BE37)*($AG37:BE37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BE37)*($AG37:BE37=2))>MAX(COLUMN($AG37:BE37)*($AG37:BE37=3)),MAX(COLUMN($AG37:BE37)*($AG37:BE37=2))>MAX(COLUMN($AG37:BE37)*($AG37:BE37=1))),IF(COLUMN(BF37)-MAX(COLUMN($AG37:BE37)*($AG37:BE37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BF37)-MAX(COLUMN($AG37:BE37)*($AG37:BE37=3))=$J37,3,0),IF(COLUMN(BF37)-MAX(COLUMN($AG37:BE37)*($AG37:BE37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BF37)*($AG37:BF37=1))>MAX(COLUMN($AG37:BF37)*($AG37:BF37=3)),MAX(COLUMN($AG37:BF37)*($AG37:BF37=1))>MAX(COLUMN($AG37:BF37)*($AG37:BF37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BG37)-MAX(COLUMN($AG37:BF37)*($AG37:BF37=1))=$J37,3,0),IF(COLUMN(BG37)-MAX(COLUMN($AG37:BF37)*($AG37:BF37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BF37)*($AG37:BF37=2))>MAX(COLUMN($AG37:BF37)*($AG37:BF37=3)),MAX(COLUMN($AG37:BF37)*($AG37:BF37=2))>MAX(COLUMN($AG37:BF37)*($AG37:BF37=1))),IF(COLUMN(BG37)-MAX(COLUMN($AG37:BF37)*($AG37:BF37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BG37)-MAX(COLUMN($AG37:BF37)*($AG37:BF37=3))=$J37,3,0),IF(COLUMN(BG37)-MAX(COLUMN($AG37:BF37)*($AG37:BF37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BG37)*($AG37:BG37=1))>MAX(COLUMN($AG37:BG37)*($AG37:BG37=3)),MAX(COLUMN($AG37:BG37)*($AG37:BG37=1))>MAX(COLUMN($AG37:BG37)*($AG37:BG37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BH37)-MAX(COLUMN($AG37:BG37)*($AG37:BG37=1))=$J37,3,0),IF(COLUMN(BH37)-MAX(COLUMN($AG37:BG37)*($AG37:BG37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BG37)*($AG37:BG37=2))>MAX(COLUMN($AG37:BG37)*($AG37:BG37=3)),MAX(COLUMN($AG37:BG37)*($AG37:BG37=2))>MAX(COLUMN($AG37:BG37)*($AG37:BG37=1))),IF(COLUMN(BH37)-MAX(COLUMN($AG37:BG37)*($AG37:BG37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BH37)-MAX(COLUMN($AG37:BG37)*($AG37:BG37=3))=$J37,3,0),IF(COLUMN(BH37)-MAX(COLUMN($AG37:BG37)*($AG37:BG37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BH37)*($AG37:BH37=1))>MAX(COLUMN($AG37:BH37)*($AG37:BH37=3)),MAX(COLUMN($AG37:BH37)*($AG37:BH37=1))>MAX(COLUMN($AG37:BH37)*($AG37:BH37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BI37)-MAX(COLUMN($AG37:BH37)*($AG37:BH37=1))=$J37,3,0),IF(COLUMN(BI37)-MAX(COLUMN($AG37:BH37)*($AG37:BH37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BH37)*($AG37:BH37=2))>MAX(COLUMN($AG37:BH37)*($AG37:BH37=3)),MAX(COLUMN($AG37:BH37)*($AG37:BH37=2))>MAX(COLUMN($AG37:BH37)*($AG37:BH37=1))),IF(COLUMN(BI37)-MAX(COLUMN($AG37:BH37)*($AG37:BH37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BI37)-MAX(COLUMN($AG37:BH37)*($AG37:BH37=3))=$J37,3,0),IF(COLUMN(BI37)-MAX(COLUMN($AG37:BH37)*($AG37:BH37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BI37)*($AG37:BI37=1))>MAX(COLUMN($AG37:BI37)*($AG37:BI37=3)),MAX(COLUMN($AG37:BI37)*($AG37:BI37=1))>MAX(COLUMN($AG37:BI37)*($AG37:BI37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BJ37)-MAX(COLUMN($AG37:BI37)*($AG37:BI37=1))=$J37,3,0),IF(COLUMN(BJ37)-MAX(COLUMN($AG37:BI37)*($AG37:BI37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BI37)*($AG37:BI37=2))>MAX(COLUMN($AG37:BI37)*($AG37:BI37=3)),MAX(COLUMN($AG37:BI37)*($AG37:BI37=2))>MAX(COLUMN($AG37:BI37)*($AG37:BI37=1))),IF(COLUMN(BJ37)-MAX(COLUMN($AG37:BI37)*($AG37:BI37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BJ37)-MAX(COLUMN($AG37:BI37)*($AG37:BI37=3))=$J37,3,0),IF(COLUMN(BJ37)-MAX(COLUMN($AG37:BI37)*($AG37:BI37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=1))>MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=3)),MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=1))>MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BK37)-MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=1))=$J37,3,0),IF(COLUMN(BK37)-MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=2))>MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=3)),MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=2))>MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=1))),IF(COLUMN(BK37)-MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BK37)-MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=3))=$J37,3,0),IF(COLUMN(BK37)-MAX(COLUMN($AG37:BJ37)*($AG37:BJ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BK37)*($AG37:BK37=1))>MAX(COLUMN($AG37:BK37)*($AG37:BK37=3)),MAX(COLUMN($AG37:BK37)*($AG37:BK37=1))>MAX(COLUMN($AG37:BK37)*($AG37:BK37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BL37)-MAX(COLUMN($AG37:BK37)*($AG37:BK37=1))=$J37,3,0),IF(COLUMN(BL37)-MAX(COLUMN($AG37:BK37)*($AG37:BK37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BK37)*($AG37:BK37=2))>MAX(COLUMN($AG37:BK37)*($AG37:BK37=3)),MAX(COLUMN($AG37:BK37)*($AG37:BK37=2))>MAX(COLUMN($AG37:BK37)*($AG37:BK37=1))),IF(COLUMN(BL37)-MAX(COLUMN($AG37:BK37)*($AG37:BK37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BL37)-MAX(COLUMN($AG37:BK37)*($AG37:BK37=3))=$J37,3,0),IF(COLUMN(BL37)-MAX(COLUMN($AG37:BK37)*($AG37:BK37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BL37)*($AG37:BL37=1))>MAX(COLUMN($AG37:BL37)*($AG37:BL37=3)),MAX(COLUMN($AG37:BL37)*($AG37:BL37=1))>MAX(COLUMN($AG37:BL37)*($AG37:BL37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BM37)-MAX(COLUMN($AG37:BL37)*($AG37:BL37=1))=$J37,3,0),IF(COLUMN(BM37)-MAX(COLUMN($AG37:BL37)*($AG37:BL37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BL37)*($AG37:BL37=2))>MAX(COLUMN($AG37:BL37)*($AG37:BL37=3)),MAX(COLUMN($AG37:BL37)*($AG37:BL37=2))>MAX(COLUMN($AG37:BL37)*($AG37:BL37=1))),IF(COLUMN(BM37)-MAX(COLUMN($AG37:BL37)*($AG37:BL37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BM37)-MAX(COLUMN($AG37:BL37)*($AG37:BL37=3))=$J37,3,0),IF(COLUMN(BM37)-MAX(COLUMN($AG37:BL37)*($AG37:BL37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BM37)*($AG37:BM37=1))>MAX(COLUMN($AG37:BM37)*($AG37:BM37=3)),MAX(COLUMN($AG37:BM37)*($AG37:BM37=1))>MAX(COLUMN($AG37:BM37)*($AG37:BM37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BN37)-MAX(COLUMN($AG37:BM37)*($AG37:BM37=1))=$J37,3,0),IF(COLUMN(BN37)-MAX(COLUMN($AG37:BM37)*($AG37:BM37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BM37)*($AG37:BM37=2))>MAX(COLUMN($AG37:BM37)*($AG37:BM37=3)),MAX(COLUMN($AG37:BM37)*($AG37:BM37=2))>MAX(COLUMN($AG37:BM37)*($AG37:BM37=1))),IF(COLUMN(BN37)-MAX(COLUMN($AG37:BM37)*($AG37:BM37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BN37)-MAX(COLUMN($AG37:BM37)*($AG37:BM37=3))=$J37,3,0),IF(COLUMN(BN37)-MAX(COLUMN($AG37:BM37)*($AG37:BM37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BN37)*($AG37:BN37=1))>MAX(COLUMN($AG37:BN37)*($AG37:BN37=3)),MAX(COLUMN($AG37:BN37)*($AG37:BN37=1))>MAX(COLUMN($AG37:BN37)*($AG37:BN37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BO37)-MAX(COLUMN($AG37:BN37)*($AG37:BN37=1))=$J37,3,0),IF(COLUMN(BO37)-MAX(COLUMN($AG37:BN37)*($AG37:BN37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BN37)*($AG37:BN37=2))>MAX(COLUMN($AG37:BN37)*($AG37:BN37=3)),MAX(COLUMN($AG37:BN37)*($AG37:BN37=2))>MAX(COLUMN($AG37:BN37)*($AG37:BN37=1))),IF(COLUMN(BO37)-MAX(COLUMN($AG37:BN37)*($AG37:BN37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BO37)-MAX(COLUMN($AG37:BN37)*($AG37:BN37=3))=$J37,3,0),IF(COLUMN(BO37)-MAX(COLUMN($AG37:BN37)*($AG37:BN37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BO37)*($AG37:BO37=1))>MAX(COLUMN($AG37:BO37)*($AG37:BO37=3)),MAX(COLUMN($AG37:BO37)*($AG37:BO37=1))>MAX(COLUMN($AG37:BO37)*($AG37:BO37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BP37)-MAX(COLUMN($AG37:BO37)*($AG37:BO37=1))=$J37,3,0),IF(COLUMN(BP37)-MAX(COLUMN($AG37:BO37)*($AG37:BO37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BO37)*($AG37:BO37=2))>MAX(COLUMN($AG37:BO37)*($AG37:BO37=3)),MAX(COLUMN($AG37:BO37)*($AG37:BO37=2))>MAX(COLUMN($AG37:BO37)*($AG37:BO37=1))),IF(COLUMN(BP37)-MAX(COLUMN($AG37:BO37)*($AG37:BO37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BP37)-MAX(COLUMN($AG37:BO37)*($AG37:BO37=3))=$J37,3,0),IF(COLUMN(BP37)-MAX(COLUMN($AG37:BO37)*($AG37:BO37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BP37)*($AG37:BP37=1))>MAX(COLUMN($AG37:BP37)*($AG37:BP37=3)),MAX(COLUMN($AG37:BP37)*($AG37:BP37=1))>MAX(COLUMN($AG37:BP37)*($AG37:BP37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BQ37)-MAX(COLUMN($AG37:BP37)*($AG37:BP37=1))=$J37,3,0),IF(COLUMN(BQ37)-MAX(COLUMN($AG37:BP37)*($AG37:BP37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BP37)*($AG37:BP37=2))>MAX(COLUMN($AG37:BP37)*($AG37:BP37=3)),MAX(COLUMN($AG37:BP37)*($AG37:BP37=2))>MAX(COLUMN($AG37:BP37)*($AG37:BP37=1))),IF(COLUMN(BQ37)-MAX(COLUMN($AG37:BP37)*($AG37:BP37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BQ37)-MAX(COLUMN($AG37:BP37)*($AG37:BP37=3))=$J37,3,0),IF(COLUMN(BQ37)-MAX(COLUMN($AG37:BP37)*($AG37:BP37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=1))>MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=3)),MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=1))>MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BR37)-MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=1))=$J37,3,0),IF(COLUMN(BR37)-MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=2))>MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=3)),MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=2))>MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=1))),IF(COLUMN(BR37)-MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BR37)-MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=3))=$J37,3,0),IF(COLUMN(BR37)-MAX(COLUMN($AG37:BQ37)*($AG37:BQ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BR37)*($AG37:BR37=1))>MAX(COLUMN($AG37:BR37)*($AG37:BR37=3)),MAX(COLUMN($AG37:BR37)*($AG37:BR37=1))>MAX(COLUMN($AG37:BR37)*($AG37:BR37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BS37)-MAX(COLUMN($AG37:BR37)*($AG37:BR37=1))=$J37,3,0),IF(COLUMN(BS37)-MAX(COLUMN($AG37:BR37)*($AG37:BR37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BR37)*($AG37:BR37=2))>MAX(COLUMN($AG37:BR37)*($AG37:BR37=3)),MAX(COLUMN($AG37:BR37)*($AG37:BR37=2))>MAX(COLUMN($AG37:BR37)*($AG37:BR37=1))),IF(COLUMN(BS37)-MAX(COLUMN($AG37:BR37)*($AG37:BR37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BS37)-MAX(COLUMN($AG37:BR37)*($AG37:BR37=3))=$J37,3,0),IF(COLUMN(BS37)-MAX(COLUMN($AG37:BR37)*($AG37:BR37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BS37)*($AG37:BS37=1))>MAX(COLUMN($AG37:BS37)*($AG37:BS37=3)),MAX(COLUMN($AG37:BS37)*($AG37:BS37=1))>MAX(COLUMN($AG37:BS37)*($AG37:BS37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BT37)-MAX(COLUMN($AG37:BS37)*($AG37:BS37=1))=$J37,3,0),IF(COLUMN(BT37)-MAX(COLUMN($AG37:BS37)*($AG37:BS37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BS37)*($AG37:BS37=2))>MAX(COLUMN($AG37:BS37)*($AG37:BS37=3)),MAX(COLUMN($AG37:BS37)*($AG37:BS37=2))>MAX(COLUMN($AG37:BS37)*($AG37:BS37=1))),IF(COLUMN(BT37)-MAX(COLUMN($AG37:BS37)*($AG37:BS37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BT37)-MAX(COLUMN($AG37:BS37)*($AG37:BS37=3))=$J37,3,0),IF(COLUMN(BT37)-MAX(COLUMN($AG37:BS37)*($AG37:BS37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BT37)*($AG37:BT37=1))>MAX(COLUMN($AG37:BT37)*($AG37:BT37=3)),MAX(COLUMN($AG37:BT37)*($AG37:BT37=1))>MAX(COLUMN($AG37:BT37)*($AG37:BT37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BU37)-MAX(COLUMN($AG37:BT37)*($AG37:BT37=1))=$J37,3,0),IF(COLUMN(BU37)-MAX(COLUMN($AG37:BT37)*($AG37:BT37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BT37)*($AG37:BT37=2))>MAX(COLUMN($AG37:BT37)*($AG37:BT37=3)),MAX(COLUMN($AG37:BT37)*($AG37:BT37=2))>MAX(COLUMN($AG37:BT37)*($AG37:BT37=1))),IF(COLUMN(BU37)-MAX(COLUMN($AG37:BT37)*($AG37:BT37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BU37)-MAX(COLUMN($AG37:BT37)*($AG37:BT37=3))=$J37,3,0),IF(COLUMN(BU37)-MAX(COLUMN($AG37:BT37)*($AG37:BT37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BU37)*($AG37:BU37=1))>MAX(COLUMN($AG37:BU37)*($AG37:BU37=3)),MAX(COLUMN($AG37:BU37)*($AG37:BU37=1))>MAX(COLUMN($AG37:BU37)*($AG37:BU37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BV37)-MAX(COLUMN($AG37:BU37)*($AG37:BU37=1))=$J37,3,0),IF(COLUMN(BV37)-MAX(COLUMN($AG37:BU37)*($AG37:BU37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BU37)*($AG37:BU37=2))>MAX(COLUMN($AG37:BU37)*($AG37:BU37=3)),MAX(COLUMN($AG37:BU37)*($AG37:BU37=2))>MAX(COLUMN($AG37:BU37)*($AG37:BU37=1))),IF(COLUMN(BV37)-MAX(COLUMN($AG37:BU37)*($AG37:BU37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BV37)-MAX(COLUMN($AG37:BU37)*($AG37:BU37=3))=$J37,3,0),IF(COLUMN(BV37)-MAX(COLUMN($AG37:BU37)*($AG37:BU37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BV37)*($AG37:BV37=1))>MAX(COLUMN($AG37:BV37)*($AG37:BV37=3)),MAX(COLUMN($AG37:BV37)*($AG37:BV37=1))>MAX(COLUMN($AG37:BV37)*($AG37:BV37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BW37)-MAX(COLUMN($AG37:BV37)*($AG37:BV37=1))=$J37,3,0),IF(COLUMN(BW37)-MAX(COLUMN($AG37:BV37)*($AG37:BV37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BV37)*($AG37:BV37=2))>MAX(COLUMN($AG37:BV37)*($AG37:BV37=3)),MAX(COLUMN($AG37:BV37)*($AG37:BV37=2))>MAX(COLUMN($AG37:BV37)*($AG37:BV37=1))),IF(COLUMN(BW37)-MAX(COLUMN($AG37:BV37)*($AG37:BV37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BW37)-MAX(COLUMN($AG37:BV37)*($AG37:BV37=3))=$J37,3,0),IF(COLUMN(BW37)-MAX(COLUMN($AG37:BV37)*($AG37:BV37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BW37)*($AG37:BW37=1))>MAX(COLUMN($AG37:BW37)*($AG37:BW37=3)),MAX(COLUMN($AG37:BW37)*($AG37:BW37=1))>MAX(COLUMN($AG37:BW37)*($AG37:BW37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BX37)-MAX(COLUMN($AG37:BW37)*($AG37:BW37=1))=$J37,3,0),IF(COLUMN(BX37)-MAX(COLUMN($AG37:BW37)*($AG37:BW37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BW37)*($AG37:BW37=2))>MAX(COLUMN($AG37:BW37)*($AG37:BW37=3)),MAX(COLUMN($AG37:BW37)*($AG37:BW37=2))>MAX(COLUMN($AG37:BW37)*($AG37:BW37=1))),IF(COLUMN(BX37)-MAX(COLUMN($AG37:BW37)*($AG37:BW37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BX37)-MAX(COLUMN($AG37:BW37)*($AG37:BW37=3))=$J37,3,0),IF(COLUMN(BX37)-MAX(COLUMN($AG37:BW37)*($AG37:BW37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BX37)*($AG37:BX37=1))>MAX(COLUMN($AG37:BX37)*($AG37:BX37=3)),MAX(COLUMN($AG37:BX37)*($AG37:BX37=1))>MAX(COLUMN($AG37:BX37)*($AG37:BX37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BY37)-MAX(COLUMN($AG37:BX37)*($AG37:BX37=1))=$J37,3,0),IF(COLUMN(BY37)-MAX(COLUMN($AG37:BX37)*($AG37:BX37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BX37)*($AG37:BX37=2))>MAX(COLUMN($AG37:BX37)*($AG37:BX37=3)),MAX(COLUMN($AG37:BX37)*($AG37:BX37=2))>MAX(COLUMN($AG37:BX37)*($AG37:BX37=1))),IF(COLUMN(BY37)-MAX(COLUMN($AG37:BX37)*($AG37:BX37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BY37)-MAX(COLUMN($AG37:BX37)*($AG37:BX37=3))=$J37,3,0),IF(COLUMN(BY37)-MAX(COLUMN($AG37:BX37)*($AG37:BX37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BY37)*($AG37:BY37=1))>MAX(COLUMN($AG37:BY37)*($AG37:BY37=3)),MAX(COLUMN($AG37:BY37)*($AG37:BY37=1))>MAX(COLUMN($AG37:BY37)*($AG37:BY37=2))),IF($K37=\"Not Possible\",IF(COLUMN(BZ37)-MAX(COLUMN($AG37:BY37)*($AG37:BY37=1))=$J37,3,0),IF(COLUMN(BZ37)-MAX(COLUMN($AG37:BY37)*($AG37:BY37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BY37)*($AG37:BY37=2))>MAX(COLUMN($AG37:BY37)*($AG37:BY37=3)),MAX(COLUMN($AG37:BY37)*($AG37:BY37=2))>MAX(COLUMN($AG37:BY37)*($AG37:BY37=1))),IF(COLUMN(BZ37)-MAX(COLUMN($AG37:BY37)*($AG37:BY37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(BZ37)-MAX(COLUMN($AG37:BY37)*($AG37:BY37=3))=$J37,3,0),IF(COLUMN(BZ37)-MAX(COLUMN($AG37:BY37)*($AG37:BY37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=1))>MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=3)),MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=1))>MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CA37)-MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=1))=$J37,3,0),IF(COLUMN(CA37)-MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=2))>MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=3)),MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=2))>MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=1))),IF(COLUMN(CA37)-MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CA37)-MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=3))=$J37,3,0),IF(COLUMN(CA37)-MAX(COLUMN($AG37:BZ37)*($AG37:BZ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CA37)*($AG37:CA37=1))>MAX(COLUMN($AG37:CA37)*($AG37:CA37=3)),MAX(COLUMN($AG37:CA37)*($AG37:CA37=1))>MAX(COLUMN($AG37:CA37)*($AG37:CA37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CB37)-MAX(COLUMN($AG37:CA37)*($AG37:CA37=1))=$J37,3,0),IF(COLUMN(CB37)-MAX(COLUMN($AG37:CA37)*($AG37:CA37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CA37)*($AG37:CA37=2))>MAX(COLUMN($AG37:CA37)*($AG37:CA37=3)),MAX(COLUMN($AG37:CA37)*($AG37:CA37=2))>MAX(COLUMN($AG37:CA37)*($AG37:CA37=1))),IF(COLUMN(CB37)-MAX(COLUMN($AG37:CA37)*($AG37:CA37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CB37)-MAX(COLUMN($AG37:CA37)*($AG37:CA37=3))=$J37,3,0),IF(COLUMN(CB37)-MAX(COLUMN($AG37:CA37)*($AG37:CA37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CB37)*($AG37:CB37=1))>MAX(COLUMN($AG37:CB37)*($AG37:CB37=3)),MAX(COLUMN($AG37:CB37)*($AG37:CB37=1))>MAX(COLUMN($AG37:CB37)*($AG37:CB37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CC37)-MAX(COLUMN($AG37:CB37)*($AG37:CB37=1))=$J37,3,0),IF(COLUMN(CC37)-MAX(COLUMN($AG37:CB37)*($AG37:CB37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CB37)*($AG37:CB37=2))>MAX(COLUMN($AG37:CB37)*($AG37:CB37=3)),MAX(COLUMN($AG37:CB37)*($AG37:CB37=2))>MAX(COLUMN($AG37:CB37)*($AG37:CB37=1))),IF(COLUMN(CC37)-MAX(COLUMN($AG37:CB37)*($AG37:CB37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CC37)-MAX(COLUMN($AG37:CB37)*($AG37:CB37=3))=$J37,3,0),IF(COLUMN(CC37)-MAX(COLUMN($AG37:CB37)*($AG37:CB37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CC37)*($AG37:CC37=1))>MAX(COLUMN($AG37:CC37)*($AG37:CC37=3)),MAX(COLUMN($AG37:CC37)*($AG37:CC37=1))>MAX(COLUMN($AG37:CC37)*($AG37:CC37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CD37)-MAX(COLUMN($AG37:CC37)*($AG37:CC37=1))=$J37,3,0),IF(COLUMN(CD37)-MAX(COLUMN($AG37:CC37)*($AG37:CC37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CC37)*($AG37:CC37=2))>MAX(COLUMN($AG37:CC37)*($AG37:CC37=3)),MAX(COLUMN($AG37:CC37)*($AG37:CC37=2))>MAX(COLUMN($AG37:CC37)*($AG37:CC37=1))),IF(COLUMN(CD37)-MAX(COLUMN($AG37:CC37)*($AG37:CC37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CD37)-MAX(COLUMN($AG37:CC37)*($AG37:CC37=3))=$J37,3,0),IF(COLUMN(CD37)-MAX(COLUMN($AG37:CC37)*($AG37:CC37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CD37)*($AG37:CD37=1))>MAX(COLUMN($AG37:CD37)*($AG37:CD37=3)),MAX(COLUMN($AG37:CD37)*($AG37:CD37=1))>MAX(COLUMN($AG37:CD37)*($AG37:CD37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CE37)-MAX(COLUMN($AG37:CD37)*($AG37:CD37=1))=$J37,3,0),IF(COLUMN(CE37)-MAX(COLUMN($AG37:CD37)*($AG37:CD37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CD37)*($AG37:CD37=2))>MAX(COLUMN($AG37:CD37)*($AG37:CD37=3)),MAX(COLUMN($AG37:CD37)*($AG37:CD37=2))>MAX(COLUMN($AG37:CD37)*($AG37:CD37=1))),IF(COLUMN(CE37)-MAX(COLUMN($AG37:CD37)*($AG37:CD37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CE37)-MAX(COLUMN($AG37:CD37)*($AG37:CD37=3))=$J37,3,0),IF(COLUMN(CE37)-MAX(COLUMN($AG37:CD37)*($AG37:CD37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CE37)*($AG37:CE37=1))>MAX(COLUMN($AG37:CE37)*($AG37:CE37=3)),MAX(COLUMN($AG37:CE37)*($AG37:CE37=1))>MAX(COLUMN($AG37:CE37)*($AG37:CE37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CF37)-MAX(COLUMN($AG37:CE37)*($AG37:CE37=1))=$J37,3,0),IF(COLUMN(CF37)-MAX(COLUMN($AG37:CE37)*($AG37:CE37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CE37)*($AG37:CE37=2))>MAX(COLUMN($AG37:CE37)*($AG37:CE37=3)),MAX(COLUMN($AG37:CE37)*($AG37:CE37=2))>MAX(COLUMN($AG37:CE37)*($AG37:CE37=1))),IF(COLUMN(CF37)-MAX(COLUMN($AG37:CE37)*($AG37:CE37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CF37)-MAX(COLUMN($AG37:CE37)*($AG37:CE37=3))=$J37,3,0),IF(COLUMN(CF37)-MAX(COLUMN($AG37:CE37)*($AG37:CE37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CF37)*($AG37:CF37=1))>MAX(COLUMN($AG37:CF37)*($AG37:CF37=3)),MAX(COLUMN($AG37:CF37)*($AG37:CF37=1))>MAX(COLUMN($AG37:CF37)*($AG37:CF37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CG37)-MAX(COLUMN($AG37:CF37)*($AG37:CF37=1))=$J37,3,0),IF(COLUMN(CG37)-MAX(COLUMN($AG37:CF37)*($AG37:CF37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CF37)*($AG37:CF37=2))>MAX(COLUMN($AG37:CF37)*($AG37:CF37=3)),MAX(COLUMN($AG37:CF37)*($AG37:CF37=2))>MAX(COLUMN($AG37:CF37)*($AG37:CF37=1))),IF(COLUMN(CG37)-MAX(COLUMN($AG37:CF37)*($AG37:CF37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CG37)-MAX(COLUMN($AG37:CF37)*($AG37:CF37=3))=$J37,3,0),IF(COLUMN(CG37)-MAX(COLUMN($AG37:CF37)*($AG37:CF37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CG37)*($AG37:CG37=1))>MAX(COLUMN($AG37:CG37)*($AG37:CG37=3)),MAX(COLUMN($AG37:CG37)*($AG37:CG37=1))>MAX(COLUMN($AG37:CG37)*($AG37:CG37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CH37)-MAX(COLUMN($AG37:CG37)*($AG37:CG37=1))=$J37,3,0),IF(COLUMN(CH37)-MAX(COLUMN($AG37:CG37)*($AG37:CG37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CG37)*($AG37:CG37=2))>MAX(COLUMN($AG37:CG37)*($AG37:CG37=3)),MAX(COLUMN($AG37:CG37)*($AG37:CG37=2))>MAX(COLUMN($AG37:CG37)*($AG37:CG37=1))),IF(COLUMN(CH37)-MAX(COLUMN($AG37:CG37)*($AG37:CG37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CH37)-MAX(COLUMN($AG37:CG37)*($AG37:CG37=3))=$J37,3,0),IF(COLUMN(CH37)-MAX(COLUMN($AG37:CG37)*($AG37:CG37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CH37)*($AG37:CH37=1))>MAX(COLUMN($AG37:CH37)*($AG37:CH37=3)),MAX(COLUMN($AG37:CH37)*($AG37:CH37=1))>MAX(COLUMN($AG37:CH37)*($AG37:CH37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CI37)-MAX(COLUMN($AG37:CH37)*($AG37:CH37=1))=$J37,3,0),IF(COLUMN(CI37)-MAX(COLUMN($AG37:CH37)*($AG37:CH37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CH37)*($AG37:CH37=2))>MAX(COLUMN($AG37:CH37)*($AG37:CH37=3)),MAX(COLUMN($AG37:CH37)*($AG37:CH37=2))>MAX(COLUMN($AG37:CH37)*($AG37:CH37=1))),IF(COLUMN(CI37)-MAX(COLUMN($AG37:CH37)*($AG37:CH37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CI37)-MAX(COLUMN($AG37:CH37)*($AG37:CH37=3))=$J37,3,0),IF(COLUMN(CI37)-MAX(COLUMN($AG37:CH37)*($AG37:CH37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CI37)*($AG37:CI37=1))>MAX(COLUMN($AG37:CI37)*($AG37:CI37=3)),MAX(COLUMN($AG37:CI37)*($AG37:CI37=1))>MAX(COLUMN($AG37:CI37)*($AG37:CI37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CJ37)-MAX(COLUMN($AG37:CI37)*($AG37:CI37=1))=$J37,3,0),IF(COLUMN(CJ37)-MAX(COLUMN($AG37:CI37)*($AG37:CI37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CI37)*($AG37:CI37=2))>MAX(COLUMN($AG37:CI37)*($AG37:CI37=3)),MAX(COLUMN($AG37:CI37)*($AG37:CI37=2))>MAX(COLUMN($AG37:CI37)*($AG37:CI37=1))),IF(COLUMN(CJ37)-MAX(COLUMN($AG37:CI37)*($AG37:CI37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CJ37)-MAX(COLUMN($AG37:CI37)*($AG37:CI37=3))=$J37,3,0),IF(COLUMN(CJ37)-MAX(COLUMN($AG37:CI37)*($AG37:CI37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=1))>MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=3)),MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=1))>MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CK37)-MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=1))=$J37,3,0),IF(COLUMN(CK37)-MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=2))>MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=3)),MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=2))>MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=1))),IF(COLUMN(CK37)-MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CK37)-MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=3))=$J37,3,0),IF(COLUMN(CK37)-MAX(COLUMN($AG37:CJ37)*($AG37:CJ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CK37)*($AG37:CK37=1))>MAX(COLUMN($AG37:CK37)*($AG37:CK37=3)),MAX(COLUMN($AG37:CK37)*($AG37:CK37=1))>MAX(COLUMN($AG37:CK37)*($AG37:CK37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CL37)-MAX(COLUMN($AG37:CK37)*($AG37:CK37=1))=$J37,3,0),IF(COLUMN(CL37)-MAX(COLUMN($AG37:CK37)*($AG37:CK37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CK37)*($AG37:CK37=2))>MAX(COLUMN($AG37:CK37)*($AG37:CK37=3)),MAX(COLUMN($AG37:CK37)*($AG37:CK37=2))>MAX(COLUMN($AG37:CK37)*($AG37:CK37=1))),IF(COLUMN(CL37)-MAX(COLUMN($AG37:CK37)*($AG37:CK37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CL37)-MAX(COLUMN($AG37:CK37)*($AG37:CK37=3))=$J37,3,0),IF(COLUMN(CL37)-MAX(COLUMN($AG37:CK37)*($AG37:CK37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CL37)*($AG37:CL37=1))>MAX(COLUMN($AG37:CL37)*($AG37:CL37=3)),MAX(COLUMN($AG37:CL37)*($AG37:CL37=1))>MAX(COLUMN($AG37:CL37)*($AG37:CL37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CM37)-MAX(COLUMN($AG37:CL37)*($AG37:CL37=1))=$J37,3,0),IF(COLUMN(CM37)-MAX(COLUMN($AG37:CL37)*($AG37:CL37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CL37)*($AG37:CL37=2))>MAX(COLUMN($AG37:CL37)*($AG37:CL37=3)),MAX(COLUMN($AG37:CL37)*($AG37:CL37=2))>MAX(COLUMN($AG37:CL37)*($AG37:CL37=1))),IF(COLUMN(CM37)-MAX(COLUMN($AG37:CL37)*($AG37:CL37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CM37)-MAX(COLUMN($AG37:CL37)*($AG37:CL37=3))=$J37,3,0),IF(COLUMN(CM37)-MAX(COLUMN($AG37:CL37)*($AG37:CL37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CM37)*($AG37:CM37=1))>MAX(COLUMN($AG37:CM37)*($AG37:CM37=3)),MAX(COLUMN($AG37:CM37)*($AG37:CM37=1))>MAX(COLUMN($AG37:CM37)*($AG37:CM37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CN37)-MAX(COLUMN($AG37:CM37)*($AG37:CM37=1))=$J37,3,0),IF(COLUMN(CN37)-MAX(COLUMN($AG37:CM37)*($AG37:CM37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CM37)*($AG37:CM37=2))>MAX(COLUMN($AG37:CM37)*($AG37:CM37=3)),MAX(COLUMN($AG37:CM37)*($AG37:CM37=2))>MAX(COLUMN($AG37:CM37)*($AG37:CM37=1))),IF(COLUMN(CN37)-MAX(COLUMN($AG37:CM37)*($AG37:CM37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CN37)-MAX(COLUMN($AG37:CM37)*($AG37:CM37=3))=$J37,3,0),IF(COLUMN(CN37)-MAX(COLUMN($AG37:CM37)*($AG37:CM37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CN37)*($AG37:CN37=1))>MAX(COLUMN($AG37:CN37)*($AG37:CN37=3)),MAX(COLUMN($AG37:CN37)*($AG37:CN37=1))>MAX(COLUMN($AG37:CN37)*($AG37:CN37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CO37)-MAX(COLUMN($AG37:CN37)*($AG37:CN37=1))=$J37,3,0),IF(COLUMN(CO37)-MAX(COLUMN($AG37:CN37)*($AG37:CN37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CN37)*($AG37:CN37=2))>MAX(COLUMN($AG37:CN37)*($AG37:CN37=3)),MAX(COLUMN($AG37:CN37)*($AG37:CN37=2))>MAX(COLUMN($AG37:CN37)*($AG37:CN37=1))),IF(COLUMN(CO37)-MAX(COLUMN($AG37:CN37)*($AG37:CN37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CO37)-MAX(COLUMN($AG37:CN37)*($AG37:CN37=3))=$J37,3,0),IF(COLUMN(CO37)-MAX(COLUMN($AG37:CN37)*($AG37:CN37=3))=$J37,2,0)))))","v":2},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CO37)*($AG37:CO37=1))>MAX(COLUMN($AG37:CO37)*($AG37:CO37=3)),MAX(COLUMN($AG37:CO37)*($AG37:CO37=1))>MAX(COLUMN($AG37:CO37)*($AG37:CO37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CP37)-MAX(COLUMN($AG37:CO37)*($AG37:CO37=1))=$J37,3,0),IF(COLUMN(CP37)-MAX(COLUMN($AG37:CO37)*($AG37:CO37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CO37)*($AG37:CO37=2))>MAX(COLUMN($AG37:CO37)*($AG37:CO37=3)),MAX(COLUMN($AG37:CO37)*($AG37:CO37=2))>MAX(COLUMN($AG37:CO37)*($AG37:CO37=1))),IF(COLUMN(CP37)-MAX(COLUMN($AG37:CO37)*($AG37:CO37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CP37)-MAX(COLUMN($AG37:CO37)*($AG37:CO37=3))=$J37,3,0),IF(COLUMN(CP37)-MAX(COLUMN($AG37:CO37)*($AG37:CO37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CP37)*($AG37:CP37=1))>MAX(COLUMN($AG37:CP37)*($AG37:CP37=3)),MAX(COLUMN($AG37:CP37)*($AG37:CP37=1))>MAX(COLUMN($AG37:CP37)*($AG37:CP37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CQ37)-MAX(COLUMN($AG37:CP37)*($AG37:CP37=1))=$J37,3,0),IF(COLUMN(CQ37)-MAX(COLUMN($AG37:CP37)*($AG37:CP37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CP37)*($AG37:CP37=2))>MAX(COLUMN($AG37:CP37)*($AG37:CP37=3)),MAX(COLUMN($AG37:CP37)*($AG37:CP37=2))>MAX(COLUMN($AG37:CP37)*($AG37:CP37=1))),IF(COLUMN(CQ37)-MAX(COLUMN($AG37:CP37)*($AG37:CP37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CQ37)-MAX(COLUMN($AG37:CP37)*($AG37:CP37=3))=$J37,3,0),IF(COLUMN(CQ37)-MAX(COLUMN($AG37:CP37)*($AG37:CP37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=1))>MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=3)),MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=1))>MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CR37)-MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=1))=$J37,3,0),IF(COLUMN(CR37)-MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=2))>MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=3)),MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=2))>MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=1))),IF(COLUMN(CR37)-MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CR37)-MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=3))=$J37,3,0),IF(COLUMN(CR37)-MAX(COLUMN($AG37:CQ37)*($AG37:CQ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CR37)*($AG37:CR37=1))>MAX(COLUMN($AG37:CR37)*($AG37:CR37=3)),MAX(COLUMN($AG37:CR37)*($AG37:CR37=1))>MAX(COLUMN($AG37:CR37)*($AG37:CR37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CS37)-MAX(COLUMN($AG37:CR37)*($AG37:CR37=1))=$J37,3,0),IF(COLUMN(CS37)-MAX(COLUMN($AG37:CR37)*($AG37:CR37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CR37)*($AG37:CR37=2))>MAX(COLUMN($AG37:CR37)*($AG37:CR37=3)),MAX(COLUMN($AG37:CR37)*($AG37:CR37=2))>MAX(COLUMN($AG37:CR37)*($AG37:CR37=1))),IF(COLUMN(CS37)-MAX(COLUMN($AG37:CR37)*($AG37:CR37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CS37)-MAX(COLUMN($AG37:CR37)*($AG37:CR37=3))=$J37,3,0),IF(COLUMN(CS37)-MAX(COLUMN($AG37:CR37)*($AG37:CR37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CS37)*($AG37:CS37=1))>MAX(COLUMN($AG37:CS37)*($AG37:CS37=3)),MAX(COLUMN($AG37:CS37)*($AG37:CS37=1))>MAX(COLUMN($AG37:CS37)*($AG37:CS37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CT37)-MAX(COLUMN($AG37:CS37)*($AG37:CS37=1))=$J37,3,0),IF(COLUMN(CT37)-MAX(COLUMN($AG37:CS37)*($AG37:CS37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CS37)*($AG37:CS37=2))>MAX(COLUMN($AG37:CS37)*($AG37:CS37=3)),MAX(COLUMN($AG37:CS37)*($AG37:CS37=2))>MAX(COLUMN($AG37:CS37)*($AG37:CS37=1))),IF(COLUMN(CT37)-MAX(COLUMN($AG37:CS37)*($AG37:CS37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CT37)-MAX(COLUMN($AG37:CS37)*($AG37:CS37=3))=$J37,3,0),IF(COLUMN(CT37)-MAX(COLUMN($AG37:CS37)*($AG37:CS37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CT37)*($AG37:CT37=1))>MAX(COLUMN($AG37:CT37)*($AG37:CT37=3)),MAX(COLUMN($AG37:CT37)*($AG37:CT37=1))>MAX(COLUMN($AG37:CT37)*($AG37:CT37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CU37)-MAX(COLUMN($AG37:CT37)*($AG37:CT37=1))=$J37,3,0),IF(COLUMN(CU37)-MAX(COLUMN($AG37:CT37)*($AG37:CT37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CT37)*($AG37:CT37=2))>MAX(COLUMN($AG37:CT37)*($AG37:CT37=3)),MAX(COLUMN($AG37:CT37)*($AG37:CT37=2))>MAX(COLUMN($AG37:CT37)*($AG37:CT37=1))),IF(COLUMN(CU37)-MAX(COLUMN($AG37:CT37)*($AG37:CT37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CU37)-MAX(COLUMN($AG37:CT37)*($AG37:CT37=3))=$J37,3,0),IF(COLUMN(CU37)-MAX(COLUMN($AG37:CT37)*($AG37:CT37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CU37)*($AG37:CU37=1))>MAX(COLUMN($AG37:CU37)*($AG37:CU37=3)),MAX(COLUMN($AG37:CU37)*($AG37:CU37=1))>MAX(COLUMN($AG37:CU37)*($AG37:CU37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CV37)-MAX(COLUMN($AG37:CU37)*($AG37:CU37=1))=$J37,3,0),IF(COLUMN(CV37)-MAX(COLUMN($AG37:CU37)*($AG37:CU37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CU37)*($AG37:CU37=2))>MAX(COLUMN($AG37:CU37)*($AG37:CU37=3)),MAX(COLUMN($AG37:CU37)*($AG37:CU37=2))>MAX(COLUMN($AG37:CU37)*($AG37:CU37=1))),IF(COLUMN(CV37)-MAX(COLUMN($AG37:CU37)*($AG37:CU37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CV37)-MAX(COLUMN($AG37:CU37)*($AG37:CU37=3))=$J37,3,0),IF(COLUMN(CV37)-MAX(COLUMN($AG37:CU37)*($AG37:CU37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CV37)*($AG37:CV37=1))>MAX(COLUMN($AG37:CV37)*($AG37:CV37=3)),MAX(COLUMN($AG37:CV37)*($AG37:CV37=1))>MAX(COLUMN($AG37:CV37)*($AG37:CV37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CW37)-MAX(COLUMN($AG37:CV37)*($AG37:CV37=1))=$J37,3,0),IF(COLUMN(CW37)-MAX(COLUMN($AG37:CV37)*($AG37:CV37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CV37)*($AG37:CV37=2))>MAX(COLUMN($AG37:CV37)*($AG37:CV37=3)),MAX(COLUMN($AG37:CV37)*($AG37:CV37=2))>MAX(COLUMN($AG37:CV37)*($AG37:CV37=1))),IF(COLUMN(CW37)-MAX(COLUMN($AG37:CV37)*($AG37:CV37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CW37)-MAX(COLUMN($AG37:CV37)*($AG37:CV37=3))=$J37,3,0),IF(COLUMN(CW37)-MAX(COLUMN($AG37:CV37)*($AG37:CV37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CW37)*($AG37:CW37=1))>MAX(COLUMN($AG37:CW37)*($AG37:CW37=3)),MAX(COLUMN($AG37:CW37)*($AG37:CW37=1))>MAX(COLUMN($AG37:CW37)*($AG37:CW37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CX37)-MAX(COLUMN($AG37:CW37)*($AG37:CW37=1))=$J37,3,0),IF(COLUMN(CX37)-MAX(COLUMN($AG37:CW37)*($AG37:CW37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CW37)*($AG37:CW37=2))>MAX(COLUMN($AG37:CW37)*($AG37:CW37=3)),MAX(COLUMN($AG37:CW37)*($AG37:CW37=2))>MAX(COLUMN($AG37:CW37)*($AG37:CW37=1))),IF(COLUMN(CX37)-MAX(COLUMN($AG37:CW37)*($AG37:CW37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CX37)-MAX(COLUMN($AG37:CW37)*($AG37:CW37=3))=$J37,3,0),IF(COLUMN(CX37)-MAX(COLUMN($AG37:CW37)*($AG37:CW37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CX37)*($AG37:CX37=1))>MAX(COLUMN($AG37:CX37)*($AG37:CX37=3)),MAX(COLUMN($AG37:CX37)*($AG37:CX37=1))>MAX(COLUMN($AG37:CX37)*($AG37:CX37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CY37)-MAX(COLUMN($AG37:CX37)*($AG37:CX37=1))=$J37,3,0),IF(COLUMN(CY37)-MAX(COLUMN($AG37:CX37)*($AG37:CX37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CX37)*($AG37:CX37=2))>MAX(COLUMN($AG37:CX37)*($AG37:CX37=3)),MAX(COLUMN($AG37:CX37)*($AG37:CX37=2))>MAX(COLUMN($AG37:CX37)*($AG37:CX37=1))),IF(COLUMN(CY37)-MAX(COLUMN($AG37:CX37)*($AG37:CX37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CY37)-MAX(COLUMN($AG37:CX37)*($AG37:CX37=3))=$J37,3,0),IF(COLUMN(CY37)-MAX(COLUMN($AG37:CX37)*($AG37:CX37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CY37)*($AG37:CY37=1))>MAX(COLUMN($AG37:CY37)*($AG37:CY37=3)),MAX(COLUMN($AG37:CY37)*($AG37:CY37=1))>MAX(COLUMN($AG37:CY37)*($AG37:CY37=2))),IF($K37=\"Not Possible\",IF(COLUMN(CZ37)-MAX(COLUMN($AG37:CY37)*($AG37:CY37=1))=$J37,3,0),IF(COLUMN(CZ37)-MAX(COLUMN($AG37:CY37)*($AG37:CY37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CY37)*($AG37:CY37=2))>MAX(COLUMN($AG37:CY37)*($AG37:CY37=3)),MAX(COLUMN($AG37:CY37)*($AG37:CY37=2))>MAX(COLUMN($AG37:CY37)*($AG37:CY37=1))),IF(COLUMN(CZ37)-MAX(COLUMN($AG37:CY37)*($AG37:CY37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(CZ37)-MAX(COLUMN($AG37:CY37)*($AG37:CY37=3))=$J37,3,0),IF(COLUMN(CZ37)-MAX(COLUMN($AG37:CY37)*($AG37:CY37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=1))>MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=3)),MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=1))>MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DA37)-MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=1))=$J37,3,0),IF(COLUMN(DA37)-MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=2))>MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=3)),MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=2))>MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=1))),IF(COLUMN(DA37)-MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DA37)-MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=3))=$J37,3,0),IF(COLUMN(DA37)-MAX(COLUMN($AG37:CZ37)*($AG37:CZ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DA37)*($AG37:DA37=1))>MAX(COLUMN($AG37:DA37)*($AG37:DA37=3)),MAX(COLUMN($AG37:DA37)*($AG37:DA37=1))>MAX(COLUMN($AG37:DA37)*($AG37:DA37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DB37)-MAX(COLUMN($AG37:DA37)*($AG37:DA37=1))=$J37,3,0),IF(COLUMN(DB37)-MAX(COLUMN($AG37:DA37)*($AG37:DA37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DA37)*($AG37:DA37=2))>MAX(COLUMN($AG37:DA37)*($AG37:DA37=3)),MAX(COLUMN($AG37:DA37)*($AG37:DA37=2))>MAX(COLUMN($AG37:DA37)*($AG37:DA37=1))),IF(COLUMN(DB37)-MAX(COLUMN($AG37:DA37)*($AG37:DA37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DB37)-MAX(COLUMN($AG37:DA37)*($AG37:DA37=3))=$J37,3,0),IF(COLUMN(DB37)-MAX(COLUMN($AG37:DA37)*($AG37:DA37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DB37)*($AG37:DB37=1))>MAX(COLUMN($AG37:DB37)*($AG37:DB37=3)),MAX(COLUMN($AG37:DB37)*($AG37:DB37=1))>MAX(COLUMN($AG37:DB37)*($AG37:DB37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DC37)-MAX(COLUMN($AG37:DB37)*($AG37:DB37=1))=$J37,3,0),IF(COLUMN(DC37)-MAX(COLUMN($AG37:DB37)*($AG37:DB37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DB37)*($AG37:DB37=2))>MAX(COLUMN($AG37:DB37)*($AG37:DB37=3)),MAX(COLUMN($AG37:DB37)*($AG37:DB37=2))>MAX(COLUMN($AG37:DB37)*($AG37:DB37=1))),IF(COLUMN(DC37)-MAX(COLUMN($AG37:DB37)*($AG37:DB37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DC37)-MAX(COLUMN($AG37:DB37)*($AG37:DB37=3))=$J37,3,0),IF(COLUMN(DC37)-MAX(COLUMN($AG37:DB37)*($AG37:DB37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DC37)*($AG37:DC37=1))>MAX(COLUMN($AG37:DC37)*($AG37:DC37=3)),MAX(COLUMN($AG37:DC37)*($AG37:DC37=1))>MAX(COLUMN($AG37:DC37)*($AG37:DC37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DD37)-MAX(COLUMN($AG37:DC37)*($AG37:DC37=1))=$J37,3,0),IF(COLUMN(DD37)-MAX(COLUMN($AG37:DC37)*($AG37:DC37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DC37)*($AG37:DC37=2))>MAX(COLUMN($AG37:DC37)*($AG37:DC37=3)),MAX(COLUMN($AG37:DC37)*($AG37:DC37=2))>MAX(COLUMN($AG37:DC37)*($AG37:DC37=1))),IF(COLUMN(DD37)-MAX(COLUMN($AG37:DC37)*($AG37:DC37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DD37)-MAX(COLUMN($AG37:DC37)*($AG37:DC37=3))=$J37,3,0),IF(COLUMN(DD37)-MAX(COLUMN($AG37:DC37)*($AG37:DC37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DD37)*($AG37:DD37=1))>MAX(COLUMN($AG37:DD37)*($AG37:DD37=3)),MAX(COLUMN($AG37:DD37)*($AG37:DD37=1))>MAX(COLUMN($AG37:DD37)*($AG37:DD37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DE37)-MAX(COLUMN($AG37:DD37)*($AG37:DD37=1))=$J37,3,0),IF(COLUMN(DE37)-MAX(COLUMN($AG37:DD37)*($AG37:DD37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DD37)*($AG37:DD37=2))>MAX(COLUMN($AG37:DD37)*($AG37:DD37=3)),MAX(COLUMN($AG37:DD37)*($AG37:DD37=2))>MAX(COLUMN($AG37:DD37)*($AG37:DD37=1))),IF(COLUMN(DE37)-MAX(COLUMN($AG37:DD37)*($AG37:DD37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DE37)-MAX(COLUMN($AG37:DD37)*($AG37:DD37=3))=$J37,3,0),IF(COLUMN(DE37)-MAX(COLUMN($AG37:DD37)*($AG37:DD37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DE37)*($AG37:DE37=1))>MAX(COLUMN($AG37:DE37)*($AG37:DE37=3)),MAX(COLUMN($AG37:DE37)*($AG37:DE37=1))>MAX(COLUMN($AG37:DE37)*($AG37:DE37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DF37)-MAX(COLUMN($AG37:DE37)*($AG37:DE37=1))=$J37,3,0),IF(COLUMN(DF37)-MAX(COLUMN($AG37:DE37)*($AG37:DE37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DE37)*($AG37:DE37=2))>MAX(COLUMN($AG37:DE37)*($AG37:DE37=3)),MAX(COLUMN($AG37:DE37)*($AG37:DE37=2))>MAX(COLUMN($AG37:DE37)*($AG37:DE37=1))),IF(COLUMN(DF37)-MAX(COLUMN($AG37:DE37)*($AG37:DE37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DF37)-MAX(COLUMN($AG37:DE37)*($AG37:DE37=3))=$J37,3,0),IF(COLUMN(DF37)-MAX(COLUMN($AG37:DE37)*($AG37:DE37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DF37)*($AG37:DF37=1))>MAX(COLUMN($AG37:DF37)*($AG37:DF37=3)),MAX(COLUMN($AG37:DF37)*($AG37:DF37=1))>MAX(COLUMN($AG37:DF37)*($AG37:DF37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DG37)-MAX(COLUMN($AG37:DF37)*($AG37:DF37=1))=$J37,3,0),IF(COLUMN(DG37)-MAX(COLUMN($AG37:DF37)*($AG37:DF37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DF37)*($AG37:DF37=2))>MAX(COLUMN($AG37:DF37)*($AG37:DF37=3)),MAX(COLUMN($AG37:DF37)*($AG37:DF37=2))>MAX(COLUMN($AG37:DF37)*($AG37:DF37=1))),IF(COLUMN(DG37)-MAX(COLUMN($AG37:DF37)*($AG37:DF37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DG37)-MAX(COLUMN($AG37:DF37)*($AG37:DF37=3))=$J37,3,0),IF(COLUMN(DG37)-MAX(COLUMN($AG37:DF37)*($AG37:DF37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DG37)*($AG37:DG37=1))>MAX(COLUMN($AG37:DG37)*($AG37:DG37=3)),MAX(COLUMN($AG37:DG37)*($AG37:DG37=1))>MAX(COLUMN($AG37:DG37)*($AG37:DG37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DH37)-MAX(COLUMN($AG37:DG37)*($AG37:DG37=1))=$J37,3,0),IF(COLUMN(DH37)-MAX(COLUMN($AG37:DG37)*($AG37:DG37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DG37)*($AG37:DG37=2))>MAX(COLUMN($AG37:DG37)*($AG37:DG37=3)),MAX(COLUMN($AG37:DG37)*($AG37:DG37=2))>MAX(COLUMN($AG37:DG37)*($AG37:DG37=1))),IF(COLUMN(DH37)-MAX(COLUMN($AG37:DG37)*($AG37:DG37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DH37)-MAX(COLUMN($AG37:DG37)*($AG37:DG37=3))=$J37,3,0),IF(COLUMN(DH37)-MAX(COLUMN($AG37:DG37)*($AG37:DG37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DH37)*($AG37:DH37=1))>MAX(COLUMN($AG37:DH37)*($AG37:DH37=3)),MAX(COLUMN($AG37:DH37)*($AG37:DH37=1))>MAX(COLUMN($AG37:DH37)*($AG37:DH37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DI37)-MAX(COLUMN($AG37:DH37)*($AG37:DH37=1))=$J37,3,0),IF(COLUMN(DI37)-MAX(COLUMN($AG37:DH37)*($AG37:DH37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DH37)*($AG37:DH37=2))>MAX(COLUMN($AG37:DH37)*($AG37:DH37=3)),MAX(COLUMN($AG37:DH37)*($AG37:DH37=2))>MAX(COLUMN($AG37:DH37)*($AG37:DH37=1))),IF(COLUMN(DI37)-MAX(COLUMN($AG37:DH37)*($AG37:DH37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DI37)-MAX(COLUMN($AG37:DH37)*($AG37:DH37=3))=$J37,3,0),IF(COLUMN(DI37)-MAX(COLUMN($AG37:DH37)*($AG37:DH37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DI37)*($AG37:DI37=1))>MAX(COLUMN($AG37:DI37)*($AG37:DI37=3)),MAX(COLUMN($AG37:DI37)*($AG37:DI37=1))>MAX(COLUMN($AG37:DI37)*($AG37:DI37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DJ37)-MAX(COLUMN($AG37:DI37)*($AG37:DI37=1))=$J37,3,0),IF(COLUMN(DJ37)-MAX(COLUMN($AG37:DI37)*($AG37:DI37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DI37)*($AG37:DI37=2))>MAX(COLUMN($AG37:DI37)*($AG37:DI37=3)),MAX(COLUMN($AG37:DI37)*($AG37:DI37=2))>MAX(COLUMN($AG37:DI37)*($AG37:DI37=1))),IF(COLUMN(DJ37)-MAX(COLUMN($AG37:DI37)*($AG37:DI37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DJ37)-MAX(COLUMN($AG37:DI37)*($AG37:DI37=3))=$J37,3,0),IF(COLUMN(DJ37)-MAX(COLUMN($AG37:DI37)*($AG37:DI37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=1))>MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=3)),MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=1))>MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DK37)-MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=1))=$J37,3,0),IF(COLUMN(DK37)-MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=2))>MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=3)),MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=2))>MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=1))),IF(COLUMN(DK37)-MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DK37)-MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=3))=$J37,3,0),IF(COLUMN(DK37)-MAX(COLUMN($AG37:DJ37)*($AG37:DJ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DK37)*($AG37:DK37=1))>MAX(COLUMN($AG37:DK37)*($AG37:DK37=3)),MAX(COLUMN($AG37:DK37)*($AG37:DK37=1))>MAX(COLUMN($AG37:DK37)*($AG37:DK37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DL37)-MAX(COLUMN($AG37:DK37)*($AG37:DK37=1))=$J37,3,0),IF(COLUMN(DL37)-MAX(COLUMN($AG37:DK37)*($AG37:DK37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DK37)*($AG37:DK37=2))>MAX(COLUMN($AG37:DK37)*($AG37:DK37=3)),MAX(COLUMN($AG37:DK37)*($AG37:DK37=2))>MAX(COLUMN($AG37:DK37)*($AG37:DK37=1))),IF(COLUMN(DL37)-MAX(COLUMN($AG37:DK37)*($AG37:DK37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DL37)-MAX(COLUMN($AG37:DK37)*($AG37:DK37=3))=$J37,3,0),IF(COLUMN(DL37)-MAX(COLUMN($AG37:DK37)*($AG37:DK37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DL37)*($AG37:DL37=1))>MAX(COLUMN($AG37:DL37)*($AG37:DL37=3)),MAX(COLUMN($AG37:DL37)*($AG37:DL37=1))>MAX(COLUMN($AG37:DL37)*($AG37:DL37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DM37)-MAX(COLUMN($AG37:DL37)*($AG37:DL37=1))=$J37,3,0),IF(COLUMN(DM37)-MAX(COLUMN($AG37:DL37)*($AG37:DL37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DL37)*($AG37:DL37=2))>MAX(COLUMN($AG37:DL37)*($AG37:DL37=3)),MAX(COLUMN($AG37:DL37)*($AG37:DL37=2))>MAX(COLUMN($AG37:DL37)*($AG37:DL37=1))),IF(COLUMN(DM37)-MAX(COLUMN($AG37:DL37)*($AG37:DL37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DM37)-MAX(COLUMN($AG37:DL37)*($AG37:DL37=3))=$J37,3,0),IF(COLUMN(DM37)-MAX(COLUMN($AG37:DL37)*($AG37:DL37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DM37)*($AG37:DM37=1))>MAX(COLUMN($AG37:DM37)*($AG37:DM37=3)),MAX(COLUMN($AG37:DM37)*($AG37:DM37=1))>MAX(COLUMN($AG37:DM37)*($AG37:DM37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DN37)-MAX(COLUMN($AG37:DM37)*($AG37:DM37=1))=$J37,3,0),IF(COLUMN(DN37)-MAX(COLUMN($AG37:DM37)*($AG37:DM37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DM37)*($AG37:DM37=2))>MAX(COLUMN($AG37:DM37)*($AG37:DM37=3)),MAX(COLUMN($AG37:DM37)*($AG37:DM37=2))>MAX(COLUMN($AG37:DM37)*($AG37:DM37=1))),IF(COLUMN(DN37)-MAX(COLUMN($AG37:DM37)*($AG37:DM37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DN37)-MAX(COLUMN($AG37:DM37)*($AG37:DM37=3))=$J37,3,0),IF(COLUMN(DN37)-MAX(COLUMN($AG37:DM37)*($AG37:DM37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DN37)*($AG37:DN37=1))>MAX(COLUMN($AG37:DN37)*($AG37:DN37=3)),MAX(COLUMN($AG37:DN37)*($AG37:DN37=1))>MAX(COLUMN($AG37:DN37)*($AG37:DN37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DO37)-MAX(COLUMN($AG37:DN37)*($AG37:DN37=1))=$J37,3,0),IF(COLUMN(DO37)-MAX(COLUMN($AG37:DN37)*($AG37:DN37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DN37)*($AG37:DN37=2))>MAX(COLUMN($AG37:DN37)*($AG37:DN37=3)),MAX(COLUMN($AG37:DN37)*($AG37:DN37=2))>MAX(COLUMN($AG37:DN37)*($AG37:DN37=1))),IF(COLUMN(DO37)-MAX(COLUMN($AG37:DN37)*($AG37:DN37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DO37)-MAX(COLUMN($AG37:DN37)*($AG37:DN37=3))=$J37,3,0),IF(COLUMN(DO37)-MAX(COLUMN($AG37:DN37)*($AG37:DN37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DO37)*($AG37:DO37=1))>MAX(COLUMN($AG37:DO37)*($AG37:DO37=3)),MAX(COLUMN($AG37:DO37)*($AG37:DO37=1))>MAX(COLUMN($AG37:DO37)*($AG37:DO37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DP37)-MAX(COLUMN($AG37:DO37)*($AG37:DO37=1))=$J37,3,0),IF(COLUMN(DP37)-MAX(COLUMN($AG37:DO37)*($AG37:DO37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DO37)*($AG37:DO37=2))>MAX(COLUMN($AG37:DO37)*($AG37:DO37=3)),MAX(COLUMN($AG37:DO37)*($AG37:DO37=2))>MAX(COLUMN($AG37:DO37)*($AG37:DO37=1))),IF(COLUMN(DP37)-MAX(COLUMN($AG37:DO37)*($AG37:DO37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DP37)-MAX(COLUMN($AG37:DO37)*($AG37:DO37=3))=$J37,3,0),IF(COLUMN(DP37)-MAX(COLUMN($AG37:DO37)*($AG37:DO37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DP37)*($AG37:DP37=1))>MAX(COLUMN($AG37:DP37)*($AG37:DP37=3)),MAX(COLUMN($AG37:DP37)*($AG37:DP37=1))>MAX(COLUMN($AG37:DP37)*($AG37:DP37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DQ37)-MAX(COLUMN($AG37:DP37)*($AG37:DP37=1))=$J37,3,0),IF(COLUMN(DQ37)-MAX(COLUMN($AG37:DP37)*($AG37:DP37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DP37)*($AG37:DP37=2))>MAX(COLUMN($AG37:DP37)*($AG37:DP37=3)),MAX(COLUMN($AG37:DP37)*($AG37:DP37=2))>MAX(COLUMN($AG37:DP37)*($AG37:DP37=1))),IF(COLUMN(DQ37)-MAX(COLUMN($AG37:DP37)*($AG37:DP37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DQ37)-MAX(COLUMN($AG37:DP37)*($AG37:DP37=3))=$J37,3,0),IF(COLUMN(DQ37)-MAX(COLUMN($AG37:DP37)*($AG37:DP37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=1))>MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=3)),MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=1))>MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DR37)-MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=1))=$J37,3,0),IF(COLUMN(DR37)-MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=2))>MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=3)),MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=2))>MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=1))),IF(COLUMN(DR37)-MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DR37)-MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=3))=$J37,3,0),IF(COLUMN(DR37)-MAX(COLUMN($AG37:DQ37)*($AG37:DQ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DR37)*($AG37:DR37=1))>MAX(COLUMN($AG37:DR37)*($AG37:DR37=3)),MAX(COLUMN($AG37:DR37)*($AG37:DR37=1))>MAX(COLUMN($AG37:DR37)*($AG37:DR37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DS37)-MAX(COLUMN($AG37:DR37)*($AG37:DR37=1))=$J37,3,0),IF(COLUMN(DS37)-MAX(COLUMN($AG37:DR37)*($AG37:DR37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DR37)*($AG37:DR37=2))>MAX(COLUMN($AG37:DR37)*($AG37:DR37=3)),MAX(COLUMN($AG37:DR37)*($AG37:DR37=2))>MAX(COLUMN($AG37:DR37)*($AG37:DR37=1))),IF(COLUMN(DS37)-MAX(COLUMN($AG37:DR37)*($AG37:DR37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DS37)-MAX(COLUMN($AG37:DR37)*($AG37:DR37=3))=$J37,3,0),IF(COLUMN(DS37)-MAX(COLUMN($AG37:DR37)*($AG37:DR37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DS37)*($AG37:DS37=1))>MAX(COLUMN($AG37:DS37)*($AG37:DS37=3)),MAX(COLUMN($AG37:DS37)*($AG37:DS37=1))>MAX(COLUMN($AG37:DS37)*($AG37:DS37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DT37)-MAX(COLUMN($AG37:DS37)*($AG37:DS37=1))=$J37,3,0),IF(COLUMN(DT37)-MAX(COLUMN($AG37:DS37)*($AG37:DS37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DS37)*($AG37:DS37=2))>MAX(COLUMN($AG37:DS37)*($AG37:DS37=3)),MAX(COLUMN($AG37:DS37)*($AG37:DS37=2))>MAX(COLUMN($AG37:DS37)*($AG37:DS37=1))),IF(COLUMN(DT37)-MAX(COLUMN($AG37:DS37)*($AG37:DS37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DT37)-MAX(COLUMN($AG37:DS37)*($AG37:DS37=3))=$J37,3,0),IF(COLUMN(DT37)-MAX(COLUMN($AG37:DS37)*($AG37:DS37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DT37)*($AG37:DT37=1))>MAX(COLUMN($AG37:DT37)*($AG37:DT37=3)),MAX(COLUMN($AG37:DT37)*($AG37:DT37=1))>MAX(COLUMN($AG37:DT37)*($AG37:DT37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DU37)-MAX(COLUMN($AG37:DT37)*($AG37:DT37=1))=$J37,3,0),IF(COLUMN(DU37)-MAX(COLUMN($AG37:DT37)*($AG37:DT37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DT37)*($AG37:DT37=2))>MAX(COLUMN($AG37:DT37)*($AG37:DT37=3)),MAX(COLUMN($AG37:DT37)*($AG37:DT37=2))>MAX(COLUMN($AG37:DT37)*($AG37:DT37=1))),IF(COLUMN(DU37)-MAX(COLUMN($AG37:DT37)*($AG37:DT37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DU37)-MAX(COLUMN($AG37:DT37)*($AG37:DT37=3))=$J37,3,0),IF(COLUMN(DU37)-MAX(COLUMN($AG37:DT37)*($AG37:DT37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DU37)*($AG37:DU37=1))>MAX(COLUMN($AG37:DU37)*($AG37:DU37=3)),MAX(COLUMN($AG37:DU37)*($AG37:DU37=1))>MAX(COLUMN($AG37:DU37)*($AG37:DU37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DV37)-MAX(COLUMN($AG37:DU37)*($AG37:DU37=1))=$J37,3,0),IF(COLUMN(DV37)-MAX(COLUMN($AG37:DU37)*($AG37:DU37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DU37)*($AG37:DU37=2))>MAX(COLUMN($AG37:DU37)*($AG37:DU37=3)),MAX(COLUMN($AG37:DU37)*($AG37:DU37=2))>MAX(COLUMN($AG37:DU37)*($AG37:DU37=1))),IF(COLUMN(DV37)-MAX(COLUMN($AG37:DU37)*($AG37:DU37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DV37)-MAX(COLUMN($AG37:DU37)*($AG37:DU37=3))=$J37,3,0),IF(COLUMN(DV37)-MAX(COLUMN($AG37:DU37)*($AG37:DU37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DV37)*($AG37:DV37=1))>MAX(COLUMN($AG37:DV37)*($AG37:DV37=3)),MAX(COLUMN($AG37:DV37)*($AG37:DV37=1))>MAX(COLUMN($AG37:DV37)*($AG37:DV37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DW37)-MAX(COLUMN($AG37:DV37)*($AG37:DV37=1))=$J37,3,0),IF(COLUMN(DW37)-MAX(COLUMN($AG37:DV37)*($AG37:DV37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DV37)*($AG37:DV37=2))>MAX(COLUMN($AG37:DV37)*($AG37:DV37=3)),MAX(COLUMN($AG37:DV37)*($AG37:DV37=2))>MAX(COLUMN($AG37:DV37)*($AG37:DV37=1))),IF(COLUMN(DW37)-MAX(COLUMN($AG37:DV37)*($AG37:DV37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DW37)-MAX(COLUMN($AG37:DV37)*($AG37:DV37=3))=$J37,3,0),IF(COLUMN(DW37)-MAX(COLUMN($AG37:DV37)*($AG37:DV37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DW37)*($AG37:DW37=1))>MAX(COLUMN($AG37:DW37)*($AG37:DW37=3)),MAX(COLUMN($AG37:DW37)*($AG37:DW37=1))>MAX(COLUMN($AG37:DW37)*($AG37:DW37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DX37)-MAX(COLUMN($AG37:DW37)*($AG37:DW37=1))=$J37,3,0),IF(COLUMN(DX37)-MAX(COLUMN($AG37:DW37)*($AG37:DW37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DW37)*($AG37:DW37=2))>MAX(COLUMN($AG37:DW37)*($AG37:DW37=3)),MAX(COLUMN($AG37:DW37)*($AG37:DW37=2))>MAX(COLUMN($AG37:DW37)*($AG37:DW37=1))),IF(COLUMN(DX37)-MAX(COLUMN($AG37:DW37)*($AG37:DW37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DX37)-MAX(COLUMN($AG37:DW37)*($AG37:DW37=3))=$J37,3,0),IF(COLUMN(DX37)-MAX(COLUMN($AG37:DW37)*($AG37:DW37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DX37)*($AG37:DX37=1))>MAX(COLUMN($AG37:DX37)*($AG37:DX37=3)),MAX(COLUMN($AG37:DX37)*($AG37:DX37=1))>MAX(COLUMN($AG37:DX37)*($AG37:DX37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DY37)-MAX(COLUMN($AG37:DX37)*($AG37:DX37=1))=$J37,3,0),IF(COLUMN(DY37)-MAX(COLUMN($AG37:DX37)*($AG37:DX37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DX37)*($AG37:DX37=2))>MAX(COLUMN($AG37:DX37)*($AG37:DX37=3)),MAX(COLUMN($AG37:DX37)*($AG37:DX37=2))>MAX(COLUMN($AG37:DX37)*($AG37:DX37=1))),IF(COLUMN(DY37)-MAX(COLUMN($AG37:DX37)*($AG37:DX37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DY37)-MAX(COLUMN($AG37:DX37)*($AG37:DX37=3))=$J37,3,0),IF(COLUMN(DY37)-MAX(COLUMN($AG37:DX37)*($AG37:DX37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DY37)*($AG37:DY37=1))>MAX(COLUMN($AG37:DY37)*($AG37:DY37=3)),MAX(COLUMN($AG37:DY37)*($AG37:DY37=1))>MAX(COLUMN($AG37:DY37)*($AG37:DY37=2))),IF($K37=\"Not Possible\",IF(COLUMN(DZ37)-MAX(COLUMN($AG37:DY37)*($AG37:DY37=1))=$J37,3,0),IF(COLUMN(DZ37)-MAX(COLUMN($AG37:DY37)*($AG37:DY37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DY37)*($AG37:DY37=2))>MAX(COLUMN($AG37:DY37)*($AG37:DY37=3)),MAX(COLUMN($AG37:DY37)*($AG37:DY37=2))>MAX(COLUMN($AG37:DY37)*($AG37:DY37=1))),IF(COLUMN(DZ37)-MAX(COLUMN($AG37:DY37)*($AG37:DY37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(DZ37)-MAX(COLUMN($AG37:DY37)*($AG37:DY37=3))=$J37,3,0),IF(COLUMN(DZ37)-MAX(COLUMN($AG37:DY37)*($AG37:DY37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=1))>MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=3)),MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=1))>MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=2))),IF($K37=\"Not Possible\",IF(COLUMN(EA37)-MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=1))=$J37,3,0),IF(COLUMN(EA37)-MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=2))>MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=3)),MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=2))>MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=1))),IF(COLUMN(EA37)-MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(EA37)-MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=3))=$J37,3,0),IF(COLUMN(EA37)-MAX(COLUMN($AG37:DZ37)*($AG37:DZ37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:EA37)*($AG37:EA37=1))>MAX(COLUMN($AG37:EA37)*($AG37:EA37=3)),MAX(COLUMN($AG37:EA37)*($AG37:EA37=1))>MAX(COLUMN($AG37:EA37)*($AG37:EA37=2))),IF($K37=\"Not Possible\",IF(COLUMN(EB37)-MAX(COLUMN($AG37:EA37)*($AG37:EA37=1))=$J37,3,0),IF(COLUMN(EB37)-MAX(COLUMN($AG37:EA37)*($AG37:EA37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:EA37)*($AG37:EA37=2))>MAX(COLUMN($AG37:EA37)*($AG37:EA37=3)),MAX(COLUMN($AG37:EA37)*($AG37:EA37=2))>MAX(COLUMN($AG37:EA37)*($AG37:EA37=1))),IF(COLUMN(EB37)-MAX(COLUMN($AG37:EA37)*($AG37:EA37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(EB37)-MAX(COLUMN($AG37:EA37)*($AG37:EA37=3))=$J37,3,0),IF(COLUMN(EB37)-MAX(COLUMN($AG37:EA37)*($AG37:EA37=3))=$J37,2,0)))))","v":0},{"$f":"IF($AG37=4,0,IF(AND(MAX(COLUMN($AG37:EB37)*($AG37:EB37=1))>MAX(COLUMN($AG37:EB37)*($AG37:EB37=3)),MAX(COLUMN($AG37:EB37)*($AG37:EB37=1))>MAX(COLUMN($AG37:EB37)*($AG37:EB37=2))),IF($K37=\"Not Possible\",IF(COLUMN(EC37)-MAX(COLUMN($AG37:EB37)*($AG37:EB37=1))=$J37,3,0),IF(COLUMN(EC37)-MAX(COLUMN($AG37:EB37)*($AG37:EB37=1))=$J37,2,0)),IF(AND(MAX(COLUMN($AG37:EB37)*($AG37:EB37=2))>MAX(COLUMN($AG37:EB37)*($AG37:EB37=3)),MAX(COLUMN($AG37:EB37)*($AG37:EB37=2))>MAX(COLUMN($AG37:EB37)*($AG37:EB37=1))),IF(COLUMN(EC37)-MAX(COLUMN($AG37:EB37)*($AG37:EB37=2))=$L37,3,0),IF($K37=\"Not Possible\",IF(COLUMN(EC37)-MAX(COLUMN($AG37:EB37)*($AG37:EB37=3))=$J37,3,0),IF(COLUMN(EC37)-MAX(COLUMN($AG37:EB37)*($AG37:EB37=3))=$J37,2,0)))))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":""},null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset class],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":""},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",Form_Asset[[#This Row],[Asset ID]]&ROW())","v":""},null,null,{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",INDEX(AssetListTbl[Best Estimate Life (5)],(MATCH(Form_Asset[[#This Row],[Sub-Asset category]],AssetListTbl[Sub-Element Category],0))))","v":""},null,null,null,null,{"$f":"MAX(COLUMN($AH38:EC38)*($AH38:EC38=2))","v":0},{"$f":"MAX(COLUMN($AH38:EC38)*($AH38:EC38=3))","v":0},{"$f":"IFERROR(100-(IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Replace]])),INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Refurb]])))),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],3,2)","v":2},{"$f":"SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Product_Stage[CO2e (t)])","v":0},{"$f":"IFERROR(SUM(Form_Elements[General Item Material])*(Form_Asset[[#This Row],[Weighted Split]]/SUM(Form_Asset[Weighted Split]))+Form_Asset[[#This Row],[Weighted Split]],0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth (wtt)]))+(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Transport]))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Non contractor People Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Contractor people transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Site establishment])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),(SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Const_Ins_InsB[CO2e (t)]))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Other Construction Waste])*Form_Asset[[#This Row],[Weighted Split]]/(SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[[Waste Co2e ]])+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New build\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]]),IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",(SUM(Form_Asset[[#This Row],[Materials]:[Waste]])-(SUM(Form_Asset[[#This Row],[Materials Transport]],Form_Asset[[#This Row],[People Transport]]*0.5,Form_Asset[[#This Row],[Plant Transport]]*0.5))),IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]])/(SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%])),0)))","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_energy[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_use_energy[CO2e (t)]),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset ref.]]=\"\",0,SUMIF(Form_Asset[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Asset[New Build Co2e])*SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%]))","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Dem - General Item Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Dem -Waste Co2e]),0)","v":0},{"$f":"(Form_Asset[[#This Row],[Plant use]]+Form_Asset[[#This Row],[Plant Transport]])*50%","v":0},{"$f":"Form_Asset[[#This Row],[People Transport]]*50%","v":0},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New Build\",1,IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",2,IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",3,IF(Form_Asset[[#This Row],[First intervention]]=\"Demolition\",4,\"\"))))","v":""},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AG38)*($AG38:AG38=1))>MAX(COLUMN($AG38:AG38)*($AG38:AG38=3)),MAX(COLUMN($AG38:AG38)*($AG38:AG38=1))>MAX(COLUMN($AG38:AG38)*($AG38:AG38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AH38)-MAX(COLUMN($AG38:AG38)*($AG38:AG38=1))=$J38,3,0),IF(COLUMN(AH38)-MAX(COLUMN($AG38:AG38)*($AG38:AG38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AG38)*($AG38:AG38=2))>MAX(COLUMN($AG38:AG38)*($AG38:AG38=3)),MAX(COLUMN($AG38:AG38)*($AG38:AG38=2))>MAX(COLUMN($AG38:AG38)*($AG38:AG38=1))),IF(COLUMN(AH38)-MAX(COLUMN($AG38:AG38)*($AG38:AG38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AH38)-MAX(COLUMN($AG38:AG38)*($AG38:AG38=3))=$J38,3,0),IF(COLUMN(AH38)-MAX(COLUMN($AG38:AG38)*($AG38:AG38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AH38)*($AG38:AH38=1))>MAX(COLUMN($AG38:AH38)*($AG38:AH38=3)),MAX(COLUMN($AG38:AH38)*($AG38:AH38=1))>MAX(COLUMN($AG38:AH38)*($AG38:AH38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AI38)-MAX(COLUMN($AG38:AH38)*($AG38:AH38=1))=$J38,3,0),IF(COLUMN(AI38)-MAX(COLUMN($AG38:AH38)*($AG38:AH38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AH38)*($AG38:AH38=2))>MAX(COLUMN($AG38:AH38)*($AG38:AH38=3)),MAX(COLUMN($AG38:AH38)*($AG38:AH38=2))>MAX(COLUMN($AG38:AH38)*($AG38:AH38=1))),IF(COLUMN(AI38)-MAX(COLUMN($AG38:AH38)*($AG38:AH38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AI38)-MAX(COLUMN($AG38:AH38)*($AG38:AH38=3))=$J38,3,0),IF(COLUMN(AI38)-MAX(COLUMN($AG38:AH38)*($AG38:AH38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AI38)*($AG38:AI38=1))>MAX(COLUMN($AG38:AI38)*($AG38:AI38=3)),MAX(COLUMN($AG38:AI38)*($AG38:AI38=1))>MAX(COLUMN($AG38:AI38)*($AG38:AI38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AJ38)-MAX(COLUMN($AG38:AI38)*($AG38:AI38=1))=$J38,3,0),IF(COLUMN(AJ38)-MAX(COLUMN($AG38:AI38)*($AG38:AI38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AI38)*($AG38:AI38=2))>MAX(COLUMN($AG38:AI38)*($AG38:AI38=3)),MAX(COLUMN($AG38:AI38)*($AG38:AI38=2))>MAX(COLUMN($AG38:AI38)*($AG38:AI38=1))),IF(COLUMN(AJ38)-MAX(COLUMN($AG38:AI38)*($AG38:AI38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AJ38)-MAX(COLUMN($AG38:AI38)*($AG38:AI38=3))=$J38,3,0),IF(COLUMN(AJ38)-MAX(COLUMN($AG38:AI38)*($AG38:AI38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=1))>MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=3)),MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=1))>MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AK38)-MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=1))=$J38,3,0),IF(COLUMN(AK38)-MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=2))>MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=3)),MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=2))>MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=1))),IF(COLUMN(AK38)-MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AK38)-MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=3))=$J38,3,0),IF(COLUMN(AK38)-MAX(COLUMN($AG38:AJ38)*($AG38:AJ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AK38)*($AG38:AK38=1))>MAX(COLUMN($AG38:AK38)*($AG38:AK38=3)),MAX(COLUMN($AG38:AK38)*($AG38:AK38=1))>MAX(COLUMN($AG38:AK38)*($AG38:AK38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AL38)-MAX(COLUMN($AG38:AK38)*($AG38:AK38=1))=$J38,3,0),IF(COLUMN(AL38)-MAX(COLUMN($AG38:AK38)*($AG38:AK38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AK38)*($AG38:AK38=2))>MAX(COLUMN($AG38:AK38)*($AG38:AK38=3)),MAX(COLUMN($AG38:AK38)*($AG38:AK38=2))>MAX(COLUMN($AG38:AK38)*($AG38:AK38=1))),IF(COLUMN(AL38)-MAX(COLUMN($AG38:AK38)*($AG38:AK38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AL38)-MAX(COLUMN($AG38:AK38)*($AG38:AK38=3))=$J38,3,0),IF(COLUMN(AL38)-MAX(COLUMN($AG38:AK38)*($AG38:AK38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AL38)*($AG38:AL38=1))>MAX(COLUMN($AG38:AL38)*($AG38:AL38=3)),MAX(COLUMN($AG38:AL38)*($AG38:AL38=1))>MAX(COLUMN($AG38:AL38)*($AG38:AL38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AM38)-MAX(COLUMN($AG38:AL38)*($AG38:AL38=1))=$J38,3,0),IF(COLUMN(AM38)-MAX(COLUMN($AG38:AL38)*($AG38:AL38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AL38)*($AG38:AL38=2))>MAX(COLUMN($AG38:AL38)*($AG38:AL38=3)),MAX(COLUMN($AG38:AL38)*($AG38:AL38=2))>MAX(COLUMN($AG38:AL38)*($AG38:AL38=1))),IF(COLUMN(AM38)-MAX(COLUMN($AG38:AL38)*($AG38:AL38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AM38)-MAX(COLUMN($AG38:AL38)*($AG38:AL38=3))=$J38,3,0),IF(COLUMN(AM38)-MAX(COLUMN($AG38:AL38)*($AG38:AL38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AM38)*($AG38:AM38=1))>MAX(COLUMN($AG38:AM38)*($AG38:AM38=3)),MAX(COLUMN($AG38:AM38)*($AG38:AM38=1))>MAX(COLUMN($AG38:AM38)*($AG38:AM38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AN38)-MAX(COLUMN($AG38:AM38)*($AG38:AM38=1))=$J38,3,0),IF(COLUMN(AN38)-MAX(COLUMN($AG38:AM38)*($AG38:AM38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AM38)*($AG38:AM38=2))>MAX(COLUMN($AG38:AM38)*($AG38:AM38=3)),MAX(COLUMN($AG38:AM38)*($AG38:AM38=2))>MAX(COLUMN($AG38:AM38)*($AG38:AM38=1))),IF(COLUMN(AN38)-MAX(COLUMN($AG38:AM38)*($AG38:AM38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AN38)-MAX(COLUMN($AG38:AM38)*($AG38:AM38=3))=$J38,3,0),IF(COLUMN(AN38)-MAX(COLUMN($AG38:AM38)*($AG38:AM38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AN38)*($AG38:AN38=1))>MAX(COLUMN($AG38:AN38)*($AG38:AN38=3)),MAX(COLUMN($AG38:AN38)*($AG38:AN38=1))>MAX(COLUMN($AG38:AN38)*($AG38:AN38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AO38)-MAX(COLUMN($AG38:AN38)*($AG38:AN38=1))=$J38,3,0),IF(COLUMN(AO38)-MAX(COLUMN($AG38:AN38)*($AG38:AN38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AN38)*($AG38:AN38=2))>MAX(COLUMN($AG38:AN38)*($AG38:AN38=3)),MAX(COLUMN($AG38:AN38)*($AG38:AN38=2))>MAX(COLUMN($AG38:AN38)*($AG38:AN38=1))),IF(COLUMN(AO38)-MAX(COLUMN($AG38:AN38)*($AG38:AN38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AO38)-MAX(COLUMN($AG38:AN38)*($AG38:AN38=3))=$J38,3,0),IF(COLUMN(AO38)-MAX(COLUMN($AG38:AN38)*($AG38:AN38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AO38)*($AG38:AO38=1))>MAX(COLUMN($AG38:AO38)*($AG38:AO38=3)),MAX(COLUMN($AG38:AO38)*($AG38:AO38=1))>MAX(COLUMN($AG38:AO38)*($AG38:AO38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AP38)-MAX(COLUMN($AG38:AO38)*($AG38:AO38=1))=$J38,3,0),IF(COLUMN(AP38)-MAX(COLUMN($AG38:AO38)*($AG38:AO38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AO38)*($AG38:AO38=2))>MAX(COLUMN($AG38:AO38)*($AG38:AO38=3)),MAX(COLUMN($AG38:AO38)*($AG38:AO38=2))>MAX(COLUMN($AG38:AO38)*($AG38:AO38=1))),IF(COLUMN(AP38)-MAX(COLUMN($AG38:AO38)*($AG38:AO38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AP38)-MAX(COLUMN($AG38:AO38)*($AG38:AO38=3))=$J38,3,0),IF(COLUMN(AP38)-MAX(COLUMN($AG38:AO38)*($AG38:AO38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AP38)*($AG38:AP38=1))>MAX(COLUMN($AG38:AP38)*($AG38:AP38=3)),MAX(COLUMN($AG38:AP38)*($AG38:AP38=1))>MAX(COLUMN($AG38:AP38)*($AG38:AP38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AQ38)-MAX(COLUMN($AG38:AP38)*($AG38:AP38=1))=$J38,3,0),IF(COLUMN(AQ38)-MAX(COLUMN($AG38:AP38)*($AG38:AP38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AP38)*($AG38:AP38=2))>MAX(COLUMN($AG38:AP38)*($AG38:AP38=3)),MAX(COLUMN($AG38:AP38)*($AG38:AP38=2))>MAX(COLUMN($AG38:AP38)*($AG38:AP38=1))),IF(COLUMN(AQ38)-MAX(COLUMN($AG38:AP38)*($AG38:AP38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AQ38)-MAX(COLUMN($AG38:AP38)*($AG38:AP38=3))=$J38,3,0),IF(COLUMN(AQ38)-MAX(COLUMN($AG38:AP38)*($AG38:AP38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=1))>MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=3)),MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=1))>MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AR38)-MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=1))=$J38,3,0),IF(COLUMN(AR38)-MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=2))>MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=3)),MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=2))>MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=1))),IF(COLUMN(AR38)-MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AR38)-MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=3))=$J38,3,0),IF(COLUMN(AR38)-MAX(COLUMN($AG38:AQ38)*($AG38:AQ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AR38)*($AG38:AR38=1))>MAX(COLUMN($AG38:AR38)*($AG38:AR38=3)),MAX(COLUMN($AG38:AR38)*($AG38:AR38=1))>MAX(COLUMN($AG38:AR38)*($AG38:AR38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AS38)-MAX(COLUMN($AG38:AR38)*($AG38:AR38=1))=$J38,3,0),IF(COLUMN(AS38)-MAX(COLUMN($AG38:AR38)*($AG38:AR38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AR38)*($AG38:AR38=2))>MAX(COLUMN($AG38:AR38)*($AG38:AR38=3)),MAX(COLUMN($AG38:AR38)*($AG38:AR38=2))>MAX(COLUMN($AG38:AR38)*($AG38:AR38=1))),IF(COLUMN(AS38)-MAX(COLUMN($AG38:AR38)*($AG38:AR38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AS38)-MAX(COLUMN($AG38:AR38)*($AG38:AR38=3))=$J38,3,0),IF(COLUMN(AS38)-MAX(COLUMN($AG38:AR38)*($AG38:AR38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AS38)*($AG38:AS38=1))>MAX(COLUMN($AG38:AS38)*($AG38:AS38=3)),MAX(COLUMN($AG38:AS38)*($AG38:AS38=1))>MAX(COLUMN($AG38:AS38)*($AG38:AS38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AT38)-MAX(COLUMN($AG38:AS38)*($AG38:AS38=1))=$J38,3,0),IF(COLUMN(AT38)-MAX(COLUMN($AG38:AS38)*($AG38:AS38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AS38)*($AG38:AS38=2))>MAX(COLUMN($AG38:AS38)*($AG38:AS38=3)),MAX(COLUMN($AG38:AS38)*($AG38:AS38=2))>MAX(COLUMN($AG38:AS38)*($AG38:AS38=1))),IF(COLUMN(AT38)-MAX(COLUMN($AG38:AS38)*($AG38:AS38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AT38)-MAX(COLUMN($AG38:AS38)*($AG38:AS38=3))=$J38,3,0),IF(COLUMN(AT38)-MAX(COLUMN($AG38:AS38)*($AG38:AS38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AT38)*($AG38:AT38=1))>MAX(COLUMN($AG38:AT38)*($AG38:AT38=3)),MAX(COLUMN($AG38:AT38)*($AG38:AT38=1))>MAX(COLUMN($AG38:AT38)*($AG38:AT38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AU38)-MAX(COLUMN($AG38:AT38)*($AG38:AT38=1))=$J38,3,0),IF(COLUMN(AU38)-MAX(COLUMN($AG38:AT38)*($AG38:AT38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AT38)*($AG38:AT38=2))>MAX(COLUMN($AG38:AT38)*($AG38:AT38=3)),MAX(COLUMN($AG38:AT38)*($AG38:AT38=2))>MAX(COLUMN($AG38:AT38)*($AG38:AT38=1))),IF(COLUMN(AU38)-MAX(COLUMN($AG38:AT38)*($AG38:AT38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AU38)-MAX(COLUMN($AG38:AT38)*($AG38:AT38=3))=$J38,3,0),IF(COLUMN(AU38)-MAX(COLUMN($AG38:AT38)*($AG38:AT38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AU38)*($AG38:AU38=1))>MAX(COLUMN($AG38:AU38)*($AG38:AU38=3)),MAX(COLUMN($AG38:AU38)*($AG38:AU38=1))>MAX(COLUMN($AG38:AU38)*($AG38:AU38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AV38)-MAX(COLUMN($AG38:AU38)*($AG38:AU38=1))=$J38,3,0),IF(COLUMN(AV38)-MAX(COLUMN($AG38:AU38)*($AG38:AU38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AU38)*($AG38:AU38=2))>MAX(COLUMN($AG38:AU38)*($AG38:AU38=3)),MAX(COLUMN($AG38:AU38)*($AG38:AU38=2))>MAX(COLUMN($AG38:AU38)*($AG38:AU38=1))),IF(COLUMN(AV38)-MAX(COLUMN($AG38:AU38)*($AG38:AU38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AV38)-MAX(COLUMN($AG38:AU38)*($AG38:AU38=3))=$J38,3,0),IF(COLUMN(AV38)-MAX(COLUMN($AG38:AU38)*($AG38:AU38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AV38)*($AG38:AV38=1))>MAX(COLUMN($AG38:AV38)*($AG38:AV38=3)),MAX(COLUMN($AG38:AV38)*($AG38:AV38=1))>MAX(COLUMN($AG38:AV38)*($AG38:AV38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AW38)-MAX(COLUMN($AG38:AV38)*($AG38:AV38=1))=$J38,3,0),IF(COLUMN(AW38)-MAX(COLUMN($AG38:AV38)*($AG38:AV38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AV38)*($AG38:AV38=2))>MAX(COLUMN($AG38:AV38)*($AG38:AV38=3)),MAX(COLUMN($AG38:AV38)*($AG38:AV38=2))>MAX(COLUMN($AG38:AV38)*($AG38:AV38=1))),IF(COLUMN(AW38)-MAX(COLUMN($AG38:AV38)*($AG38:AV38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AW38)-MAX(COLUMN($AG38:AV38)*($AG38:AV38=3))=$J38,3,0),IF(COLUMN(AW38)-MAX(COLUMN($AG38:AV38)*($AG38:AV38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AW38)*($AG38:AW38=1))>MAX(COLUMN($AG38:AW38)*($AG38:AW38=3)),MAX(COLUMN($AG38:AW38)*($AG38:AW38=1))>MAX(COLUMN($AG38:AW38)*($AG38:AW38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AX38)-MAX(COLUMN($AG38:AW38)*($AG38:AW38=1))=$J38,3,0),IF(COLUMN(AX38)-MAX(COLUMN($AG38:AW38)*($AG38:AW38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AW38)*($AG38:AW38=2))>MAX(COLUMN($AG38:AW38)*($AG38:AW38=3)),MAX(COLUMN($AG38:AW38)*($AG38:AW38=2))>MAX(COLUMN($AG38:AW38)*($AG38:AW38=1))),IF(COLUMN(AX38)-MAX(COLUMN($AG38:AW38)*($AG38:AW38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AX38)-MAX(COLUMN($AG38:AW38)*($AG38:AW38=3))=$J38,3,0),IF(COLUMN(AX38)-MAX(COLUMN($AG38:AW38)*($AG38:AW38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AX38)*($AG38:AX38=1))>MAX(COLUMN($AG38:AX38)*($AG38:AX38=3)),MAX(COLUMN($AG38:AX38)*($AG38:AX38=1))>MAX(COLUMN($AG38:AX38)*($AG38:AX38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AY38)-MAX(COLUMN($AG38:AX38)*($AG38:AX38=1))=$J38,3,0),IF(COLUMN(AY38)-MAX(COLUMN($AG38:AX38)*($AG38:AX38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AX38)*($AG38:AX38=2))>MAX(COLUMN($AG38:AX38)*($AG38:AX38=3)),MAX(COLUMN($AG38:AX38)*($AG38:AX38=2))>MAX(COLUMN($AG38:AX38)*($AG38:AX38=1))),IF(COLUMN(AY38)-MAX(COLUMN($AG38:AX38)*($AG38:AX38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AY38)-MAX(COLUMN($AG38:AX38)*($AG38:AX38=3))=$J38,3,0),IF(COLUMN(AY38)-MAX(COLUMN($AG38:AX38)*($AG38:AX38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AY38)*($AG38:AY38=1))>MAX(COLUMN($AG38:AY38)*($AG38:AY38=3)),MAX(COLUMN($AG38:AY38)*($AG38:AY38=1))>MAX(COLUMN($AG38:AY38)*($AG38:AY38=2))),IF($K38=\"Not Possible\",IF(COLUMN(AZ38)-MAX(COLUMN($AG38:AY38)*($AG38:AY38=1))=$J38,3,0),IF(COLUMN(AZ38)-MAX(COLUMN($AG38:AY38)*($AG38:AY38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AY38)*($AG38:AY38=2))>MAX(COLUMN($AG38:AY38)*($AG38:AY38=3)),MAX(COLUMN($AG38:AY38)*($AG38:AY38=2))>MAX(COLUMN($AG38:AY38)*($AG38:AY38=1))),IF(COLUMN(AZ38)-MAX(COLUMN($AG38:AY38)*($AG38:AY38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(AZ38)-MAX(COLUMN($AG38:AY38)*($AG38:AY38=3))=$J38,3,0),IF(COLUMN(AZ38)-MAX(COLUMN($AG38:AY38)*($AG38:AY38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=1))>MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=3)),MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=1))>MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BA38)-MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=1))=$J38,3,0),IF(COLUMN(BA38)-MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=2))>MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=3)),MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=2))>MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=1))),IF(COLUMN(BA38)-MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BA38)-MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=3))=$J38,3,0),IF(COLUMN(BA38)-MAX(COLUMN($AG38:AZ38)*($AG38:AZ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BA38)*($AG38:BA38=1))>MAX(COLUMN($AG38:BA38)*($AG38:BA38=3)),MAX(COLUMN($AG38:BA38)*($AG38:BA38=1))>MAX(COLUMN($AG38:BA38)*($AG38:BA38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BB38)-MAX(COLUMN($AG38:BA38)*($AG38:BA38=1))=$J38,3,0),IF(COLUMN(BB38)-MAX(COLUMN($AG38:BA38)*($AG38:BA38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BA38)*($AG38:BA38=2))>MAX(COLUMN($AG38:BA38)*($AG38:BA38=3)),MAX(COLUMN($AG38:BA38)*($AG38:BA38=2))>MAX(COLUMN($AG38:BA38)*($AG38:BA38=1))),IF(COLUMN(BB38)-MAX(COLUMN($AG38:BA38)*($AG38:BA38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BB38)-MAX(COLUMN($AG38:BA38)*($AG38:BA38=3))=$J38,3,0),IF(COLUMN(BB38)-MAX(COLUMN($AG38:BA38)*($AG38:BA38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BB38)*($AG38:BB38=1))>MAX(COLUMN($AG38:BB38)*($AG38:BB38=3)),MAX(COLUMN($AG38:BB38)*($AG38:BB38=1))>MAX(COLUMN($AG38:BB38)*($AG38:BB38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BC38)-MAX(COLUMN($AG38:BB38)*($AG38:BB38=1))=$J38,3,0),IF(COLUMN(BC38)-MAX(COLUMN($AG38:BB38)*($AG38:BB38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BB38)*($AG38:BB38=2))>MAX(COLUMN($AG38:BB38)*($AG38:BB38=3)),MAX(COLUMN($AG38:BB38)*($AG38:BB38=2))>MAX(COLUMN($AG38:BB38)*($AG38:BB38=1))),IF(COLUMN(BC38)-MAX(COLUMN($AG38:BB38)*($AG38:BB38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BC38)-MAX(COLUMN($AG38:BB38)*($AG38:BB38=3))=$J38,3,0),IF(COLUMN(BC38)-MAX(COLUMN($AG38:BB38)*($AG38:BB38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BC38)*($AG38:BC38=1))>MAX(COLUMN($AG38:BC38)*($AG38:BC38=3)),MAX(COLUMN($AG38:BC38)*($AG38:BC38=1))>MAX(COLUMN($AG38:BC38)*($AG38:BC38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BD38)-MAX(COLUMN($AG38:BC38)*($AG38:BC38=1))=$J38,3,0),IF(COLUMN(BD38)-MAX(COLUMN($AG38:BC38)*($AG38:BC38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BC38)*($AG38:BC38=2))>MAX(COLUMN($AG38:BC38)*($AG38:BC38=3)),MAX(COLUMN($AG38:BC38)*($AG38:BC38=2))>MAX(COLUMN($AG38:BC38)*($AG38:BC38=1))),IF(COLUMN(BD38)-MAX(COLUMN($AG38:BC38)*($AG38:BC38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BD38)-MAX(COLUMN($AG38:BC38)*($AG38:BC38=3))=$J38,3,0),IF(COLUMN(BD38)-MAX(COLUMN($AG38:BC38)*($AG38:BC38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BD38)*($AG38:BD38=1))>MAX(COLUMN($AG38:BD38)*($AG38:BD38=3)),MAX(COLUMN($AG38:BD38)*($AG38:BD38=1))>MAX(COLUMN($AG38:BD38)*($AG38:BD38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BE38)-MAX(COLUMN($AG38:BD38)*($AG38:BD38=1))=$J38,3,0),IF(COLUMN(BE38)-MAX(COLUMN($AG38:BD38)*($AG38:BD38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BD38)*($AG38:BD38=2))>MAX(COLUMN($AG38:BD38)*($AG38:BD38=3)),MAX(COLUMN($AG38:BD38)*($AG38:BD38=2))>MAX(COLUMN($AG38:BD38)*($AG38:BD38=1))),IF(COLUMN(BE38)-MAX(COLUMN($AG38:BD38)*($AG38:BD38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BE38)-MAX(COLUMN($AG38:BD38)*($AG38:BD38=3))=$J38,3,0),IF(COLUMN(BE38)-MAX(COLUMN($AG38:BD38)*($AG38:BD38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BE38)*($AG38:BE38=1))>MAX(COLUMN($AG38:BE38)*($AG38:BE38=3)),MAX(COLUMN($AG38:BE38)*($AG38:BE38=1))>MAX(COLUMN($AG38:BE38)*($AG38:BE38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BF38)-MAX(COLUMN($AG38:BE38)*($AG38:BE38=1))=$J38,3,0),IF(COLUMN(BF38)-MAX(COLUMN($AG38:BE38)*($AG38:BE38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BE38)*($AG38:BE38=2))>MAX(COLUMN($AG38:BE38)*($AG38:BE38=3)),MAX(COLUMN($AG38:BE38)*($AG38:BE38=2))>MAX(COLUMN($AG38:BE38)*($AG38:BE38=1))),IF(COLUMN(BF38)-MAX(COLUMN($AG38:BE38)*($AG38:BE38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BF38)-MAX(COLUMN($AG38:BE38)*($AG38:BE38=3))=$J38,3,0),IF(COLUMN(BF38)-MAX(COLUMN($AG38:BE38)*($AG38:BE38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BF38)*($AG38:BF38=1))>MAX(COLUMN($AG38:BF38)*($AG38:BF38=3)),MAX(COLUMN($AG38:BF38)*($AG38:BF38=1))>MAX(COLUMN($AG38:BF38)*($AG38:BF38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BG38)-MAX(COLUMN($AG38:BF38)*($AG38:BF38=1))=$J38,3,0),IF(COLUMN(BG38)-MAX(COLUMN($AG38:BF38)*($AG38:BF38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BF38)*($AG38:BF38=2))>MAX(COLUMN($AG38:BF38)*($AG38:BF38=3)),MAX(COLUMN($AG38:BF38)*($AG38:BF38=2))>MAX(COLUMN($AG38:BF38)*($AG38:BF38=1))),IF(COLUMN(BG38)-MAX(COLUMN($AG38:BF38)*($AG38:BF38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BG38)-MAX(COLUMN($AG38:BF38)*($AG38:BF38=3))=$J38,3,0),IF(COLUMN(BG38)-MAX(COLUMN($AG38:BF38)*($AG38:BF38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BG38)*($AG38:BG38=1))>MAX(COLUMN($AG38:BG38)*($AG38:BG38=3)),MAX(COLUMN($AG38:BG38)*($AG38:BG38=1))>MAX(COLUMN($AG38:BG38)*($AG38:BG38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BH38)-MAX(COLUMN($AG38:BG38)*($AG38:BG38=1))=$J38,3,0),IF(COLUMN(BH38)-MAX(COLUMN($AG38:BG38)*($AG38:BG38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BG38)*($AG38:BG38=2))>MAX(COLUMN($AG38:BG38)*($AG38:BG38=3)),MAX(COLUMN($AG38:BG38)*($AG38:BG38=2))>MAX(COLUMN($AG38:BG38)*($AG38:BG38=1))),IF(COLUMN(BH38)-MAX(COLUMN($AG38:BG38)*($AG38:BG38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BH38)-MAX(COLUMN($AG38:BG38)*($AG38:BG38=3))=$J38,3,0),IF(COLUMN(BH38)-MAX(COLUMN($AG38:BG38)*($AG38:BG38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BH38)*($AG38:BH38=1))>MAX(COLUMN($AG38:BH38)*($AG38:BH38=3)),MAX(COLUMN($AG38:BH38)*($AG38:BH38=1))>MAX(COLUMN($AG38:BH38)*($AG38:BH38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BI38)-MAX(COLUMN($AG38:BH38)*($AG38:BH38=1))=$J38,3,0),IF(COLUMN(BI38)-MAX(COLUMN($AG38:BH38)*($AG38:BH38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BH38)*($AG38:BH38=2))>MAX(COLUMN($AG38:BH38)*($AG38:BH38=3)),MAX(COLUMN($AG38:BH38)*($AG38:BH38=2))>MAX(COLUMN($AG38:BH38)*($AG38:BH38=1))),IF(COLUMN(BI38)-MAX(COLUMN($AG38:BH38)*($AG38:BH38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BI38)-MAX(COLUMN($AG38:BH38)*($AG38:BH38=3))=$J38,3,0),IF(COLUMN(BI38)-MAX(COLUMN($AG38:BH38)*($AG38:BH38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BI38)*($AG38:BI38=1))>MAX(COLUMN($AG38:BI38)*($AG38:BI38=3)),MAX(COLUMN($AG38:BI38)*($AG38:BI38=1))>MAX(COLUMN($AG38:BI38)*($AG38:BI38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BJ38)-MAX(COLUMN($AG38:BI38)*($AG38:BI38=1))=$J38,3,0),IF(COLUMN(BJ38)-MAX(COLUMN($AG38:BI38)*($AG38:BI38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BI38)*($AG38:BI38=2))>MAX(COLUMN($AG38:BI38)*($AG38:BI38=3)),MAX(COLUMN($AG38:BI38)*($AG38:BI38=2))>MAX(COLUMN($AG38:BI38)*($AG38:BI38=1))),IF(COLUMN(BJ38)-MAX(COLUMN($AG38:BI38)*($AG38:BI38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BJ38)-MAX(COLUMN($AG38:BI38)*($AG38:BI38=3))=$J38,3,0),IF(COLUMN(BJ38)-MAX(COLUMN($AG38:BI38)*($AG38:BI38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=1))>MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=3)),MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=1))>MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BK38)-MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=1))=$J38,3,0),IF(COLUMN(BK38)-MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=2))>MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=3)),MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=2))>MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=1))),IF(COLUMN(BK38)-MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BK38)-MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=3))=$J38,3,0),IF(COLUMN(BK38)-MAX(COLUMN($AG38:BJ38)*($AG38:BJ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BK38)*($AG38:BK38=1))>MAX(COLUMN($AG38:BK38)*($AG38:BK38=3)),MAX(COLUMN($AG38:BK38)*($AG38:BK38=1))>MAX(COLUMN($AG38:BK38)*($AG38:BK38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BL38)-MAX(COLUMN($AG38:BK38)*($AG38:BK38=1))=$J38,3,0),IF(COLUMN(BL38)-MAX(COLUMN($AG38:BK38)*($AG38:BK38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BK38)*($AG38:BK38=2))>MAX(COLUMN($AG38:BK38)*($AG38:BK38=3)),MAX(COLUMN($AG38:BK38)*($AG38:BK38=2))>MAX(COLUMN($AG38:BK38)*($AG38:BK38=1))),IF(COLUMN(BL38)-MAX(COLUMN($AG38:BK38)*($AG38:BK38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BL38)-MAX(COLUMN($AG38:BK38)*($AG38:BK38=3))=$J38,3,0),IF(COLUMN(BL38)-MAX(COLUMN($AG38:BK38)*($AG38:BK38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BL38)*($AG38:BL38=1))>MAX(COLUMN($AG38:BL38)*($AG38:BL38=3)),MAX(COLUMN($AG38:BL38)*($AG38:BL38=1))>MAX(COLUMN($AG38:BL38)*($AG38:BL38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BM38)-MAX(COLUMN($AG38:BL38)*($AG38:BL38=1))=$J38,3,0),IF(COLUMN(BM38)-MAX(COLUMN($AG38:BL38)*($AG38:BL38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BL38)*($AG38:BL38=2))>MAX(COLUMN($AG38:BL38)*($AG38:BL38=3)),MAX(COLUMN($AG38:BL38)*($AG38:BL38=2))>MAX(COLUMN($AG38:BL38)*($AG38:BL38=1))),IF(COLUMN(BM38)-MAX(COLUMN($AG38:BL38)*($AG38:BL38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BM38)-MAX(COLUMN($AG38:BL38)*($AG38:BL38=3))=$J38,3,0),IF(COLUMN(BM38)-MAX(COLUMN($AG38:BL38)*($AG38:BL38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BM38)*($AG38:BM38=1))>MAX(COLUMN($AG38:BM38)*($AG38:BM38=3)),MAX(COLUMN($AG38:BM38)*($AG38:BM38=1))>MAX(COLUMN($AG38:BM38)*($AG38:BM38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BN38)-MAX(COLUMN($AG38:BM38)*($AG38:BM38=1))=$J38,3,0),IF(COLUMN(BN38)-MAX(COLUMN($AG38:BM38)*($AG38:BM38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BM38)*($AG38:BM38=2))>MAX(COLUMN($AG38:BM38)*($AG38:BM38=3)),MAX(COLUMN($AG38:BM38)*($AG38:BM38=2))>MAX(COLUMN($AG38:BM38)*($AG38:BM38=1))),IF(COLUMN(BN38)-MAX(COLUMN($AG38:BM38)*($AG38:BM38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BN38)-MAX(COLUMN($AG38:BM38)*($AG38:BM38=3))=$J38,3,0),IF(COLUMN(BN38)-MAX(COLUMN($AG38:BM38)*($AG38:BM38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BN38)*($AG38:BN38=1))>MAX(COLUMN($AG38:BN38)*($AG38:BN38=3)),MAX(COLUMN($AG38:BN38)*($AG38:BN38=1))>MAX(COLUMN($AG38:BN38)*($AG38:BN38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BO38)-MAX(COLUMN($AG38:BN38)*($AG38:BN38=1))=$J38,3,0),IF(COLUMN(BO38)-MAX(COLUMN($AG38:BN38)*($AG38:BN38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BN38)*($AG38:BN38=2))>MAX(COLUMN($AG38:BN38)*($AG38:BN38=3)),MAX(COLUMN($AG38:BN38)*($AG38:BN38=2))>MAX(COLUMN($AG38:BN38)*($AG38:BN38=1))),IF(COLUMN(BO38)-MAX(COLUMN($AG38:BN38)*($AG38:BN38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BO38)-MAX(COLUMN($AG38:BN38)*($AG38:BN38=3))=$J38,3,0),IF(COLUMN(BO38)-MAX(COLUMN($AG38:BN38)*($AG38:BN38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BO38)*($AG38:BO38=1))>MAX(COLUMN($AG38:BO38)*($AG38:BO38=3)),MAX(COLUMN($AG38:BO38)*($AG38:BO38=1))>MAX(COLUMN($AG38:BO38)*($AG38:BO38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BP38)-MAX(COLUMN($AG38:BO38)*($AG38:BO38=1))=$J38,3,0),IF(COLUMN(BP38)-MAX(COLUMN($AG38:BO38)*($AG38:BO38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BO38)*($AG38:BO38=2))>MAX(COLUMN($AG38:BO38)*($AG38:BO38=3)),MAX(COLUMN($AG38:BO38)*($AG38:BO38=2))>MAX(COLUMN($AG38:BO38)*($AG38:BO38=1))),IF(COLUMN(BP38)-MAX(COLUMN($AG38:BO38)*($AG38:BO38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BP38)-MAX(COLUMN($AG38:BO38)*($AG38:BO38=3))=$J38,3,0),IF(COLUMN(BP38)-MAX(COLUMN($AG38:BO38)*($AG38:BO38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BP38)*($AG38:BP38=1))>MAX(COLUMN($AG38:BP38)*($AG38:BP38=3)),MAX(COLUMN($AG38:BP38)*($AG38:BP38=1))>MAX(COLUMN($AG38:BP38)*($AG38:BP38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BQ38)-MAX(COLUMN($AG38:BP38)*($AG38:BP38=1))=$J38,3,0),IF(COLUMN(BQ38)-MAX(COLUMN($AG38:BP38)*($AG38:BP38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BP38)*($AG38:BP38=2))>MAX(COLUMN($AG38:BP38)*($AG38:BP38=3)),MAX(COLUMN($AG38:BP38)*($AG38:BP38=2))>MAX(COLUMN($AG38:BP38)*($AG38:BP38=1))),IF(COLUMN(BQ38)-MAX(COLUMN($AG38:BP38)*($AG38:BP38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BQ38)-MAX(COLUMN($AG38:BP38)*($AG38:BP38=3))=$J38,3,0),IF(COLUMN(BQ38)-MAX(COLUMN($AG38:BP38)*($AG38:BP38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=1))>MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=3)),MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=1))>MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BR38)-MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=1))=$J38,3,0),IF(COLUMN(BR38)-MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=2))>MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=3)),MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=2))>MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=1))),IF(COLUMN(BR38)-MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BR38)-MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=3))=$J38,3,0),IF(COLUMN(BR38)-MAX(COLUMN($AG38:BQ38)*($AG38:BQ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BR38)*($AG38:BR38=1))>MAX(COLUMN($AG38:BR38)*($AG38:BR38=3)),MAX(COLUMN($AG38:BR38)*($AG38:BR38=1))>MAX(COLUMN($AG38:BR38)*($AG38:BR38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BS38)-MAX(COLUMN($AG38:BR38)*($AG38:BR38=1))=$J38,3,0),IF(COLUMN(BS38)-MAX(COLUMN($AG38:BR38)*($AG38:BR38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BR38)*($AG38:BR38=2))>MAX(COLUMN($AG38:BR38)*($AG38:BR38=3)),MAX(COLUMN($AG38:BR38)*($AG38:BR38=2))>MAX(COLUMN($AG38:BR38)*($AG38:BR38=1))),IF(COLUMN(BS38)-MAX(COLUMN($AG38:BR38)*($AG38:BR38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BS38)-MAX(COLUMN($AG38:BR38)*($AG38:BR38=3))=$J38,3,0),IF(COLUMN(BS38)-MAX(COLUMN($AG38:BR38)*($AG38:BR38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BS38)*($AG38:BS38=1))>MAX(COLUMN($AG38:BS38)*($AG38:BS38=3)),MAX(COLUMN($AG38:BS38)*($AG38:BS38=1))>MAX(COLUMN($AG38:BS38)*($AG38:BS38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BT38)-MAX(COLUMN($AG38:BS38)*($AG38:BS38=1))=$J38,3,0),IF(COLUMN(BT38)-MAX(COLUMN($AG38:BS38)*($AG38:BS38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BS38)*($AG38:BS38=2))>MAX(COLUMN($AG38:BS38)*($AG38:BS38=3)),MAX(COLUMN($AG38:BS38)*($AG38:BS38=2))>MAX(COLUMN($AG38:BS38)*($AG38:BS38=1))),IF(COLUMN(BT38)-MAX(COLUMN($AG38:BS38)*($AG38:BS38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BT38)-MAX(COLUMN($AG38:BS38)*($AG38:BS38=3))=$J38,3,0),IF(COLUMN(BT38)-MAX(COLUMN($AG38:BS38)*($AG38:BS38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BT38)*($AG38:BT38=1))>MAX(COLUMN($AG38:BT38)*($AG38:BT38=3)),MAX(COLUMN($AG38:BT38)*($AG38:BT38=1))>MAX(COLUMN($AG38:BT38)*($AG38:BT38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BU38)-MAX(COLUMN($AG38:BT38)*($AG38:BT38=1))=$J38,3,0),IF(COLUMN(BU38)-MAX(COLUMN($AG38:BT38)*($AG38:BT38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BT38)*($AG38:BT38=2))>MAX(COLUMN($AG38:BT38)*($AG38:BT38=3)),MAX(COLUMN($AG38:BT38)*($AG38:BT38=2))>MAX(COLUMN($AG38:BT38)*($AG38:BT38=1))),IF(COLUMN(BU38)-MAX(COLUMN($AG38:BT38)*($AG38:BT38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BU38)-MAX(COLUMN($AG38:BT38)*($AG38:BT38=3))=$J38,3,0),IF(COLUMN(BU38)-MAX(COLUMN($AG38:BT38)*($AG38:BT38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BU38)*($AG38:BU38=1))>MAX(COLUMN($AG38:BU38)*($AG38:BU38=3)),MAX(COLUMN($AG38:BU38)*($AG38:BU38=1))>MAX(COLUMN($AG38:BU38)*($AG38:BU38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BV38)-MAX(COLUMN($AG38:BU38)*($AG38:BU38=1))=$J38,3,0),IF(COLUMN(BV38)-MAX(COLUMN($AG38:BU38)*($AG38:BU38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BU38)*($AG38:BU38=2))>MAX(COLUMN($AG38:BU38)*($AG38:BU38=3)),MAX(COLUMN($AG38:BU38)*($AG38:BU38=2))>MAX(COLUMN($AG38:BU38)*($AG38:BU38=1))),IF(COLUMN(BV38)-MAX(COLUMN($AG38:BU38)*($AG38:BU38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BV38)-MAX(COLUMN($AG38:BU38)*($AG38:BU38=3))=$J38,3,0),IF(COLUMN(BV38)-MAX(COLUMN($AG38:BU38)*($AG38:BU38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BV38)*($AG38:BV38=1))>MAX(COLUMN($AG38:BV38)*($AG38:BV38=3)),MAX(COLUMN($AG38:BV38)*($AG38:BV38=1))>MAX(COLUMN($AG38:BV38)*($AG38:BV38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BW38)-MAX(COLUMN($AG38:BV38)*($AG38:BV38=1))=$J38,3,0),IF(COLUMN(BW38)-MAX(COLUMN($AG38:BV38)*($AG38:BV38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BV38)*($AG38:BV38=2))>MAX(COLUMN($AG38:BV38)*($AG38:BV38=3)),MAX(COLUMN($AG38:BV38)*($AG38:BV38=2))>MAX(COLUMN($AG38:BV38)*($AG38:BV38=1))),IF(COLUMN(BW38)-MAX(COLUMN($AG38:BV38)*($AG38:BV38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BW38)-MAX(COLUMN($AG38:BV38)*($AG38:BV38=3))=$J38,3,0),IF(COLUMN(BW38)-MAX(COLUMN($AG38:BV38)*($AG38:BV38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BW38)*($AG38:BW38=1))>MAX(COLUMN($AG38:BW38)*($AG38:BW38=3)),MAX(COLUMN($AG38:BW38)*($AG38:BW38=1))>MAX(COLUMN($AG38:BW38)*($AG38:BW38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BX38)-MAX(COLUMN($AG38:BW38)*($AG38:BW38=1))=$J38,3,0),IF(COLUMN(BX38)-MAX(COLUMN($AG38:BW38)*($AG38:BW38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BW38)*($AG38:BW38=2))>MAX(COLUMN($AG38:BW38)*($AG38:BW38=3)),MAX(COLUMN($AG38:BW38)*($AG38:BW38=2))>MAX(COLUMN($AG38:BW38)*($AG38:BW38=1))),IF(COLUMN(BX38)-MAX(COLUMN($AG38:BW38)*($AG38:BW38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BX38)-MAX(COLUMN($AG38:BW38)*($AG38:BW38=3))=$J38,3,0),IF(COLUMN(BX38)-MAX(COLUMN($AG38:BW38)*($AG38:BW38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BX38)*($AG38:BX38=1))>MAX(COLUMN($AG38:BX38)*($AG38:BX38=3)),MAX(COLUMN($AG38:BX38)*($AG38:BX38=1))>MAX(COLUMN($AG38:BX38)*($AG38:BX38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BY38)-MAX(COLUMN($AG38:BX38)*($AG38:BX38=1))=$J38,3,0),IF(COLUMN(BY38)-MAX(COLUMN($AG38:BX38)*($AG38:BX38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BX38)*($AG38:BX38=2))>MAX(COLUMN($AG38:BX38)*($AG38:BX38=3)),MAX(COLUMN($AG38:BX38)*($AG38:BX38=2))>MAX(COLUMN($AG38:BX38)*($AG38:BX38=1))),IF(COLUMN(BY38)-MAX(COLUMN($AG38:BX38)*($AG38:BX38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BY38)-MAX(COLUMN($AG38:BX38)*($AG38:BX38=3))=$J38,3,0),IF(COLUMN(BY38)-MAX(COLUMN($AG38:BX38)*($AG38:BX38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BY38)*($AG38:BY38=1))>MAX(COLUMN($AG38:BY38)*($AG38:BY38=3)),MAX(COLUMN($AG38:BY38)*($AG38:BY38=1))>MAX(COLUMN($AG38:BY38)*($AG38:BY38=2))),IF($K38=\"Not Possible\",IF(COLUMN(BZ38)-MAX(COLUMN($AG38:BY38)*($AG38:BY38=1))=$J38,3,0),IF(COLUMN(BZ38)-MAX(COLUMN($AG38:BY38)*($AG38:BY38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BY38)*($AG38:BY38=2))>MAX(COLUMN($AG38:BY38)*($AG38:BY38=3)),MAX(COLUMN($AG38:BY38)*($AG38:BY38=2))>MAX(COLUMN($AG38:BY38)*($AG38:BY38=1))),IF(COLUMN(BZ38)-MAX(COLUMN($AG38:BY38)*($AG38:BY38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(BZ38)-MAX(COLUMN($AG38:BY38)*($AG38:BY38=3))=$J38,3,0),IF(COLUMN(BZ38)-MAX(COLUMN($AG38:BY38)*($AG38:BY38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=1))>MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=3)),MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=1))>MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CA38)-MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=1))=$J38,3,0),IF(COLUMN(CA38)-MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=2))>MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=3)),MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=2))>MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=1))),IF(COLUMN(CA38)-MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CA38)-MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=3))=$J38,3,0),IF(COLUMN(CA38)-MAX(COLUMN($AG38:BZ38)*($AG38:BZ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CA38)*($AG38:CA38=1))>MAX(COLUMN($AG38:CA38)*($AG38:CA38=3)),MAX(COLUMN($AG38:CA38)*($AG38:CA38=1))>MAX(COLUMN($AG38:CA38)*($AG38:CA38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CB38)-MAX(COLUMN($AG38:CA38)*($AG38:CA38=1))=$J38,3,0),IF(COLUMN(CB38)-MAX(COLUMN($AG38:CA38)*($AG38:CA38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CA38)*($AG38:CA38=2))>MAX(COLUMN($AG38:CA38)*($AG38:CA38=3)),MAX(COLUMN($AG38:CA38)*($AG38:CA38=2))>MAX(COLUMN($AG38:CA38)*($AG38:CA38=1))),IF(COLUMN(CB38)-MAX(COLUMN($AG38:CA38)*($AG38:CA38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CB38)-MAX(COLUMN($AG38:CA38)*($AG38:CA38=3))=$J38,3,0),IF(COLUMN(CB38)-MAX(COLUMN($AG38:CA38)*($AG38:CA38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CB38)*($AG38:CB38=1))>MAX(COLUMN($AG38:CB38)*($AG38:CB38=3)),MAX(COLUMN($AG38:CB38)*($AG38:CB38=1))>MAX(COLUMN($AG38:CB38)*($AG38:CB38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CC38)-MAX(COLUMN($AG38:CB38)*($AG38:CB38=1))=$J38,3,0),IF(COLUMN(CC38)-MAX(COLUMN($AG38:CB38)*($AG38:CB38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CB38)*($AG38:CB38=2))>MAX(COLUMN($AG38:CB38)*($AG38:CB38=3)),MAX(COLUMN($AG38:CB38)*($AG38:CB38=2))>MAX(COLUMN($AG38:CB38)*($AG38:CB38=1))),IF(COLUMN(CC38)-MAX(COLUMN($AG38:CB38)*($AG38:CB38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CC38)-MAX(COLUMN($AG38:CB38)*($AG38:CB38=3))=$J38,3,0),IF(COLUMN(CC38)-MAX(COLUMN($AG38:CB38)*($AG38:CB38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CC38)*($AG38:CC38=1))>MAX(COLUMN($AG38:CC38)*($AG38:CC38=3)),MAX(COLUMN($AG38:CC38)*($AG38:CC38=1))>MAX(COLUMN($AG38:CC38)*($AG38:CC38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CD38)-MAX(COLUMN($AG38:CC38)*($AG38:CC38=1))=$J38,3,0),IF(COLUMN(CD38)-MAX(COLUMN($AG38:CC38)*($AG38:CC38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CC38)*($AG38:CC38=2))>MAX(COLUMN($AG38:CC38)*($AG38:CC38=3)),MAX(COLUMN($AG38:CC38)*($AG38:CC38=2))>MAX(COLUMN($AG38:CC38)*($AG38:CC38=1))),IF(COLUMN(CD38)-MAX(COLUMN($AG38:CC38)*($AG38:CC38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CD38)-MAX(COLUMN($AG38:CC38)*($AG38:CC38=3))=$J38,3,0),IF(COLUMN(CD38)-MAX(COLUMN($AG38:CC38)*($AG38:CC38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CD38)*($AG38:CD38=1))>MAX(COLUMN($AG38:CD38)*($AG38:CD38=3)),MAX(COLUMN($AG38:CD38)*($AG38:CD38=1))>MAX(COLUMN($AG38:CD38)*($AG38:CD38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CE38)-MAX(COLUMN($AG38:CD38)*($AG38:CD38=1))=$J38,3,0),IF(COLUMN(CE38)-MAX(COLUMN($AG38:CD38)*($AG38:CD38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CD38)*($AG38:CD38=2))>MAX(COLUMN($AG38:CD38)*($AG38:CD38=3)),MAX(COLUMN($AG38:CD38)*($AG38:CD38=2))>MAX(COLUMN($AG38:CD38)*($AG38:CD38=1))),IF(COLUMN(CE38)-MAX(COLUMN($AG38:CD38)*($AG38:CD38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CE38)-MAX(COLUMN($AG38:CD38)*($AG38:CD38=3))=$J38,3,0),IF(COLUMN(CE38)-MAX(COLUMN($AG38:CD38)*($AG38:CD38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CE38)*($AG38:CE38=1))>MAX(COLUMN($AG38:CE38)*($AG38:CE38=3)),MAX(COLUMN($AG38:CE38)*($AG38:CE38=1))>MAX(COLUMN($AG38:CE38)*($AG38:CE38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CF38)-MAX(COLUMN($AG38:CE38)*($AG38:CE38=1))=$J38,3,0),IF(COLUMN(CF38)-MAX(COLUMN($AG38:CE38)*($AG38:CE38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CE38)*($AG38:CE38=2))>MAX(COLUMN($AG38:CE38)*($AG38:CE38=3)),MAX(COLUMN($AG38:CE38)*($AG38:CE38=2))>MAX(COLUMN($AG38:CE38)*($AG38:CE38=1))),IF(COLUMN(CF38)-MAX(COLUMN($AG38:CE38)*($AG38:CE38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CF38)-MAX(COLUMN($AG38:CE38)*($AG38:CE38=3))=$J38,3,0),IF(COLUMN(CF38)-MAX(COLUMN($AG38:CE38)*($AG38:CE38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CF38)*($AG38:CF38=1))>MAX(COLUMN($AG38:CF38)*($AG38:CF38=3)),MAX(COLUMN($AG38:CF38)*($AG38:CF38=1))>MAX(COLUMN($AG38:CF38)*($AG38:CF38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CG38)-MAX(COLUMN($AG38:CF38)*($AG38:CF38=1))=$J38,3,0),IF(COLUMN(CG38)-MAX(COLUMN($AG38:CF38)*($AG38:CF38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CF38)*($AG38:CF38=2))>MAX(COLUMN($AG38:CF38)*($AG38:CF38=3)),MAX(COLUMN($AG38:CF38)*($AG38:CF38=2))>MAX(COLUMN($AG38:CF38)*($AG38:CF38=1))),IF(COLUMN(CG38)-MAX(COLUMN($AG38:CF38)*($AG38:CF38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CG38)-MAX(COLUMN($AG38:CF38)*($AG38:CF38=3))=$J38,3,0),IF(COLUMN(CG38)-MAX(COLUMN($AG38:CF38)*($AG38:CF38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CG38)*($AG38:CG38=1))>MAX(COLUMN($AG38:CG38)*($AG38:CG38=3)),MAX(COLUMN($AG38:CG38)*($AG38:CG38=1))>MAX(COLUMN($AG38:CG38)*($AG38:CG38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CH38)-MAX(COLUMN($AG38:CG38)*($AG38:CG38=1))=$J38,3,0),IF(COLUMN(CH38)-MAX(COLUMN($AG38:CG38)*($AG38:CG38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CG38)*($AG38:CG38=2))>MAX(COLUMN($AG38:CG38)*($AG38:CG38=3)),MAX(COLUMN($AG38:CG38)*($AG38:CG38=2))>MAX(COLUMN($AG38:CG38)*($AG38:CG38=1))),IF(COLUMN(CH38)-MAX(COLUMN($AG38:CG38)*($AG38:CG38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CH38)-MAX(COLUMN($AG38:CG38)*($AG38:CG38=3))=$J38,3,0),IF(COLUMN(CH38)-MAX(COLUMN($AG38:CG38)*($AG38:CG38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CH38)*($AG38:CH38=1))>MAX(COLUMN($AG38:CH38)*($AG38:CH38=3)),MAX(COLUMN($AG38:CH38)*($AG38:CH38=1))>MAX(COLUMN($AG38:CH38)*($AG38:CH38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CI38)-MAX(COLUMN($AG38:CH38)*($AG38:CH38=1))=$J38,3,0),IF(COLUMN(CI38)-MAX(COLUMN($AG38:CH38)*($AG38:CH38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CH38)*($AG38:CH38=2))>MAX(COLUMN($AG38:CH38)*($AG38:CH38=3)),MAX(COLUMN($AG38:CH38)*($AG38:CH38=2))>MAX(COLUMN($AG38:CH38)*($AG38:CH38=1))),IF(COLUMN(CI38)-MAX(COLUMN($AG38:CH38)*($AG38:CH38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CI38)-MAX(COLUMN($AG38:CH38)*($AG38:CH38=3))=$J38,3,0),IF(COLUMN(CI38)-MAX(COLUMN($AG38:CH38)*($AG38:CH38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CI38)*($AG38:CI38=1))>MAX(COLUMN($AG38:CI38)*($AG38:CI38=3)),MAX(COLUMN($AG38:CI38)*($AG38:CI38=1))>MAX(COLUMN($AG38:CI38)*($AG38:CI38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CJ38)-MAX(COLUMN($AG38:CI38)*($AG38:CI38=1))=$J38,3,0),IF(COLUMN(CJ38)-MAX(COLUMN($AG38:CI38)*($AG38:CI38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CI38)*($AG38:CI38=2))>MAX(COLUMN($AG38:CI38)*($AG38:CI38=3)),MAX(COLUMN($AG38:CI38)*($AG38:CI38=2))>MAX(COLUMN($AG38:CI38)*($AG38:CI38=1))),IF(COLUMN(CJ38)-MAX(COLUMN($AG38:CI38)*($AG38:CI38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CJ38)-MAX(COLUMN($AG38:CI38)*($AG38:CI38=3))=$J38,3,0),IF(COLUMN(CJ38)-MAX(COLUMN($AG38:CI38)*($AG38:CI38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=1))>MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=3)),MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=1))>MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CK38)-MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=1))=$J38,3,0),IF(COLUMN(CK38)-MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=2))>MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=3)),MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=2))>MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=1))),IF(COLUMN(CK38)-MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CK38)-MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=3))=$J38,3,0),IF(COLUMN(CK38)-MAX(COLUMN($AG38:CJ38)*($AG38:CJ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CK38)*($AG38:CK38=1))>MAX(COLUMN($AG38:CK38)*($AG38:CK38=3)),MAX(COLUMN($AG38:CK38)*($AG38:CK38=1))>MAX(COLUMN($AG38:CK38)*($AG38:CK38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CL38)-MAX(COLUMN($AG38:CK38)*($AG38:CK38=1))=$J38,3,0),IF(COLUMN(CL38)-MAX(COLUMN($AG38:CK38)*($AG38:CK38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CK38)*($AG38:CK38=2))>MAX(COLUMN($AG38:CK38)*($AG38:CK38=3)),MAX(COLUMN($AG38:CK38)*($AG38:CK38=2))>MAX(COLUMN($AG38:CK38)*($AG38:CK38=1))),IF(COLUMN(CL38)-MAX(COLUMN($AG38:CK38)*($AG38:CK38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CL38)-MAX(COLUMN($AG38:CK38)*($AG38:CK38=3))=$J38,3,0),IF(COLUMN(CL38)-MAX(COLUMN($AG38:CK38)*($AG38:CK38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CL38)*($AG38:CL38=1))>MAX(COLUMN($AG38:CL38)*($AG38:CL38=3)),MAX(COLUMN($AG38:CL38)*($AG38:CL38=1))>MAX(COLUMN($AG38:CL38)*($AG38:CL38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CM38)-MAX(COLUMN($AG38:CL38)*($AG38:CL38=1))=$J38,3,0),IF(COLUMN(CM38)-MAX(COLUMN($AG38:CL38)*($AG38:CL38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CL38)*($AG38:CL38=2))>MAX(COLUMN($AG38:CL38)*($AG38:CL38=3)),MAX(COLUMN($AG38:CL38)*($AG38:CL38=2))>MAX(COLUMN($AG38:CL38)*($AG38:CL38=1))),IF(COLUMN(CM38)-MAX(COLUMN($AG38:CL38)*($AG38:CL38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CM38)-MAX(COLUMN($AG38:CL38)*($AG38:CL38=3))=$J38,3,0),IF(COLUMN(CM38)-MAX(COLUMN($AG38:CL38)*($AG38:CL38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CM38)*($AG38:CM38=1))>MAX(COLUMN($AG38:CM38)*($AG38:CM38=3)),MAX(COLUMN($AG38:CM38)*($AG38:CM38=1))>MAX(COLUMN($AG38:CM38)*($AG38:CM38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CN38)-MAX(COLUMN($AG38:CM38)*($AG38:CM38=1))=$J38,3,0),IF(COLUMN(CN38)-MAX(COLUMN($AG38:CM38)*($AG38:CM38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CM38)*($AG38:CM38=2))>MAX(COLUMN($AG38:CM38)*($AG38:CM38=3)),MAX(COLUMN($AG38:CM38)*($AG38:CM38=2))>MAX(COLUMN($AG38:CM38)*($AG38:CM38=1))),IF(COLUMN(CN38)-MAX(COLUMN($AG38:CM38)*($AG38:CM38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CN38)-MAX(COLUMN($AG38:CM38)*($AG38:CM38=3))=$J38,3,0),IF(COLUMN(CN38)-MAX(COLUMN($AG38:CM38)*($AG38:CM38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CN38)*($AG38:CN38=1))>MAX(COLUMN($AG38:CN38)*($AG38:CN38=3)),MAX(COLUMN($AG38:CN38)*($AG38:CN38=1))>MAX(COLUMN($AG38:CN38)*($AG38:CN38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CO38)-MAX(COLUMN($AG38:CN38)*($AG38:CN38=1))=$J38,3,0),IF(COLUMN(CO38)-MAX(COLUMN($AG38:CN38)*($AG38:CN38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CN38)*($AG38:CN38=2))>MAX(COLUMN($AG38:CN38)*($AG38:CN38=3)),MAX(COLUMN($AG38:CN38)*($AG38:CN38=2))>MAX(COLUMN($AG38:CN38)*($AG38:CN38=1))),IF(COLUMN(CO38)-MAX(COLUMN($AG38:CN38)*($AG38:CN38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CO38)-MAX(COLUMN($AG38:CN38)*($AG38:CN38=3))=$J38,3,0),IF(COLUMN(CO38)-MAX(COLUMN($AG38:CN38)*($AG38:CN38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CO38)*($AG38:CO38=1))>MAX(COLUMN($AG38:CO38)*($AG38:CO38=3)),MAX(COLUMN($AG38:CO38)*($AG38:CO38=1))>MAX(COLUMN($AG38:CO38)*($AG38:CO38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CP38)-MAX(COLUMN($AG38:CO38)*($AG38:CO38=1))=$J38,3,0),IF(COLUMN(CP38)-MAX(COLUMN($AG38:CO38)*($AG38:CO38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CO38)*($AG38:CO38=2))>MAX(COLUMN($AG38:CO38)*($AG38:CO38=3)),MAX(COLUMN($AG38:CO38)*($AG38:CO38=2))>MAX(COLUMN($AG38:CO38)*($AG38:CO38=1))),IF(COLUMN(CP38)-MAX(COLUMN($AG38:CO38)*($AG38:CO38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CP38)-MAX(COLUMN($AG38:CO38)*($AG38:CO38=3))=$J38,3,0),IF(COLUMN(CP38)-MAX(COLUMN($AG38:CO38)*($AG38:CO38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CP38)*($AG38:CP38=1))>MAX(COLUMN($AG38:CP38)*($AG38:CP38=3)),MAX(COLUMN($AG38:CP38)*($AG38:CP38=1))>MAX(COLUMN($AG38:CP38)*($AG38:CP38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CQ38)-MAX(COLUMN($AG38:CP38)*($AG38:CP38=1))=$J38,3,0),IF(COLUMN(CQ38)-MAX(COLUMN($AG38:CP38)*($AG38:CP38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CP38)*($AG38:CP38=2))>MAX(COLUMN($AG38:CP38)*($AG38:CP38=3)),MAX(COLUMN($AG38:CP38)*($AG38:CP38=2))>MAX(COLUMN($AG38:CP38)*($AG38:CP38=1))),IF(COLUMN(CQ38)-MAX(COLUMN($AG38:CP38)*($AG38:CP38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CQ38)-MAX(COLUMN($AG38:CP38)*($AG38:CP38=3))=$J38,3,0),IF(COLUMN(CQ38)-MAX(COLUMN($AG38:CP38)*($AG38:CP38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=1))>MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=3)),MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=1))>MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CR38)-MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=1))=$J38,3,0),IF(COLUMN(CR38)-MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=2))>MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=3)),MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=2))>MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=1))),IF(COLUMN(CR38)-MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CR38)-MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=3))=$J38,3,0),IF(COLUMN(CR38)-MAX(COLUMN($AG38:CQ38)*($AG38:CQ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CR38)*($AG38:CR38=1))>MAX(COLUMN($AG38:CR38)*($AG38:CR38=3)),MAX(COLUMN($AG38:CR38)*($AG38:CR38=1))>MAX(COLUMN($AG38:CR38)*($AG38:CR38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CS38)-MAX(COLUMN($AG38:CR38)*($AG38:CR38=1))=$J38,3,0),IF(COLUMN(CS38)-MAX(COLUMN($AG38:CR38)*($AG38:CR38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CR38)*($AG38:CR38=2))>MAX(COLUMN($AG38:CR38)*($AG38:CR38=3)),MAX(COLUMN($AG38:CR38)*($AG38:CR38=2))>MAX(COLUMN($AG38:CR38)*($AG38:CR38=1))),IF(COLUMN(CS38)-MAX(COLUMN($AG38:CR38)*($AG38:CR38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CS38)-MAX(COLUMN($AG38:CR38)*($AG38:CR38=3))=$J38,3,0),IF(COLUMN(CS38)-MAX(COLUMN($AG38:CR38)*($AG38:CR38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CS38)*($AG38:CS38=1))>MAX(COLUMN($AG38:CS38)*($AG38:CS38=3)),MAX(COLUMN($AG38:CS38)*($AG38:CS38=1))>MAX(COLUMN($AG38:CS38)*($AG38:CS38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CT38)-MAX(COLUMN($AG38:CS38)*($AG38:CS38=1))=$J38,3,0),IF(COLUMN(CT38)-MAX(COLUMN($AG38:CS38)*($AG38:CS38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CS38)*($AG38:CS38=2))>MAX(COLUMN($AG38:CS38)*($AG38:CS38=3)),MAX(COLUMN($AG38:CS38)*($AG38:CS38=2))>MAX(COLUMN($AG38:CS38)*($AG38:CS38=1))),IF(COLUMN(CT38)-MAX(COLUMN($AG38:CS38)*($AG38:CS38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CT38)-MAX(COLUMN($AG38:CS38)*($AG38:CS38=3))=$J38,3,0),IF(COLUMN(CT38)-MAX(COLUMN($AG38:CS38)*($AG38:CS38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CT38)*($AG38:CT38=1))>MAX(COLUMN($AG38:CT38)*($AG38:CT38=3)),MAX(COLUMN($AG38:CT38)*($AG38:CT38=1))>MAX(COLUMN($AG38:CT38)*($AG38:CT38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CU38)-MAX(COLUMN($AG38:CT38)*($AG38:CT38=1))=$J38,3,0),IF(COLUMN(CU38)-MAX(COLUMN($AG38:CT38)*($AG38:CT38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CT38)*($AG38:CT38=2))>MAX(COLUMN($AG38:CT38)*($AG38:CT38=3)),MAX(COLUMN($AG38:CT38)*($AG38:CT38=2))>MAX(COLUMN($AG38:CT38)*($AG38:CT38=1))),IF(COLUMN(CU38)-MAX(COLUMN($AG38:CT38)*($AG38:CT38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CU38)-MAX(COLUMN($AG38:CT38)*($AG38:CT38=3))=$J38,3,0),IF(COLUMN(CU38)-MAX(COLUMN($AG38:CT38)*($AG38:CT38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CU38)*($AG38:CU38=1))>MAX(COLUMN($AG38:CU38)*($AG38:CU38=3)),MAX(COLUMN($AG38:CU38)*($AG38:CU38=1))>MAX(COLUMN($AG38:CU38)*($AG38:CU38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CV38)-MAX(COLUMN($AG38:CU38)*($AG38:CU38=1))=$J38,3,0),IF(COLUMN(CV38)-MAX(COLUMN($AG38:CU38)*($AG38:CU38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CU38)*($AG38:CU38=2))>MAX(COLUMN($AG38:CU38)*($AG38:CU38=3)),MAX(COLUMN($AG38:CU38)*($AG38:CU38=2))>MAX(COLUMN($AG38:CU38)*($AG38:CU38=1))),IF(COLUMN(CV38)-MAX(COLUMN($AG38:CU38)*($AG38:CU38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CV38)-MAX(COLUMN($AG38:CU38)*($AG38:CU38=3))=$J38,3,0),IF(COLUMN(CV38)-MAX(COLUMN($AG38:CU38)*($AG38:CU38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CV38)*($AG38:CV38=1))>MAX(COLUMN($AG38:CV38)*($AG38:CV38=3)),MAX(COLUMN($AG38:CV38)*($AG38:CV38=1))>MAX(COLUMN($AG38:CV38)*($AG38:CV38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CW38)-MAX(COLUMN($AG38:CV38)*($AG38:CV38=1))=$J38,3,0),IF(COLUMN(CW38)-MAX(COLUMN($AG38:CV38)*($AG38:CV38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CV38)*($AG38:CV38=2))>MAX(COLUMN($AG38:CV38)*($AG38:CV38=3)),MAX(COLUMN($AG38:CV38)*($AG38:CV38=2))>MAX(COLUMN($AG38:CV38)*($AG38:CV38=1))),IF(COLUMN(CW38)-MAX(COLUMN($AG38:CV38)*($AG38:CV38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CW38)-MAX(COLUMN($AG38:CV38)*($AG38:CV38=3))=$J38,3,0),IF(COLUMN(CW38)-MAX(COLUMN($AG38:CV38)*($AG38:CV38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CW38)*($AG38:CW38=1))>MAX(COLUMN($AG38:CW38)*($AG38:CW38=3)),MAX(COLUMN($AG38:CW38)*($AG38:CW38=1))>MAX(COLUMN($AG38:CW38)*($AG38:CW38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CX38)-MAX(COLUMN($AG38:CW38)*($AG38:CW38=1))=$J38,3,0),IF(COLUMN(CX38)-MAX(COLUMN($AG38:CW38)*($AG38:CW38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CW38)*($AG38:CW38=2))>MAX(COLUMN($AG38:CW38)*($AG38:CW38=3)),MAX(COLUMN($AG38:CW38)*($AG38:CW38=2))>MAX(COLUMN($AG38:CW38)*($AG38:CW38=1))),IF(COLUMN(CX38)-MAX(COLUMN($AG38:CW38)*($AG38:CW38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CX38)-MAX(COLUMN($AG38:CW38)*($AG38:CW38=3))=$J38,3,0),IF(COLUMN(CX38)-MAX(COLUMN($AG38:CW38)*($AG38:CW38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CX38)*($AG38:CX38=1))>MAX(COLUMN($AG38:CX38)*($AG38:CX38=3)),MAX(COLUMN($AG38:CX38)*($AG38:CX38=1))>MAX(COLUMN($AG38:CX38)*($AG38:CX38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CY38)-MAX(COLUMN($AG38:CX38)*($AG38:CX38=1))=$J38,3,0),IF(COLUMN(CY38)-MAX(COLUMN($AG38:CX38)*($AG38:CX38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CX38)*($AG38:CX38=2))>MAX(COLUMN($AG38:CX38)*($AG38:CX38=3)),MAX(COLUMN($AG38:CX38)*($AG38:CX38=2))>MAX(COLUMN($AG38:CX38)*($AG38:CX38=1))),IF(COLUMN(CY38)-MAX(COLUMN($AG38:CX38)*($AG38:CX38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CY38)-MAX(COLUMN($AG38:CX38)*($AG38:CX38=3))=$J38,3,0),IF(COLUMN(CY38)-MAX(COLUMN($AG38:CX38)*($AG38:CX38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CY38)*($AG38:CY38=1))>MAX(COLUMN($AG38:CY38)*($AG38:CY38=3)),MAX(COLUMN($AG38:CY38)*($AG38:CY38=1))>MAX(COLUMN($AG38:CY38)*($AG38:CY38=2))),IF($K38=\"Not Possible\",IF(COLUMN(CZ38)-MAX(COLUMN($AG38:CY38)*($AG38:CY38=1))=$J38,3,0),IF(COLUMN(CZ38)-MAX(COLUMN($AG38:CY38)*($AG38:CY38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CY38)*($AG38:CY38=2))>MAX(COLUMN($AG38:CY38)*($AG38:CY38=3)),MAX(COLUMN($AG38:CY38)*($AG38:CY38=2))>MAX(COLUMN($AG38:CY38)*($AG38:CY38=1))),IF(COLUMN(CZ38)-MAX(COLUMN($AG38:CY38)*($AG38:CY38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(CZ38)-MAX(COLUMN($AG38:CY38)*($AG38:CY38=3))=$J38,3,0),IF(COLUMN(CZ38)-MAX(COLUMN($AG38:CY38)*($AG38:CY38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=1))>MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=3)),MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=1))>MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DA38)-MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=1))=$J38,3,0),IF(COLUMN(DA38)-MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=2))>MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=3)),MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=2))>MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=1))),IF(COLUMN(DA38)-MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DA38)-MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=3))=$J38,3,0),IF(COLUMN(DA38)-MAX(COLUMN($AG38:CZ38)*($AG38:CZ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DA38)*($AG38:DA38=1))>MAX(COLUMN($AG38:DA38)*($AG38:DA38=3)),MAX(COLUMN($AG38:DA38)*($AG38:DA38=1))>MAX(COLUMN($AG38:DA38)*($AG38:DA38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DB38)-MAX(COLUMN($AG38:DA38)*($AG38:DA38=1))=$J38,3,0),IF(COLUMN(DB38)-MAX(COLUMN($AG38:DA38)*($AG38:DA38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DA38)*($AG38:DA38=2))>MAX(COLUMN($AG38:DA38)*($AG38:DA38=3)),MAX(COLUMN($AG38:DA38)*($AG38:DA38=2))>MAX(COLUMN($AG38:DA38)*($AG38:DA38=1))),IF(COLUMN(DB38)-MAX(COLUMN($AG38:DA38)*($AG38:DA38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DB38)-MAX(COLUMN($AG38:DA38)*($AG38:DA38=3))=$J38,3,0),IF(COLUMN(DB38)-MAX(COLUMN($AG38:DA38)*($AG38:DA38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DB38)*($AG38:DB38=1))>MAX(COLUMN($AG38:DB38)*($AG38:DB38=3)),MAX(COLUMN($AG38:DB38)*($AG38:DB38=1))>MAX(COLUMN($AG38:DB38)*($AG38:DB38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DC38)-MAX(COLUMN($AG38:DB38)*($AG38:DB38=1))=$J38,3,0),IF(COLUMN(DC38)-MAX(COLUMN($AG38:DB38)*($AG38:DB38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DB38)*($AG38:DB38=2))>MAX(COLUMN($AG38:DB38)*($AG38:DB38=3)),MAX(COLUMN($AG38:DB38)*($AG38:DB38=2))>MAX(COLUMN($AG38:DB38)*($AG38:DB38=1))),IF(COLUMN(DC38)-MAX(COLUMN($AG38:DB38)*($AG38:DB38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DC38)-MAX(COLUMN($AG38:DB38)*($AG38:DB38=3))=$J38,3,0),IF(COLUMN(DC38)-MAX(COLUMN($AG38:DB38)*($AG38:DB38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DC38)*($AG38:DC38=1))>MAX(COLUMN($AG38:DC38)*($AG38:DC38=3)),MAX(COLUMN($AG38:DC38)*($AG38:DC38=1))>MAX(COLUMN($AG38:DC38)*($AG38:DC38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DD38)-MAX(COLUMN($AG38:DC38)*($AG38:DC38=1))=$J38,3,0),IF(COLUMN(DD38)-MAX(COLUMN($AG38:DC38)*($AG38:DC38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DC38)*($AG38:DC38=2))>MAX(COLUMN($AG38:DC38)*($AG38:DC38=3)),MAX(COLUMN($AG38:DC38)*($AG38:DC38=2))>MAX(COLUMN($AG38:DC38)*($AG38:DC38=1))),IF(COLUMN(DD38)-MAX(COLUMN($AG38:DC38)*($AG38:DC38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DD38)-MAX(COLUMN($AG38:DC38)*($AG38:DC38=3))=$J38,3,0),IF(COLUMN(DD38)-MAX(COLUMN($AG38:DC38)*($AG38:DC38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DD38)*($AG38:DD38=1))>MAX(COLUMN($AG38:DD38)*($AG38:DD38=3)),MAX(COLUMN($AG38:DD38)*($AG38:DD38=1))>MAX(COLUMN($AG38:DD38)*($AG38:DD38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DE38)-MAX(COLUMN($AG38:DD38)*($AG38:DD38=1))=$J38,3,0),IF(COLUMN(DE38)-MAX(COLUMN($AG38:DD38)*($AG38:DD38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DD38)*($AG38:DD38=2))>MAX(COLUMN($AG38:DD38)*($AG38:DD38=3)),MAX(COLUMN($AG38:DD38)*($AG38:DD38=2))>MAX(COLUMN($AG38:DD38)*($AG38:DD38=1))),IF(COLUMN(DE38)-MAX(COLUMN($AG38:DD38)*($AG38:DD38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DE38)-MAX(COLUMN($AG38:DD38)*($AG38:DD38=3))=$J38,3,0),IF(COLUMN(DE38)-MAX(COLUMN($AG38:DD38)*($AG38:DD38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DE38)*($AG38:DE38=1))>MAX(COLUMN($AG38:DE38)*($AG38:DE38=3)),MAX(COLUMN($AG38:DE38)*($AG38:DE38=1))>MAX(COLUMN($AG38:DE38)*($AG38:DE38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DF38)-MAX(COLUMN($AG38:DE38)*($AG38:DE38=1))=$J38,3,0),IF(COLUMN(DF38)-MAX(COLUMN($AG38:DE38)*($AG38:DE38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DE38)*($AG38:DE38=2))>MAX(COLUMN($AG38:DE38)*($AG38:DE38=3)),MAX(COLUMN($AG38:DE38)*($AG38:DE38=2))>MAX(COLUMN($AG38:DE38)*($AG38:DE38=1))),IF(COLUMN(DF38)-MAX(COLUMN($AG38:DE38)*($AG38:DE38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DF38)-MAX(COLUMN($AG38:DE38)*($AG38:DE38=3))=$J38,3,0),IF(COLUMN(DF38)-MAX(COLUMN($AG38:DE38)*($AG38:DE38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DF38)*($AG38:DF38=1))>MAX(COLUMN($AG38:DF38)*($AG38:DF38=3)),MAX(COLUMN($AG38:DF38)*($AG38:DF38=1))>MAX(COLUMN($AG38:DF38)*($AG38:DF38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DG38)-MAX(COLUMN($AG38:DF38)*($AG38:DF38=1))=$J38,3,0),IF(COLUMN(DG38)-MAX(COLUMN($AG38:DF38)*($AG38:DF38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DF38)*($AG38:DF38=2))>MAX(COLUMN($AG38:DF38)*($AG38:DF38=3)),MAX(COLUMN($AG38:DF38)*($AG38:DF38=2))>MAX(COLUMN($AG38:DF38)*($AG38:DF38=1))),IF(COLUMN(DG38)-MAX(COLUMN($AG38:DF38)*($AG38:DF38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DG38)-MAX(COLUMN($AG38:DF38)*($AG38:DF38=3))=$J38,3,0),IF(COLUMN(DG38)-MAX(COLUMN($AG38:DF38)*($AG38:DF38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DG38)*($AG38:DG38=1))>MAX(COLUMN($AG38:DG38)*($AG38:DG38=3)),MAX(COLUMN($AG38:DG38)*($AG38:DG38=1))>MAX(COLUMN($AG38:DG38)*($AG38:DG38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DH38)-MAX(COLUMN($AG38:DG38)*($AG38:DG38=1))=$J38,3,0),IF(COLUMN(DH38)-MAX(COLUMN($AG38:DG38)*($AG38:DG38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DG38)*($AG38:DG38=2))>MAX(COLUMN($AG38:DG38)*($AG38:DG38=3)),MAX(COLUMN($AG38:DG38)*($AG38:DG38=2))>MAX(COLUMN($AG38:DG38)*($AG38:DG38=1))),IF(COLUMN(DH38)-MAX(COLUMN($AG38:DG38)*($AG38:DG38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DH38)-MAX(COLUMN($AG38:DG38)*($AG38:DG38=3))=$J38,3,0),IF(COLUMN(DH38)-MAX(COLUMN($AG38:DG38)*($AG38:DG38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DH38)*($AG38:DH38=1))>MAX(COLUMN($AG38:DH38)*($AG38:DH38=3)),MAX(COLUMN($AG38:DH38)*($AG38:DH38=1))>MAX(COLUMN($AG38:DH38)*($AG38:DH38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DI38)-MAX(COLUMN($AG38:DH38)*($AG38:DH38=1))=$J38,3,0),IF(COLUMN(DI38)-MAX(COLUMN($AG38:DH38)*($AG38:DH38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DH38)*($AG38:DH38=2))>MAX(COLUMN($AG38:DH38)*($AG38:DH38=3)),MAX(COLUMN($AG38:DH38)*($AG38:DH38=2))>MAX(COLUMN($AG38:DH38)*($AG38:DH38=1))),IF(COLUMN(DI38)-MAX(COLUMN($AG38:DH38)*($AG38:DH38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DI38)-MAX(COLUMN($AG38:DH38)*($AG38:DH38=3))=$J38,3,0),IF(COLUMN(DI38)-MAX(COLUMN($AG38:DH38)*($AG38:DH38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DI38)*($AG38:DI38=1))>MAX(COLUMN($AG38:DI38)*($AG38:DI38=3)),MAX(COLUMN($AG38:DI38)*($AG38:DI38=1))>MAX(COLUMN($AG38:DI38)*($AG38:DI38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DJ38)-MAX(COLUMN($AG38:DI38)*($AG38:DI38=1))=$J38,3,0),IF(COLUMN(DJ38)-MAX(COLUMN($AG38:DI38)*($AG38:DI38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DI38)*($AG38:DI38=2))>MAX(COLUMN($AG38:DI38)*($AG38:DI38=3)),MAX(COLUMN($AG38:DI38)*($AG38:DI38=2))>MAX(COLUMN($AG38:DI38)*($AG38:DI38=1))),IF(COLUMN(DJ38)-MAX(COLUMN($AG38:DI38)*($AG38:DI38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DJ38)-MAX(COLUMN($AG38:DI38)*($AG38:DI38=3))=$J38,3,0),IF(COLUMN(DJ38)-MAX(COLUMN($AG38:DI38)*($AG38:DI38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=1))>MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=3)),MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=1))>MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DK38)-MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=1))=$J38,3,0),IF(COLUMN(DK38)-MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=2))>MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=3)),MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=2))>MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=1))),IF(COLUMN(DK38)-MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DK38)-MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=3))=$J38,3,0),IF(COLUMN(DK38)-MAX(COLUMN($AG38:DJ38)*($AG38:DJ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DK38)*($AG38:DK38=1))>MAX(COLUMN($AG38:DK38)*($AG38:DK38=3)),MAX(COLUMN($AG38:DK38)*($AG38:DK38=1))>MAX(COLUMN($AG38:DK38)*($AG38:DK38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DL38)-MAX(COLUMN($AG38:DK38)*($AG38:DK38=1))=$J38,3,0),IF(COLUMN(DL38)-MAX(COLUMN($AG38:DK38)*($AG38:DK38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DK38)*($AG38:DK38=2))>MAX(COLUMN($AG38:DK38)*($AG38:DK38=3)),MAX(COLUMN($AG38:DK38)*($AG38:DK38=2))>MAX(COLUMN($AG38:DK38)*($AG38:DK38=1))),IF(COLUMN(DL38)-MAX(COLUMN($AG38:DK38)*($AG38:DK38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DL38)-MAX(COLUMN($AG38:DK38)*($AG38:DK38=3))=$J38,3,0),IF(COLUMN(DL38)-MAX(COLUMN($AG38:DK38)*($AG38:DK38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DL38)*($AG38:DL38=1))>MAX(COLUMN($AG38:DL38)*($AG38:DL38=3)),MAX(COLUMN($AG38:DL38)*($AG38:DL38=1))>MAX(COLUMN($AG38:DL38)*($AG38:DL38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DM38)-MAX(COLUMN($AG38:DL38)*($AG38:DL38=1))=$J38,3,0),IF(COLUMN(DM38)-MAX(COLUMN($AG38:DL38)*($AG38:DL38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DL38)*($AG38:DL38=2))>MAX(COLUMN($AG38:DL38)*($AG38:DL38=3)),MAX(COLUMN($AG38:DL38)*($AG38:DL38=2))>MAX(COLUMN($AG38:DL38)*($AG38:DL38=1))),IF(COLUMN(DM38)-MAX(COLUMN($AG38:DL38)*($AG38:DL38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DM38)-MAX(COLUMN($AG38:DL38)*($AG38:DL38=3))=$J38,3,0),IF(COLUMN(DM38)-MAX(COLUMN($AG38:DL38)*($AG38:DL38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DM38)*($AG38:DM38=1))>MAX(COLUMN($AG38:DM38)*($AG38:DM38=3)),MAX(COLUMN($AG38:DM38)*($AG38:DM38=1))>MAX(COLUMN($AG38:DM38)*($AG38:DM38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DN38)-MAX(COLUMN($AG38:DM38)*($AG38:DM38=1))=$J38,3,0),IF(COLUMN(DN38)-MAX(COLUMN($AG38:DM38)*($AG38:DM38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DM38)*($AG38:DM38=2))>MAX(COLUMN($AG38:DM38)*($AG38:DM38=3)),MAX(COLUMN($AG38:DM38)*($AG38:DM38=2))>MAX(COLUMN($AG38:DM38)*($AG38:DM38=1))),IF(COLUMN(DN38)-MAX(COLUMN($AG38:DM38)*($AG38:DM38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DN38)-MAX(COLUMN($AG38:DM38)*($AG38:DM38=3))=$J38,3,0),IF(COLUMN(DN38)-MAX(COLUMN($AG38:DM38)*($AG38:DM38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DN38)*($AG38:DN38=1))>MAX(COLUMN($AG38:DN38)*($AG38:DN38=3)),MAX(COLUMN($AG38:DN38)*($AG38:DN38=1))>MAX(COLUMN($AG38:DN38)*($AG38:DN38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DO38)-MAX(COLUMN($AG38:DN38)*($AG38:DN38=1))=$J38,3,0),IF(COLUMN(DO38)-MAX(COLUMN($AG38:DN38)*($AG38:DN38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DN38)*($AG38:DN38=2))>MAX(COLUMN($AG38:DN38)*($AG38:DN38=3)),MAX(COLUMN($AG38:DN38)*($AG38:DN38=2))>MAX(COLUMN($AG38:DN38)*($AG38:DN38=1))),IF(COLUMN(DO38)-MAX(COLUMN($AG38:DN38)*($AG38:DN38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DO38)-MAX(COLUMN($AG38:DN38)*($AG38:DN38=3))=$J38,3,0),IF(COLUMN(DO38)-MAX(COLUMN($AG38:DN38)*($AG38:DN38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DO38)*($AG38:DO38=1))>MAX(COLUMN($AG38:DO38)*($AG38:DO38=3)),MAX(COLUMN($AG38:DO38)*($AG38:DO38=1))>MAX(COLUMN($AG38:DO38)*($AG38:DO38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DP38)-MAX(COLUMN($AG38:DO38)*($AG38:DO38=1))=$J38,3,0),IF(COLUMN(DP38)-MAX(COLUMN($AG38:DO38)*($AG38:DO38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DO38)*($AG38:DO38=2))>MAX(COLUMN($AG38:DO38)*($AG38:DO38=3)),MAX(COLUMN($AG38:DO38)*($AG38:DO38=2))>MAX(COLUMN($AG38:DO38)*($AG38:DO38=1))),IF(COLUMN(DP38)-MAX(COLUMN($AG38:DO38)*($AG38:DO38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DP38)-MAX(COLUMN($AG38:DO38)*($AG38:DO38=3))=$J38,3,0),IF(COLUMN(DP38)-MAX(COLUMN($AG38:DO38)*($AG38:DO38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DP38)*($AG38:DP38=1))>MAX(COLUMN($AG38:DP38)*($AG38:DP38=3)),MAX(COLUMN($AG38:DP38)*($AG38:DP38=1))>MAX(COLUMN($AG38:DP38)*($AG38:DP38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DQ38)-MAX(COLUMN($AG38:DP38)*($AG38:DP38=1))=$J38,3,0),IF(COLUMN(DQ38)-MAX(COLUMN($AG38:DP38)*($AG38:DP38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DP38)*($AG38:DP38=2))>MAX(COLUMN($AG38:DP38)*($AG38:DP38=3)),MAX(COLUMN($AG38:DP38)*($AG38:DP38=2))>MAX(COLUMN($AG38:DP38)*($AG38:DP38=1))),IF(COLUMN(DQ38)-MAX(COLUMN($AG38:DP38)*($AG38:DP38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DQ38)-MAX(COLUMN($AG38:DP38)*($AG38:DP38=3))=$J38,3,0),IF(COLUMN(DQ38)-MAX(COLUMN($AG38:DP38)*($AG38:DP38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=1))>MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=3)),MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=1))>MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DR38)-MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=1))=$J38,3,0),IF(COLUMN(DR38)-MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=2))>MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=3)),MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=2))>MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=1))),IF(COLUMN(DR38)-MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DR38)-MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=3))=$J38,3,0),IF(COLUMN(DR38)-MAX(COLUMN($AG38:DQ38)*($AG38:DQ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DR38)*($AG38:DR38=1))>MAX(COLUMN($AG38:DR38)*($AG38:DR38=3)),MAX(COLUMN($AG38:DR38)*($AG38:DR38=1))>MAX(COLUMN($AG38:DR38)*($AG38:DR38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DS38)-MAX(COLUMN($AG38:DR38)*($AG38:DR38=1))=$J38,3,0),IF(COLUMN(DS38)-MAX(COLUMN($AG38:DR38)*($AG38:DR38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DR38)*($AG38:DR38=2))>MAX(COLUMN($AG38:DR38)*($AG38:DR38=3)),MAX(COLUMN($AG38:DR38)*($AG38:DR38=2))>MAX(COLUMN($AG38:DR38)*($AG38:DR38=1))),IF(COLUMN(DS38)-MAX(COLUMN($AG38:DR38)*($AG38:DR38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DS38)-MAX(COLUMN($AG38:DR38)*($AG38:DR38=3))=$J38,3,0),IF(COLUMN(DS38)-MAX(COLUMN($AG38:DR38)*($AG38:DR38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DS38)*($AG38:DS38=1))>MAX(COLUMN($AG38:DS38)*($AG38:DS38=3)),MAX(COLUMN($AG38:DS38)*($AG38:DS38=1))>MAX(COLUMN($AG38:DS38)*($AG38:DS38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DT38)-MAX(COLUMN($AG38:DS38)*($AG38:DS38=1))=$J38,3,0),IF(COLUMN(DT38)-MAX(COLUMN($AG38:DS38)*($AG38:DS38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DS38)*($AG38:DS38=2))>MAX(COLUMN($AG38:DS38)*($AG38:DS38=3)),MAX(COLUMN($AG38:DS38)*($AG38:DS38=2))>MAX(COLUMN($AG38:DS38)*($AG38:DS38=1))),IF(COLUMN(DT38)-MAX(COLUMN($AG38:DS38)*($AG38:DS38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DT38)-MAX(COLUMN($AG38:DS38)*($AG38:DS38=3))=$J38,3,0),IF(COLUMN(DT38)-MAX(COLUMN($AG38:DS38)*($AG38:DS38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DT38)*($AG38:DT38=1))>MAX(COLUMN($AG38:DT38)*($AG38:DT38=3)),MAX(COLUMN($AG38:DT38)*($AG38:DT38=1))>MAX(COLUMN($AG38:DT38)*($AG38:DT38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DU38)-MAX(COLUMN($AG38:DT38)*($AG38:DT38=1))=$J38,3,0),IF(COLUMN(DU38)-MAX(COLUMN($AG38:DT38)*($AG38:DT38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DT38)*($AG38:DT38=2))>MAX(COLUMN($AG38:DT38)*($AG38:DT38=3)),MAX(COLUMN($AG38:DT38)*($AG38:DT38=2))>MAX(COLUMN($AG38:DT38)*($AG38:DT38=1))),IF(COLUMN(DU38)-MAX(COLUMN($AG38:DT38)*($AG38:DT38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DU38)-MAX(COLUMN($AG38:DT38)*($AG38:DT38=3))=$J38,3,0),IF(COLUMN(DU38)-MAX(COLUMN($AG38:DT38)*($AG38:DT38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DU38)*($AG38:DU38=1))>MAX(COLUMN($AG38:DU38)*($AG38:DU38=3)),MAX(COLUMN($AG38:DU38)*($AG38:DU38=1))>MAX(COLUMN($AG38:DU38)*($AG38:DU38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DV38)-MAX(COLUMN($AG38:DU38)*($AG38:DU38=1))=$J38,3,0),IF(COLUMN(DV38)-MAX(COLUMN($AG38:DU38)*($AG38:DU38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DU38)*($AG38:DU38=2))>MAX(COLUMN($AG38:DU38)*($AG38:DU38=3)),MAX(COLUMN($AG38:DU38)*($AG38:DU38=2))>MAX(COLUMN($AG38:DU38)*($AG38:DU38=1))),IF(COLUMN(DV38)-MAX(COLUMN($AG38:DU38)*($AG38:DU38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DV38)-MAX(COLUMN($AG38:DU38)*($AG38:DU38=3))=$J38,3,0),IF(COLUMN(DV38)-MAX(COLUMN($AG38:DU38)*($AG38:DU38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DV38)*($AG38:DV38=1))>MAX(COLUMN($AG38:DV38)*($AG38:DV38=3)),MAX(COLUMN($AG38:DV38)*($AG38:DV38=1))>MAX(COLUMN($AG38:DV38)*($AG38:DV38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DW38)-MAX(COLUMN($AG38:DV38)*($AG38:DV38=1))=$J38,3,0),IF(COLUMN(DW38)-MAX(COLUMN($AG38:DV38)*($AG38:DV38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DV38)*($AG38:DV38=2))>MAX(COLUMN($AG38:DV38)*($AG38:DV38=3)),MAX(COLUMN($AG38:DV38)*($AG38:DV38=2))>MAX(COLUMN($AG38:DV38)*($AG38:DV38=1))),IF(COLUMN(DW38)-MAX(COLUMN($AG38:DV38)*($AG38:DV38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DW38)-MAX(COLUMN($AG38:DV38)*($AG38:DV38=3))=$J38,3,0),IF(COLUMN(DW38)-MAX(COLUMN($AG38:DV38)*($AG38:DV38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DW38)*($AG38:DW38=1))>MAX(COLUMN($AG38:DW38)*($AG38:DW38=3)),MAX(COLUMN($AG38:DW38)*($AG38:DW38=1))>MAX(COLUMN($AG38:DW38)*($AG38:DW38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DX38)-MAX(COLUMN($AG38:DW38)*($AG38:DW38=1))=$J38,3,0),IF(COLUMN(DX38)-MAX(COLUMN($AG38:DW38)*($AG38:DW38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DW38)*($AG38:DW38=2))>MAX(COLUMN($AG38:DW38)*($AG38:DW38=3)),MAX(COLUMN($AG38:DW38)*($AG38:DW38=2))>MAX(COLUMN($AG38:DW38)*($AG38:DW38=1))),IF(COLUMN(DX38)-MAX(COLUMN($AG38:DW38)*($AG38:DW38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DX38)-MAX(COLUMN($AG38:DW38)*($AG38:DW38=3))=$J38,3,0),IF(COLUMN(DX38)-MAX(COLUMN($AG38:DW38)*($AG38:DW38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DX38)*($AG38:DX38=1))>MAX(COLUMN($AG38:DX38)*($AG38:DX38=3)),MAX(COLUMN($AG38:DX38)*($AG38:DX38=1))>MAX(COLUMN($AG38:DX38)*($AG38:DX38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DY38)-MAX(COLUMN($AG38:DX38)*($AG38:DX38=1))=$J38,3,0),IF(COLUMN(DY38)-MAX(COLUMN($AG38:DX38)*($AG38:DX38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DX38)*($AG38:DX38=2))>MAX(COLUMN($AG38:DX38)*($AG38:DX38=3)),MAX(COLUMN($AG38:DX38)*($AG38:DX38=2))>MAX(COLUMN($AG38:DX38)*($AG38:DX38=1))),IF(COLUMN(DY38)-MAX(COLUMN($AG38:DX38)*($AG38:DX38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DY38)-MAX(COLUMN($AG38:DX38)*($AG38:DX38=3))=$J38,3,0),IF(COLUMN(DY38)-MAX(COLUMN($AG38:DX38)*($AG38:DX38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DY38)*($AG38:DY38=1))>MAX(COLUMN($AG38:DY38)*($AG38:DY38=3)),MAX(COLUMN($AG38:DY38)*($AG38:DY38=1))>MAX(COLUMN($AG38:DY38)*($AG38:DY38=2))),IF($K38=\"Not Possible\",IF(COLUMN(DZ38)-MAX(COLUMN($AG38:DY38)*($AG38:DY38=1))=$J38,3,0),IF(COLUMN(DZ38)-MAX(COLUMN($AG38:DY38)*($AG38:DY38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DY38)*($AG38:DY38=2))>MAX(COLUMN($AG38:DY38)*($AG38:DY38=3)),MAX(COLUMN($AG38:DY38)*($AG38:DY38=2))>MAX(COLUMN($AG38:DY38)*($AG38:DY38=1))),IF(COLUMN(DZ38)-MAX(COLUMN($AG38:DY38)*($AG38:DY38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(DZ38)-MAX(COLUMN($AG38:DY38)*($AG38:DY38=3))=$J38,3,0),IF(COLUMN(DZ38)-MAX(COLUMN($AG38:DY38)*($AG38:DY38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=1))>MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=3)),MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=1))>MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=2))),IF($K38=\"Not Possible\",IF(COLUMN(EA38)-MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=1))=$J38,3,0),IF(COLUMN(EA38)-MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=2))>MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=3)),MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=2))>MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=1))),IF(COLUMN(EA38)-MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(EA38)-MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=3))=$J38,3,0),IF(COLUMN(EA38)-MAX(COLUMN($AG38:DZ38)*($AG38:DZ38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:EA38)*($AG38:EA38=1))>MAX(COLUMN($AG38:EA38)*($AG38:EA38=3)),MAX(COLUMN($AG38:EA38)*($AG38:EA38=1))>MAX(COLUMN($AG38:EA38)*($AG38:EA38=2))),IF($K38=\"Not Possible\",IF(COLUMN(EB38)-MAX(COLUMN($AG38:EA38)*($AG38:EA38=1))=$J38,3,0),IF(COLUMN(EB38)-MAX(COLUMN($AG38:EA38)*($AG38:EA38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:EA38)*($AG38:EA38=2))>MAX(COLUMN($AG38:EA38)*($AG38:EA38=3)),MAX(COLUMN($AG38:EA38)*($AG38:EA38=2))>MAX(COLUMN($AG38:EA38)*($AG38:EA38=1))),IF(COLUMN(EB38)-MAX(COLUMN($AG38:EA38)*($AG38:EA38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(EB38)-MAX(COLUMN($AG38:EA38)*($AG38:EA38=3))=$J38,3,0),IF(COLUMN(EB38)-MAX(COLUMN($AG38:EA38)*($AG38:EA38=3))=$J38,2,0)))))","v":0},{"$f":"IF($AG38=4,0,IF(AND(MAX(COLUMN($AG38:EB38)*($AG38:EB38=1))>MAX(COLUMN($AG38:EB38)*($AG38:EB38=3)),MAX(COLUMN($AG38:EB38)*($AG38:EB38=1))>MAX(COLUMN($AG38:EB38)*($AG38:EB38=2))),IF($K38=\"Not Possible\",IF(COLUMN(EC38)-MAX(COLUMN($AG38:EB38)*($AG38:EB38=1))=$J38,3,0),IF(COLUMN(EC38)-MAX(COLUMN($AG38:EB38)*($AG38:EB38=1))=$J38,2,0)),IF(AND(MAX(COLUMN($AG38:EB38)*($AG38:EB38=2))>MAX(COLUMN($AG38:EB38)*($AG38:EB38=3)),MAX(COLUMN($AG38:EB38)*($AG38:EB38=2))>MAX(COLUMN($AG38:EB38)*($AG38:EB38=1))),IF(COLUMN(EC38)-MAX(COLUMN($AG38:EB38)*($AG38:EB38=2))=$L38,3,0),IF($K38=\"Not Possible\",IF(COLUMN(EC38)-MAX(COLUMN($AG38:EB38)*($AG38:EB38=3))=$J38,3,0),IF(COLUMN(EC38)-MAX(COLUMN($AG38:EB38)*($AG38:EB38=3))=$J38,2,0)))))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":""},null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset class],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":""},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",Form_Asset[[#This Row],[Asset ID]]&ROW())","v":""},null,null,{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",INDEX(AssetListTbl[Best Estimate Life (5)],(MATCH(Form_Asset[[#This Row],[Sub-Asset category]],AssetListTbl[Sub-Element Category],0))))","v":""},null,null,null,null,{"$f":"MAX(COLUMN($AH39:EC39)*($AH39:EC39=2))","v":0},{"$f":"MAX(COLUMN($AH39:EC39)*($AH39:EC39=3))","v":0},{"$f":"IFERROR(100-(IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Replace]])),INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Refurb]])))),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],3,2)","v":2},{"$f":"SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Product_Stage[CO2e (t)])","v":0},{"$f":"IFERROR(SUM(Form_Elements[General Item Material])*(Form_Asset[[#This Row],[Weighted Split]]/SUM(Form_Asset[Weighted Split]))+Form_Asset[[#This Row],[Weighted Split]],0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth (wtt)]))+(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Transport]))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Non contractor People Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Contractor people transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Site establishment])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),(SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Const_Ins_InsB[CO2e (t)]))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Other Construction Waste])*Form_Asset[[#This Row],[Weighted Split]]/(SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[[Waste Co2e ]])+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New build\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]]),IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",(SUM(Form_Asset[[#This Row],[Materials]:[Waste]])-(SUM(Form_Asset[[#This Row],[Materials Transport]],Form_Asset[[#This Row],[People Transport]]*0.5,Form_Asset[[#This Row],[Plant Transport]]*0.5))),IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]])/(SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%])),0)))","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_energy[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_use_energy[CO2e (t)]),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset ref.]]=\"\",0,SUMIF(Form_Asset[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Asset[New Build Co2e])*SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%]))","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Dem - General Item Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Dem -Waste Co2e]),0)","v":0},{"$f":"(Form_Asset[[#This Row],[Plant use]]+Form_Asset[[#This Row],[Plant Transport]])*50%","v":0},{"$f":"Form_Asset[[#This Row],[People Transport]]*50%","v":0},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New Build\",1,IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",2,IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",3,IF(Form_Asset[[#This Row],[First intervention]]=\"Demolition\",4,\"\"))))","v":""},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AG39)*($AG39:AG39=1))>MAX(COLUMN($AG39:AG39)*($AG39:AG39=3)),MAX(COLUMN($AG39:AG39)*($AG39:AG39=1))>MAX(COLUMN($AG39:AG39)*($AG39:AG39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AH39)-MAX(COLUMN($AG39:AG39)*($AG39:AG39=1))=$J39,3,0),IF(COLUMN(AH39)-MAX(COLUMN($AG39:AG39)*($AG39:AG39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AG39)*($AG39:AG39=2))>MAX(COLUMN($AG39:AG39)*($AG39:AG39=3)),MAX(COLUMN($AG39:AG39)*($AG39:AG39=2))>MAX(COLUMN($AG39:AG39)*($AG39:AG39=1))),IF(COLUMN(AH39)-MAX(COLUMN($AG39:AG39)*($AG39:AG39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AH39)-MAX(COLUMN($AG39:AG39)*($AG39:AG39=3))=$J39,3,0),IF(COLUMN(AH39)-MAX(COLUMN($AG39:AG39)*($AG39:AG39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AH39)*($AG39:AH39=1))>MAX(COLUMN($AG39:AH39)*($AG39:AH39=3)),MAX(COLUMN($AG39:AH39)*($AG39:AH39=1))>MAX(COLUMN($AG39:AH39)*($AG39:AH39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AI39)-MAX(COLUMN($AG39:AH39)*($AG39:AH39=1))=$J39,3,0),IF(COLUMN(AI39)-MAX(COLUMN($AG39:AH39)*($AG39:AH39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AH39)*($AG39:AH39=2))>MAX(COLUMN($AG39:AH39)*($AG39:AH39=3)),MAX(COLUMN($AG39:AH39)*($AG39:AH39=2))>MAX(COLUMN($AG39:AH39)*($AG39:AH39=1))),IF(COLUMN(AI39)-MAX(COLUMN($AG39:AH39)*($AG39:AH39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AI39)-MAX(COLUMN($AG39:AH39)*($AG39:AH39=3))=$J39,3,0),IF(COLUMN(AI39)-MAX(COLUMN($AG39:AH39)*($AG39:AH39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AI39)*($AG39:AI39=1))>MAX(COLUMN($AG39:AI39)*($AG39:AI39=3)),MAX(COLUMN($AG39:AI39)*($AG39:AI39=1))>MAX(COLUMN($AG39:AI39)*($AG39:AI39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AJ39)-MAX(COLUMN($AG39:AI39)*($AG39:AI39=1))=$J39,3,0),IF(COLUMN(AJ39)-MAX(COLUMN($AG39:AI39)*($AG39:AI39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AI39)*($AG39:AI39=2))>MAX(COLUMN($AG39:AI39)*($AG39:AI39=3)),MAX(COLUMN($AG39:AI39)*($AG39:AI39=2))>MAX(COLUMN($AG39:AI39)*($AG39:AI39=1))),IF(COLUMN(AJ39)-MAX(COLUMN($AG39:AI39)*($AG39:AI39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AJ39)-MAX(COLUMN($AG39:AI39)*($AG39:AI39=3))=$J39,3,0),IF(COLUMN(AJ39)-MAX(COLUMN($AG39:AI39)*($AG39:AI39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=1))>MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=3)),MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=1))>MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AK39)-MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=1))=$J39,3,0),IF(COLUMN(AK39)-MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=2))>MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=3)),MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=2))>MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=1))),IF(COLUMN(AK39)-MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AK39)-MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=3))=$J39,3,0),IF(COLUMN(AK39)-MAX(COLUMN($AG39:AJ39)*($AG39:AJ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AK39)*($AG39:AK39=1))>MAX(COLUMN($AG39:AK39)*($AG39:AK39=3)),MAX(COLUMN($AG39:AK39)*($AG39:AK39=1))>MAX(COLUMN($AG39:AK39)*($AG39:AK39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AL39)-MAX(COLUMN($AG39:AK39)*($AG39:AK39=1))=$J39,3,0),IF(COLUMN(AL39)-MAX(COLUMN($AG39:AK39)*($AG39:AK39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AK39)*($AG39:AK39=2))>MAX(COLUMN($AG39:AK39)*($AG39:AK39=3)),MAX(COLUMN($AG39:AK39)*($AG39:AK39=2))>MAX(COLUMN($AG39:AK39)*($AG39:AK39=1))),IF(COLUMN(AL39)-MAX(COLUMN($AG39:AK39)*($AG39:AK39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AL39)-MAX(COLUMN($AG39:AK39)*($AG39:AK39=3))=$J39,3,0),IF(COLUMN(AL39)-MAX(COLUMN($AG39:AK39)*($AG39:AK39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AL39)*($AG39:AL39=1))>MAX(COLUMN($AG39:AL39)*($AG39:AL39=3)),MAX(COLUMN($AG39:AL39)*($AG39:AL39=1))>MAX(COLUMN($AG39:AL39)*($AG39:AL39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AM39)-MAX(COLUMN($AG39:AL39)*($AG39:AL39=1))=$J39,3,0),IF(COLUMN(AM39)-MAX(COLUMN($AG39:AL39)*($AG39:AL39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AL39)*($AG39:AL39=2))>MAX(COLUMN($AG39:AL39)*($AG39:AL39=3)),MAX(COLUMN($AG39:AL39)*($AG39:AL39=2))>MAX(COLUMN($AG39:AL39)*($AG39:AL39=1))),IF(COLUMN(AM39)-MAX(COLUMN($AG39:AL39)*($AG39:AL39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AM39)-MAX(COLUMN($AG39:AL39)*($AG39:AL39=3))=$J39,3,0),IF(COLUMN(AM39)-MAX(COLUMN($AG39:AL39)*($AG39:AL39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AM39)*($AG39:AM39=1))>MAX(COLUMN($AG39:AM39)*($AG39:AM39=3)),MAX(COLUMN($AG39:AM39)*($AG39:AM39=1))>MAX(COLUMN($AG39:AM39)*($AG39:AM39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AN39)-MAX(COLUMN($AG39:AM39)*($AG39:AM39=1))=$J39,3,0),IF(COLUMN(AN39)-MAX(COLUMN($AG39:AM39)*($AG39:AM39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AM39)*($AG39:AM39=2))>MAX(COLUMN($AG39:AM39)*($AG39:AM39=3)),MAX(COLUMN($AG39:AM39)*($AG39:AM39=2))>MAX(COLUMN($AG39:AM39)*($AG39:AM39=1))),IF(COLUMN(AN39)-MAX(COLUMN($AG39:AM39)*($AG39:AM39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AN39)-MAX(COLUMN($AG39:AM39)*($AG39:AM39=3))=$J39,3,0),IF(COLUMN(AN39)-MAX(COLUMN($AG39:AM39)*($AG39:AM39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AN39)*($AG39:AN39=1))>MAX(COLUMN($AG39:AN39)*($AG39:AN39=3)),MAX(COLUMN($AG39:AN39)*($AG39:AN39=1))>MAX(COLUMN($AG39:AN39)*($AG39:AN39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AO39)-MAX(COLUMN($AG39:AN39)*($AG39:AN39=1))=$J39,3,0),IF(COLUMN(AO39)-MAX(COLUMN($AG39:AN39)*($AG39:AN39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AN39)*($AG39:AN39=2))>MAX(COLUMN($AG39:AN39)*($AG39:AN39=3)),MAX(COLUMN($AG39:AN39)*($AG39:AN39=2))>MAX(COLUMN($AG39:AN39)*($AG39:AN39=1))),IF(COLUMN(AO39)-MAX(COLUMN($AG39:AN39)*($AG39:AN39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AO39)-MAX(COLUMN($AG39:AN39)*($AG39:AN39=3))=$J39,3,0),IF(COLUMN(AO39)-MAX(COLUMN($AG39:AN39)*($AG39:AN39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AO39)*($AG39:AO39=1))>MAX(COLUMN($AG39:AO39)*($AG39:AO39=3)),MAX(COLUMN($AG39:AO39)*($AG39:AO39=1))>MAX(COLUMN($AG39:AO39)*($AG39:AO39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AP39)-MAX(COLUMN($AG39:AO39)*($AG39:AO39=1))=$J39,3,0),IF(COLUMN(AP39)-MAX(COLUMN($AG39:AO39)*($AG39:AO39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AO39)*($AG39:AO39=2))>MAX(COLUMN($AG39:AO39)*($AG39:AO39=3)),MAX(COLUMN($AG39:AO39)*($AG39:AO39=2))>MAX(COLUMN($AG39:AO39)*($AG39:AO39=1))),IF(COLUMN(AP39)-MAX(COLUMN($AG39:AO39)*($AG39:AO39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AP39)-MAX(COLUMN($AG39:AO39)*($AG39:AO39=3))=$J39,3,0),IF(COLUMN(AP39)-MAX(COLUMN($AG39:AO39)*($AG39:AO39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AP39)*($AG39:AP39=1))>MAX(COLUMN($AG39:AP39)*($AG39:AP39=3)),MAX(COLUMN($AG39:AP39)*($AG39:AP39=1))>MAX(COLUMN($AG39:AP39)*($AG39:AP39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AQ39)-MAX(COLUMN($AG39:AP39)*($AG39:AP39=1))=$J39,3,0),IF(COLUMN(AQ39)-MAX(COLUMN($AG39:AP39)*($AG39:AP39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AP39)*($AG39:AP39=2))>MAX(COLUMN($AG39:AP39)*($AG39:AP39=3)),MAX(COLUMN($AG39:AP39)*($AG39:AP39=2))>MAX(COLUMN($AG39:AP39)*($AG39:AP39=1))),IF(COLUMN(AQ39)-MAX(COLUMN($AG39:AP39)*($AG39:AP39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AQ39)-MAX(COLUMN($AG39:AP39)*($AG39:AP39=3))=$J39,3,0),IF(COLUMN(AQ39)-MAX(COLUMN($AG39:AP39)*($AG39:AP39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=1))>MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=3)),MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=1))>MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AR39)-MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=1))=$J39,3,0),IF(COLUMN(AR39)-MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=2))>MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=3)),MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=2))>MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=1))),IF(COLUMN(AR39)-MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AR39)-MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=3))=$J39,3,0),IF(COLUMN(AR39)-MAX(COLUMN($AG39:AQ39)*($AG39:AQ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AR39)*($AG39:AR39=1))>MAX(COLUMN($AG39:AR39)*($AG39:AR39=3)),MAX(COLUMN($AG39:AR39)*($AG39:AR39=1))>MAX(COLUMN($AG39:AR39)*($AG39:AR39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AS39)-MAX(COLUMN($AG39:AR39)*($AG39:AR39=1))=$J39,3,0),IF(COLUMN(AS39)-MAX(COLUMN($AG39:AR39)*($AG39:AR39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AR39)*($AG39:AR39=2))>MAX(COLUMN($AG39:AR39)*($AG39:AR39=3)),MAX(COLUMN($AG39:AR39)*($AG39:AR39=2))>MAX(COLUMN($AG39:AR39)*($AG39:AR39=1))),IF(COLUMN(AS39)-MAX(COLUMN($AG39:AR39)*($AG39:AR39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AS39)-MAX(COLUMN($AG39:AR39)*($AG39:AR39=3))=$J39,3,0),IF(COLUMN(AS39)-MAX(COLUMN($AG39:AR39)*($AG39:AR39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AS39)*($AG39:AS39=1))>MAX(COLUMN($AG39:AS39)*($AG39:AS39=3)),MAX(COLUMN($AG39:AS39)*($AG39:AS39=1))>MAX(COLUMN($AG39:AS39)*($AG39:AS39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AT39)-MAX(COLUMN($AG39:AS39)*($AG39:AS39=1))=$J39,3,0),IF(COLUMN(AT39)-MAX(COLUMN($AG39:AS39)*($AG39:AS39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AS39)*($AG39:AS39=2))>MAX(COLUMN($AG39:AS39)*($AG39:AS39=3)),MAX(COLUMN($AG39:AS39)*($AG39:AS39=2))>MAX(COLUMN($AG39:AS39)*($AG39:AS39=1))),IF(COLUMN(AT39)-MAX(COLUMN($AG39:AS39)*($AG39:AS39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AT39)-MAX(COLUMN($AG39:AS39)*($AG39:AS39=3))=$J39,3,0),IF(COLUMN(AT39)-MAX(COLUMN($AG39:AS39)*($AG39:AS39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AT39)*($AG39:AT39=1))>MAX(COLUMN($AG39:AT39)*($AG39:AT39=3)),MAX(COLUMN($AG39:AT39)*($AG39:AT39=1))>MAX(COLUMN($AG39:AT39)*($AG39:AT39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AU39)-MAX(COLUMN($AG39:AT39)*($AG39:AT39=1))=$J39,3,0),IF(COLUMN(AU39)-MAX(COLUMN($AG39:AT39)*($AG39:AT39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AT39)*($AG39:AT39=2))>MAX(COLUMN($AG39:AT39)*($AG39:AT39=3)),MAX(COLUMN($AG39:AT39)*($AG39:AT39=2))>MAX(COLUMN($AG39:AT39)*($AG39:AT39=1))),IF(COLUMN(AU39)-MAX(COLUMN($AG39:AT39)*($AG39:AT39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AU39)-MAX(COLUMN($AG39:AT39)*($AG39:AT39=3))=$J39,3,0),IF(COLUMN(AU39)-MAX(COLUMN($AG39:AT39)*($AG39:AT39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AU39)*($AG39:AU39=1))>MAX(COLUMN($AG39:AU39)*($AG39:AU39=3)),MAX(COLUMN($AG39:AU39)*($AG39:AU39=1))>MAX(COLUMN($AG39:AU39)*($AG39:AU39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AV39)-MAX(COLUMN($AG39:AU39)*($AG39:AU39=1))=$J39,3,0),IF(COLUMN(AV39)-MAX(COLUMN($AG39:AU39)*($AG39:AU39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AU39)*($AG39:AU39=2))>MAX(COLUMN($AG39:AU39)*($AG39:AU39=3)),MAX(COLUMN($AG39:AU39)*($AG39:AU39=2))>MAX(COLUMN($AG39:AU39)*($AG39:AU39=1))),IF(COLUMN(AV39)-MAX(COLUMN($AG39:AU39)*($AG39:AU39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AV39)-MAX(COLUMN($AG39:AU39)*($AG39:AU39=3))=$J39,3,0),IF(COLUMN(AV39)-MAX(COLUMN($AG39:AU39)*($AG39:AU39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AV39)*($AG39:AV39=1))>MAX(COLUMN($AG39:AV39)*($AG39:AV39=3)),MAX(COLUMN($AG39:AV39)*($AG39:AV39=1))>MAX(COLUMN($AG39:AV39)*($AG39:AV39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AW39)-MAX(COLUMN($AG39:AV39)*($AG39:AV39=1))=$J39,3,0),IF(COLUMN(AW39)-MAX(COLUMN($AG39:AV39)*($AG39:AV39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AV39)*($AG39:AV39=2))>MAX(COLUMN($AG39:AV39)*($AG39:AV39=3)),MAX(COLUMN($AG39:AV39)*($AG39:AV39=2))>MAX(COLUMN($AG39:AV39)*($AG39:AV39=1))),IF(COLUMN(AW39)-MAX(COLUMN($AG39:AV39)*($AG39:AV39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AW39)-MAX(COLUMN($AG39:AV39)*($AG39:AV39=3))=$J39,3,0),IF(COLUMN(AW39)-MAX(COLUMN($AG39:AV39)*($AG39:AV39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AW39)*($AG39:AW39=1))>MAX(COLUMN($AG39:AW39)*($AG39:AW39=3)),MAX(COLUMN($AG39:AW39)*($AG39:AW39=1))>MAX(COLUMN($AG39:AW39)*($AG39:AW39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AX39)-MAX(COLUMN($AG39:AW39)*($AG39:AW39=1))=$J39,3,0),IF(COLUMN(AX39)-MAX(COLUMN($AG39:AW39)*($AG39:AW39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AW39)*($AG39:AW39=2))>MAX(COLUMN($AG39:AW39)*($AG39:AW39=3)),MAX(COLUMN($AG39:AW39)*($AG39:AW39=2))>MAX(COLUMN($AG39:AW39)*($AG39:AW39=1))),IF(COLUMN(AX39)-MAX(COLUMN($AG39:AW39)*($AG39:AW39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AX39)-MAX(COLUMN($AG39:AW39)*($AG39:AW39=3))=$J39,3,0),IF(COLUMN(AX39)-MAX(COLUMN($AG39:AW39)*($AG39:AW39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AX39)*($AG39:AX39=1))>MAX(COLUMN($AG39:AX39)*($AG39:AX39=3)),MAX(COLUMN($AG39:AX39)*($AG39:AX39=1))>MAX(COLUMN($AG39:AX39)*($AG39:AX39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AY39)-MAX(COLUMN($AG39:AX39)*($AG39:AX39=1))=$J39,3,0),IF(COLUMN(AY39)-MAX(COLUMN($AG39:AX39)*($AG39:AX39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AX39)*($AG39:AX39=2))>MAX(COLUMN($AG39:AX39)*($AG39:AX39=3)),MAX(COLUMN($AG39:AX39)*($AG39:AX39=2))>MAX(COLUMN($AG39:AX39)*($AG39:AX39=1))),IF(COLUMN(AY39)-MAX(COLUMN($AG39:AX39)*($AG39:AX39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AY39)-MAX(COLUMN($AG39:AX39)*($AG39:AX39=3))=$J39,3,0),IF(COLUMN(AY39)-MAX(COLUMN($AG39:AX39)*($AG39:AX39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AY39)*($AG39:AY39=1))>MAX(COLUMN($AG39:AY39)*($AG39:AY39=3)),MAX(COLUMN($AG39:AY39)*($AG39:AY39=1))>MAX(COLUMN($AG39:AY39)*($AG39:AY39=2))),IF($K39=\"Not Possible\",IF(COLUMN(AZ39)-MAX(COLUMN($AG39:AY39)*($AG39:AY39=1))=$J39,3,0),IF(COLUMN(AZ39)-MAX(COLUMN($AG39:AY39)*($AG39:AY39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AY39)*($AG39:AY39=2))>MAX(COLUMN($AG39:AY39)*($AG39:AY39=3)),MAX(COLUMN($AG39:AY39)*($AG39:AY39=2))>MAX(COLUMN($AG39:AY39)*($AG39:AY39=1))),IF(COLUMN(AZ39)-MAX(COLUMN($AG39:AY39)*($AG39:AY39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(AZ39)-MAX(COLUMN($AG39:AY39)*($AG39:AY39=3))=$J39,3,0),IF(COLUMN(AZ39)-MAX(COLUMN($AG39:AY39)*($AG39:AY39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=1))>MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=3)),MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=1))>MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BA39)-MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=1))=$J39,3,0),IF(COLUMN(BA39)-MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=2))>MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=3)),MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=2))>MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=1))),IF(COLUMN(BA39)-MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BA39)-MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=3))=$J39,3,0),IF(COLUMN(BA39)-MAX(COLUMN($AG39:AZ39)*($AG39:AZ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BA39)*($AG39:BA39=1))>MAX(COLUMN($AG39:BA39)*($AG39:BA39=3)),MAX(COLUMN($AG39:BA39)*($AG39:BA39=1))>MAX(COLUMN($AG39:BA39)*($AG39:BA39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BB39)-MAX(COLUMN($AG39:BA39)*($AG39:BA39=1))=$J39,3,0),IF(COLUMN(BB39)-MAX(COLUMN($AG39:BA39)*($AG39:BA39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BA39)*($AG39:BA39=2))>MAX(COLUMN($AG39:BA39)*($AG39:BA39=3)),MAX(COLUMN($AG39:BA39)*($AG39:BA39=2))>MAX(COLUMN($AG39:BA39)*($AG39:BA39=1))),IF(COLUMN(BB39)-MAX(COLUMN($AG39:BA39)*($AG39:BA39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BB39)-MAX(COLUMN($AG39:BA39)*($AG39:BA39=3))=$J39,3,0),IF(COLUMN(BB39)-MAX(COLUMN($AG39:BA39)*($AG39:BA39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BB39)*($AG39:BB39=1))>MAX(COLUMN($AG39:BB39)*($AG39:BB39=3)),MAX(COLUMN($AG39:BB39)*($AG39:BB39=1))>MAX(COLUMN($AG39:BB39)*($AG39:BB39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BC39)-MAX(COLUMN($AG39:BB39)*($AG39:BB39=1))=$J39,3,0),IF(COLUMN(BC39)-MAX(COLUMN($AG39:BB39)*($AG39:BB39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BB39)*($AG39:BB39=2))>MAX(COLUMN($AG39:BB39)*($AG39:BB39=3)),MAX(COLUMN($AG39:BB39)*($AG39:BB39=2))>MAX(COLUMN($AG39:BB39)*($AG39:BB39=1))),IF(COLUMN(BC39)-MAX(COLUMN($AG39:BB39)*($AG39:BB39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BC39)-MAX(COLUMN($AG39:BB39)*($AG39:BB39=3))=$J39,3,0),IF(COLUMN(BC39)-MAX(COLUMN($AG39:BB39)*($AG39:BB39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BC39)*($AG39:BC39=1))>MAX(COLUMN($AG39:BC39)*($AG39:BC39=3)),MAX(COLUMN($AG39:BC39)*($AG39:BC39=1))>MAX(COLUMN($AG39:BC39)*($AG39:BC39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BD39)-MAX(COLUMN($AG39:BC39)*($AG39:BC39=1))=$J39,3,0),IF(COLUMN(BD39)-MAX(COLUMN($AG39:BC39)*($AG39:BC39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BC39)*($AG39:BC39=2))>MAX(COLUMN($AG39:BC39)*($AG39:BC39=3)),MAX(COLUMN($AG39:BC39)*($AG39:BC39=2))>MAX(COLUMN($AG39:BC39)*($AG39:BC39=1))),IF(COLUMN(BD39)-MAX(COLUMN($AG39:BC39)*($AG39:BC39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BD39)-MAX(COLUMN($AG39:BC39)*($AG39:BC39=3))=$J39,3,0),IF(COLUMN(BD39)-MAX(COLUMN($AG39:BC39)*($AG39:BC39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BD39)*($AG39:BD39=1))>MAX(COLUMN($AG39:BD39)*($AG39:BD39=3)),MAX(COLUMN($AG39:BD39)*($AG39:BD39=1))>MAX(COLUMN($AG39:BD39)*($AG39:BD39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BE39)-MAX(COLUMN($AG39:BD39)*($AG39:BD39=1))=$J39,3,0),IF(COLUMN(BE39)-MAX(COLUMN($AG39:BD39)*($AG39:BD39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BD39)*($AG39:BD39=2))>MAX(COLUMN($AG39:BD39)*($AG39:BD39=3)),MAX(COLUMN($AG39:BD39)*($AG39:BD39=2))>MAX(COLUMN($AG39:BD39)*($AG39:BD39=1))),IF(COLUMN(BE39)-MAX(COLUMN($AG39:BD39)*($AG39:BD39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BE39)-MAX(COLUMN($AG39:BD39)*($AG39:BD39=3))=$J39,3,0),IF(COLUMN(BE39)-MAX(COLUMN($AG39:BD39)*($AG39:BD39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BE39)*($AG39:BE39=1))>MAX(COLUMN($AG39:BE39)*($AG39:BE39=3)),MAX(COLUMN($AG39:BE39)*($AG39:BE39=1))>MAX(COLUMN($AG39:BE39)*($AG39:BE39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BF39)-MAX(COLUMN($AG39:BE39)*($AG39:BE39=1))=$J39,3,0),IF(COLUMN(BF39)-MAX(COLUMN($AG39:BE39)*($AG39:BE39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BE39)*($AG39:BE39=2))>MAX(COLUMN($AG39:BE39)*($AG39:BE39=3)),MAX(COLUMN($AG39:BE39)*($AG39:BE39=2))>MAX(COLUMN($AG39:BE39)*($AG39:BE39=1))),IF(COLUMN(BF39)-MAX(COLUMN($AG39:BE39)*($AG39:BE39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BF39)-MAX(COLUMN($AG39:BE39)*($AG39:BE39=3))=$J39,3,0),IF(COLUMN(BF39)-MAX(COLUMN($AG39:BE39)*($AG39:BE39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BF39)*($AG39:BF39=1))>MAX(COLUMN($AG39:BF39)*($AG39:BF39=3)),MAX(COLUMN($AG39:BF39)*($AG39:BF39=1))>MAX(COLUMN($AG39:BF39)*($AG39:BF39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BG39)-MAX(COLUMN($AG39:BF39)*($AG39:BF39=1))=$J39,3,0),IF(COLUMN(BG39)-MAX(COLUMN($AG39:BF39)*($AG39:BF39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BF39)*($AG39:BF39=2))>MAX(COLUMN($AG39:BF39)*($AG39:BF39=3)),MAX(COLUMN($AG39:BF39)*($AG39:BF39=2))>MAX(COLUMN($AG39:BF39)*($AG39:BF39=1))),IF(COLUMN(BG39)-MAX(COLUMN($AG39:BF39)*($AG39:BF39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BG39)-MAX(COLUMN($AG39:BF39)*($AG39:BF39=3))=$J39,3,0),IF(COLUMN(BG39)-MAX(COLUMN($AG39:BF39)*($AG39:BF39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BG39)*($AG39:BG39=1))>MAX(COLUMN($AG39:BG39)*($AG39:BG39=3)),MAX(COLUMN($AG39:BG39)*($AG39:BG39=1))>MAX(COLUMN($AG39:BG39)*($AG39:BG39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BH39)-MAX(COLUMN($AG39:BG39)*($AG39:BG39=1))=$J39,3,0),IF(COLUMN(BH39)-MAX(COLUMN($AG39:BG39)*($AG39:BG39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BG39)*($AG39:BG39=2))>MAX(COLUMN($AG39:BG39)*($AG39:BG39=3)),MAX(COLUMN($AG39:BG39)*($AG39:BG39=2))>MAX(COLUMN($AG39:BG39)*($AG39:BG39=1))),IF(COLUMN(BH39)-MAX(COLUMN($AG39:BG39)*($AG39:BG39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BH39)-MAX(COLUMN($AG39:BG39)*($AG39:BG39=3))=$J39,3,0),IF(COLUMN(BH39)-MAX(COLUMN($AG39:BG39)*($AG39:BG39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BH39)*($AG39:BH39=1))>MAX(COLUMN($AG39:BH39)*($AG39:BH39=3)),MAX(COLUMN($AG39:BH39)*($AG39:BH39=1))>MAX(COLUMN($AG39:BH39)*($AG39:BH39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BI39)-MAX(COLUMN($AG39:BH39)*($AG39:BH39=1))=$J39,3,0),IF(COLUMN(BI39)-MAX(COLUMN($AG39:BH39)*($AG39:BH39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BH39)*($AG39:BH39=2))>MAX(COLUMN($AG39:BH39)*($AG39:BH39=3)),MAX(COLUMN($AG39:BH39)*($AG39:BH39=2))>MAX(COLUMN($AG39:BH39)*($AG39:BH39=1))),IF(COLUMN(BI39)-MAX(COLUMN($AG39:BH39)*($AG39:BH39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BI39)-MAX(COLUMN($AG39:BH39)*($AG39:BH39=3))=$J39,3,0),IF(COLUMN(BI39)-MAX(COLUMN($AG39:BH39)*($AG39:BH39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BI39)*($AG39:BI39=1))>MAX(COLUMN($AG39:BI39)*($AG39:BI39=3)),MAX(COLUMN($AG39:BI39)*($AG39:BI39=1))>MAX(COLUMN($AG39:BI39)*($AG39:BI39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BJ39)-MAX(COLUMN($AG39:BI39)*($AG39:BI39=1))=$J39,3,0),IF(COLUMN(BJ39)-MAX(COLUMN($AG39:BI39)*($AG39:BI39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BI39)*($AG39:BI39=2))>MAX(COLUMN($AG39:BI39)*($AG39:BI39=3)),MAX(COLUMN($AG39:BI39)*($AG39:BI39=2))>MAX(COLUMN($AG39:BI39)*($AG39:BI39=1))),IF(COLUMN(BJ39)-MAX(COLUMN($AG39:BI39)*($AG39:BI39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BJ39)-MAX(COLUMN($AG39:BI39)*($AG39:BI39=3))=$J39,3,0),IF(COLUMN(BJ39)-MAX(COLUMN($AG39:BI39)*($AG39:BI39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=1))>MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=3)),MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=1))>MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BK39)-MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=1))=$J39,3,0),IF(COLUMN(BK39)-MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=2))>MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=3)),MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=2))>MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=1))),IF(COLUMN(BK39)-MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BK39)-MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=3))=$J39,3,0),IF(COLUMN(BK39)-MAX(COLUMN($AG39:BJ39)*($AG39:BJ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BK39)*($AG39:BK39=1))>MAX(COLUMN($AG39:BK39)*($AG39:BK39=3)),MAX(COLUMN($AG39:BK39)*($AG39:BK39=1))>MAX(COLUMN($AG39:BK39)*($AG39:BK39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BL39)-MAX(COLUMN($AG39:BK39)*($AG39:BK39=1))=$J39,3,0),IF(COLUMN(BL39)-MAX(COLUMN($AG39:BK39)*($AG39:BK39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BK39)*($AG39:BK39=2))>MAX(COLUMN($AG39:BK39)*($AG39:BK39=3)),MAX(COLUMN($AG39:BK39)*($AG39:BK39=2))>MAX(COLUMN($AG39:BK39)*($AG39:BK39=1))),IF(COLUMN(BL39)-MAX(COLUMN($AG39:BK39)*($AG39:BK39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BL39)-MAX(COLUMN($AG39:BK39)*($AG39:BK39=3))=$J39,3,0),IF(COLUMN(BL39)-MAX(COLUMN($AG39:BK39)*($AG39:BK39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BL39)*($AG39:BL39=1))>MAX(COLUMN($AG39:BL39)*($AG39:BL39=3)),MAX(COLUMN($AG39:BL39)*($AG39:BL39=1))>MAX(COLUMN($AG39:BL39)*($AG39:BL39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BM39)-MAX(COLUMN($AG39:BL39)*($AG39:BL39=1))=$J39,3,0),IF(COLUMN(BM39)-MAX(COLUMN($AG39:BL39)*($AG39:BL39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BL39)*($AG39:BL39=2))>MAX(COLUMN($AG39:BL39)*($AG39:BL39=3)),MAX(COLUMN($AG39:BL39)*($AG39:BL39=2))>MAX(COLUMN($AG39:BL39)*($AG39:BL39=1))),IF(COLUMN(BM39)-MAX(COLUMN($AG39:BL39)*($AG39:BL39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BM39)-MAX(COLUMN($AG39:BL39)*($AG39:BL39=3))=$J39,3,0),IF(COLUMN(BM39)-MAX(COLUMN($AG39:BL39)*($AG39:BL39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BM39)*($AG39:BM39=1))>MAX(COLUMN($AG39:BM39)*($AG39:BM39=3)),MAX(COLUMN($AG39:BM39)*($AG39:BM39=1))>MAX(COLUMN($AG39:BM39)*($AG39:BM39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BN39)-MAX(COLUMN($AG39:BM39)*($AG39:BM39=1))=$J39,3,0),IF(COLUMN(BN39)-MAX(COLUMN($AG39:BM39)*($AG39:BM39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BM39)*($AG39:BM39=2))>MAX(COLUMN($AG39:BM39)*($AG39:BM39=3)),MAX(COLUMN($AG39:BM39)*($AG39:BM39=2))>MAX(COLUMN($AG39:BM39)*($AG39:BM39=1))),IF(COLUMN(BN39)-MAX(COLUMN($AG39:BM39)*($AG39:BM39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BN39)-MAX(COLUMN($AG39:BM39)*($AG39:BM39=3))=$J39,3,0),IF(COLUMN(BN39)-MAX(COLUMN($AG39:BM39)*($AG39:BM39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BN39)*($AG39:BN39=1))>MAX(COLUMN($AG39:BN39)*($AG39:BN39=3)),MAX(COLUMN($AG39:BN39)*($AG39:BN39=1))>MAX(COLUMN($AG39:BN39)*($AG39:BN39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BO39)-MAX(COLUMN($AG39:BN39)*($AG39:BN39=1))=$J39,3,0),IF(COLUMN(BO39)-MAX(COLUMN($AG39:BN39)*($AG39:BN39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BN39)*($AG39:BN39=2))>MAX(COLUMN($AG39:BN39)*($AG39:BN39=3)),MAX(COLUMN($AG39:BN39)*($AG39:BN39=2))>MAX(COLUMN($AG39:BN39)*($AG39:BN39=1))),IF(COLUMN(BO39)-MAX(COLUMN($AG39:BN39)*($AG39:BN39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BO39)-MAX(COLUMN($AG39:BN39)*($AG39:BN39=3))=$J39,3,0),IF(COLUMN(BO39)-MAX(COLUMN($AG39:BN39)*($AG39:BN39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BO39)*($AG39:BO39=1))>MAX(COLUMN($AG39:BO39)*($AG39:BO39=3)),MAX(COLUMN($AG39:BO39)*($AG39:BO39=1))>MAX(COLUMN($AG39:BO39)*($AG39:BO39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BP39)-MAX(COLUMN($AG39:BO39)*($AG39:BO39=1))=$J39,3,0),IF(COLUMN(BP39)-MAX(COLUMN($AG39:BO39)*($AG39:BO39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BO39)*($AG39:BO39=2))>MAX(COLUMN($AG39:BO39)*($AG39:BO39=3)),MAX(COLUMN($AG39:BO39)*($AG39:BO39=2))>MAX(COLUMN($AG39:BO39)*($AG39:BO39=1))),IF(COLUMN(BP39)-MAX(COLUMN($AG39:BO39)*($AG39:BO39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BP39)-MAX(COLUMN($AG39:BO39)*($AG39:BO39=3))=$J39,3,0),IF(COLUMN(BP39)-MAX(COLUMN($AG39:BO39)*($AG39:BO39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BP39)*($AG39:BP39=1))>MAX(COLUMN($AG39:BP39)*($AG39:BP39=3)),MAX(COLUMN($AG39:BP39)*($AG39:BP39=1))>MAX(COLUMN($AG39:BP39)*($AG39:BP39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BQ39)-MAX(COLUMN($AG39:BP39)*($AG39:BP39=1))=$J39,3,0),IF(COLUMN(BQ39)-MAX(COLUMN($AG39:BP39)*($AG39:BP39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BP39)*($AG39:BP39=2))>MAX(COLUMN($AG39:BP39)*($AG39:BP39=3)),MAX(COLUMN($AG39:BP39)*($AG39:BP39=2))>MAX(COLUMN($AG39:BP39)*($AG39:BP39=1))),IF(COLUMN(BQ39)-MAX(COLUMN($AG39:BP39)*($AG39:BP39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BQ39)-MAX(COLUMN($AG39:BP39)*($AG39:BP39=3))=$J39,3,0),IF(COLUMN(BQ39)-MAX(COLUMN($AG39:BP39)*($AG39:BP39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=1))>MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=3)),MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=1))>MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BR39)-MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=1))=$J39,3,0),IF(COLUMN(BR39)-MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=2))>MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=3)),MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=2))>MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=1))),IF(COLUMN(BR39)-MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BR39)-MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=3))=$J39,3,0),IF(COLUMN(BR39)-MAX(COLUMN($AG39:BQ39)*($AG39:BQ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BR39)*($AG39:BR39=1))>MAX(COLUMN($AG39:BR39)*($AG39:BR39=3)),MAX(COLUMN($AG39:BR39)*($AG39:BR39=1))>MAX(COLUMN($AG39:BR39)*($AG39:BR39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BS39)-MAX(COLUMN($AG39:BR39)*($AG39:BR39=1))=$J39,3,0),IF(COLUMN(BS39)-MAX(COLUMN($AG39:BR39)*($AG39:BR39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BR39)*($AG39:BR39=2))>MAX(COLUMN($AG39:BR39)*($AG39:BR39=3)),MAX(COLUMN($AG39:BR39)*($AG39:BR39=2))>MAX(COLUMN($AG39:BR39)*($AG39:BR39=1))),IF(COLUMN(BS39)-MAX(COLUMN($AG39:BR39)*($AG39:BR39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BS39)-MAX(COLUMN($AG39:BR39)*($AG39:BR39=3))=$J39,3,0),IF(COLUMN(BS39)-MAX(COLUMN($AG39:BR39)*($AG39:BR39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BS39)*($AG39:BS39=1))>MAX(COLUMN($AG39:BS39)*($AG39:BS39=3)),MAX(COLUMN($AG39:BS39)*($AG39:BS39=1))>MAX(COLUMN($AG39:BS39)*($AG39:BS39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BT39)-MAX(COLUMN($AG39:BS39)*($AG39:BS39=1))=$J39,3,0),IF(COLUMN(BT39)-MAX(COLUMN($AG39:BS39)*($AG39:BS39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BS39)*($AG39:BS39=2))>MAX(COLUMN($AG39:BS39)*($AG39:BS39=3)),MAX(COLUMN($AG39:BS39)*($AG39:BS39=2))>MAX(COLUMN($AG39:BS39)*($AG39:BS39=1))),IF(COLUMN(BT39)-MAX(COLUMN($AG39:BS39)*($AG39:BS39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BT39)-MAX(COLUMN($AG39:BS39)*($AG39:BS39=3))=$J39,3,0),IF(COLUMN(BT39)-MAX(COLUMN($AG39:BS39)*($AG39:BS39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BT39)*($AG39:BT39=1))>MAX(COLUMN($AG39:BT39)*($AG39:BT39=3)),MAX(COLUMN($AG39:BT39)*($AG39:BT39=1))>MAX(COLUMN($AG39:BT39)*($AG39:BT39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BU39)-MAX(COLUMN($AG39:BT39)*($AG39:BT39=1))=$J39,3,0),IF(COLUMN(BU39)-MAX(COLUMN($AG39:BT39)*($AG39:BT39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BT39)*($AG39:BT39=2))>MAX(COLUMN($AG39:BT39)*($AG39:BT39=3)),MAX(COLUMN($AG39:BT39)*($AG39:BT39=2))>MAX(COLUMN($AG39:BT39)*($AG39:BT39=1))),IF(COLUMN(BU39)-MAX(COLUMN($AG39:BT39)*($AG39:BT39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BU39)-MAX(COLUMN($AG39:BT39)*($AG39:BT39=3))=$J39,3,0),IF(COLUMN(BU39)-MAX(COLUMN($AG39:BT39)*($AG39:BT39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BU39)*($AG39:BU39=1))>MAX(COLUMN($AG39:BU39)*($AG39:BU39=3)),MAX(COLUMN($AG39:BU39)*($AG39:BU39=1))>MAX(COLUMN($AG39:BU39)*($AG39:BU39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BV39)-MAX(COLUMN($AG39:BU39)*($AG39:BU39=1))=$J39,3,0),IF(COLUMN(BV39)-MAX(COLUMN($AG39:BU39)*($AG39:BU39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BU39)*($AG39:BU39=2))>MAX(COLUMN($AG39:BU39)*($AG39:BU39=3)),MAX(COLUMN($AG39:BU39)*($AG39:BU39=2))>MAX(COLUMN($AG39:BU39)*($AG39:BU39=1))),IF(COLUMN(BV39)-MAX(COLUMN($AG39:BU39)*($AG39:BU39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BV39)-MAX(COLUMN($AG39:BU39)*($AG39:BU39=3))=$J39,3,0),IF(COLUMN(BV39)-MAX(COLUMN($AG39:BU39)*($AG39:BU39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BV39)*($AG39:BV39=1))>MAX(COLUMN($AG39:BV39)*($AG39:BV39=3)),MAX(COLUMN($AG39:BV39)*($AG39:BV39=1))>MAX(COLUMN($AG39:BV39)*($AG39:BV39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BW39)-MAX(COLUMN($AG39:BV39)*($AG39:BV39=1))=$J39,3,0),IF(COLUMN(BW39)-MAX(COLUMN($AG39:BV39)*($AG39:BV39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BV39)*($AG39:BV39=2))>MAX(COLUMN($AG39:BV39)*($AG39:BV39=3)),MAX(COLUMN($AG39:BV39)*($AG39:BV39=2))>MAX(COLUMN($AG39:BV39)*($AG39:BV39=1))),IF(COLUMN(BW39)-MAX(COLUMN($AG39:BV39)*($AG39:BV39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BW39)-MAX(COLUMN($AG39:BV39)*($AG39:BV39=3))=$J39,3,0),IF(COLUMN(BW39)-MAX(COLUMN($AG39:BV39)*($AG39:BV39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BW39)*($AG39:BW39=1))>MAX(COLUMN($AG39:BW39)*($AG39:BW39=3)),MAX(COLUMN($AG39:BW39)*($AG39:BW39=1))>MAX(COLUMN($AG39:BW39)*($AG39:BW39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BX39)-MAX(COLUMN($AG39:BW39)*($AG39:BW39=1))=$J39,3,0),IF(COLUMN(BX39)-MAX(COLUMN($AG39:BW39)*($AG39:BW39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BW39)*($AG39:BW39=2))>MAX(COLUMN($AG39:BW39)*($AG39:BW39=3)),MAX(COLUMN($AG39:BW39)*($AG39:BW39=2))>MAX(COLUMN($AG39:BW39)*($AG39:BW39=1))),IF(COLUMN(BX39)-MAX(COLUMN($AG39:BW39)*($AG39:BW39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BX39)-MAX(COLUMN($AG39:BW39)*($AG39:BW39=3))=$J39,3,0),IF(COLUMN(BX39)-MAX(COLUMN($AG39:BW39)*($AG39:BW39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BX39)*($AG39:BX39=1))>MAX(COLUMN($AG39:BX39)*($AG39:BX39=3)),MAX(COLUMN($AG39:BX39)*($AG39:BX39=1))>MAX(COLUMN($AG39:BX39)*($AG39:BX39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BY39)-MAX(COLUMN($AG39:BX39)*($AG39:BX39=1))=$J39,3,0),IF(COLUMN(BY39)-MAX(COLUMN($AG39:BX39)*($AG39:BX39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BX39)*($AG39:BX39=2))>MAX(COLUMN($AG39:BX39)*($AG39:BX39=3)),MAX(COLUMN($AG39:BX39)*($AG39:BX39=2))>MAX(COLUMN($AG39:BX39)*($AG39:BX39=1))),IF(COLUMN(BY39)-MAX(COLUMN($AG39:BX39)*($AG39:BX39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BY39)-MAX(COLUMN($AG39:BX39)*($AG39:BX39=3))=$J39,3,0),IF(COLUMN(BY39)-MAX(COLUMN($AG39:BX39)*($AG39:BX39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BY39)*($AG39:BY39=1))>MAX(COLUMN($AG39:BY39)*($AG39:BY39=3)),MAX(COLUMN($AG39:BY39)*($AG39:BY39=1))>MAX(COLUMN($AG39:BY39)*($AG39:BY39=2))),IF($K39=\"Not Possible\",IF(COLUMN(BZ39)-MAX(COLUMN($AG39:BY39)*($AG39:BY39=1))=$J39,3,0),IF(COLUMN(BZ39)-MAX(COLUMN($AG39:BY39)*($AG39:BY39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BY39)*($AG39:BY39=2))>MAX(COLUMN($AG39:BY39)*($AG39:BY39=3)),MAX(COLUMN($AG39:BY39)*($AG39:BY39=2))>MAX(COLUMN($AG39:BY39)*($AG39:BY39=1))),IF(COLUMN(BZ39)-MAX(COLUMN($AG39:BY39)*($AG39:BY39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(BZ39)-MAX(COLUMN($AG39:BY39)*($AG39:BY39=3))=$J39,3,0),IF(COLUMN(BZ39)-MAX(COLUMN($AG39:BY39)*($AG39:BY39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=1))>MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=3)),MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=1))>MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CA39)-MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=1))=$J39,3,0),IF(COLUMN(CA39)-MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=2))>MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=3)),MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=2))>MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=1))),IF(COLUMN(CA39)-MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CA39)-MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=3))=$J39,3,0),IF(COLUMN(CA39)-MAX(COLUMN($AG39:BZ39)*($AG39:BZ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CA39)*($AG39:CA39=1))>MAX(COLUMN($AG39:CA39)*($AG39:CA39=3)),MAX(COLUMN($AG39:CA39)*($AG39:CA39=1))>MAX(COLUMN($AG39:CA39)*($AG39:CA39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CB39)-MAX(COLUMN($AG39:CA39)*($AG39:CA39=1))=$J39,3,0),IF(COLUMN(CB39)-MAX(COLUMN($AG39:CA39)*($AG39:CA39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CA39)*($AG39:CA39=2))>MAX(COLUMN($AG39:CA39)*($AG39:CA39=3)),MAX(COLUMN($AG39:CA39)*($AG39:CA39=2))>MAX(COLUMN($AG39:CA39)*($AG39:CA39=1))),IF(COLUMN(CB39)-MAX(COLUMN($AG39:CA39)*($AG39:CA39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CB39)-MAX(COLUMN($AG39:CA39)*($AG39:CA39=3))=$J39,3,0),IF(COLUMN(CB39)-MAX(COLUMN($AG39:CA39)*($AG39:CA39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CB39)*($AG39:CB39=1))>MAX(COLUMN($AG39:CB39)*($AG39:CB39=3)),MAX(COLUMN($AG39:CB39)*($AG39:CB39=1))>MAX(COLUMN($AG39:CB39)*($AG39:CB39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CC39)-MAX(COLUMN($AG39:CB39)*($AG39:CB39=1))=$J39,3,0),IF(COLUMN(CC39)-MAX(COLUMN($AG39:CB39)*($AG39:CB39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CB39)*($AG39:CB39=2))>MAX(COLUMN($AG39:CB39)*($AG39:CB39=3)),MAX(COLUMN($AG39:CB39)*($AG39:CB39=2))>MAX(COLUMN($AG39:CB39)*($AG39:CB39=1))),IF(COLUMN(CC39)-MAX(COLUMN($AG39:CB39)*($AG39:CB39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CC39)-MAX(COLUMN($AG39:CB39)*($AG39:CB39=3))=$J39,3,0),IF(COLUMN(CC39)-MAX(COLUMN($AG39:CB39)*($AG39:CB39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CC39)*($AG39:CC39=1))>MAX(COLUMN($AG39:CC39)*($AG39:CC39=3)),MAX(COLUMN($AG39:CC39)*($AG39:CC39=1))>MAX(COLUMN($AG39:CC39)*($AG39:CC39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CD39)-MAX(COLUMN($AG39:CC39)*($AG39:CC39=1))=$J39,3,0),IF(COLUMN(CD39)-MAX(COLUMN($AG39:CC39)*($AG39:CC39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CC39)*($AG39:CC39=2))>MAX(COLUMN($AG39:CC39)*($AG39:CC39=3)),MAX(COLUMN($AG39:CC39)*($AG39:CC39=2))>MAX(COLUMN($AG39:CC39)*($AG39:CC39=1))),IF(COLUMN(CD39)-MAX(COLUMN($AG39:CC39)*($AG39:CC39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CD39)-MAX(COLUMN($AG39:CC39)*($AG39:CC39=3))=$J39,3,0),IF(COLUMN(CD39)-MAX(COLUMN($AG39:CC39)*($AG39:CC39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CD39)*($AG39:CD39=1))>MAX(COLUMN($AG39:CD39)*($AG39:CD39=3)),MAX(COLUMN($AG39:CD39)*($AG39:CD39=1))>MAX(COLUMN($AG39:CD39)*($AG39:CD39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CE39)-MAX(COLUMN($AG39:CD39)*($AG39:CD39=1))=$J39,3,0),IF(COLUMN(CE39)-MAX(COLUMN($AG39:CD39)*($AG39:CD39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CD39)*($AG39:CD39=2))>MAX(COLUMN($AG39:CD39)*($AG39:CD39=3)),MAX(COLUMN($AG39:CD39)*($AG39:CD39=2))>MAX(COLUMN($AG39:CD39)*($AG39:CD39=1))),IF(COLUMN(CE39)-MAX(COLUMN($AG39:CD39)*($AG39:CD39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CE39)-MAX(COLUMN($AG39:CD39)*($AG39:CD39=3))=$J39,3,0),IF(COLUMN(CE39)-MAX(COLUMN($AG39:CD39)*($AG39:CD39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CE39)*($AG39:CE39=1))>MAX(COLUMN($AG39:CE39)*($AG39:CE39=3)),MAX(COLUMN($AG39:CE39)*($AG39:CE39=1))>MAX(COLUMN($AG39:CE39)*($AG39:CE39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CF39)-MAX(COLUMN($AG39:CE39)*($AG39:CE39=1))=$J39,3,0),IF(COLUMN(CF39)-MAX(COLUMN($AG39:CE39)*($AG39:CE39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CE39)*($AG39:CE39=2))>MAX(COLUMN($AG39:CE39)*($AG39:CE39=3)),MAX(COLUMN($AG39:CE39)*($AG39:CE39=2))>MAX(COLUMN($AG39:CE39)*($AG39:CE39=1))),IF(COLUMN(CF39)-MAX(COLUMN($AG39:CE39)*($AG39:CE39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CF39)-MAX(COLUMN($AG39:CE39)*($AG39:CE39=3))=$J39,3,0),IF(COLUMN(CF39)-MAX(COLUMN($AG39:CE39)*($AG39:CE39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CF39)*($AG39:CF39=1))>MAX(COLUMN($AG39:CF39)*($AG39:CF39=3)),MAX(COLUMN($AG39:CF39)*($AG39:CF39=1))>MAX(COLUMN($AG39:CF39)*($AG39:CF39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CG39)-MAX(COLUMN($AG39:CF39)*($AG39:CF39=1))=$J39,3,0),IF(COLUMN(CG39)-MAX(COLUMN($AG39:CF39)*($AG39:CF39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CF39)*($AG39:CF39=2))>MAX(COLUMN($AG39:CF39)*($AG39:CF39=3)),MAX(COLUMN($AG39:CF39)*($AG39:CF39=2))>MAX(COLUMN($AG39:CF39)*($AG39:CF39=1))),IF(COLUMN(CG39)-MAX(COLUMN($AG39:CF39)*($AG39:CF39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CG39)-MAX(COLUMN($AG39:CF39)*($AG39:CF39=3))=$J39,3,0),IF(COLUMN(CG39)-MAX(COLUMN($AG39:CF39)*($AG39:CF39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CG39)*($AG39:CG39=1))>MAX(COLUMN($AG39:CG39)*($AG39:CG39=3)),MAX(COLUMN($AG39:CG39)*($AG39:CG39=1))>MAX(COLUMN($AG39:CG39)*($AG39:CG39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CH39)-MAX(COLUMN($AG39:CG39)*($AG39:CG39=1))=$J39,3,0),IF(COLUMN(CH39)-MAX(COLUMN($AG39:CG39)*($AG39:CG39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CG39)*($AG39:CG39=2))>MAX(COLUMN($AG39:CG39)*($AG39:CG39=3)),MAX(COLUMN($AG39:CG39)*($AG39:CG39=2))>MAX(COLUMN($AG39:CG39)*($AG39:CG39=1))),IF(COLUMN(CH39)-MAX(COLUMN($AG39:CG39)*($AG39:CG39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CH39)-MAX(COLUMN($AG39:CG39)*($AG39:CG39=3))=$J39,3,0),IF(COLUMN(CH39)-MAX(COLUMN($AG39:CG39)*($AG39:CG39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CH39)*($AG39:CH39=1))>MAX(COLUMN($AG39:CH39)*($AG39:CH39=3)),MAX(COLUMN($AG39:CH39)*($AG39:CH39=1))>MAX(COLUMN($AG39:CH39)*($AG39:CH39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CI39)-MAX(COLUMN($AG39:CH39)*($AG39:CH39=1))=$J39,3,0),IF(COLUMN(CI39)-MAX(COLUMN($AG39:CH39)*($AG39:CH39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CH39)*($AG39:CH39=2))>MAX(COLUMN($AG39:CH39)*($AG39:CH39=3)),MAX(COLUMN($AG39:CH39)*($AG39:CH39=2))>MAX(COLUMN($AG39:CH39)*($AG39:CH39=1))),IF(COLUMN(CI39)-MAX(COLUMN($AG39:CH39)*($AG39:CH39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CI39)-MAX(COLUMN($AG39:CH39)*($AG39:CH39=3))=$J39,3,0),IF(COLUMN(CI39)-MAX(COLUMN($AG39:CH39)*($AG39:CH39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CI39)*($AG39:CI39=1))>MAX(COLUMN($AG39:CI39)*($AG39:CI39=3)),MAX(COLUMN($AG39:CI39)*($AG39:CI39=1))>MAX(COLUMN($AG39:CI39)*($AG39:CI39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CJ39)-MAX(COLUMN($AG39:CI39)*($AG39:CI39=1))=$J39,3,0),IF(COLUMN(CJ39)-MAX(COLUMN($AG39:CI39)*($AG39:CI39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CI39)*($AG39:CI39=2))>MAX(COLUMN($AG39:CI39)*($AG39:CI39=3)),MAX(COLUMN($AG39:CI39)*($AG39:CI39=2))>MAX(COLUMN($AG39:CI39)*($AG39:CI39=1))),IF(COLUMN(CJ39)-MAX(COLUMN($AG39:CI39)*($AG39:CI39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CJ39)-MAX(COLUMN($AG39:CI39)*($AG39:CI39=3))=$J39,3,0),IF(COLUMN(CJ39)-MAX(COLUMN($AG39:CI39)*($AG39:CI39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=1))>MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=3)),MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=1))>MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CK39)-MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=1))=$J39,3,0),IF(COLUMN(CK39)-MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=2))>MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=3)),MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=2))>MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=1))),IF(COLUMN(CK39)-MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CK39)-MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=3))=$J39,3,0),IF(COLUMN(CK39)-MAX(COLUMN($AG39:CJ39)*($AG39:CJ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CK39)*($AG39:CK39=1))>MAX(COLUMN($AG39:CK39)*($AG39:CK39=3)),MAX(COLUMN($AG39:CK39)*($AG39:CK39=1))>MAX(COLUMN($AG39:CK39)*($AG39:CK39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CL39)-MAX(COLUMN($AG39:CK39)*($AG39:CK39=1))=$J39,3,0),IF(COLUMN(CL39)-MAX(COLUMN($AG39:CK39)*($AG39:CK39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CK39)*($AG39:CK39=2))>MAX(COLUMN($AG39:CK39)*($AG39:CK39=3)),MAX(COLUMN($AG39:CK39)*($AG39:CK39=2))>MAX(COLUMN($AG39:CK39)*($AG39:CK39=1))),IF(COLUMN(CL39)-MAX(COLUMN($AG39:CK39)*($AG39:CK39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CL39)-MAX(COLUMN($AG39:CK39)*($AG39:CK39=3))=$J39,3,0),IF(COLUMN(CL39)-MAX(COLUMN($AG39:CK39)*($AG39:CK39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CL39)*($AG39:CL39=1))>MAX(COLUMN($AG39:CL39)*($AG39:CL39=3)),MAX(COLUMN($AG39:CL39)*($AG39:CL39=1))>MAX(COLUMN($AG39:CL39)*($AG39:CL39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CM39)-MAX(COLUMN($AG39:CL39)*($AG39:CL39=1))=$J39,3,0),IF(COLUMN(CM39)-MAX(COLUMN($AG39:CL39)*($AG39:CL39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CL39)*($AG39:CL39=2))>MAX(COLUMN($AG39:CL39)*($AG39:CL39=3)),MAX(COLUMN($AG39:CL39)*($AG39:CL39=2))>MAX(COLUMN($AG39:CL39)*($AG39:CL39=1))),IF(COLUMN(CM39)-MAX(COLUMN($AG39:CL39)*($AG39:CL39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CM39)-MAX(COLUMN($AG39:CL39)*($AG39:CL39=3))=$J39,3,0),IF(COLUMN(CM39)-MAX(COLUMN($AG39:CL39)*($AG39:CL39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CM39)*($AG39:CM39=1))>MAX(COLUMN($AG39:CM39)*($AG39:CM39=3)),MAX(COLUMN($AG39:CM39)*($AG39:CM39=1))>MAX(COLUMN($AG39:CM39)*($AG39:CM39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CN39)-MAX(COLUMN($AG39:CM39)*($AG39:CM39=1))=$J39,3,0),IF(COLUMN(CN39)-MAX(COLUMN($AG39:CM39)*($AG39:CM39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CM39)*($AG39:CM39=2))>MAX(COLUMN($AG39:CM39)*($AG39:CM39=3)),MAX(COLUMN($AG39:CM39)*($AG39:CM39=2))>MAX(COLUMN($AG39:CM39)*($AG39:CM39=1))),IF(COLUMN(CN39)-MAX(COLUMN($AG39:CM39)*($AG39:CM39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CN39)-MAX(COLUMN($AG39:CM39)*($AG39:CM39=3))=$J39,3,0),IF(COLUMN(CN39)-MAX(COLUMN($AG39:CM39)*($AG39:CM39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CN39)*($AG39:CN39=1))>MAX(COLUMN($AG39:CN39)*($AG39:CN39=3)),MAX(COLUMN($AG39:CN39)*($AG39:CN39=1))>MAX(COLUMN($AG39:CN39)*($AG39:CN39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CO39)-MAX(COLUMN($AG39:CN39)*($AG39:CN39=1))=$J39,3,0),IF(COLUMN(CO39)-MAX(COLUMN($AG39:CN39)*($AG39:CN39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CN39)*($AG39:CN39=2))>MAX(COLUMN($AG39:CN39)*($AG39:CN39=3)),MAX(COLUMN($AG39:CN39)*($AG39:CN39=2))>MAX(COLUMN($AG39:CN39)*($AG39:CN39=1))),IF(COLUMN(CO39)-MAX(COLUMN($AG39:CN39)*($AG39:CN39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CO39)-MAX(COLUMN($AG39:CN39)*($AG39:CN39=3))=$J39,3,0),IF(COLUMN(CO39)-MAX(COLUMN($AG39:CN39)*($AG39:CN39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CO39)*($AG39:CO39=1))>MAX(COLUMN($AG39:CO39)*($AG39:CO39=3)),MAX(COLUMN($AG39:CO39)*($AG39:CO39=1))>MAX(COLUMN($AG39:CO39)*($AG39:CO39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CP39)-MAX(COLUMN($AG39:CO39)*($AG39:CO39=1))=$J39,3,0),IF(COLUMN(CP39)-MAX(COLUMN($AG39:CO39)*($AG39:CO39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CO39)*($AG39:CO39=2))>MAX(COLUMN($AG39:CO39)*($AG39:CO39=3)),MAX(COLUMN($AG39:CO39)*($AG39:CO39=2))>MAX(COLUMN($AG39:CO39)*($AG39:CO39=1))),IF(COLUMN(CP39)-MAX(COLUMN($AG39:CO39)*($AG39:CO39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CP39)-MAX(COLUMN($AG39:CO39)*($AG39:CO39=3))=$J39,3,0),IF(COLUMN(CP39)-MAX(COLUMN($AG39:CO39)*($AG39:CO39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CP39)*($AG39:CP39=1))>MAX(COLUMN($AG39:CP39)*($AG39:CP39=3)),MAX(COLUMN($AG39:CP39)*($AG39:CP39=1))>MAX(COLUMN($AG39:CP39)*($AG39:CP39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CQ39)-MAX(COLUMN($AG39:CP39)*($AG39:CP39=1))=$J39,3,0),IF(COLUMN(CQ39)-MAX(COLUMN($AG39:CP39)*($AG39:CP39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CP39)*($AG39:CP39=2))>MAX(COLUMN($AG39:CP39)*($AG39:CP39=3)),MAX(COLUMN($AG39:CP39)*($AG39:CP39=2))>MAX(COLUMN($AG39:CP39)*($AG39:CP39=1))),IF(COLUMN(CQ39)-MAX(COLUMN($AG39:CP39)*($AG39:CP39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CQ39)-MAX(COLUMN($AG39:CP39)*($AG39:CP39=3))=$J39,3,0),IF(COLUMN(CQ39)-MAX(COLUMN($AG39:CP39)*($AG39:CP39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=1))>MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=3)),MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=1))>MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CR39)-MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=1))=$J39,3,0),IF(COLUMN(CR39)-MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=2))>MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=3)),MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=2))>MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=1))),IF(COLUMN(CR39)-MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CR39)-MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=3))=$J39,3,0),IF(COLUMN(CR39)-MAX(COLUMN($AG39:CQ39)*($AG39:CQ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CR39)*($AG39:CR39=1))>MAX(COLUMN($AG39:CR39)*($AG39:CR39=3)),MAX(COLUMN($AG39:CR39)*($AG39:CR39=1))>MAX(COLUMN($AG39:CR39)*($AG39:CR39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CS39)-MAX(COLUMN($AG39:CR39)*($AG39:CR39=1))=$J39,3,0),IF(COLUMN(CS39)-MAX(COLUMN($AG39:CR39)*($AG39:CR39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CR39)*($AG39:CR39=2))>MAX(COLUMN($AG39:CR39)*($AG39:CR39=3)),MAX(COLUMN($AG39:CR39)*($AG39:CR39=2))>MAX(COLUMN($AG39:CR39)*($AG39:CR39=1))),IF(COLUMN(CS39)-MAX(COLUMN($AG39:CR39)*($AG39:CR39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CS39)-MAX(COLUMN($AG39:CR39)*($AG39:CR39=3))=$J39,3,0),IF(COLUMN(CS39)-MAX(COLUMN($AG39:CR39)*($AG39:CR39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CS39)*($AG39:CS39=1))>MAX(COLUMN($AG39:CS39)*($AG39:CS39=3)),MAX(COLUMN($AG39:CS39)*($AG39:CS39=1))>MAX(COLUMN($AG39:CS39)*($AG39:CS39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CT39)-MAX(COLUMN($AG39:CS39)*($AG39:CS39=1))=$J39,3,0),IF(COLUMN(CT39)-MAX(COLUMN($AG39:CS39)*($AG39:CS39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CS39)*($AG39:CS39=2))>MAX(COLUMN($AG39:CS39)*($AG39:CS39=3)),MAX(COLUMN($AG39:CS39)*($AG39:CS39=2))>MAX(COLUMN($AG39:CS39)*($AG39:CS39=1))),IF(COLUMN(CT39)-MAX(COLUMN($AG39:CS39)*($AG39:CS39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CT39)-MAX(COLUMN($AG39:CS39)*($AG39:CS39=3))=$J39,3,0),IF(COLUMN(CT39)-MAX(COLUMN($AG39:CS39)*($AG39:CS39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CT39)*($AG39:CT39=1))>MAX(COLUMN($AG39:CT39)*($AG39:CT39=3)),MAX(COLUMN($AG39:CT39)*($AG39:CT39=1))>MAX(COLUMN($AG39:CT39)*($AG39:CT39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CU39)-MAX(COLUMN($AG39:CT39)*($AG39:CT39=1))=$J39,3,0),IF(COLUMN(CU39)-MAX(COLUMN($AG39:CT39)*($AG39:CT39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CT39)*($AG39:CT39=2))>MAX(COLUMN($AG39:CT39)*($AG39:CT39=3)),MAX(COLUMN($AG39:CT39)*($AG39:CT39=2))>MAX(COLUMN($AG39:CT39)*($AG39:CT39=1))),IF(COLUMN(CU39)-MAX(COLUMN($AG39:CT39)*($AG39:CT39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CU39)-MAX(COLUMN($AG39:CT39)*($AG39:CT39=3))=$J39,3,0),IF(COLUMN(CU39)-MAX(COLUMN($AG39:CT39)*($AG39:CT39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CU39)*($AG39:CU39=1))>MAX(COLUMN($AG39:CU39)*($AG39:CU39=3)),MAX(COLUMN($AG39:CU39)*($AG39:CU39=1))>MAX(COLUMN($AG39:CU39)*($AG39:CU39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CV39)-MAX(COLUMN($AG39:CU39)*($AG39:CU39=1))=$J39,3,0),IF(COLUMN(CV39)-MAX(COLUMN($AG39:CU39)*($AG39:CU39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CU39)*($AG39:CU39=2))>MAX(COLUMN($AG39:CU39)*($AG39:CU39=3)),MAX(COLUMN($AG39:CU39)*($AG39:CU39=2))>MAX(COLUMN($AG39:CU39)*($AG39:CU39=1))),IF(COLUMN(CV39)-MAX(COLUMN($AG39:CU39)*($AG39:CU39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CV39)-MAX(COLUMN($AG39:CU39)*($AG39:CU39=3))=$J39,3,0),IF(COLUMN(CV39)-MAX(COLUMN($AG39:CU39)*($AG39:CU39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CV39)*($AG39:CV39=1))>MAX(COLUMN($AG39:CV39)*($AG39:CV39=3)),MAX(COLUMN($AG39:CV39)*($AG39:CV39=1))>MAX(COLUMN($AG39:CV39)*($AG39:CV39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CW39)-MAX(COLUMN($AG39:CV39)*($AG39:CV39=1))=$J39,3,0),IF(COLUMN(CW39)-MAX(COLUMN($AG39:CV39)*($AG39:CV39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CV39)*($AG39:CV39=2))>MAX(COLUMN($AG39:CV39)*($AG39:CV39=3)),MAX(COLUMN($AG39:CV39)*($AG39:CV39=2))>MAX(COLUMN($AG39:CV39)*($AG39:CV39=1))),IF(COLUMN(CW39)-MAX(COLUMN($AG39:CV39)*($AG39:CV39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CW39)-MAX(COLUMN($AG39:CV39)*($AG39:CV39=3))=$J39,3,0),IF(COLUMN(CW39)-MAX(COLUMN($AG39:CV39)*($AG39:CV39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CW39)*($AG39:CW39=1))>MAX(COLUMN($AG39:CW39)*($AG39:CW39=3)),MAX(COLUMN($AG39:CW39)*($AG39:CW39=1))>MAX(COLUMN($AG39:CW39)*($AG39:CW39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CX39)-MAX(COLUMN($AG39:CW39)*($AG39:CW39=1))=$J39,3,0),IF(COLUMN(CX39)-MAX(COLUMN($AG39:CW39)*($AG39:CW39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CW39)*($AG39:CW39=2))>MAX(COLUMN($AG39:CW39)*($AG39:CW39=3)),MAX(COLUMN($AG39:CW39)*($AG39:CW39=2))>MAX(COLUMN($AG39:CW39)*($AG39:CW39=1))),IF(COLUMN(CX39)-MAX(COLUMN($AG39:CW39)*($AG39:CW39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CX39)-MAX(COLUMN($AG39:CW39)*($AG39:CW39=3))=$J39,3,0),IF(COLUMN(CX39)-MAX(COLUMN($AG39:CW39)*($AG39:CW39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CX39)*($AG39:CX39=1))>MAX(COLUMN($AG39:CX39)*($AG39:CX39=3)),MAX(COLUMN($AG39:CX39)*($AG39:CX39=1))>MAX(COLUMN($AG39:CX39)*($AG39:CX39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CY39)-MAX(COLUMN($AG39:CX39)*($AG39:CX39=1))=$J39,3,0),IF(COLUMN(CY39)-MAX(COLUMN($AG39:CX39)*($AG39:CX39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CX39)*($AG39:CX39=2))>MAX(COLUMN($AG39:CX39)*($AG39:CX39=3)),MAX(COLUMN($AG39:CX39)*($AG39:CX39=2))>MAX(COLUMN($AG39:CX39)*($AG39:CX39=1))),IF(COLUMN(CY39)-MAX(COLUMN($AG39:CX39)*($AG39:CX39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CY39)-MAX(COLUMN($AG39:CX39)*($AG39:CX39=3))=$J39,3,0),IF(COLUMN(CY39)-MAX(COLUMN($AG39:CX39)*($AG39:CX39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CY39)*($AG39:CY39=1))>MAX(COLUMN($AG39:CY39)*($AG39:CY39=3)),MAX(COLUMN($AG39:CY39)*($AG39:CY39=1))>MAX(COLUMN($AG39:CY39)*($AG39:CY39=2))),IF($K39=\"Not Possible\",IF(COLUMN(CZ39)-MAX(COLUMN($AG39:CY39)*($AG39:CY39=1))=$J39,3,0),IF(COLUMN(CZ39)-MAX(COLUMN($AG39:CY39)*($AG39:CY39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CY39)*($AG39:CY39=2))>MAX(COLUMN($AG39:CY39)*($AG39:CY39=3)),MAX(COLUMN($AG39:CY39)*($AG39:CY39=2))>MAX(COLUMN($AG39:CY39)*($AG39:CY39=1))),IF(COLUMN(CZ39)-MAX(COLUMN($AG39:CY39)*($AG39:CY39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(CZ39)-MAX(COLUMN($AG39:CY39)*($AG39:CY39=3))=$J39,3,0),IF(COLUMN(CZ39)-MAX(COLUMN($AG39:CY39)*($AG39:CY39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=1))>MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=3)),MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=1))>MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DA39)-MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=1))=$J39,3,0),IF(COLUMN(DA39)-MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=2))>MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=3)),MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=2))>MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=1))),IF(COLUMN(DA39)-MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DA39)-MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=3))=$J39,3,0),IF(COLUMN(DA39)-MAX(COLUMN($AG39:CZ39)*($AG39:CZ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DA39)*($AG39:DA39=1))>MAX(COLUMN($AG39:DA39)*($AG39:DA39=3)),MAX(COLUMN($AG39:DA39)*($AG39:DA39=1))>MAX(COLUMN($AG39:DA39)*($AG39:DA39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DB39)-MAX(COLUMN($AG39:DA39)*($AG39:DA39=1))=$J39,3,0),IF(COLUMN(DB39)-MAX(COLUMN($AG39:DA39)*($AG39:DA39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DA39)*($AG39:DA39=2))>MAX(COLUMN($AG39:DA39)*($AG39:DA39=3)),MAX(COLUMN($AG39:DA39)*($AG39:DA39=2))>MAX(COLUMN($AG39:DA39)*($AG39:DA39=1))),IF(COLUMN(DB39)-MAX(COLUMN($AG39:DA39)*($AG39:DA39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DB39)-MAX(COLUMN($AG39:DA39)*($AG39:DA39=3))=$J39,3,0),IF(COLUMN(DB39)-MAX(COLUMN($AG39:DA39)*($AG39:DA39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DB39)*($AG39:DB39=1))>MAX(COLUMN($AG39:DB39)*($AG39:DB39=3)),MAX(COLUMN($AG39:DB39)*($AG39:DB39=1))>MAX(COLUMN($AG39:DB39)*($AG39:DB39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DC39)-MAX(COLUMN($AG39:DB39)*($AG39:DB39=1))=$J39,3,0),IF(COLUMN(DC39)-MAX(COLUMN($AG39:DB39)*($AG39:DB39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DB39)*($AG39:DB39=2))>MAX(COLUMN($AG39:DB39)*($AG39:DB39=3)),MAX(COLUMN($AG39:DB39)*($AG39:DB39=2))>MAX(COLUMN($AG39:DB39)*($AG39:DB39=1))),IF(COLUMN(DC39)-MAX(COLUMN($AG39:DB39)*($AG39:DB39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DC39)-MAX(COLUMN($AG39:DB39)*($AG39:DB39=3))=$J39,3,0),IF(COLUMN(DC39)-MAX(COLUMN($AG39:DB39)*($AG39:DB39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DC39)*($AG39:DC39=1))>MAX(COLUMN($AG39:DC39)*($AG39:DC39=3)),MAX(COLUMN($AG39:DC39)*($AG39:DC39=1))>MAX(COLUMN($AG39:DC39)*($AG39:DC39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DD39)-MAX(COLUMN($AG39:DC39)*($AG39:DC39=1))=$J39,3,0),IF(COLUMN(DD39)-MAX(COLUMN($AG39:DC39)*($AG39:DC39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DC39)*($AG39:DC39=2))>MAX(COLUMN($AG39:DC39)*($AG39:DC39=3)),MAX(COLUMN($AG39:DC39)*($AG39:DC39=2))>MAX(COLUMN($AG39:DC39)*($AG39:DC39=1))),IF(COLUMN(DD39)-MAX(COLUMN($AG39:DC39)*($AG39:DC39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DD39)-MAX(COLUMN($AG39:DC39)*($AG39:DC39=3))=$J39,3,0),IF(COLUMN(DD39)-MAX(COLUMN($AG39:DC39)*($AG39:DC39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DD39)*($AG39:DD39=1))>MAX(COLUMN($AG39:DD39)*($AG39:DD39=3)),MAX(COLUMN($AG39:DD39)*($AG39:DD39=1))>MAX(COLUMN($AG39:DD39)*($AG39:DD39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DE39)-MAX(COLUMN($AG39:DD39)*($AG39:DD39=1))=$J39,3,0),IF(COLUMN(DE39)-MAX(COLUMN($AG39:DD39)*($AG39:DD39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DD39)*($AG39:DD39=2))>MAX(COLUMN($AG39:DD39)*($AG39:DD39=3)),MAX(COLUMN($AG39:DD39)*($AG39:DD39=2))>MAX(COLUMN($AG39:DD39)*($AG39:DD39=1))),IF(COLUMN(DE39)-MAX(COLUMN($AG39:DD39)*($AG39:DD39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DE39)-MAX(COLUMN($AG39:DD39)*($AG39:DD39=3))=$J39,3,0),IF(COLUMN(DE39)-MAX(COLUMN($AG39:DD39)*($AG39:DD39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DE39)*($AG39:DE39=1))>MAX(COLUMN($AG39:DE39)*($AG39:DE39=3)),MAX(COLUMN($AG39:DE39)*($AG39:DE39=1))>MAX(COLUMN($AG39:DE39)*($AG39:DE39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DF39)-MAX(COLUMN($AG39:DE39)*($AG39:DE39=1))=$J39,3,0),IF(COLUMN(DF39)-MAX(COLUMN($AG39:DE39)*($AG39:DE39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DE39)*($AG39:DE39=2))>MAX(COLUMN($AG39:DE39)*($AG39:DE39=3)),MAX(COLUMN($AG39:DE39)*($AG39:DE39=2))>MAX(COLUMN($AG39:DE39)*($AG39:DE39=1))),IF(COLUMN(DF39)-MAX(COLUMN($AG39:DE39)*($AG39:DE39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DF39)-MAX(COLUMN($AG39:DE39)*($AG39:DE39=3))=$J39,3,0),IF(COLUMN(DF39)-MAX(COLUMN($AG39:DE39)*($AG39:DE39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DF39)*($AG39:DF39=1))>MAX(COLUMN($AG39:DF39)*($AG39:DF39=3)),MAX(COLUMN($AG39:DF39)*($AG39:DF39=1))>MAX(COLUMN($AG39:DF39)*($AG39:DF39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DG39)-MAX(COLUMN($AG39:DF39)*($AG39:DF39=1))=$J39,3,0),IF(COLUMN(DG39)-MAX(COLUMN($AG39:DF39)*($AG39:DF39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DF39)*($AG39:DF39=2))>MAX(COLUMN($AG39:DF39)*($AG39:DF39=3)),MAX(COLUMN($AG39:DF39)*($AG39:DF39=2))>MAX(COLUMN($AG39:DF39)*($AG39:DF39=1))),IF(COLUMN(DG39)-MAX(COLUMN($AG39:DF39)*($AG39:DF39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DG39)-MAX(COLUMN($AG39:DF39)*($AG39:DF39=3))=$J39,3,0),IF(COLUMN(DG39)-MAX(COLUMN($AG39:DF39)*($AG39:DF39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DG39)*($AG39:DG39=1))>MAX(COLUMN($AG39:DG39)*($AG39:DG39=3)),MAX(COLUMN($AG39:DG39)*($AG39:DG39=1))>MAX(COLUMN($AG39:DG39)*($AG39:DG39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DH39)-MAX(COLUMN($AG39:DG39)*($AG39:DG39=1))=$J39,3,0),IF(COLUMN(DH39)-MAX(COLUMN($AG39:DG39)*($AG39:DG39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DG39)*($AG39:DG39=2))>MAX(COLUMN($AG39:DG39)*($AG39:DG39=3)),MAX(COLUMN($AG39:DG39)*($AG39:DG39=2))>MAX(COLUMN($AG39:DG39)*($AG39:DG39=1))),IF(COLUMN(DH39)-MAX(COLUMN($AG39:DG39)*($AG39:DG39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DH39)-MAX(COLUMN($AG39:DG39)*($AG39:DG39=3))=$J39,3,0),IF(COLUMN(DH39)-MAX(COLUMN($AG39:DG39)*($AG39:DG39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DH39)*($AG39:DH39=1))>MAX(COLUMN($AG39:DH39)*($AG39:DH39=3)),MAX(COLUMN($AG39:DH39)*($AG39:DH39=1))>MAX(COLUMN($AG39:DH39)*($AG39:DH39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DI39)-MAX(COLUMN($AG39:DH39)*($AG39:DH39=1))=$J39,3,0),IF(COLUMN(DI39)-MAX(COLUMN($AG39:DH39)*($AG39:DH39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DH39)*($AG39:DH39=2))>MAX(COLUMN($AG39:DH39)*($AG39:DH39=3)),MAX(COLUMN($AG39:DH39)*($AG39:DH39=2))>MAX(COLUMN($AG39:DH39)*($AG39:DH39=1))),IF(COLUMN(DI39)-MAX(COLUMN($AG39:DH39)*($AG39:DH39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DI39)-MAX(COLUMN($AG39:DH39)*($AG39:DH39=3))=$J39,3,0),IF(COLUMN(DI39)-MAX(COLUMN($AG39:DH39)*($AG39:DH39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DI39)*($AG39:DI39=1))>MAX(COLUMN($AG39:DI39)*($AG39:DI39=3)),MAX(COLUMN($AG39:DI39)*($AG39:DI39=1))>MAX(COLUMN($AG39:DI39)*($AG39:DI39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DJ39)-MAX(COLUMN($AG39:DI39)*($AG39:DI39=1))=$J39,3,0),IF(COLUMN(DJ39)-MAX(COLUMN($AG39:DI39)*($AG39:DI39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DI39)*($AG39:DI39=2))>MAX(COLUMN($AG39:DI39)*($AG39:DI39=3)),MAX(COLUMN($AG39:DI39)*($AG39:DI39=2))>MAX(COLUMN($AG39:DI39)*($AG39:DI39=1))),IF(COLUMN(DJ39)-MAX(COLUMN($AG39:DI39)*($AG39:DI39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DJ39)-MAX(COLUMN($AG39:DI39)*($AG39:DI39=3))=$J39,3,0),IF(COLUMN(DJ39)-MAX(COLUMN($AG39:DI39)*($AG39:DI39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=1))>MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=3)),MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=1))>MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DK39)-MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=1))=$J39,3,0),IF(COLUMN(DK39)-MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=2))>MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=3)),MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=2))>MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=1))),IF(COLUMN(DK39)-MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DK39)-MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=3))=$J39,3,0),IF(COLUMN(DK39)-MAX(COLUMN($AG39:DJ39)*($AG39:DJ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DK39)*($AG39:DK39=1))>MAX(COLUMN($AG39:DK39)*($AG39:DK39=3)),MAX(COLUMN($AG39:DK39)*($AG39:DK39=1))>MAX(COLUMN($AG39:DK39)*($AG39:DK39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DL39)-MAX(COLUMN($AG39:DK39)*($AG39:DK39=1))=$J39,3,0),IF(COLUMN(DL39)-MAX(COLUMN($AG39:DK39)*($AG39:DK39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DK39)*($AG39:DK39=2))>MAX(COLUMN($AG39:DK39)*($AG39:DK39=3)),MAX(COLUMN($AG39:DK39)*($AG39:DK39=2))>MAX(COLUMN($AG39:DK39)*($AG39:DK39=1))),IF(COLUMN(DL39)-MAX(COLUMN($AG39:DK39)*($AG39:DK39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DL39)-MAX(COLUMN($AG39:DK39)*($AG39:DK39=3))=$J39,3,0),IF(COLUMN(DL39)-MAX(COLUMN($AG39:DK39)*($AG39:DK39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DL39)*($AG39:DL39=1))>MAX(COLUMN($AG39:DL39)*($AG39:DL39=3)),MAX(COLUMN($AG39:DL39)*($AG39:DL39=1))>MAX(COLUMN($AG39:DL39)*($AG39:DL39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DM39)-MAX(COLUMN($AG39:DL39)*($AG39:DL39=1))=$J39,3,0),IF(COLUMN(DM39)-MAX(COLUMN($AG39:DL39)*($AG39:DL39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DL39)*($AG39:DL39=2))>MAX(COLUMN($AG39:DL39)*($AG39:DL39=3)),MAX(COLUMN($AG39:DL39)*($AG39:DL39=2))>MAX(COLUMN($AG39:DL39)*($AG39:DL39=1))),IF(COLUMN(DM39)-MAX(COLUMN($AG39:DL39)*($AG39:DL39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DM39)-MAX(COLUMN($AG39:DL39)*($AG39:DL39=3))=$J39,3,0),IF(COLUMN(DM39)-MAX(COLUMN($AG39:DL39)*($AG39:DL39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DM39)*($AG39:DM39=1))>MAX(COLUMN($AG39:DM39)*($AG39:DM39=3)),MAX(COLUMN($AG39:DM39)*($AG39:DM39=1))>MAX(COLUMN($AG39:DM39)*($AG39:DM39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DN39)-MAX(COLUMN($AG39:DM39)*($AG39:DM39=1))=$J39,3,0),IF(COLUMN(DN39)-MAX(COLUMN($AG39:DM39)*($AG39:DM39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DM39)*($AG39:DM39=2))>MAX(COLUMN($AG39:DM39)*($AG39:DM39=3)),MAX(COLUMN($AG39:DM39)*($AG39:DM39=2))>MAX(COLUMN($AG39:DM39)*($AG39:DM39=1))),IF(COLUMN(DN39)-MAX(COLUMN($AG39:DM39)*($AG39:DM39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DN39)-MAX(COLUMN($AG39:DM39)*($AG39:DM39=3))=$J39,3,0),IF(COLUMN(DN39)-MAX(COLUMN($AG39:DM39)*($AG39:DM39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DN39)*($AG39:DN39=1))>MAX(COLUMN($AG39:DN39)*($AG39:DN39=3)),MAX(COLUMN($AG39:DN39)*($AG39:DN39=1))>MAX(COLUMN($AG39:DN39)*($AG39:DN39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DO39)-MAX(COLUMN($AG39:DN39)*($AG39:DN39=1))=$J39,3,0),IF(COLUMN(DO39)-MAX(COLUMN($AG39:DN39)*($AG39:DN39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DN39)*($AG39:DN39=2))>MAX(COLUMN($AG39:DN39)*($AG39:DN39=3)),MAX(COLUMN($AG39:DN39)*($AG39:DN39=2))>MAX(COLUMN($AG39:DN39)*($AG39:DN39=1))),IF(COLUMN(DO39)-MAX(COLUMN($AG39:DN39)*($AG39:DN39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DO39)-MAX(COLUMN($AG39:DN39)*($AG39:DN39=3))=$J39,3,0),IF(COLUMN(DO39)-MAX(COLUMN($AG39:DN39)*($AG39:DN39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DO39)*($AG39:DO39=1))>MAX(COLUMN($AG39:DO39)*($AG39:DO39=3)),MAX(COLUMN($AG39:DO39)*($AG39:DO39=1))>MAX(COLUMN($AG39:DO39)*($AG39:DO39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DP39)-MAX(COLUMN($AG39:DO39)*($AG39:DO39=1))=$J39,3,0),IF(COLUMN(DP39)-MAX(COLUMN($AG39:DO39)*($AG39:DO39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DO39)*($AG39:DO39=2))>MAX(COLUMN($AG39:DO39)*($AG39:DO39=3)),MAX(COLUMN($AG39:DO39)*($AG39:DO39=2))>MAX(COLUMN($AG39:DO39)*($AG39:DO39=1))),IF(COLUMN(DP39)-MAX(COLUMN($AG39:DO39)*($AG39:DO39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DP39)-MAX(COLUMN($AG39:DO39)*($AG39:DO39=3))=$J39,3,0),IF(COLUMN(DP39)-MAX(COLUMN($AG39:DO39)*($AG39:DO39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DP39)*($AG39:DP39=1))>MAX(COLUMN($AG39:DP39)*($AG39:DP39=3)),MAX(COLUMN($AG39:DP39)*($AG39:DP39=1))>MAX(COLUMN($AG39:DP39)*($AG39:DP39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DQ39)-MAX(COLUMN($AG39:DP39)*($AG39:DP39=1))=$J39,3,0),IF(COLUMN(DQ39)-MAX(COLUMN($AG39:DP39)*($AG39:DP39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DP39)*($AG39:DP39=2))>MAX(COLUMN($AG39:DP39)*($AG39:DP39=3)),MAX(COLUMN($AG39:DP39)*($AG39:DP39=2))>MAX(COLUMN($AG39:DP39)*($AG39:DP39=1))),IF(COLUMN(DQ39)-MAX(COLUMN($AG39:DP39)*($AG39:DP39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DQ39)-MAX(COLUMN($AG39:DP39)*($AG39:DP39=3))=$J39,3,0),IF(COLUMN(DQ39)-MAX(COLUMN($AG39:DP39)*($AG39:DP39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=1))>MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=3)),MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=1))>MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DR39)-MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=1))=$J39,3,0),IF(COLUMN(DR39)-MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=2))>MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=3)),MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=2))>MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=1))),IF(COLUMN(DR39)-MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DR39)-MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=3))=$J39,3,0),IF(COLUMN(DR39)-MAX(COLUMN($AG39:DQ39)*($AG39:DQ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DR39)*($AG39:DR39=1))>MAX(COLUMN($AG39:DR39)*($AG39:DR39=3)),MAX(COLUMN($AG39:DR39)*($AG39:DR39=1))>MAX(COLUMN($AG39:DR39)*($AG39:DR39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DS39)-MAX(COLUMN($AG39:DR39)*($AG39:DR39=1))=$J39,3,0),IF(COLUMN(DS39)-MAX(COLUMN($AG39:DR39)*($AG39:DR39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DR39)*($AG39:DR39=2))>MAX(COLUMN($AG39:DR39)*($AG39:DR39=3)),MAX(COLUMN($AG39:DR39)*($AG39:DR39=2))>MAX(COLUMN($AG39:DR39)*($AG39:DR39=1))),IF(COLUMN(DS39)-MAX(COLUMN($AG39:DR39)*($AG39:DR39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DS39)-MAX(COLUMN($AG39:DR39)*($AG39:DR39=3))=$J39,3,0),IF(COLUMN(DS39)-MAX(COLUMN($AG39:DR39)*($AG39:DR39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DS39)*($AG39:DS39=1))>MAX(COLUMN($AG39:DS39)*($AG39:DS39=3)),MAX(COLUMN($AG39:DS39)*($AG39:DS39=1))>MAX(COLUMN($AG39:DS39)*($AG39:DS39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DT39)-MAX(COLUMN($AG39:DS39)*($AG39:DS39=1))=$J39,3,0),IF(COLUMN(DT39)-MAX(COLUMN($AG39:DS39)*($AG39:DS39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DS39)*($AG39:DS39=2))>MAX(COLUMN($AG39:DS39)*($AG39:DS39=3)),MAX(COLUMN($AG39:DS39)*($AG39:DS39=2))>MAX(COLUMN($AG39:DS39)*($AG39:DS39=1))),IF(COLUMN(DT39)-MAX(COLUMN($AG39:DS39)*($AG39:DS39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DT39)-MAX(COLUMN($AG39:DS39)*($AG39:DS39=3))=$J39,3,0),IF(COLUMN(DT39)-MAX(COLUMN($AG39:DS39)*($AG39:DS39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DT39)*($AG39:DT39=1))>MAX(COLUMN($AG39:DT39)*($AG39:DT39=3)),MAX(COLUMN($AG39:DT39)*($AG39:DT39=1))>MAX(COLUMN($AG39:DT39)*($AG39:DT39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DU39)-MAX(COLUMN($AG39:DT39)*($AG39:DT39=1))=$J39,3,0),IF(COLUMN(DU39)-MAX(COLUMN($AG39:DT39)*($AG39:DT39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DT39)*($AG39:DT39=2))>MAX(COLUMN($AG39:DT39)*($AG39:DT39=3)),MAX(COLUMN($AG39:DT39)*($AG39:DT39=2))>MAX(COLUMN($AG39:DT39)*($AG39:DT39=1))),IF(COLUMN(DU39)-MAX(COLUMN($AG39:DT39)*($AG39:DT39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DU39)-MAX(COLUMN($AG39:DT39)*($AG39:DT39=3))=$J39,3,0),IF(COLUMN(DU39)-MAX(COLUMN($AG39:DT39)*($AG39:DT39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DU39)*($AG39:DU39=1))>MAX(COLUMN($AG39:DU39)*($AG39:DU39=3)),MAX(COLUMN($AG39:DU39)*($AG39:DU39=1))>MAX(COLUMN($AG39:DU39)*($AG39:DU39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DV39)-MAX(COLUMN($AG39:DU39)*($AG39:DU39=1))=$J39,3,0),IF(COLUMN(DV39)-MAX(COLUMN($AG39:DU39)*($AG39:DU39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DU39)*($AG39:DU39=2))>MAX(COLUMN($AG39:DU39)*($AG39:DU39=3)),MAX(COLUMN($AG39:DU39)*($AG39:DU39=2))>MAX(COLUMN($AG39:DU39)*($AG39:DU39=1))),IF(COLUMN(DV39)-MAX(COLUMN($AG39:DU39)*($AG39:DU39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DV39)-MAX(COLUMN($AG39:DU39)*($AG39:DU39=3))=$J39,3,0),IF(COLUMN(DV39)-MAX(COLUMN($AG39:DU39)*($AG39:DU39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DV39)*($AG39:DV39=1))>MAX(COLUMN($AG39:DV39)*($AG39:DV39=3)),MAX(COLUMN($AG39:DV39)*($AG39:DV39=1))>MAX(COLUMN($AG39:DV39)*($AG39:DV39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DW39)-MAX(COLUMN($AG39:DV39)*($AG39:DV39=1))=$J39,3,0),IF(COLUMN(DW39)-MAX(COLUMN($AG39:DV39)*($AG39:DV39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DV39)*($AG39:DV39=2))>MAX(COLUMN($AG39:DV39)*($AG39:DV39=3)),MAX(COLUMN($AG39:DV39)*($AG39:DV39=2))>MAX(COLUMN($AG39:DV39)*($AG39:DV39=1))),IF(COLUMN(DW39)-MAX(COLUMN($AG39:DV39)*($AG39:DV39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DW39)-MAX(COLUMN($AG39:DV39)*($AG39:DV39=3))=$J39,3,0),IF(COLUMN(DW39)-MAX(COLUMN($AG39:DV39)*($AG39:DV39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DW39)*($AG39:DW39=1))>MAX(COLUMN($AG39:DW39)*($AG39:DW39=3)),MAX(COLUMN($AG39:DW39)*($AG39:DW39=1))>MAX(COLUMN($AG39:DW39)*($AG39:DW39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DX39)-MAX(COLUMN($AG39:DW39)*($AG39:DW39=1))=$J39,3,0),IF(COLUMN(DX39)-MAX(COLUMN($AG39:DW39)*($AG39:DW39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DW39)*($AG39:DW39=2))>MAX(COLUMN($AG39:DW39)*($AG39:DW39=3)),MAX(COLUMN($AG39:DW39)*($AG39:DW39=2))>MAX(COLUMN($AG39:DW39)*($AG39:DW39=1))),IF(COLUMN(DX39)-MAX(COLUMN($AG39:DW39)*($AG39:DW39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DX39)-MAX(COLUMN($AG39:DW39)*($AG39:DW39=3))=$J39,3,0),IF(COLUMN(DX39)-MAX(COLUMN($AG39:DW39)*($AG39:DW39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DX39)*($AG39:DX39=1))>MAX(COLUMN($AG39:DX39)*($AG39:DX39=3)),MAX(COLUMN($AG39:DX39)*($AG39:DX39=1))>MAX(COLUMN($AG39:DX39)*($AG39:DX39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DY39)-MAX(COLUMN($AG39:DX39)*($AG39:DX39=1))=$J39,3,0),IF(COLUMN(DY39)-MAX(COLUMN($AG39:DX39)*($AG39:DX39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DX39)*($AG39:DX39=2))>MAX(COLUMN($AG39:DX39)*($AG39:DX39=3)),MAX(COLUMN($AG39:DX39)*($AG39:DX39=2))>MAX(COLUMN($AG39:DX39)*($AG39:DX39=1))),IF(COLUMN(DY39)-MAX(COLUMN($AG39:DX39)*($AG39:DX39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DY39)-MAX(COLUMN($AG39:DX39)*($AG39:DX39=3))=$J39,3,0),IF(COLUMN(DY39)-MAX(COLUMN($AG39:DX39)*($AG39:DX39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DY39)*($AG39:DY39=1))>MAX(COLUMN($AG39:DY39)*($AG39:DY39=3)),MAX(COLUMN($AG39:DY39)*($AG39:DY39=1))>MAX(COLUMN($AG39:DY39)*($AG39:DY39=2))),IF($K39=\"Not Possible\",IF(COLUMN(DZ39)-MAX(COLUMN($AG39:DY39)*($AG39:DY39=1))=$J39,3,0),IF(COLUMN(DZ39)-MAX(COLUMN($AG39:DY39)*($AG39:DY39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DY39)*($AG39:DY39=2))>MAX(COLUMN($AG39:DY39)*($AG39:DY39=3)),MAX(COLUMN($AG39:DY39)*($AG39:DY39=2))>MAX(COLUMN($AG39:DY39)*($AG39:DY39=1))),IF(COLUMN(DZ39)-MAX(COLUMN($AG39:DY39)*($AG39:DY39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(DZ39)-MAX(COLUMN($AG39:DY39)*($AG39:DY39=3))=$J39,3,0),IF(COLUMN(DZ39)-MAX(COLUMN($AG39:DY39)*($AG39:DY39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=1))>MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=3)),MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=1))>MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=2))),IF($K39=\"Not Possible\",IF(COLUMN(EA39)-MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=1))=$J39,3,0),IF(COLUMN(EA39)-MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=2))>MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=3)),MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=2))>MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=1))),IF(COLUMN(EA39)-MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(EA39)-MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=3))=$J39,3,0),IF(COLUMN(EA39)-MAX(COLUMN($AG39:DZ39)*($AG39:DZ39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:EA39)*($AG39:EA39=1))>MAX(COLUMN($AG39:EA39)*($AG39:EA39=3)),MAX(COLUMN($AG39:EA39)*($AG39:EA39=1))>MAX(COLUMN($AG39:EA39)*($AG39:EA39=2))),IF($K39=\"Not Possible\",IF(COLUMN(EB39)-MAX(COLUMN($AG39:EA39)*($AG39:EA39=1))=$J39,3,0),IF(COLUMN(EB39)-MAX(COLUMN($AG39:EA39)*($AG39:EA39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:EA39)*($AG39:EA39=2))>MAX(COLUMN($AG39:EA39)*($AG39:EA39=3)),MAX(COLUMN($AG39:EA39)*($AG39:EA39=2))>MAX(COLUMN($AG39:EA39)*($AG39:EA39=1))),IF(COLUMN(EB39)-MAX(COLUMN($AG39:EA39)*($AG39:EA39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(EB39)-MAX(COLUMN($AG39:EA39)*($AG39:EA39=3))=$J39,3,0),IF(COLUMN(EB39)-MAX(COLUMN($AG39:EA39)*($AG39:EA39=3))=$J39,2,0)))))","v":0},{"$f":"IF($AG39=4,0,IF(AND(MAX(COLUMN($AG39:EB39)*($AG39:EB39=1))>MAX(COLUMN($AG39:EB39)*($AG39:EB39=3)),MAX(COLUMN($AG39:EB39)*($AG39:EB39=1))>MAX(COLUMN($AG39:EB39)*($AG39:EB39=2))),IF($K39=\"Not Possible\",IF(COLUMN(EC39)-MAX(COLUMN($AG39:EB39)*($AG39:EB39=1))=$J39,3,0),IF(COLUMN(EC39)-MAX(COLUMN($AG39:EB39)*($AG39:EB39=1))=$J39,2,0)),IF(AND(MAX(COLUMN($AG39:EB39)*($AG39:EB39=2))>MAX(COLUMN($AG39:EB39)*($AG39:EB39=3)),MAX(COLUMN($AG39:EB39)*($AG39:EB39=2))>MAX(COLUMN($AG39:EB39)*($AG39:EB39=1))),IF(COLUMN(EC39)-MAX(COLUMN($AG39:EB39)*($AG39:EB39=2))=$L39,3,0),IF($K39=\"Not Possible\",IF(COLUMN(EC39)-MAX(COLUMN($AG39:EB39)*($AG39:EB39=3))=$J39,3,0),IF(COLUMN(EC39)-MAX(COLUMN($AG39:EB39)*($AG39:EB39=3))=$J39,2,0)))))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":""},null,{"$f":"IFERROR(IF(Form_Asset[[#This Row],[Asset description]]=\"\",\"\",INDEX(Form_Elements[Asset class],MATCH(Form_Asset[[#This Row],[Asset description]],Form_Elements[Asset description],0))),\"\")","v":""},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",Form_Asset[[#This Row],[Asset ID]]&ROW())","v":""},null,null,{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset category]]=\"\",\"\",INDEX(AssetListTbl[Best Estimate Life (5)],(MATCH(Form_Asset[[#This Row],[Sub-Asset category]],AssetListTbl[Sub-Element Category],0))))","v":""},null,null,null,null,{"$f":"MAX(COLUMN($AH40:EC40)*($AH40:EC40=2))","v":0},{"$f":"MAX(COLUMN($AH40:EC40)*($AH40:EC40=3))","v":0},{"$f":"IFERROR(100-(IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Replace]])),INDIRECT(ADDRESS(29,Form_Asset[[#This Row],[Last Refurb]])))),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Last Replace]]>Form_Asset[[#This Row],[Last Refurb]],3,2)","v":2},{"$f":"SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Product_Stage[CO2e (t)])","v":0},{"$f":"IFERROR(SUM(Form_Elements[General Item Material])*(Form_Asset[[#This Row],[Weighted Split]]/SUM(Form_Asset[Weighted Split]))+Form_Asset[[#This Row],[Weighted Split]],0)","v":0},{"$f":"IFERROR((SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road Co2e (wtt)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Road C02e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth Co2e (com)])+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Total Oth (wtt)]))+(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Transport]))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Non contractor People Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Contractor people transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant Transport])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Site establishment])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(IF($D$88=\"Summary\",((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),(SUMIF(Form_Const_Ins_InsB[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Const_Ins_InsB[CO2e (t)]))+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Plant use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Other Construction Waste])*Form_Asset[[#This Row],[Weighted Split]]/(SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[[Waste Co2e ]])+((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[General Item Material Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New build\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]]),IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",(SUM(Form_Asset[[#This Row],[Materials]:[Waste]])-(SUM(Form_Asset[[#This Row],[Materials Transport]],Form_Asset[[#This Row],[People Transport]]*0.5,Form_Asset[[#This Row],[Plant Transport]]*0.5))),IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",SUM(Form_Asset[[#This Row],[Materials]:[Waste]])/(SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%])),0)))","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Use])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split]))),0)","v":0},{"$f":"IFERROR(SUMIF(Form_use_energy[Sub-Asset Ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_use_energy[CO2e (t)]),0)","v":0},{"$f":"IF(Form_Asset[[#This Row],[Sub-Asset ref.]]=\"\",0,SUMIF(Form_Asset[Sub-Asset ref.],Form_Asset[Sub-Asset ref.],Form_Asset[New Build Co2e])*SUMIF(Refurb_Poss_Tbl[Refurbishment Possible],Form_Asset[[#This Row],[Refurbishment type]],Refurb_Poss_Tbl[%]))","v":0},{"$f":"IFERROR(((SUMIF(Form_Elements[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Elements[Dem - General Item Waste])))*Form_Asset[[#This Row],[Weighted Split]]/((SUMIF(Form_Asset[Asset ID],Form_Asset[[#This Row],[Asset ID]],Form_Asset[Weighted Split])))+SUMIF(Form_Product_Stage[Sub-Asset ref.],Form_Asset[[#This Row],[Sub-Asset ref.]],Form_Product_Stage[Dem -Waste Co2e]),0)","v":0},{"$f":"(Form_Asset[[#This Row],[Plant use]]+Form_Asset[[#This Row],[Plant Transport]])*50%","v":0},{"$f":"Form_Asset[[#This Row],[People Transport]]*50%","v":0},{"$f":"IF(Form_Asset[[#This Row],[First intervention]]=\"New Build\",1,IF(Form_Asset[[#This Row],[First intervention]]=\"Refurbishment\",2,IF(Form_Asset[[#This Row],[First intervention]]=\"Replacement\",3,IF(Form_Asset[[#This Row],[First intervention]]=\"Demolition\",4,\"\"))))","v":""},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AG40)*($AG40:AG40=1))>MAX(COLUMN($AG40:AG40)*($AG40:AG40=3)),MAX(COLUMN($AG40:AG40)*($AG40:AG40=1))>MAX(COLUMN($AG40:AG40)*($AG40:AG40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AH40)-MAX(COLUMN($AG40:AG40)*($AG40:AG40=1))=$J40,3,0),IF(COLUMN(AH40)-MAX(COLUMN($AG40:AG40)*($AG40:AG40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AG40)*($AG40:AG40=2))>MAX(COLUMN($AG40:AG40)*($AG40:AG40=3)),MAX(COLUMN($AG40:AG40)*($AG40:AG40=2))>MAX(COLUMN($AG40:AG40)*($AG40:AG40=1))),IF(COLUMN(AH40)-MAX(COLUMN($AG40:AG40)*($AG40:AG40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AH40)-MAX(COLUMN($AG40:AG40)*($AG40:AG40=3))=$J40,3,0),IF(COLUMN(AH40)-MAX(COLUMN($AG40:AG40)*($AG40:AG40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AH40)*($AG40:AH40=1))>MAX(COLUMN($AG40:AH40)*($AG40:AH40=3)),MAX(COLUMN($AG40:AH40)*($AG40:AH40=1))>MAX(COLUMN($AG40:AH40)*($AG40:AH40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AI40)-MAX(COLUMN($AG40:AH40)*($AG40:AH40=1))=$J40,3,0),IF(COLUMN(AI40)-MAX(COLUMN($AG40:AH40)*($AG40:AH40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AH40)*($AG40:AH40=2))>MAX(COLUMN($AG40:AH40)*($AG40:AH40=3)),MAX(COLUMN($AG40:AH40)*($AG40:AH40=2))>MAX(COLUMN($AG40:AH40)*($AG40:AH40=1))),IF(COLUMN(AI40)-MAX(COLUMN($AG40:AH40)*($AG40:AH40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AI40)-MAX(COLUMN($AG40:AH40)*($AG40:AH40=3))=$J40,3,0),IF(COLUMN(AI40)-MAX(COLUMN($AG40:AH40)*($AG40:AH40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AI40)*($AG40:AI40=1))>MAX(COLUMN($AG40:AI40)*($AG40:AI40=3)),MAX(COLUMN($AG40:AI40)*($AG40:AI40=1))>MAX(COLUMN($AG40:AI40)*($AG40:AI40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AJ40)-MAX(COLUMN($AG40:AI40)*($AG40:AI40=1))=$J40,3,0),IF(COLUMN(AJ40)-MAX(COLUMN($AG40:AI40)*($AG40:AI40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AI40)*($AG40:AI40=2))>MAX(COLUMN($AG40:AI40)*($AG40:AI40=3)),MAX(COLUMN($AG40:AI40)*($AG40:AI40=2))>MAX(COLUMN($AG40:AI40)*($AG40:AI40=1))),IF(COLUMN(AJ40)-MAX(COLUMN($AG40:AI40)*($AG40:AI40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AJ40)-MAX(COLUMN($AG40:AI40)*($AG40:AI40=3))=$J40,3,0),IF(COLUMN(AJ40)-MAX(COLUMN($AG40:AI40)*($AG40:AI40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=1))>MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=3)),MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=1))>MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AK40)-MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=1))=$J40,3,0),IF(COLUMN(AK40)-MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=2))>MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=3)),MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=2))>MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=1))),IF(COLUMN(AK40)-MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AK40)-MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=3))=$J40,3,0),IF(COLUMN(AK40)-MAX(COLUMN($AG40:AJ40)*($AG40:AJ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AK40)*($AG40:AK40=1))>MAX(COLUMN($AG40:AK40)*($AG40:AK40=3)),MAX(COLUMN($AG40:AK40)*($AG40:AK40=1))>MAX(COLUMN($AG40:AK40)*($AG40:AK40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AL40)-MAX(COLUMN($AG40:AK40)*($AG40:AK40=1))=$J40,3,0),IF(COLUMN(AL40)-MAX(COLUMN($AG40:AK40)*($AG40:AK40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AK40)*($AG40:AK40=2))>MAX(COLUMN($AG40:AK40)*($AG40:AK40=3)),MAX(COLUMN($AG40:AK40)*($AG40:AK40=2))>MAX(COLUMN($AG40:AK40)*($AG40:AK40=1))),IF(COLUMN(AL40)-MAX(COLUMN($AG40:AK40)*($AG40:AK40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AL40)-MAX(COLUMN($AG40:AK40)*($AG40:AK40=3))=$J40,3,0),IF(COLUMN(AL40)-MAX(COLUMN($AG40:AK40)*($AG40:AK40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AL40)*($AG40:AL40=1))>MAX(COLUMN($AG40:AL40)*($AG40:AL40=3)),MAX(COLUMN($AG40:AL40)*($AG40:AL40=1))>MAX(COLUMN($AG40:AL40)*($AG40:AL40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AM40)-MAX(COLUMN($AG40:AL40)*($AG40:AL40=1))=$J40,3,0),IF(COLUMN(AM40)-MAX(COLUMN($AG40:AL40)*($AG40:AL40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AL40)*($AG40:AL40=2))>MAX(COLUMN($AG40:AL40)*($AG40:AL40=3)),MAX(COLUMN($AG40:AL40)*($AG40:AL40=2))>MAX(COLUMN($AG40:AL40)*($AG40:AL40=1))),IF(COLUMN(AM40)-MAX(COLUMN($AG40:AL40)*($AG40:AL40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AM40)-MAX(COLUMN($AG40:AL40)*($AG40:AL40=3))=$J40,3,0),IF(COLUMN(AM40)-MAX(COLUMN($AG40:AL40)*($AG40:AL40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AM40)*($AG40:AM40=1))>MAX(COLUMN($AG40:AM40)*($AG40:AM40=3)),MAX(COLUMN($AG40:AM40)*($AG40:AM40=1))>MAX(COLUMN($AG40:AM40)*($AG40:AM40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AN40)-MAX(COLUMN($AG40:AM40)*($AG40:AM40=1))=$J40,3,0),IF(COLUMN(AN40)-MAX(COLUMN($AG40:AM40)*($AG40:AM40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AM40)*($AG40:AM40=2))>MAX(COLUMN($AG40:AM40)*($AG40:AM40=3)),MAX(COLUMN($AG40:AM40)*($AG40:AM40=2))>MAX(COLUMN($AG40:AM40)*($AG40:AM40=1))),IF(COLUMN(AN40)-MAX(COLUMN($AG40:AM40)*($AG40:AM40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AN40)-MAX(COLUMN($AG40:AM40)*($AG40:AM40=3))=$J40,3,0),IF(COLUMN(AN40)-MAX(COLUMN($AG40:AM40)*($AG40:AM40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AN40)*($AG40:AN40=1))>MAX(COLUMN($AG40:AN40)*($AG40:AN40=3)),MAX(COLUMN($AG40:AN40)*($AG40:AN40=1))>MAX(COLUMN($AG40:AN40)*($AG40:AN40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AO40)-MAX(COLUMN($AG40:AN40)*($AG40:AN40=1))=$J40,3,0),IF(COLUMN(AO40)-MAX(COLUMN($AG40:AN40)*($AG40:AN40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AN40)*($AG40:AN40=2))>MAX(COLUMN($AG40:AN40)*($AG40:AN40=3)),MAX(COLUMN($AG40:AN40)*($AG40:AN40=2))>MAX(COLUMN($AG40:AN40)*($AG40:AN40=1))),IF(COLUMN(AO40)-MAX(COLUMN($AG40:AN40)*($AG40:AN40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AO40)-MAX(COLUMN($AG40:AN40)*($AG40:AN40=3))=$J40,3,0),IF(COLUMN(AO40)-MAX(COLUMN($AG40:AN40)*($AG40:AN40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AO40)*($AG40:AO40=1))>MAX(COLUMN($AG40:AO40)*($AG40:AO40=3)),MAX(COLUMN($AG40:AO40)*($AG40:AO40=1))>MAX(COLUMN($AG40:AO40)*($AG40:AO40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AP40)-MAX(COLUMN($AG40:AO40)*($AG40:AO40=1))=$J40,3,0),IF(COLUMN(AP40)-MAX(COLUMN($AG40:AO40)*($AG40:AO40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AO40)*($AG40:AO40=2))>MAX(COLUMN($AG40:AO40)*($AG40:AO40=3)),MAX(COLUMN($AG40:AO40)*($AG40:AO40=2))>MAX(COLUMN($AG40:AO40)*($AG40:AO40=1))),IF(COLUMN(AP40)-MAX(COLUMN($AG40:AO40)*($AG40:AO40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AP40)-MAX(COLUMN($AG40:AO40)*($AG40:AO40=3))=$J40,3,0),IF(COLUMN(AP40)-MAX(COLUMN($AG40:AO40)*($AG40:AO40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AP40)*($AG40:AP40=1))>MAX(COLUMN($AG40:AP40)*($AG40:AP40=3)),MAX(COLUMN($AG40:AP40)*($AG40:AP40=1))>MAX(COLUMN($AG40:AP40)*($AG40:AP40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AQ40)-MAX(COLUMN($AG40:AP40)*($AG40:AP40=1))=$J40,3,0),IF(COLUMN(AQ40)-MAX(COLUMN($AG40:AP40)*($AG40:AP40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AP40)*($AG40:AP40=2))>MAX(COLUMN($AG40:AP40)*($AG40:AP40=3)),MAX(COLUMN($AG40:AP40)*($AG40:AP40=2))>MAX(COLUMN($AG40:AP40)*($AG40:AP40=1))),IF(COLUMN(AQ40)-MAX(COLUMN($AG40:AP40)*($AG40:AP40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AQ40)-MAX(COLUMN($AG40:AP40)*($AG40:AP40=3))=$J40,3,0),IF(COLUMN(AQ40)-MAX(COLUMN($AG40:AP40)*($AG40:AP40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=1))>MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=3)),MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=1))>MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AR40)-MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=1))=$J40,3,0),IF(COLUMN(AR40)-MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=2))>MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=3)),MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=2))>MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=1))),IF(COLUMN(AR40)-MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AR40)-MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=3))=$J40,3,0),IF(COLUMN(AR40)-MAX(COLUMN($AG40:AQ40)*($AG40:AQ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AR40)*($AG40:AR40=1))>MAX(COLUMN($AG40:AR40)*($AG40:AR40=3)),MAX(COLUMN($AG40:AR40)*($AG40:AR40=1))>MAX(COLUMN($AG40:AR40)*($AG40:AR40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AS40)-MAX(COLUMN($AG40:AR40)*($AG40:AR40=1))=$J40,3,0),IF(COLUMN(AS40)-MAX(COLUMN($AG40:AR40)*($AG40:AR40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AR40)*($AG40:AR40=2))>MAX(COLUMN($AG40:AR40)*($AG40:AR40=3)),MAX(COLUMN($AG40:AR40)*($AG40:AR40=2))>MAX(COLUMN($AG40:AR40)*($AG40:AR40=1))),IF(COLUMN(AS40)-MAX(COLUMN($AG40:AR40)*($AG40:AR40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AS40)-MAX(COLUMN($AG40:AR40)*($AG40:AR40=3))=$J40,3,0),IF(COLUMN(AS40)-MAX(COLUMN($AG40:AR40)*($AG40:AR40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AS40)*($AG40:AS40=1))>MAX(COLUMN($AG40:AS40)*($AG40:AS40=3)),MAX(COLUMN($AG40:AS40)*($AG40:AS40=1))>MAX(COLUMN($AG40:AS40)*($AG40:AS40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AT40)-MAX(COLUMN($AG40:AS40)*($AG40:AS40=1))=$J40,3,0),IF(COLUMN(AT40)-MAX(COLUMN($AG40:AS40)*($AG40:AS40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AS40)*($AG40:AS40=2))>MAX(COLUMN($AG40:AS40)*($AG40:AS40=3)),MAX(COLUMN($AG40:AS40)*($AG40:AS40=2))>MAX(COLUMN($AG40:AS40)*($AG40:AS40=1))),IF(COLUMN(AT40)-MAX(COLUMN($AG40:AS40)*($AG40:AS40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AT40)-MAX(COLUMN($AG40:AS40)*($AG40:AS40=3))=$J40,3,0),IF(COLUMN(AT40)-MAX(COLUMN($AG40:AS40)*($AG40:AS40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AT40)*($AG40:AT40=1))>MAX(COLUMN($AG40:AT40)*($AG40:AT40=3)),MAX(COLUMN($AG40:AT40)*($AG40:AT40=1))>MAX(COLUMN($AG40:AT40)*($AG40:AT40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AU40)-MAX(COLUMN($AG40:AT40)*($AG40:AT40=1))=$J40,3,0),IF(COLUMN(AU40)-MAX(COLUMN($AG40:AT40)*($AG40:AT40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AT40)*($AG40:AT40=2))>MAX(COLUMN($AG40:AT40)*($AG40:AT40=3)),MAX(COLUMN($AG40:AT40)*($AG40:AT40=2))>MAX(COLUMN($AG40:AT40)*($AG40:AT40=1))),IF(COLUMN(AU40)-MAX(COLUMN($AG40:AT40)*($AG40:AT40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AU40)-MAX(COLUMN($AG40:AT40)*($AG40:AT40=3))=$J40,3,0),IF(COLUMN(AU40)-MAX(COLUMN($AG40:AT40)*($AG40:AT40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AU40)*($AG40:AU40=1))>MAX(COLUMN($AG40:AU40)*($AG40:AU40=3)),MAX(COLUMN($AG40:AU40)*($AG40:AU40=1))>MAX(COLUMN($AG40:AU40)*($AG40:AU40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AV40)-MAX(COLUMN($AG40:AU40)*($AG40:AU40=1))=$J40,3,0),IF(COLUMN(AV40)-MAX(COLUMN($AG40:AU40)*($AG40:AU40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AU40)*($AG40:AU40=2))>MAX(COLUMN($AG40:AU40)*($AG40:AU40=3)),MAX(COLUMN($AG40:AU40)*($AG40:AU40=2))>MAX(COLUMN($AG40:AU40)*($AG40:AU40=1))),IF(COLUMN(AV40)-MAX(COLUMN($AG40:AU40)*($AG40:AU40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AV40)-MAX(COLUMN($AG40:AU40)*($AG40:AU40=3))=$J40,3,0),IF(COLUMN(AV40)-MAX(COLUMN($AG40:AU40)*($AG40:AU40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AV40)*($AG40:AV40=1))>MAX(COLUMN($AG40:AV40)*($AG40:AV40=3)),MAX(COLUMN($AG40:AV40)*($AG40:AV40=1))>MAX(COLUMN($AG40:AV40)*($AG40:AV40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AW40)-MAX(COLUMN($AG40:AV40)*($AG40:AV40=1))=$J40,3,0),IF(COLUMN(AW40)-MAX(COLUMN($AG40:AV40)*($AG40:AV40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AV40)*($AG40:AV40=2))>MAX(COLUMN($AG40:AV40)*($AG40:AV40=3)),MAX(COLUMN($AG40:AV40)*($AG40:AV40=2))>MAX(COLUMN($AG40:AV40)*($AG40:AV40=1))),IF(COLUMN(AW40)-MAX(COLUMN($AG40:AV40)*($AG40:AV40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AW40)-MAX(COLUMN($AG40:AV40)*($AG40:AV40=3))=$J40,3,0),IF(COLUMN(AW40)-MAX(COLUMN($AG40:AV40)*($AG40:AV40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AW40)*($AG40:AW40=1))>MAX(COLUMN($AG40:AW40)*($AG40:AW40=3)),MAX(COLUMN($AG40:AW40)*($AG40:AW40=1))>MAX(COLUMN($AG40:AW40)*($AG40:AW40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AX40)-MAX(COLUMN($AG40:AW40)*($AG40:AW40=1))=$J40,3,0),IF(COLUMN(AX40)-MAX(COLUMN($AG40:AW40)*($AG40:AW40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AW40)*($AG40:AW40=2))>MAX(COLUMN($AG40:AW40)*($AG40:AW40=3)),MAX(COLUMN($AG40:AW40)*($AG40:AW40=2))>MAX(COLUMN($AG40:AW40)*($AG40:AW40=1))),IF(COLUMN(AX40)-MAX(COLUMN($AG40:AW40)*($AG40:AW40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AX40)-MAX(COLUMN($AG40:AW40)*($AG40:AW40=3))=$J40,3,0),IF(COLUMN(AX40)-MAX(COLUMN($AG40:AW40)*($AG40:AW40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AX40)*($AG40:AX40=1))>MAX(COLUMN($AG40:AX40)*($AG40:AX40=3)),MAX(COLUMN($AG40:AX40)*($AG40:AX40=1))>MAX(COLUMN($AG40:AX40)*($AG40:AX40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AY40)-MAX(COLUMN($AG40:AX40)*($AG40:AX40=1))=$J40,3,0),IF(COLUMN(AY40)-MAX(COLUMN($AG40:AX40)*($AG40:AX40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AX40)*($AG40:AX40=2))>MAX(COLUMN($AG40:AX40)*($AG40:AX40=3)),MAX(COLUMN($AG40:AX40)*($AG40:AX40=2))>MAX(COLUMN($AG40:AX40)*($AG40:AX40=1))),IF(COLUMN(AY40)-MAX(COLUMN($AG40:AX40)*($AG40:AX40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AY40)-MAX(COLUMN($AG40:AX40)*($AG40:AX40=3))=$J40,3,0),IF(COLUMN(AY40)-MAX(COLUMN($AG40:AX40)*($AG40:AX40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AY40)*($AG40:AY40=1))>MAX(COLUMN($AG40:AY40)*($AG40:AY40=3)),MAX(COLUMN($AG40:AY40)*($AG40:AY40=1))>MAX(COLUMN($AG40:AY40)*($AG40:AY40=2))),IF($K40=\"Not Possible\",IF(COLUMN(AZ40)-MAX(COLUMN($AG40:AY40)*($AG40:AY40=1))=$J40,3,0),IF(COLUMN(AZ40)-MAX(COLUMN($AG40:AY40)*($AG40:AY40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AY40)*($AG40:AY40=2))>MAX(COLUMN($AG40:AY40)*($AG40:AY40=3)),MAX(COLUMN($AG40:AY40)*($AG40:AY40=2))>MAX(COLUMN($AG40:AY40)*($AG40:AY40=1))),IF(COLUMN(AZ40)-MAX(COLUMN($AG40:AY40)*($AG40:AY40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(AZ40)-MAX(COLUMN($AG40:AY40)*($AG40:AY40=3))=$J40,3,0),IF(COLUMN(AZ40)-MAX(COLUMN($AG40:AY40)*($AG40:AY40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=1))>MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=3)),MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=1))>MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BA40)-MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=1))=$J40,3,0),IF(COLUMN(BA40)-MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=2))>MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=3)),MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=2))>MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=1))),IF(COLUMN(BA40)-MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BA40)-MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=3))=$J40,3,0),IF(COLUMN(BA40)-MAX(COLUMN($AG40:AZ40)*($AG40:AZ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BA40)*($AG40:BA40=1))>MAX(COLUMN($AG40:BA40)*($AG40:BA40=3)),MAX(COLUMN($AG40:BA40)*($AG40:BA40=1))>MAX(COLUMN($AG40:BA40)*($AG40:BA40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BB40)-MAX(COLUMN($AG40:BA40)*($AG40:BA40=1))=$J40,3,0),IF(COLUMN(BB40)-MAX(COLUMN($AG40:BA40)*($AG40:BA40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BA40)*($AG40:BA40=2))>MAX(COLUMN($AG40:BA40)*($AG40:BA40=3)),MAX(COLUMN($AG40:BA40)*($AG40:BA40=2))>MAX(COLUMN($AG40:BA40)*($AG40:BA40=1))),IF(COLUMN(BB40)-MAX(COLUMN($AG40:BA40)*($AG40:BA40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BB40)-MAX(COLUMN($AG40:BA40)*($AG40:BA40=3))=$J40,3,0),IF(COLUMN(BB40)-MAX(COLUMN($AG40:BA40)*($AG40:BA40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BB40)*($AG40:BB40=1))>MAX(COLUMN($AG40:BB40)*($AG40:BB40=3)),MAX(COLUMN($AG40:BB40)*($AG40:BB40=1))>MAX(COLUMN($AG40:BB40)*($AG40:BB40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BC40)-MAX(COLUMN($AG40:BB40)*($AG40:BB40=1))=$J40,3,0),IF(COLUMN(BC40)-MAX(COLUMN($AG40:BB40)*($AG40:BB40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BB40)*($AG40:BB40=2))>MAX(COLUMN($AG40:BB40)*($AG40:BB40=3)),MAX(COLUMN($AG40:BB40)*($AG40:BB40=2))>MAX(COLUMN($AG40:BB40)*($AG40:BB40=1))),IF(COLUMN(BC40)-MAX(COLUMN($AG40:BB40)*($AG40:BB40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BC40)-MAX(COLUMN($AG40:BB40)*($AG40:BB40=3))=$J40,3,0),IF(COLUMN(BC40)-MAX(COLUMN($AG40:BB40)*($AG40:BB40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BC40)*($AG40:BC40=1))>MAX(COLUMN($AG40:BC40)*($AG40:BC40=3)),MAX(COLUMN($AG40:BC40)*($AG40:BC40=1))>MAX(COLUMN($AG40:BC40)*($AG40:BC40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BD40)-MAX(COLUMN($AG40:BC40)*($AG40:BC40=1))=$J40,3,0),IF(COLUMN(BD40)-MAX(COLUMN($AG40:BC40)*($AG40:BC40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BC40)*($AG40:BC40=2))>MAX(COLUMN($AG40:BC40)*($AG40:BC40=3)),MAX(COLUMN($AG40:BC40)*($AG40:BC40=2))>MAX(COLUMN($AG40:BC40)*($AG40:BC40=1))),IF(COLUMN(BD40)-MAX(COLUMN($AG40:BC40)*($AG40:BC40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BD40)-MAX(COLUMN($AG40:BC40)*($AG40:BC40=3))=$J40,3,0),IF(COLUMN(BD40)-MAX(COLUMN($AG40:BC40)*($AG40:BC40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BD40)*($AG40:BD40=1))>MAX(COLUMN($AG40:BD40)*($AG40:BD40=3)),MAX(COLUMN($AG40:BD40)*($AG40:BD40=1))>MAX(COLUMN($AG40:BD40)*($AG40:BD40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BE40)-MAX(COLUMN($AG40:BD40)*($AG40:BD40=1))=$J40,3,0),IF(COLUMN(BE40)-MAX(COLUMN($AG40:BD40)*($AG40:BD40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BD40)*($AG40:BD40=2))>MAX(COLUMN($AG40:BD40)*($AG40:BD40=3)),MAX(COLUMN($AG40:BD40)*($AG40:BD40=2))>MAX(COLUMN($AG40:BD40)*($AG40:BD40=1))),IF(COLUMN(BE40)-MAX(COLUMN($AG40:BD40)*($AG40:BD40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BE40)-MAX(COLUMN($AG40:BD40)*($AG40:BD40=3))=$J40,3,0),IF(COLUMN(BE40)-MAX(COLUMN($AG40:BD40)*($AG40:BD40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BE40)*($AG40:BE40=1))>MAX(COLUMN($AG40:BE40)*($AG40:BE40=3)),MAX(COLUMN($AG40:BE40)*($AG40:BE40=1))>MAX(COLUMN($AG40:BE40)*($AG40:BE40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BF40)-MAX(COLUMN($AG40:BE40)*($AG40:BE40=1))=$J40,3,0),IF(COLUMN(BF40)-MAX(COLUMN($AG40:BE40)*($AG40:BE40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BE40)*($AG40:BE40=2))>MAX(COLUMN($AG40:BE40)*($AG40:BE40=3)),MAX(COLUMN($AG40:BE40)*($AG40:BE40=2))>MAX(COLUMN($AG40:BE40)*($AG40:BE40=1))),IF(COLUMN(BF40)-MAX(COLUMN($AG40:BE40)*($AG40:BE40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BF40)-MAX(COLUMN($AG40:BE40)*($AG40:BE40=3))=$J40,3,0),IF(COLUMN(BF40)-MAX(COLUMN($AG40:BE40)*($AG40:BE40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BF40)*($AG40:BF40=1))>MAX(COLUMN($AG40:BF40)*($AG40:BF40=3)),MAX(COLUMN($AG40:BF40)*($AG40:BF40=1))>MAX(COLUMN($AG40:BF40)*($AG40:BF40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BG40)-MAX(COLUMN($AG40:BF40)*($AG40:BF40=1))=$J40,3,0),IF(COLUMN(BG40)-MAX(COLUMN($AG40:BF40)*($AG40:BF40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BF40)*($AG40:BF40=2))>MAX(COLUMN($AG40:BF40)*($AG40:BF40=3)),MAX(COLUMN($AG40:BF40)*($AG40:BF40=2))>MAX(COLUMN($AG40:BF40)*($AG40:BF40=1))),IF(COLUMN(BG40)-MAX(COLUMN($AG40:BF40)*($AG40:BF40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BG40)-MAX(COLUMN($AG40:BF40)*($AG40:BF40=3))=$J40,3,0),IF(COLUMN(BG40)-MAX(COLUMN($AG40:BF40)*($AG40:BF40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BG40)*($AG40:BG40=1))>MAX(COLUMN($AG40:BG40)*($AG40:BG40=3)),MAX(COLUMN($AG40:BG40)*($AG40:BG40=1))>MAX(COLUMN($AG40:BG40)*($AG40:BG40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BH40)-MAX(COLUMN($AG40:BG40)*($AG40:BG40=1))=$J40,3,0),IF(COLUMN(BH40)-MAX(COLUMN($AG40:BG40)*($AG40:BG40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BG40)*($AG40:BG40=2))>MAX(COLUMN($AG40:BG40)*($AG40:BG40=3)),MAX(COLUMN($AG40:BG40)*($AG40:BG40=2))>MAX(COLUMN($AG40:BG40)*($AG40:BG40=1))),IF(COLUMN(BH40)-MAX(COLUMN($AG40:BG40)*($AG40:BG40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BH40)-MAX(COLUMN($AG40:BG40)*($AG40:BG40=3))=$J40,3,0),IF(COLUMN(BH40)-MAX(COLUMN($AG40:BG40)*($AG40:BG40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BH40)*($AG40:BH40=1))>MAX(COLUMN($AG40:BH40)*($AG40:BH40=3)),MAX(COLUMN($AG40:BH40)*($AG40:BH40=1))>MAX(COLUMN($AG40:BH40)*($AG40:BH40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BI40)-MAX(COLUMN($AG40:BH40)*($AG40:BH40=1))=$J40,3,0),IF(COLUMN(BI40)-MAX(COLUMN($AG40:BH40)*($AG40:BH40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BH40)*($AG40:BH40=2))>MAX(COLUMN($AG40:BH40)*($AG40:BH40=3)),MAX(COLUMN($AG40:BH40)*($AG40:BH40=2))>MAX(COLUMN($AG40:BH40)*($AG40:BH40=1))),IF(COLUMN(BI40)-MAX(COLUMN($AG40:BH40)*($AG40:BH40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BI40)-MAX(COLUMN($AG40:BH40)*($AG40:BH40=3))=$J40,3,0),IF(COLUMN(BI40)-MAX(COLUMN($AG40:BH40)*($AG40:BH40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BI40)*($AG40:BI40=1))>MAX(COLUMN($AG40:BI40)*($AG40:BI40=3)),MAX(COLUMN($AG40:BI40)*($AG40:BI40=1))>MAX(COLUMN($AG40:BI40)*($AG40:BI40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BJ40)-MAX(COLUMN($AG40:BI40)*($AG40:BI40=1))=$J40,3,0),IF(COLUMN(BJ40)-MAX(COLUMN($AG40:BI40)*($AG40:BI40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BI40)*($AG40:BI40=2))>MAX(COLUMN($AG40:BI40)*($AG40:BI40=3)),MAX(COLUMN($AG40:BI40)*($AG40:BI40=2))>MAX(COLUMN($AG40:BI40)*($AG40:BI40=1))),IF(COLUMN(BJ40)-MAX(COLUMN($AG40:BI40)*($AG40:BI40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BJ40)-MAX(COLUMN($AG40:BI40)*($AG40:BI40=3))=$J40,3,0),IF(COLUMN(BJ40)-MAX(COLUMN($AG40:BI40)*($AG40:BI40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=1))>MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=3)),MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=1))>MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BK40)-MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=1))=$J40,3,0),IF(COLUMN(BK40)-MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=2))>MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=3)),MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=2))>MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=1))),IF(COLUMN(BK40)-MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BK40)-MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=3))=$J40,3,0),IF(COLUMN(BK40)-MAX(COLUMN($AG40:BJ40)*($AG40:BJ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BK40)*($AG40:BK40=1))>MAX(COLUMN($AG40:BK40)*($AG40:BK40=3)),MAX(COLUMN($AG40:BK40)*($AG40:BK40=1))>MAX(COLUMN($AG40:BK40)*($AG40:BK40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BL40)-MAX(COLUMN($AG40:BK40)*($AG40:BK40=1))=$J40,3,0),IF(COLUMN(BL40)-MAX(COLUMN($AG40:BK40)*($AG40:BK40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BK40)*($AG40:BK40=2))>MAX(COLUMN($AG40:BK40)*($AG40:BK40=3)),MAX(COLUMN($AG40:BK40)*($AG40:BK40=2))>MAX(COLUMN($AG40:BK40)*($AG40:BK40=1))),IF(COLUMN(BL40)-MAX(COLUMN($AG40:BK40)*($AG40:BK40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BL40)-MAX(COLUMN($AG40:BK40)*($AG40:BK40=3))=$J40,3,0),IF(COLUMN(BL40)-MAX(COLUMN($AG40:BK40)*($AG40:BK40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BL40)*($AG40:BL40=1))>MAX(COLUMN($AG40:BL40)*($AG40:BL40=3)),MAX(COLUMN($AG40:BL40)*($AG40:BL40=1))>MAX(COLUMN($AG40:BL40)*($AG40:BL40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BM40)-MAX(COLUMN($AG40:BL40)*($AG40:BL40=1))=$J40,3,0),IF(COLUMN(BM40)-MAX(COLUMN($AG40:BL40)*($AG40:BL40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BL40)*($AG40:BL40=2))>MAX(COLUMN($AG40:BL40)*($AG40:BL40=3)),MAX(COLUMN($AG40:BL40)*($AG40:BL40=2))>MAX(COLUMN($AG40:BL40)*($AG40:BL40=1))),IF(COLUMN(BM40)-MAX(COLUMN($AG40:BL40)*($AG40:BL40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BM40)-MAX(COLUMN($AG40:BL40)*($AG40:BL40=3))=$J40,3,0),IF(COLUMN(BM40)-MAX(COLUMN($AG40:BL40)*($AG40:BL40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BM40)*($AG40:BM40=1))>MAX(COLUMN($AG40:BM40)*($AG40:BM40=3)),MAX(COLUMN($AG40:BM40)*($AG40:BM40=1))>MAX(COLUMN($AG40:BM40)*($AG40:BM40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BN40)-MAX(COLUMN($AG40:BM40)*($AG40:BM40=1))=$J40,3,0),IF(COLUMN(BN40)-MAX(COLUMN($AG40:BM40)*($AG40:BM40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BM40)*($AG40:BM40=2))>MAX(COLUMN($AG40:BM40)*($AG40:BM40=3)),MAX(COLUMN($AG40:BM40)*($AG40:BM40=2))>MAX(COLUMN($AG40:BM40)*($AG40:BM40=1))),IF(COLUMN(BN40)-MAX(COLUMN($AG40:BM40)*($AG40:BM40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BN40)-MAX(COLUMN($AG40:BM40)*($AG40:BM40=3))=$J40,3,0),IF(COLUMN(BN40)-MAX(COLUMN($AG40:BM40)*($AG40:BM40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BN40)*($AG40:BN40=1))>MAX(COLUMN($AG40:BN40)*($AG40:BN40=3)),MAX(COLUMN($AG40:BN40)*($AG40:BN40=1))>MAX(COLUMN($AG40:BN40)*($AG40:BN40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BO40)-MAX(COLUMN($AG40:BN40)*($AG40:BN40=1))=$J40,3,0),IF(COLUMN(BO40)-MAX(COLUMN($AG40:BN40)*($AG40:BN40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BN40)*($AG40:BN40=2))>MAX(COLUMN($AG40:BN40)*($AG40:BN40=3)),MAX(COLUMN($AG40:BN40)*($AG40:BN40=2))>MAX(COLUMN($AG40:BN40)*($AG40:BN40=1))),IF(COLUMN(BO40)-MAX(COLUMN($AG40:BN40)*($AG40:BN40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BO40)-MAX(COLUMN($AG40:BN40)*($AG40:BN40=3))=$J40,3,0),IF(COLUMN(BO40)-MAX(COLUMN($AG40:BN40)*($AG40:BN40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BO40)*($AG40:BO40=1))>MAX(COLUMN($AG40:BO40)*($AG40:BO40=3)),MAX(COLUMN($AG40:BO40)*($AG40:BO40=1))>MAX(COLUMN($AG40:BO40)*($AG40:BO40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BP40)-MAX(COLUMN($AG40:BO40)*($AG40:BO40=1))=$J40,3,0),IF(COLUMN(BP40)-MAX(COLUMN($AG40:BO40)*($AG40:BO40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BO40)*($AG40:BO40=2))>MAX(COLUMN($AG40:BO40)*($AG40:BO40=3)),MAX(COLUMN($AG40:BO40)*($AG40:BO40=2))>MAX(COLUMN($AG40:BO40)*($AG40:BO40=1))),IF(COLUMN(BP40)-MAX(COLUMN($AG40:BO40)*($AG40:BO40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BP40)-MAX(COLUMN($AG40:BO40)*($AG40:BO40=3))=$J40,3,0),IF(COLUMN(BP40)-MAX(COLUMN($AG40:BO40)*($AG40:BO40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BP40)*($AG40:BP40=1))>MAX(COLUMN($AG40:BP40)*($AG40:BP40=3)),MAX(COLUMN($AG40:BP40)*($AG40:BP40=1))>MAX(COLUMN($AG40:BP40)*($AG40:BP40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BQ40)-MAX(COLUMN($AG40:BP40)*($AG40:BP40=1))=$J40,3,0),IF(COLUMN(BQ40)-MAX(COLUMN($AG40:BP40)*($AG40:BP40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BP40)*($AG40:BP40=2))>MAX(COLUMN($AG40:BP40)*($AG40:BP40=3)),MAX(COLUMN($AG40:BP40)*($AG40:BP40=2))>MAX(COLUMN($AG40:BP40)*($AG40:BP40=1))),IF(COLUMN(BQ40)-MAX(COLUMN($AG40:BP40)*($AG40:BP40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BQ40)-MAX(COLUMN($AG40:BP40)*($AG40:BP40=3))=$J40,3,0),IF(COLUMN(BQ40)-MAX(COLUMN($AG40:BP40)*($AG40:BP40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=1))>MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=3)),MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=1))>MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BR40)-MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=1))=$J40,3,0),IF(COLUMN(BR40)-MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=2))>MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=3)),MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=2))>MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=1))),IF(COLUMN(BR40)-MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BR40)-MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=3))=$J40,3,0),IF(COLUMN(BR40)-MAX(COLUMN($AG40:BQ40)*($AG40:BQ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BR40)*($AG40:BR40=1))>MAX(COLUMN($AG40:BR40)*($AG40:BR40=3)),MAX(COLUMN($AG40:BR40)*($AG40:BR40=1))>MAX(COLUMN($AG40:BR40)*($AG40:BR40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BS40)-MAX(COLUMN($AG40:BR40)*($AG40:BR40=1))=$J40,3,0),IF(COLUMN(BS40)-MAX(COLUMN($AG40:BR40)*($AG40:BR40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BR40)*($AG40:BR40=2))>MAX(COLUMN($AG40:BR40)*($AG40:BR40=3)),MAX(COLUMN($AG40:BR40)*($AG40:BR40=2))>MAX(COLUMN($AG40:BR40)*($AG40:BR40=1))),IF(COLUMN(BS40)-MAX(COLUMN($AG40:BR40)*($AG40:BR40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BS40)-MAX(COLUMN($AG40:BR40)*($AG40:BR40=3))=$J40,3,0),IF(COLUMN(BS40)-MAX(COLUMN($AG40:BR40)*($AG40:BR40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BS40)*($AG40:BS40=1))>MAX(COLUMN($AG40:BS40)*($AG40:BS40=3)),MAX(COLUMN($AG40:BS40)*($AG40:BS40=1))>MAX(COLUMN($AG40:BS40)*($AG40:BS40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BT40)-MAX(COLUMN($AG40:BS40)*($AG40:BS40=1))=$J40,3,0),IF(COLUMN(BT40)-MAX(COLUMN($AG40:BS40)*($AG40:BS40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BS40)*($AG40:BS40=2))>MAX(COLUMN($AG40:BS40)*($AG40:BS40=3)),MAX(COLUMN($AG40:BS40)*($AG40:BS40=2))>MAX(COLUMN($AG40:BS40)*($AG40:BS40=1))),IF(COLUMN(BT40)-MAX(COLUMN($AG40:BS40)*($AG40:BS40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BT40)-MAX(COLUMN($AG40:BS40)*($AG40:BS40=3))=$J40,3,0),IF(COLUMN(BT40)-MAX(COLUMN($AG40:BS40)*($AG40:BS40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BT40)*($AG40:BT40=1))>MAX(COLUMN($AG40:BT40)*($AG40:BT40=3)),MAX(COLUMN($AG40:BT40)*($AG40:BT40=1))>MAX(COLUMN($AG40:BT40)*($AG40:BT40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BU40)-MAX(COLUMN($AG40:BT40)*($AG40:BT40=1))=$J40,3,0),IF(COLUMN(BU40)-MAX(COLUMN($AG40:BT40)*($AG40:BT40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BT40)*($AG40:BT40=2))>MAX(COLUMN($AG40:BT40)*($AG40:BT40=3)),MAX(COLUMN($AG40:BT40)*($AG40:BT40=2))>MAX(COLUMN($AG40:BT40)*($AG40:BT40=1))),IF(COLUMN(BU40)-MAX(COLUMN($AG40:BT40)*($AG40:BT40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BU40)-MAX(COLUMN($AG40:BT40)*($AG40:BT40=3))=$J40,3,0),IF(COLUMN(BU40)-MAX(COLUMN($AG40:BT40)*($AG40:BT40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BU40)*($AG40:BU40=1))>MAX(COLUMN($AG40:BU40)*($AG40:BU40=3)),MAX(COLUMN($AG40:BU40)*($AG40:BU40=1))>MAX(COLUMN($AG40:BU40)*($AG40:BU40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BV40)-MAX(COLUMN($AG40:BU40)*($AG40:BU40=1))=$J40,3,0),IF(COLUMN(BV40)-MAX(COLUMN($AG40:BU40)*($AG40:BU40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BU40)*($AG40:BU40=2))>MAX(COLUMN($AG40:BU40)*($AG40:BU40=3)),MAX(COLUMN($AG40:BU40)*($AG40:BU40=2))>MAX(COLUMN($AG40:BU40)*($AG40:BU40=1))),IF(COLUMN(BV40)-MAX(COLUMN($AG40:BU40)*($AG40:BU40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BV40)-MAX(COLUMN($AG40:BU40)*($AG40:BU40=3))=$J40,3,0),IF(COLUMN(BV40)-MAX(COLUMN($AG40:BU40)*($AG40:BU40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BV40)*($AG40:BV40=1))>MAX(COLUMN($AG40:BV40)*($AG40:BV40=3)),MAX(COLUMN($AG40:BV40)*($AG40:BV40=1))>MAX(COLUMN($AG40:BV40)*($AG40:BV40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BW40)-MAX(COLUMN($AG40:BV40)*($AG40:BV40=1))=$J40,3,0),IF(COLUMN(BW40)-MAX(COLUMN($AG40:BV40)*($AG40:BV40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BV40)*($AG40:BV40=2))>MAX(COLUMN($AG40:BV40)*($AG40:BV40=3)),MAX(COLUMN($AG40:BV40)*($AG40:BV40=2))>MAX(COLUMN($AG40:BV40)*($AG40:BV40=1))),IF(COLUMN(BW40)-MAX(COLUMN($AG40:BV40)*($AG40:BV40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BW40)-MAX(COLUMN($AG40:BV40)*($AG40:BV40=3))=$J40,3,0),IF(COLUMN(BW40)-MAX(COLUMN($AG40:BV40)*($AG40:BV40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BW40)*($AG40:BW40=1))>MAX(COLUMN($AG40:BW40)*($AG40:BW40=3)),MAX(COLUMN($AG40:BW40)*($AG40:BW40=1))>MAX(COLUMN($AG40:BW40)*($AG40:BW40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BX40)-MAX(COLUMN($AG40:BW40)*($AG40:BW40=1))=$J40,3,0),IF(COLUMN(BX40)-MAX(COLUMN($AG40:BW40)*($AG40:BW40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BW40)*($AG40:BW40=2))>MAX(COLUMN($AG40:BW40)*($AG40:BW40=3)),MAX(COLUMN($AG40:BW40)*($AG40:BW40=2))>MAX(COLUMN($AG40:BW40)*($AG40:BW40=1))),IF(COLUMN(BX40)-MAX(COLUMN($AG40:BW40)*($AG40:BW40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BX40)-MAX(COLUMN($AG40:BW40)*($AG40:BW40=3))=$J40,3,0),IF(COLUMN(BX40)-MAX(COLUMN($AG40:BW40)*($AG40:BW40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BX40)*($AG40:BX40=1))>MAX(COLUMN($AG40:BX40)*($AG40:BX40=3)),MAX(COLUMN($AG40:BX40)*($AG40:BX40=1))>MAX(COLUMN($AG40:BX40)*($AG40:BX40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BY40)-MAX(COLUMN($AG40:BX40)*($AG40:BX40=1))=$J40,3,0),IF(COLUMN(BY40)-MAX(COLUMN($AG40:BX40)*($AG40:BX40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BX40)*($AG40:BX40=2))>MAX(COLUMN($AG40:BX40)*($AG40:BX40=3)),MAX(COLUMN($AG40:BX40)*($AG40:BX40=2))>MAX(COLUMN($AG40:BX40)*($AG40:BX40=1))),IF(COLUMN(BY40)-MAX(COLUMN($AG40:BX40)*($AG40:BX40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BY40)-MAX(COLUMN($AG40:BX40)*($AG40:BX40=3))=$J40,3,0),IF(COLUMN(BY40)-MAX(COLUMN($AG40:BX40)*($AG40:BX40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BY40)*($AG40:BY40=1))>MAX(COLUMN($AG40:BY40)*($AG40:BY40=3)),MAX(COLUMN($AG40:BY40)*($AG40:BY40=1))>MAX(COLUMN($AG40:BY40)*($AG40:BY40=2))),IF($K40=\"Not Possible\",IF(COLUMN(BZ40)-MAX(COLUMN($AG40:BY40)*($AG40:BY40=1))=$J40,3,0),IF(COLUMN(BZ40)-MAX(COLUMN($AG40:BY40)*($AG40:BY40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BY40)*($AG40:BY40=2))>MAX(COLUMN($AG40:BY40)*($AG40:BY40=3)),MAX(COLUMN($AG40:BY40)*($AG40:BY40=2))>MAX(COLUMN($AG40:BY40)*($AG40:BY40=1))),IF(COLUMN(BZ40)-MAX(COLUMN($AG40:BY40)*($AG40:BY40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(BZ40)-MAX(COLUMN($AG40:BY40)*($AG40:BY40=3))=$J40,3,0),IF(COLUMN(BZ40)-MAX(COLUMN($AG40:BY40)*($AG40:BY40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=1))>MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=3)),MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=1))>MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CA40)-MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=1))=$J40,3,0),IF(COLUMN(CA40)-MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=2))>MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=3)),MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=2))>MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=1))),IF(COLUMN(CA40)-MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CA40)-MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=3))=$J40,3,0),IF(COLUMN(CA40)-MAX(COLUMN($AG40:BZ40)*($AG40:BZ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CA40)*($AG40:CA40=1))>MAX(COLUMN($AG40:CA40)*($AG40:CA40=3)),MAX(COLUMN($AG40:CA40)*($AG40:CA40=1))>MAX(COLUMN($AG40:CA40)*($AG40:CA40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CB40)-MAX(COLUMN($AG40:CA40)*($AG40:CA40=1))=$J40,3,0),IF(COLUMN(CB40)-MAX(COLUMN($AG40:CA40)*($AG40:CA40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CA40)*($AG40:CA40=2))>MAX(COLUMN($AG40:CA40)*($AG40:CA40=3)),MAX(COLUMN($AG40:CA40)*($AG40:CA40=2))>MAX(COLUMN($AG40:CA40)*($AG40:CA40=1))),IF(COLUMN(CB40)-MAX(COLUMN($AG40:CA40)*($AG40:CA40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CB40)-MAX(COLUMN($AG40:CA40)*($AG40:CA40=3))=$J40,3,0),IF(COLUMN(CB40)-MAX(COLUMN($AG40:CA40)*($AG40:CA40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CB40)*($AG40:CB40=1))>MAX(COLUMN($AG40:CB40)*($AG40:CB40=3)),MAX(COLUMN($AG40:CB40)*($AG40:CB40=1))>MAX(COLUMN($AG40:CB40)*($AG40:CB40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CC40)-MAX(COLUMN($AG40:CB40)*($AG40:CB40=1))=$J40,3,0),IF(COLUMN(CC40)-MAX(COLUMN($AG40:CB40)*($AG40:CB40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CB40)*($AG40:CB40=2))>MAX(COLUMN($AG40:CB40)*($AG40:CB40=3)),MAX(COLUMN($AG40:CB40)*($AG40:CB40=2))>MAX(COLUMN($AG40:CB40)*($AG40:CB40=1))),IF(COLUMN(CC40)-MAX(COLUMN($AG40:CB40)*($AG40:CB40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CC40)-MAX(COLUMN($AG40:CB40)*($AG40:CB40=3))=$J40,3,0),IF(COLUMN(CC40)-MAX(COLUMN($AG40:CB40)*($AG40:CB40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CC40)*($AG40:CC40=1))>MAX(COLUMN($AG40:CC40)*($AG40:CC40=3)),MAX(COLUMN($AG40:CC40)*($AG40:CC40=1))>MAX(COLUMN($AG40:CC40)*($AG40:CC40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CD40)-MAX(COLUMN($AG40:CC40)*($AG40:CC40=1))=$J40,3,0),IF(COLUMN(CD40)-MAX(COLUMN($AG40:CC40)*($AG40:CC40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CC40)*($AG40:CC40=2))>MAX(COLUMN($AG40:CC40)*($AG40:CC40=3)),MAX(COLUMN($AG40:CC40)*($AG40:CC40=2))>MAX(COLUMN($AG40:CC40)*($AG40:CC40=1))),IF(COLUMN(CD40)-MAX(COLUMN($AG40:CC40)*($AG40:CC40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CD40)-MAX(COLUMN($AG40:CC40)*($AG40:CC40=3))=$J40,3,0),IF(COLUMN(CD40)-MAX(COLUMN($AG40:CC40)*($AG40:CC40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CD40)*($AG40:CD40=1))>MAX(COLUMN($AG40:CD40)*($AG40:CD40=3)),MAX(COLUMN($AG40:CD40)*($AG40:CD40=1))>MAX(COLUMN($AG40:CD40)*($AG40:CD40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CE40)-MAX(COLUMN($AG40:CD40)*($AG40:CD40=1))=$J40,3,0),IF(COLUMN(CE40)-MAX(COLUMN($AG40:CD40)*($AG40:CD40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CD40)*($AG40:CD40=2))>MAX(COLUMN($AG40:CD40)*($AG40:CD40=3)),MAX(COLUMN($AG40:CD40)*($AG40:CD40=2))>MAX(COLUMN($AG40:CD40)*($AG40:CD40=1))),IF(COLUMN(CE40)-MAX(COLUMN($AG40:CD40)*($AG40:CD40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CE40)-MAX(COLUMN($AG40:CD40)*($AG40:CD40=3))=$J40,3,0),IF(COLUMN(CE40)-MAX(COLUMN($AG40:CD40)*($AG40:CD40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CE40)*($AG40:CE40=1))>MAX(COLUMN($AG40:CE40)*($AG40:CE40=3)),MAX(COLUMN($AG40:CE40)*($AG40:CE40=1))>MAX(COLUMN($AG40:CE40)*($AG40:CE40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CF40)-MAX(COLUMN($AG40:CE40)*($AG40:CE40=1))=$J40,3,0),IF(COLUMN(CF40)-MAX(COLUMN($AG40:CE40)*($AG40:CE40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CE40)*($AG40:CE40=2))>MAX(COLUMN($AG40:CE40)*($AG40:CE40=3)),MAX(COLUMN($AG40:CE40)*($AG40:CE40=2))>MAX(COLUMN($AG40:CE40)*($AG40:CE40=1))),IF(COLUMN(CF40)-MAX(COLUMN($AG40:CE40)*($AG40:CE40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CF40)-MAX(COLUMN($AG40:CE40)*($AG40:CE40=3))=$J40,3,0),IF(COLUMN(CF40)-MAX(COLUMN($AG40:CE40)*($AG40:CE40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CF40)*($AG40:CF40=1))>MAX(COLUMN($AG40:CF40)*($AG40:CF40=3)),MAX(COLUMN($AG40:CF40)*($AG40:CF40=1))>MAX(COLUMN($AG40:CF40)*($AG40:CF40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CG40)-MAX(COLUMN($AG40:CF40)*($AG40:CF40=1))=$J40,3,0),IF(COLUMN(CG40)-MAX(COLUMN($AG40:CF40)*($AG40:CF40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CF40)*($AG40:CF40=2))>MAX(COLUMN($AG40:CF40)*($AG40:CF40=3)),MAX(COLUMN($AG40:CF40)*($AG40:CF40=2))>MAX(COLUMN($AG40:CF40)*($AG40:CF40=1))),IF(COLUMN(CG40)-MAX(COLUMN($AG40:CF40)*($AG40:CF40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CG40)-MAX(COLUMN($AG40:CF40)*($AG40:CF40=3))=$J40,3,0),IF(COLUMN(CG40)-MAX(COLUMN($AG40:CF40)*($AG40:CF40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CG40)*($AG40:CG40=1))>MAX(COLUMN($AG40:CG40)*($AG40:CG40=3)),MAX(COLUMN($AG40:CG40)*($AG40:CG40=1))>MAX(COLUMN($AG40:CG40)*($AG40:CG40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CH40)-MAX(COLUMN($AG40:CG40)*($AG40:CG40=1))=$J40,3,0),IF(COLUMN(CH40)-MAX(COLUMN($AG40:CG40)*($AG40:CG40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CG40)*($AG40:CG40=2))>MAX(COLUMN($AG40:CG40)*($AG40:CG40=3)),MAX(COLUMN($AG40:CG40)*($AG40:CG40=2))>MAX(COLUMN($AG40:CG40)*($AG40:CG40=1))),IF(COLUMN(CH40)-MAX(COLUMN($AG40:CG40)*($AG40:CG40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CH40)-MAX(COLUMN($AG40:CG40)*($AG40:CG40=3))=$J40,3,0),IF(COLUMN(CH40)-MAX(COLUMN($AG40:CG40)*($AG40:CG40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CH40)*($AG40:CH40=1))>MAX(COLUMN($AG40:CH40)*($AG40:CH40=3)),MAX(COLUMN($AG40:CH40)*($AG40:CH40=1))>MAX(COLUMN($AG40:CH40)*($AG40:CH40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CI40)-MAX(COLUMN($AG40:CH40)*($AG40:CH40=1))=$J40,3,0),IF(COLUMN(CI40)-MAX(COLUMN($AG40:CH40)*($AG40:CH40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CH40)*($AG40:CH40=2))>MAX(COLUMN($AG40:CH40)*($AG40:CH40=3)),MAX(COLUMN($AG40:CH40)*($AG40:CH40=2))>MAX(COLUMN($AG40:CH40)*($AG40:CH40=1))),IF(COLUMN(CI40)-MAX(COLUMN($AG40:CH40)*($AG40:CH40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CI40)-MAX(COLUMN($AG40:CH40)*($AG40:CH40=3))=$J40,3,0),IF(COLUMN(CI40)-MAX(COLUMN($AG40:CH40)*($AG40:CH40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CI40)*($AG40:CI40=1))>MAX(COLUMN($AG40:CI40)*($AG40:CI40=3)),MAX(COLUMN($AG40:CI40)*($AG40:CI40=1))>MAX(COLUMN($AG40:CI40)*($AG40:CI40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CJ40)-MAX(COLUMN($AG40:CI40)*($AG40:CI40=1))=$J40,3,0),IF(COLUMN(CJ40)-MAX(COLUMN($AG40:CI40)*($AG40:CI40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CI40)*($AG40:CI40=2))>MAX(COLUMN($AG40:CI40)*($AG40:CI40=3)),MAX(COLUMN($AG40:CI40)*($AG40:CI40=2))>MAX(COLUMN($AG40:CI40)*($AG40:CI40=1))),IF(COLUMN(CJ40)-MAX(COLUMN($AG40:CI40)*($AG40:CI40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CJ40)-MAX(COLUMN($AG40:CI40)*($AG40:CI40=3))=$J40,3,0),IF(COLUMN(CJ40)-MAX(COLUMN($AG40:CI40)*($AG40:CI40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=1))>MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=3)),MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=1))>MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CK40)-MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=1))=$J40,3,0),IF(COLUMN(CK40)-MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=2))>MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=3)),MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=2))>MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=1))),IF(COLUMN(CK40)-MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CK40)-MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=3))=$J40,3,0),IF(COLUMN(CK40)-MAX(COLUMN($AG40:CJ40)*($AG40:CJ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CK40)*($AG40:CK40=1))>MAX(COLUMN($AG40:CK40)*($AG40:CK40=3)),MAX(COLUMN($AG40:CK40)*($AG40:CK40=1))>MAX(COLUMN($AG40:CK40)*($AG40:CK40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CL40)-MAX(COLUMN($AG40:CK40)*($AG40:CK40=1))=$J40,3,0),IF(COLUMN(CL40)-MAX(COLUMN($AG40:CK40)*($AG40:CK40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CK40)*($AG40:CK40=2))>MAX(COLUMN($AG40:CK40)*($AG40:CK40=3)),MAX(COLUMN($AG40:CK40)*($AG40:CK40=2))>MAX(COLUMN($AG40:CK40)*($AG40:CK40=1))),IF(COLUMN(CL40)-MAX(COLUMN($AG40:CK40)*($AG40:CK40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CL40)-MAX(COLUMN($AG40:CK40)*($AG40:CK40=3))=$J40,3,0),IF(COLUMN(CL40)-MAX(COLUMN($AG40:CK40)*($AG40:CK40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CL40)*($AG40:CL40=1))>MAX(COLUMN($AG40:CL40)*($AG40:CL40=3)),MAX(COLUMN($AG40:CL40)*($AG40:CL40=1))>MAX(COLUMN($AG40:CL40)*($AG40:CL40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CM40)-MAX(COLUMN($AG40:CL40)*($AG40:CL40=1))=$J40,3,0),IF(COLUMN(CM40)-MAX(COLUMN($AG40:CL40)*($AG40:CL40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CL40)*($AG40:CL40=2))>MAX(COLUMN($AG40:CL40)*($AG40:CL40=3)),MAX(COLUMN($AG40:CL40)*($AG40:CL40=2))>MAX(COLUMN($AG40:CL40)*($AG40:CL40=1))),IF(COLUMN(CM40)-MAX(COLUMN($AG40:CL40)*($AG40:CL40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CM40)-MAX(COLUMN($AG40:CL40)*($AG40:CL40=3))=$J40,3,0),IF(COLUMN(CM40)-MAX(COLUMN($AG40:CL40)*($AG40:CL40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CM40)*($AG40:CM40=1))>MAX(COLUMN($AG40:CM40)*($AG40:CM40=3)),MAX(COLUMN($AG40:CM40)*($AG40:CM40=1))>MAX(COLUMN($AG40:CM40)*($AG40:CM40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CN40)-MAX(COLUMN($AG40:CM40)*($AG40:CM40=1))=$J40,3,0),IF(COLUMN(CN40)-MAX(COLUMN($AG40:CM40)*($AG40:CM40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CM40)*($AG40:CM40=2))>MAX(COLUMN($AG40:CM40)*($AG40:CM40=3)),MAX(COLUMN($AG40:CM40)*($AG40:CM40=2))>MAX(COLUMN($AG40:CM40)*($AG40:CM40=1))),IF(COLUMN(CN40)-MAX(COLUMN($AG40:CM40)*($AG40:CM40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CN40)-MAX(COLUMN($AG40:CM40)*($AG40:CM40=3))=$J40,3,0),IF(COLUMN(CN40)-MAX(COLUMN($AG40:CM40)*($AG40:CM40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CN40)*($AG40:CN40=1))>MAX(COLUMN($AG40:CN40)*($AG40:CN40=3)),MAX(COLUMN($AG40:CN40)*($AG40:CN40=1))>MAX(COLUMN($AG40:CN40)*($AG40:CN40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CO40)-MAX(COLUMN($AG40:CN40)*($AG40:CN40=1))=$J40,3,0),IF(COLUMN(CO40)-MAX(COLUMN($AG40:CN40)*($AG40:CN40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CN40)*($AG40:CN40=2))>MAX(COLUMN($AG40:CN40)*($AG40:CN40=3)),MAX(COLUMN($AG40:CN40)*($AG40:CN40=2))>MAX(COLUMN($AG40:CN40)*($AG40:CN40=1))),IF(COLUMN(CO40)-MAX(COLUMN($AG40:CN40)*($AG40:CN40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CO40)-MAX(COLUMN($AG40:CN40)*($AG40:CN40=3))=$J40,3,0),IF(COLUMN(CO40)-MAX(COLUMN($AG40:CN40)*($AG40:CN40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CO40)*($AG40:CO40=1))>MAX(COLUMN($AG40:CO40)*($AG40:CO40=3)),MAX(COLUMN($AG40:CO40)*($AG40:CO40=1))>MAX(COLUMN($AG40:CO40)*($AG40:CO40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CP40)-MAX(COLUMN($AG40:CO40)*($AG40:CO40=1))=$J40,3,0),IF(COLUMN(CP40)-MAX(COLUMN($AG40:CO40)*($AG40:CO40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CO40)*($AG40:CO40=2))>MAX(COLUMN($AG40:CO40)*($AG40:CO40=3)),MAX(COLUMN($AG40:CO40)*($AG40:CO40=2))>MAX(COLUMN($AG40:CO40)*($AG40:CO40=1))),IF(COLUMN(CP40)-MAX(COLUMN($AG40:CO40)*($AG40:CO40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CP40)-MAX(COLUMN($AG40:CO40)*($AG40:CO40=3))=$J40,3,0),IF(COLUMN(CP40)-MAX(COLUMN($AG40:CO40)*($AG40:CO40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CP40)*($AG40:CP40=1))>MAX(COLUMN($AG40:CP40)*($AG40:CP40=3)),MAX(COLUMN($AG40:CP40)*($AG40:CP40=1))>MAX(COLUMN($AG40:CP40)*($AG40:CP40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CQ40)-MAX(COLUMN($AG40:CP40)*($AG40:CP40=1))=$J40,3,0),IF(COLUMN(CQ40)-MAX(COLUMN($AG40:CP40)*($AG40:CP40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CP40)*($AG40:CP40=2))>MAX(COLUMN($AG40:CP40)*($AG40:CP40=3)),MAX(COLUMN($AG40:CP40)*($AG40:CP40=2))>MAX(COLUMN($AG40:CP40)*($AG40:CP40=1))),IF(COLUMN(CQ40)-MAX(COLUMN($AG40:CP40)*($AG40:CP40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CQ40)-MAX(COLUMN($AG40:CP40)*($AG40:CP40=3))=$J40,3,0),IF(COLUMN(CQ40)-MAX(COLUMN($AG40:CP40)*($AG40:CP40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=1))>MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=3)),MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=1))>MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CR40)-MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=1))=$J40,3,0),IF(COLUMN(CR40)-MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=2))>MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=3)),MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=2))>MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=1))),IF(COLUMN(CR40)-MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CR40)-MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=3))=$J40,3,0),IF(COLUMN(CR40)-MAX(COLUMN($AG40:CQ40)*($AG40:CQ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CR40)*($AG40:CR40=1))>MAX(COLUMN($AG40:CR40)*($AG40:CR40=3)),MAX(COLUMN($AG40:CR40)*($AG40:CR40=1))>MAX(COLUMN($AG40:CR40)*($AG40:CR40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CS40)-MAX(COLUMN($AG40:CR40)*($AG40:CR40=1))=$J40,3,0),IF(COLUMN(CS40)-MAX(COLUMN($AG40:CR40)*($AG40:CR40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CR40)*($AG40:CR40=2))>MAX(COLUMN($AG40:CR40)*($AG40:CR40=3)),MAX(COLUMN($AG40:CR40)*($AG40:CR40=2))>MAX(COLUMN($AG40:CR40)*($AG40:CR40=1))),IF(COLUMN(CS40)-MAX(COLUMN($AG40:CR40)*($AG40:CR40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CS40)-MAX(COLUMN($AG40:CR40)*($AG40:CR40=3))=$J40,3,0),IF(COLUMN(CS40)-MAX(COLUMN($AG40:CR40)*($AG40:CR40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CS40)*($AG40:CS40=1))>MAX(COLUMN($AG40:CS40)*($AG40:CS40=3)),MAX(COLUMN($AG40:CS40)*($AG40:CS40=1))>MAX(COLUMN($AG40:CS40)*($AG40:CS40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CT40)-MAX(COLUMN($AG40:CS40)*($AG40:CS40=1))=$J40,3,0),IF(COLUMN(CT40)-MAX(COLUMN($AG40:CS40)*($AG40:CS40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CS40)*($AG40:CS40=2))>MAX(COLUMN($AG40:CS40)*($AG40:CS40=3)),MAX(COLUMN($AG40:CS40)*($AG40:CS40=2))>MAX(COLUMN($AG40:CS40)*($AG40:CS40=1))),IF(COLUMN(CT40)-MAX(COLUMN($AG40:CS40)*($AG40:CS40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CT40)-MAX(COLUMN($AG40:CS40)*($AG40:CS40=3))=$J40,3,0),IF(COLUMN(CT40)-MAX(COLUMN($AG40:CS40)*($AG40:CS40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CT40)*($AG40:CT40=1))>MAX(COLUMN($AG40:CT40)*($AG40:CT40=3)),MAX(COLUMN($AG40:CT40)*($AG40:CT40=1))>MAX(COLUMN($AG40:CT40)*($AG40:CT40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CU40)-MAX(COLUMN($AG40:CT40)*($AG40:CT40=1))=$J40,3,0),IF(COLUMN(CU40)-MAX(COLUMN($AG40:CT40)*($AG40:CT40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CT40)*($AG40:CT40=2))>MAX(COLUMN($AG40:CT40)*($AG40:CT40=3)),MAX(COLUMN($AG40:CT40)*($AG40:CT40=2))>MAX(COLUMN($AG40:CT40)*($AG40:CT40=1))),IF(COLUMN(CU40)-MAX(COLUMN($AG40:CT40)*($AG40:CT40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CU40)-MAX(COLUMN($AG40:CT40)*($AG40:CT40=3))=$J40,3,0),IF(COLUMN(CU40)-MAX(COLUMN($AG40:CT40)*($AG40:CT40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CU40)*($AG40:CU40=1))>MAX(COLUMN($AG40:CU40)*($AG40:CU40=3)),MAX(COLUMN($AG40:CU40)*($AG40:CU40=1))>MAX(COLUMN($AG40:CU40)*($AG40:CU40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CV40)-MAX(COLUMN($AG40:CU40)*($AG40:CU40=1))=$J40,3,0),IF(COLUMN(CV40)-MAX(COLUMN($AG40:CU40)*($AG40:CU40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CU40)*($AG40:CU40=2))>MAX(COLUMN($AG40:CU40)*($AG40:CU40=3)),MAX(COLUMN($AG40:CU40)*($AG40:CU40=2))>MAX(COLUMN($AG40:CU40)*($AG40:CU40=1))),IF(COLUMN(CV40)-MAX(COLUMN($AG40:CU40)*($AG40:CU40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CV40)-MAX(COLUMN($AG40:CU40)*($AG40:CU40=3))=$J40,3,0),IF(COLUMN(CV40)-MAX(COLUMN($AG40:CU40)*($AG40:CU40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CV40)*($AG40:CV40=1))>MAX(COLUMN($AG40:CV40)*($AG40:CV40=3)),MAX(COLUMN($AG40:CV40)*($AG40:CV40=1))>MAX(COLUMN($AG40:CV40)*($AG40:CV40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CW40)-MAX(COLUMN($AG40:CV40)*($AG40:CV40=1))=$J40,3,0),IF(COLUMN(CW40)-MAX(COLUMN($AG40:CV40)*($AG40:CV40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CV40)*($AG40:CV40=2))>MAX(COLUMN($AG40:CV40)*($AG40:CV40=3)),MAX(COLUMN($AG40:CV40)*($AG40:CV40=2))>MAX(COLUMN($AG40:CV40)*($AG40:CV40=1))),IF(COLUMN(CW40)-MAX(COLUMN($AG40:CV40)*($AG40:CV40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CW40)-MAX(COLUMN($AG40:CV40)*($AG40:CV40=3))=$J40,3,0),IF(COLUMN(CW40)-MAX(COLUMN($AG40:CV40)*($AG40:CV40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CW40)*($AG40:CW40=1))>MAX(COLUMN($AG40:CW40)*($AG40:CW40=3)),MAX(COLUMN($AG40:CW40)*($AG40:CW40=1))>MAX(COLUMN($AG40:CW40)*($AG40:CW40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CX40)-MAX(COLUMN($AG40:CW40)*($AG40:CW40=1))=$J40,3,0),IF(COLUMN(CX40)-MAX(COLUMN($AG40:CW40)*($AG40:CW40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CW40)*($AG40:CW40=2))>MAX(COLUMN($AG40:CW40)*($AG40:CW40=3)),MAX(COLUMN($AG40:CW40)*($AG40:CW40=2))>MAX(COLUMN($AG40:CW40)*($AG40:CW40=1))),IF(COLUMN(CX40)-MAX(COLUMN($AG40:CW40)*($AG40:CW40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CX40)-MAX(COLUMN($AG40:CW40)*($AG40:CW40=3))=$J40,3,0),IF(COLUMN(CX40)-MAX(COLUMN($AG40:CW40)*($AG40:CW40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CX40)*($AG40:CX40=1))>MAX(COLUMN($AG40:CX40)*($AG40:CX40=3)),MAX(COLUMN($AG40:CX40)*($AG40:CX40=1))>MAX(COLUMN($AG40:CX40)*($AG40:CX40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CY40)-MAX(COLUMN($AG40:CX40)*($AG40:CX40=1))=$J40,3,0),IF(COLUMN(CY40)-MAX(COLUMN($AG40:CX40)*($AG40:CX40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CX40)*($AG40:CX40=2))>MAX(COLUMN($AG40:CX40)*($AG40:CX40=3)),MAX(COLUMN($AG40:CX40)*($AG40:CX40=2))>MAX(COLUMN($AG40:CX40)*($AG40:CX40=1))),IF(COLUMN(CY40)-MAX(COLUMN($AG40:CX40)*($AG40:CX40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CY40)-MAX(COLUMN($AG40:CX40)*($AG40:CX40=3))=$J40,3,0),IF(COLUMN(CY40)-MAX(COLUMN($AG40:CX40)*($AG40:CX40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CY40)*($AG40:CY40=1))>MAX(COLUMN($AG40:CY40)*($AG40:CY40=3)),MAX(COLUMN($AG40:CY40)*($AG40:CY40=1))>MAX(COLUMN($AG40:CY40)*($AG40:CY40=2))),IF($K40=\"Not Possible\",IF(COLUMN(CZ40)-MAX(COLUMN($AG40:CY40)*($AG40:CY40=1))=$J40,3,0),IF(COLUMN(CZ40)-MAX(COLUMN($AG40:CY40)*($AG40:CY40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CY40)*($AG40:CY40=2))>MAX(COLUMN($AG40:CY40)*($AG40:CY40=3)),MAX(COLUMN($AG40:CY40)*($AG40:CY40=2))>MAX(COLUMN($AG40:CY40)*($AG40:CY40=1))),IF(COLUMN(CZ40)-MAX(COLUMN($AG40:CY40)*($AG40:CY40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(CZ40)-MAX(COLUMN($AG40:CY40)*($AG40:CY40=3))=$J40,3,0),IF(COLUMN(CZ40)-MAX(COLUMN($AG40:CY40)*($AG40:CY40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=1))>MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=3)),MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=1))>MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DA40)-MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=1))=$J40,3,0),IF(COLUMN(DA40)-MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=2))>MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=3)),MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=2))>MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=1))),IF(COLUMN(DA40)-MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DA40)-MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=3))=$J40,3,0),IF(COLUMN(DA40)-MAX(COLUMN($AG40:CZ40)*($AG40:CZ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DA40)*($AG40:DA40=1))>MAX(COLUMN($AG40:DA40)*($AG40:DA40=3)),MAX(COLUMN($AG40:DA40)*($AG40:DA40=1))>MAX(COLUMN($AG40:DA40)*($AG40:DA40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DB40)-MAX(COLUMN($AG40:DA40)*($AG40:DA40=1))=$J40,3,0),IF(COLUMN(DB40)-MAX(COLUMN($AG40:DA40)*($AG40:DA40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DA40)*($AG40:DA40=2))>MAX(COLUMN($AG40:DA40)*($AG40:DA40=3)),MAX(COLUMN($AG40:DA40)*($AG40:DA40=2))>MAX(COLUMN($AG40:DA40)*($AG40:DA40=1))),IF(COLUMN(DB40)-MAX(COLUMN($AG40:DA40)*($AG40:DA40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DB40)-MAX(COLUMN($AG40:DA40)*($AG40:DA40=3))=$J40,3,0),IF(COLUMN(DB40)-MAX(COLUMN($AG40:DA40)*($AG40:DA40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DB40)*($AG40:DB40=1))>MAX(COLUMN($AG40:DB40)*($AG40:DB40=3)),MAX(COLUMN($AG40:DB40)*($AG40:DB40=1))>MAX(COLUMN($AG40:DB40)*($AG40:DB40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DC40)-MAX(COLUMN($AG40:DB40)*($AG40:DB40=1))=$J40,3,0),IF(COLUMN(DC40)-MAX(COLUMN($AG40:DB40)*($AG40:DB40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DB40)*($AG40:DB40=2))>MAX(COLUMN($AG40:DB40)*($AG40:DB40=3)),MAX(COLUMN($AG40:DB40)*($AG40:DB40=2))>MAX(COLUMN($AG40:DB40)*($AG40:DB40=1))),IF(COLUMN(DC40)-MAX(COLUMN($AG40:DB40)*($AG40:DB40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DC40)-MAX(COLUMN($AG40:DB40)*($AG40:DB40=3))=$J40,3,0),IF(COLUMN(DC40)-MAX(COLUMN($AG40:DB40)*($AG40:DB40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DC40)*($AG40:DC40=1))>MAX(COLUMN($AG40:DC40)*($AG40:DC40=3)),MAX(COLUMN($AG40:DC40)*($AG40:DC40=1))>MAX(COLUMN($AG40:DC40)*($AG40:DC40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DD40)-MAX(COLUMN($AG40:DC40)*($AG40:DC40=1))=$J40,3,0),IF(COLUMN(DD40)-MAX(COLUMN($AG40:DC40)*($AG40:DC40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DC40)*($AG40:DC40=2))>MAX(COLUMN($AG40:DC40)*($AG40:DC40=3)),MAX(COLUMN($AG40:DC40)*($AG40:DC40=2))>MAX(COLUMN($AG40:DC40)*($AG40:DC40=1))),IF(COLUMN(DD40)-MAX(COLUMN($AG40:DC40)*($AG40:DC40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DD40)-MAX(COLUMN($AG40:DC40)*($AG40:DC40=3))=$J40,3,0),IF(COLUMN(DD40)-MAX(COLUMN($AG40:DC40)*($AG40:DC40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DD40)*($AG40:DD40=1))>MAX(COLUMN($AG40:DD40)*($AG40:DD40=3)),MAX(COLUMN($AG40:DD40)*($AG40:DD40=1))>MAX(COLUMN($AG40:DD40)*($AG40:DD40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DE40)-MAX(COLUMN($AG40:DD40)*($AG40:DD40=1))=$J40,3,0),IF(COLUMN(DE40)-MAX(COLUMN($AG40:DD40)*($AG40:DD40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DD40)*($AG40:DD40=2))>MAX(COLUMN($AG40:DD40)*($AG40:DD40=3)),MAX(COLUMN($AG40:DD40)*($AG40:DD40=2))>MAX(COLUMN($AG40:DD40)*($AG40:DD40=1))),IF(COLUMN(DE40)-MAX(COLUMN($AG40:DD40)*($AG40:DD40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DE40)-MAX(COLUMN($AG40:DD40)*($AG40:DD40=3))=$J40,3,0),IF(COLUMN(DE40)-MAX(COLUMN($AG40:DD40)*($AG40:DD40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DE40)*($AG40:DE40=1))>MAX(COLUMN($AG40:DE40)*($AG40:DE40=3)),MAX(COLUMN($AG40:DE40)*($AG40:DE40=1))>MAX(COLUMN($AG40:DE40)*($AG40:DE40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DF40)-MAX(COLUMN($AG40:DE40)*($AG40:DE40=1))=$J40,3,0),IF(COLUMN(DF40)-MAX(COLUMN($AG40:DE40)*($AG40:DE40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DE40)*($AG40:DE40=2))>MAX(COLUMN($AG40:DE40)*($AG40:DE40=3)),MAX(COLUMN($AG40:DE40)*($AG40:DE40=2))>MAX(COLUMN($AG40:DE40)*($AG40:DE40=1))),IF(COLUMN(DF40)-MAX(COLUMN($AG40:DE40)*($AG40:DE40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DF40)-MAX(COLUMN($AG40:DE40)*($AG40:DE40=3))=$J40,3,0),IF(COLUMN(DF40)-MAX(COLUMN($AG40:DE40)*($AG40:DE40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DF40)*($AG40:DF40=1))>MAX(COLUMN($AG40:DF40)*($AG40:DF40=3)),MAX(COLUMN($AG40:DF40)*($AG40:DF40=1))>MAX(COLUMN($AG40:DF40)*($AG40:DF40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DG40)-MAX(COLUMN($AG40:DF40)*($AG40:DF40=1))=$J40,3,0),IF(COLUMN(DG40)-MAX(COLUMN($AG40:DF40)*($AG40:DF40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DF40)*($AG40:DF40=2))>MAX(COLUMN($AG40:DF40)*($AG40:DF40=3)),MAX(COLUMN($AG40:DF40)*($AG40:DF40=2))>MAX(COLUMN($AG40:DF40)*($AG40:DF40=1))),IF(COLUMN(DG40)-MAX(COLUMN($AG40:DF40)*($AG40:DF40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DG40)-MAX(COLUMN($AG40:DF40)*($AG40:DF40=3))=$J40,3,0),IF(COLUMN(DG40)-MAX(COLUMN($AG40:DF40)*($AG40:DF40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DG40)*($AG40:DG40=1))>MAX(COLUMN($AG40:DG40)*($AG40:DG40=3)),MAX(COLUMN($AG40:DG40)*($AG40:DG40=1))>MAX(COLUMN($AG40:DG40)*($AG40:DG40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DH40)-MAX(COLUMN($AG40:DG40)*($AG40:DG40=1))=$J40,3,0),IF(COLUMN(DH40)-MAX(COLUMN($AG40:DG40)*($AG40:DG40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DG40)*($AG40:DG40=2))>MAX(COLUMN($AG40:DG40)*($AG40:DG40=3)),MAX(COLUMN($AG40:DG40)*($AG40:DG40=2))>MAX(COLUMN($AG40:DG40)*($AG40:DG40=1))),IF(COLUMN(DH40)-MAX(COLUMN($AG40:DG40)*($AG40:DG40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DH40)-MAX(COLUMN($AG40:DG40)*($AG40:DG40=3))=$J40,3,0),IF(COLUMN(DH40)-MAX(COLUMN($AG40:DG40)*($AG40:DG40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DH40)*($AG40:DH40=1))>MAX(COLUMN($AG40:DH40)*($AG40:DH40=3)),MAX(COLUMN($AG40:DH40)*($AG40:DH40=1))>MAX(COLUMN($AG40:DH40)*($AG40:DH40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DI40)-MAX(COLUMN($AG40:DH40)*($AG40:DH40=1))=$J40,3,0),IF(COLUMN(DI40)-MAX(COLUMN($AG40:DH40)*($AG40:DH40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DH40)*($AG40:DH40=2))>MAX(COLUMN($AG40:DH40)*($AG40:DH40=3)),MAX(COLUMN($AG40:DH40)*($AG40:DH40=2))>MAX(COLUMN($AG40:DH40)*($AG40:DH40=1))),IF(COLUMN(DI40)-MAX(COLUMN($AG40:DH40)*($AG40:DH40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DI40)-MAX(COLUMN($AG40:DH40)*($AG40:DH40=3))=$J40,3,0),IF(COLUMN(DI40)-MAX(COLUMN($AG40:DH40)*($AG40:DH40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DI40)*($AG40:DI40=1))>MAX(COLUMN($AG40:DI40)*($AG40:DI40=3)),MAX(COLUMN($AG40:DI40)*($AG40:DI40=1))>MAX(COLUMN($AG40:DI40)*($AG40:DI40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DJ40)-MAX(COLUMN($AG40:DI40)*($AG40:DI40=1))=$J40,3,0),IF(COLUMN(DJ40)-MAX(COLUMN($AG40:DI40)*($AG40:DI40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DI40)*($AG40:DI40=2))>MAX(COLUMN($AG40:DI40)*($AG40:DI40=3)),MAX(COLUMN($AG40:DI40)*($AG40:DI40=2))>MAX(COLUMN($AG40:DI40)*($AG40:DI40=1))),IF(COLUMN(DJ40)-MAX(COLUMN($AG40:DI40)*($AG40:DI40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DJ40)-MAX(COLUMN($AG40:DI40)*($AG40:DI40=3))=$J40,3,0),IF(COLUMN(DJ40)-MAX(COLUMN($AG40:DI40)*($AG40:DI40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=1))>MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=3)),MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=1))>MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DK40)-MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=1))=$J40,3,0),IF(COLUMN(DK40)-MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=2))>MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=3)),MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=2))>MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=1))),IF(COLUMN(DK40)-MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DK40)-MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=3))=$J40,3,0),IF(COLUMN(DK40)-MAX(COLUMN($AG40:DJ40)*($AG40:DJ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DK40)*($AG40:DK40=1))>MAX(COLUMN($AG40:DK40)*($AG40:DK40=3)),MAX(COLUMN($AG40:DK40)*($AG40:DK40=1))>MAX(COLUMN($AG40:DK40)*($AG40:DK40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DL40)-MAX(COLUMN($AG40:DK40)*($AG40:DK40=1))=$J40,3,0),IF(COLUMN(DL40)-MAX(COLUMN($AG40:DK40)*($AG40:DK40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DK40)*($AG40:DK40=2))>MAX(COLUMN($AG40:DK40)*($AG40:DK40=3)),MAX(COLUMN($AG40:DK40)*($AG40:DK40=2))>MAX(COLUMN($AG40:DK40)*($AG40:DK40=1))),IF(COLUMN(DL40)-MAX(COLUMN($AG40:DK40)*($AG40:DK40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DL40)-MAX(COLUMN($AG40:DK40)*($AG40:DK40=3))=$J40,3,0),IF(COLUMN(DL40)-MAX(COLUMN($AG40:DK40)*($AG40:DK40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DL40)*($AG40:DL40=1))>MAX(COLUMN($AG40:DL40)*($AG40:DL40=3)),MAX(COLUMN($AG40:DL40)*($AG40:DL40=1))>MAX(COLUMN($AG40:DL40)*($AG40:DL40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DM40)-MAX(COLUMN($AG40:DL40)*($AG40:DL40=1))=$J40,3,0),IF(COLUMN(DM40)-MAX(COLUMN($AG40:DL40)*($AG40:DL40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DL40)*($AG40:DL40=2))>MAX(COLUMN($AG40:DL40)*($AG40:DL40=3)),MAX(COLUMN($AG40:DL40)*($AG40:DL40=2))>MAX(COLUMN($AG40:DL40)*($AG40:DL40=1))),IF(COLUMN(DM40)-MAX(COLUMN($AG40:DL40)*($AG40:DL40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DM40)-MAX(COLUMN($AG40:DL40)*($AG40:DL40=3))=$J40,3,0),IF(COLUMN(DM40)-MAX(COLUMN($AG40:DL40)*($AG40:DL40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DM40)*($AG40:DM40=1))>MAX(COLUMN($AG40:DM40)*($AG40:DM40=3)),MAX(COLUMN($AG40:DM40)*($AG40:DM40=1))>MAX(COLUMN($AG40:DM40)*($AG40:DM40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DN40)-MAX(COLUMN($AG40:DM40)*($AG40:DM40=1))=$J40,3,0),IF(COLUMN(DN40)-MAX(COLUMN($AG40:DM40)*($AG40:DM40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DM40)*($AG40:DM40=2))>MAX(COLUMN($AG40:DM40)*($AG40:DM40=3)),MAX(COLUMN($AG40:DM40)*($AG40:DM40=2))>MAX(COLUMN($AG40:DM40)*($AG40:DM40=1))),IF(COLUMN(DN40)-MAX(COLUMN($AG40:DM40)*($AG40:DM40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DN40)-MAX(COLUMN($AG40:DM40)*($AG40:DM40=3))=$J40,3,0),IF(COLUMN(DN40)-MAX(COLUMN($AG40:DM40)*($AG40:DM40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DN40)*($AG40:DN40=1))>MAX(COLUMN($AG40:DN40)*($AG40:DN40=3)),MAX(COLUMN($AG40:DN40)*($AG40:DN40=1))>MAX(COLUMN($AG40:DN40)*($AG40:DN40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DO40)-MAX(COLUMN($AG40:DN40)*($AG40:DN40=1))=$J40,3,0),IF(COLUMN(DO40)-MAX(COLUMN($AG40:DN40)*($AG40:DN40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DN40)*($AG40:DN40=2))>MAX(COLUMN($AG40:DN40)*($AG40:DN40=3)),MAX(COLUMN($AG40:DN40)*($AG40:DN40=2))>MAX(COLUMN($AG40:DN40)*($AG40:DN40=1))),IF(COLUMN(DO40)-MAX(COLUMN($AG40:DN40)*($AG40:DN40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DO40)-MAX(COLUMN($AG40:DN40)*($AG40:DN40=3))=$J40,3,0),IF(COLUMN(DO40)-MAX(COLUMN($AG40:DN40)*($AG40:DN40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DO40)*($AG40:DO40=1))>MAX(COLUMN($AG40:DO40)*($AG40:DO40=3)),MAX(COLUMN($AG40:DO40)*($AG40:DO40=1))>MAX(COLUMN($AG40:DO40)*($AG40:DO40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DP40)-MAX(COLUMN($AG40:DO40)*($AG40:DO40=1))=$J40,3,0),IF(COLUMN(DP40)-MAX(COLUMN($AG40:DO40)*($AG40:DO40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DO40)*($AG40:DO40=2))>MAX(COLUMN($AG40:DO40)*($AG40:DO40=3)),MAX(COLUMN($AG40:DO40)*($AG40:DO40=2))>MAX(COLUMN($AG40:DO40)*($AG40:DO40=1))),IF(COLUMN(DP40)-MAX(COLUMN($AG40:DO40)*($AG40:DO40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DP40)-MAX(COLUMN($AG40:DO40)*($AG40:DO40=3))=$J40,3,0),IF(COLUMN(DP40)-MAX(COLUMN($AG40:DO40)*($AG40:DO40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DP40)*($AG40:DP40=1))>MAX(COLUMN($AG40:DP40)*($AG40:DP40=3)),MAX(COLUMN($AG40:DP40)*($AG40:DP40=1))>MAX(COLUMN($AG40:DP40)*($AG40:DP40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DQ40)-MAX(COLUMN($AG40:DP40)*($AG40:DP40=1))=$J40,3,0),IF(COLUMN(DQ40)-MAX(COLUMN($AG40:DP40)*($AG40:DP40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DP40)*($AG40:DP40=2))>MAX(COLUMN($AG40:DP40)*($AG40:DP40=3)),MAX(COLUMN($AG40:DP40)*($AG40:DP40=2))>MAX(COLUMN($AG40:DP40)*($AG40:DP40=1))),IF(COLUMN(DQ40)-MAX(COLUMN($AG40:DP40)*($AG40:DP40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DQ40)-MAX(COLUMN($AG40:DP40)*($AG40:DP40=3))=$J40,3,0),IF(COLUMN(DQ40)-MAX(COLUMN($AG40:DP40)*($AG40:DP40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=1))>MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=3)),MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=1))>MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DR40)-MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=1))=$J40,3,0),IF(COLUMN(DR40)-MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=2))>MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=3)),MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=2))>MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=1))),IF(COLUMN(DR40)-MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DR40)-MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=3))=$J40,3,0),IF(COLUMN(DR40)-MAX(COLUMN($AG40:DQ40)*($AG40:DQ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DR40)*($AG40:DR40=1))>MAX(COLUMN($AG40:DR40)*($AG40:DR40=3)),MAX(COLUMN($AG40:DR40)*($AG40:DR40=1))>MAX(COLUMN($AG40:DR40)*($AG40:DR40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DS40)-MAX(COLUMN($AG40:DR40)*($AG40:DR40=1))=$J40,3,0),IF(COLUMN(DS40)-MAX(COLUMN($AG40:DR40)*($AG40:DR40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DR40)*($AG40:DR40=2))>MAX(COLUMN($AG40:DR40)*($AG40:DR40=3)),MAX(COLUMN($AG40:DR40)*($AG40:DR40=2))>MAX(COLUMN($AG40:DR40)*($AG40:DR40=1))),IF(COLUMN(DS40)-MAX(COLUMN($AG40:DR40)*($AG40:DR40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DS40)-MAX(COLUMN($AG40:DR40)*($AG40:DR40=3))=$J40,3,0),IF(COLUMN(DS40)-MAX(COLUMN($AG40:DR40)*($AG40:DR40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DS40)*($AG40:DS40=1))>MAX(COLUMN($AG40:DS40)*($AG40:DS40=3)),MAX(COLUMN($AG40:DS40)*($AG40:DS40=1))>MAX(COLUMN($AG40:DS40)*($AG40:DS40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DT40)-MAX(COLUMN($AG40:DS40)*($AG40:DS40=1))=$J40,3,0),IF(COLUMN(DT40)-MAX(COLUMN($AG40:DS40)*($AG40:DS40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DS40)*($AG40:DS40=2))>MAX(COLUMN($AG40:DS40)*($AG40:DS40=3)),MAX(COLUMN($AG40:DS40)*($AG40:DS40=2))>MAX(COLUMN($AG40:DS40)*($AG40:DS40=1))),IF(COLUMN(DT40)-MAX(COLUMN($AG40:DS40)*($AG40:DS40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DT40)-MAX(COLUMN($AG40:DS40)*($AG40:DS40=3))=$J40,3,0),IF(COLUMN(DT40)-MAX(COLUMN($AG40:DS40)*($AG40:DS40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DT40)*($AG40:DT40=1))>MAX(COLUMN($AG40:DT40)*($AG40:DT40=3)),MAX(COLUMN($AG40:DT40)*($AG40:DT40=1))>MAX(COLUMN($AG40:DT40)*($AG40:DT40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DU40)-MAX(COLUMN($AG40:DT40)*($AG40:DT40=1))=$J40,3,0),IF(COLUMN(DU40)-MAX(COLUMN($AG40:DT40)*($AG40:DT40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DT40)*($AG40:DT40=2))>MAX(COLUMN($AG40:DT40)*($AG40:DT40=3)),MAX(COLUMN($AG40:DT40)*($AG40:DT40=2))>MAX(COLUMN($AG40:DT40)*($AG40:DT40=1))),IF(COLUMN(DU40)-MAX(COLUMN($AG40:DT40)*($AG40:DT40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DU40)-MAX(COLUMN($AG40:DT40)*($AG40:DT40=3))=$J40,3,0),IF(COLUMN(DU40)-MAX(COLUMN($AG40:DT40)*($AG40:DT40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DU40)*($AG40:DU40=1))>MAX(COLUMN($AG40:DU40)*($AG40:DU40=3)),MAX(COLUMN($AG40:DU40)*($AG40:DU40=1))>MAX(COLUMN($AG40:DU40)*($AG40:DU40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DV40)-MAX(COLUMN($AG40:DU40)*($AG40:DU40=1))=$J40,3,0),IF(COLUMN(DV40)-MAX(COLUMN($AG40:DU40)*($AG40:DU40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DU40)*($AG40:DU40=2))>MAX(COLUMN($AG40:DU40)*($AG40:DU40=3)),MAX(COLUMN($AG40:DU40)*($AG40:DU40=2))>MAX(COLUMN($AG40:DU40)*($AG40:DU40=1))),IF(COLUMN(DV40)-MAX(COLUMN($AG40:DU40)*($AG40:DU40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DV40)-MAX(COLUMN($AG40:DU40)*($AG40:DU40=3))=$J40,3,0),IF(COLUMN(DV40)-MAX(COLUMN($AG40:DU40)*($AG40:DU40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DV40)*($AG40:DV40=1))>MAX(COLUMN($AG40:DV40)*($AG40:DV40=3)),MAX(COLUMN($AG40:DV40)*($AG40:DV40=1))>MAX(COLUMN($AG40:DV40)*($AG40:DV40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DW40)-MAX(COLUMN($AG40:DV40)*($AG40:DV40=1))=$J40,3,0),IF(COLUMN(DW40)-MAX(COLUMN($AG40:DV40)*($AG40:DV40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DV40)*($AG40:DV40=2))>MAX(COLUMN($AG40:DV40)*($AG40:DV40=3)),MAX(COLUMN($AG40:DV40)*($AG40:DV40=2))>MAX(COLUMN($AG40:DV40)*($AG40:DV40=1))),IF(COLUMN(DW40)-MAX(COLUMN($AG40:DV40)*($AG40:DV40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DW40)-MAX(COLUMN($AG40:DV40)*($AG40:DV40=3))=$J40,3,0),IF(COLUMN(DW40)-MAX(COLUMN($AG40:DV40)*($AG40:DV40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DW40)*($AG40:DW40=1))>MAX(COLUMN($AG40:DW40)*($AG40:DW40=3)),MAX(COLUMN($AG40:DW40)*($AG40:DW40=1))>MAX(COLUMN($AG40:DW40)*($AG40:DW40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DX40)-MAX(COLUMN($AG40:DW40)*($AG40:DW40=1))=$J40,3,0),IF(COLUMN(DX40)-MAX(COLUMN($AG40:DW40)*($AG40:DW40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DW40)*($AG40:DW40=2))>MAX(COLUMN($AG40:DW40)*($AG40:DW40=3)),MAX(COLUMN($AG40:DW40)*($AG40:DW40=2))>MAX(COLUMN($AG40:DW40)*($AG40:DW40=1))),IF(COLUMN(DX40)-MAX(COLUMN($AG40:DW40)*($AG40:DW40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DX40)-MAX(COLUMN($AG40:DW40)*($AG40:DW40=3))=$J40,3,0),IF(COLUMN(DX40)-MAX(COLUMN($AG40:DW40)*($AG40:DW40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DX40)*($AG40:DX40=1))>MAX(COLUMN($AG40:DX40)*($AG40:DX40=3)),MAX(COLUMN($AG40:DX40)*($AG40:DX40=1))>MAX(COLUMN($AG40:DX40)*($AG40:DX40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DY40)-MAX(COLUMN($AG40:DX40)*($AG40:DX40=1))=$J40,3,0),IF(COLUMN(DY40)-MAX(COLUMN($AG40:DX40)*($AG40:DX40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DX40)*($AG40:DX40=2))>MAX(COLUMN($AG40:DX40)*($AG40:DX40=3)),MAX(COLUMN($AG40:DX40)*($AG40:DX40=2))>MAX(COLUMN($AG40:DX40)*($AG40:DX40=1))),IF(COLUMN(DY40)-MAX(COLUMN($AG40:DX40)*($AG40:DX40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DY40)-MAX(COLUMN($AG40:DX40)*($AG40:DX40=3))=$J40,3,0),IF(COLUMN(DY40)-MAX(COLUMN($AG40:DX40)*($AG40:DX40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DY40)*($AG40:DY40=1))>MAX(COLUMN($AG40:DY40)*($AG40:DY40=3)),MAX(COLUMN($AG40:DY40)*($AG40:DY40=1))>MAX(COLUMN($AG40:DY40)*($AG40:DY40=2))),IF($K40=\"Not Possible\",IF(COLUMN(DZ40)-MAX(COLUMN($AG40:DY40)*($AG40:DY40=1))=$J40,3,0),IF(COLUMN(DZ40)-MAX(COLUMN($AG40:DY40)*($AG40:DY40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DY40)*($AG40:DY40=2))>MAX(COLUMN($AG40:DY40)*($AG40:DY40=3)),MAX(COLUMN($AG40:DY40)*($AG40:DY40=2))>MAX(COLUMN($AG40:DY40)*($AG40:DY40=1))),IF(COLUMN(DZ40)-MAX(COLUMN($AG40:DY40)*($AG40:DY40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(DZ40)-MAX(COLUMN($AG40:DY40)*($AG40:DY40=3))=$J40,3,0),IF(COLUMN(DZ40)-MAX(COLUMN($AG40:DY40)*($AG40:DY40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=1))>MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=3)),MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=1))>MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=2))),IF($K40=\"Not Possible\",IF(COLUMN(EA40)-MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=1))=$J40,3,0),IF(COLUMN(EA40)-MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=2))>MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=3)),MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=2))>MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=1))),IF(COLUMN(EA40)-MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(EA40)-MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=3))=$J40,3,0),IF(COLUMN(EA40)-MAX(COLUMN($AG40:DZ40)*($AG40:DZ40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:EA40)*($AG40:EA40=1))>MAX(COLUMN($AG40:EA40)*($AG40:EA40=3)),MAX(COLUMN($AG40:EA40)*($AG40:EA40=1))>MAX(COLUMN($AG40:EA40)*($AG40:EA40=2))),IF($K40=\"Not Possible\",IF(COLUMN(EB40)-MAX(COLUMN($AG40:EA40)*($AG40:EA40=1))=$J40,3,0),IF(COLUMN(EB40)-MAX(COLUMN($AG40:EA40)*($AG40:EA40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:EA40)*($AG40:EA40=2))>MAX(COLUMN($AG40:EA40)*($AG40:EA40=3)),MAX(COLUMN($AG40:EA40)*($AG40:EA40=2))>MAX(COLUMN($AG40:EA40)*($AG40:EA40=1))),IF(COLUMN(EB40)-MAX(COLUMN($AG40:EA40)*($AG40:EA40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(EB40)-MAX(COLUMN($AG40:EA40)*($AG40:EA40=3))=$J40,3,0),IF(COLUMN(EB40)-MAX(COLUMN($AG40:EA40)*($AG40:EA40=3))=$J40,2,0)))))","v":0},{"$f":"IF($AG40=4,0,IF(AND(MAX(COLUMN($AG40:EB40)*($AG40:EB40=1))>MAX(COLUMN($AG40:EB40)*($AG40:EB40=3)),MAX(COLUMN($AG40:EB40)*($AG40:EB40=1))>MAX(COLUMN($AG40:EB40)*($AG40:EB40=2))),IF($K40=\"Not Possible\",IF(COLUMN(EC40)-MAX(COLUMN($AG40:EB40)*($AG40:EB40=1))=$J40,3,0),IF(COLUMN(EC40)-MAX(COLUMN($AG40:EB40)*($AG40:EB40=1))=$J40,2,0)),IF(AND(MAX(COLUMN($AG40:EB40)*($AG40:EB40=2))>MAX(COLUMN($AG40:EB40)*($AG40:EB40=3)),MAX(COLUMN($AG40:EB40)*($AG40:EB40=2))>MAX(COLUMN($AG40:EB40)*($AG40:EB40=1))),IF(COLUMN(EC40)-MAX(COLUMN($AG40:EB40)*($AG40:EB40=2))=$L40,3,0),IF($K40=\"Not Possible\",IF(COLUMN(EC40)-MAX(COLUMN($AG40:EB40)*($AG40:EB40=3))=$J40,3,0),IF(COLUMN(EC40)-MAX(COLUMN($AG40:EB40)*($AG40:EB40=3))=$J40,2,0)))))","v":0}]
[null,null,null,null,null,null,"General Item"]
[]
[null,null,"Total project whole life carbon",null,{"$f":"SUM(E45,E139,E190,E195,E197,E202)","v":10431.990501132997}]
[]
[null,null,"Capital carbon",null,{"$f":"SUM(E46,E61,E87)","v":1833.0440159490679}]
[null,null,"Materials",null,{"$f":"SUM(Form_Elements[Capital - Materials])","v":1809.4145040000001}]
[null,null,"Materials",null,null,null,null,null,null,null,null,"Waste",null,null,null,"Transport of materials"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a"]
[]
[null,null,"Sub-Asset ref.","Sub-Asset description","Material","Material type","Material description","Measure units","Quantity","CO2e (t)","Blank","Waste %","Reused / Recycle / Removed","Distance to waste disposal","Blank2","Mode of transport","Supplier distance to site","Distance (km)","Other modes of transport used","Other distance (km)","Load no.","Rounded Load no.","Total Road C02e (com)","Total Oth Co2e (com)","Total Road Co2e (wtt)","Total Oth (wtt)","% of material Co2e (waste)","Waste distance","Waste (t)","Waste Co2e ","Dem % of material Co2e (waste)","Dem - Waste (t)","Dem -Waste Co2e"]
[null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Product_Stage[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":"BridEA0333"},"Desk","Steel","Plate - UK (EU) Average Recycled Content","N/A","m3",66.3,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[Quantity]]*(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],Form_Product_Stage[[#This Row],[Measure units]])))),\"\")","v":858.4523999999999},null,0.05,"Recycle","Local",null,"HGV","Local",{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Supplier distance to site]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Supplier distance to site]],SupplierDistance[],2,FALSE)),\"\")","v":25},"Freight Train",30,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))/(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Max Wieght]))),\"\")","v":15.67090909090909},{"$f":"IFERROR(ROUNDUP(Form_Product_Stage[[#This Row],[Load no.]],),\"\")","v":16},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Combustion Measure t CO2e]))*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":0.36262800000000001},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[Combustion Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/\n(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":0.43920700199999996},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[WTT Measure t CO2e])*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":7.9222834399999997E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[WTT Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":9.3395483999999987E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*Form_Product_Stage[[#This Row],[Waste %]],\"\")","v":42.922619999999995},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":25},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[% of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":3.2321249999999999},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":0.11133904821463124},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*(100%-Form_Product_Stage[[#This Row],[Waste %]]),\"\")","v":815.52977999999985},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Dem % of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":61.410374999999995},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Dem - Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":2.1154419160779936}]
[null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Product_Stage[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":"BridEA0333"},"Desk","Timber","Hardboard","N/A","m3",54,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[Quantity]]*(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],Form_Product_Stage[[#This Row],[Measure units]])))),\"\")","v":25.055999999999997},null,0.05,"Recycle","Local",null,"HGV","Local",{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Supplier distance to site]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Supplier distance to site]],SupplierDistance[],2,FALSE)),\"\")","v":25},"Freight Train",30,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))/(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Max Wieght]))),\"\")","v":1.3090909090909089},{"$f":"IFERROR(ROUNDUP(Form_Product_Stage[[#This Row],[Load no.]],),\"\")","v":2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Combustion Measure t CO2e]))*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":4.5328500000000001E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[Combustion Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/\n(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":3.6689759999999995E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[WTT Measure t CO2e])*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":9.9028542999999997E-3},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[WTT Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":7.8019199999999986E-3},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*Form_Product_Stage[[#This Row],[Waste %]],\"\")","v":1.2527999999999999},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":25},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[% of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":0.27},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":9.3008602755000006E-3},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*(100%-Form_Product_Stage[[#This Row],[Waste %]]),\"\")","v":23.803199999999997},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Dem % of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":5.13},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Dem - Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":0.1767163452345}]
[null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Product_Stage[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":"BridEA0334"},"Abutment","Concrete","Reinforced Precast Concrete (General)","32/40 MPa","m3",47.67,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[Quantity]]*(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],Form_Product_Stage[[#This Row],[Measure units]])))),\"\")","v":27.229103999999996},null,0.15,"Removed","Local",null,"HGV","Local",{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Supplier distance to site]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Supplier distance to site]],SupplierDistance[],2,FALSE)),\"\")","v":25},"Freight Train",30,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))/(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Max Wieght]))),\"\")","v":3.4669090909090907},{"$f":"IFERROR(ROUNDUP(Form_Product_Stage[[#This Row],[Load no.]],),\"\")","v":4},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Combustion Measure t CO2e]))*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":9.0657000000000001E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[Combustion Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/\n(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":9.7166714399999979E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[WTT Measure t CO2e])*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":1.9805708599999999E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[WTT Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":2.0662084799999998E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*Form_Product_Stage[[#This Row],[Waste %]],\"\")","v":4.084365599999999},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":25},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[% of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":2.1451499999999997},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":7.3895334888847489E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*(100%-Form_Product_Stage[[#This Row],[Waste %]]),\"\")","v":23.144738399999994},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Dem % of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":12.155849999999997},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Dem - Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":0.41874023103680236}]
[null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Product_Stage[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":"BridEA0335"},"Handrail","Steel","Stainless","N/A","m3",18,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[Quantity]]*(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],Form_Product_Stage[[#This Row],[Measure units]])))),\"\")","v":885.6},null,0.05,"Recycle","Local",null,"HGV","Local",{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Supplier distance to site]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Supplier distance to site]],SupplierDistance[],2,FALSE)),\"\")","v":25},"Freight Train",30,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))/(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Max Wieght]))),\"\")","v":4.3636363636363633},{"$f":"IFERROR(ROUNDUP(Form_Product_Stage[[#This Row],[Load no.]],),\"\")","v":5},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Combustion Measure t CO2e]))*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":0.11332125},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[Combustion Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/\n(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":0.12229919999999998},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[WTT Measure t CO2e])*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":2.4757135750000003E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[WTT Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":2.6006399999999999E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*Form_Product_Stage[[#This Row],[Waste %]],\"\")","v":44.28},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":25},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[% of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":0.9},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":3.1002867585E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*(100%-Form_Product_Stage[[#This Row],[Waste %]]),\"\")","v":841.31999999999994},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Dem % of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":17.099999999999998},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Dem - Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":0.58905448411499983}]
[null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Product_Stage[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":"BridEA0336"},"Concrete wingwall","Concrete","Reinforced Precast Concrete (General)","32/40 MPa","m3",17.5,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[Quantity]]*(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],Form_Product_Stage[[#This Row],[Measure units]])))),\"\")","v":9.9959999999999987},null,0.15,"Removed","Local",null,"HGV","Local",{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Supplier distance to site]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Supplier distance to site]],SupplierDistance[],2,FALSE)),\"\")","v":25},"Freight Train",30,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))/(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Max Wieght]))),\"\")","v":1.2727272727272725},{"$f":"IFERROR(ROUNDUP(Form_Product_Stage[[#This Row],[Load no.]],),\"\")","v":2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Combustion Measure t CO2e]))*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":4.5328500000000001E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[Combustion Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/\n(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":3.5670599999999997E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[WTT Measure t CO2e])*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":9.9028542999999997E-3},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[WTT Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":7.5851999999999985E-3},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*Form_Product_Stage[[#This Row],[Waste %]],\"\")","v":1.4993999999999998},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":25},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[% of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":0.78749999999999998},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":2.7127509136874998E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*(100%-Form_Product_Stage[[#This Row],[Waste %]]),\"\")","v":8.496599999999999},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Dem % of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":4.4624999999999995},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Dem - Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":0.15372255177562497}]
[null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Product_Stage[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":"BridEA0337"},"Erosion protection","Stone","General (Stone)","N/A","m3",19.5,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[Quantity]]*(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],Form_Product_Stage[[#This Row],[Measure units]])))),\"\")","v":3.081},null,0.05,"Reused","Local",null,"HGV","Local",{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Supplier distance to site]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Supplier distance to site]],SupplierDistance[],2,FALSE)),\"\")","v":25},"Freight Train",30,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))/(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Max Wieght]))),\"\")","v":1.1818181818181819},{"$f":"IFERROR(ROUNDUP(Form_Product_Stage[[#This Row],[Load no.]],),\"\")","v":2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Combustion Measure t CO2e]))*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":4.5328500000000001E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[Combustion Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/\n(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":3.3122699999999998E-2},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[WTT Measure t CO2e])*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":9.9028542999999997E-3},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[WTT Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":7.0434E-3},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*Form_Product_Stage[[#This Row],[Waste %]],\"\")","v":0.15405000000000002},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":25},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[% of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":0.24375000000000002},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":0},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*(100%-Form_Product_Stage[[#This Row],[Waste %]]),\"\")","v":2.9269499999999997},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Dem % of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":4.6312499999999996},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Dem - Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Product_Stage[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[Quantity]]*(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],Form_Product_Stage[[#This Row],[Measure units]])))),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Supplier distance to site]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Supplier distance to site]],SupplierDistance[],2,FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))/(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Max Wieght]))),\"\")","v":""},{"$f":"IFERROR(ROUNDUP(Form_Product_Stage[[#This Row],[Load no.]],),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Combustion Measure t CO2e]))*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[Combustion Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/\n(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[WTT Measure t CO2e])*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[WTT Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*Form_Product_Stage[[#This Row],[Waste %]],\"\")","v":""},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[% of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":""},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*(100%-Form_Product_Stage[[#This Row],[Waste %]]),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Dem % of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":""},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Dem - Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":""}]
[null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Product_Stage[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Product_Stage[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[Quantity]]*(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],Form_Product_Stage[[#This Row],[Measure units]])))),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Supplier distance to site]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Supplier distance to site]],SupplierDistance[],2,FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Material]]=\"\",\"\",(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))/(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Max Wieght]))),\"\")","v":""},{"$f":"IFERROR(ROUNDUP(Form_Product_Stage[[#This Row],[Load no.]],),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[Combustion Measure t CO2e]))*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[Combustion Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/\n(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Rounded Load no.]]*SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Mode of transport]],PlantDistance[WTT Measure t CO2e])*Form_Product_Stage[[#This Row],[Distance (km)]],\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Other distance (km)]]*(SUMIF(PlantDistance[Mode],Form_Product_Stage[[#This Row],[Other modes of transport used]],PlantDistance[WTT Measure t CO2e])*(Form_Product_Stage[[#This Row],[CO2e (t)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\")))),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*Form_Product_Stage[[#This Row],[Waste %]],\"\")","v":""},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Product_Stage[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[% of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":""},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[CO2e (t)]]*(100%-Form_Product_Stage[[#This Row],[Waste %]]),\"\")","v":""},{"$f":"IFERROR(Form_Product_Stage[[#This Row],[Dem % of material Co2e (waste)]]/(SUMIFS(MaterialsData[Co2e value],MaterialsData[M1],Form_Product_Stage[[#This Row],[Material]],MaterialsData[M1.1],Form_Product_Stage[[#This Row],[Material type]],MaterialsData[M1.1.1],Form_Product_Stage[[#This Row],[Material description]],MaterialsData[Unit],\"t\"))/8,\"\")","v":""},{"$f":"IFERROR(IF(Form_Product_Stage[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,(Form_Product_Stage[[#This Row],[Dem - Waste (t)]]*0.001377905226)*Form_Product_Stage[[#This Row],[Waste distance]]),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_Product_Stage[CO2e (t)])","v":1809.4145040000001}]
[]
[null,null,"Transport",null,{"$f":"SUM(Form_Elements[Capital - Transport])","v":12.088101592966996}]
[null,null,"Method Used:","Summary"]
[null,null,"Summary"]
[null,null,"Transport of materials",null,null,null,"Transport of non-contractor people",null,null,"Transport of contractor people",null,null,"Transport of plant"]
[null,null,null,null,null,"a"]
[null,null,"Mode of Transport","Distance (km)","Total Co2e (t)","Size of Project","EA staff","Consultants","Column1","Labour","Management staff",null,"Transport of plant"]
[null,null,"Road",{"$f":"IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Distance (km)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Other distance (km)]))","v":150},{"$f":"IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Total Road Co2e (wtt)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Total Oth (wtt)]))+(IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Total Road C02e (com)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Total Oth Co2e (com)])))","v":0.85608599164999988},{"$f":"IFERROR(IF(Form_Mod_2[Total construction cost]<1500000,DistanceLists!AK5,IF(AND(Form_Mod_2[Total construction cost]>=1500000,Form_Mod_2[Total construction cost]<5000000),DistanceLists!AK4,IF(AND(Form_Mod_2[Total construction cost]>=5000000,Form_Mod_2[Total construction cost]<10000000),DistanceLists!AK3,IF(Form_Mod_2[Total construction cost]>=10000000,DistanceLists!AK2,\"\")))),\"Construction Cost Error in Model Details Section\")","v":"Small (construction cost less than £1.5million, fewer than 8 people permanently on site)"},{"$f":"IFERROR(((Form_Mod_2[Total salaries cost]/44)*(SUMIF(AvgDistanceData_tbl[Area],Form_Mod_2[Project Location],AvgDistanceData_tbl[(2011) Average distance commuted to work (km)])*10)/40)*(0.000181845555555556),\"\")","v":0.291366174242425},{"$f":"IFERROR(((Form_Mod_2[Total consultant cost]/54)*(SUMIF(AvgDistanceData_tbl[Area],Form_Mod_2[Project Location],AvgDistanceData_tbl[(2011) Average distance commuted to work (km)])*10)/40)*(0.000181845555555556),\"\")","v":0.94963790123457026},null,{"$f":"IFERROR(SUMIF(ProjectSizeTransport[Size of project],Form_Const_Tran_LabourA64[Size of Project],ProjectSizeTransport[Labour Travel t CO2e per week])*(INT((Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7)+MOD(((Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7),1)*7/10),0)","v":6.7112927999999989},{"$f":"IFERROR(SUMIF(ProjectSizeTransport[Size of project],Form_Const_Tran_LabourA64[Size of Project],ProjectSizeTransport[Management Staff Travel t CO2e per week])*(INT((Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7)+MOD(((Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7),1)*7/10),0)","v":2.0879577599999997},null,{"$f":"IFERROR(SUMIF(PlantTranSum_tbl[Plant Transport (sum) Size of project],Form_Const_Tran_LabourA64[Size of Project],PlantTranSum_tbl[Total]),0)","v":0.26511050064000002}]
[null,null,"Aeroplane - Freight",{"$f":"IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Distance (km)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Other distance (km)]))","v":0},{"$f":"IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Total Road Co2e (wtt)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Total Oth (wtt)]))+(IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Total Road C02e (com)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Total Oth Co2e (com)])))","v":0}]
[null,null,"Freight Train",{"$f":"IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Distance (km)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Other distance (km)]))","v":180},{"$f":"IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Total Road Co2e (wtt)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Total Oth (wtt)]))+(IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Total Road C02e (com)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Total Oth Co2e (com)])))","v":0.92665046519999983}]
[null,null,"Cargo Ship",{"$f":"IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Distance (km)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Other distance (km)]))","v":0},{"$f":"IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Total Road Co2e (wtt)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Total Oth (wtt)]))+(IF(Form_Const_Tran_Mat[[#This Row],[Mode of Transport]]=\"Road\",SUM(Form_Product_Stage[Total Road C02e (com)]),SUMIF(Form_Product_Stage[Other modes of transport used],Form_Const_Tran_Mat[[#This Row],[Mode of Transport]],Form_Product_Stage[Total Oth Co2e (com)])))","v":0}]
[null,null,null,null,{"$f":"SUBTOTAL(109,Form_Const_Tran_Mat[Total Co2e (t)])","v":1.7827364568499997}]
[]
[null,null,"Detailed"]
[null,null,"Transport contractor/sub contractor people",null,null,null,null,null,null,null,"Transport of plant"]
[]
[null,null,"Vehicles","1-5 km","6-10 km","11-20 km","21-50 km","51+ k","CO2e (t)",null,"Vehicles","1-5 km","6-10 km","11-20 km","21-50 km","51+ k","CO2e (t)"]
[null,null,"Car",null,null,300,null,null,{"$f":"IFERROR(((Form_Const_Tran_LabourB.1[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_LabourB.1[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_LabourB.1[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_LabourB.1[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_LabourB.1[[#This Row],[51+ k]]*100))*(SUMIF(VehicleList_tbl[Vehicle],Form_Const_Tran_LabourB.1[[#This Row],[Vehicles]],VehicleList_tbl[Avrg])),\"\")","v":1.0170376666666667},null,"Tractor",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_Plant[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_Plant[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_Plant[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_Plant[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_Plant[[#This Row],[51+ k]]*100))*0.001104627086,\"\")","v":0}]
[null,null,"Car Share",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_LabourB.1[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_LabourB.1[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_LabourB.1[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_LabourB.1[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_LabourB.1[[#This Row],[51+ k]]*100))*(SUMIF(VehicleList_tbl[Vehicle],Form_Const_Tran_LabourB.1[[#This Row],[Vehicles]],VehicleList_tbl[Avrg])),\"\")","v":0},null,"Asphalt Paver",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_Plant[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_Plant[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_Plant[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_Plant[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_Plant[[#This Row],[51+ k]]*100))*0.001104627086,\"\")","v":0}]
[null,null,"Motorbike",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_LabourB.1[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_LabourB.1[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_LabourB.1[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_LabourB.1[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_LabourB.1[[#This Row],[51+ k]]*100))*(SUMIF(VehicleList_tbl[Vehicle],Form_Const_Tran_LabourB.1[[#This Row],[Vehicles]],VehicleList_tbl[Avrg])),\"\")","v":0},null,"Crane",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_Plant[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_Plant[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_Plant[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_Plant[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_Plant[[#This Row],[51+ k]]*100))*0.001104627086,\"\")","v":0}]
[null,null,"Bicycle",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_LabourB.1[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_LabourB.1[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_LabourB.1[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_LabourB.1[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_LabourB.1[[#This Row],[51+ k]]*100))*(SUMIF(VehicleList_tbl[Vehicle],Form_Const_Tran_LabourB.1[[#This Row],[Vehicles]],VehicleList_tbl[Avrg])),\"\")","v":0},null,"Excavators",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_Plant[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_Plant[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_Plant[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_Plant[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_Plant[[#This Row],[51+ k]]*100))*0.001104627086,\"\")","v":0}]
[null,null,"Walking",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_LabourB.1[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_LabourB.1[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_LabourB.1[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_LabourB.1[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_LabourB.1[[#This Row],[51+ k]]*100))*(SUMIF(VehicleList_tbl[Vehicle],Form_Const_Tran_LabourB.1[[#This Row],[Vehicles]],VehicleList_tbl[Avrg])),\"\")","v":0},null,"Piling Plant",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_Plant[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_Plant[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_Plant[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_Plant[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_Plant[[#This Row],[51+ k]]*100))*0.001104627086,\"\")","v":0}]
[null,null,"Van",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_LabourB.1[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_LabourB.1[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_LabourB.1[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_LabourB.1[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_LabourB.1[[#This Row],[51+ k]]*100))*(SUMIF(VehicleList_tbl[Vehicle],Form_Const_Tran_LabourB.1[[#This Row],[Vehicles]],VehicleList_tbl[Avrg])),\"\")","v":0},null,"Rollers",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_Plant[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_Plant[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_Plant[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_Plant[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_Plant[[#This Row],[51+ k]]*100))*0.001104627086,\"\")","v":0}]
[null,null,"Rail",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_LabourB.1[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_LabourB.1[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_LabourB.1[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_LabourB.1[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_LabourB.1[[#This Row],[51+ k]]*100))*(SUMIF(VehicleList_tbl[Vehicle],Form_Const_Tran_LabourB.1[[#This Row],[Vehicles]],VehicleList_tbl[Avrg])),\"\")","v":0},null,"Dozers",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_Plant[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_Plant[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_Plant[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_Plant[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_Plant[[#This Row],[51+ k]]*100))*0.001104627086,\"\")","v":0}]
[null,null,"Bus",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_LabourB.1[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_LabourB.1[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_LabourB.1[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_LabourB.1[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_LabourB.1[[#This Row],[51+ k]]*100))*(SUMIF(VehicleList_tbl[Vehicle],Form_Const_Tran_LabourB.1[[#This Row],[Vehicles]],VehicleList_tbl[Avrg])),\"\")","v":0},null,"Dumpers",null,null,null,null,null,{"$f":"IFERROR(((Form_Const_Tran_Plant[[#This Row],[1-5 km]]*3)+(Form_Const_Tran_Plant[[#This Row],[6-10 km]]*8)+(Form_Const_Tran_Plant[[#This Row],[11-20 km]]*15.5)+(Form_Const_Tran_Plant[[#This Row],[21-50 km]]*35.5)+(Form_Const_Tran_Plant[[#This Row],[51+ k]]*100))*0.001104627086,\"\")","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_Const_Tran_LabourB.1[CO2e (t)])","v":1.0170376666666667},null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_Const_Tran_Plant[CO2e (t)])","v":0}]
[]
[null,null,"Installation",null,{"$f":"SUM(Form_Elements[Capital - Installation])","v":11.541410356100858}]
[null,null,"Method Used:","Summary"]
[null,null,"Summary"]
[null,null,"Site Establishment",null,null,"Plant use"]
[]
[]
[null,null,"Size of Project","CO2e (t)",null,"Plant fuel","Measure (Litres)","CO2e (t)"]
[null,null,{"$f":"IF((INT(Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7)<24,\"Small (Less than 6 months)\",\nIF((INT(Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7)>72,\"Large (18 months+)\",\nIF(OR((INT(Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7)>=24,(INT(Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7)<72),\"Medium (6 - 18 months)\",\"\")))","v":"Small (Less than 6 months)"},{"$f":"IFERROR(IF(Form_Mod_2[Construction start date]=\"\",0,(INT(Form_Mod_2[Construction finish date]-Form_Mod_2[Construction start date])/7)*(SUMIF(ValList_FuelType_OnSiteOverheads[Size of project],Form_Const_Ins_OnsiteA[Size of Project],ValList_FuelType_OnSiteOverheads[t CO2e per week]))+SUMIF(ValList_FuelType_OnSiteOverheads[Size of project],Form_Const_Ins_OnsiteA[Size of Project],ValList_FuelType_OnSiteOverheads[t CO2e Cabin Setup])),0)","v":11.288744736},null,"Petrol",null,{"$f":"IFERROR(Form_Const_Ins_InsA69[[#This Row],[Measure (Litres)]]*(SUMIF(PlantFuel_tbl[Fuel],Form_Const_Ins_InsA69[[#This Row],[Plant fuel]],PlantFuel_tbl[t CO2e/litre])),\"\")","v":0}]
[null,null,null,null,null,"Biodiesel [Standard]",null,{"$f":"IFERROR(Form_Const_Ins_InsA69[[#This Row],[Measure (Litres)]]*(SUMIF(PlantFuel_tbl[Fuel],Form_Const_Ins_InsA69[[#This Row],[Plant fuel]],PlantFuel_tbl[t CO2e/litre])),\"\")","v":0}]
[null,null,null,null,null,"Diesel [Red]",null,{"$f":"IFERROR(Form_Const_Ins_InsA69[[#This Row],[Measure (Litres)]]*(SUMIF(PlantFuel_tbl[Fuel],Form_Const_Ins_InsA69[[#This Row],[Plant fuel]],PlantFuel_tbl[t CO2e/litre])),\"\")","v":0}]
[null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_Const_Ins_InsA69[CO2e (t)])","v":0}]
[]
[null,null,"Detailed"]
[null,null,"Site Establishment"]
[]
[null,null,"Fuel Type","Unit","Consumption","CO2e (t)"]
[null,null,"Electricity ",{"$f":"IFERROR(VLOOKUP(Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[[Fuel Type: On Site Accomodation ]:[Unit]],2,FALSE),\"\")","v":"kWh"},null,{"$f":"Form_Const_Ins_OnsiteB[[#This Row],[Consumption]]*(SUMIF(OnSiteAccom_FuelType_TBL[Fuel Type: On Site Accomodation ],Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[Total t CO2e/unit]))","v":0}]
[null,null,"Natural Gas",{"$f":"IFERROR(VLOOKUP(Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[[Fuel Type: On Site Accomodation ]:[Unit]],2,FALSE),\"\")","v":"m3"},null,{"$f":"Form_Const_Ins_OnsiteB[[#This Row],[Consumption]]*(SUMIF(OnSiteAccom_FuelType_TBL[Fuel Type: On Site Accomodation ],Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[Total t CO2e/unit]))","v":0}]
[null,null,"Gas Oil [Red Diesel]",{"$f":"IFERROR(VLOOKUP(Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[[Fuel Type: On Site Accomodation ]:[Unit]],2,FALSE),\"\")","v":"litres"},null,{"$f":"Form_Const_Ins_OnsiteB[[#This Row],[Consumption]]*(SUMIF(OnSiteAccom_FuelType_TBL[Fuel Type: On Site Accomodation ],Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[Total t CO2e/unit]))","v":0}]
[null,null,"Petrol",{"$f":"IFERROR(VLOOKUP(Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[[Fuel Type: On Site Accomodation ]:[Unit]],2,FALSE),\"\")","v":"litres"},null,{"$f":"Form_Const_Ins_OnsiteB[[#This Row],[Consumption]]*(SUMIF(OnSiteAccom_FuelType_TBL[Fuel Type: On Site Accomodation ],Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[Total t CO2e/unit]))","v":0}]
[null,null,"Diesel",{"$f":"IFERROR(VLOOKUP(Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[[Fuel Type: On Site Accomodation ]:[Unit]],2,FALSE),\"\")","v":"litres"},null,{"$f":"Form_Const_Ins_OnsiteB[[#This Row],[Consumption]]*(SUMIF(OnSiteAccom_FuelType_TBL[Fuel Type: On Site Accomodation ],Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[Total t CO2e/unit]))","v":0}]
[null,null,"Water",{"$f":"IFERROR(VLOOKUP(Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[[Fuel Type: On Site Accomodation ]:[Unit]],2,FALSE),\"\")","v":"litres"},null,{"$f":"Form_Const_Ins_OnsiteB[[#This Row],[Consumption]]*(SUMIF(OnSiteAccom_FuelType_TBL[Fuel Type: On Site Accomodation ],Form_Const_Ins_OnsiteB[[#This Row],[Fuel Type]],OnSiteAccom_FuelType_TBL[Total t CO2e/unit]))","v":0}]
[null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_Const_Ins_OnsiteB[CO2e (t)])","v":0}]
[]
[null,null,"Plant use"]
[]
[]
[null,null,"Sub-Asset Ref.","Sub-Asset description","Plant","Plant type","Activity","Hours on site","Fuel type","Utlilisation ","Utilisation (Manual Input)","Consumption l/hr","Total ltrs of fuel used","CO2e (t)"]
[null,null,{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":""},null,null,null,null,null,null,{"$f":"INDEX(PlantDetailTbl[Utilization Factor],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0))","v":0},null,{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]*INDEX(PlantDetailTbl[Consumption of fuel (l/hr)],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0)),\"\")","v":0},{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]]>0,(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]],(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]),\"\")","v":0},{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Total ltrs of fuel used]]*SUMIF(PlantFuel_tbl[Fuel],Form_Const_Ins_InsB[[#This Row],[Fuel type]],PlantFuel_tbl[t CO2e/litre]),\"\")","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":""},null,null,null,null,null,null,{"$f":"INDEX(PlantDetailTbl[Utilization Factor],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0))","v":0},null,{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]*INDEX(PlantDetailTbl[Consumption of fuel (l/hr)],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0)),\"\")","v":0},{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]]>0,(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]],(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]),\"\")","v":0},{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Total ltrs of fuel used]]*SUMIF(PlantFuel_tbl[Fuel],Form_Const_Ins_InsB[[#This Row],[Fuel type]],PlantFuel_tbl[t CO2e/litre]),\"\")","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":""},null,null,null,null,null,null,{"$f":"INDEX(PlantDetailTbl[Utilization Factor],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0))","v":0},null,{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]*INDEX(PlantDetailTbl[Consumption of fuel (l/hr)],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0)),\"\")","v":0},{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]]>0,(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]],(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]),\"\")","v":0},{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Total ltrs of fuel used]]*SUMIF(PlantFuel_tbl[Fuel],Form_Const_Ins_InsB[[#This Row],[Fuel type]],PlantFuel_tbl[t CO2e/litre]),\"\")","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":""},null,null,null,null,null,null,{"$f":"INDEX(PlantDetailTbl[Utilization Factor],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0))","v":0},null,{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]*INDEX(PlantDetailTbl[Consumption of fuel (l/hr)],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0)),\"\")","v":0},{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]]>0,(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]],(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]),\"\")","v":0},{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Total ltrs of fuel used]]*SUMIF(PlantFuel_tbl[Fuel],Form_Const_Ins_InsB[[#This Row],[Fuel type]],PlantFuel_tbl[t CO2e/litre]),\"\")","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]]=\"General Item\",\"GenEA1\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_Const_Ins_InsB[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0))))),\"\")","v":""},null,null,null,null,null,null,{"$f":"INDEX(PlantDetailTbl[Utilization Factor],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0))","v":0},null,{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]*INDEX(PlantDetailTbl[Consumption of fuel (l/hr)],MATCH(1,(Form_Const_Ins_InsB[[#This Row],[Plant]]=PlantDetailTbl[Plant])*(Form_Const_Ins_InsB[[#This Row],[Plant type]]=PlantDetailTbl[Plant Item]),0)),\"\")","v":0},{"$f":"IFERROR(IF(Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]]>0,(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utilisation (Manual Input)]],(Form_Const_Ins_InsB[[#This Row],[Hours on site]]*Form_Const_Ins_InsB[[#This Row],[Consumption l/hr]])*Form_Const_Ins_InsB[[#This Row],[Utlilisation ]]),\"\")","v":0},{"$f":"IFERROR(Form_Const_Ins_InsB[[#This Row],[Total ltrs of fuel used]]*SUMIF(PlantFuel_tbl[Fuel],Form_Const_Ins_InsB[[#This Row],[Fuel type]],PlantFuel_tbl[t CO2e/litre]),\"\")","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_Const_Ins_InsB[CO2e (t)])","v":0}]
[]
[null,null,"Materials waste",null,null,null,"Other construction waste"]
[]
[]
[]
[null,null,"Reused / Recycle / Removed","Distance Travelled","CO2e (t)",null,"Material","Quantity (t)","Reused / Recycle / Removed","Distance to waste disposal","Distance","CO2e (t)"]
[null,null,"Reused",{"$f":"SUMIF(Form_Product_Stage[Reused / Recycle / Removed],Form_Const_Ins_VirgWaste70[[#This Row],[Reused / Recycle / Removed]],Form_Product_Stage[Waste distance])","v":25},{"$f":"SUMIF(Form_Product_Stage[Reused / Recycle / Removed],Form_Const_Ins_VirgWaste70[[#This Row],[Reused / Recycle / Removed]],Form_Product_Stage[[Waste Co2e ]])","v":0},null,null,null,null,null,{"$f":"IFERROR(IF(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR((IF(Form_Const_Ins_ConsWaste[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,((Form_Const_Ins_ConsWaste[[#This Row],[Quantity (t)]]/8)*0.001377905226)*Form_Const_Ins_ConsWaste[[#This Row],[Distance]])),\"\")","v":""}]
[null,null,"Recycle",{"$f":"SUMIF(Form_Product_Stage[Reused / Recycle / Removed],Form_Const_Ins_VirgWaste70[[#This Row],[Reused / Recycle / Removed]],Form_Product_Stage[Waste distance])","v":75},{"$f":"SUMIF(Form_Product_Stage[Reused / Recycle / Removed],Form_Const_Ins_VirgWaste70[[#This Row],[Reused / Recycle / Removed]],Form_Product_Stage[[Waste Co2e ]])","v":0.15164277607513124},null,null,null,null,null,{"$f":"IFERROR(IF(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR((IF(Form_Const_Ins_ConsWaste[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,((Form_Const_Ins_ConsWaste[[#This Row],[Quantity (t)]]/8)*0.001377905226)*Form_Const_Ins_ConsWaste[[#This Row],[Distance]])),\"\")","v":""}]
[null,null,"Removed",{"$f":"SUMIF(Form_Product_Stage[Reused / Recycle / Removed],Form_Const_Ins_VirgWaste70[[#This Row],[Reused / Recycle / Removed]],Form_Product_Stage[Waste distance])","v":50},{"$f":"SUMIF(Form_Product_Stage[Reused / Recycle / Removed],Form_Const_Ins_VirgWaste70[[#This Row],[Reused / Recycle / Removed]],Form_Product_Stage[[Waste Co2e ]])","v":0.10102284402572248},null,null,null,null,null,{"$f":"IFERROR(IF(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR((IF(Form_Const_Ins_ConsWaste[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,((Form_Const_Ins_ConsWaste[[#This Row],[Quantity (t)]]/8)*0.001377905226)*Form_Const_Ins_ConsWaste[[#This Row],[Distance]])),\"\")","v":""}]
[null,null,null,null,{"$f":"SUBTOTAL(109,Form_Const_Ins_VirgWaste70[CO2e (t)])","v":0.25266562010085369},null,null,null,null,null,{"$f":"IFERROR(IF(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR((IF(Form_Const_Ins_ConsWaste[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,((Form_Const_Ins_ConsWaste[[#This Row],[Quantity (t)]]/8)*0.001377905226)*Form_Const_Ins_ConsWaste[[#This Row],[Distance]])),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR((IF(Form_Const_Ins_ConsWaste[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,((Form_Const_Ins_ConsWaste[[#This Row],[Quantity (t)]]/8)*0.001377905226)*Form_Const_Ins_ConsWaste[[#This Row],[Distance]])),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR((IF(Form_Const_Ins_ConsWaste[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,((Form_Const_Ins_ConsWaste[[#This Row],[Quantity (t)]]/8)*0.001377905226)*Form_Const_Ins_ConsWaste[[#This Row],[Distance]])),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]]=\"\",\"\",VLOOKUP(Form_Const_Ins_ConsWaste[[#This Row],[Distance to waste disposal]],SupplierDistance[],2,FALSE)),\"\")","v":""},{"$f":"IFERROR((IF(Form_Const_Ins_ConsWaste[[#This Row],[Reused / Recycle / Removed]]=\"Reused\",0,((Form_Const_Ins_ConsWaste[[#This Row],[Quantity (t)]]/8)*0.001377905226)*Form_Const_Ins_ConsWaste[[#This Row],[Distance]])),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_Const_Ins_ConsWaste[CO2e (t)])","v":0}]
[]
[]
[null,null,"Lifecycle carbon",null,{"$f":"SUM(E139,E190,E195,E197,E202)","v":8598.9464851839293}]
[]
[null,null,"Operational carbon",null,{"$f":"SUM(E140,E153,E166,E176)","v":8106.0783515732601}]
[null,null,"Use",null,{"$f":"SUM(Form_Elements[Operational - Use])","v":3.5292202163767392}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a","a","a"]
[]
[null,null,"Asset Ref.","Asset Description","Use description","Mode of transport","Fuel type","No. of people traveling by","No. of days manned per year","Return distance to manned asset (km)","CO2e (t)"]
[null,null,{"$f":"IFERROR(IF(Form_use_use[[#This Row],[Asset Description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_use_use[[#This Row],[Asset Description]],Form_Elements[Asset description],0))),\"\")","v":"BridEA03"},"Footbridge","People access","Car","Petrol",2,5,50,{"$f":"IF(Form_use_use[[#This Row],[Mode of transport]]=\"\",0,(((Form_use_use[[#This Row],[Return distance to manned asset (km)]]*Form_use_use[[#This Row],[No. of days manned per year]]))*(SUMIFS(PersonalVehicle_tbl[Total t CO2e/litre],PersonalVehicle_tbl[Vehicle],Form_use_use[[#This Row],[Mode of transport]],PersonalVehicle_tbl[Fuel],Form_use_use[[#This Row],[Fuel type]])*Form_use_use[[#This Row],[No. of people traveling by]])))","v":0.11245000000000001}]
[null,null,{"$f":"IFERROR(IF(Form_use_use[[#This Row],[Asset Description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_use_use[[#This Row],[Asset Description]],Form_Elements[Asset description],0))),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(Form_use_use[[#This Row],[Mode of transport]]=\"\",0,(((Form_use_use[[#This Row],[Return distance to manned asset (km)]]*Form_use_use[[#This Row],[No. of days manned per year]]))*(SUMIFS(PersonalVehicle_tbl[Total t CO2e/litre],PersonalVehicle_tbl[Vehicle],Form_use_use[[#This Row],[Mode of transport]],PersonalVehicle_tbl[Fuel],Form_use_use[[#This Row],[Fuel type]])*Form_use_use[[#This Row],[No. of people traveling by]])))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_use[[#This Row],[Asset Description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_use_use[[#This Row],[Asset Description]],Form_Elements[Asset description],0))),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(Form_use_use[[#This Row],[Mode of transport]]=\"\",0,(((Form_use_use[[#This Row],[Return distance to manned asset (km)]]*Form_use_use[[#This Row],[No. of days manned per year]]))*(SUMIFS(PersonalVehicle_tbl[Total t CO2e/litre],PersonalVehicle_tbl[Vehicle],Form_use_use[[#This Row],[Mode of transport]],PersonalVehicle_tbl[Fuel],Form_use_use[[#This Row],[Fuel type]])*Form_use_use[[#This Row],[No. of people traveling by]])))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_use[[#This Row],[Asset Description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_use_use[[#This Row],[Asset Description]],Form_Elements[Asset description],0))),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(Form_use_use[[#This Row],[Mode of transport]]=\"\",0,(((Form_use_use[[#This Row],[Return distance to manned asset (km)]]*Form_use_use[[#This Row],[No. of days manned per year]]))*(SUMIFS(PersonalVehicle_tbl[Total t CO2e/litre],PersonalVehicle_tbl[Vehicle],Form_use_use[[#This Row],[Mode of transport]],PersonalVehicle_tbl[Fuel],Form_use_use[[#This Row],[Fuel type]])*Form_use_use[[#This Row],[No. of people traveling by]])))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_use[[#This Row],[Asset Description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_use_use[[#This Row],[Asset Description]],Form_Elements[Asset description],0))),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(Form_use_use[[#This Row],[Mode of transport]]=\"\",0,(((Form_use_use[[#This Row],[Return distance to manned asset (km)]]*Form_use_use[[#This Row],[No. of days manned per year]]))*(SUMIFS(PersonalVehicle_tbl[Total t CO2e/litre],PersonalVehicle_tbl[Vehicle],Form_use_use[[#This Row],[Mode of transport]],PersonalVehicle_tbl[Fuel],Form_use_use[[#This Row],[Fuel type]])*Form_use_use[[#This Row],[No. of people traveling by]])))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_use[[#This Row],[Asset Description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_use_use[[#This Row],[Asset Description]],Form_Elements[Asset description],0))),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(Form_use_use[[#This Row],[Mode of transport]]=\"\",0,(((Form_use_use[[#This Row],[Return distance to manned asset (km)]]*Form_use_use[[#This Row],[No. of days manned per year]]))*(SUMIFS(PersonalVehicle_tbl[Total t CO2e/litre],PersonalVehicle_tbl[Vehicle],Form_use_use[[#This Row],[Mode of transport]],PersonalVehicle_tbl[Fuel],Form_use_use[[#This Row],[Fuel type]])*Form_use_use[[#This Row],[No. of people traveling by]])))","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_use[[#This Row],[Asset Description]]=\"\",\"\",INDEX(Form_Elements[Asset ID],MATCH(Form_use_use[[#This Row],[Asset Description]],Form_Elements[Asset description],0))),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(Form_use_use[[#This Row],[Mode of transport]]=\"\",0,(((Form_use_use[[#This Row],[Return distance to manned asset (km)]]*Form_use_use[[#This Row],[No. of days manned per year]]))*(SUMIFS(PersonalVehicle_tbl[Total t CO2e/litre],PersonalVehicle_tbl[Vehicle],Form_use_use[[#This Row],[Mode of transport]],PersonalVehicle_tbl[Fuel],Form_use_use[[#This Row],[Fuel type]])*Form_use_use[[#This Row],[No. of people traveling by]])))","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_use_use[CO2e (t)])","v":0.11245000000000001}]
[]
[null,null,"Maintenance",null,{"$f":"SUM(Form_Elements[Operational - Maintenance])","v":6732.681317044955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100]
[null,null,"Sub-Asset Ref.","Sub-Asset description","Maintenance category","Maintenance description","Mode of transport","Return transport distance (km)","Materials","Plant","Waste","Overhead","Annual intervention fequency","Interventions per year","Exceptional intervention year","CO2e (t) per intervention","Material"," Plant","Transport","blank5","blank6","blank7","blank8","blank9","blank10","blank11","0","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24","25","26","27","28","29","30","31","32","33","34","35","36","37","38","39","40","41","42","43","44","45","46","47","48","49","50","51","52","53","54","55","56","57","58","59","60","61","62","63","64","65","66","67","68","69","70","71","72","73","74","75","76","77","78","79","80","81","82","83","84","85","86","87","88","89","90","91","92","93","94","95","96","97","98","99","100"]
[null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_Maintenance[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":"BridEA0333"},"Desk","Minimum Need","Safety Inspection","Van",50,"Low","Low",{"$f":"\"Not used\"","v":"Not used"},{"$f":"\"Not used\"","v":"Not used"},"Every year",null,null,{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_Maintenance[[#This Row],[Material]:[Transport]]))","v":88.366127158000012},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[[#This Row],[Materials]],MaintRepLMH[Value]))","v":88.350840000000005},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[Plant],MaintRepLMH[Value]))","v":0},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_Maintenance[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_Maintenance[[#This Row],[Return transport distance (km)]])","v":1.5287157999999999E-2},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.366127158000012}]
[null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_Maintenance[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":"BridEA0334"},"Abutment","Minimum Need","Special inspection","Van",50,"Medium","Low","Not used","Not used","Every year",null,null,{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_Maintenance[[#This Row],[Material]:[Transport]]))","v":27.244391157999996},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[[#This Row],[Materials]],MaintRepLMH[Value]))","v":27.229103999999996},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[Plant],MaintRepLMH[Value]))","v":0},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_Maintenance[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_Maintenance[[#This Row],[Return transport distance (km)]])","v":1.5287157999999999E-2},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":27.244391157999996}]
[null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_Maintenance[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":"BridEA0335"},"Handrail","Minimum Need","Visual inspection","Van",50,"Low","Low","Not used","Not used","Every year",null,null,{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_Maintenance[[#This Row],[Material]:[Transport]]))","v":88.575287158000009},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[[#This Row],[Materials]],MaintRepLMH[Value]))","v":88.56},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[Plant],MaintRepLMH[Value]))","v":0},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_Maintenance[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_Maintenance[[#This Row],[Return transport distance (km)]])","v":1.5287157999999999E-2},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009}]
[null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_Maintenance[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":"BridEA0336"},"Concrete wingwall","Identified Need","Special inspection","Van",50,"Medium","Low","Not used","Not used","Every year",null,null,{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_Maintenance[[#This Row],[Material]:[Transport]]))","v":10.011287157999998},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[[#This Row],[Materials]],MaintRepLMH[Value]))","v":9.9959999999999987},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[Plant],MaintRepLMH[Value]))","v":0},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_Maintenance[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_Maintenance[[#This Row],[Return transport distance (km)]])","v":1.5287157999999999E-2},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":10.011287157999998}]
[null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_Maintenance[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":"BridEA0337"},"Erosion protection","Identified Need","Vegetation maintenance","Van",50,"Low","Low",{"$f":"\"Not used\"","v":"Not used"},"Not used","Every year",null,null,{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_Maintenance[[#This Row],[Material]:[Transport]]))","v":0.32338715800000006},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[[#This Row],[Materials]],MaintRepLMH[Value]))","v":0.30810000000000004},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[Plant],MaintRepLMH[Value]))","v":0},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_Maintenance[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_Maintenance[[#This Row],[Return transport distance (km)]])","v":1.5287157999999999E-2},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0.32338715800000006}]
[null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_Maintenance[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,null,null,"Not used","Not used",null,null,null,{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_Maintenance[[#This Row],[Material]:[Transport]]))","v":0},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[[#This Row],[Materials]],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[Plant],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_Maintenance[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_Maintenance[[#This Row],[Return transport distance (km)]])","v":""},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_Maintenance[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,null,null,"Not used","Not used",null,null,null,{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_Maintenance[[#This Row],[Material]:[Transport]]))","v":0},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[[#This Row],[Materials]],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_Maintenance[Plant],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_Maintenance[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_Maintenance[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_Maintenance[[#This Row],[Return transport distance (km)]])","v":""},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$155=Form_use_Maintenance[[#This Row],[Exceptional intervention year]],Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_Maintenance[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_Maintenance[[#This Row],[Interventions per year]]*Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$155,VLOOKUP(Form_use_Maintenance[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_Maintenance[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_use_Maintenance[CO2e (t) per intervention])","v":214.52047979}]
[]
[null,null,"Repair",null,{"$f":"SUM(Form_Elements[Operational -Repair])","v":1369.8678143119284}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a",null,null,null,null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100]
[null,null,"Sub-Asset Ref.","Sub-Asset description","Repair category","Repair description","Mode of transport","Return transport distance (km)","Materials","Plant","Waste","Overhead","Annual intervention fequency","Interventions per year","Exceptional intervention year","CO2e (t) per intervention","Material"," Plant","Transport","blank5","blank6","blank7","blank8","blank9","blank92","blank10","0","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24","25","26","27","28","29","30","31","32","33","34","35","36","37","38","39","40","41","42","43","44","45","46","47","48","49","50","51","52","53","54","55","56","57","58","59","60","61","62","63","64","65","66","67","68","69","70","71","72","73","74","75","76","77","78","79","80","81","82","83","84","85","86","87","88","89","90","91","92","93","94","95","96","97","98","99","100"]
[null,null,{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_repair[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":"BridEA0335"},"Handrail","Not used","Damaged","Van",50,"Low","Low",{"$f":"\"Not used\"","v":"Not used"},{"$f":"\"Not used\"","v":"Not used"},"Every 2 years",null,null,{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_repair[[#This Row],[Material]:[Transport]]))","v":88.575287158000009},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_repair[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_repair[[#This Row],[Materials]],MaintRepLMH[Value]))","v":88.56},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_repair[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_repair[Plant],MaintRepLMH[Value]))","v":0},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_repair[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_repair[[#This Row],[Return transport distance (km)]])","v":1.5287157999999999E-2},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":88.575287158000009}]
[null,null,{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_repair[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,"Not used",null,null,null,null,null,"Not used","Not used",null,null,null,{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_repair[[#This Row],[Material]:[Transport]]))","v":0},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_repair[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_repair[[#This Row],[Materials]],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_repair[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_repair[Plant],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_repair[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_repair[[#This Row],[Return transport distance (km)]])","v":""},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_repair[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,"Not used",null,null,null,null,null,"Not used","Not used",null,null,null,{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_repair[[#This Row],[Material]:[Transport]]))","v":0},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_repair[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_repair[[#This Row],[Materials]],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_repair[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_repair[Plant],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_repair[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_repair[[#This Row],[Return transport distance (km)]])","v":""},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_repair[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,"Not used",null,null,null,null,null,"Not used","Not used",null,null,null,{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",0,SUM(Form_use_repair[[#This Row],[Material]:[Transport]]))","v":0},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_repair[[#This Row],[Sub-Asset Ref.]],Form_Asset[Materials])*SUMIF(MaintRepLMH[M/R Level],Form_use_repair[[#This Row],[Materials]],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(Form_Asset[Sub-Asset ref.],Form_use_repair[[#This Row],[Sub-Asset Ref.]],Form_Asset[Plant use])*SUMIF(MaintRepLMH[M/R Level],Form_use_repair[Plant],MaintRepLMH[Value]))","v":""},{"$f":"IF(Form_use_repair[[#This Row],[Sub-Asset Ref.]]=\"\",\"\",SUMIF(PlantDistance[Mode],Form_use_repair[[#This Row],[Mode of transport]],PlantDistance[Total t CO2e])*Form_use_repair[[#This Row],[Return transport distance (km)]])","v":""},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!AZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!AZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!BZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!BZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CX$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CX$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CY$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CY$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!CZ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!CZ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DA$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DA$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DB$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DB$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DC$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DC$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DD$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DD$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DE$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DE$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DF$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DF$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DG$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DG$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DH$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DH$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DI$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DI$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DJ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DJ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DK$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DK$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DL$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DL$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DM$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DM$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DN$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DN$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DO$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DO$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DP$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DP$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DQ$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DQ$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DR$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DR$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DS$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DS$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DT$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DT$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DU$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DU$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DV$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DV$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0},{"$f":"IFERROR(IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"Exceptional\",IF(Calculator!DW$168=Form_use_repair[[#This Row],[Exceptional intervention year]],Form_use_repair[[#This Row],[CO2e (t) per intervention]],0),IF(Form_use_repair[[#This Row],[Annual intervention fequency]]=\"> 1 per year\",Form_use_repair[[#This Row],[Interventions per year]]*Form_use_repair[[#This Row],[CO2e (t) per intervention]],IF(MOD(Calculator!DW$168,VLOOKUP(Form_use_repair[[#This Row],[Annual intervention fequency]],AnnualInterventionFrequency[],2,0))=0,Form_use_repair[[#This Row],[CO2e (t) per intervention]],0))),0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_use_repair[CO2e (t) per intervention])","v":88.575287158000009}]
[]
[null,null,"Energy",null,{"$f":"SUM(Form_Elements[Operational - Energy])","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a","a","a"]
[]
[null,null,"Sub-Asset Ref.","Sub-Asset description","Name plate (kW)","Overall efficiency rating (%)","Load rating (%)","Use factor (%)","Power absorbed (KW)","Hours / Year","Annual power consumed (kW)","CO2e (t)"]
[null,null,{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_energy[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(AND(Form_use_energy[[#This Row],[Name plate (kW)]]>0,Form_use_energy[[#This Row],[Overall efficiency rating (%)]]>0),(Form_use_energy[[#This Row],[Name plate (kW)]]/Form_use_energy[[#This Row],[Overall efficiency rating (%)]])*Form_use_energy[[#This Row],[Load rating (%)]]*Form_use_energy[[#This Row],[Use factor (%)]],0))","v":""},{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",ValList_OP_EnergyHoursperYear[Use Energy Hours per year])","v":""},{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Power absorbed (KW)]]>0,Form_use_energy[[#This Row],[Power absorbed (KW)]]*Form_use_energy[[#This Row],[Hours / Year]],\"\"),\"\")","v":""},{"$f":"IFERROR(Form_use_energy[[#This Row],[Annual power consumed (kW)]]*UseEnergyCo2e[Electicity (kW)  t CO2e],0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_energy[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(AND(Form_use_energy[[#This Row],[Name plate (kW)]]>0,Form_use_energy[[#This Row],[Overall efficiency rating (%)]]>0),(Form_use_energy[[#This Row],[Name plate (kW)]]/Form_use_energy[[#This Row],[Overall efficiency rating (%)]])*Form_use_energy[[#This Row],[Load rating (%)]]*Form_use_energy[[#This Row],[Use factor (%)]],0))","v":""},{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",ValList_OP_EnergyHoursperYear[Use Energy Hours per year])","v":""},{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Power absorbed (KW)]]>0,Form_use_energy[[#This Row],[Power absorbed (KW)]]*Form_use_energy[[#This Row],[Hours / Year]],\"\"),\"\")","v":""},{"$f":"IFERROR(Form_use_energy[[#This Row],[Annual power consumed (kW)]]*UseEnergyCo2e[Electicity (kW)  t CO2e],0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_energy[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(AND(Form_use_energy[[#This Row],[Name plate (kW)]]>0,Form_use_energy[[#This Row],[Overall efficiency rating (%)]]>0),(Form_use_energy[[#This Row],[Name plate (kW)]]/Form_use_energy[[#This Row],[Overall efficiency rating (%)]])*Form_use_energy[[#This Row],[Load rating (%)]]*Form_use_energy[[#This Row],[Use factor (%)]],0))","v":""},{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",ValList_OP_EnergyHoursperYear[Use Energy Hours per year])","v":""},{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Power absorbed (KW)]]>0,Form_use_energy[[#This Row],[Power absorbed (KW)]]*Form_use_energy[[#This Row],[Hours / Year]],\"\"),\"\")","v":""},{"$f":"IFERROR(Form_use_energy[[#This Row],[Annual power consumed (kW)]]*UseEnergyCo2e[Electicity (kW)  t CO2e],0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_energy[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(AND(Form_use_energy[[#This Row],[Name plate (kW)]]>0,Form_use_energy[[#This Row],[Overall efficiency rating (%)]]>0),(Form_use_energy[[#This Row],[Name plate (kW)]]/Form_use_energy[[#This Row],[Overall efficiency rating (%)]])*Form_use_energy[[#This Row],[Load rating (%)]]*Form_use_energy[[#This Row],[Use factor (%)]],0))","v":""},{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",ValList_OP_EnergyHoursperYear[Use Energy Hours per year])","v":""},{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Power absorbed (KW)]]>0,Form_use_energy[[#This Row],[Power absorbed (KW)]]*Form_use_energy[[#This Row],[Hours / Year]],\"\"),\"\")","v":""},{"$f":"IFERROR(Form_use_energy[[#This Row],[Annual power consumed (kW)]]*UseEnergyCo2e[Electicity (kW)  t CO2e],0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_energy[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(AND(Form_use_energy[[#This Row],[Name plate (kW)]]>0,Form_use_energy[[#This Row],[Overall efficiency rating (%)]]>0),(Form_use_energy[[#This Row],[Name plate (kW)]]/Form_use_energy[[#This Row],[Overall efficiency rating (%)]])*Form_use_energy[[#This Row],[Load rating (%)]]*Form_use_energy[[#This Row],[Use factor (%)]],0))","v":""},{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",ValList_OP_EnergyHoursperYear[Use Energy Hours per year])","v":""},{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Power absorbed (KW)]]>0,Form_use_energy[[#This Row],[Power absorbed (KW)]]*Form_use_energy[[#This Row],[Hours / Year]],\"\"),\"\")","v":""},{"$f":"IFERROR(Form_use_energy[[#This Row],[Annual power consumed (kW)]]*UseEnergyCo2e[Electicity (kW)  t CO2e],0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_energy[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(AND(Form_use_energy[[#This Row],[Name plate (kW)]]>0,Form_use_energy[[#This Row],[Overall efficiency rating (%)]]>0),(Form_use_energy[[#This Row],[Name plate (kW)]]/Form_use_energy[[#This Row],[Overall efficiency rating (%)]])*Form_use_energy[[#This Row],[Load rating (%)]]*Form_use_energy[[#This Row],[Use factor (%)]],0))","v":""},{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",ValList_OP_EnergyHoursperYear[Use Energy Hours per year])","v":""},{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Power absorbed (KW)]]>0,Form_use_energy[[#This Row],[Power absorbed (KW)]]*Form_use_energy[[#This Row],[Hours / Year]],\"\"),\"\")","v":""},{"$f":"IFERROR(Form_use_energy[[#This Row],[Annual power consumed (kW)]]*UseEnergyCo2e[Electicity (kW)  t CO2e],0)","v":0}]
[null,null,{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",INDEX(Form_Asset[Sub-Asset ref.],(MATCH(Form_use_energy[[#This Row],[Sub-Asset description]],Form_Asset[Sub-Asset description],0)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",IF(AND(Form_use_energy[[#This Row],[Name plate (kW)]]>0,Form_use_energy[[#This Row],[Overall efficiency rating (%)]]>0),(Form_use_energy[[#This Row],[Name plate (kW)]]/Form_use_energy[[#This Row],[Overall efficiency rating (%)]])*Form_use_energy[[#This Row],[Load rating (%)]]*Form_use_energy[[#This Row],[Use factor (%)]],0))","v":""},{"$f":"IF(Form_use_energy[[#This Row],[Sub-Asset description]]=\"\",\"\",ValList_OP_EnergyHoursperYear[Use Energy Hours per year])","v":""},{"$f":"IFERROR(IF(Form_use_energy[[#This Row],[Power absorbed (KW)]]>0,Form_use_energy[[#This Row],[Power absorbed (KW)]]*Form_use_energy[[#This Row],[Hours / Year]],\"\"),\"\")","v":""},{"$f":"IFERROR(Form_use_energy[[#This Row],[Annual power consumed (kW)]]*UseEnergyCo2e[Electicity (kW)  t CO2e],0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(109,Form_use_energy[CO2e (t)])","v":0}]
[]
[]
[null,null,"Replacement carbon",null,{"$f":"SUM(E191,E192,E193)","v":722.43695498945851}]
[null,null,"Materials",null,{"$f":"SUM(Form_Elements[Replacement - Materials])","v":713.0893246782565}]
[null,null,"Transport",null,{"$f":"SUM(Form_Elements[Replacement - Transport])","v":4.8106945515317321}]
[null,null,"Installation",null,{"$f":"SUM(Form_Elements[Replacement - Installation])","v":4.5369357596703406}]
[]
[null,null,"Refurbishment carbon",null,{"$f":"SUM(Form_Elements[Refurbishment])","v":231.23957849294123}]
[]
[null,null,"Demolition carbon",null,{"$f":"SUM(E198,E199,E200)","v":3.6201670655063309}]
[null,null,"Material waste",null,{"$f":"SUM(FlatData!$AV$1:$AV$4800)","v":1.5894975176412192}]
[null,null,"Plant",null,{"$f":"SUM(FlatData!$AW$1:$AW$4800)","v":5.2239955921811312E-2}]
[null,null,"People",null,{"$f":"SUM(FlatData!$AX$1:$AX$4800)","v":1.9784295919433004}]
[]
[null,null,"Residual carbon",null,{"$f":"SUM(Form_Elements[Residual])","v":-464.42856693723741}]

{"sheet":"Instructions","index":9,"n_rows":28,"n_cols":2,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[null,"General instructions"]
[]
[]
[]
[null,"Before starting, make sure that Macros are enabled in Microsoft Excel."]
[]
[null,"Only certain parts of the whole life carbon assessment require manual entry of information. The other parts are automatically generated by the calculator based on the information entered manually. This includes the summary information. The automatically generated information is only created when the manual entry parts are completed in full and the green button entitled 'Recalculate and create summary' is pressed. It is therefore important that the following steps are followed within the Calculator sheet in order to create an accurate whole life carbon assessment."]
[]
[null,"1) Complete the Project Details section. Complete this in full before proceeding as some of this information informs calculations in the sheet."]
[]
[null,"2) Complete the Assets section. This must contain all standard Environment Agency Assets that form part of the project. Do not enter 'general items' such as temporary works - such items are assessed within the calculator and are allocated to the Assets automatically."]
[]
[null,"3) Complete the Sub-Assets sections. This section allows Assets to be broken down into separate parts that each have different useful lives, enabling the whole life calculation to function. All Sub-Assets relating to each Asset must be entered. If an Asset does not need to be broken down into Sub-Assets, enter a single Sub-Asset item for that Asset."]
[]
[null,"4) Complete the Capital Carbon section. Use the instructions provided for each data entry field for support and refer to the Carbon Planning Tool User Guide for further information."]
[]
[null,"5) Complete the Operational Carbon section. Again, use the instructions provided for each data entry field for support and refer to the Carbon Planning Tool User Guide for further information."]
[]
[null,"6) Click the green 'Recalculate and create summary' button at the top-left of the Calculator sheet. Depending on how large your project is, the calculator will take a few seconds to process the information - please be patient. You will then be taken to the Summary sheet where you can analyse the whole life carbon for your project. At this point, all whole life carbon figures will be completed within the Calculator sheet as well."]
[]
[null,"7) You may subsequently amend the information entered in the Calculator sheet. Following any amendments, click the 'Recalculate and create summary' button to refresh the whole life carbon figures."]
[]
[null,"NB. If you are using Microsoft Excel 2003 or older, some functionality may not work and you should seek further guidance how to proceed."]

{"sheet":"Model","index":10,"n_rows":2,"n_cols":23,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Asset ID","Asset class","Asset description","Asset measure","Asset unit","Asset value","1B1S Project ref.","Version","Gateway","Capital - Materials","Capital - Transport","Capital - Installation","Operational - Use","Operational - Maintenance","Operational -Repair","Operational - Energy","Replacement - Materials","Replacement - Transport","Replacement - Installation","Refurbishment","Demolition","Residual","Whole Life Carbon"]
["CulvEA08","Other","Example Asset",0,"TBC",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"ValidationLists","index":11,"n_rows":113,"n_cols":14,"rows_kept":113,"cut":false,"hidden":true,"merged":[]}
[null,null,"Intervention",null,"Fuel Type: On Site Accomodation ","Unit","Total t CO2e/unit",null,"Fuel","Unit","t CO2e/litre",null,"Year","Disocunt Factor"]
[null,null,"New Build",null,"Electricity ","kWh",5.6952999999999995E-4,null,"Petrol","litre",2.1914E-3,null,0,1]
[null,null,"Replacement",null,"Natural Gas","m3",2.3077000000000002E-3,null,"Diesel [Red]","litre",2.669143577E-3,null,1,0.96618357487922713]
[null,null,"Refurbishment",null,"Gas Oil [Red Diesel]","litres",3.5114703749999998E-3,null,"Biodiesel [Standard]","litre",2.6023999999999999E-3,null,2,0.93351070036640305]
[null,null,"Demolition",null,"Petrol","litres",2.6418000000000001E-3,null,null,null,null,null,3,0.90194270566802237]
[null,null,null,null,"Diesel","litres",3.0713999999999997E-3,null,null,null,null,null,4,0.87144222769857238]
[null,null,null,null,"Water","litres",3.4410000000000002E-7,null,null,null,null,null,5,0.84197316685852419]
[null,null,"Gateway",null,null,null,null,null,null,null,null,null,6,0.81350064430775282]
[null,null,"G1",null,null,null,null,null,null,null,null,null,7,0.78599096068381913]
[null,null,"G3",null,"On Site Overheads - Method A",null,null,null,null,null,null,null,8,0.75941155621625056]
[null,null,"G4",null,"Size of project","t CO2e per week","t CO2e Cabin Setup",null,null,null,null,null,9,0.73373097218961414]
[null,null,"G6",null,"Large (18 months+)",1.210801968,1.1821531823999998,null,null,null,null,null,10,0.70891881370977217]
[null,null,"Theoretical Model",null,"Medium (6 - 18 months)",0.71760780000000002,0.63362599919999996,null,null,null,null,null,11,0.68494571372924851]
[null,null,null,null,"Small (Less than 6 months)",0.63794942399999999,0.17019763199999999,null,null,null,null,null,12,0.66178329828912896]
[null,null,null,null,null,null,null,null,null,null,null,null,13,0.63940415293635666]
[null,null,"Maintenane Intervention",null,null,null,null,null,null,null,null,null,14,0.61778179027667302]
[null,null,"Frequent",null,null,null,null,null,null,null,null,null,15,0.59689061862480497]
[null,null,"Intermitten",null,null,null,null,null,null,null,null,null,16,0.57670591171478747]
[null,null,"Emergency",null,"Maintenance Material","Co2e",null,null,null,null,null,null,17,0.55720377943457733]
[null,null,null,null,"N/A",null,null,null,null,null,null,null,18,0.53836113955031628]
[null,null,null,null,"Low",null,null,null,null,null,null,null,19,0.52015569038677911]
[null,null,"Assessment Period",null,"Medium",null,null,null,null,null,null,null,20,0.50256588443167061]
[null,null,"Q1",null,"High",null,null,null,null,null,null,null,21,0.48557090283253213]
[null,null,"Q2",null,null,null,null,null,null,null,null,null,22,0.46915063075606966]
[null,null,"Q3",null,null,null,null,null,null,null,null,null,23,0.45328563358074364]
[null,null,"Q4",null,"Maintenance Plant","Co2e",null,null,null,null,null,null,24,0.43795713389443841]
[null,null,null,null,"N/A",null,null,null,null,null,null,null,25,0.42314698926998884]
[null,null,null,null,"Low",null,null,null,null,null,null,null,26,0.40883767079225974]
[null,null,null,null,"Medium",null,null,null,null,null,null,null,27,0.39501224231136206]
[null,null,"Organisation",null,"High",null,null,null,null,null,null,null,28,0.38165434039745127]
[null,null,"Consultant",null,null,null,null,null,null,null,null,null,29,0.36874815497338298]
[null,null,"Environment Agency",null,null,null,null,null,null,null,null,null,30,0.35627841060230236]
[null,null,"Contractor",null,null,null,null,null,null,null,null,null,31,0.39998714516107459]
[null,null,null,null,null,null,null,null,null,null,null,null,32,0.38833703413696569]
[null,null,null,null,null,null,null,null,null,null,null,null,33,0.37702624673491814]
[null,null,null,null,null,null,null,null,null,null,null,null,34,0.36604489974263904]
[null,null,null,null,null,null,null,null,null,null,null,null,35,0.35538339780838735]
[null,null,null,null,null,null,null,null,null,null,null,null,36,0.34503242505668674]
[null,"Element Id","Element Description","Element Unit",null,null,null,null,null,null,null,null,37,0.33498293694823961]
[null,"BarrEA01","Barrier","m2",null,null,null,null,null,null,null,null,38,0.3252261523769317]
[null,"BeacEA02","Beach Recharge","m3",null,null,null,null,null,null,null,null,39,0.31575354599702099]
[null,"BridEA03","Bridge - Pedestrian","m2",null,null,null,null,null,null,null,null,40,0.30655684077380685]
[null,"BridEA04","Bridge - Vehicle Access","m2",null,null,null,null,null,null,null,null,41,0.29762800075126877]
[null,"ChanEA05","Channel - RC","m3",null,null,null,null,null,null,null,null,42,0.28895922403035801]
[null,"ContEA06","Control Building","m2",null,null,null,null,null,null,null,null,43,0.28054293595180391]
[null,"CulvEA07","Culvert ","m3",null,null,null,null,null,null,null,null,44,0.27237178247747956]
[null,"CulvEA10","Culvert Inlet/outlet Works","m2",null,null,null,null,null,null,null,null,45,0.26443862376454325]
[null,"DredEA11","Dredging Works","m3",null,null,null,null,null,null,null,null,46,0.25673652792674101]
[null,"DuneEA12","Dune Stabilisation","m3",null,null,null,null,null,null,null,null,47,0.24925876497741845]
[null,"ElecEA13","Electricity Supply","kWh",null,null,null,null,null,null,null,null,48,0.24199880094894996]
[null,"EmbaEA14","Embankment - Modify","m3",null,null,null,null,null,null,null,null,49,0.2349502921834466]
[null,"EmbaEA15","Embankment - New","m3",null,null,null,null,null,null,null,null,50,0.22810707978975397]
[null,"EnhaEA16","Enhanced Siltation","m3",null,null,null,null,null,null,null,null,51,0.22146318426189707]
[null,"ErosEA17","Erosion Protection ","m2",null,null,null,null,null,null,null,null,52,0.215012800254269]
[null,"ErosEA18","Erosion Protection - Geotextile","m2",null,null,null,null,null,null,null,null,53,0.20875029150899907]
[null,"ErosEA19","Erosion Protection - Grasscrete","m2",null,null,null,null,null,null,null,null,54,0.20267018593106703]
[null,"FielEA20","Field Drainage","m3",null,null,null,null,null,null,null,null,55,0.19676717080686118]
[null,"FishEA21","Fish Pass - Larinier - Bypass Weir","m3",null,null,null,null,null,null,null,null,56,0.19103608816200118]
[null,"FishEA22","Fish Pass - Larinier - Through Weir","m3",null,null,null,null,null,null,null,null,57,0.18547193025437006]
[null,"FishEA23","Fish Pass - Pool & Traverse","m3","Annual Intervention Fequency","No. of Interventions",null,null,null,null,null,null,58,0.18006983519841754]
[null,"FlapEA24","Flap Valve","mm dia","> 1 per year",null,null,null,null,null,null,null,59,0.17482508271691022]
[null,"FlooEA25","Flood Storage Reservoir","m3","Every year",1,null,null,null,null,null,null,60,0.1697330900164177]
[null,"FlowEA26","Flow Measurement - Control Channel Section","m3","Every 2 years",2,null,null,null,null,null,null,61,0.16478940778292983]
[null,"FlowEA27","Flow Measurement - Weir","m3","Every 3 years",3,null,null,null,null,null,null,62,0.15998971629410663]
[null,"GrouEA29","Groundwater Monitoring Boreholes","m3","Every 4 years",4,null,null,null,null,null,null,63,0.15532982164476369]
[null,"HabiEA30","Habitat Creation","m2","Every 5 years",5,null,null,null,null,null,null,64,0.15080565208229488]
[null,"HardEA31","Hard Landscaping","m2","Exceptional",null,null,null,null,null,null,null,65,0.14641325444882999]
[null,"HeadEA32","Headwall","mm dia",null,null,null,null,null,null,null,null,66,0.14214879072701941]
[null,"LandEA33","Land Remediation","m3",null,null,null,null,null,null,null,null,67,0.1380085346864266]
[null,"NaviEA34","Navigation Lock","m2",null,null,null,null,null,null,null,null,68,0.13398886862759865]
[null,"Non-EA35","Non-tidal Wall - Retaining - Concrete","m3",null,null,null,null,null,null,null,null,69,0.13008628022096957]
[null,"Non-EA36","Non-tidal Wall - Retaining - Masonry","m3","Use Energy Hours per year",null,null,null,null,null,null,null,70,0.12629735943783454]
[null,"Non-EA37","Non-tidal Wall - Retaining - Sheetpiled","m3",8760,null,null,null,null,null,null,null,71,0.12261879557071313]
[null,"OffsEA38","Offshore Breakwater - Submerged","tonnes",null,null,null,null,null,null,null,null,72,0.1190473743404982]
[null,"OffsEA39","Offshore Breakwater - Unsubmerged","tonnes",null,null,null,null,null,null,null,null,73,0.11557997508786232]
[null,"OutfEA40","Outfall Structure","mm dia","Electicity (kW)  t CO2e",null,null,null,null,null,null,null,74,0.11221356804646829]
[null,"PathEA41","Path/Track/Road","m2",4.9425999999999995E-4,null,null,null,null,null,null,null,75,0.10894521169560026]
[null,"PipeEA42","Pipes & Drains - Clay","m3",null,null,null,null,null,null,null,null,76,0.15310389176729922]
[null,"PipeEA43","Pipes & Drains - Concrete","m3",null,null,null,null,null,null,null,null,77,0.14936965050468218]
[null,"PipeEA44","Pipes & Drains - Plastic","m3",null,null,null,null,null,null,null,null,78,0.14572648829725093]
[null,"PumpEA45","Pumping Station - Land Drainage","kWh","New",1,null,null,null,null,null,null,79,0.14217218370463502]
[null,"PumpEA46","Pumping Station - Sewerage","kWh","Refurb",2,null,null,null,null,null,null,80,0.13870456946793663]
[null,"PumpEA47","Pumping Station - Surface Water","kWh","Replace",3,null,null,null,null,null,null,81,0.13532153118823087]
[null,"ReveEA48","Revetment Works - PCC","tonnes","Demolish",4,null,null,null,null,null,null,82,0.13202100603729841]
[null,"ReveEA49","Revetment Works - Rock Armour","tonnes","After Dem",5,null,null,null,null,null,null,83,0.12880098149980332]
[null,"ReveEA50","Revetment Works - Soft/geotextile ","m2","Blank",0,null,null,null,null,null,null,84,0.1256594941461496]
[null,"RiveEA51","River Gauging Station","m2",null,null,null,null,null,null,null,null,85,0.1225946284352679]
[null,"RiveEA52","River Restoration","m2",null,null,null,null,null,null,null,null,86,0.11960451554660284]
[null,"TidaEA71","Sea Wall - Retaining - Concrete","m3",null,null,null,null,null,null,null,null,87,0.11668733224058814]
[null,"ServEA53","Service Diversion - Electricity","m","Water Use",null,null,null,null,null,null,null,88,0.11384129974691526]
[null,"ServEA54","Service Diversion - Gas Main","m","Water Supply",{"$f":"(344.1/1000)/1000000","v":3.4410000000000002E-7},null,null,null,null,null,null,89,0.11106468267991736]
[null,"ServEA55","Service Diversion - Sewer","m","Water Treatment",{"$f":"(708.5/1000)/1000000","v":7.0849999999999997E-7},null,null,null,null,null,null,90,0.10835578798040717]
[null,"ServEA56","Service Diversion - Telecoms","m",null,null,null,null,null,null,null,null,91,0.10571296388332406]
[null,"ServEA57","Service Diversion - Water","m",null,null,null,null,null,null,null,null,92,0.10313459891056008]
[null,"SluiEA58","Sluices/penstocks","m2",null,null,null,null,null,null,null,null,93,0.10061912088835129]
[null,"SoftEA59","Soft Landscaping - Grassland","m2","Refurbishment Possible","%",null,null,null,null,null,null,94,9.8164995988635415E-2]
[null,"SoftEA60","Soft Landscaping - Shrubs/Tress","m2","Minor Refurbishment",0.1,null,null,null,null,null,null,95,9.577072779379063E-2]
[null,"TeleEA61","Telemetry Link","m","Moderate Refurbishment",0.25,null,null,null,null,null,null,96,9.3434856384185999E-2]
[null,"TidaEA62","Tidal Gate","m2","Major Refurbishment",0.5,null,null,null,null,null,null,97,9.1155957447986352E-2]
[null,"TidaEA63","Tidal Wall - Retaining - Concrete","m3","Not Possible",0,null,null,null,null,null,null,98,8.8932641412669614E-2]
[null,"TidaEA64","Tidal Wall - Retaining - Masonry","m3",null,null,null,null,null,null,null,null,99,8.6763552597726459E-2]
[null,"TidaEA65","Tidal Wall - Retaining - Sheetpiled","m2",null,null,null,null,null,null,null,null,100,8.4647368388025807E-2]
[null,"TrasEA66","Trash Screen","tonnes","M/R Level","Value"]
[null,"TunnEA67","Tunnelling","m3","Low",0.1]
[null,"WallEA68","Wall Raising","m2","Medium",1]
[null,"WeirEA69","Weir ","m2","High",5]
[null,"CulvEA08","Other","TBC","Not applicable",0]
[null,"FlooEA70","Flood gates","m2"]
[null,"BeacEA71","Beach control structures","m2"]
[null,"EnviEA72","Environmental Enhancements","m2"]
[null,"MotoEA73","Motor Control Centre","kW"]
[null,"SiltEA74","Silt removal","m3"]
[null,"SingEA75","Single Property Protection Measures","nr."]

{"sheet":"AssetList","index":12,"n_rows":65,"n_cols":4,"rows_kept":65,"cut":false,"hidden":true,"merged":[]}
["Sub-Element Category","Unit","Best Estimate Life (5)","Refurb Life"]
["Actuator ","kw",15,15]
["Barriers","m2",60,60]
["Beach Recharge","m2",120,120]
["Bridges","m2",60,60]
["Building","m2",60,60]
["Building Services - Eletrical System","m2",25,25]
["Building Services - Heating System","m2",15,15]
["Building Services - Ventilation","m2",15,15]
["Culvert","m3",120,120]
["Drainage","m3",60,60]
["Dredging ","m3",120,120]
["Dune Stabilisation","m3",40,40]
["Electricity Supply","kWh",60,60]
["Embankment - Coastal ","m3",50,50]
["Embankment - Fluvial ","m2",130,130]
["Engine ","hp",30,30]
["Enhanced Siltation","m3",60,60]
["Erosion Protection","m2",60,60]
["Fish Pass","m3",60,60]
["Flap Valve","mm Dia",40,40]
["Flood Storage Reservoir","m3",120,120]
["Gear Box","hp",30,30]
["Groundwater Monitoring Boreholes","m3",120,120]
["Habitat Creation","m2",60,60]
["Headwall","mm dia",80,80]
["HV Equipment","KV",25,25]
["Land Remediation","m3",120,120]
["Lanscaping","m2",60,60]
["MCC Controls","KW",20,20]
["Motor","KW",30,30]
["Navigation Lock","m2",60,60]
["Offshore Breakwater - Submerged","tonnes",120,120]
["Offshore Breakwater - Unsubmerged","tonnes",120,120]
["Other","TBC",100,100]
["Outfall Structure","m3",60,60]
["Paths/tracks/roads","m2",60,60]
["Pump","l/s",30,30]
["Pumping Station - Building","m2",60,60]
["RC Channel","m3",120,120]
["Revetment - Geotextile ","m2",60,60]
["Revetment - Hard","tonnes",120,120]
["River Gauging Station","m2",40,40]
["River Restoration","m2",40,40]
["Service Diversion - Electricity","m",120,120]
["Service Diversion - Gas Main","m",120,120]
["Service Diversion - Sewer","m",120,120]
["Service Diversion - Telecoms","m",120,120]
["Service Diversion - Water","m",120,120]
["Shingle","m3",40,40]
["Sluices/penstocks","m2",40,40]
["Telemetry Link","m",20,20]
["Tidal Gate","m2",60,60]
["Trash Screen","tonnes",40,40]
["Tunnelling","m3",120,120]
["Wall - Coastal","m2",80,80]
["Wall - Fluvial ","m2",130,130]
["Wall Raising","m2",60,60]
["Weir","m2",120,120]
["Flood gates","m2",35,35]
["Beach control structures","m2",120,120]
["Environmental Enhancements","m2",60,60]
["Motor Control Centre","kW",20,20]
["Silt removal","m3",40,40]
["Single Property Protection Measures","nr.",60,60]

{"sheet":"MaterialsData","index":13,"n_rows":650,"n_cols":5,"rows_kept":650,"cut":false,"hidden":true,"merged":[]}
["M1","M1.1","M1.1.1","Unit","Co2e value"]
["Aggregate","General (Gravel or Crushed Rock)","N/A","t",5.1999999999999998E-3]
["Aggregate","General (Gravel or Crushed Rock)","N/A","m3",1.04E-2]
["Aggregate","Quarried Aggregate","N/A","t",5.1999999999999998E-3]
["Aggregate","Quarried Aggregate","N/A","m3",1.04E-2]
["Aggregate","Recycled Aggregate","N/A","t",5.1999999999999998E-3]
["Aggregate","Recycled Aggregate","N/A","m3",1.04E-2]
["Aggregate","Marine Aggregate","N/A","t",8.0000000000000002E-3]
["Aggregate","Marine Aggregate","N/A","m3",1.6E-2]
["Aluminium","General (Aluminium)","General","t",9.16]
["Aluminium","General (Aluminium)","General","m3",24.732000000000003]
["Aluminium","General (Aluminium)","Virgin","t",12.79]
["Aluminium","General (Aluminium)","Virgin","m3",34.533000000000001]
["Aluminium","General (Aluminium)","Recycled","t",1.81]
["Aluminium","General (Aluminium)","Recycled","m3",4.8870000000000005]
["Asphalt","General ","N/A","t",7.5999999999999998E-2]
["Asphalt","General ","N/A","m3",0.12920000000000001]
["Asphalt","Asphalt, 4% (bitumen) binder content (by mass)","N/A","t",6.6000000000000003E-2]
["Asphalt","Asphalt, 4% (bitumen) binder content (by mass)","N/A","m3",0.11220000000000001]
["Asphalt","Asphalt, 5% binder content","N/A","t",7.0999999999999994E-2]
["Asphalt","Asphalt, 5% binder content","N/A","m3",0.12069999999999999]
["Asphalt","Asphalt, 6% binder content","N/A","t",7.5999999999999998E-2]
["Asphalt","Asphalt, 6% binder content","N/A","m3",0.12919999999999998]
["Asphalt","Asphalt, 7% binder content","N/A","t",8.1000000000000003E-2]
["Asphalt","Asphalt, 7% binder content","N/A","m3",0.13769999999999999]
["Asphalt","Asphalt, 8% binder content","N/A","t",8.5999999999999993E-2]
["Asphalt","Asphalt, 8% binder content","N/A","m3",0.1462]
["Bricks","General (Bricks)","N/A","t",0.24]
["Bricks","General (Bricks)","N/A","m3",0.45599999999999996]
["Bricks","General (Bricks)","Per Single Brick","t",5.5000000000000003E-4]
["Cement","Average CEM I Portland Cement, 94% Clinker","N/A","t",0.95]
["Cement","Average CEM I Portland Cement, 94% Clinker","N/A","m3",1.4249999999999998]
["Cement","Ground Granulated Blastfurnace Slag (GGBS)","N/A","t",8.3000000000000004E-2]
["Cement","Ground Granulated Blastfurnace Slag (GGBS)","N/A","m3",0.1245]
["Cement","Fly Ash","N/A","t",8.0000000000000002E-3]
["Cement","Fly Ash","N/A","m3",1.2E-2]
["Cement","Portland Limestone Cement","CEM II/A-LL or L (20% limestone)","t",0.75]
["Cement","Portland Limestone Cement","CEM II/A-LL or L (20% limestone)","m3",1.125]
["Cement","Portland Limestone Cement","CEM II/A-LL or L (13% limestone)","t",0.81499999999999995]
["Cement","Portland Limestone Cement","CEM II/A-LL or L (13% limestone)","m3",1.2224999999999999]
["Cement","Portland Limestone Cement","CEM II/A-LL or L (6% limestone)","t",0.88]
["Cement","Portland Limestone Cement","CEM II/A-LL or L (6% limestone)","m3",1.32]
["Cement","Portland Fly Ash Cement","CEM II/A-V (20% Fly Ash)","t",0.75]
["Cement","Portland Fly Ash Cement","CEM II/A-V (20% Fly Ash)","m3",1.125]
["Cement","Portland Fly Ash Cement","CEM II/A-V (13% Fly Ash)","t",0.81]
["Cement","Portland Fly Ash Cement","CEM II/A-V (13% Fly Ash)","m3",1.2150000000000001]
["Cement","Portland Fly Ash Cement","CEM II/A-V (6% Fly Ash)","t",0.87]
["Cement","Portland Fly Ash Cement","CEM II/A-V (6% Fly Ash)","m3",1.3049999999999999]
["Cement","Portland Fly Ash Cement","CEM II/A-V (35% Fly Ash)","t",0.61]
["Cement","Portland Fly Ash Cement","CEM II/A-V (35% Fly Ash)","m3",0.91500000000000004]
["Cement","Portland Fly Ash Cement","CEM II/A-V (28% Fly Ash)","t",0.67]
["Cement","Portland Fly Ash Cement","CEM II/A-V (28% Fly Ash)","m3",1.0050000000000001]
["Cement","Portland Fly Ash Cement","CEM II/A-V (21% Fly Ash)","t",0.73]
["Cement","Portland Fly Ash Cement","CEM II/A-V (21% Fly Ash)","m3",1.095]
["Cement","Portland Slag Cement","CEM II/B-S (35% GGBS)","t",0.62]
["Cement","Portland Slag Cement","CEM II/B-S (35% GGBS)","m3",0.92999999999999994]
["Cement","Portland Slag Cement","CEM II/B-S (28% GGBS)","t",0.68]
["Cement","Portland Slag Cement","CEM II/B-S (28% GGBS)","m3",1.02]
["Cement","Portland Slag Cement","CEM II/B-S (21% GGBS)","t",0.74]
["Cement","Portland Slag Cement","CEM II/B-S (21% GGBS)","m3",1.1099999999999999]
["Cement","Blastfurnace Cement","CEM III/A (65% GGBS)","t",0.36]
["Cement","Blastfurnace Cement","CEM III/A (65% GGBS)","m3",0.54]
["Cement","Blastfurnace Cement","CEM III/A (50.5% GGBS)","t",0.48]
["Cement","Blastfurnace Cement","CEM III/A (50.5% GGBS)","m3",0.72]
["Cement","Blastfurnace Cement","CEM III/A (36% GGBS)","t",0.61]
["Cement","Blastfurnace Cement","CEM III/A (36% GGBS)","m3",0.91500000000000004]
["Cement","Blastfurnace Cement","CEM III/A (80% GGBS)","t",0.23]
["Cement","Blastfurnace Cement","CEM III/A (80% GGBS)","m3",0.34500000000000003]
["Cement","Blastfurnace Cement","CEM III/A (73% GGBS)","t",0.28499999999999998]
["Cement","Blastfurnace Cement","CEM III/A (73% GGBS)","m3",0.42749999999999999]
["Cement","Blastfurnace Cement","CEM III/A (66% GGBS)","t",0.34]
["Cement","Blastfurnace Cement","CEM III/A (66% GGBS)","m3",0.51]
["Cement","Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (55% GGBS)","t",0.42]
["Cement","Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (55% GGBS)","m3",0.63]
["Cement","Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (45.5% GGBS)","t",0.505]
["Cement","Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (45.5% GGBS)","m3",0.75750000000000006]
["Cement","Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (36% GGBS)","t",0.59]
["Cement","Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (36% GGBS)","m3",0.88500000000000001]
["Cement","General","N/A","t",0.74]
["Cement","General","N/A","m3",1.3764000000000001]
["Cement","6-20% Fly Ash (CEM II/A-V)","N/A","t",0.82499999999999996]
["Cement","6-20% Fly Ash (CEM II/A-V)","N/A","m3",1.2374999999999998]
["Cement","21-35% Fly Ash (CEM II/B-V)","N/A","t",0.68500000000000005]
["Cement","21-35% Fly Ash (CEM II/B-V)","N/A","m3",1.0275000000000001]
["Cement","21-35% GGBS (CEM II/B-S)","N/A","t",0.71]
["Cement","21-35% GGBS (CEM II/B-S)","N/A","m3",1.0649999999999999]
["Cement","36-65% GGBS (CEM III/A)","N/A","t",0.51500000000000001]
["Cement","36-65% GGBS (CEM III/A)","N/A","m3",0.77249999999999996]
["Cement","66-80% GGBS (CEM III/B)","N/A","t",0.32]
["Cement","66-80% GGBS (CEM III/B)","N/A","m3",0.48]
["Cement","Cement stabilised soil @ 5%","N/A","t",6.0999999999999999E-2]
["Cement","Cement stabilised soil @ 5%","N/A","m3",9.1499999999999998E-2]
["Cement","Cement stabilised soil @ 8%","N/A","t",8.4000000000000005E-2]
["Cement","Cement stabilised soil @ 8%","N/A","m3",0.126]
["Cement","GGBS stabilised soil","N/A","t",4.7E-2]
["Cement","GGBS stabilised soil","N/A","m3",7.0500000000000007E-2]
["Cement","Fly ash stabilised soil","N/A","t",4.1000000000000002E-2]
["Cement","Fly ash stabilised soil","N/A","m3",6.1499999999999999E-2]
["Clay","Vitrified clay pipe DN 100 & DN 150","N/A","t",0.46]
["Clay","Vitrified clay pipe DN 100 & DN 150","N/A","m3",1.1040000000000001]
["Clay","Vitrified clay pipe DN 200 & DN 300","N/A","t",0.5]
["Clay","Vitrified clay pipe DN 200 & DN 300","N/A","m3",1.2]
["Clay","Vitrified clay pipe DN 500","N/A","t",0.55000000000000004]
["Clay","Vitrified clay pipe DN 500","N/A","m3",1.32]
["Copper","EU Tube & Sheet","General","t",2.71]
["Copper","EU Tube & Sheet","General","m3",24.119]
["Copper","EU Tube & Sheet","Virgin","t",3.81]
["Copper","EU Tube & Sheet","Virgin","m3",33.908999999999999]
["Copper","EU Tube & Sheet","Recycled","t",0.84]
["Copper","EU Tube & Sheet","Recycled","m3",7.476]
["Copper","Reused ","N/A","t",0.27]
["Copper","Reused ","N/A","m3",2.4030000000000005]
["Glass","General","N/A","t",0.95]
["Glass","General","N/A","m3",2.375]
["Insulation","General Insulation","N/A","t",1.86]
["Insulation","General Insulation","N/A","m3",7.4400000000000008E-2]
["Iron","General (Iron)","N/A","t",2.0322399999999998]
["Iron","General (Iron)","N/A","m3",16.054696]
["Lead","General (Lead)","General","t",1.6680999999999999]
["Lead","General (Lead)","General","m3",18.849530000000001]
["Lead","General (Lead)","Virgin","t",3.37]
["Lead","General (Lead)","Virgin","m3",38.081000000000003]
["Lead","General (Lead)","Recycled","t",0.57999999999999996]
["Lead","General (Lead)","Recycled","m3",6.5540000000000003]
["Lime","General (Lime)","N/A","t",0.78]
["Lime","General (Lime)","N/A","m3",0.93599999999999994]
["Miscellaneous","Damp Proof Course/Membrane","N/A","t",4.2]
["Miscellaneous","Damp Proof Course/Membrane","N/A","m2",3.7799999999999999E-3]
["Miscellaneous","Grit","N/A","t",7.0000000000000001E-3]
["Miscellaneous","Grit","N/A","m3",1.4E-2]
["Miscellaneous","Ground Limestone","N/A","t",3.2000000000000001E-2]
["Miscellaneous","Ground Limestone","N/A","m3",2.8800000000000003E-2]
["Miscellaneous","Glass Reinforced Plastic - GRP - Fibreglass","N/A","t",8.1]
["Miscellaneous","Glass Reinforced Plastic - GRP - Fibreglass","N/A","m3",13.77]
["Paint","General (Paint)","N/A","t",2.91]
["Paint","General (Paint)","N/A","m3",3.492]
["Plaster","General (Gypsum)","N/A","t",0.13]
["Plaster","General (Gypsum)","N/A","m3",0.16900000000000001]
["Plaster","Plasterboard","N/A","t",0.39]
["Plaster","Plasterboard","N/A","m3",0.39]
["Plastics","General (Plastics)","N/A","t",3.31]
["Plastics","General (Plastics)","N/A","m3",4.5678000000000001]
["Plastics","General Polyethylene","N/A","t",2.54]
["Plastics","General Polyethylene","N/A","m3",2.3368000000000002]
["Plastics","HDPE Pipe","N/A","t",2.52]
["Plastics","HDPE Pipe","N/A","m3",2.6460000000000004]
["Plastics","PVC General","N/A","t",3.1]
["Plastics","PVC General","N/A","m3",4.2779999999999996]
["Plastics","PVC Pipe","N/A","t",3.23]
["Plastics","PVC Pipe","N/A","m3",4.5542999999999996]
["Sand","General (Sand)","N/A","t",5.1000000000000004E-3]
["Sand","General (Sand)","N/A","m3",1.1424000000000002E-2]
["Soil/Clay","General (Rammed Soil)","N/A","t",2.4E-2]
["Soil/Clay","General (Rammed Soil)","N/A","m3",4.0800000000000003E-2]
["Stone","General (Stone)","N/A","t",7.9000000000000001E-2]
["Stone","General (Stone)","N/A","m3",0.158]
["Stone","Granite","N/A","t",0.7]
["Stone","Granite","N/A","m3",2.0299999999999998]
["Stone","Limestone","N/A","t",0.09]
["Stone","Limestone","N/A","m3",0.19800000000000001]
["Stone","Marble","N/A","t",0.13]
["Stone","Sandstone","N/A","t",0.06]
["Stone","Sandstone","N/A","m3",0.13200000000000001]
["Stone","Slate","N/A","t",3.5000000000000003E-2]
["Stone","Slate","N/A","m3",9.4500000000000015E-2]
["Stone","Shale","N/A","t",2E-3]
["Stone","Shale","N/A","m3",5.4000000000000003E-3]
["Timber","General (Timber)","N/A","t",0.31]
["Timber","General (Timber)","N/A","m3",0.155]
["Timber","Glue Laminated timber ","N/A","t",0.42]
["Timber","Glue Laminated timber ","N/A","m3",0.21]
["Timber","Hardboard","N/A","t",0.57999999999999996]
["Timber","Hardboard","N/A","m3",0.46399999999999997]
["Timber","MDF","N/A","t",0.39]
["Timber","MDF","N/A","m2",5.460000000000001E-2]
["Timber","Plywood","N/A","t",0.45]
["Timber","Plywood","N/A","m2",4.9500000000000002E-2]
["Timber","Reclaimed Timber","N/A","t",0.03]
["Timber","Reclaimed Timber","N/A","m3",2.1000000000000001E-2]
["Zinc","General (Zinc)","N/A","t",3.09]
["Zinc","Virgin","N/A","t",4.18]
["Zinc","Recycled","N/A","t",0.52]
["Roads","Asphalt road - Hot construction method ","Construction","m2",3.2799999999999996E-2]
["Roads","Asphalt road - Cold construction method ","Construction","m2",2.8199999999999999E-2]
["Steel","General - UK (EU) Average Recycled Content","N/A","t",1.46]
["Steel","General - UK (EU) Average Recycled Content","N/A","m3",11.388]
["Steel","Bar & Rod - UK (EU) Average Recycled Content","N/A","t",1.4]
["Steel","Bar & Rod - UK (EU) Average Recycled Content","N/A","m3",10.92]
["Steel","Coil (Sheet) - UK (EU) Average Recycled Content","N/A","t",1.38]
["Steel","Coil (Sheet) - UK (EU) Average Recycled Content","N/A","m3",10.763999999999999]
["Steel","Coil (Sheet) - Galvanised - UK (EU) Average Recycled Content","N/A","t",1.54]
["Steel","Coil (Sheet) - Galvanised - UK (EU) Average Recycled Content","N/A","m3",12.012]
["Steel","Engineering Steel - Recycled","N/A","t",0.72]
["Steel","Engineering Steel - Recycled","N/A","m3",5.6159999999999997]
["Steel","Pipe - UK (EU) Average Recycled Content","N/A","t",1.45]
["Steel","Pipe - UK (EU) Average Recycled Content","N/A","m3",11.309999999999999]
["Steel","Plate - UK (EU) Average Recycled Content","N/A","t",1.66]
["Steel","Plate - UK (EU) Average Recycled Content","N/A","m3",12.947999999999999]
["Steel","Stainless","N/A","t",6.15]
["Steel","Stainless","N/A","m3",49.2]
["Steel","Reused ","N/A","t",0.14599999999999999]
["Steel","Reused ","N/A","m3",1.1387999999999998]
["Concrete","In-situ Concrete (General)","General","t",0.107]
["Concrete","In-situ Concrete (General)","General","m3",0.25679999999999997]
["Concrete","In-situ Concrete (General)","16/20 Mpa","t",0.1]
["Concrete","In-situ Concrete (General)","16/20 Mpa","m3",0.24]
["Concrete","In-situ Concrete (General)","20/25 MPa","t",0.107]
["Concrete","In-situ Concrete (General)","20/25 MPa","m3",0.25679999999999997]
["Concrete","In-situ Concrete (General)","25/30 MPa","t",0.113]
["Concrete","In-situ Concrete (General)","25/30 MPa","m3",0.2712]
["Concrete","In-situ Concrete (General)","28/35 MPa","t",0.12]
["Concrete","In-situ Concrete (General)","28/35 MPa","m3",0.28799999999999998]
["Concrete","In-situ Concrete (General)","32/40 MPa","t",0.13200000000000001]
["Concrete","In-situ Concrete (General)","32/40 MPa","m3",0.31680000000000003]
["Concrete","In-situ Concrete (General)","40/50 MPa","t",0.151]
["Concrete","In-situ Concrete (General)","40/50 MPa","m3",0.3624]
["Concrete","In-situ Concrete (CEM 1)","GEN 0 (6/8 MPa)","t",7.6056223933197512E-2]
["Concrete","In-situ Concrete (CEM 1)","GEN 0 (6/8 MPa)","m3",0.18253493743967403]
["Concrete","In-situ Concrete (CEM 1)","GEN 1 (8/10 MPa) ","t",0.10386736430985342]
["Concrete","In-situ Concrete (CEM 1)","GEN 1 (8/10 MPa) ","m3",0.2492816743436482]
["Concrete","In-situ Concrete (CEM 1)","GEN 2 (12/15 MPa) ","t",0.11381080474907539]
["Concrete","In-situ Concrete (CEM 1)","GEN 2 (12/15 MPa) ","m3",0.27314593139778093]
["Concrete","In-situ Concrete (CEM 1)","GEN 3 (16/20 MPa) ","t",0.1227451113421755]
["Concrete","In-situ Concrete (CEM 1)","GEN 3 (16/20 MPa) ","m3",0.29458826722122117]
["Concrete","In-situ Concrete (CEM 1)","RC 20/25 (20/25 MPa) ","t",0.13206895301252261]
["Concrete","In-situ Concrete (CEM 1)","RC 20/25 (20/25 MPa) ","m3",0.31696548723005424]
["Concrete","In-situ Concrete (CEM 1)","RC 25/30 (25/30 MPa) ","t",0.14005626539266883]
["Concrete","In-situ Concrete (CEM 1)","RC 25/30 (25/30 MPa) ","m3",0.33613503694240515]
["Concrete","In-situ Concrete (CEM 1)","RC 28/35 (28/35 MPa) ","t",0.14801934402577693]
["Concrete","In-situ Concrete (CEM 1)","RC 28/35 (28/35 MPa) ","m3",0.35524642566186465]
["Concrete","In-situ Concrete (CEM 1)","RC 32/40 (32/40 MPa)","t",0.1629726106383044]
["Concrete","In-situ Concrete (CEM 1)","RC 32/40 (32/40 MPa)","m3",0.39113426553193054]
["Concrete","In-situ Concrete (CEM 1)","RC 40/50 (40/50 Mpa)","t",0.18784953969440599]
["Concrete","In-situ Concrete (CEM 1)","RC 40/50 (40/50 Mpa)","m3",0.45083889526657434]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","t",6.9162119731383837E-2]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","m3",0.1659890873553212]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","t",6.1372111207213247E-2]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","m3",0.14729306689731178]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","t",9.3634783151117201E-2]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","m3",0.22472347956268127]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","t",8.2211164792537095E-2]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","m3",0.19730679550208902]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","t",0.10461450307968014]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","m3",0.25107480739123234]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","t",9.2635694503475224E-2]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","m3",0.22232566680834054]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","t",0.11220320877484814]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","m3",0.26928770105963551]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","t",9.9577966407624854E-2]
["Concrete","In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","m3",0.23898711937829964]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","t",0.1219053607385972]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","m3",0.29257286577263325]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","t",0.10766218771465649]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","m3",0.25838925051517558]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","t",0.12954369607804206]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","m3",0.31090487058730093]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","t",0.1146626330090819]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","m3",0.27519031922179654]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","t",0.13801120386270863]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","m3",0.3312268892705007]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","t",0.12374131044667398]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","m3",0.29697914507201756]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","t",0.15241036951716433]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","m3",0.36578488684119437]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","t",0.13629697668084267]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","m3",0.32711274403402241]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","t",0.17438915168252622]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","m3",0.41853396403806292]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","t",0.15509320233120771]
["Concrete","In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","m3",0.37222368559489849]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","t",6.0070811868456399E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","m3",0.14416994848429535]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","t",4.5006416186552801E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","m3",0.10801539884772672]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","t",7.9950944919938413E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","m3",0.1918822678078522]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","t",5.7874792562995957E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","m3",0.13889950215119029]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","t",8.7878329728629287E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","m3",0.21090799134871027]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","t",6.5391795867461466E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","m3",0.15694031008190751]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","t",9.6015711542619342E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","m3",0.23043770770228642]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","t",6.9679689013701807E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","m3",0.16723125363288432]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","t",0.10405135090427084]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","m3",0.24972324217024999]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","t",7.6510695631907363E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","m3",0.18362566951657766]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","t",0.11098175073618008]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","m3",0.26635620176683217]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","t",8.1394937176048579E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","m3",0.19534784922251658]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","t",0.11866342669428036]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","m3",0.28479222406627286]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","t",8.788522278282615E-2]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","m3",0.21092453467878275]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","t",0.1332653290161302]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","m3",0.31983678963871248]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","t",0.10031952788639446]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","m3",0.2407668669273467]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","t",0.15320197226662277]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","m3",0.36768473343989466]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","t",0.11487805733476771]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","m3",0.27570733760344246]
["Concrete","Reinforced In-situ Concrete (General)","General","t",0.184]
["Concrete","Reinforced In-situ Concrete (General)","General","m3",0.44159999999999999]
["Concrete","Reinforced In-situ Concrete (General)","16/20 Mpa","t",0.17699999999999999]
["Concrete","Reinforced In-situ Concrete (General)","16/20 Mpa","m3",0.42479999999999996]
["Concrete","Reinforced In-situ Concrete (General)","20/25 MPa","t",0.184]
["Concrete","Reinforced In-situ Concrete (General)","20/25 MPa","m3",0.44159999999999999]
["Concrete","Reinforced In-situ Concrete (General)","25/30 MPa","t",0.19]
["Concrete","Reinforced In-situ Concrete (General)","25/30 MPa","m3",0.45599999999999996]
["Concrete","Reinforced In-situ Concrete (General)","28/35 MPa","t",0.19700000000000001]
["Concrete","Reinforced In-situ Concrete (General)","28/35 MPa","m3",0.4728]
["Concrete","Reinforced In-situ Concrete (General)","32/40 MPa","t",0.20900000000000002]
["Concrete","Reinforced In-situ Concrete (General)","32/40 MPa","m3",0.50160000000000005]
["Concrete","Reinforced In-situ Concrete (General)","40/50 MPa","t",0.22799999999999998]
["Concrete","Reinforced In-situ Concrete (General)","40/50 MPa","m3",0.54719999999999991]
["Concrete","Reinforced In-situ Concrete (CEM 1)","GEN 0 (6/8 MPa)","t",0.15305622393319751]
["Concrete","Reinforced In-situ Concrete (CEM 1)","GEN 0 (6/8 MPa)","m3",0.36733493743967399]
["Concrete","Reinforced In-situ Concrete (CEM 1)","GEN 1 (8/10 MPa) ","t",0.18086736430985342]
["Concrete","Reinforced In-situ Concrete (CEM 1)","GEN 1 (8/10 MPa) ","m3",0.43408167434364819]
["Concrete","Reinforced In-situ Concrete (CEM 1)","GEN 2 (12/15 MPa) ","t",0.19081080474907539]
["Concrete","Reinforced In-situ Concrete (CEM 1)","GEN 2 (12/15 MPa) ","m3",0.45794593139778089]
["Concrete","Reinforced In-situ Concrete (CEM 1)","GEN 3 (16/20 MPa) ","t",0.19974511134217549]
["Concrete","Reinforced In-situ Concrete (CEM 1)","GEN 3 (16/20 MPa) ","m3",0.47938826722122113]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 20/25 (20/25 MPa) ","t",0.2090689530125226]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 20/25 (20/25 MPa) ","m3",0.50176548723005421]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 25/30 (25/30 MPa) ","t",0.21705626539266881]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 25/30 (25/30 MPa) ","m3",0.52093503694240517]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 28/35 (28/35 MPa) ","t",0.22501934402577695]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 28/35 (28/35 MPa) ","m3",0.54004642566186467]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 32/40 (32/40 MPa)","t",0.23997261063830438]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 32/40 (32/40 MPa)","m3",0.5759342655319305]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 40/50 (40/50 Mpa)","t",0.264849539694406]
["Concrete","Reinforced In-situ Concrete (CEM 1)","RC 40/50 (40/50 Mpa)","m3",0.63563889526657436]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","t",0.14616211973138382]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","m3",0.35078908735532116]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","t",0.13837211120721324]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","m3",0.33209306689731177]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","t",0.17063478315111719]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","m3",0.40952347956268126]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","t",0.15921116479253711]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","m3",0.38210679550208904]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","t",0.18161450307968013]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","m3",0.4358748073912323]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","t",0.16963569450347521]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","m3",0.4071256668083405]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","t",0.18920320877484814]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","m3",0.45408770105963553]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","t",0.17657796640762485]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","m3",0.42378711937829966]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","t",0.19890536073859721]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","m3",0.47737286577263327]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","t",0.18466218771465648]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","m3",0.44318925051517555]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","t",0.20654369607804207]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","m3",0.49570487058730095]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","t",0.1916626330090819]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","m3",0.45999031922179656]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","t",0.21501120386270861]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","m3",0.51602688927050067]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","t",0.20074131044667398]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","m3",0.48177914507201752]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","t",0.22941036951716431]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","m3",0.55058488684119433]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","t",0.21329697668084269]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","m3",0.51191274403402243]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","t",0.25138915168252624]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","m3",0.60333396403806294]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","t",0.23209320233120773]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","m3",0.55702368559489857]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","t",0.1370708118684564]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","m3",0.32896994848429534]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","t",0.12200641618655281]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","m3",0.29281539884772673]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","t",0.15695094491993841]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","m3",0.37668226780785219]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","t",0.13487479256299595]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","m3",0.32369950215119025]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","t",0.16487832972862929]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","m3",0.39570799134871026]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","t",0.14239179586746148]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","m3",0.34174031008190753]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","t",0.17301571154261935]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","m3",0.41523770770228646]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","t",0.14667968901370182]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","m3",0.35203125363288434]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","t",0.18105135090427082]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","m3",0.43452324217024996]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","t",0.15351069563190736]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","m3",0.36842566951657768]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","t",0.18798175073618006]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","m3",0.45115620176683213]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","t",0.15839493717604858]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","m3",0.3801478492225166]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","t",0.19566342669428036]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","m3",0.46959222406627282]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","t",0.16488522278282614]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","m3",0.39572453467878271]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","t",0.21026532901613021]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","m3",0.5046367896387125]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","t",0.17731952788639446]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","m3",0.42556686692734669]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","t",0.23020197226662276]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","m3",0.55248473343989457]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","t",0.1918780573347677]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","m3",0.46050733760344248]
["Concrete","Precast Concrete (General)","General","t",0.13600000000000001]
["Concrete","Precast Concrete (General)","General","m3",0.32640000000000002]
["Concrete","Precast Concrete (General)","16/20 Mpa","t",0.129]
["Concrete","Precast Concrete (General)","16/20 Mpa","m3",0.30959999999999999]
["Concrete","Precast Concrete (General)","20/25 MPa","t",0.13600000000000001]
["Concrete","Precast Concrete (General)","20/25 MPa","m3",0.32640000000000002]
["Concrete","Precast Concrete (General)","25/30 MPa","t",0.14200000000000002]
["Concrete","Precast Concrete (General)","25/30 MPa","m3",0.34080000000000005]
["Concrete","Precast Concrete (General)","28/35 MPa","t",0.14899999999999999]
["Concrete","Precast Concrete (General)","28/35 MPa","m3",0.35759999999999997]
["Concrete","Precast Concrete (General)","32/40 MPa","t",0.161]
["Concrete","Precast Concrete (General)","32/40 MPa","m3",0.38640000000000002]
["Concrete","Precast Concrete (General)","40/50 MPa","t",0.18]
["Concrete","Precast Concrete (General)","40/50 MPa","m3",0.432]
["Concrete","Precast Concrete (CEM 1)","GEN 0 (6/8 MPa)","t",0.10505622393319751]
["Concrete","Precast Concrete (CEM 1)","GEN 0 (6/8 MPa)","m3",0.25213493743967402]
["Concrete","Precast Concrete (CEM 1)","GEN 1 (8/10 MPa) ","t",0.13286736430985344]
["Concrete","Precast Concrete (CEM 1)","GEN 1 (8/10 MPa) ","m3",0.31888167434364822]
["Concrete","Precast Concrete (CEM 1)","GEN 2 (12/15 MPa) ","t",0.1428108047490754]
["Concrete","Precast Concrete (CEM 1)","GEN 2 (12/15 MPa) ","m3",0.34274593139778092]
["Concrete","Precast Concrete (CEM 1)","GEN 3 (16/20 MPa) ","t",0.1517451113421755]
["Concrete","Precast Concrete (CEM 1)","GEN 3 (16/20 MPa) ","m3",0.36418826722122116]
["Concrete","Precast Concrete (CEM 1)","RC 20/25 (20/25 MPa) ","t",0.16106895301252261]
["Concrete","Precast Concrete (CEM 1)","RC 20/25 (20/25 MPa) ","m3",0.38656548723005424]
["Concrete","Precast Concrete (CEM 1)","RC 25/30 (25/30 MPa) ","t",0.16905626539266883]
["Concrete","Precast Concrete (CEM 1)","RC 25/30 (25/30 MPa) ","m3",0.40573503694240515]
["Concrete","Precast Concrete (CEM 1)","RC 28/35 (28/35 MPa) ","t",0.17701934402577693]
["Concrete","Precast Concrete (CEM 1)","RC 28/35 (28/35 MPa) ","m3",0.42484642566186465]
["Concrete","Precast Concrete (CEM 1)","RC 32/40 (32/40 MPa)","t",0.1919726106383044]
["Concrete","Precast Concrete (CEM 1)","RC 32/40 (32/40 MPa)","m3",0.46073426553193053]
["Concrete","Precast Concrete (CEM 1)","RC 40/50 (40/50 Mpa)","t",0.21684953969440598]
["Concrete","Precast Concrete (CEM 1)","RC 40/50 (40/50 Mpa)","m3",0.52043889526657439]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","t",9.8162119731383835E-2]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","m3",0.23558908735532119]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","t",9.0372111207213252E-2]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","m3",0.2168930668973118]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","t",0.1226347831511172]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","m3",0.29432347956268129]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","t",0.11121116479253709]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","m3",0.26690679550208901]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","t",0.13361450307968015]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","m3",0.32067480739123233]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","t",0.12163569450347522]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","m3",0.29192566680834053]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","t",0.14120320877484815]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","m3",0.33888770105963556]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","t",0.12857796640762487]
["Concrete","Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","m3",0.30858711937829969]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","t",0.1509053607385972]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","m3",0.36217286577263325]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","t",0.13666218771465649]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","m3",0.32798925051517558]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","t",0.15854369607804206]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","m3",0.38050487058730093]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","t",0.14366263300908191]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","m3",0.34479031922179659]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","t",0.16701120386270862]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","m3",0.4008268892705007]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","t",0.15274131044667399]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","m3",0.36657914507201755]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","t",0.18141036951716433]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","m3",0.43538488684119436]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","t",0.16529697668084267]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","m3",0.3967127440340224]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","t",0.20338915168252622]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","m3",0.48813396403806292]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","t",0.18409320233120771]
["Concrete","Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","m3",0.44182368559489849]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","t",8.9070811868456404E-2]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","m3",0.21376994848429537]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","t",7.4006416186552806E-2]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","m3",0.17761539884772673]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","t",0.10895094491993841]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","m3",0.26148226780785216]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","t",8.6874792562995962E-2]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","m3",0.20849950215119031]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","t",0.11687832972862928]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","m3",0.28050799134871029]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","t",9.4391795867461464E-2]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","m3",0.2265403100819075]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","t",0.12501571154261934]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","m3",0.30003770770228638]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","t",9.8679689013701805E-2]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","m3",0.23683125363288432]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","t",0.13305135090427084]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","m3",0.31932324217024999]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","t",0.10551069563190736]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","m3",0.25322566951657766]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","t",0.13998175073618008]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","m3",0.33595620176683216]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","t",0.11039493717604858]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","m3",0.26494784922251657]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","t",0.14766342669428037]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","m3",0.35439222406627285]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","t",0.11688522278282615]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","m3",0.28052453467878274]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","t",0.16226532901613019]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","m3",0.38943678963871248]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","t",0.12931952788639448]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","m3",0.31036686692734672]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","t",0.18220197226662277]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","m3",0.43728473343989466]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","t",0.14387805733476772]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","m3",0.34530733760344251]
["Concrete","Reinforced Precast Concrete (General)","General","t",0.21300000000000002]
["Concrete","Reinforced Precast Concrete (General)","General","m3",0.51119999999999999]
["Concrete","Reinforced Precast Concrete (General)","16/20 Mpa","t",0.20600000000000002]
["Concrete","Reinforced Precast Concrete (General)","16/20 Mpa","m3",0.49440000000000001]
["Concrete","Reinforced Precast Concrete (General)","20/25 MPa","t",0.21300000000000002]
["Concrete","Reinforced Precast Concrete (General)","20/25 MPa","m3",0.51119999999999999]
["Concrete","Reinforced Precast Concrete (General)","25/30 MPa","t",0.21900000000000003]
["Concrete","Reinforced Precast Concrete (General)","25/30 MPa","m3",0.52560000000000007]
["Concrete","Reinforced Precast Concrete (General)","28/35 MPa","t",0.22599999999999998]
["Concrete","Reinforced Precast Concrete (General)","28/35 MPa","m3",0.54239999999999988]
["Concrete","Reinforced Precast Concrete (General)","32/40 MPa","t",0.23799999999999999]
["Concrete","Reinforced Precast Concrete (General)","32/40 MPa","m3",0.57119999999999993]
["Concrete","Reinforced Precast Concrete (General)","40/50 MPa","t",0.25700000000000001]
["Concrete","Reinforced Precast Concrete (General)","40/50 MPa","m3",0.61680000000000001]
["Concrete","Reinforced Precast Concrete (CEM 1)","GEN 0 (6/8 MPa)- 0% Cement Replacement - Fly Ash","t",0.18205622393319751]
["Concrete","Reinforced Precast Concrete (CEM 1)","GEN 0 (6/8 MPa)- 0% Cement Replacement - Fly Ash","m3",0.43693493743967399]
["Concrete","Reinforced Precast Concrete (CEM 1)","GEN 1 (8/10 MPa)- 0% Cement Replacement - Fly Ash","t",0.20986736430985342]
["Concrete","Reinforced Precast Concrete (CEM 1)","GEN 1 (8/10 MPa)- 0% Cement Replacement - Fly Ash","m3",0.50368167434364819]
["Concrete","Reinforced Precast Concrete (CEM 1)","GEN 2 (12/15 MPa)- 0% Cement Replacement - Fly Ash","t",0.21981080474907538]
["Concrete","Reinforced Precast Concrete (CEM 1)","GEN 2 (12/15 MPa)- 0% Cement Replacement - Fly Ash","m3",0.52754593139778094]
["Concrete","Reinforced Precast Concrete (CEM 1)","GEN 3 (16/20 MPa) - 0% Cement Replacement - Fly Ash","t",0.22874511134217551]
["Concrete","Reinforced Precast Concrete (CEM 1)","GEN 3 (16/20 MPa) - 0% Cement Replacement - Fly Ash","m3",0.54898826722122118]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 20/25 (20/25 MPa) - 0% Cement Replacement - Fly Ash","t",0.23806895301252262]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 20/25 (20/25 MPa) - 0% Cement Replacement - Fly Ash","m3",0.57136548723005431]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 25/30 (25/30 MPa) - 0% Cement Replacement - Fly Ash","t",0.24605626539266884]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 25/30 (25/30 MPa) - 0% Cement Replacement - Fly Ash","m3",0.59053503694240517]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 28/35 (28/35 MPa) - 0% Cement Replacement - Fly Ash","t",0.25401934402577692]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 28/35 (28/35 MPa) - 0% Cement Replacement - Fly Ash","m3",0.60964642566186455]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 32/40 (32/40 MPa) - 0% Cement Replacement - Fly Ash","t",0.26897261063830441]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 32/40 (32/40 MPa) - 0% Cement Replacement - Fly Ash","m3",0.64553426553193061]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 40/50 (40/50 Mpa) - 0% Cement Replacement - Fly Ash","t",0.29384953969440597]
["Concrete","Reinforced Precast Concrete (CEM 1)","RC 40/50 (40/50 Mpa) - 0% Cement Replacement - Fly Ash","m3",0.70523889526657435]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","t",0.17516211973138385]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","m3",0.42038908735532121]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","t",0.16737211120721324]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","m3",0.40169306689731177]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","t",0.19963478315111721]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement","m3",0.47912347956268131]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","t",0.18821116479253708]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","m3",0.45170679550208898]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","t",0.21061450307968016]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","m3",0.50547480739123241]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","t",0.19863569450347524]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement","m3",0.47672566680834055]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","t",0.21820320877484817]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","m3",0.52368770105963558]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","t",0.20557796640762488]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","m3",0.49338711937829971]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","t",0.22790536073859718]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","m3",0.54697286577263327]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","t",0.2136621877146565]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","m3",0.51278925051517554]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","t",0.23554369607804204]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","m3",0.56530487058730083]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","t",0.2206626330090819]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","m3",0.52959031922179656]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","t",0.24401120386270864]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","m3",0.58562688927050066]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","t",0.22974131044667401]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","m3",0.55137914507201757]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","t",0.25841036951716434]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","m3",0.62018488684119444]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","t",0.24229697668084266]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","m3",0.58151274403402231]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","t",0.28038915168252621]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","m3",0.67293396403806283]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","t",0.2610932023312077]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","m3",0.62662368559489845]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","t",0.1660708118684564]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 0 (6/8 MPa)- 15% Cement Replacement ","m3",0.39856994848429533]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","t",0.15100641618655281]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 0 (6/8 MPa) - 30% Cement Replacement ","m3",0.36241539884772672]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 1 (8/10 MPa)- 15% Cement Replacement","t",0.18595094491993841]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 1 (8/10 MPa)- 15% Cement Replacement","m3",0.44628226780785218]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","t",0.16387479256299597]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 1 (8/10 MPa) - 30% Cement Replacement ","m3",0.39329950215119031]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","t",0.19387832972862928]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 2 (12/15 MPa) - 15% Cement Replacement ","m3",0.46530799134871026]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 2 (12/15 MPa) - 30% Cement Replacement","t",0.17139179586746145]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 2 (12/15 MPa) - 30% Cement Replacement","m3",0.41134031008190747]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","t",0.20201571154261933]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 3 (16/20 MPa) - 15% Cement Replacement ","m3",0.48483770770228635]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","t",0.17567968901370179]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","GEN 3 (16/20 MPa) - 30% Cement Replacement ","m3",0.42163125363288428]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","t",0.21005135090427085]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ","m3",0.50412324217025006]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","t",0.18251069563190736]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ","m3",0.43802566951657768]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","t",0.21698175073618009]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ","m3",0.52075620176683224]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","t",0.18739493717604858]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ","m3",0.44974784922251654]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","t",0.22466342669428035]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ","m3",0.53919222406627287]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","t",0.19388522278282616]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ","m3",0.46532453467878276]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","t",0.23926532901613018]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 32/40 (32/40 MPa) - 15% Cement Replacement","m3",0.57423678963871239]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","t",0.20631952788639446]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ","m3",0.49516686692734668]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","t",0.25920197226662278]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ","m3",0.62208473343989468]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","t",0.22087805733476773]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ","m3",0.53010733760344253]
["Concrete","Concrete Blocks","Block - 8 MPa Compressive Strength","t",6.3E-2]
["Concrete","Concrete Blocks","Block - 8 MPa Compressive Strength","m3",6.93E-2]
["Concrete","Concrete Blocks","Block - 10 MPa","t",7.8E-2]
["Concrete","Concrete Blocks","Block - 10 MPa","m3",9.3600000000000003E-2]
["Concrete","Concrete Blocks","Block - 12 MPa","t",8.7999999999999995E-2]
["Concrete","Concrete Blocks","Block - 12 MPa","m3",0.1144]
["Concrete","Concrete Blocks","Block - 13 MPa","t",0.107]
["Concrete","Concrete Blocks","Block - 13 MPa","m3",0.14979999999999999]
["Concrete","Concrete Blocks","Autoclaved Aerated Blocks (AACs)","t",0.3075]
["Concrete","Concrete Blocks","Autoclaved Aerated Blocks (AACs)","m3",0.246]
["Concrete","Proportions Method (Cement:Sand:Aggregate)","1:1:2","t",0.20599999999999999]
["Concrete","Proportions Method (Cement:Sand:Aggregate)","1:1.5:3 ","t",0.155]
["Concrete","Proportions Method (Cement:Sand:Aggregate)","1:2:4","t",0.124]
["Concrete","Proportions Method (Cement:Sand:Aggregate)","1:2.5:5","t",0.104]
["Concrete","Proportions Method (Cement:Sand:Aggregate)","1:3:6 ","t",0.09]
["Concrete","Proportions Method (Cement:Sand:Aggregate)","1:4:8","t",7.3999999999999996E-2]
["Metal","Handrail","Galvanised with fittings","t",2.1999999999999999E-2]
["Metal","Handrail","Galvanised with fittings","m",2.6399999999999997E-4]
["Metal","Handrail","Stainless steel with fittings","t",8.5999999999999993E-2]
["Metal","Handrail","Stainless steel with fittings","m",1.0319999999999999E-3]
["Metal","Sheet Piling","Light Use","t",0.12]
["Metal","Sheet Piling","Light Use","m2",1.2E-2]
["Metal","Sheet Piling","Medium Use","t",0.15]
["Metal","Sheet Piling","Medium Use","m2",1.95E-2]
["Metal","Sheet Piling","Heavy Use","t",0.2]
["Metal","Sheet Piling","Heavy Use","m2",3.8000000000000006E-2]
["Metal","Flap Valves","DN 100 & DN 150","t",0.01]
["Metal","Flap Valves","DN 100 & DN 150","item",8.0000000000000007E-5]
["Metal","Flap Valves","DN 200 & DN 300","t",0.02]
["Metal","Flap Valves","DN 200 & DN 300","item",4.0000000000000002E-4]
["Metal","Flap Valves","DN 500","t",0.06]
["Metal","Flap Valves","DN 500","item",3.5999999999999999E-3]

{"sheet":"MaterialValidationList","index":14,"n_rows":307,"n_cols":10,"rows_kept":307,"cut":false,"hidden":true,"merged":[]}
["Material","Material Type",null,"Material",null,"Material Type","Material Description",null,"Material","MeasureUnit"]
["Aggregate","General (Gravel or Crushed Rock)",null,"Aggregate",null,"21-35% Fly Ash (CEM II/B-V)","N/A",null,"General (Gravel or Crushed Rock)","t"]
["Aggregate","Quarried Aggregate",null,"Aluminium",null,"21-35% GGBS (CEM II/B-S)","N/A",null,"General (Gravel or Crushed Rock)","m3"]
["Aggregate","Recycled Aggregate",null,"Asphalt",null,"36-65% GGBS (CEM III/A)","N/A",null,"Quarried Aggregate","t"]
["Aggregate","Marine Aggregate",null,"Bricks",null,"6-20% Fly Ash (CEM II/A-V)","N/A",null,"Quarried Aggregate","m3"]
["Aluminium","General (Aluminium)",null,"Cement",null,"66-80% GGBS (CEM III/B)","N/A",null,"Recycled Aggregate","t"]
["Asphalt","General ",null,"Clay",null,"Asphalt road - Cold construction method ","Construction",null,"Recycled Aggregate","m3"]
["Asphalt","Asphalt, 4% (bitumen) binder content (by mass)",null,"Concrete",null,"Asphalt road - Hot construction method ","Construction",null,"Marine Aggregate","t"]
["Asphalt","Asphalt, 5% binder content",null,"Copper",null,"Asphalt, 4% (bitumen) binder content (by mass)","N/A",null,"Marine Aggregate","m3"]
["Asphalt","Asphalt, 6% binder content",null,"Glass",null,"Asphalt, 5% binder content","N/A",null,"General (Aluminium)","t"]
["Asphalt","Asphalt, 7% binder content",null,"Insulation",null,"Asphalt, 6% binder content","N/A",null,"General (Aluminium)","m3"]
["Asphalt","Asphalt, 8% binder content",null,"Iron",null,"Asphalt, 7% binder content","N/A",null,"General ","t"]
["Bricks","General (Bricks)",null,"Lead",null,"Asphalt, 8% binder content","N/A",null,"General ","m3"]
["Cement","Average CEM I Portland Cement, 94% Clinker",null,"Lime",null,"Average CEM I Portland Cement, 94% Clinker","N/A",null,"Asphalt, 4% (bitumen) binder content (by mass)","t"]
["Cement","Ground Granulated Blastfurnace Slag (GGBS)",null,"Metal",null,"Bar & Rod - UK (EU) Average Recycled Content","N/A",null,"Asphalt, 4% (bitumen) binder content (by mass)","m3"]
["Cement","Fly Ash",null,"Miscellaneous",null,"Blastfurnace Cement","CEM III/A (65% GGBS)",null,"Asphalt, 5% binder content","t"]
["Cement","Portland Limestone Cement",null,"Paint",null,"Blastfurnace Cement","CEM III/A (50.5% GGBS)",null,"Asphalt, 5% binder content","m3"]
["Cement","Portland Fly Ash Cement",null,"Plaster",null,"Blastfurnace Cement","CEM III/A (36% GGBS)",null,"Asphalt, 6% binder content","t"]
["Cement","Portland Slag Cement",null,"Plastics",null,"Blastfurnace Cement","CEM III/A (80% GGBS)",null,"Asphalt, 6% binder content","m3"]
["Cement","Blastfurnace Cement",null,"Roads",null,"Blastfurnace Cement","CEM III/A (73% GGBS)",null,"Asphalt, 7% binder content","t"]
["Cement","Pozzolanic (Siliceous Fly Ash) Cement",null,"Sand",null,"Blastfurnace Cement","CEM III/A (66% GGBS)",null,"Asphalt, 7% binder content","m3"]
["Cement","General",null,"Soil/Clay",null,"Cement stabilised soil @ 5%","N/A",null,"Asphalt, 8% binder content","t"]
["Cement","6-20% Fly Ash (CEM II/A-V)",null,"Steel",null,"Cement stabilised soil @ 8%","N/A",null,"Asphalt, 8% binder content","m3"]
["Cement","21-35% Fly Ash (CEM II/B-V)",null,"Stone",null,"Coil (Sheet) - Galvanised - UK (EU) Average Recycled Content","N/A",null,"General (Bricks)","t"]
["Cement","21-35% GGBS (CEM II/B-S)",null,"Timber",null,"Coil (Sheet) - UK (EU) Average Recycled Content","N/A",null,"General (Bricks)","m3"]
["Cement","36-65% GGBS (CEM III/A)",null,"Zinc",null,"Concrete Blocks","Block - 8 MPa Compressive Strength",null,"Average CEM I Portland Cement, 94% Clinker","t"]
["Cement","66-80% GGBS (CEM III/B)",null,null,null,"Concrete Blocks","Block - 10 MPa",null,"Average CEM I Portland Cement, 94% Clinker","m3"]
["Cement","Cement stabilised soil @ 5%",null,null,null,"Concrete Blocks","Block - 12 MPa",null,"Ground Granulated Blastfurnace Slag (GGBS)","t"]
["Cement","Cement stabilised soil @ 8%",null,null,null,"Concrete Blocks","Block - 13 MPa",null,"Ground Granulated Blastfurnace Slag (GGBS)","m3"]
["Cement","GGBS stabilised soil",null,null,null,"Concrete Blocks","Autoclaved Aerated Blocks (AACs)",null,"Fly Ash","t"]
["Cement","Fly ash stabilised soil",null,null,null,"Damp Proof Course/Membrane","N/A",null,"Fly Ash","m3"]
["Clay","Vitrified clay pipe DN 100 & DN 150",null,null,null,"Engineering Steel - Recycled","N/A",null,"Portland Limestone Cement","t"]
["Clay","Vitrified clay pipe DN 200 & DN 300",null,null,null,"EU Tube & Sheet","General",null,"Portland Limestone Cement","m3"]
["Clay","Vitrified clay pipe DN 500",null,null,null,"EU Tube & Sheet","Virgin",null,"Portland Fly Ash Cement","t"]
["Copper","EU Tube & Sheet",null,null,null,"EU Tube & Sheet","Recycled",null,"Portland Fly Ash Cement","m3"]
["Copper","Reused ",null,null,null,"Flap Valves","DN 100 & DN 150",null,"Portland Slag Cement","t"]
["Insulation","General Insulation",null,null,null,"Flap Valves","DN 200 & DN 300",null,"Portland Slag Cement","m3"]
["Iron","General (Iron)",null,null,null,"Flap Valves","DN 500",null,"Blastfurnace Cement","t"]
["Lead","General (Lead)",null,null,null,"Fly Ash","N/A",null,"Blastfurnace Cement","m3"]
["Lime","General (Lime)",null,null,null,"Fly ash stabilised soil","N/A",null,"Pozzolanic (Siliceous Fly Ash) Cement","t"]
["Miscellaneous","Damp Proof Course/Membrane",null,null,null,"General","N/A",null,"Pozzolanic (Siliceous Fly Ash) Cement","m3"]
["Miscellaneous","Grit",null,null,null,"General","N/A",null,"General","t"]
["Miscellaneous","Ground Limestone",null,null,null,"General ","N/A",null,"General","m3"]
["Miscellaneous","Glass Reinforced Plastic - GRP - Fibreglass",null,null,null,"General - UK (EU) Average Recycled Content","N/A",null,"6-20% Fly Ash (CEM II/A-V)","t"]
["Paint","General (Paint)",null,null,null,"General (Aluminium)","General",null,"6-20% Fly Ash (CEM II/A-V)","m3"]
["Plaster","General (Gypsum)",null,null,null,"General (Aluminium)","Virgin",null,"21-35% Fly Ash (CEM II/B-V)","t"]
["Plaster","Plasterboard",null,null,null,"General (Aluminium)","Recycled",null,"21-35% Fly Ash (CEM II/B-V)","m3"]
["Plastics","General (Plastics)",null,null,null,"General (Bricks)","N/A",null,"21-35% GGBS (CEM II/B-S)","t"]
["Plastics","General Polyethylene",null,null,null,"General (Bricks)","Per Single Brick",null,"21-35% GGBS (CEM II/B-S)","m3"]
["Plastics","HDPE Pipe",null,null,null,"General (Gravel or Crushed Rock)","N/A",null,"36-65% GGBS (CEM III/A)","t"]
["Plastics","PVC General",null,null,null,"General (Gypsum)","N/A",null,"36-65% GGBS (CEM III/A)","m3"]
["Plastics","PVC Pipe",null,null,null,"General (Iron)","N/A",null,"66-80% GGBS (CEM III/B)","t"]
["Sand","General (Sand)",null,null,null,"General (Lead)","General",null,"66-80% GGBS (CEM III/B)","m3"]
["Soil/Clay","General (Rammed Soil)",null,null,null,"General (Lead)","Virgin",null,"Cement stabilised soil @ 5%","t"]
["Stone","General (Stone)",null,null,null,"General (Lead)","Recycled",null,"Cement stabilised soil @ 5%","m3"]
["Stone","Granite",null,null,null,"General (Lime)","N/A",null,"Cement stabilised soil @ 8%","t"]
["Stone","Limestone",null,null,null,"General (Paint)","N/A",null,"Cement stabilised soil @ 8%","m3"]
["Stone","Marble",null,null,null,"General (Plastics)","N/A",null,"GGBS stabilised soil","t"]
["Stone","Sandstone",null,null,null,"General (Rammed Soil)","N/A",null,"GGBS stabilised soil","m3"]
["Stone","Slate",null,null,null,"General (Sand)","N/A",null,"Fly ash stabilised soil","t"]
["Stone","Shale",null,null,null,"General (Stone)","N/A",null,"Fly ash stabilised soil","m3"]
["Timber","General (Timber)",null,null,null,"General (Timber)","N/A",null,"Vitrified clay pipe DN 100 & DN 150","t"]
["Timber","Glue Laminated timber ",null,null,null,"General (Zinc)","N/A",null,"Vitrified clay pipe DN 100 & DN 150","m3"]
["Timber","Hardboard",null,null,null,"General Insulation","N/A",null,"Vitrified clay pipe DN 200 & DN 300","t"]
["Timber","MDF",null,null,null,"General Polyethylene","N/A",null,"Vitrified clay pipe DN 200 & DN 300","m3"]
["Timber","Plywood",null,null,null,"GGBS stabilised soil","N/A",null,"Vitrified clay pipe DN 500","t"]
["Timber","Reclaimed Timber",null,null,null,"Glass Reinforced Plastic - GRP - Fibreglass","N/A",null,"Vitrified clay pipe DN 500","m3"]
["Zinc","General (Zinc)",null,null,null,"Glue Laminated timber ","N/A",null,"EU Tube & Sheet","t"]
["Zinc","Virgin",null,null,null,"Granite","N/A",null,"EU Tube & Sheet","m3"]
["Zinc","Recycled",null,null,null,"Grit","N/A",null,"Reused ","t"]
["Roads","Asphalt road - Hot construction method ",null,null,null,"Ground Granulated Blastfurnace Slag (GGBS)","N/A",null,"Reused ","m3"]
["Roads","Asphalt road - Cold construction method ",null,null,null,"Ground Limestone","N/A",null,"General Insulation","t"]
["Steel","General - UK (EU) Average Recycled Content",null,null,null,"Handrail","Galvanised with fittings",null,"General Insulation","m3"]
["Steel","Bar & Rod - UK (EU) Average Recycled Content",null,null,null,"Handrail","Stainless steel with fittings",null,"General (Iron)","t"]
["Steel","Coil (Sheet) - UK (EU) Average Recycled Content",null,null,null,"Hardboard","N/A",null,"General (Iron)","m3"]
["Steel","Coil (Sheet) - Galvanised - UK (EU) Average Recycled Content",null,null,null,"HDPE Pipe","N/A",null,"General (Lead)","t"]
["Steel","Engineering Steel - Recycled",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ",null,"General (Lead)","m3"]
["Steel","Pipe - UK (EU) Average Recycled Content",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ",null,"General (Lime)","t"]
["Steel","Plate - UK (EU) Average Recycled Content",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement",null,"General (Lime)","m3"]
["Steel","Stainless",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ",null,"Damp Proof Course/Membrane","t"]
["Concrete","In-situ Concrete (General)",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ",null,"Damp Proof Course/Membrane","m2"]
["Concrete","In-situ Concrete (CEM 1)",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ",null,"Grit","t"]
["Concrete","In-situ Concrete (Fly Ash Replacement)",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ",null,"Grit","m3"]
["Concrete","In-situ Concrete (Blast Furnace Slag Replacement)",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement",null,"Ground Limestone","t"]
["Concrete","Reinforced In-situ Concrete (General)",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ",null,"Ground Limestone","m3"]
["Concrete","Reinforced In-situ Concrete (CEM 1)",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ",null,"Glass Reinforced Plastic - GRP - Fibreglass","t"]
["Concrete","Reinforced In-situ Concrete (Fly Ash Replacement)",null,null,null,"In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ",null,"Glass Reinforced Plastic - GRP - Fibreglass","m3"]
["Concrete","Reinforced In-situ Concrete (Blast Furnace Slag Replacement)",null,null,null,"In-situ Concrete (CEM 1)","GEN 0 (6/8 MPa)",null,"General (Paint)","t"]
["Concrete","Precast Concrete (General)",null,null,null,"In-situ Concrete (CEM 1)","GEN 2 (12/15 MPa) ",null,"General (Paint)","m3"]
["Concrete","Precast Concrete (CEM 1)",null,null,null,"In-situ Concrete (CEM 1)","RC 20/25 (20/25 MPa) ",null,"General (Gypsum)","t"]
["Concrete","Precast Concrete (Fly Ash Replacement)",null,null,null,"In-situ Concrete (CEM 1)","RC 28/35 (28/35 MPa) ",null,"General (Gypsum)","m3"]
["Concrete","Precast Concrete (Blast Furnace Slag Replacement)",null,null,null,"In-situ Concrete (CEM 1)","RC 40/50 (40/50 Mpa)",null,"Plasterboard","t"]
["Concrete","Reinforced Precast Concrete (General)",null,null,null,"In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ",null,"Plasterboard","m3"]
["Concrete","Reinforced Precast Concrete (CEM 1)",null,null,null,"In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ",null,"General (Plastics)","t"]
["Concrete","Reinforced Precast Concrete (Fly Ash Replacement)",null,null,null,"In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement",null,"General (Plastics)","m3"]
["Concrete","Reinforced Precast Concrete (Blast Furnace Slag)",null,null,null,"In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ",null,"General Polyethylene","t"]
["Concrete","Concrete Blocks",null,null,null,"In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ",null,"General Polyethylene","m3"]
["Concrete","Proportions Method (Cement:Sand:Aggregate)",null,null,null,"In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ",null,"HDPE Pipe","t"]
["Metal","Handrail",null,null,null,"In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ",null,"HDPE Pipe","m3"]
["Metal","Sheet Piling",null,null,null,"In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ",null,"PVC General","t"]
["Metal","Flap Valves",null,null,null,"In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ",null,"PVC General","m3"]
[null,null,null,null,null,"In-situ Concrete (General)","16/20 Mpa",null,"PVC Pipe","t"]
[null,null,null,null,null,"In-situ Concrete (General)","25/30 MPa",null,"PVC Pipe","m3"]
[null,null,null,null,null,"In-situ Concrete (General)","32/40 MPa",null,"General (Sand)","t"]
[null,null,null,null,null,"Limestone","N/A",null,"General (Sand)","m3"]
[null,null,null,null,null,"Marine Aggregate","N/A",null,"General (Rammed Soil)","t"]
[null,null,null,null,null,"MDF","N/A",null,"General (Rammed Soil)","m3"]
[null,null,null,null,null,"Pipe - UK (EU) Average Recycled Content","N/A",null,"General (Stone)","t"]
[null,null,null,null,null,"Plasterboard","N/A",null,"General (Stone)","m3"]
[null,null,null,null,null,"Plate - UK (EU) Average Recycled Content","N/A",null,"Granite","t"]
[null,null,null,null,null,"Plywood","N/A",null,"Granite","m3"]
[null,null,null,null,null,"Portland Fly Ash Cement","CEM II/A-V (20% Fly Ash)",null,"Limestone","t"]
[null,null,null,null,null,"Portland Fly Ash Cement","CEM II/A-V (13% Fly Ash)",null,"Limestone","m3"]
[null,null,null,null,null,"Portland Fly Ash Cement","CEM II/A-V (6% Fly Ash)",null,"Marble","t"]
[null,null,null,null,null,"Portland Fly Ash Cement","CEM II/A-V (35% Fly Ash)",null,"Sandstone","t"]
[null,null,null,null,null,"Portland Fly Ash Cement","CEM II/A-V (28% Fly Ash)",null,"Sandstone","m3"]
[null,null,null,null,null,"Portland Fly Ash Cement","CEM II/A-V (21% Fly Ash)",null,"Slate","t"]
[null,null,null,null,null,"Portland Limestone Cement","CEM II/A-LL or L (20% limestone)",null,"Slate","m3"]
[null,null,null,null,null,"Portland Limestone Cement","CEM II/A-LL or L (13% limestone)",null,"Shale","t"]
[null,null,null,null,null,"Portland Limestone Cement","CEM II/A-LL or L (6% limestone)",null,"Shale","m3"]
[null,null,null,null,null,"Portland Slag Cement","CEM II/B-S (35% GGBS)",null,"General (Timber)","t"]
[null,null,null,null,null,"Portland Slag Cement","CEM II/B-S (28% GGBS)",null,"General (Timber)","m3"]
[null,null,null,null,null,"Portland Slag Cement","CEM II/B-S (21% GGBS)",null,"Glue Laminated timber ","t"]
[null,null,null,null,null,"Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (55% GGBS)",null,"Glue Laminated timber ","m3"]
[null,null,null,null,null,"Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (45.5% GGBS)",null,"Hardboard","t"]
[null,null,null,null,null,"Pozzolanic (Siliceous Fly Ash) Cement","CEM IV/B-V (36% GGBS)",null,"Hardboard","m3"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ",null,"MDF","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ",null,"MDF","m2"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement",null,"Plywood","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ",null,"Plywood","m2"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ",null,"Reclaimed Timber","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement",null,"Reclaimed Timber","m3"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ",null,"General (Zinc)","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ",null,"Virgin","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ",null,"Recycled","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ",null,"Asphalt road - Hot construction method ","m2"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ",null,"Asphalt road - Cold construction method ","m2"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ",null,"General - UK (EU) Average Recycled Content","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ",null,"General - UK (EU) Average Recycled Content","m3"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ",null,"Bar & Rod - UK (EU) Average Recycled Content","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement",null,"Bar & Rod - UK (EU) Average Recycled Content","m3"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ",null,"Coil (Sheet) - UK (EU) Average Recycled Content","t"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ",null,"Coil (Sheet) - UK (EU) Average Recycled Content","m3"]
[null,null,null,null,null,"Precast Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ",null,"Coil (Sheet) - Galvanised - UK (EU) Average Recycled Content","t"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","GEN 0 (6/8 MPa)",null,"Coil (Sheet) - Galvanised - UK (EU) Average Recycled Content","m3"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","GEN 1 (8/10 MPa) ",null,"Engineering Steel - Recycled","t"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","GEN 2 (12/15 MPa) ",null,"Engineering Steel - Recycled","m3"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","GEN 3 (16/20 MPa) ",null,"Pipe - UK (EU) Average Recycled Content","t"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","RC 20/25 (20/25 MPa) ",null,"Pipe - UK (EU) Average Recycled Content","m3"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","RC 25/30 (25/30 MPa) ",null,"Plate - UK (EU) Average Recycled Content","t"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","RC 28/35 (28/35 MPa) ",null,"Plate - UK (EU) Average Recycled Content","m3"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","RC 32/40 (32/40 MPa)",null,"Stainless","t"]
[null,null,null,null,null,"Precast Concrete (CEM 1)","RC 40/50 (40/50 Mpa)",null,"Stainless","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ",null,"In-situ Concrete (General)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ",null,"In-situ Concrete (General)","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement",null,"In-situ Concrete (CEM 1)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ",null,"In-situ Concrete (CEM 1)","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement ",null,"In-situ Concrete (Fly Ash Replacement)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement",null,"In-situ Concrete (Fly Ash Replacement)","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement ",null,"In-situ Concrete (Blast Furnace Slag Replacement)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement ",null,"In-situ Concrete (Blast Furnace Slag Replacement)","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement ",null,"Reinforced In-situ Concrete (General)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement ",null,"Reinforced In-situ Concrete (General)","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement ",null,"Reinforced In-situ Concrete (CEM 1)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement ",null,"Reinforced In-situ Concrete (CEM 1)","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement ",null,"Reinforced In-situ Concrete (Fly Ash Replacement)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement ",null,"Reinforced In-situ Concrete (Fly Ash Replacement)","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement",null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement ",null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","m3"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement ",null,"Precast Concrete (General)","t"]
[null,null,null,null,null,"Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement ",null,"Precast Concrete (General)","m3"]
[null,null,null,null,null,"Precast Concrete (General)","General",null,"Precast Concrete (CEM 1)","t"]
[null,null,null,null,null,"Precast Concrete (General)","16/20 Mpa",null,"Precast Concrete (CEM 1)","m3"]
[null,null,null,null,null,"Precast Concrete (General)","20/25 MPa",null,"Precast Concrete (Fly Ash Replacement)","t"]
[null,null,null,null,null,"Precast Concrete (General)","25/30 MPa",null,"Precast Concrete (Fly Ash Replacement)","m3"]
[null,null,null,null,null,"Precast Concrete (General)","28/35 MPa",null,"Precast Concrete (Blast Furnace Slag Replacement)","t"]
[null,null,null,null,null,"Precast Concrete (General)","32/40 MPa",null,"Precast Concrete (Blast Furnace Slag Replacement)","m3"]
[null,null,null,null,null,"Precast Concrete (General)","40/50 MPa",null,"Reinforced Precast Concrete (General)","t"]
[null,null,null,null,null,"Proportions Method (Cement:Sand:Aggregate)","1:1:2",null,"Reinforced Precast Concrete (General)","m3"]
[null,null,null,null,null,"Proportions Method (Cement:Sand:Aggregate)","1:1.5:3 ",null,"Reinforced Precast Concrete (CEM 1)","t"]
[null,null,null,null,null,"Proportions Method (Cement:Sand:Aggregate)","1:2:4",null,"Reinforced Precast Concrete (CEM 1)","m3"]
[null,null,null,null,null,"Proportions Method (Cement:Sand:Aggregate)","1:2.5:5",null,"Reinforced Precast Concrete (Fly Ash Replacement)","t"]
[null,null,null,null,null,"Proportions Method (Cement:Sand:Aggregate)","1:3:6 ",null,"Reinforced Precast Concrete (Fly Ash Replacement)","m3"]
[null,null,null,null,null,"Proportions Method (Cement:Sand:Aggregate)","1:4:8 ",null,"Reinforced Precast Concrete (Blast Furnace Slag)","t"]
[null,null,null,null,null,"PVC General","N/A",null,"Reinforced Precast Concrete (Blast Furnace Slag)","m3"]
[null,null,null,null,null,"PVC Pipe","N/A",null,"Concrete Blocks","t"]
[null,null,null,null,null,"Quarried Aggregate","N/A",null,"Concrete Blocks","m3"]
[null,null,null,null,null,"Reclaimed Timber","N/A",null,"Proportions Method (Cement:Sand:Aggregate)","t"]
[null,null,null,null,null,"Recycled","N/A",null,"Handrail","t"]
[null,null,null,null,null,"Recycled Aggregate","N/A",null,"Handrail","m"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement ",null,"Sheet Piling","t"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement ",null,"Sheet Piling","m2"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement",null,"Flap Valves","t"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement ",null,"Flap Valves","item"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Blast Furnace Slag Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","GEN 0 (6/8 MPa)"]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","GEN 1 (8/10 MPa) "]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","GEN 2 (12/15 MPa) "]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","GEN 3 (16/20 MPa) "]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","RC 20/25 (20/25 MPa) "]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","RC 25/30 (25/30 MPa) "]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","RC 28/35 (28/35 MPa) "]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","RC 32/40 (32/40 MPa)"]
[null,null,null,null,null,"Reinforced In-situ Concrete (CEM 1)","RC 40/50 (40/50 Mpa)"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement"]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced In-situ Concrete (General)","General"]
[null,null,null,null,null,"Reinforced In-situ Concrete (General)","16/20 Mpa"]
[null,null,null,null,null,"Reinforced In-situ Concrete (General)","20/25 MPa"]
[null,null,null,null,null,"Reinforced In-situ Concrete (General)","25/30 MPa"]
[null,null,null,null,null,"Reinforced In-situ Concrete (General)","28/35 MPa"]
[null,null,null,null,null,"Reinforced In-situ Concrete (General)","32/40 MPa"]
[null,null,null,null,null,"Reinforced In-situ Concrete (General)","40/50 MPa"]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","GEN 0 (6/8 MPa)- 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","GEN 0 (6/8 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","GEN 1 (8/10 MPa)- 15% Cement Replacement"]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","GEN 1 (8/10 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","GEN 2 (12/15 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","GEN 2 (12/15 MPa) - 30% Cement Replacement"]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","GEN 3 (16/20 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","GEN 3 (16/20 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 20/25 (20/25 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 20/25 (20/25 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 25/30 (25/30 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 25/30 (25/30 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 28/35 (28/35 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 28/35 (28/35 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 32/40 (32/40 MPa) - 15% Cement Replacement"]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 32/40 (32/40 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 40/50 (40/50 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Blast Furnace Slag)","RC 40/50 (40/50 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","GEN 0 (6/8 MPa)- 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","GEN 1 (8/10 MPa)- 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","GEN 2 (12/15 MPa)- 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","GEN 3 (16/20 MPa) - 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","RC 20/25 (20/25 MPa) - 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","RC 25/30 (25/30 MPa) - 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","RC 28/35 (28/35 MPa) - 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","RC 32/40 (32/40 MPa) - 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (CEM 1)","RC 40/50 (40/50 Mpa) - 0% Cement Replacement - Fly Ash"]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa)- 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","GEN 0 (6/8 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa)- 15% Cement Replacement"]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","GEN 1 (8/10 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","GEN 2 (12/15 MPa) - 30% Cement Replacement"]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","GEN 3 (16/20 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 20/25 (20/25 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 25/30 (25/30 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 28/35 (28/35 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 15% Cement Replacement"]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 32/40 (32/40 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 15% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (Fly Ash Replacement)","RC 40/50 (40/50 MPa) - 30% Cement Replacement "]
[null,null,null,null,null,"Reinforced Precast Concrete (General)","General"]
[null,null,null,null,null,"Reinforced Precast Concrete (General)","16/20 Mpa"]
[null,null,null,null,null,"Reinforced Precast Concrete (General)","20/25 MPa"]
[null,null,null,null,null,"Reinforced Precast Concrete (General)","25/30 MPa"]
[null,null,null,null,null,"Reinforced Precast Concrete (General)","28/35 MPa"]
[null,null,null,null,null,"Reinforced Precast Concrete (General)","32/40 MPa"]
[null,null,null,null,null,"Reinforced Precast Concrete (General)","40/50 MPa"]
[null,null,null,null,null,"Reused ","N/A"]
[null,null,null,null,null,"Reused ","N/A"]
[null,null,null,null,null,"Sandstone","N/A"]
[null,null,null,null,null,"Shale","N/A"]
[null,null,null,null,null,"Sheet Piling","Light Use"]
[null,null,null,null,null,"Sheet Piling","Medium Use"]
[null,null,null,null,null,"Sheet Piling","Heavy Use"]
[null,null,null,null,null,"Slate","N/A"]
[null,null,null,null,null,"Stainless","N/A"]
[null,null,null,null,null,"Virgin","N/A"]
[null,null,null,null,null,"Vitrified clay pipe DN 100 & DN 150","N/A"]
[null,null,null,null,null,"Vitrified clay pipe DN 200 & DN 300","N/A"]
[null,null,null,null,null,"Vitrified clay pipe DN 500","N/A"]

{"sheet":"PlantList","index":15,"n_rows":60,"n_cols":11,"rows_kept":60,"cut":false,"hidden":true,"merged":[]}
["Plant",null,"Plant","Plant Item","Consumption of fuel (l/hr)","Utilization Factor","litre / hr","CO2e / hr [Combustion]","CO2e / hr [WTT]","Total CO2e / hr","Reference"]
["Tractor",null,"Tractor","68 - 116 hp",9,0.75,6.75,1.8016719144750001E-2,3.9534749999999997E-3,2.1970194144750002E-2,"SPONS 2014"]
["Asphalt Paver",null,"Asphalt Paver","24KW Engine",6.2,0.8,4.9600000000000009,1.3238952141920002E-2,2.9050720000000003E-3,1.6144024141920003E-2,"SPONS Civils 2009"]
["Asphalt Equipment ",null,"Asphalt Paver","35KW Engine",8.1999999999999993,0.8,6.56,1.750958186512E-2,3.8421919999999995E-3,2.1351773865120001E-2,"SPONS Civils 2009"]
["Compactor plate",null,"Asphalt Paver","80KW Engine",17,0.8,13.600000000000001,3.6300352647200003E-2,7.9655200000000002E-3,4.4265872647200007E-2,"SPONS Civils 2009"]
["Compressor",null,"Asphalt Equipment ","Paver - Bitelli BB650",16,0.65,10.4,2.77590932008E-2,6.0912800000000001E-3,3.3850373200800005E-2,"SPONS 2014"]
["Concrete Equipment",null,"Asphalt Equipment ","Macadam Laying Machine",30,0.65,19.5,5.20482997515E-2,1.142115E-2,6.3469449751499998E-2,"SPONS 2006"]
["Mixer",null,"Compactor plate","64kg",0.9,0.75,0.67500000000000004,1.8016719144750002E-3,3.953475E-4,2.1970194144750005E-3,"SPONS Civils 2009"]
["Crane",null,"Compactor plate","140kg",0.8,0.75,0.60000000000000009,1.6014861462000003E-3,3.5142000000000002E-4,1.9529061462000004E-3,"SPONS Civils 2009"]
["Generator",null,"Compactor plate","180kg",1.2,0.75,0.89999999999999991,2.4022292192999997E-3,5.2712999999999989E-4,2.9293592192999999E-3,"SPONS Civils 2009"]
["Excavators",null,"Compactor plate","345kg",0.9,0.75,0.67500000000000004,1.8016719144750002E-3,3.953475E-4,2.1970194144750005E-3,"SPONS Civils 2009"]
["Piling Plant",null,"Compressor","3.5 m3/min",5.9,0.85,5.0150000000000006,1.3385755038655002E-2,2.9372855000000002E-3,1.6323040538655003E-2,"SPONS Civils 2009"]
["Rollers",null,"Compressor","10 m3/min",18,0.85,15.299999999999999,4.0837896728099995E-2,8.961209999999999E-3,4.97991067281E-2,"SPONS Civils 2009"]
["Dozers",null,"Compressor","Tractor mounted",9,0.85,7.6499999999999995,2.0418948364049998E-2,4.4806049999999995E-3,2.489955336405E-2,"SPONS Civils 2009"]
["Loaders",null,"Concrete Equipment","Poker Vibrators",1.5,0.75,1.125,3.0027865241249998E-3,6.5891249999999995E-4,3.6616990241250002E-3,"SPONS Civils 2009"]
["Scrapers",null,"Concrete Equipment","Tamper and screeder",1,0.75,0.75]
["Skidsteer ",null,"Mixer","5/3.5",1.2,0.75,0.89999999999999991,2.4022292192999997E-3,5.2712999999999989E-4,2.9293592192999999E-3,"SPONS 2014"]
["Graders",null,"Mixer","Truck Mixer 6m3",14,0.75,10.5,2.8026007558499998E-2,6.1498500000000001E-3,3.41758575585E-2,"SPONS Civils 2009"]
["Dumpers",null,"Crane","Mobile - 15 t",5.0999999999999996,0.5,2.5499999999999998,6.8063161213499992E-3,1.4935349999999998E-3,8.2998511213499999E-3,"SPONS 2014"]
["Pumps",null,"Crane","Mobile - 40 t",6.3,0.5,3.15,8.4078022675500002E-3,1.8449549999999999E-3,1.0252757267550001E-2]
["Access Platforms",null,"Crane","Crawler - 30 - 50t",3.5,0.25,0.875,2.3355006298750002E-3,5.1248750000000001E-4,2.8479881298750002E-3,"SPONS 2006"]
["Road Vehicles",null,"Generator","4 kVA",1.6,null,null,null,null,null,"SPONS 2014"]
["Small Plant",null,"Generator","25 kVA",4.9000000000000004,null,null,null,null,null,"SPONS 2014"]
[null,null,"Excavators","Mini Digger <6 ton",5,0.75,3.75,1.0009288413749999E-2,2.196375E-3,1.2205663413750002E-2,"SPONS 2014"]
[null,null,"Excavators","Hydraulic Crawler Backacter - 3.5t",4,0.8,3.2,8.541259446400001E-3,1.8742400000000001E-3,1.0415499446400002E-2,"SPONS Civils 2009"]
[null,null,"Excavators","Hydraulic Crawler Backacter - 11.5t",9.5,0.8,7.6000000000000005,2.02854911852E-2,4.4513199999999999E-3,2.4736811185200002E-2,"SPONS Civils 2009"]
[null,null,"Excavators","Hydraulic Crawler Backacter - 23.5t",19,0.8,15.200000000000001,4.0570982370400001E-2,8.9026399999999999E-3,4.9473622370400004E-2,"SPONS Civils 2009"]
[null,null,"Excavators","Hydraulic Crawler Backacter - 60t",52,0.8,41.6,0.1110363728032,2.4365120000000001E-2,0.13540149280320002,"SPONS Civils 2009"]
[null,null,"Piling Plant","Pilling Hammer - 1,500 kg",6,0.75,4.5,1.2011146096499999E-2,2.6356499999999998E-3,1.4646796096500001E-2,"SPONS Civils 2009"]
[null,null,"Piling Plant","Pilling Hammer - 5,000 kg",16,0.75,12,3.2029722923999998E-2,7.0283999999999998E-3,3.9058122924000002E-2,"SPONS Civils 2009"]
[null,null,"Piling Plant","Pilling Hammer - 10,000 kg",35,0.75,26.25,7.0065018896249998E-2,1.5374624999999999E-2,8.543964389625E-2,"SPONS Civils 2009"]
[null,null,"Piling Plant","Piling Extractor",20,0.75,15,4.0037153654999998E-2,8.7854999999999999E-3,4.8822653655000006E-2,"SPONS Civils 2009"]
[null,null,"Rollers","BW 90 AD",2,0.75,1.5,4.0037153654999998E-3,8.7854999999999997E-4,4.8822653655000003E-3,"SPONS 2014"]
[null,null,"Rollers","BW 120 AD",4.4000000000000004,0.75,3.3000000000000003,8.8081738041000009E-3,1.9328100000000001E-3,1.0740983804100001E-2,"SPONS 2014"]
[null,null,"Rollers","BW6 (towed)",7.6,0.75,5.6999999999999993,1.5214118388899998E-2,3.3384899999999995E-3,1.8552608388899997E-2,"SPONS 2014"]
[null,null,"Dozers","CAT D6N",21,0.8,16.8,4.4841612093599999E-2,9.8397599999999995E-3,5.4681372093600009E-2,"SPONS 2014"]
[null,null,"Dozers","CAT D8T",38,0.8,30.400000000000002,8.1141964740800002E-2,1.780528E-2,9.8947244740800008E-2,"SPONS 2014"]
[null,null,"Dozers","Skid Steer Loaders",3.5,0.75,2.625,7.0065018896249996E-3,1.5374625E-3,8.543964389625E-3,"SPONS Civils 2009"]
[null,null,"Loaders","CAT 953C",18,0.75,13.5,3.6033438289500001E-2,7.9069499999999994E-3,4.3940388289500004E-2,"SPONS 2014"]
[null,null,"Scrapers","CAT 621G",41.5,0.8,33.200000000000003,8.8615566756400005E-2,1.9445240000000003E-2,0.10806080675640002,"SPONS 2014"]
[null,null,"Scrapers","CAT 657E",125,0.8,100,0.26691435769999999,5.8569999999999997E-2,0.3254843577,"SPONS 2014"]
[null,null,"Skidsteer ","Bobcat 553",3.4,0.75,2.5499999999999998,6.8063161213499992E-3,1.4935349999999998E-3,8.2998511213499999E-3,"SPONS 2014"]
[null,null,"Graders","CAT 140H",19,0.75,14.25,3.8035295972249999E-2,8.3462250000000005E-3,4.6381520972250005E-2,"SPONS 2014"]
[null,null,"Dumpers","2 tonne",3,0.75,2.25,6.0055730482499996E-3,1.3178249999999999E-3,7.3233980482500004E-3,"SPONS 2014"]
[null,null,"Dumpers","Volvo A25D",17,0.75,12.75,3.4031580606750003E-2,7.467675E-3,4.1499255606750003E-2,"SPONS 2014"]
[null,null,"Dumpers","36 tonne",25,0.75,18.75,5.0046442068750002E-2,1.0981875E-2,6.1028317068750004E-2,"SPONS 2014"]
[null,null,"Pumps","75 mm 65 m3/hr",1.1000000000000001,null,null,null,null,null,"SPONS 2014"]
[null,null,"Pumps","150mm 360 m3/hr",4.2,null,null,null,null,null,"SPONS 2014"]
[null,null,"Access Platforms","Telescopic 14m",2,0.5,1,2.669143577E-3,5.8569999999999998E-4,3.2548435770000002E-3,"SPONS 2006"]
[null,null,"Access Platforms","Scissor Type - 8m",1.5,0.5,0.75,2.0018576827499999E-3,4.3927499999999998E-4,2.4411326827500001E-3,"SPONS Civils 2009"]
[null,null,"Access Platforms","Vehicle Mounted - 12m",2,0.5,1,2.669143577E-3,5.8569999999999998E-4,3.2548435770000002E-3,"SPONS Civils 2009"]
[null,null,"Road Vehicles","16 t tipper",35,0.8,28,7.4736020156000005E-2,1.63996E-2,9.1135620156000005E-2,"SPONS 2006"]
[null,null,"Road Vehicles","24 t tipper",40,0.8,32,8.5412594464E-2,1.8742399999999999E-2,0.10415499446400001,"SPONS 2006"]
[null,null,"Road Vehicles","Low loader wagon",40,0.8,32,8.5412594464E-2,1.8742399999999999E-2,0.10415499446400001,"SPONS 2006"]
[null,null,"Road Vehicles","Concrete wagon",20.5,0.75,15.375,4.1038082496375E-2,9.0051374999999996E-3,5.0043219996375003E-2,"SPONS 2006"]
[null,null,"Road Vehicles","Platform lorry",15,0.8,12,3.2029722923999998E-2,7.0283999999999998E-3,3.9058122924000002E-2,"SPONS 2006"]
[null,null,"Road Vehicles","Road Sweeper",12,0.75,9,2.4022292192999999E-2,5.2712999999999996E-3,2.9293592193000002E-2,"SPONS 2006"]
[null,null,"Small Plant","Stihl Saw",0.2,0.75,0.15000000000000002,4.0037153655000007E-4,8.7855000000000005E-5,4.8822653655000009E-4,"SPONS 2006"]
[null,null,"Small Plant","Floor Cutting Saw",0.3,0.75,0.22499999999999998,6.0055730482499992E-4,1.3178249999999997E-4,7.3233980482499998E-4,"SPONS 2006"]
[null,null,"Small Plant","Power Generator upto 8kva",1.8,0.85,1.53,4.0837896728100004E-3,8.9612099999999994E-4,4.9799106728100001E-3,"SPONS 2006"]

{"sheet":"DistanceLists","index":16,"n_rows":361,"n_cols":42,"rows_kept":361,"cut":false,"hidden":true,"merged":[]}
["Distance to site","Avg Distance",null,null,"Vehicle","Avrg",null,"Fuel",null,"Vehicle",null,"Vehicle","Fuel","Unit","Total t CO2e/litre",null,"Region",null,"ONS Ref.","Region","Area","(2011) Average distance commuted to work (km)",null,"Other Mode of Transport",null,"Mode","Type","Max Wieght","Unit","Combustion Measure t CO2e","WTT Measure t CO2e","Total t CO2e",null,"Maintenance Vehicle","Average C02e t",null,"Size of project","Labour Travel t CO2e per week","Management Staff Travel t CO2e per week",null,"Plant Transport (sum) Size of project","Total"]
["Local",25,null,null,"Car",2.1871777777777778E-4,null,"Diesel",null,"Car",null,"Car","Diesel","km",2.5976333333333331E-4,null,"East Midlands",null,"E12000001","North East","North East",16.5,null,"Aeroplane - Freight",null,"Van","Average (up to 3.5 tonnes)",3.5,"km",2.5092315999999997E-4,5.482E-5,3.0574315999999999E-4,null,"Car",1.8184555555555599E-4,null,"Very large (construction cost more than £10 million, more than 25 people permanently on site)",2.1551999999999998,0.77587200000000001,null,"Very large (construction cost more than £10 million, more than 25 people permanently on site)",1.2592748780399998]
["Regional",100,null,null,"Motorbike",1.3287000000000002E-4,null,"Petrol",null,"Motorbike",null,"Car","Petrol","km",2.2490000000000002E-4,null,"East of England",null,"E06000048","North East","Northumberland",21.4,null,"Freight Train",null,"HGV","All HGVs",33,"km",9.0656999999999999E-4,1.98057086E-4,1.104627086E-3,null,"Van",2.5092315999999997E-4,null,"Large (construction cost £5 to £10 million, between 16 & 25 people permanently on site)",1.7241599999999999,0.43103999999999998,null,"Large (construction cost £5 to £10 million, between 16 & 25 people permanently on site)",0.99416437740000019]
["National",500,null,null,"Car Share",0,null,"Hybrid",null,"Bicycle",null,"Car","Hybrid","km",1.7149000000000003E-4,null,"Inner London",null,"E06000047","North East","County Durham",17.399999999999999,null,"Cargo Ship",null,"Aeroplane - Freight","Average ",null,"tonne.km",2.6899666666666665E-3,2.9310000000000002E-4,2.9830666666666667E-3,null,"HGV",8.3060000000000002E-4,null,"Medium (construction cost £1.5 to £5million, between 9 & 15 people permanently on site)",1.0344959999999999,0.2241408,null,"Medium (construction cost £1.5 to £5million, between 9 & 15 people permanently on site)",0.66277625160000009]
[null,null,null,null,"Bicycle",0,null,"N/A",null,"Walking",null,"Motorbike","Petrol","km",1.3287000000000002E-4,null,"London",null,"E06000003","North East","Redcar and Cleveland",17.2,null,null,null,"Freight Train","Average ",null,"tonne.km",2.8309999999999998E-5,6.02E-6,3.4329999999999998E-5,null,null,null,null,"Small (construction cost less than £1.5million, fewer than 8 people permanently on site)",0.387936,0.1206912,null,"Small (construction cost less than £1.5million, fewer than 8 people permanently on site)",0.26511050064000002]
[null,null,null,null,"Walking",0,null,"Average",null,"Rail",null,"Bicycle","N/A","km",0,null,"North East",null,"E08000023","North East","South Tyneside",16.100000000000001,null,null,null,"Cargo Ship","General Cargo - Average",null,"tonne.km",1.3154000000000001E-5,2.4559999999999999E-6,1.5610000000000001E-5]
[null,null,null,null,"Rail",5.6039999999999999E-5,null,null,null,"Van",null,"Walking","N/A","km",0,null,"North West",null,"E06000004","North East","Stockton-on-Tees",15.9]
[null,null,null,null,"Van",3.0574315999999999E-4,null,null,null,"Bus",null,"Rail","N/A","km",5.6039999999999999E-5,null,"Outer London",null,"E06000001","North East","Hartlepool",15.9,null,"Mode"]
[null,null,null,null,"Bus",1.2354E-4,null,null,null,null,null,"Van","N/A","km",3.0574315999999999E-4,null,"South East",null,"E06000005","North East","Darlington",15.7,null,"Van"]
[null,null,null,null,null,null,null,null,null,null,null,"Bus","N/A",null,1.2354E-4,null,"South West",null,"E08000022","North East","North Tyneside",15.5,null,"HGV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wales",null,"E08000021","North East","Newcastle upon Tyne",15.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"West Midlands",null,"E08000024","North East","Sunderland",14.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yorkshire & Humber",null,"E06000002","North East","Middlesbrough",14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000020","North East","Gateshead",14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E12000002","North West","North West",14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000030","North West","Eden",20]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000026","North West","Allerdale",18.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000031","North West","South Lakeland",17.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000050","North West","Cheshire West and Chester",17.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000049","North West","Cheshire East",16.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000029","North West","Copeland",16.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000121","North West","Lancaster",16.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000125","North West","Rossendale",15.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000014","North West","Sefton",15.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000127","North West","West Lancashire",15.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000124","North West","Ribble Valley",15.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000128","North West","Wyre",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000118","North West","Chorley",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000007","North West","Warrington",15]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000015","North West","Wirral",14.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000028","North West","Carlisle",14.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000006","North West","Halton",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000119","North West","Fylde",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000013","North West","St. Helens",14.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000122","North West","Pendle",14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000011","North West","Knowsley",13.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000010","North West","Wigan",13.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000002","North West","Bury",13.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000012","North West","Liverpool",13.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000001","North West","Bolton",13]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000126","North West","South Ribble",13]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000009","North West","Trafford",12.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000008","North West","Blackburn with Darwen",12.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000123","North West","Preston",12.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000006","North West","Salford",12.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000007","North West","Stockport",12.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000003","North West","Manchester",12.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000005","North West","Rochdale",12.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000117","North West","Burnley",12.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000120","North West","Hyndburn",11.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000009","North West","Blackpool",11.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000008","North West","Tameside",11.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000004","North West","Oldham",11.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000027","North West","Barrow-in-Furness",11.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E12000003","Yorkshire & Humber","Yorkshire & Humber",14.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000167","Yorkshire & Humber","Ryedale",21.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000169","Yorkshire & Humber","Selby",21.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000166","Yorkshire & Humber","Richmondshire",21.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000163","Yorkshire & Humber","Craven",21.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000164","Yorkshire & Humber","Hambleton",20.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000011","Yorkshire & Humber","East Riding of Yorkshire",18.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000165","Yorkshire & Humber","Harrogate",16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000013","Yorkshire & Humber","North Lincolnshire",16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000168","Yorkshire & Humber","Scarborough",16.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000017","Yorkshire & Humber","Doncaster",16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000014","Yorkshire & Humber","York",15.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000016","Yorkshire & Humber","Barnsley",14.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000018","Yorkshire & Humber","Rotherham",14.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000019","Yorkshire & Humber","Sheffield",14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000036","Yorkshire & Humber","Wakefield",13.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000012","Yorkshire & Humber","North East Lincolnshire",13.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000035","Yorkshire & Humber","Leeds",13.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000034","Yorkshire & Humber","Kirklees",12.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000032","Yorkshire & Humber","Bradford",12.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000033","Yorkshire & Humber","Calderdale",12.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000010","Yorkshire & Humber","Kingston upon Hull, City of",11.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E12000004","East Midlands","East Midlands",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000017","East Midlands","Rutland",20.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000155","East Midlands","South Northamptonshire",20.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000141","East Midlands","South Kesteven",20.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000142","East Midlands","West Lindsey",19.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000139","East Midlands","North Kesteven",19.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000152","East Midlands","East Northamptonshire",19.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000151","East Midlands","Daventry",19.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000175","East Midlands","Newark and Sherwood",18.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000137","East Midlands","East Lindsey",18.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000131","East Midlands","Harborough",18.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000176","East Midlands","Rushcliffe",18]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000133","East Midlands","Melton",17.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000035","East Midlands","Derbyshire Dales",17.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000171","East Midlands","Bassetlaw",17.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000140","East Midlands","South Holland",17.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000033","East Midlands","Bolsover",16.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000039","East Midlands","South Derbyshire",16.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000156","East Midlands","Wellingborough",16.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000134","East Midlands","North West Leicestershire",16.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000038","East Midlands","North East Derbyshire",15.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000153","East Midlands","Kettering",15.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000037","East Midlands","High Peak",15.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000150","East Midlands","Corby",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000132","East Midlands","Hinckley and Bosworth",15.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000172","East Midlands","Broxtowe",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000174","East Midlands","Mansfield",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000034","East Midlands","Chesterfield",14.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000130","East Midlands","Charnwood",14.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000032","East Midlands","Amber Valley",13.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000138","East Midlands","Lincoln",13.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000170","East Midlands","Ashfield",13.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000154","East Midlands","Northampton",13.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000018","East Midlands","Nottingham",13.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000036","East Midlands","Erewash",13.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000136","East Midlands","Boston",13.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000173","East Midlands","Gedling",13.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000129","East Midlands","Blaby",13.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000015","East Midlands","Derby",12.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000135","East Midlands","Oadby and Wigston",12]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000016","East Midlands","Leicester",10.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E12000005","West Midlands","West Midlands",14.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000221","West Midlands","Stratford-on-Avon",18.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000051","West Midlands","Shropshire",18.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000235","West Midlands","Malvern Hills",18.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000238","West Midlands","Wychavon",17.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000194","West Midlands","Lichfield",17.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000019","West Midlands","Herefordshire, County of",16.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000234","West Midlands","Bromsgrove",16.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000197","West Midlands","Stafford",16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000196","West Midlands","South Staffordshire",15.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000220","West Midlands","Rugby",15.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000222","West Midlands","Warwick",15.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000198","West Midlands","Staffordshire Moorlands",15.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000218","West Midlands","North Warwickshire",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000020","West Midlands","Telford and Wrekin",15.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000192","West Midlands","Cannock Chase",14.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000239","West Midlands","Wyre Forest",14.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000193","West Midlands","East Staffordshire",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000199","West Midlands","Tamworth",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000029","West Midlands","Solihull",14.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000237","West Midlands","Worcester",14.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000195","West Midlands","Newcastle-under-Lyme",14.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000219","West Midlands","Nuneaton and Bedworth",13.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000031","West Midlands","Wolverhampton",13.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000236","West Midlands","Redditch",12.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000026","West Midlands","Coventry",12.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000025","West Midlands","Birmingham",12.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000021","West Midlands","Stoke-on-Trent",11.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000030","West Midlands","Walsall",11.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000027","West Midlands","Dudley",11.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E08000028","West Midlands","Sandwell",10.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E12000006","East of England","East of England",17.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000077","East of England","Uttlesford",22.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000074","East of England","Maldon",21.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000067","East of England","Braintree",21.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000011","East of England","Huntingdonshire",20.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000147","East of England","North Norfolk",20.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000009","East of England","East Cambridgeshire",20.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000075","East of England","Rochford",20.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000203","East of England","Mid Suffolk",20]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000143","East of England","Breckland",19.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000076","East of England","Tendring",19.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000099","East of England","North Hertfordshire",19.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000200","East of England","Babergh",19.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000056","East of England","Central Bedfordshire",19.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000068","East of England","Brentwood",18.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000069","East of England","Castle Point",18.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000070","East of England","Chelmsford",18.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000071","East of England","Colchester",18.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000010","East of England","Fenland",18.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000146","East of England","King`s Lynn and West Norfolk",18.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000097","East of England","East Hertfordshire",18.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000149","East of England","South Norfolk",18.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000033","East of England","Southend-on-Sea",17.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000100","East of England","St Albans",17.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000066","East of England","Basildon",17.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000034","East of England","Thurrock",17.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000012","East of England","South Cambridgeshire",17.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000205","East of England","Suffolk Coastal",17.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000204","East of England","St Edmundsbury",17.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000201","East of England","Forest Heath",16.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000145","East of England","Great Yarmouth",16.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000206","East of England","Waveney",16.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000055","East of England","Bedford",16.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000096","East of England","Dacorum",16.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000072","East of England","Epping Forest",15.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000031","East of England","Peterborough",15.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000102","East of England","Three Rivers",15.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000101","East of England","Stevenage",15.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000144","East of England","Broadland",14.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000032","East of England","Luton",14.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000104","East of England","Welwyn Hatfield",14.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000095","East of England","Broxbourne",14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000098","East of England","Hertsmere",13.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000202","East of England","Ipswich",13.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000103","East of England","Watford",13.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000073","East of England","Harlow",12.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000008","East of England","Cambridge",12.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000148","East of England","Norwich",11.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E12000007","London","London",11.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E13000001","Inner London","Inner London",9.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000025","London","Newham",12.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000023","London","Lewisham",11]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000014","London","Haringey",10.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000032","London","Wandsworth",10.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000022","London","Lambeth",9.6999999999999993]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000028","London","Southwark",9.1999999999999993]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000013","London","Hammersmith and Fulham",9.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000030","London","Tower Hamlets",8.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000020","London","Kensington and Chelsea",8.6999999999999993]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000012","London","Hackney",8.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000007","London","Camden",8.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000033","London","Westminster",8.1999999999999993]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000019","London","Islington",8.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000001","London","City of London",7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E13000002","Outer London","Outer London",12.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000016","London","Havering",14.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000002","London","Barking and Dagenham",13.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000004","London","Bexley",13.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000006","London","Bromley",13.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000008","London","Croydon",13.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000026","London","Redbridge",13.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000015","London","Harrow",12.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000027","London","Richmond upon Thames",12.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000021","London","Kingston upon Thames",12.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000011","London","Greenwich",12.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000017","London","Hillingdon",12.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000010","London","Enfield",11.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000024","London","Merton",11.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000029","London","Sutton",11.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000031","London","Waltham Forest",11.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000009","London","Ealing",11.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000003","London","Barnet",11.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000018","London","Hounslow",11.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E09000005","London","Brent",10.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E12000008","South East","South East",16.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000094","South East","Winchester",21]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000105","South East","Ashford",20.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000085","South East","East Hampshire",20.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000216","South East","Waverley",20.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000065","South East","Wealden",20.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000116","South East","Tunbridge Wells",19.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000064","South East","Rother",19.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000106","South East","Canterbury",19.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000112","South East","Shepway",19.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000113","South East","Swale",19.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000228","South East","Mid Sussex",19.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000004","South East","Aylesbury Vale",19.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000111","South East","Sevenoaks",19.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000063","South East","Lewes",19.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000227","South East","Horsham",19]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000115","South East","Tonbridge and Malling",18.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000043","South East","Brighton and Hove",18.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000005","South East","Chiltern",18.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000108","South East","Dover",18.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000089","South East","Hart",18.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000035","South East","Medway",18.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000114","South East","Thanet",18.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000109","South East","Gravesham",18.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000225","South East","Chichester",18.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000110","South East","Maidstone",17.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000093","South East","Test Valley",17.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000215","South East","Tandridge",17.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000181","South East","West Oxfordshire",17.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000091","South East","New Forest",17.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000179","South East","South Oxfordshire",17.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000084","South East","Basingstoke and Deane",17]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000177","South East","Cherwell",16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000037","South East","West Berkshire",16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000224","South East","Arun",16.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000209","South East","Guildford",16.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000217","South East","Woking",16.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000214","South East","Surrey Heath",16.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000006","South East","South Bucks",16.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000007","South East","Wycombe",16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000087","South East","Fareham",15.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000180","South East","Vale of White Horse",15.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000041","South East","Wokingham",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000107","South East","Dartford",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000210","South East","Mole Valley",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000042","South East","Milton Keynes",15.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000207","South East","Elmbridge",15.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000062","South East","Hastings",15.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000223","South East","Adur",15.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000040","South East","Windsor and Maidenhead",15.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000211","South East","Reigate and Banstead",15.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000090","South East","Havant",14.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000229","South East","Worthing",14.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000092","South East","Rushmoor",14.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000061","South East","Eastbourne",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000086","South East","Eastleigh",14.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000226","South East","Crawley",14.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000038","South East","Reading",14.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000036","South East","Bracknell Forest",14.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000088","South East","Gosport",14.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000044","South East","Portsmouth",13.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000212","South East","Runnymede",13.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000208","South East","Epsom and Ewell",13.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000046","South East","Isle of Wight",12.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000045","South East","Southampton",12.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000039","South East","Slough",12.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000178","South East","Oxford",12.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000213","South East","Spelthorne",11.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E12000009","South West","South West",16.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000053","South West","Isles of Scilly",30.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000047","South West","West Devon",23.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000044","South West","South Hams",22.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000079","South West","Cotswold",21.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000052","South West","Cornwall",19.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000042","South West","Mid Devon",19.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000054","South West","Wiltshire",18.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000191","South West","West Somerset",18.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000050","South West","North Dorset",18.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000080","South West","Forest of Dean",18.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000046","South West","Torridge",18.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000052","South West","West Dorset",18]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000040","South West","East Devon",18]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000024","South West","North Somerset",17.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000049","South West","East Dorset",17.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000051","South West","Purbeck",17.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000188","South West","Sedgemoor",17.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000045","South West","Teignbridge",17.100000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000082","South West","Stroud",17]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000187","South West","Mendip",16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000026","South West","Plymouth",16.399999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000189","South West","South Somerset",16.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000030","South West","Swindon",15.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000053","South West","Weymouth and Portland",15.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000043","South West","North Devon",15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000190","South West","Taunton Deane",14.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000048","South West","Christchurch",14.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000025","South West","South Gloucestershire",14.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000022","South West","Bath and North East Somerset",14.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000083","South West","Tewkesbury",14.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000027","South West","Torbay",13.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000028","South West","Bournemouth",13.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000029","South West","Poole",13.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000078","South West","Cheltenham",13.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000081","South West","Gloucester",12.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E06000023","South West","Bristol, City of",12]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E07000041","South West","Exeter",11.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W92000004","Wales","Wales",16.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000001","Wales","Anglesey",22.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000023","Wales","Powys",22.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000021","Wales","Monmouthshire",21.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000002","Wales","Gwynedd",21.6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000008","Wales","Ceredigion",21.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000009","Wales","Pembrokeshire",20.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000010","Wales","Carmarthenshire",20.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000003","Wales","Conwy",18.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000004","Wales","Denbighshire",17.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000005","Wales","Flintshire",16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000013","Wales","Bridgend",16.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000014","Wales","The Vale of Glamorgan",16.600000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000012","Wales","Neath Port Talbot",16.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000016","Wales","Rhondda, Cynon, Taff",16.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000024","Wales","Merthyr Tydfil",15.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000019","Wales","Blaenau Gwent",15.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000011","Wales","Swansea",14.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000022","Wales","Newport",14.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000006","Wales","Wrexham",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000018","Wales","Caerphilly",14.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000020","Wales","Torfaen",13.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W06000015","Wales","Cardiff",12.7]